================================================================================
Intel(R) Server Board S3200SH/S3210SH System Firmware Update Package for 
Intel(R) Deployment Assistant, Intel(R) One Boot Flash Update Utility, 
The embedded EFI Shell, Windows* Preboot Execution Environment 
================================================================================
Intel Enterprise Platform & Services Division - Marketing
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================
DATE    : Jan  18, 2012
TO      : Intel(R) Server Board S3200SH/S3210SH
SUBJECT : Release Notes for System Firmware Update Package 
================================================================================
                              ABOUT THIS RELEASE
================================================================================
BIOS   : S3200X38.86B.00.00.0052   Build Date :  Nov  29, 2010
BMC    : 40
FRUSDR : 15  
================================================================================
                           Support Platforms and Dependency
================================================================================
Intel(R) Server Board S3200SH/S3210SH Processors supported: 
  Intel(R) Xeon(R) Processor 3300 Series
  Intel(R) Xeon(R) Processor 3200 Series
  Intel(R) Xeon(R) Processor 3100 Series
  Intel(R) Xeon(R) Processor 3000 Series
  Intel(R) Core(TM) 2 Quad Desktop processors
  Intel(R) Core(TM) 2 Duo Desktop processors
  Intel(R) Core(TM) 2 Extreme processors

Microcode update versions:
CPUID   Microcode   
06F2h       5Dh
06F6h       D0h
06F7h       6Ah
06FBh	    B6h
06FDh	    A3h
10661h      38h
10676h      60Fh
10677h      70Ah                                                
1067Ah      A0Bh     

Intel (R) Matrix Storage OpROM: v7.5.0.1017 
LSI OpRom                     : version 10101641
SATA AHCI BIOS                : Release Date 01-05-2007
NIC                           : Intel (R) Boot Agent GE v1.2.60
VGA                           : VBE BIOS V3.8SL
Memory Reference Code 1.32

REVISION INFORMATION RETURNED BY GET DEVICE ID COMMAND:
Operational mode              :	v00.35
UBoot mode                    :	v01.09
Device ID                     :	0x21 (Integrated BMC 2K7 Firmware)
Manufacturer ID               :	0x000157 (Intel Corporation)
Product ID                    :	0x003A (S3210SH)

Dependency:
BIOS must be at R0020 and Integrated BMC FW at v.24 before running this update.
================================================================================
                  System Firmware Update Package Usage instructions                   
================================================================================
This package can be updated using one of the following methods:
 - The embedded EFI shell
 - Intel(R) Deployment Assistant
 - Windows* or Linux* operating system using Intel(R) One-boot Flash Update (OFU)
   v9.70 Build 3.4 or later)
 - Windows* Preboot Execution Environment (WinPE)

To Update from the embedded EFI Shell

update system firmware from Intel server EFI shell by the following steps:
- Download Intel server system firmware update package from support.intel.com
- Unzip package and copy all files to a folder in USB disk on key 
- Insert USB disk on key to server USB port
- Reboot server to EFI shell
- Run command "map -r" in EFI shell to mount USB disk on key
- Run command "fs0:" to change folder to USB disk on key, USB key may also mount to
  fs1:. The number of "fs" is dependent on the result of command "map -r"
- Change folder to the folder storing the firmware package
- Run command "startup.nsh" to start firmware update process

Please refer to "EFI_Instructions.pdf" in this firmware package for a quick guide to 
use the of EFI commands

To Update from Intel(R) Deployment Assistant (IDA)

The Intel(R) Deployment Assistant software is easy to use and is present on the 
"Intel(R) Server Deployment toolkit" CD shipped with the system.
User can download the latest version IDA CD ISO image from support.intel.com
To use the IDA CD to update the system firmware:
- Boot server with IDA CD
- Select "Get System Updates" 
- Choose one of the three options 

  . From support.intel.com
    Automatically downloads the latest Firmware Update Package from Intel 
    It requires Internet connection
    Enter your local IP address and proxy configuration
    Click "Next" to start the download and update process

  . From my network
    Download the latest Firmware Update Package from support.intel.com and copy 
    it to a Windows* shared folder
    Enter your local IP address, the Windows* file server name, and a
    Windows user name and password
    Select the firmware package in pop-up window
    Click "Next" to start the update process

  . From USB Disk on Key or Hard Disk
    Download the latest Firmware Update Package from support.intel.com and copy it 
    to a USB key, then insert the key into the server USB port
    Click "Browse"
    Select the firmware package in pop-up window
    Click "Next" to start the update process
    
  Note: The Firmware Update Package is in the ZIP file format. Do not unzip 
        before copying to a Windows* shared folder or USB disk.

To update from Windows* and Linux* or operating systems using the Intel(R) One Boot
Flash Update Utility (OFU)

Intel(R) One boot Flash Update utility can be downloaded from support.intel.com
and it is part of the "BIOS, Firmware Update & Configuration Utilities" for 
Windows* and Linux*. Please refer to Intel OFU user guide about the details of 
installation and usage of OFU.

Use OFU to update system firmware by the following steps:
- Install OFU on Windows* or Linux* system
- Download the latest firmware update package from support.intel.com
- Unzip package to a folder
- Run the following command in Windows* command line/Linux* terminal window:
  <OFU install folder name>:\flashupdt -u  <package folder name>\flashupdt.cfg
                       
To update from Windows* Preboot Execution Environment (WinPE)

The System Firmware Update Package can be inserted to Windows* PE customized image 
for creating a bootable Windows* PE CD. User is able to update system firmware from 
customized WinPE CD by the following steps:
- Boot server with customized WinPE CD
- Run script "WinPE21_x64_Update.bat" or "WinPE20_x86_Update.bat" 
  (name may be varied depends on your own customization)
  
Note:
1. The Intel(R) OFU utility is case sensitive. Therefore, when you transfer the 
Firmware Update Package using USB key from a Microsoft Windows* system to a Linux
environment, you must first extract under the Linux* environment. Otherwise, you 
will need to mount the USB key manually with ¡°vfat¡± option under Linux to avoid 
conversion from upper case to lower case and vice versa.

2. In this SFUP package, Intel only provides batch file "WinPE20_x86_Update.bat"
for WinPE2.0 32 bit solution and "WinPE21_x64_Update.bat" for WinPE2.1 64 bit solution 
as examples. Please refer to white paper "White Paper-Intel Server Utilities Procedure 
for WinPE.pdf" for details on building your own customized WinPE CD.

3. Windows PE 2.0 - built from Windows Vista SP1 32bit

4. Windows PE 2.1 - built from Windows Vista SP1 or Windows Server 2008, EM64T

=============================================================================
                        BIOS RECOVERY INSTRUCTIONS
=============================================================================
Recovery process can be initiated by setting the recovery jumper (called force 
recovery)

A BIOS recovery can be accomplished from SATA CD and USB Mass Storage device. 
Please note that recovery from USB floppy is not supported on this platform. 

SATA CD image for recovery is created using El-Torito format image (which is 
bootable).

The recovery media must contain the image file: FV_MAIN.FV, under the root directory. 
And also the following files: 
1.	IFLASH32.EFI
2.	*.CAP
3.	Startup.nsh 

Note: 
Please use the Startup.nsh file under the Recovery folder for BIOS recovery. 

The BIOS starts the recovery process by first loading and booting to the recovery 
image file (FV_MAIN.FV) on the root directory of the recovery media (SATA CD or USB 
disk). This process takes place before any video or console is available. Once the 
system boots to this recovery image file (FV_MAIN.FV), it would boot automatically 
into EFI Shell and invoke the Startup.nsh. and the flash update application 
(IFLASH32.EFI). 

IFLASH32.EFI requires the supporting BIOS Capsule image file (*.CAP).  

At last, there would have two short beeps indicating the completion of the recovery. 
User should switch the recovery jumper back to normal operation and restart the system 
by doing power cycle.


The following steps illustrate the recovery process:
1.  Power off the system, insert recovery media.
2.  Switch the recovery jumper,The details of the jumper can be found in the Board TPS. 
3.  Power on the system.
4.  The BIOS POST screen will appear and display the progress, and system would 
    automatically boot to the EFI SHELL.
5.  Startup.NSH file would be automatically invoked. It will initiate the flash update 
    (IFLASH32.EFI)  with new capsule file (*.CAP). The message will be displayed if 
    flash update succeeds. 
6.  Once the flash update is completed, two beeps would be heard. User should Power off 
    the system, and revert the recovery jumper back to normal operation.
7.  Power on the system. 

DON'T INTERRUPT THE POST PROCESS AT THE FIRST BOOT.

================================================================================
                         BIOS Changes in release 52
================================================================================
BIOS R52 Issues Fixed:
- Added	Microcode Update - SRV_P_96 to address the following:
	Intel?Xeon?Processor 3000 Series Specification Update, Erratum AP129

BIOS R51 Issues Fixed:
- "Pause" key will cause POST hang
Added: 
- LOGO security issue
- Support second source of flash chip

BIOS R49 Issues Fixed:
- Updated SMM memory utilization

BIOS R47 Issues Fixed:
- PS2 Keyboard/Mouse can not work with E5200 CPU.
- Front panel USB port can not recognize USB1.1 device.

BIOS R46 Issues Fixed:
- PCI-E Network Adapter Wake On LAN can't power on monitor issue.
Added: 
- EFI bootable support 

BIOS R45 Issues Fixed:
- CPU family name change from "Core 2 Duo" to "Core 2"
Added: 
- Add USB device boot priority item in setup.
- SMS 3.0 IPMI set Boot device order command support.
- Add "FWVERSIONDATA" NVRAM variable to support OA2.0.
- OHCI USB card support.

BIOS R44 Issues Fixed:
- N/A
Added: 
- E-0 and R-0 CPU microcode support. 

================================================================================
                         BMC Changes in release 40
================================================================================
BMC FW40:
- Fixed S3210SH BMC Gateway IP can not be set issue
BMC FW39:
- Update fix for issue "Resume on AC Power Loss option does not work as design"

BMC FW38:
- Fixed issue "Resume on AC Power Loss option does not work as design"

BMC FW37:
- Fixed issue "Cannot ping the BMC LAN interface after setting IP address and 
  mask after a force BMC update."

BMC FW36:
- Added support for Micronix Flash device.
- Updated Driver Source file headers previously missed.

BMC FW35:
- Updated Driver Source file headers. 

BMC FW34:
- Fixed issue "Use SysCfg to configure BMC's IPMI IP address causes BMC hang." 

BMC FW33:
- Updated I2C driver to fix HSC FW Update issues.

BMC FW32 Issues Fixed:
- Remotely resetting SR1530SH via IPMI results in BMC hang
- User ID 1 disabled after AC cycle
- 8190 Watchdog timer error

BMC FW31 Issues Fixed:
- BMC firmware crashes when telnet to it
- HSC Get Buffer Size command returns extra one byte

BMC FW30 Issues Fixed:
- SYSFAN3 and SYSFAN4 speeds are going low when rebooting the system from Windows

BMC FW29 Issues Fixed:
- FRUSDR.EFI's PROBE "PING" command does not work with HSC
- IPMB communication to HSBP fails and hangs IPMB
- Not able to update BP6 firmware

================================================================================
                     FRUSDR Changes in release 15
================================================================================   FRUSDR 15 Issues Fixed:
- Removed PCI fan monitoring on SR1530SH
 
FRUSDR 14 Issues Fixed:
- N/A
Added:
Increased Product Area of FRU by 24 bytes to allow 14 byte Serial numbers.

FRUSDR 13 Issues Fixed:
- N/A

FRUSDR 12 Issues Fixed:
- Removed possible long delay when checking for HSC

FRUSDR 11 Issues Fixed:
- N/A
Added:
- Message when detecting HSC for notification of possible long delay
=============================================================================
                            LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products. 
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation may 
have patents or pending patent applications, trademarks, copyrights, or other 
intellectual property rights that relate to the presented subject matter.  
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any 
such patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product 
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 
*Other names and brands are the property of their respective owners.
Copyright (c) 2012 Intel Corporation.

A portion of this firmware is open source code, which falls under the
GPL 2.0 license.  

[END OF RELEASE NOTES]
