================================================================================
Intel(R) Server Board S2400LP Family
Intel(R) Server System H2000LP Family Firmware Update Package
for Intel(R) Deployment Assistant, Intel(R) One Boot Flash Update Utility, 
The embedded EFI Shell, Windows* Preboot Execution Environment 
================================================================================
Intel Enterprise Platform & Services Division - Marketing
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================
DATE    : May. 15, 2012
TO      : Intel(R) Server Board S2400LP Family
	  Intel(R) Server System H2000LP Family customers
SUBJECT : Release Notes for System Firmware Update Package 
================================================================================
                              ABOUT THIS RELEASE
================================================================================
BIOS   : 01.02.0006
ME     : 02.01.05.091
BMC    : 1.06.3137
FRUSDR : 1.05
================================================================================
                           Support Platforms and Dependency
================================================================================
Processors supported: 
Intel(R) Xeon processor E5-2600/2400 series

Microcode update versions:
Intel(R) Xeon processor E5-2600/2400 series C0 stepping: 0x80000513 CPUID = 0x206D5
Intel(R) Xeon processor E5-2600/2400 series C1 stepping: 0x80000615 CPUID = 0x206D6
Intel(R) Xeon processor E5-2600/2400 series C2 stepping: 0x8000070A CPUID = 0x206D7


Production boards:
  Product		    Fab Version	      
  S2400LP		    Fab2 or above     

Before update to the BIOS/ME/BMC/FRUSDR contained in the package, please check in BIOS 
set up menu and verify your board has below BIOS/ME/BMC/FRUSDR versions installed:

  - BIOS R043.1, or later Version
  - ME 02.01.05.69 or later Version
  - BMC 01.00.2812 or later Version
  - FRUSDR 1.04 or later version

The following update process must be followed to ensure a trouble free update.
1.	BMC firmware to 1.00 or later
2.	BIOS x043.1 or later
3.	Manageability Engine (ME) firmware 02.01.05.69 or later
4.	Latest FRU/SDR package specific to the baseboard.

================================================================================
                  System Firmware Update Package Usage instructions                   
================================================================================
This package can be updated using one of the following methods:
 - The embedded UEFI shell
 - Intel(R) Deployment Assistant
 - Windows* or Linux* operating system using Intel(R) One-boot Flash Update (OFU)
   V11.0 Build 7 or later)
 - Windows* Preboot Execution Environment (WinPE)

To Update from the embedded EFI Shell

update system firmware from Intel server EFI shell by the following steps:
- Download Intel server system firmware update package from http://www.intel.com/support/
- Unzip package and copy all files to root folder in USB disk on key 
- Insert USB disk on key to server USB port
- Reboot server, system will start BIOS/BMC/FRUSDR update automatically

  If case for some reason or you didn't put unzipped package under root folder of USB key, 
  you can do it by:
- Reboot server to EFI shell manually
- Run command "map -r" in EFI shell to mount USB disk on key
- Run command "fs0:" to change folder to USB disk on key, USB key may also mount to
  fs1:. The number of "fs" is dependent on the result of command "map -r"
- Change folder to the folder storing the firmware package
- Run command "startup.nsh" to start firmware update process

Please refer to "EFI_Instructions.pdf" in this firmware package for a quick guide to 
use the EFI commands

To Update from Intel(R) Deployment Assistant (IDA)

The Intel(R) Deployment Assistant software is easy to use and is present on the 
"Intel(R) Server Deployment & Management" DVD shipped with the system.
User can download the latest version IDA CD ISO image from http://www.intel.com/support/
To use the IDA CD to update the system firmware:
- Boot server with IDA CD
- Select "Get System Updates" 
- Choose one of the three options 

  . From http://www.intel.com/support/
    Automatically downloads the latest Firmware Update Package from Intel 
    It requires Internet connection
    Enter your local IP address and proxy configuration
    Click "Next" to start the download and update process

  . From my network
    Download the latest Firmware Update Package from http://www.intel.com/support/ and copy 
    it to a Windows* shared folder
    Enter your local IP address, the Windows* file server name, and a
    Windows user name and password
    Select the firmware package in pop-up window
    Click "Next" to start the update process

  . From USB Disk on Key or Hard Disk
    Download the latest Firmware Update Package from http://www.intel.com/support/ and copy it 
    to a USB key, then insert the key into the server USB port
    Click "Browse"
    Select the firmware package in pop-up window
    Click "Next" to start the update process
    
  Note: The Firmware Update Package is in the ZIP file format. Do not unzip 
        before copying to a Windows* shared folder or USB disk.

To update from Windows* and Linux* or operating systems using the Intel(R) One Boot
Flash Update Utility (OFU)

Intel(R) One boot Flash Update utility can be downloaded from http://www.intel.com/support/
and it is part of the "BIOS, Firmware Update & Configuration Utilities" for 
Windows* and Linux*. Please refer to Intel OFU user guide about the details of 
installation and usage of OFU.

Use OFU to update system firmware by the following steps:
- Install OFU on Windows* or Linux* system
- Download the latest firmware update package from http://www.intel.com/support/
- Unzip package to a folder
- Run the following command in Windows* command line/Linux* terminal window:
  <OFU install folder name>:\flashupdt -u  <package folder name>\flashupdt.cfg
                       
To update from Windows* Preboot Execution Environment (WinPE)

The System Firmware Update Package can be inserted to Windows* PE customized image 
for creating a bootable Windows* PE CD. User is able to update system firmware from 
customized WinPE CD by the following steps:
- Boot server with customized WinPE CD
- Run script "WinPE21_x64_Update.bat" or "WinPE20_x86_Update.bat" 
  (name may be varied depends on your own customization)
  
Note:
1. The Intel(R) OFU utility is case sensitive. Therefore, when you transfer the 
Firmware Update Package using USB key from a Microsoft Windows* system to a Linux
environment, you must first extract under the Linux* environment. Otherwise, you 
will need to mount the USB key manually with 'vfat' option under Linux to avoid 
conversion from upper case to lower case and vice versa.

2. To make Intel(R) OFU utility run properly under x86 or x64 OS, you have to read
OFU releaenotes on known issues for OFU installation.

3. In this SFUP package, Intel only provide batch file "WinPE_x86_Update.bat"
for WinPE2.0 32 bit solution "WinPE_x64_Update.bat" for WinPE2.1/3.0 64 bit 
solution as an example. Please refer to white paper "White Paper-Intel Server 
Utilities Procedure for WinPE.pdf" for details on building your own customized 
WinPE CD.

4. Windows PE 2.0 - built from Windows Vista SP1 32bit or EM64T
5. Windows PE 2.1 - built from Windows Vista SP1 or Windows Server 2008, EM64T
6. Windows PE 3.1 - built from Windows Server 2008R2, EM64T
7. Microsoft IPMI driver is loaded by default from WinPE CD, if you want to use 
Intel IPMI driver instead of MS IPMI driver for firmware update, you can un-install
Microsoft IPMI driver by:
                Devicesetup.exe ¨Cv remove *IPI0001
                Note: IPI0001 is the device ID for Microsoft IPMI driver.

=================================================================================   
 	            BIOS 01.02.0006
=================================================================================  
Others:
- Update ME version to 02.01.05.091,

================================================================================
	            ME 02.01.05.091
================================================================================
- Fixed: Fix for Double AC cycle for recognizing OPROM changes.

================================================================================
                    BMC Changes in release 1.06.3156
================================================================================
Note: The update package provided for this release was validated with BIOS
release x045.
- Fixed: Patch fixes a problem with excessive Power Supply SEL events for 1200W
         power supplies.
- Fixed: Update cipher suite LAN parameters to be consistent with IPMI spec
- Fixed: Update S2400LP SDR for factory build, FAN4a~6b was added 
- Fixed: Changed Node Manager SEL entry descriptions.
- Fixed: Update for S2400LP to solve the FAN5a~6b reading zero issue reported
         by the factory. 
- Fixed: Update S2400EP Default SDR
- Fixed: Add more thorough checking to Embedded Web Server action image
         validation
- Fixed: Update SDR on slave node, PSU temp sensors will be in Disabled status,
         while other PSU sensors are correct 
- Fixed: A failed node can't be power-offed gracefully by BMC when there is a
         simulated critical event of a temp sensor and stopped ystem fan.
- Fixed: "Shutdown Policy" available after BIOS update
         - BMC returned the wrong completion code of 'get shutdown policy'
           command on non-halfwidth platform.
- Fixed: Allow OEM Embedded Web Server image to be completely removed to
         factory settings
- Fixed: SNMP alert and Email alert can't be received when node manager power
         policy defined threshold is exceededon S2400EP  
- Fixed: The status LED will be solid amber for a while after an AC cycle on
         S2400EP, S1400FP, and S1400SP.
- Fixed: S2400LP DIMM event SEL does not match with the location in the board. 
- Fixed: Sometimes the minimum power reading is 0W on the power statistics page
         - Fixed for all platforms.
- Fixed: Unexpected results with PS fault condition(FP Status LED, BMC Sensors)
- Fixed: Slow Fan Limit event verification failed on 1200W PSU
         - Failed Power Supply status was not being maintained. Will not clear
           the PS Fault status until the Power Good is negated.
- Fixed: Read platform debug command after exitng the debug log file transfer
         mode, the response is failed
- Fixed: BMC may hold IPMB CLK low after BMC reset if the BMC is addressed over
         IPMB and the BMC resets before that I2C transaction completes. 
- Fixed: BB +1.1V STBY low critical log during DC off
         - The 1.1V Stby voltage sensor was generating events when the power
           button was held in over 4 sec.
- Fixed: Emulex* Pilot III P02 Chip - Prefetchable bit (BAR10-BIT3) is not set
         for memory range.
- Added: Add a software-only method to replace public key and API to query key
         info

================================================================================
                    FRUSDR Changes in release 1.05
================================================================================    

S2400LP_FRUSDR_0105:
- Update some clamp record 
- Update some stepwise record
- Update DIMM Air Velocity record
- Update Normal Control Value in domain configuration record
- Update  Aggregate Sensor record
- Update System Airflow Formula Record
- Update fans-off record

=============================================================================
                            LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products. 
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation may 
have patents or pending patent applications, trademarks, copyrights, or other 
intellectual property rights that relate to the presented subject matter.  
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any 
such patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product 
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 
*Other names and brands are the property of their respective owners.
Copyright (c) 2012 Intel Corporation.

A portion of this firmware is open source code, which falls under the
GPL 2.0 license.  

[END OF RELEASE NOTES]
