EFI System Firmware Update Package Install Instructions

Intel(R) Server Board S2600GZ/GL, Intel(R) Server System R1000GZ/GL and 
Intel(R) Server System R2000GZ/GL product family
Firmware Update Package Update Instructions 

Released - June 21 2012

*************************************************************************************
This Update package includes the following system software updates:

  System BIOS  - 01.03.0002
  ME Firmware  - 02.01.05.107
  BMC Firmware - 01.10.3560
  FRUSDR       - 1.04

Important NOTES: 

- All the updates provided in this package are EFI based (unless otherwise noted).To 
  run these updates, you must boot the system to the embedded EFI shell and then 
  access the USB flash drive or hard disk containing the system software updates.


*************************************************************************************
                       SYSTEM HARDWARE and SOFTWARE REQUIREMENTS
*************************************************************************************
The contents of this update package is used to update the System Firmware for 
the following Intel Server Products only:

  - Intel(R) Server Board S2600GZ/GL Fab 3 or later
  - Intel(R) Server System R1000GZ/GL product family with Intel(R) Server Board S2600GZ/GL Fab 3 
    or later
  - Intel(R) Server System R2000GZ/GL product family with Intel(R) Server Board S2600GZ/GL Fab 3 
    or later

  - BIOS 01.01.1002, or later Version
  - ME 02.01.05.069 or later Version
  - BMC 01.00.2612 or later Version
  - FRUSDR 1.01 or later version

The utilities used to update the System Firmware are:
  - Iflash32 11.0 build 8
  - FWPIAUPD 11.0 build 6
  - FRUSDR 11.0 build 9

*************************************************************************************
                 Standard Update Procedure from the embedded EFI Shell
*************************************************************************************

- Unzip package and copy all files to a folder in USB flash drive
- Insert USB flash drive to server / workstation USB port
- Boot Server to EFI shell
- Run command "map -r" in EFI shell to mount USB flash drive
- Run command "fs0:" to change folder to USB flash drive, the USB flash drive may also mount to
  fs1:. The number of "fs#" is dependent on the result of command "map -r"
- Change folder to the folder storing the firmware package
- Run command "Startup.nsh" to start updating all the firmware and BIOS


Warning: 
!!Do NOT reboot or shut down power from your system during following software update!!


*************************************************************************************
If you want to update single components like BMC/BIOS/ME/FRUSDR separately, please go to the 
root folder and execute the specified scripts separately, and follow below 
update process to ensure trouble free update:
  1) BMC firmware update
  2) BIOS update
  3) Manageability Engine (ME) Firmware update
  4) FRUSDR update
*************************************************************************************

*************************************************************************************
                                Update BMC Firmware
*************************************************************************************
1) Boot the system to the EFI shell and go to root folder
2) At the shell prompt, run "BMC.nsh" to start BMC Firmware update
3) When complete, go to the BIOS update section described below, or power off the 
   system and cycle AC power before continuing.

*************************************************************************************
                                 Update System BIOS 
*************************************************************************************

1) Boot the system to the EFI shell and go to root folder
2) At the shell prompt, run "BIOS.nsh" to start BIOS update
3) When complete, reboot the system and enter BIOS Setup by pressing the F2 Key during
   POST 
4) Verify the BIOS string on main BIOS menu
5) Press F9 to load defaults and press F10 to save and reset the system
6) Go to the ME firmware update section described below
The BIOS update is complete. Either reboot the server or go to the ME firmware Update section 
described below.


*************************************************************************************
                                   Update ME Firmware
*************************************************************************************
1) Boot the system to the EFI shell and go to root folder
2) At the shell prompt, run "ME.nsh" to start ME firmware update
3) When complete, go to the FRUSDR update section described below, or power off the 
   system and cycle AC power before continuing.
   
*************************************************************************************
                                      Update FRUSDR
*************************************************************************************
1) Boot the system to the EFI shell and go to root folder
2) At the EFI command prompt, run "FRUSDR.nsh" to start FRUSDR update
3) Answer questions and enter desired information when prompted.
4) When complete, reboot the system by front control panel

*************************************************************************************
                                    Verifying updates
*************************************************************************************

1)  During POST, hit the F2 Key when prompted to access the BIOS Setup Utility
2)  Hit the F9 key to load BIOS Defaults
3)  At the MAIN menu verify the BIOS revision is correct
4)  Move cursor to the SERVER MANAGEMENT Menu
5)  Move cursor down to the SYSTEM INFORMATION Option and hit Enter
6)  Verify the BMC Firmware revision is correct
7)  Verify the SDR revision is correct
8)  Verify the ME Firmware revision is correct
9)  Hit the F10 Key to save changes and Exit


The System Software Update is Complete.





