=============================================================================
    Intel(R) Server Platform S2600WP FRU/SDR Update Release Notes
=============================================================================

INTEL Enterprise Platform & Services Marketing
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA

=============================================================================

DATE:   June 15, 2012

TO:	    Intel(R) Server Platform S2600WP customers

SUBJECT:    IBMC(R) FRU/SDR update package S2600WP_FRUSDR_1.05 release notes

=============================================================================
                               LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products.
No license, express or implied, by estoppel or otherwise, to any intellectual
property rights is granted by this document. Except as provided in Intel's
Terms and Conditions of Sale for such products, Intel assumes no liability
whatsoever, and Intel disclaims any express or implied warranty, relating to
sale and/or use of Intel products including liability or warranties relating
to fitness for a particular purpose, merchantability, or infringement of any
patent, copyright or other intellectual property right. Intel Corporation may
have patents or pending patent applications, trademarks, copyrights, or other
intellectual property rights that relate to the presented subject matter.
The furnishing of documents and other materials and information does not
provide any license, express or implied, by estoppel or otherwise, to any
such patents, trademarks, copyrights, or other intellectual property rights.
Intel products are not intended for use in medical, life saving, or life
sustaining applications. Intel may make changes to specifications and product
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation.

*Other names and brands are the property of their respective owners.

Copyright (c) 2010 - 2011 Intel Corporation.

=============================================================================
                              ABOUT THIS RELEASE
=============================================================================

SDR file version: 1.05
Baseboard FRU file version: 0.02
Master configuration file version: 1.05
FRUSDR loader version: 11.0 Build 11

=============================================================================
        SYSTEM HARDWARE & SOFTWARE REQUIREMENTS/REVISIONS
=============================================================================

- This FRU/SDR package has only been tested on S2600WP FAB1 baseboards.

- BMC firmware rev 00.21 (or later) MUST be preinstalled prior to installing
  this FRU/SDR package.

- BIOS R0034 or later

=============================================================================
                      IMPORTANT INSTALLATION NOTES
=============================================================================

- None

=============================================================================
            INSTALLATION PROCEDURE
=============================================================================

1. Ensure BMC release 00.21 or later is pre-installed before attempting this
   FRU/SDR update.

2. Copy all of the files in the S2600WP_FRUSDR_1.05.zip archive to a USB key,
   hard disk drive or floppy drive.
   All of the files in this zip archive must reside in the same directory.

3. Boot to EFI and then run the following command to display the
   contents of the baseboard FRU device:

    FRUSDR /d FRU

   If device is empty(which is the case for all new FAB1 baseboards) or corrupted, then
   execute the following command to program the empty FRU device:

   For S2600WP:
        FRUSDR /fru S2600WP.fru

4. Now execute the following command to bring up the main FRU/SDR load menu:

    FRUSDR /cfg master.cfg


5. Select the option which is applicable to what you want to do. On a brand
   new baseboard I would highly recommend to run option 3 to program both
   the FRU and SDR. By reprogramming the FRU you will be given the option
   to input data from the keyboard into various chassis, board and product
   areas. Ensure that you select the correct chassis from the chassis
   selection menu otherwise your fan sensors will not be configured
   properly.

6. Once the package has finished its installation, I would highly recommend
   to DC power off the system and cycle AC power.

=============================================================================
                           KNOWN ISSUES/WORKAROUNDS
=============================================================================
S2600WP_02:
- Known issue: The first time to update FRU will fail. Please use another method 
  to update FRU the first time you update FRU. Frusdr.efi /fru S2600WP.fru.
 

=============================================================================
                           FEATURES ADDED
=============================================================================
S2600WP_1.05:
- Modify HSBP FRU address in master.cfg to "AC" from "AE".
- Modify to probe IO Module FRU device instead of temperature device in master.cfg.
- Modify to set Other Chassis if GPU node power board is detected.
- Modify SDR 'Exit Air Temp' (Sensor#: 2Eh) Settable / Readable Threshold Masks
  to 0000h from 1B1Bh.
- Modify SDR 'Pwr Unit Redund' (Sensor#: 02h) Sensor Capabilities to 00h from 40h

S2600WP_1.04:
- Update SDR as per S2600WP FSC Config Sheet Rev 2.5.xlsm.
- Update FRUSDR.efi to Build 11.
- Add FRUSDR loader version into ReleaseNote.txt
- Modify SDR 'Powerville Temp' (Sensor#: 2Fh) to 'LAN NIC Temp'.

S2600WP_1.03:
- Update SDR as per S2600WP FSC Config Sheet Rev 2.4.xlsm.
- Modify SDR 'HDD 1 Status' (Sensor#: F0h) to 'HDD 0 Status'.
- Modify SDR 'HDD 2 Status' (Sensor#: F1h) to 'HDD 1 Status'.
- Modify SDR 'HDD 3 Status' (Sensor#: F2h) to 'HDD 2 Status'.
- Modify SDR 'HDD 4 Status' (Sensor#: F3h) to 'HDD 3 Status'.

S2600WP_1.02:
- Add PSU Redundant sensor when using two 1600W PSU.
- Update FRUSDR.efi to Build 9.

S2600WP_1.01:
- Update SDR as per S2600WP FSC Config Sheet Rev 2.3.xlsm.
- Modify Entity ID of 'HSBP Temp' from 0x0F to 0x40.
- Modify Entity Instances for Entity ID 0x0F.

S2600WP_1.00:
- Modify the chassis name form "Bobcat Peak 2U4N 2.5 / 3.5 SKU" 
  to "Intel(R) Server Chassis - H2216/H2312"

S2600WP_08:
- Add SDRs for 1600W(IS162F22).
- Add PBA Number G48583 for IB-QDR SKU.
- Add PBA Number G48605 for IB-FDR SKU.
- Add new SDR 'Auto Shutdown'.

S2600WP_07:
- Update SDR as per S2600WP FSC Config Sheet Rev 1.9.xlsm.
- Fix Sensor Owner ID from 33h to 01h for BIOS SDR 'QPI Link Width'.
- Fix Sensor Number from 10h to 11h for BIOS SDR 'Sparing Rdnc'.
- Modify Entity instance of SDRs.
- Add Half-Width Virtual Exit Air Temperature Sub Record for H2300WP/H2200WP.

S2600WP_06:
- Update SDR as per S2600WP FSC Config Sheet Rev 1.7.xlsm.

S2600WP_05:
- Add/Modify SDRs(Sensor Owner = 01h or 33h) to accord Romley_BIOS_EPS [0_55].pdf.

S2600WP_04:
- Update SDR as per S2600WP FSC Config Sheet Rev 1.5.xlsm.
- Remove 'PX MemYY VRD Hot' SDRs (Sensor#: 94h, 95h, 96h, 97h).
- Add SDR Type 11 (FRU), 'Pwr Supply 1 FRU', 'Pwr Supply 2 FRU', and 'HS Backplane'.
- Add 'IO Mod Presence' SDR.
- Remove the MENU "Bobcat Peak 2U2N 2.5 / 3.5 SKU" from master.cfg.

S2600WP_03:
- Update SDR as per S2600WP FSC Config Sheet Rev 1.4.xlsm.
- Modified SDR name 'MTT CPU1', 'MTT CPU2' to 'P1 MTT', 'P2 MTT'.
- Modified Sensor Type and Event/Reading Base Type of sensor #C0 and #C1 SDR

S2600WP_02:
- Update SDR as per S2600WP FSC Config Sheet Rev 1.3.xlsm.
- Update frusdr.efi to Version 11.0 Build 5.

FWP_01:
- This package is only for PO builds.
- Update SDR as per S2600WP FSC Config Sheet Rev 1.1.xlsm.

=============================================================================
                           ISSUES FIXED
=============================================================================
S2600WP_1.04:
- [EPSD100020956]: BMC auto reset after flashing FRUSDR completed.
- [EPSD100228348]: FRUSDR utility will reflash BMC after update SDR on WashingtonPass

S2600WP_1.01:
- None.

S2600WP_1.00:
- None.

S2600WP_08:
- None.

S2600WP_07:
- None.

S2600WP_06:
- [EPSD100017013]: Status LED will amber blinking when system power on before 
  BIOS post screen.
- [EPSD100017369]: Detect Temperture Exit Air Temp (#0x2E) Upper Non-Critical,
  Upper Critical event when plugged all nodes in chassis.
  
S2600WP_05:
- None.

S2600WP_04:
- [EPSD100017413]: Detect "P1/2 Mem01/23 VRD Hot (#0x94)(#0x95)(#0x96)(#0x97)" 
  event generate in SEL after boot in OS and let it idle.

S2600WP_03:
- None.

S2600WP_02:
- None.

FWP_01:
- None.

=============================================================================
                             REFERENCE MATERIAL
=============================================================================
S2600WP FSC Config Sheet Rev 2.5.xlsm datasheet
[END OF RELEASE NOTES]