================================================================================
Intel(R) Server Board S2600JF, Intel(R) Server System H2000JF Product Family 
Firmware Update Package for Intel(R) Deployment Assistant, Intel(R) One Boot 
Flash Update Utility, The embedded EFI Shell, Windows* Preboot Execution Environment 
================================================================================
Intel Enterprise Platform & Services Division - Marketing
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================
DATE    : 	June 29, 2012
TO      : 	Intel(R) Server Board S2600JF, Intel(R) Server System H2000JF
                Product Family customers
SUBJECT : 	Release Notes for System Firmware Update Package 
================================================================================
                              ABOUT THIS RELEASE
================================================================================
BIOS   : 01.03.0002
ME     : 02.01.05.107
BMC    : 01.10.3656
FRUSDR : 1.08
================================================================================
                           Support Platforms and Dependency
================================================================================
Intel(R) Server Processors supported: 
  Intel(R) Xeon(R) Processor E5-2600 series

Microcode update versions: 
Intel(R) Xeon processor E5-2600/2400 series C0 stepping: 0x80000513 CPUID = 0x206D5
Intel(R) Xeon processor E5-2600/2400 series C1 stepping: 0x80000613 CPUID = 0x206D6
Intel(R) Xeon processor E5-2600/2400 series C2 stepping: 0x80000708 CPUID = 0x206D7

Production boards:
  Product		Fab Version	      
  S2600JF		Fab3 or above     

The following update process must be followed to ensure a trouble free update.
1.	BMC firmware
2.	BIOS
3.	Manageability Engine (ME) firmware
4.	FRUSDR

================================================================================
                  System Firmware Update Package Usage instructions                   
================================================================================
This package can be updated using one of the following methods:
 - The embedded UEFI shell
 - Intel(R) Deployment Assistant
 - Windows* or Linux* operating system using Intel(R) One-boot Flash Update (OFU)
   V11.0 Build 9 or later)
 - Windows* Preboot Execution Environment (WinPE)

To update from the embedded EFI Shell

Update system firmware from Intel server EFI shell by the following steps:
- Download Intel server system firmware update package from http://downloadcenter.intel.com/
- Unzip package and copy all files to root folder in USB flash drive 
- Insert USB flash drive to server USB port
- Reboot server, system will start BIOS/BMC/FRUSDR update automatically

  If the unzipped package is not under the root folder of USB flash drive:
- Reboot server to EFI shell manually
- Run command "map -r" in EFI shell to find the mount point of the USB flash drive
- The USB flash drive may mount to fs0: or fs1: or other. 
- Run command "fs0:" or other to change folder to USB flash drive, 
- Change folder to the folder storing the firmware package
- Run command "startup.nsh" to start firmware update process

Please refer to "EFI_Instructions.pdf" in this firmware package for a quick guide to 
use the EFI commands

To Update from Intel(R) Deployment Assistant (IDA)

The Intel(R) Deployment Assistant software is easy to use and is present on the 
"Intel(R) Server Deployment & Management" DVD shipped with the system.
User can download the latest version IDA CD ISO image from http://downloadcenter.intel.com/
To use the IDA CD to update the system firmware:
- Boot server with IDA CD
- Select "Get System Updates" 
- Choose one of the three options 

  . From http://www.intel.com/support/
    Automatically downloads the latest Firmware Update Package from Intel 
    Requires Internet connection
    Enter your local IP address and proxy configuration
    Click "Next" to start the download and update process

  . From my network
    Download the latest Firmware Update Package from http://downloadcenter.intel.com/ and copy 
    it to a Windows* shared folder
    Enter your local IP address, the Windows* file server name, and a
    Windows user name and password
    Select the firmware package in pop-up window
    Click "Next" to start the update process

  . From USB flash drive or Hard Disk
    Download the latest Firmware Update Package from http://downloadcenter.intel.com/ and copy it 
    to a USB flash drive, then insert the USB flash drive into the server USB port
    Click "Browse"
    Select the firmware package in pop-up window
    Click "Next" to start the update process
    
  Note: The Firmware Update Package is in the ZIP file format. Do not unzip 
        before copying to a Windows* shared folder or USB flash drive.

To update from Windows* and Linux* or operating systems using the Intel(R) One Boot
Flash Update Utility (OFU)

Intel(R) One boot Flash Update utility can be downloaded from http://downloadcenter.intel.com/
and it is part of the "BIOS, Firmware Update & Configuration Utilities" for 
Windows* and Linux*. Please refer to Intel OFU user guide about the details of 
installation and usage of OFU.

Use OFU to update system firmware by the following steps:
- Install OFU on Windows* or Linux* system
- Download the latest firmware update package from http://downloadcenter.intel.com/
- Unzip package to a folder
- Run the following command in Windows* command line/Linux* terminal window:
  <OFU install folder name>:\flashupdt -u  <package folder name>\flashupdt.cfg
                       
To update from Windows* Preboot Execution Environment (WinPE)

The System Firmware Update Package can be inserted to Windows* PE customized image 
for creating a bootable Windows* PE CD. User is able to update system firmware from 
customized WinPE CD by the following steps:
- Boot server with customized WinPE CD
- Run script "WinPE21_x64_Update.bat" or "WinPE20_x86_Update.bat" 
  (name may be varied depends on your own customization)
  
Note:
1. The Intel(R) OFU utility is case sensitive. Therefore, when you transfer the 
Firmware Update Package using USB flash drive from a Microsoft Windows* system to a Linux
environment, you must first extract under the Linux* environment. Otherwise, you 
will need to mount the USB flash drive manually with 'vfat' option under Linux to avoid 
conversion from upper case to lower case and vice versa.

2. To make Intel(R) OFU utility run properly under x86 or x64 OS, you have to read
OFU release notes on known issues for OFU installation.

3. In this SFUP package, Intel only provide batch file "WinPE_x86_Update.bat"
for WinPE2.0 32 bit solution "WinPE_x64_Update.bat" for WinPE2.1/3.0 64 bit 
solution as an example. Please refer to white paper "White Paper-Intel Server 
Utilities Procedure for WinPE.pdf" for details on building your own customized 
WinPE CD.

4. Windows PE 2.0 - built from Windows Vista SP1 32bit or EM64T
5. Windows PE 2.1 - built from Windows Vista SP1 or Windows Server 2008, EM64T
6. Windows PE 3.1 - built from Windows Server 2008R2, EM64T
7. Microsoft IPMI driver is loaded by default from WinPE CD, if you want to use 
Intel IPMI driver instead of MS IPMI driver for firmware update, you can un-install
Microsoft IPMI driver by:
                Devicesetup.exe ¨Cv remove *IPI0001
                Note: IPI0001 is the device ID for Microsoft IPMI driver.

================================================================================
                   BIOS changes in release 01.03.0002
================================================================================
- Fixed: NIC Information can not be saved in the Sysinfo log file and it cannot be 
	 retrieved or set using the syscfg utility. 
- Fixed: If Remotely redirecting an ISO image from a client and the target system 
	 is restarted, the target system will automatically boot to the redirected 
	 ISO image and start an OS installation.

================================================================================
                   ME Changes in release 02.01.05.107
================================================================================
- Fixed: FW may hang in initialization state after the update of entire ME
         region is interrupted by AC loss. 
         - None of the available ME resets (AC cycle or Global Reset or Power
           Button Override) can get ME out of the error condition, only
           reflashing ME image. 
- Fixed: FW may become unresponsive after switching from Recovery to
         Operational (e.g. during Direct Update).
         - Global Reset or Power Button Override can’t get ME out of the error
           condition. 

================================================================================
                   BMC Changes in release 01.10.3656
================================================================================
- Fixed: NPD I2C fails to respond after NACK no hold time case.
- Fixed: Updated FRUSDR files.
         - S2400BB to version 0.09
         - S2600CP to version 1.06
         - S2600CO to version 1.07
         - W2600CR to version 1.07
         - S2400EP to version 1.00
         - S2600IP to version 1.07
         - S2600JF to version 1.07
         - S2400LP to version 1.06
         - S2600CP to version 1.07
         - S2600CO to version 1.08
         - W2600CR/S2600IP to version 1.08
         - S2400GP to version 1.05
         - S1600JP to version 0.05
         - S2600JF to version 1.08 
         - S4600LH to version 0.12
         - S2600WP to version 1.05
         - S2600GZ/S2600GL to version 1.03
- Fixed: Adjust RGMII Tx clock delay to -250ps for S1400SP according to SI
         requirement
- Fixed: Command OEM Get Reading. will now return units-based value converted
         by using .y=Mx+B
- Fixed: Fixes to LCD Code defects identified in code review were incorporated
- Fixed: Some strings on LCD were formerly displayed improperly on LCD
- Fixed: Increased total SDR record length to 0x48h from 0x40h to accommodate
         the S4600LH SDR requirements
- Fixed: S1600JP: Corrects the baseboard temperature sensor mapping so that it
         works
- Fixed: After forcing a CATERR on S4600LH, the debug information from Embedded
         Web Server lacks some information
- Fixed: LAN channel cannot get DHCP IPv4 address after disabling VLAN on it
- Fixed: NMI sensor event isn't logged after issuing "chassis control" command
         to trigger NMI
- Fixed: SUT hang at POSTCODE: 0x63 while BMC LAN connected to a switch loop
         environment
         - BMC would freeze under heavy network traffic loads (e.g. broadcast
           storm)
- Fixed: S4600LH: Fan speed reading not correct
         - Added other chassis support in S4600LH and corrected RPM calc
         - Also updated S1400FP/S1400SP SDR to reflect change.
- Fixed: Network Interface hold time was out of spec for S2600GZ/S2600GL and
         S2400BB
- Fixed: Issuing incorrect "Set CR Configuration" command returns wrong error
         code
- Fixed: LCP error messages are not scrolling automatically without pressing
         LEFT and RIGHT keys
- Fixed: LCP default banner text when server with normal health is displaying
         some junk characters at the end
- Fixed: Number of characters displaying in LCP display is only 16 but it
         should be 18 characters
- Fixed: LCP displays "No BIOS POST C" when enter into LPC under VIEW menu
- Fixed: Unable to view the entire IP or Gateway or Subnet addresses using LCP
         display, last digit is missing during display.
- Fixed: Firmware information contents in LCP displaying does not match the
         actual version
- Fixed: Banner text is not reflecting correct information after selecting SM,
         LPC, or POW as a banner
- Fixed: LCP default screen after power on is not the correct banner text
- Fixed: S2400SC shows no socket present in CPU information page of Embedded
         Web Server
         - SMBIOS rev 2.7.1 added additional socket types. This change adds
           those types to the SMBIOS translation tables.
- Fixed: Updated S4600LH SDR to resolve issues where fans specified in FCT
         SDRs couldn't be controlled with fan domains.
- Fixed: BMC 1.08 S4600LH SDR was missing Sensor 0x2C (Riser 2 Left Forward
         Temperature)
- Fixed: Exit Air Temp reading mismatch when using IPMI command under Linux
         - The sensor initialization code was checking both assertion and 
           deassertion enables and settable/readable thresholds before actually
           setting the thresholds. This was causing the Exit Air Temp sensor to
           fail to set thresholds (all thresholds became 0)
- Fixed: Host name is not included in Email Alert subject line
         - Subject line could potentially be set before host name was set. This
           change sets the subject line again after the host name is changed
- Fixed: BMC FW must satisfy open source advertising clause for OpenSSL
         - Added "About" button to top bar to satisfy item 6 in the OpenSSL
           license.
- Added: Changed SDR of S2600CP, S2600CO, W2600CR/S2600IP, and S2400GP to add
         Dynamic Power Unit Redundancy Sensors
- Added: Add S1600JP and S2600WP PCIeSlotMap Table
- Added: Adds option (0xfe) for SlotIPMB command to ignore mux completely

================================================================================
                   FRUSDR Changes in release 1.08
================================================================================    
- None

=============================================================================
                            LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products. 
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation may 
have patents or pending patent applications, trademarks, copyrights, or other 
intellectual property rights that relate to the presented subject matter.  
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any 
such patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product 
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 
*Other names and brands are the property of their respective owners.
Copyright (c) 2012 Intel Corporation.

A portion of this firmware is open source code, which falls under the
GPL 2.0 license.  

[END OF RELEASE NOTES]
