================================================================================
Intel(R) Server Board S2600WP Family
Intel(R) Server System H2000WP Family Firmware Update Package
for Intel(R) Deployment Assistant, Intel(R) One Boot Flash Update Utility, 
The embedded EFI Shell, Windows* Preboot Execution Environment 
================================================================================
Intel Enterprise Platform & Services Division - Marketing
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================
DATE    : Jun 29, 2012
TO      : Intel(R) Server Board S2600WP Family
	  Intel(R) Server System H2000WP Family customers
SUBJECT : Release Notes for System Firmware Update Package 
================================================================================
                              ABOUT THIS RELEASE
================================================================================
BIOS   : 01.03.0002
ME     : 02.01.05.107
BMC    : 01.10.3656
FRUSDR : 1.05
================================================================================
                           Support Platforms and Dependency
================================================================================
Processors supported: 
Intel(R) Xeon processor E5-2600 series

Microcode update versions:
Intel(R) Xeon processor E5-2600 series C0 stepping: 0x80000513 CPUID = 0x206D5
Intel(R) Xeon processor E5-2600 series C1 stepping: 0x80000615 CPUID = 0x206D6
Intel(R) Xeon processor E5-2600 series C2 stepping: 0x8000070A CPUID = 0x206D7


On-Board Component Option ROM Versions:
Integrated BMC Matrox VGA           : VBE BIOS V3.8SQ
1G PXE Option ROM                   : Intel(R) Boot Agent GE v1.3.81
10G PXE Option ROM                  : Intel(R) Boot Agent XE v2.1.96
iSCSI Option ROM                    : Intel(R) iSCSI Remote Boot version 2.7.97
FCoE Option ROM                     : Intel(R) 10G FCoE OpROM v1.7.07
SAS RAID Option ROM - RSTe for C0   : v3.0.1.2101
SAS RAID Option ROM - RSTe for B0   : v3.0.1.2101
SATA RAID Option ROM - RSTe         : v3.0.1.2101
SATA RSTe EFI driver Version        : v3.0.1.2101
SAS RSTe EFI driver Version         : v3.0.1.2101
SATA ESRTII RAID Option ROM - AHCI  : AHCI.01061105I
SAS ESRTII RAID Option ROM - SCU    : SCU.01060930I
ACM				    : v1.0PV
Intel(R) QPI Reference Code Version : 01.00.00.06
Memory Reference Code Version       : 01.00.00.06

Management Engine Firmware Version  : 02.01.05.107


  

The following update process must be followed to ensure a trouble free update.
1.	BMC firmware to 1.04 or later
2.	BIOS 1.02 or later
3.	Manageability Engine (ME) firmware 02.01.05.69 or later
4.	Latest FRU/SDR package specific to the H2000WP/S2600WP.

================================================================================
                  System Firmware Update Package Usage instructions                   
================================================================================
This package can be updated using one of the following methods:
 - The embedded UEFI shell
 - Intel(R) Deployment Assistant
 - Windows* or Linux* operating system using Intel(R) One-boot Flash Update (OFU)
   V11.0 Build 9 or later)
 - Windows* Preboot Execution Environment (WinPE)

To Update from the embedded EFI Shell

update system firmware from Intel server EFI shell by the following steps:
- Download Intel server system firmware update package from support.intel.com
- Unzip package and copy all files to root folder in USB disk on key 
- Insert USB disk on key to server USB port
- Reboot server, system will start BIOS/BMC/FRUSDR update automatically

  If case for some reason or you didn't put unzipped package under root folder of USB key, 
  you can do it by:
- Reboot server to EFI shell manually
- Run command "map -r" in EFI shell to mount USB disk on key
- Run command "fs0:" to change folder to USB disk on key, USB key may also mount to
  fs1:. The number of "fs" is dependent on the result of command "map -r"
- Change folder to the folder storing the firmware package
- Run command "startup.nsh" to start firmware update process

Please refer to "EFI_Instructions.pdf" in this firmware package for a quick guide to 
use the EFI commands

To Update from Intel(R) Deployment Assistant (IDA)

The Intel(R) Deployment Assistant software is easy to use and is present on the 
"Intel(R) Server Deployment toolkit" CD shipped with the system.
User can download the latest version IDA CD ISO image from support.intel.com
To use the IDA CD to update the system firmware:
- Boot server with IDA CD
- Select "Get System Updates" 
- Choose one of the three options 

  . From support.intel.com
    Automatically downloads the latest Firmware Update Package from Intel 
    It requires Internet connection
    Enter your local IP address and proxy configuration
    Click "Next" to start the download and update process

  . From my network
    Download the latest Firmware Update Package from support.intel.com and copy 
    it to a Windows* shared folder
    Enter your local IP address, the Windows* file server name, and a
    Windows user name and password
    Select the firmware package in pop-up window
    Click "Next" to start the update process

  . From USB Disk on Key or Hard Disk
    Download the latest Firmware Update Package from support.intel.com and copy it 
    to a USB key, then insert the key into the server USB port
    Click "Browse"
    Select the firmware package in pop-up window
    Click "Next" to start the update process
    
  Note: The Firmware Update Package is in the ZIP file format. Do not unzip 
        before copying to a Windows* shared folder or USB disk.

To update from Windows* and Linux* or operating systems using the Intel(R) One Boot
Flash Update Utility (OFU)

Intel(R) One boot Flash Update utility can be downloaded from support.intel.com
and it is part of the "BIOS, Firmware Update & Configuration Utilities" for 
Windows* and Linux*. Please refer to Intel OFU user guide about the details of 
installation and usage of OFU.

Use OFU to update system firmware by the following steps:
- Install OFU on Windows* or Linux* system
- Download the latest firmware update package from support.intel.com
- Unzip package to a folder
- Run the following command in Windows* command line/Linux* terminal window:
  <OFU install folder name>:\flashupdt -u  <package folder name>\flashupdt.cfg
                       
To update from Windows* Preboot Execution Environment (WinPE)

The System Firmware Update Package can be inserted to Windows* PE customized image 
for creating a bootable Windows* PE CD. User is able to update system firmware from 
customized WinPE CD by the following steps:
- Boot server with customized WinPE CD
- Run script "WinPE21_x64_Update.bat" or "WinPE20_x86_Update.bat" 
  (name may be varied depends on your own customization)
  
Note:
1. The Intel(R) OFU utility is case sensitive. Therefore, when you transfer the 
Firmware Update Package using USB key from a Microsoft Windows* system to a Linux
environment, you must first extract under the Linux* environment. Otherwise, you 
will need to mount the USB key manually with 'vfat' option under Linux to avoid 
conversion from upper case to lower case and vice versa.

2. To make Intel(R) OFU utility run properly under x86 or x64 OS, you have to read
OFU releaenotes on known issues for OFU installation.

3. In this SFUP package, Intel only provide batch file "WinPE_x86_Update.bat"
for WinPE2.0 32 bit solution "WinPE_x64_Update.bat" for WinPE2.1/3.0 64 bit 
solution as an example. Please refer to white paper "White Paper-Intel Server 
Utilities Procedure for WinPE.pdf" for details on building your own customized 
WinPE CD.

4. Windows PE 2.0 - built from Windows Vista SP1 32bit or EM64T
5. Windows PE 2.1 - built from Windows Vista SP1 or Windows Server 2008, EM64T
6. Windows PE 3.1 - built from Windows Server 2008R2, EM64T
7. Microsoft IPMI driver is loaded by default from WinPE CD, if you want to use 
Intel IPMI driver instead of MS IPMI driver for firmware update, you can un-install
Microsoft IPMI driver by:
                Devicesetup.exe ¨Cv remove *IPI0001
                Note: IPI0001 is the device ID for Microsoft IPMI driver.





================================================================================   
 				BIOS 01.03.0002
=================================================================================  
- Fixed: NIC Information can not be saved in the Sysinfo log file and it cannot be 
	 retrieved or set using the syscfg utility. 
- Fixed: If Remotely redirecting an ISO image from a client and the target system is restarted, 
	 the target system will automatically boot to the redirected ISO image and start an OS installation.

================================================================================   
 				BIOS 01.03.0001
================================================================================= 
- Fixed: On GUID based partitions any SMI call freezes system.
- Fixed: When the baseboard LAN IPV6 is enabled in BIOS setup, the RMM4 configuration is greyed out.
- Fixed: Unable to disable onboard NIC ports in BIOS setup.
- Fixed: C1E is disabled when both C3 and C6 processor Cstates are disabled in BIOS setup.
- Fixed: In BIOS setup, Serial B is incorrectly set to disabled by default and cannot be enabled.
- Fixed: TPM Admin Control option should be disabled (grayed out) when the BIOS admin password is not set.

================================================================================   
 				BIOS 01.02.0010
=================================================================================  
- Fixed: Onboard NIC2 MAC address can not be shown correctly and it can't boot to PXE from NIC2 on
         Intel(R) Server Board S2400EP. 

================================================================================   
 				BIOS 01.02.0009
=================================================================================  
- Fixed: Update add-in video output policy

================================================================================   
 				BIOS 01.02.0008
=================================================================================  
- Fixed: PCIe slot 5 max link width can only be detectes as x4 on Intel(R) Server Board S1400FP.
- Fixed: EFI network stack incorrectly uses Mezzenine NIC port.
- Fixed: FRB2 timer will reset the system after 6 minutes when entering BIOS Setup via the <F6> boot menu.
- Fixed: System cannot enter EUP Lot6 deep sleep mode.
- Fixed: PCIe link speed changes occur without logging a SEL event.
- Fixed: During POST, populeated PCIe slots numbers are incorrectly identified.
- Fixed: Cannot change Serial Port A to IRQ3 on Intel(R) Server Board S2600JF.
- Fixed: NIC1 and NIC2 cannot be disabled on Intel(R) Server Board S2400SC.
- Fixed: ACPI errors are reported in dmesg.log in SUSE* Linux* 11 SP2 RC x64.

================================================================================ 
 				BIOS 01.02.0007
=================================================================================
- Fixed: W2600CR Windows* 7 WHQL cert Failure - Single computer Display object Test Failure

================================================================================ 
 				BIOS 01.02.0006
=================================================================================
Others:
- Update ME version to 02.01.05.091
=================================================================================     
 				BIOS 01.02.0004                                     
=================================================================================
- Fixed:  S4 resume function is not stable on S2400BB.
- Fixed:  Correct some products' onboard slot numbers shown in Windows device manage
- Fixed:  Some NIC IO Modules cann't be displayed in the NIC Configuration page of BIOS Setup.
- Fixed:  Added specific blades items for S2600KI
- Fixed:  Workstation System cannot enter S3 state in UEFI Windows* 7.
- Fixed:  Onboard NIC device still can be detected in OS after disabled in BIOS
- Fixed:  MAC addresses are not shown in BIOS setup on S2400EP Dual port SKU.
- Fixed:  Some BIOS setup pages have incorrect strings and use incorrect format
- Fixed:  ME interface fails sometime after S3 resume back on S2600CP
- Fixed:  SMBIOS Type 8 of some product has some incorrect information
- Fixed:  Intel(R) X520-T2 10G NIC did not work at expected PCI-E link speed
- Fixed:  The HDD Fault LED on HSBP might behave incorrectly under some specific configurations.
- Fixed:  System sometimes can’t detect PCI-x storage card.

Others:
- Update new processor microcode and onboard device option roms

=================================================================================     
 				BIOS 01.02.0003                                      
=================================================================================
- Fixed:  NIC1 and NIC2 cannot be disabled in BIOS setup.
- Fixed:  Legacy VGA on CPU socket one is greyed out when add-in VGA card is associated
          with CPU socket 2.
- Fixed:  Serial over LAN cannot be activated via IPMI with Console Redirection enabled
          in BIOS setup. 
- Fixed:  PXE OPRom inoperative.
- Fixed:  ISCSI option missing on some platforms. 
- Fixed:  Implementation of "Iflash32 -rd" to load defaults on next system reset.
- Fixed:  The DIMM fault LED behaves incorrectly on DIMM_D3 under memory Sparing mode.
- Fixed:  Some Intel(R) NIC IO modules can't be detected under Microsoft* Windows* 2008 SP2.
- Fixed:  The information for Onboard NICs is shown incorrectly in BIOS setup.
- Fixed:  RAID RSTe OpROM fails to launch on AHCI SATA ports in RAID configuration.
- Fixed:  There is no "RMM4 IPv6 Enable/Disable" option in BIOS setup.
- Fixed:  The default value of Lan port PXE will show disabled for Intel(R) NIC I/O module.
- Fixed:  CPU information is shown incorrectly in SMBIOS table if the user populates
          different frequency processors.
- Fixed:  Active Processor Cores cannot be changed in BIOS setup.
- Fixed:  Turbo boost will be disabled when choosing the balanced performance policy in
          BIOS setup.
- Fixed:  Unexpected SEL entries logged after BIOS update.

=================================================================================     
 				BIOS 01.01.1002                                      
================================================================================= 
- First production release BIOS.
================================================================================
			 ME Issues fixed in 02.01.05.107 release
================================================================================
- Fixed: FW may hang in initialization state after the update of entire ME
         region is interrupted by AC loss. 
         - None of the available ME resets (AC cycle or Global Reset or Power
           Button Override) can get ME out of the error condition, only
           reflashing ME image. 
- Fixed: FW may become unresponsive after switching from Recovery to
         Operational (e.g. during Direct Update).
         - Global Reset or Power Button Override can’t get ME out of the error
           condition. 

================================================================================
			02.01.05.091
================================================================================
- Fixed: Fix for Double AC cycle for recognizing OPROM changes

================================================================================
                   ME Changes in release 02.01.05.069
================================================================================

- Fixed: ME FW Health Event with Event Data 2 = 0 (Recovery GPIO forced) will
         be generated after IPMI command "Force ME Recovery" issuing.
- Fixed: ME FW unexpectedly resets when SMLink clock held low for a long period
         of time
- Fixed: Sometimes system stops responding after Power Cycle.

===============================================================================
			02.01.05.064
===============================================================================
- First production release of ME



===============================================================================
                               BMC changes in release  01.10.3656
===============================================================================
-Fixed: NPD board I2C fails to respond after NACK no hold time case.


===============================================================================
                                01.10.3560
===============================================================================
- Fixed: Updated FRUSDR files.
         - S2400BB to version 0.09
         - S2600CP to version 1.06
         - S2600CO to version 1.07
         - W2600CR to version 1.07
         - S2400EP to version 1.00
         - S2600IP to version 1.07
         - S2600JF to version 1.07
         - S2400LP to version 1.06
         - S2600CP to version 1.07
         - S2600CO to version 1.08
         - W2600CR/S2600IP to version 1.08
         - S2400GP to version 1.05
         - S1600JP to version 0.05
         - S2600JF to version 1.08 
         - S4600LH to version 0.12
         - S2600WP to version 1.05
         - S2600GZ/S2600GL to version 1.03
- Fixed: Adjust RGMII Tx clock delay to -250ps for S1400SP according to SI
         requirement
- Fixed: Command OEM Get Reading. will now return units-based value converted
         by using .y=Mx+B
- Fixed: Fixes to LCD Code defects identified in code review were incorporated
- Fixed: Some strings on LCD were formerly displayed improperly on LCD
- Fixed: Increased total SDR record length to 0x48h from 0x40h to accommodate
         the S4600LH SDR requirements
- Fixed: S1600JP: Corrects the baseboard temperature sensor mapping so that it
         works
- Fixed: After forcing a CATERR on S4600LH, the debug information from Embedded
         Web Server lacks some information
- Fixed: LAN channel cannot get DHCP IPv4 address after disabling VLAN on it
- Fixed: NMI sensor event isn't logged after issuing "chassis control" command
         to trigger NMI
- Fixed: SUT hang at POSTCODE: 0x63 while BMC LAN connected to a switch loop
         environment
         - BMC would freeze under heavy network traffic loads (e.g. broadcast
           storm)
- Fixed: S4600LH: Fan speed reading not correct
         - Added other chassis support in S4600LH and corrected RPM calc
         - Also updated S1400FP/S1400SP SDR to reflect change.
- Fixed: Network Interface hold time was out of spec for S2600GZ/S2600GL and
         S2400BB
- Fixed: Issuing incorrect "Set CR Configuration" command returns wrong error
         code
- Fixed: LCP error messages are not scrolling automatically without pressing
         LEFT and RIGHT keys
- Fixed: LCP default banner text when server with normal health is displaying
         some junk characters at the end
- Fixed: Number of characters displaying in LCP display is only 16 but it
         should be 18 characters
- Fixed: LCP displays "No BIOS POST C" when enter into LPC under VIEW menu
- Fixed: Unable to view the entire IP or Gateway or Subnet addresses using LCP
         display, last digit is missing during display.
- Fixed: Firmware information contents in LCP displaying does not match the
         actual version
- Fixed: Banner text is not reflecting correct information after selecting SM,
         LPC, or POW as a banner
- Fixed: LCP default screen after power on is not the correct banner text
- Fixed: S2400SC shows no socket present in CPU information page of Embedded
         Web Server
         - SMBIOS rev 2.7.1 added additional socket types. This change adds
           those types to the SMBIOS translation tables.
- Fixed: Updated S4600LH SDR to resolve issues where fans specified in FCT
         SDRs couldn't be controlled with fan domains.
- Fixed: BMC 1.08 S4600LH SDR was missing Sensor 0x2C (Riser 2 Left Forward
         Temperature)
- Fixed: Exit Air Temp reading mismatch when using IPMI command under Linux
         - The sensor initialization code was checking both assertion and 
           deassertion enables and settable/readable thresholds before actually
           setting the thresholds. This was causing the Exit Air Temp sensor to
           fail to set thresholds (all thresholds became 0)
- Fixed: Host name is not included in Email Alert subject line
         - Subject line could potentially be set before host name was set. This
           change sets the subject line again after the host name is changed
- Fixed: BMC FW must satisfy open source advertising clause for OpenSSL
         - Added "About" button to top bar to satisfy item 6 in the OpenSSL
           license.
- Added: Changed SDR of S2600CP, S2600CO, W2600CR/S2600IP, and S2400GP to add
         Dynamic Power Unit Redundancy Sensors
- Added: Add S1600JP and S2600WP PCIeSlotMap Table
- Added: Adds option (0xfe) for SlotIPMB command to ignore mux completely

===============================================================================
                                01.09.3404
===============================================================================
- Fixed: Update FRUSDR packages to following versions:
         - S1600JP: S1600JP_FRUSDR_0.03
         - S1400SP: S1400SP_FRUSDR_01
         - S2400LP: S2400LP_FRUSDR_0105
         - S2400SC: S2400SC_FRUSDR_0104
         - S2400BB: S2400BB_FRUSDR_08
         - S2400EP: S2400EP_FRUSDR_03
         - S2600WP: S2600WP_FRUSDR_1.03
         - S1600JP: S1600JP_FRUSDR_0.04
         - S4600LH: S4600LH_FRUSDR_11
- Note: Testing with BIOS/2050_Package.zip (2.05 BIOS) with ME 02.01.05.091
        UBoot increments to 1.11 in this release due to changes in LCD
        handling
- Fixed: S2400EP: Add one additional 250ps delay for Tx clock and MAC0 drive
         strength to improve Signal Integrity on S2400EP
- Fixed: Fixed a case that had been missed for LDAP login to EWS.
- Fixed: uboot not updated after BMC FW updated when BMC executing from uboot
- Fixed: Wrong DIMM location is displayed in Embedded Web Server when a
         non-working DIMM is populated
- Fixed: Fixes to LCD module to address occcasional failures in Fan Speed
         Control tests.
- Fixed: LED control and status changes for S1400FP and S1400SP.
- Fixed: Updated the text output of ews-oem-tools to match documentation
- Fixed: Channel 1 or channel 2 LAN cannot ping through with IPV6 address when
         the LAN cables are both installed.
- Fixed: Corrected typoes in Embedded Web Server online help page.
- Fixed: S2400LP: After successful issue command to load BMC configuration
         default, "shutdown policy" option is not set to "disabled" which is
         the default
- Fixed: LCD SN [Server Name] displays different values at VIEW menu and SN as
         a banner
- Fixed: S2400BB: System Fans are constantly boosting and all sensors = OK

===============================================================================
                                01.08.3329
===============================================================================
- Fixed: Updated S1600JP SDR to 0.03
- Fixed: Updated S1400SP GPIO table to improve Fan Tach reading.
- Fixed: BMC was sending PMBus command to non-supported CR feature PSU.
- Fixed: Update S4600LH SDR and associated zip to sync with latest FSC sheet
         Rev0.5,Version (v6)
- Fixed: Removing 1600 W S2 PSU FW image from the BMC.
- Fixed: S4600LH: Added debug to identify cause of system resets after CATERR.
- Fixed: IPv6 not working when 2 NCSI channels enabled or Failover is enabled:
- Fixed: There is an error message on Virtual Front Panel page when logging
         into the Embedded Web Server with user privilege.
- Fixed: Virtual Front Panel power LED always solid green when system is in s1
         state.
- Fixed: Event description different when viewed in Embedded Web Console vs.
         when saved via EWC.
         - Added decode of OEM event type 0x70, sensor type 0x2B events.
- Fixed: Embedded Web Server user disappears when  privilege is set to 5 using
         ipmitool.
- Fixed: BMC unresponsive when added all the users and then deleted all the
         users from Embedded Web Server
- Added: Added S1600JP to initial platform list
- Added: Add zlib license info to OEM Embedded Web Services documentation.
- Added: OEM Command to enable/disable BMC Services. This implements a command
         to enable/disable BMC Services and another to get current state.
         Currently controls sshd (SMASH), Web Console, and rKVM.

===============================================================================
                                01.07.3244
===============================================================================
** NOTE: THERE IS A CHANGE TO THE PASSWORD SYSTEM USED BY SSH AND SMASH.
         - As a result SMASH users may be informed of a possible security
           attack, by the utility, when they first log in after updating.
           This is not an attack, it is an update which will take place once.

- Fixed: Updated S1400SP SDR, update SAS module presence sensor number to 0x2d
- Fixed: S2400BB - Default and FCT version 0.07 SDR files provided.
- Fixed: Update FRUSDR package (and defaults) for S4600LH to revision 08
- Fixed: Updated SDRs for S4600LH platform:
         - Modified and added SDR
         - Modified HSBP temp SDR threshold values
         - Corrected problem with S4600LH FRUSDR with Other chassis options
           that was causing system fan issues.
         - Some of the sensor numbers used were the same as other platforms,
           resulting in some erroneous displays of processor fan info. The
           Sensor numbers have been changed to avoid conflict
- Fixed: Adding S1400FP SDR. Updates S1400FP and S1400SP DIMM offsets in the
         web display, and also adds information on S1400FP Fan Fault LED.
- Fixed: BMC sshd password set to invalid by default
- Fixed: Additional support for SSL - spec requires that user can upload both
         certificate and private key, now supported
- Fixed: Update U-boot version to 1.8
- Fixed: BMC boot up had a window where BMC HW watchdog was not enabled.
         - Changed to 4 minutes so that if BMC fails to start, the hardware
           watchdog will trigger.
- Fixed: When the BMC reboots with an active SOL session, the SOL mux was not
         automatically reset to redirect serial data out the system serial
         port. This prevented both SOL and system serial from working. Now
         resets SOL mux at BMC boot to prevent this situation.
- Fixed: The PET Acknowledge command was requiring an open IPMI session. As per
         IPMI spec, this command will be sessionless and belongs to same class
         as Get Channel Authentication capabilities.
- Fixed: Enter Firmware Transfer Mode will generated a unexpected log about FW
         update status
- Fixed: When Exit FW transfer happens after the download of the image (i.e
         aborted before programming), the update failure sel event was not
         logged
- Fixed: HSBP unresponsive after FW update.
- Fixed: HSBP FRU information was sometimes unreadable via IPMITOOL.
- Fixed: Combined both debug files into a single zip. Passwords on individual
         files are unchanged. Container zip has no password. Modified system
         debug commands to only accept log type 0x00 as a parameter, since
         there is now only one file generated.
- Fixed: BMC disk drive numbering scheme does not match LSI tools (RWC2 and
         webBIOS) numbering scheme and marketing’s documentation
         - The BMC was using 1 based drive numbers, while documentation
           specified 0 based numbers. This change implements the changes for
           S2600GZ/S2600GL SDR as well as internaming conventions for the
           sensor numbers.
- Fixed: HSBP Drive Slot Sensors report drive removal and insertion on every
         warm reboot
- Fixed: GRUB serial terminal causes BMC distress
- Fixed: Get DIMM Offset command was rejecting any DIMM number greater than 48
         with completion code 0xCC.
- Added: "Get drive fault LED status" and "Set drive fault LED status" IPMI
         commands
- Added: All files required to support the add-in LCD hardware on S2600CP,
         S2600GL, and S2600GZ have been added.  User can now plug in module and
         traverse the LCD menus by pressing the buttons provided on the LCD
         hardware module.

===============================================================================
                                01.06.3156 & 00.36.3156
===============================================================================
Note: The update package provided for this release was validated with BIOS
release x045.
- Fixed: Patch fixes a problem with excessive Power Supply SEL events for 1200W
         power supplies.
- Fixed: Update cipher suite LAN parameters to be consistent with IPMI spec
- Fixed: Update S2400LP SDR for factory build, FAN4a~6b was added
- Fixed: Changed Node Manager SEL entry descriptions.
- Fixed: Update for S2400LP to solve the FAN5a~6b reading zero issue reported
         by the factory.
- Fixed: Update S2400EP Default SDR
- Fixed: Add more thorough checking to Embedded Web Server action image
         validation
- Fixed: Update SDR on slave node, PSU temp sensors will be in Disabled status,
         while other PSU sensors are correct
- Fixed: A failed node can't be power-offed gracefully by BMC when there is a
         simulated critical event of a temp sensor and stopped ystem fan.
- Fixed: "Shutdown Policy" available after BIOS update
         - BMC returned the wrong completion code of 'get shutdown policy'
           command on non-halfwidth platform.
- Fixed: Allow OEM Embedded Web Server image to be completely removed to
         factory settings
- Fixed: SNMP alert and Email alert can't be received when node manager power
         policy defined threshold is exceededon S2400EP
- Fixed: The status LED will be solid amber for a while after an AC cycle on
         S2400EP, S1400FP, and S1400SP.
- Fixed: S2400LP DIMM event SEL does not match with the location in the board.
- Fixed: Sometimes the minimum power reading is 0W on the power statistics page
         - Fixed for all platforms.
- Fixed: Unexpected results with PS fault condition(FP Status LED, BMC Sensors)
- Fixed: Slow Fan Limit event verification failed on 1200W PSU
         - Failed Power Supply status was not being maintained. Will not clear
           the PS Fault status until the Power Good is negated.
- Fixed: Read platform debug command after exitng the debug log file transfer
         mode, the response is failed
- Fixed: BMC may hold IPMB CLK low after BMC reset if the BMC is addressed over
         IPMB and the BMC resets before that I2C transaction completes.
- Fixed: BB +1.1V STBY low critical log during DC off
         - The 1.1V Stby voltage sensor was generating events when the power
           button was held in over 4 sec.
- Fixed: Emulex* Pilot III P02 Chip - Prefetchable bit (BAR10-BIT3) is not set
         for memory range.
- Fixed: S4600LH: Add Memory Trip support for CPU 3 and CPU 4
- Fixed: S4600LH: Updated SDR version to 08.
- Fixed: S4600LH: Fixed the System Fans reading.
- Fixed: Incorporated generally released Linux driver fixes for bonding-related
         bugs, glitches, etc.
- Fixed: The cramfs tools used in Embedded Web Server image were licensed as
         GPL, these have been rewritten. In more paranoia was added in image
         creation, throwing errors if anything but regular files are in the
         source directory.  This prevents symlink and device node attacks.
         Also added is code to allow for building .deb, .rpm and .msi install
         packages. Currently the windows installer only does 32-bit, but the
         linux packages are available in both 32- and 64-bit varieties.
         Some of these changes are outlined in the updated user document that
         gets distributed with the binary.
- Fixed: Corrects a reaction to bad OEM records in SDR. Previously, this would
         report an error and reset the entire SDR with default values. This is
         not required, and the delete step will no longer happen.
- Fixed: Modified uboot handling of Enter FW Transfer Mode command to return
         completion code 0x80 (already in FW transfer mode) if the Enter FW
         Transfer Mode command has been sent previously.
- Fixed: 1200W power supplies were generating spurious Fan Failure events.
- Fixed: HSBP FW crash during firmware image updates.
- Fixed: PS temperature cannot be read after power cycling over night.
- Fixed: BMC boot up has a window where BMC HW watchdog is not enabled
         -BMC HW WDT was defaulted to trigger after 18 hours. This default
          timeout has been changed to 4 minutes.
- Added: Add a software-only method to replace public key and API to query key
         info

===============================================================================
                                01.05.2974
===============================================================================
Note: The update package provided for this release was validated with BIOS
      release x045.
- Fixed: Update default SDR of S2600CO to version 1.04.
         Update default SDR of W2600CR/S2600IP to version 1.03.
         Update default SDR of S2400BB to version 0.06.
- Fixed: Updates PSU FW for 460W CRPS PSU to DPS-460KB A S3 3.09.29
         - This version contains a fix to set the SMBALERT interval to 30
           seconds.
- Fixed: Insert two DIMMs on channel A1 and A2, and inject an ECC error at A1,
         the event log will record correctable ECC at B1.
         - S2400GP: The channel number for DIMMS on channel A1 and A2 were
           being recorded incorrectly as being channel B1 when correctable ECC
           errors were injected.
- Fixed: Sometimes the minimum power reading is 0W on the Embedded Web Server
         power statistics page.
         - For S2400SC ME must receive a Reset NM Statistics command upon
           entering ACPI state S0 to get an accurate minimum power reading.
- Fixed: The Hex data of the sel event retrieved by Intel(R) Hybrid Cloud (IHC)
         is different from those in selviewer.
- Fixed: Execute Get DIMM info command to check Empty slot response "0x03"
         - Per EPS an empty DIMM slot should return 0x83 but was returning 0x03
- Fixed: Perform Action Button is disabled when Graceful OS shutdown option is
         used in Embedded Web Server
         - The Graceful OS Shutdown action caused the "Perform Action" button
           in the Embedded Web Server to be disabled during the process,
           however it wasn't re-enabled until the user reloaded the page.
           This change disables the button after any action, and re-enables the
           button after any power-control action completes.
- Fixed: Embedded Web Server Remote Control Page - Message is not consistent
         across all pages for a User with USER privilege.
         - Embedded Web Server Remote Control Page: Remote KVM is not available
           except to users with ADMIN or better privileges. The informational
           message was not consistent across all pages for a User connected
           with USER privilege. Logging into the EWS with a non-admin user, and
           attempting to open an Remote KVM window, will now redirect to a page
           explaining this. The help page has also been updated with this
           information.
- Fixed: KVM - Help Button - About "Jviewer" copyright statement is wrong.
           - The copyright date presented by JViewer in the Help->About
           interaction should now show copyright 2011 rather than 2005.
- Fixed: Embedded Web Console: Node Manager page hard shutdown does not seem to
         be a hard shutdown.
         - According to the Node Manager documentation, a hard shutdown is used
           but NM actually attempts a graceful shutdown first, only performing
           the hard shutdown if the graceful shutdown stalls for 30 seconds.
           The Embedded Web Server description and help page should correctly
           indicate that this is the expected behavior.
- Fixed: Get Chassis Status command identify LED with wrong status
         - The Get Chassis Status command was not returning the correct
           "Identification LED" status.
- Fixed: Fans stay boosted after BMC force update followed by SDR update
         - Fans should no longer boost after updating the SDR after a forced FW
           update.
- Fixed: Empty or Unconfigured HDD will continuously report faulty or
         assert/deassert
         - Fixes an issue where a system with ESRTII RAID 5, configured with
           three HDDs and a fourth installed but set either unconfigured or
           global-hot-spare, would generate numerous spurious drive fault
           errors to the System Event Log.
- Fixed: Firmware hang if BMC is crashed one time and BMC cold reset is
         executed 3 times after a crash within 30 minutes.
- Fixed: There is a typo error in BMC WebUI help document for "Alert Email"
         sub-menu
- Added: Adds new de-pop PBA (G49054-XXX) for S2600JF. Halfwidth projects will
         auto load de-pop SKU SDR when PBA# of FRU is G49054-XXX.

===============================================================================
                                01.04.2963
===============================================================================
Note that this release is intended to fix a single issue for the S2400SC
platform. It was provided only for that platform.
- Fixed: On S2400SC, sometimes the minimum power reading is 0W on the Embedded
         Web Console power statistics page.

================================================================================
                   BMC Changes in release 1.04.2896
================================================================================

- Fixed: Update to PSU FW for 460W CRPS PSU - contains fix to set the SMBALERT
         interval to 30 seconds.
- Fixed: Empty or Unconfigured HDD will continuously report drive faults
         - There were many spurious drive fault SELs when ESRTII RAID5 was
           configured with 3 disks and 1 hotspare or an unconfigured disk.
           This change, with HSBP FRUSDR package 02, will correct the spurious
           SEL errors.
- Fixed: Firmware stuck if BMC is crashed and then a BMC cold reset is executed
         3 times within the next 30 minutes

===============================================================================
                                01.04.2774
===============================================================================
- Fixed: Fixed issue where during reboot the BMC was not disabling the i2c-4
         channel, resulting in spurious SEL entries from the Management Engine.
- Fixed: New FW drop for the PMAX issue in PSU FW for 750W, 1200W S3/00
         revisions.
- Fixed: Additional FW drop for i2c timeout issue - 2nd timeout happening after
         a i2c reset for 750W, 1200W S3/00F
- Fixed: Fixed issue with bridging commands to ME via BMC IPMI.
- Fixed: Updates SDR for some boards to newest versions:
         - S2600WP IB/De-pop SKU to version 00.08
         - S2600JF IB/De-pop SKU to version 1.03
         - S2600CP to version 1.03
         - S2400GP to version 1.00
- Fixed: VCCQ VR temperature sensors were not working in S2400BB
- Fixed: Duplicated warning event logged about senor unavailable generated
         during ME update
         - Changed the BMC to not count update mode codes against the
           management subsystem health sensor.
- Fixed: Login through SMASH with LDAP authorized user and password failed
         - Enabled the use of LDAP authorization for SMASH logins to BMC. To
           use this there must be an LDAP server (not the BMC) which can
           authorize a user with a given password, and the BMC must be
           configured to allow LDAP with that server, and to map to an allowed
           set of functions.
- Fixed: IPv6 auto-configure mode not working 
- Fixed: Initialized Node Presence pins as Output-High for S2400LP, S2600JF,
         and S2600WP.
- Fixed: IPv6 ping failed after LAN failover enabled
- Fixed: When the Onboard NIC 1 is disabled in BIOS the system fans boost
- Fixed: RMS25CB080 SAS Mod Temp sensor has Unknown Health/Reading
- Fixed: ME events are not interpreted in Embedded Web Server SEL log
- Fixed: S2600JF PSOC HSBP temperature sensor intermittently unavailable during
         node hotplug
- Added: The BMC will now check the most significant bit (bit 7) of the PSU FW
         major revision number. If it is set to 1 then the BMC will refuse to
         downgrade the supply to any earlier revision.
         - Added since power supply stability issues can arise if power
           supplies are updated to an earlier revision of the power supply FW.
           This ONLY applies for this revision of BMC and later.

===============================================================================
                                01.03.2674
===============================================================================
- Fixed: Update SDR of S2600CP to version 1.02.
- Fixed: Update SDR of W2600CR and S2600IP to version to 1.02.
- Fixed: Updated PSU FW for 1200W CRPS (S3 and 00 model) to correct the issue
         in S2600JF system, where system shuts down under certain conditions.
- Fixed: The description of a memory thermal trip event is incorrect.
         - For S2400SC and S2400LP, CPU1/2 DIMM channel 0 is not used. When
           DIMM thermal trip events are found on CPU1 they should show in the
           SEL as "CPU1, DIMMA", and when found on CPU2, as "CPU2, DIMMD"
- Fixed: It is hard to enter BIOS Setup via press F2 in KVM console when using
         LAN2.
- Fixed: An error dialog box pop-up was appearing when accessing the Alerts
         page on platforms that only support a single onboard shared NIC.
- Fixed: The fault reason is "Temperature has crossed critical value" on 
         Virtual Front Panel when SUT was powered off due to processor thermal
         trip.
         - Sensor severity for thermal trip was incorrect. It should now read
           "Thermal fault" on VFP when the system under test powers off due to
           processor thermal trip.
- Fixed: Dump debug file with non-redundant PSU, no information in PEC feature
         support status.
         - When installing a non-redundant PSU, an advisory is now added to the
           system debug log.
- Fixed: Alerts taking 10 seconds after an AC cycle.
- Fixed: On Half Width Form Factor platforms one Node reports raid rebuild that
         happened on another Node, these two Nodes share a HSBP.
- Fixed: Seeing excessive Frame Errors on RMM4 PHY when EEE (energy efficient
         ethernet) function was enabled.
         - When RMM4 PHY EEE (energy efficient ethernet) is enabled, receive
           frame errors increased to an unacceptable level. EEE has been 
           disabled.
- Fixed: Voltage 1.1V Standby monitoring for W2600CR, S2600IP, and S400GP not
         supported while in standby mode.
- Added: Node Auto-Shutdown behavior has been defined for multi-node systems
         (S2600JF, S2400LP, S2600WP). "BMC will turn off designated nodes in
         event of PS failure resulting in PSU not able to supply enough power
         and throttling the node. Based on BIOS setup and slot position of the
         board, BMC will forcefully shut down the node throttling due to PSU
         not supplying enough power."
         - With a properly configured system where nodes have a shutdown
           policy configured in BIOS to permit it, the last two nodes in the
           chassis can be shut down rather than running in a degraded state,
           allowing the remaining node(s) to work at full efficiency to
           complete tasks.

===============================================================================
                                01.02.2608
===============================================================================
- Fixed: This build will be tested with the 041 BIOS release.
- Fixed: Updates to the zip-bundled FRUSDR packages are provided as follows:
         - S2600CP_FRUSDR_100.zip updated to S2600CP_FRUSDR_101.zip
         - S2600CO_FRUSDR_1.00.zip updated to S2600CO_FRUSDR_1.01.zip
         - S2600GZ_FRUSDR_08.zip updated to S2600GZ_FRUSDR_100.zip
         - S2600JF_FRUSDR_1.00.zip updated to S2600JF_FRUSDR_1.01.zip
         - S2400LP_FRUSDR_11.zip updated to S2400LP_FRUSDR_13.zip
         - S2400SC_FRUSDR_23.zip updated to S2400SC_FRUSDR_24.zip
         - S2600WP_FRUSDR_06.zip updated to S2600WP_FRUSDR_07.zip
         - Updated W2600CR and S2600IP SDR version to 1.01
- Fixed: The Chassis Intrusion flag is cleared when a Get Chassis Status
         command is processed.
         - The Get Chassis Status command now reads the state of the sensor
           rather than the value of the flag, when reporting chassis intrusion
           state.
- Fixed: Restores the Cipher Suites and features for RMCP+ which had been
         added then removed.
- Fixed: BMC NVRAM incorrect after DHCP configuration
- Fixed: Reduce RMM4 link speed on some platforms for EMI reductions.
         - On platforms S2600CP, S2600IP, W2600CR, S2600CO, S2400GP, S2400SC,
           and S1400FP, RMM4 Dedicated Management NIC should only connect at
           100MBps.
- Fixed: For S2600JF and S2600WP changed RGMII drive strength to correct EMI
         issues.
- Fixed: There is an error message on Virtual Front Panel page when logging
         into Embedded Web Server with user privilege.
          - When logging in with an account which only has the "user" privilege
            set, the "wait" status should not be displayed for the Virtual
            Front Panel.
- Fixed: The format of memory location error message in Embedded Web Server is
         different from SELviewer.
- Fixed: Update FW under EFI Shell using wrong package will cause a hang at
         "BMC Firmware Update Status".
         - If update fails it should now provide an advisory as expected.
- Fixed: S2400LP systems could experience an "NMI activated-system halted"
         error during system reset.
- Fixed: Embedded Web Server - "LOADING...PLEASE WAIT" is not displayed when
         clicking the refresh link.
         - There was text that was white on a white background. This is
         redundant, as the moving gif is visible, and an accepted form of
         loading indicator. This removes the invisible text.
- Fixed: When BMC is booting the on board Status LED is solid Green, the FP
         Status LED is off.
         - For S2600CO, when BMC is booting, the on board Status LED and FP
           status LED now follow the same blink and color status values as
           other platforms.
- Fixed: Static IPs are still retained when all the LAN 1 & LAN 3 IP set to
         DHCP
- Fixed: Reading more than 106 bytes from ID ROM caused an error if the IPMI
         requests was sent via RMCP
- Fixed: Alerts taking 10s after an AC cycle.
- Fixed: The last two SEL record datas retrieved by iHC are incorrect when the
         SEL is full.
- Fixed: Clear the SEL and issue Get all SEL Entries using wget in Linux, the
         response is incorrect.
- Fixed: Clear the events, there is no Hex version of "the log area has been
         cleared" when reading events using wget.
- Fixed: The last SEL record data retrieved by iHC was missing compared with
         the selviewer tool.
- Fixed: SEL/Power/FWver handlers are not giving error response for iHC
         negative testing.
- Fixed: Channel Access Disabling command not working correctly.
         - Channel Access flag was not checked before sending the PEF entry.
           This was causing some alerts to be lost.
- Fixed: Power Supply Sensors can get disabled on non-master half-width boards
         - Power Supply Sensors on Half Width boards could be disabled and not
           re-enabled.

===============================================================================
                                01.01.2484
===============================================================================
- Fixed: S1600JP Porting code checked in
- Fixed: Added FRU id for external fan controller board detection.
- Fixed: Updated S2400EP Default.sdr and FCT.sdr according to 1.0 sys config
         table
- Fixed: Fixed ID LED issue broken by fix for chassis issue 
- Fixed: HSBP changes: for half-width backplanes, a complex formula decides
         which BMC will act as CMM for the chassis. Added new logic in CMC to
         monitor and grant the PSoC* ownership every 10 seconds. This should
         prevent deadlock issues.
- Fixed: Implemented FWupdate status sensor to log BMC build id (binary) and ME
         build id (bcd) plus decoding logic has been added in Embedded Web
         Server
- Fixed: Modified as per the latest S4600LH SGPIO table 
- Fixed: Updated FCT and Default SDRs as per the S4600LH latest FSC sheet
- Fixed: Updated S4600LH Default.sdr and FCT.sdr according to config table 1.0 
- Fixed: Modified the Bus number for external fan board FRU
- Fixed: Updated S2400SC Default.sdr and FCT.sdr
- Fixed: SDR S2600JF IB/Depop Factory SDRs are updated to V1.01
- Fixed: SDR Update Default/FCT.sdr of S2600CP to version 1.01.
- Fixed: SDR Update Default/FCT.sdr of S2600CO to version 1.01. 
- Fixed: SDR Update Default/FCT.sdr of W2600CR/S2600IP to version 1.01.
- Fixed: SDR Update S2600WP IB/Depop factory SDRs to V0.07
- Fixed: S2600KI BMC specific: SOL - last couple characters not echo'ed back,
         fixed
- Fixed: In Embedded Web Server cannot see the RMM4 LAN alerts setting when
         using IDA to set it.
         - Corrected the alert entry and destination selector configuration
           similar to IDA, so configuration by Embedded Web Server will be
           visible to IDA and vice versa.
- Fixed: W2600CR: IPMITOOL cannot activate SOL session, with console
         redirection enabled via serial port B
- Fixed: W2600CR: DPCCLI cannot be redirected to the serial B output with the
         console redirection enable on serial port B
         - W2600CR board doesn't have COM port COMA, SOL was failing because
           default port was COMA. Now checks for COMB as well.
- Fixed: Debug dump now contains BMC revision number.
- Fixed: Removed almost all BMC centric debug dump from the regular file. Also,
         removed memory info and processes info in the regular debug dump file.
- Fixed: No information about support PEC in debug file.
         - Add information about support PEC in debug file
- Fixed: Send IPMI command to Read Platform Debug Log file has response "C1"
         - Command to Read Platform Debug Log file was returning Normal
           Completion in a circumstance where it should have returned invalid
           command (C1)
- Fixed: Stop the PSU fan, system status LED blink green. after a while, it
         return to solid green, but the PSU FAN still remain stopped
         - Updates to PSU Firmware for 460W and 1200W 00 & S3F power supplies
- Fixed: The VR Watchdog Timeout sensor will auto re-arm within 1 second when
         system power good is deasserted and held deasserted
         - When the VR timeout event was asserted, the VR timeout flag was
           cleared. It resulted in a deassertion in the next sensor scan. Will
           not clear the flag until the VR power good# is asserted
- Fixed: S2400SC: When causing a CPU 2 fan failure ,the rear fan fault LED will
         turn to solid amber
         - CPU2 FAN fault LED and Rear FAN fault LED SGPIO number was swapped,
           resulting in incorrect LED lighting amber when one or the other
           failed
- Fixed: There are some failures in the VLAN ID  stress test .
         - VLAN config fixes:
           - VLAN ID was not always being read back correctly.
           - Fixed to return IPMI value for VLAN ID, not stale value 
           - Fixed VLAN Priority to work like all the other network parameters
           - Fixed IPv6 support
           - Fixed setting IPv6 to DHCP on web, which was erroneously returning
             IPMI Error 213
- Fixed: The Virtual Front Panel chassis ID LED blinking frequency is not
         synchronized with the front panel chassis ID LED
         - Virtual Front Panel was not reflecting chassis ID LED blink. It now
           detects and replicates this
- Fixed: There is a "BB +1.1V STBY low critical" event in SEL after AC cycling
         the SUT
         - 1.1V Standby voltage senor generating unwanted events when AC was
           removed with DC power on. Root caused to the 1.1V Stby voltage rail
           dropping very rapidly when AC is removed from a system that has DC
           power on. The BMC runs for a longer period so it saw the voltage
           drop out and generated events for it. Fix is to ignore voltage lower
           threshold crossings on this sensor if AC power is removed with DC
           power on.
- Fixed: Issue "Set CR Configuration" command with invalid value, the response
         isn't the correct error code
         - Was setting the user specific ranking. Ranking should be unique and
           less than number of working PS, should reject invalid numbers now.
- Fixed: S2600WP: MBE/DBE memory error did not sent SNMP and Email Alerts
- Fixed: Continuous Add SEL requests via KCS or IPMB leads to BMC auto-reset
- Fixed: Fwpiaupdt 11 Build 2: BMC update takes too long in all OS and EFI
- Fixed: Webserver sometimes shows socket error and does not respond till
         timeout when buttons pressed in quick succession
         - The refresh button at the bottom of the sensor reading page wasn't
           set to disable after a request, allowing for multiple rapid-fire
           requests with a very large overhead. The refresh button is now
           locked until the request completes, to prevent ASP floods on the
           sensor reading page.
- Fixed: RMM4 Ping Pong test failing with latest BMC 1.00
         - RMCP PING packets with non-0xff sequence were being dropped, but
           non-0xFF sequence numbers are allowed when the sender wants an ACK
           reply.
- Fixed: Update to BMC 1.0 with boot flag alone, doesn't reflect the boot area
         version
- Fixed: BMC Debug console constantly reporting "Invalid Logical GPIO: 197. Max
         is 161!" errors
- Fixed: S2600KI: DIMM Thermal Margin sensor readings should not be available
         in OLTT mode
- Fixed: Extended SEL severity code for Deassertions has non-informational
         severity
- Added: FRU IDs for PCI Risers 3 and 4 for S4600LH 
- Added: Initial FRUSDR release package for S4600LH
- Added: IO Module 2 support for S4600LH
- Added: IO Module 2 temp sensor support for S4600LH 
- Added: P3 and P4 related voltage sensors support for S4600LH
- Added: System fan1 and fan2 sensor numbers for S4600LH baseboard only support
- Added: BMC command implemented to read the ID and system fault LED

===============================================================================
                                01.00.2612
===============================================================================
- First production release of BMC


================================================================================
                   FRUSDR Changes in release 1.00
================================================================================    
S2600WP_1.00:
- None.

S2600WP_08:
- None.

S2600WP_07:
- None.

S2600WP_06:
- [EPSD100017013]: Status LED will amber blinking when system power on before 
  BIOS post screen.
- [EPSD100017369]: Detect Temperture Exit Air Temp (#0x2E) Upper Non-Critical,
  Upper Critical event when plugged all nodes in chassis.
  
S2600WP_05:
- None.

S2600WP_04:
- [EPSD100017413]: Detect "P1/2 Mem01/23 VRD Hot (#0x94)(#0x95)(#0x96)(#0x97)" 
  event generate in SEL after boot in OS and let it idle.

S2600WP_03:
- None.

S2600WP_02:
- None.

FWP_01:
- None.


=============================================================================
                            LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products. 
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation may 
have patents or pending patent applications, trademarks, copyrights, or other 
intellectual property rights that relate to the presented subject matter.  
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any 
such patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product 
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 
*Other names and brands are the property of their respective owners.
Copyright (c) 2012 Intel Corporation.

A portion of this firmware is open source code, which falls under the
GPL 2.0 license.  

[END OF RELEASE NOTES]
