//****************************************************************************
//                          Intel Corporation
//                    Jones Farm, Hillsboro, Oregon
//                           (503) 696-8080
//
//                Intel Corporation Proprietary Information
//     Copyright (c) 2010 - 2012 Intel Corporation, All Rights Reserved
//****************************************************************************
//
//
// File Header Information
//

_LF_NAME       'Copper Pass SDR File'
_LF_VERSION    '1.09'
_LF_FMT_VER    '1.50'
_IPMI_VERSION  '2.00'

//
// SDR Header Information
//

_SDR (
_START_ADDR     0000
_DATA_LEN       0000
_NVS_TYPE       'IMBDEVICE'
_DEV_BUS        FF
_DEV_ADDRESS    20

//====================================================================//
// (1) Chassis related TAG
//====================================================================//
// _SDR_TAG    'P4000_BASE'             // SDRs for Intel(R) Server Chassis P4000M Non Redundant Fan passive heatsink SKU
// _SDR_TAG    'P4000'                  // SDRs for Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU
// _SDR_TAG    'P4000_ACTIVE'           // SDRs for Intel(R) Server Chassis P4000M Non Redundant Fan 150w active SKU
// _SDR_TAG    'OTHER'                  // SDRs for OTHER chassis
// _SDR_TAG    'OTHER_SR'               // SDRs for OTHER(Slow Ramp) chassis
// _SDR_TAG    'OTHER_MR'               // SDRs for OTHER(Medium Ramp) chassis
// _SDR_TAG    'OTHER_FR'               // SDRs for OTHER(Fast Ramp) chassis

//====================================================================//
// (2) Processor related sensors
//====================================================================//
// _SDR_TAG     'PROC_1'                // SDRs for Processor 1
// _SDR_TAG     'PROC_2'                // SDRs for Processor 2

//====================================================================//
// (3) Temperature sensors
//====================================================================//
// _SDR_TAG    'FP_TEMP'                // SDR for Front Panel Temp
// _SDR_TAG    'EATEMP'                 // SDR for Exit Air Temp

//====================================================================//
// (4) Fan sensors
//====================================================================//
// _SDR_TAG   'PROC1_FAN'               // Processor Fan 1
// _SDR_TAG   'PROC2_FAN'               // Processor Fan 2
// _SDR_TAG   'OTHER_FAN_1'             // System Fan 1
// _SDR_TAG   'OTHER_FAN_2'             // System Fan 2
// _SDR_TAG   'OTHER_FAN_3'             // System Fan 3
// _SDR_TAG   'OTHER_FAN_4'             // System Fan 4
// _SDR_TAG   'OTHER_FAN_5'             // System Fan 5
// _SDR_TAG   'OTHER_FAN_6'             // System Fan 6
// _SDR_TAG   'OTHER_REAR_FAN'          // Rear Fan
// _SDR_TAG   'FAN_120_1'               // System Fan 1 (120mm Core)
// _SDR_TAG   'FAN_120_2'               // System Fan 2 (120mm PCI)
// _SDR_TAG   'FAN_1'                   // System Fan 1 (80mm)
// _SDR_TAG   'FAN_2'                   // System Fan 2 (80mm)
// _SDR_TAG   'FAN_3'                   // System Fan 3 (80mm)
// _SDR_TAG   'FAN_4'                   // System Fan 4 (80mm)
// _SDR_TAG   'FAN_5'                   // System Fan 5 (80mm)
// _SDR_TAG   'FCT_FAN_6'               // System Fan 6 for FCT/FCT2
// _SDR_TAG   'FAN_REDUN_FLAG'          // Fan Redundancy Sensor for third-party chassis

//====================================================================//
// (5) Chassis Intrusion
//====================================================================//
// _SDR_TAG     'CHASSIS_INTRU'         // Physical Security sensor
// _SDR_TAG     'NO_CHASSIS_INTRU'      // Physical Security Sensor with lan leash lost event mask only

//====================================================================//
// (6) Front Panel NMI Button
//====================================================================//
//_SDR_TAG    'FP_NMI'

//====================================================================//
// (7) Other device sensors
//====================================================================//
// _SDR_TAG    'HSBP_1_BP4'             // SDR for 4 port HSBP 1
// _SDR_TAG    'HSBP_2_BP4'             // SDR for 4 port HSBP 2
// _SDR_TAG    'HSBP_3_BP4'             // SDR for 4 port HSBP 3
// _SDR_TAG    'HSBP_1_BP8'             // SDR for 8 port HSBP 1
// _SDR_TAG    'HSBP_2_BP8'             // SDR for 8 port HSBP 2
// _SDR_TAG    'HSBP_3_BP8'             // SDR for 8 port HSBP 3
// _SDR_TAG    'IO_MOD'                 // SDR for I/O module
// _SDR_TAG    'SAS_MOD'                // SDR for SAS module

//====================================================================//
// (8) Power Supply related sensors
//====================================================================//
// _SDR_TAG    'PS_REDUNDANCY'          // Redundant Power Supply
// _SDR_TAG    '460_PS1'                // 460W Power Supply 1.
// _SDR_TAG    '460_PS2'                // 460W Power Supply 2.
// _SDR_TAG    '750_PS1'                // 750W Power Supply 1.
// _SDR_TAG    '750_PS2'                // 750W Power Supply 2.
// _SDR_TAG    '1200_PS1'               // 1200W Power Supply 1.
// _SDR_TAG    '1200_PS2'               // 1200W Power Supply 2.

//====================================================================//
// (9) Factory sensors
//====================================================================//
// _SDR_TAG     'SHIP'                  // SDRs for Shippings
// _SDR_TAG     'FCT'                   // SDRs for FCT
// _SDR_TAG     'FCT2'                  // SDRs for FCT2

//====================================================================//
_SDR_TYPE   02
_REC_LEN    002F

   // Sensor Record Header
   0001               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   01                 // Sensor Number

   // Record Body Bytes
   15                 // Entity ID - power management / power distribution board
   01                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   40                 // Sensor Capabilities
   09                 // Sensor Type - power unit
   6F                 // Event / Reading Base Type
   7100               // Assertion Event Mask   --Power down/A/C lost/Soft power control failure/Power unit failure =7100
   7100               // Deassertion Event Mask --Power down/A/C lost/Soft power control failure/Power unit failure =7100
   7100               // Reading Mask & Settable / Readable Threshold Masks --Power down/A/C lost/Soft power control failure/Power unit failure =7100
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Pwr Unit Status'  // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PS_REDUNDANCY'
_REC_LEN    002F

   // Sensor Record Header
   0002               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   02                 // Sensor Number

   // Record Body Bytes
   15                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   09                 // Sensor Type
   0B                 // Event / Reading Base Type
   FF00               // Assertion Event Mask   --Redundancy regained/Non-red: suff res from redund/Redundancy lost/Redundancy degraded/Non-red: suff from insuff/Non-red: insufficient/Redun degrade from full/Redun degrade from non-redundant=FF00
   0000               // Deassertion Event Mask --Redundancy regained/Non-red: suff res from redund/Redundancy lost/Redundancy degraded/Non-red: suff from insuff/Non-red: insufficient/Redun degrade from full/Redun degrade from non-redundant=FF00
   FF00               // Reading Mask & Settable / Readable Threshold Masks
                      //--Redundancy regained/Non-red: suff res from redund/Redundancy lost/Redundancy degraded/Non-red: suff from insuff/Non-red: insufficient/Redun degrade from full/Redun degrade from non-redundant=FF00
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Pwr Unit Redund'  // String Bytes

//====================================================================//
_SDR_TYPE   02
_REC_LEN    002D

   // Sensor Record Header
   0003               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   03                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   23                 // Sensor Type
   6F                 // Event / Reading Base Type
   0F01               // Assertion Event Mask   --Timer expired, status only/Hard reset/Power down/Power cycle/Timer interrupt =0F01
   0000               // Deassertion Event Mask --No Deassertion =0000
   0F01               // Reading Mask & Settable / Readable Threshold Masks --Timer expired, status only/Hard reset/Power down/Power cycle/Timer interrupt =0F01
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'IPMI Watchdog'    // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'CHASSIS_INTRU'
_REC_LEN    002E

   // Sensor Record Header
   0004               // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   04                 // Sensor Number

   // Record Body Bytes
   17                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   05                 // Sensor Type
   6F                 // Event / Reading Base Type
   1100               // Assertion Event Mask   --Chassis intrusion/LAN leash lost 1 =1100
   1100               // Deassertion Event Mask --Chassis intrusion/LAN leash lost 1 =1100
   1100               // Reading Mask & Settable / Readable Threshold Masks --Chassis intrusion/LAN leash lost 1 =1100
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Physical Scrty'   // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'NO_CHASSIS_INTRU'
_REC_LEN    002E

   // Sensor Record Header
   0005               // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   04                 // Sensor Number

   // Record Body Bytes
   17                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   05                 // Sensor Type
   6F                 // Event / Reading Base Type
   1000               // Assertion Event Mask   -- LAN leash lost =1000
   1000               // Deassertion Event Mask -- LAN leash lost =1000
   1000               // Reading Mask & Settable / Readable Threshold Masks -- LAN leash lost =1000
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Physical Scrty'   // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'FP_NMI'
_REC_LEN    002F

   // Sensor Record Header
   0006               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   05                 // Sensor Number

   // Record Body Bytes
   0C                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   13                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Assertion Event Mask   --Front panel NMI/diagnostic interrupt = 0100
   0000               // Deassertion Event Mask --No Deassertion =0000
   0100               // Reading Mask & Settable / Readable Threshold Masks --Front panel NMI/diagnostic interrupt = 0100
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'FP NMI Diag Int'  // String Bytes

//====================================================================//
_SDR_TYPE   02
_REC_LEN    002B

   // Sensor Record Header
   0007               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   06                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   41                 // Sensor Capabilities
   F3                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --State asserted =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'SMI Timeout'      // String Bytes

//====================================================================//
_SDR_TYPE   02
_REC_LEN    0030

   // Sensor Record Header
   0008               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   07                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   10                 // Sensor Type
   6F                 // Event / Reading Base Type
   0400               // Assertion Event Mask  --Log area reset / cleared =0400
   0000               // Deassertion Event Mask --N/A
   0400               // Reading Mask & Settable / Readable Threshold Masks --Log area reset / cleared =0400
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'System Event Log' // String Bytes

//====================================================================//
_SDR_TYPE   02
_REC_LEN    002C

   // Sensor Record Header
   0009               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   08                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   12                 // Sensor Type
   6F                 // Event / Reading Base Type
   1000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   1000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'System Event'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_REC_LEN    0026

   // Sensor Record Header
   000A               // Record ID
   51                 // SDR Version
   02                 // Record Type
   21                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   09                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   14                 // Sensor Type
   6F                 // Event / Reading Base Type
   0500               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0500               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C6                 // Type/Length Code
   'Button'           // String Bytes

//====================================================================//
_SDR_TYPE      03
_REC_LEN       001D

   // Sensor Record Header
   000B               // Record ID
   51                 // SDR Version
   03                 // Record Type
   18                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0A                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   28                // Sensor type
   03                // Event/Reading Type Code
   0100              // Sensor Record Sharing
   00                // Reserved
   00                // OEM
   CC                 // Type/Length Code
   'BMC Watchdog'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_REC_LEN    002B

   // Sensor Record Header
   000C               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0B                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   02                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --State asserted =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'VR Watchdog'      // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'P4000'
_SDR_TAG    'FAN_REDUN_FLAG'
_SDR_TAG    'FCT'
_SDR_TAG    'FCT2'
_REC_LEN    002E

   // Sensor Record Header
   000D               // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0C                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   04                 // Sensor Type
   0B                 // Event / Reading Base Type
   FF00               // Assertion Event Mask   --Redundancy regained/Non-red: suff res from redund/Redundancy lost/Redundancy degraded/Non-red: suff from insuff/Non-red: insufficient/Redun degrade from full/Redun degrade from non-redundant=FF00
   FF00               // Deassertion Event Mask --Redundancy regained/Non-red: suff res from redund/Redundancy lost/Redundancy degraded/Non-red: suff from insuff/Non-red: insufficient/Redun degrade from full/Redun degrade from non-redundant=FF00
   FF00               // Reading Mask & Settable / Readable Threshold Masks
                      //--Redundancy regained/Non-red: suff res from redund/Redundancy lost/Redundancy degraded/Non-red: suff from insuff/Non-red: insufficient/Redun degrade from full/Redun degrade from non-redundant=FF00
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Fan Redundancy'   // String Bytes

//====================================================================//
_SDR_TYPE   02
_REC_LEN    002E

   // Sensor Record Header
   000E               // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0D                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   01                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --State asserted =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'SSB Therm Trip'   // String Bytes

//====================================================================//
_SDR_TYPE   02
_REC_LEN    002D

   // Sensor Record Header
   000F               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   10                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   28                 // Sensor Type
   6F                 // Event / Reading Base Type
   1000               // Assertion Event Mask   --State asserted =1000
   0000               // Deassertion Event Mask --State asserted =0000
   1000               // Reading Mask & Settable / Readable Threshold Masks --State asserted =1000
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'BMC FW Health'    // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    003E

   // Sensor Record Header
   0010               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   11                 // Sensor Number

   // Record Body Bytes
   17                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   63                 // Sensor Capabilities
   0B                 // Sensor Type -- (Other unit based sensor)
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   11                 // Sensor Units 2 -- (CFM)
   00                 // Sensor Units 3
   00                 // Linearization
   02                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   5A                 // Nominal Reading (5Ah = 180 CFM)
   B4                 // Normal Maximum (B4h = 360 CFM)
   00                 // Normal Minimum (00h = 0 CFM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 510 CFM)
   00                 // Sensor Minimum Reading (00h = 0 CFM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'System Airflow'   // String Bytes

//====================================================================//
_SDR_TYPE   03
_REC_LEN    0021

   // Sensor Record Header
   0011               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1C                 // Record Length
   
   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   12                 // Sensor Number
   
   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   2B                 // Sensor type
   70                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'FW Update Status' // String Bytes


//====================================================================//
//
// Baseboard and chassis related temperature related sensors
//
//====================================================================//
_SDR_TYPE   01
_REC_LEN    003C

   // Sensor Record Header
   0012               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   20                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type -- (Temperature)
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- (Degrees C)
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   3A                 // Normal Reading (3Ah = 58 degrees C)
   69                 // Normal Maximum (69h = 105 degrees C)
   0A                 // Normal Minimum (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   73                 // Upper critical (73h = 115 degrees C)
   6E                 // Upper non-critical (6Eh = 110 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (00h = 0 degrees C)
   05                 // Lower non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'BB EDGE Temp'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'FP_TEMP'
_REC_LEN    0040

   // Sensor Record Header
   0013               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   21                 // Sensor Number

   // Record Body Bytes
   40                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- (Degrees C)
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   1C                 // Normal Reading (1Ch = 28 degrees C)
   2D                 // Normal Maximum (2Dh = 45 degrees C)
   0A                 // Normal Minimum (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   37                 // Upper critical (37h = 55 degrees C)
   32                 // Upper non-critical (32h = 50 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (00h = 0 degrees C)
   05                 // Lower non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   D0                 // Type/Length Code
   'Front Panel Temp' // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    0038

   // Sensor Record Header
   0014               // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   22                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type -- (Temperature)
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- (Degrees C)
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   34                 // Normal Reading (34h = 52 degrees C)
   5D                 // Normal Maximum (5Dh = 93 degrees C)
   0A                 // Normal Minimum (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   67                 // Upper critical (67h = 103 degrees C)
   62                 // Upper non-critical (62h = 98 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (00h = 0 degrees C)
   05                 // Lower non-critical (05h = 05 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C8                 // Type/Length Code
   'SSB Temp'         // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    003B

   // Sensor Record Header
   0015               // Record ID
   51                 // SDR Version
   01                 // Record Type
   36                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   23                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type -- (Temperature)
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- (Degrees C)
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   3A                 // Normal Reading (3Ah = 58 degrees C)
   69                 // Normal Maximum (69h = 105 degrees C)
   0A                 // Normal Minimum (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   73                 // Upper critical (73h = 115 degrees C)
   6E                 // Upper non-critical (6Eh = 110 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (00h = 0 degrees C)
   05                 // Lower non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'BB BMC Temp'      // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    003D

   // Sensor Record Header
   0016               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   24                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type -- (Temperature)
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- (Degrees C)
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   3A                 // Normal Reading (3Ah = 58 degrees C)
   69                 // Normal Maximum (69h = 105 degrees C)
   0A                 // Normal Minimum (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   73                 // Upper critical (73h = 115 degrees C)
   6E                 // Upper non-critical (6Eh = 110 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (00h = 0 degrees C)
   05                 // Lower non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'BB P2 VR Temp'    // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    003E

   // Sensor Record Header
   0017               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   25                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type -- (Temperature)
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- (Degrees C)
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   3A                 // Normal Reading (3Ah = 58 degrees C)
   69                 // Normal Maximum (69h = 105 degrees C)
   0A                 // Normal Minimum (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   73                 // Upper critical (73h = 115 degrees C)
   6E                 // Upper non-critical (6Eh = 110 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (00h = 0 degrees C)
   05                 // Lower non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'BB MEM VR Temp'   // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'HSBP_1_BP4'
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    003B

   // Sensor Record Header
   0018               // Record ID
   51                 // SDR Version
   01                 // Record Type
   36                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   29                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   7D                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask    --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask  --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   3A                 // Normal Reading (3Ah = 58 degrees C)
   69                 // Normal Maximum (69h = 105 degrees C)
   0A                 // Normal Minimum (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   73                 // Upper critical (73h = 115 degrees C)
   6E                 // Upper non-critical (6Eh = 110 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (00h = 0 degrees C)
   05                 // Lower non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type Length Code
   'HSBP 1 Temp'      // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'HSBP_2_BP4'
_SDR_TAG    'HSBP_2_BP8'
_REC_LEN    003B

   // Sensor Record Header
   0019               // Record ID
   51                 // SDR Version
   01                 // Record Type
   36                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   2A                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   02                 // Entity Instance
   7D                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask    --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask  --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   3A                 // Normal Reading (3Ah = 58 degrees C)
   69                 // Normal Maximum (69h = 105 degrees C)
   0A                 // Normal Minimum (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   73                 // Upper critical (73h = 115 degrees C)
   6E                 // Upper non-critical (6Eh = 110 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (00h = 0 degrees C)
   05                 // Lower non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type Length Code
   'HSBP 2 Temp'      // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'HSBP_3_BP4'
_SDR_TAG    'HSBP_3_BP8'
_REC_LEN    003B

   // Sensor Record Header
   001A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   36                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   2B                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   03                 // Entity Instance
   7D                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask    --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask  --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   3A                 // Normal Reading (3Ah = 58 degrees C)
   69                 // Normal Maximum (69h = 105 degrees C)
   0A                 // Normal Minimum (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   73                 // Upper critical (73h = 115 degrees C)
   6E                 // Upper non-critical (6Eh = 110 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (00h = 0 degrees C)
   05                 // Lower non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type Length Code
   'HSBP 3 Temp'      // String Bytes
   
//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'EATEMP'
_REC_LEN    003D

   // Sensor Record Header
   001B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   2E                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type -- (Temperature)
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask   --[u,l][c,nc]=0000
   0000               // Deassertion Event Mask --[u,l][c,nc]=0000
   0000               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=0000
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- (Degrees C)
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   28                 // Normal Reading (28h = 40 degrees C)
   46                 // Normal Maximum (46h = 70 degrees C)
   0A                 // Normal Minimum (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   55                 // Upper critical (55h = 85 degrees C)
   50                 // Upper non-critical (50h = 80 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (00h = 0 degrees C)
   05                 // Lower non-critical (05h = 05 degrees C)
   //------------------------------------------------------------------//
   04                 // Positive hysteresis value
   04                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   47                 // OEM
   CD                 // Type/Length Code
   'Exit Air Temp'    // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    003C

   // Sensor Record Header
   001C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   2F                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   3C                 // Normal Reading (3Ch = 60 degrees C)
   6E                 // Normal Maximum (6Eh = 110 degrees C)
   0A                 // Normal Minimum (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   78                 // Upper critical (78h = 120 degrees C)
   73                 // Upper non-critical (73h = 115 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (00h =0 degrees C)
   05                 // Lower non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CC                 // Type/Length Code
   'LAN NIC Temp'     // String Bytes

//====================================================================//
//
// Fan tachometer sensors
//
//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_1'
_REC_LEN    003C

   // Sensor Record Header
   001D               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   30                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   82                 // Normal Reading (82h == 12750 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   05                 // Normal Minimum (05h == 500 RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 25000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   03                 // Lower critical (03h == 300 RPM)
   04                 // Lower non-critical (04h == 400 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 1'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'FAN_1'
_REC_LEN    003C

   // Sensor Record Header
   001E               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   30                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   21                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   87                 // Normal Reading (87h == 4500 RPM)
   FF                 // Normal Maximum (FFh == 8500 RPM)
   0F                 // Normal Minimum (0Fh == 500 RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 8500 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   06                 // Lower critical (06h == 200 RPM)
   09                 // Lower non-critical (09h == 300 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 1'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'FAN_120_1'
_REC_LEN    003C

   // Sensor Record Header
   001F               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   30                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   0E                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   97                 // Normal Reading (97h == 2200 RPM)
   FF                 // Normal Maximum (FFh == 3700 RPM)
   30                 // Normal Minimum (30h == 700  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 3700 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   21                 // Lower critical (21h == 490 RPM)
   26                 // Lower non-critical (26h == 560 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 1'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_2'
_REC_LEN    003C

   // Sensor Record Header
   0020               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   31                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   03                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   82                 // Normal Reading (82h == 12750 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   05                 // Normal Minimum (05h == 500 RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 25000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   03                 // Lower critical (03h == 300 RPM)
   04                 // Lower non-critical (04h == 400 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 2'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'FAN_2'
_REC_LEN    003C

   // Sensor Record Header
   0021               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   31                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   03                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   21                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   87                 // Normal Reading (87h == 4500 RPM)
   FF                 // Normal Maximum (FFh == 8500 RPM)
   0F                 // Normal Minimum (0Fh == 500 RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 8500 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   06                 // Lower critical (06h == 200 RPM)
   09                 // Lower non-critical (09h == 300 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 2'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'FAN_120_2'
_REC_LEN    003C

   // Sensor Record Header
   0022               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   31                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   03                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   14                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   90                 // Normal Reading (90h == 3000 RPM)
   FF                 // Normal Maximum (FFh == 5300 RPM)
   21                 // Normal Minimum (21h == 700  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 5300 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   17                 // Lower critical (17h == 490 RPM)
   1A                 // Lower non-critical (1Ah == 560 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 2'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_3'
_REC_LEN    003C

   // Sensor Record Header
   0023               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   32                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   04                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   82                 // Normal Reading (82h == 12750 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   05                 // Normal Minimum (05h == 500 RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 25000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   03                 // Lower critical (03h == 300 RPM)
   04                 // Lower non-critical (04h == 400 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 3'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'FAN_3'
_REC_LEN    003C

   // Sensor Record Header
   0024               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   32                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   04                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   21                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   87                 // Normal Reading (87h == 4500 RPM)
   FF                 // Normal Maximum (FFh == 8500 RPM)
   0F                 // Normal Minimum (0Fh == 500 RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 8500 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   06                 // Lower critical (06h == 200 RPM)
   09                 // Lower non-critical (09h == 300 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 3'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_4'
_REC_LEN    003C

   // Sensor Record Header
   0025               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   33                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   05                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   82                 // Normal Reading (82h == 12750 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   05                 // Normal Minimum (05h == 500 RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 25000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   03                 // Lower critical (03h == 300 RPM)
   04                 // Lower non-critical (04h == 400 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 4'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'FAN_4'
_REC_LEN    003C

   // Sensor Record Header
   0026               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   33                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   05                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   21                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   87                 // Normal Reading (87h == 4500 RPM)
   FF                 // Normal Maximum (FFh == 8500 RPM)
   0F                 // Normal Minimum (0Fh == 500 RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 8500 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   06                 // Lower critical (06h == 200 RPM)
   09                 // Lower non-critical (09h == 300 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 4'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_5'
_REC_LEN    003C

   // Sensor Record Header
   0027               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   34                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   06                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   82                 // Normal Reading (82h == 12750 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   05                 // Normal Minimum (05h == 500 RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 25000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   03                 // Lower critical (03h == 300 RPM)
   04                 // Lower non-critical (04h == 400 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 5'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'FAN_5'
_REC_LEN    003C

   // Sensor Record Header
   0028               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   34                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   06                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   21                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   87                 // Normal Reading (87h == 4500 RPM)
   FF                 // Normal Maximum (FFh == 8500 RPM)
   0F                 // Normal Minimum (0Fh == 500 RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 8500 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   06                 // Lower critical (06h == 200 RPM)
   09                 // Lower non-critical (09h == 300 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 5'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_6'
_SDR_TAG    'FCT_FAN_6'
_REC_LEN    003C

   // Sensor Record Header
   0029               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   35                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   07                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   82                 // Normal Reading (82h == 12750 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   05                 // Normal Minimum (05h == 500 RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 25000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   03                 // Lower critical (03h == 300 RPM)
   04                 // Lower non-critical (04h == 400 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 6'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC1_FAN'
_REC_LEN    003F

   // Sensor Record Header
   002A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   36                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   08                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   82                 // Normal Reading (82h == 12750 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   05                 // Normal Minimum (05h == 500 RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 25000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   03                 // Lower critical (03h == 300 RPM)
   04                 // Lower non-critical (04h == 400 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   03                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CF                 // Type/Length Code
   'Processor 1 Fan'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC2_FAN'
_REC_LEN    003F

   // Sensor Record Header
   002B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   37                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   09                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   82                 // Normal Reading (82h == 12750 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   05                 // Normal Minimum (05h == 500 RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 25000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   03                 // Lower critical (03h == 300 RPM)
   04                 // Lower non-critical (04h == 400 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   03                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CF                 // Type/Length Code
   'Processor 2 Fan'  // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_REAR_FAN'
_REC_LEN    0038

   // Sensor Record Header
   002C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   38                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0A                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   82                 // Normal Reading (82h == 12750 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   05                 // Normal Minimum (05h == 500 RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 25000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   03                 // Lower critical (03h == 300 RPM)
   04                 // Lower non-critical (04h == 400 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   C8                 // Type/Length Code
   'Rear Fan'         // String Bytes

//====================================================================//
//
// Fan presence sensors (Only supported with hot-swappable fans)
//
//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'FAN_1'
_REC_LEN    002D

   // Sensor Record Header
   002D               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   40                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   04                 // Sensor Type
   08                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --Device present =0200
   0200               // Deassertion Event Mask --Device present =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --Device present =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Fan 1 Present'    // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'FAN_2'
_REC_LEN    002D

   // Sensor Record Header
   002E               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   41                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   03                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   04                 // Sensor Type
   08                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --Device present =0200
   0200               // Deassertion Event Mask --Device present =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --Device present =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Fan 2 Present'    // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'FAN_3'
_REC_LEN    002D

   // Sensor Record Header
   002F               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   42                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   04                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   04                 // Sensor Type
   08                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --Device present =0200
   0200               // Deassertion Event Mask --Device present =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --Device present =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Fan 3 Present'    // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'FAN_4'
_REC_LEN    002D

   // Sensor Record Header
   0030               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   43                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   05                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   04                 // Sensor Type
   08                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --Device present =0200
   0200               // Deassertion Event Mask --Device present =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --Device present =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Fan 4 Present'   // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'FAN_5'
_REC_LEN    002D

   // Sensor Record Header
   0031               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   44                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   06                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   04                 // Sensor Type
   08                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --Device present =0200
   0200               // Deassertion Event Mask --Device present =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --Device present =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Fan 5 Present'   // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'FCT_FAN_6'
_REC_LEN    002D

   // Sensor Record Header
   0032               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   45                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   07                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   04                 // Sensor Type
   08                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --Device present =0200
   0200               // Deassertion Event Mask --Device present =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --Device present =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Fan 6 Present'    // String Bytes

//====================================================================//
//
// Power supply sensors (Only supported with PMBus enabled power supplies)
//
//====================================================================//
_SDR_TYPE   02
_SDR_TAG    '460_PS1'
_SDR_TAG    '750_PS1'
_SDR_TAG    '1200_PS1'
_REC_LEN    002A

   // Sensor Record Header
   0033               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   50                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   08                 // Sensor Type
   6F                 // Event / Reading Base Type
   4F00               // Assertion Event Mask   --Presence/Failure/Predictive Failure/A/C lost/Configuration error =4F00
   4F00               // Deassertion Event Mask --Presence/Failure/Predictive Failure/A/C lost/Configuration error =4F00
   4F00               // Reading Mask & Settable / Readable Threshold Masks --Presence/Failure/Predictive Failure/A/C lost/Configuration error =4F00
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'PS1 Status'       // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    '460_PS2'
_SDR_TAG    '750_PS2'
_SDR_TAG    '1200_PS2'
_REC_LEN    002A

   // Sensor Record Header
   0034               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   51                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   08                 // Sensor Type
   6F                 // Event / Reading Base Type
   4F00               // Assertion Event Mask   --Presence/Failure/Predictive Failure/A/C lost/Configuration error =4F00
   4F00               // Deassertion Event Mask --Presence/Failure/Predictive Failure/A/C lost/Configuration error =4F00
   4F00               // Reading Mask & Settable / Readable Threshold Masks --Presence/Failure/Predictive Failure/A/C lost/Configuration error =4F00
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'PS2 Status'       // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '460_PS1'
_REC_LEN    003C

   // Sensor Record Header
   0035               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   54                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   03                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   56                 // Nomnal Reading (56h=258.0Watt)
   AC                 // Normal Maximum (ACh=516.0Watt)
   00                 // Normal Minimum (00h=0Watt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh=765.0Watt)
   00                 // Sensor Minimum Reading (00h=0.0Watt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   CC                 // Upper critical (CCh=612.0Watt)
   BC                 // Upper non-critical (BCh=564.0Watt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'PS1 Power In'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '750_PS1'
_REC_LEN    003C

   // Sensor Record Header
   0036               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   54                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   04                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   66                 // Nomnal Reading (66h=408.0Watt)
   CC                 // Normal Maximum (CCh=816.0Watt)
   00                 // Normal Minimum (00h=0Watt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh=1020.0Watt)
   00                 // Sensor Minimum Reading (00h=0.0Watt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   E6                 // Upper critical (E6h=920.0Watt)
   D9                 // Upper non-critical (D9h=868.0Watt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'PS1 Power In'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '1200_PS1'
_REC_LEN    003C

   // Sensor Record Header
   0037               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   54                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   07                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   5E                 // Nomnal Reading (5Eh=658.0Watt)
   BC                 // Normal Maximum (BCh=1316.0Watt)
   00                 // Normal Minimum (00h=0Watt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh=1785.0Watt)
   00                 // Sensor Minimum Reading (00h=0.0Watt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   FA                 // Upper critical (FAh=1750.0Watt)
   DB                 // Upper non-critical (DBh=1533.0Watt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'PS1 Power In'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '460_PS2'
_REC_LEN    003C

   // Sensor Record Header
   0038               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   55                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   03                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   56                 // Nomnal Reading (56h=258.0Watt)
   AC                 // Normal Maximum (ACh=516.0Watt)
   00                 // Normal Minimum (00h=0Watt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh=765.0Watt)
   00                 // Sensor Minimum Reading (00h=0.0Watt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   CC                 // Upper critical (CCh=612.0Watt)
   BC                 // Upper non-critical (BCh=564.0Watt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'PS2 Power In'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '750_PS2'
_REC_LEN    003C

   // Sensor Record Header
   0039               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   55                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   04                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   66                 // Nomnal Reading (66h=408.0Watt)
   CC                 // Normal Maximum (CCh=816.0Watt)
   00                 // Normal Minimum (00h=0Watt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh=1020.0Watt)
   00                 // Sensor Minimum Reading (00h=0.0Watt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   E6                 // Upper critical (E6h=920.0Watt)
   D9                 // Upper non-critical (D9h=868.0Watt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'PS2 Power In'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '1200_PS2'
_REC_LEN    003C

   // Sensor Record Header
   003A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   55                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   07                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   5E                 // Nomnal Reading (5Eh=658.0Watt)
   BC                 // Normal Maximum (BCh=1316.0Watt)
   00                 // Normal Minimum (00h=0Watt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh=1785.0Watt)
   00                 // Sensor Minimum Reading (00h=0.0Watt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   FA                 // Upper critical (FAh=1750.0Watt)
   DB                 // Upper non-critical (DBh=1533.0Watt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'PS2 Power In'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '460_PS1'
_REC_LEN    003E

   // Sensor Record Header
   003B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   58                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   32                 // Normal Reading (32h = 50 %)
   64                 // Normal Maximum (64h = 100 %)
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   76                 // Upper critical (76h = 118.0 %)
   64                 // Upper non-critical (64h = 100.0 %)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical  (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysterisis value
   00                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS1 Curr Out %'   // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '750_PS1'
_REC_LEN    003E

   // Sensor Record Header
   003C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   58                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   32                 // Normal Reading (32h = 50 %)
   64                 // Normal Maximum (64h = 100 %)
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   70                 // Upper critical (70h = 112.0 %)
   64                 // Upper non-critical (64h = 100.0 %)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical  (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysterisis value
   00                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS1 Curr Out %'   // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '1200_PS1'
_REC_LEN    003E

   // Sensor Record Header
   003D               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   58                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   32                 // Normal Reading (32h = 50 %)
   64                 // Normal Maximum (64h = 100 %)
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   85                 // Upper critical (85h = 133.0 %)
   64                 // Upper non-critical (64h = 100.0 %)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical  (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysterisis value
   00                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS1 Curr Out %'   // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '460_PS2'
_REC_LEN    003E

   // Sensor Record Header
   003E               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   59                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   32                 // Normal Reading (32h = 50 %)
   64                 // Normal Maximum (64h = 100 %)
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   76                 // Upper critical (76h = 118.0 %)
   64                 // Upper non-critical (64h = 100.0 %)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical  (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysterisis value
   00                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS2 Curr Out %'   // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '750_PS2'
_REC_LEN    003E

   // Sensor Record Header
   003F               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   59                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   32                 // Normal Reading (32h = 50 %)
   64                 // Normal Maximum (64h = 100 %)
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   70                 // Upper critical (70h = 112.0 %)
   64                 // Upper non-critical (64h = 100.0 %)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical  (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysterisis value
   00                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS2 Curr Out %'   // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '1200_PS2'
_REC_LEN    003E

   // Sensor Record Header
   0040               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   59                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   32                 // Normal Reading (32h = 50 %)
   64                 // Normal Maximum (64h = 100 %)
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   85                 // Upper critical (85h = 133.0 %)
   64                 // Upper non-critical (64h = 100.0 %)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical  (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysterisis value
   00                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS2 Curr Out %'   // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '460_PS1'
_SDR_TAG    '750_PS1'
_SDR_TAG    '1200_PS1'
_REC_LEN    003F

   // Sensor Record Header
   0041               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   5C                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   01                 // Sensor Type -- Temp
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- Degrees C
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   1C                 // Normal Reading (1Ch = 28 degrees C)
   37                 // Normal Maximum (37h = 55 degrees C)
   05                 // Normal Minimum (05h = 5 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   41                 // Upper critical (41h = 65 degrees C)
   3C                 // Upper non-critical (3Ch = 60 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CF                 // Type/Length Code
   'PS1 Temperature'  // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '460_PS2'
_SDR_TAG    '750_PS2'
_SDR_TAG    '1200_PS2'
_REC_LEN    003F

   // Sensor Record Header
   0042               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   5D                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   01                 // Sensor Type -- Temp
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- Degrees C
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   1C                 // Normal Reading (1Ch = 28 degrees C)
   37                 // Normal Maximum (37h = 55 degrees C)
   05                 // Normal Minimum (05h = 5 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   41                 // Upper critical (41h = 65 degrees C)
   3C                 // Upper non-critical (3Ch = 60 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CF                 // Type/Length Code
   'PS2 Temperature'  // String Bytes

//====================================================================//
//
// Backplane Status
//
//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_1_BP4'
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    002B

   // Sensor Record Header
   0043               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   69                 // Sensor Number

   // Record Body Bytes
   16                 // Entity ID - chassis back panel board
   01                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   40                 // Sensor Capabilities
   16                 // Sensor Type - microcontroller
   0A                 // Event / Reading Base Type
   1000               // Assertion Event Mask   -- transition to Off Line =1000
   1000               // Deassertion Event Mask -- transition to Off Line =1000
   1000               // Reading Mask & Settable / Readable Threshold Masks --transition to Off Line =1000
   00                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'HSC1 Status'       // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_2_BP4'
_SDR_TAG    'HSBP_2_BP8'
_REC_LEN    002B

   // Sensor Record Header
   0044               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   6A                 // Sensor Number

   // Record Body Bytes
   16                 // Entity ID - chassis back panel board
   02                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   40                 // Sensor Capabilities
   16                 // Sensor Type - microcontroller
   0A                 // Event / Reading Base Type
   1000               // Assertion Event Mask   -- transition to Off Line =1000
   1000               // Deassertion Event Mask -- transition to Off Line =1000
   1000               // Reading Mask & Settable / Readable Threshold Masks --transition to Off Line =1000
   00                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'HSC2 Status'       // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_3_BP4'
_SDR_TAG    'HSBP_3_BP8'
_REC_LEN    002B

   // Sensor Record Header
   0045               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   6B                 // Sensor Number

   // Record Body Bytes
   16                 // Entity ID - chassis back panel board
   03                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   40                 // Sensor Capabilities
   16                 // Sensor Type - microcontroller
   0A                 // Event / Reading Base Type
   1000               // Assertion Event Mask   -- transition to Off Line =1000
   1000               // Deassertion Event Mask -- transition to Off Line =1000
   1000               // Reading Mask & Settable / Readable Threshold Masks --transition to Off Line =1000
   00                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'HSC3 Status'      // String Bytes

//====================================================================//
//
// Processor (CPU) & DIMM sensors
//
//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROC_1'
_REC_LEN    0029

   // Sensor Record Header
   0046               // Record ID
   51                 // SDR Version
   02                 // Record Type
   24                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   70                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   6F                 // Event / Reading Base Type
   8200               // Assertion Event Mask   --Thermal trip/Presence =8200
   8200               // Deassertion Event Mask --Thermal trip/Presence =8200
   8200               // Reading Mask & Settable / Readable Threshold Masks --Thermal trip/Presence=8200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'P1 Status'        // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROC_2'
_REC_LEN    0029

   // Sensor Record Header
   0047               // Record ID
   51                 // SDR Version
   02                 // Record Type
   24                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   71                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   6F                 // Event / Reading Base Type
   8200               // Assertion Event Mask   --Thermal trip/Presence =8200
   8200               // Deassertion Event Mask --Thermal trip/Presence =8200
   8200               // Reading Mask & Settable / Readable Threshold Masks --Thermal trip/Presence=8200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'P2 Status'        // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_1'
_REC_LEN    003F

   // Sensor Record Header
   0048               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   74                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- (Degrees C)
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   F1                 // Normal Reading (F1h = -15 degree C)
   00                 // Normal Maximum (00h = 0 degree C)
   BA                 // Normal Minimum (BAh = -70 degree C)
   //------------------------------------------------------------------//
   00                 // Sensor Maximum Reading (00h = 0 degree C)
   80                 // Sensor Minimum Reading (80h = -128 degree C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degree C)
   00                 // Upper critical (00h = 0 degree C)
   00                 // Upper non-critical (00h = 0 degree C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degree C)
   00                 // Lower critical (00h = 0 degree C)
   00                 // Lower non-critical (00h = 0 degree C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CF                 // Type/Length Code
   'P1 Therm Margin'  // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_2'
_REC_LEN    003F

   // Sensor Record Header
   0049               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   75                 // Sensor Number

   // Record Body Byte
   03                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- (Degrees C)
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   F1                 // Normal Reading (F1h = -15 degree C)
   00                 // Normal Maximum (00h = 0 degree C)
   BA                 // Normal Minimum (BAh = -70 degree C)
   //------------------------------------------------------------------//
   00                 // Sensor Maximum Reading (00h = 0 degree C)
   80                 // Sensor Minimum Reading (80h = -128 degree C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degree C)
   00                 // Upper critical (00h = 0 degree C)
   00                 // Upper non-critical (00h = 0 degree C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degree C)
   00                 // Lower critical (00h = 0 degree C)
   00                 // Lower non-critical (00h = 0 degree C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CF                 // Type/Length Code
   'P2 Therm Margin'  // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_1'
_REC_LEN    003F

   // Sensor Record Header
   004A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   78                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   00                 // Normal Reading (00h = 0 %)
   14                 // Normal Maximum (14h = 20 %)
   00                 // Normal Minimum (00h = 0 %)
   //------------------------------------------------------------------//
   64                 // Sensor Maximum Reading (64h = 100 %)
   00                 // Sensor Minimum Reading (00h = 0 %)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 %)
   32                 // Upper critical (32h = 50 %)
   1E                 // Upper non-critical (1Eh = 30 %)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 %)
   00                 // Lower critical (00h = 0 %)
   00                 // Lower non-critical (00h = 0 %)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'P1 Therm Ctrl %'  // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_2'
_REC_LEN    003F

   // Sensor Record Header
   004B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   79                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   00                 // Normal Reading (00h = 0 %)
   14                 // Normal Maximum (14h = 20 %)
   00                 // Normal Minimum (00h = 0 %)
   //------------------------------------------------------------------//
   64                 // Sensor Maximum Reading (64h = 100 %)
   00                 // Sensor Minimum Reading (00h = 0 %)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 %)
   32                 // Upper critical (32h = 50 %)
   1E                 // Upper non-critical (1Eh = 30 %)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 %)
   00                 // Lower critical (00h = 0 %)
   00                 // Lower non-critical (00h = 0 %)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'P2 Therm Ctrl %'  // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROC_1'
_REC_LEN    0027

   // Sensor Record Header
   004C               // Record ID
   51                 // SDR Version
   02                 // Record Type
   22                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   7C                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   41                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --State asserted =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C7                 // Type/Length Code
   'P1 ERR2'          // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROC_2'
_REC_LEN    0027

   // Sensor Record Header
   004D               // Record ID
   51                 // SDR Version
   02                 // Record Type
   22                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   7D                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   41                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --State asserted =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C7                 // Type/Length Code
   'P2 ERR2'          // String Bytes

//====================================================================//
_SDR_TYPE   02
_REC_LEN    0026

   // Sensor Record Header
   004E               // Record ID
   51                 // SDR Version
   02                 // Record Type
   21                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   80                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C6                 // Type/Length Code
   'CATERR'           // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROC_1'
_REC_LEN    0030

   // Sensor Record Header
   004F               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   81                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'P1 MSID Mismatch' // String Bytes

//====================================================================//
_SDR_TYPE   02
_REC_LEN    002B

   // Sensor Record Header
   0050               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   82                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'CPU Missing'      // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_1'
_REC_LEN    0040

   // Sensor Record Header
   0051               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   83                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   F1                 // Normal Reading (F1h = -15 degree C)
   00                 // Normal Maximum (00h = 0 degree C)
   BA                 // Normal Minimum (BAh = -70 degree C)
   //------------------------------------------------------------------//
   00                 // Sensor Maximum Reading (00h = 0 degree C)
   80                 // Sensor Minimum Reading (80h = -128 degree C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degree C)
   0F                 // Upper critical (0Fh = 15 degree C)
   0A                 // Upper non-critical (0Ah = 10 degree C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degree C)
   00                 // Lower critical (00h = 0 degree C)
   00                 // Lower non-critical (00h = 0 degree C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   D0                 // Type/Length Code
   'P1 DTS Therm Mgn' // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_2'
_REC_LEN    0040

   // Sensor Record Header
   0052               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   84                 // Sensor Number

   // Record Body Byte
   03                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   F1                 // Normal Reading (F1h = -15 degree C)
   00                 // Normal Maximum (00h = 0 degree C)
   BA                 // Normal Minimum (BAh = -70 degree C)
   //------------------------------------------------------------------//
   00                 // Sensor Maximum Reading (00h = 0 degree C)
   80                 // Sensor Minimum Reading (80h = -128 degree C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degree C)
   0F                 // Upper critical (0Fh = 15 degree C)
   0A                 // Upper non-critical (0Ah = 10 degree C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degree C)
   00                 // Lower critical (00h = 0 degree C)
   00                 // Lower non-critical (00h = 0 degree C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   D0                 // Type/Length Code
   'P2 DTS Therm Mgn' // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROC_2'
_REC_LEN    0030

   // Sensor Record Header
   0053               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   87                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'P2 MSID Mismatch'  // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROC_1'
_REC_LEN    002A

   // Sensor Record Header
   0054               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   90                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   01                 // Sensor Type
   05                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --Limit exceeded =0200
   0200               // Deassertion Event Mask --Limit exceeded =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --Limit exceeded =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'P1 VRD Hot'       // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROC_2'
_REC_LEN    002A

   // Sensor Record Header
   0055               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   91                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   01                 // Sensor Type
   05                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --Limit exceeded =0200
   0200               // Deassertion Event Mask --Limit exceeded =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --Limit exceeded =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'P2 VRD Hot'       // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROC_1'
_REC_LEN    0030

   // Sensor Record Header
   0056               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   94                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   01                 // Sensor Type
   05                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --Limit exceeded =0200
   0200               // Deassertion Event Mask --Limit exceeded =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --Limit exceeded =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'P1 MEM01 VRD Hot' // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROC_1'
_REC_LEN    0030

   // Sensor Record Header
   0057               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   95                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   01                 // Sensor Type
   05                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --Limit exceeded =0200
   0200               // Deassertion Event Mask --Limit exceeded =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --Limit exceeded =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'P1 MEM23 VRD Hot' // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROC_2'
_REC_LEN    0030

   // Sensor Record Header
   0058               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   96                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   01                 // Sensor Type
   05                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --Limit exceeded =0200
   0200               // Deassertion Event Mask --Limit exceeded =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --Limit exceeded =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'P2 MEM01 VRD Hot' // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROC_2'
_REC_LEN    0030

   // Sensor Record Header
   0059               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   97                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   01                 // Sensor Type
   05                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --Limit exceeded =0200
   0200               // Deassertion Event Mask --Limit exceeded =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --Limit exceeded =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'P2 MEM23 VRD Hot' // String Bytes

//====================================================================//
//
// Power supply fan tachometer sensors
//
//====================================================================//
_SDR_TYPE   02
_SDR_TAG    '460_PS1'
_SDR_TAG    '750_PS1'
_REC_LEN    002C

   // Sensor Record Header
   005A               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   A0                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0B                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   00                 // Sensor Capabilities -- Manual Rearm
   04                 // Sensor Type - Fan
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Mask
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'PS1 Fan Fail'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    '1200_PS1'
_REC_LEN    002F

   // Sensor Record Header
   005B               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   A0                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0B                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   00                 // Sensor Capabilities -- Manual Rearm
   04                 // Sensor Type - Fan
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Mask
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS1 1a Fan Fail'  // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    '1200_PS1'
_REC_LEN    002F

   // Sensor Record Header
   005C               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   A1                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0C                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   00                 // Sensor Capabilities -- Manual Rearm
   04                 // Sensor Type - Fan
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Mask
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS1 1b Fan Fail'  // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    '460_PS2'
_SDR_TAG    '750_PS2'
_REC_LEN    002C

   // Sensor Record Header
   005D               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   A4                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0D                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   00                 // Sensor Capabilities -- Manual Rearm
   04                 // Sensor Type - Fan
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Mask
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'PS2 Fan Fail'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    '1200_PS2'
_REC_LEN    002F

   // Sensor Record Header
   005E               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   A4                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0D                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   00                 // Sensor Capabilities -- Manual Rearm
   04                 // Sensor Type - Fan
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Mask
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS2 1a Fan Fail'  // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    '1200_PS2'
_REC_LEN    002F

   // Sensor Record Header
   005F               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   A5                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0E                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   00                 // Sensor Capabilities -- Manual Rearm
   04                 // Sensor Type - Fan
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Mask
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS2 1b Fan Fail'  // String Bytes

//====================================================================//
//
// Memory thermal margin sensors
//
//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_1'
_REC_LEN    0040

   // Sensor Record Header
   0060               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   B0                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   EC                 // Normal Reading(ECh = -20 degrees C)
   00                 // Normal Maximum (00h = 0 degrees C)
   BA                 // Normal Minimum (BAh = -70 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degrees C)
   0A                 // Upper critical (0Ah = 10 degrees C)
   05                 // Upper non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degrees C)
   00                 // Lower critical (00h = 0 degrees C)
   00                 // Lower non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   D0                 // Type/Length Code
   'DIMM Thrm Mrgn 1' // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_1'
_REC_LEN    0040

   // Sensor Record Header
   0061               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   B1                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   EC                 // Normal Reading(ECh = -20 degrees C)
   00                 // Normal Maximum (00h = 0 degrees C)
   BA                 // Normal Minimum (BAh = -70 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degrees C)
   0A                 // Upper critical (0Ah = 10 degrees C)
   05                 // Upper non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degrees C)
   00                 // Lower critical (00h = 0 degrees C)
   00                 // Lower non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   D0                 // Type/Length Code
   'DIMM Thrm Mrgn 2' // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_2'
_REC_LEN    0040

   // Sensor Record Header
   0062               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   B2                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   EC                 // Normal Reading(ECh = -20 degrees C)
   00                 // Normal Maximum (00h = 0 degrees C)
   BA                 // Normal Minimum (BAh = -70 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degrees C)
   0A                 // Upper critical (0Ah = 10 degrees C)
   05                 // Upper non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degrees C)
   00                 // Lower critical (00h = 0 degrees C)
   00                 // Lower non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   D0                 // Type/Length Code
   'DIMM Thrm Mrgn 3' // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_2'
_REC_LEN    0040

   // Sensor Record Header
   0063               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   B3                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   EC                 // Normal Reading(ECh = -20 degrees C)
   00                 // Normal Maximum (00h = 0 degrees C)
   BA                 // Normal Minimum (BAh = -70 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degrees C)
   0A                 // Upper critical (0Ah = 10 degrees C)
   05                 // Upper non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degrees C)
   00                 // Lower critical (00h = 0 degrees C)
   00                 // Lower non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   D0                 // Type/Length Code
   'DIMM Thrm Mrgn 4' // String Bytes

//====================================================================//
//
// Memory thermal trip sensors
//
//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROC_1'
_REC_LEN    0030

   // Sensor Record Header
   0064               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   C0                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   0C                 // Sensor Type
   6F                 // Event / Reading Base Type
   0004               // Assertion Event Mask   --State asserted =0004
   0004               // Deassertion Event Mask --State asserted =0004
   0004               // Reading Mask & Settable / Readable Threshold Masks --State asserted =0004
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'Mem P1 Thrm Trip' // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROC_2'
_REC_LEN    0030

   // Sensor Record Header
   0065               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   C1                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   0C                 // Sensor Type
   6F                 // Event / Reading Base Type
   0004               // Assertion Event Mask   --State asserted =0004
   0004               // Deassertion Event Mask --State asserted =0004
   0004               // Reading Mask & Settable / Readable Threshold Masks --State asserted =0004
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'Mem P2 Thrm Trip' // String Bytes

//====================================================================//
//
// Global aggregate thermal margin sensors
//
//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'P4000_BASE'
_SDR_TAG    'P4000'
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    003E

   // Sensor Record Header
   0066               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   C8                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask   --[u][c,nc]=0000
   0000               // Deassertion Event Mask --[u][c,nc]=0000
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   EC                 // Normal Reading(ECh = -20 degrees C)
   00                 // Normal Maximum (00h = 0 degrees C)
   BA                 // Normal Minimum (BAh = -70 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degrees C)
   00                 // Upper critical (00h = 0 degrees C)
   00                 // Upper non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degrees C)
   00                 // Lower critical (00h = 0 degrees C)
   00                 // Lower non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CE                 // Type/Length Code
   'Agg Thrm Mgn 1'   // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'P4000_BASE'
_SDR_TAG    'P4000'
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    003E

   // Sensor Record Header
   0067               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   C9                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask   --[u][c,nc]=0000
   0000               // Deassertion Event Mask --[u][c,nc]=0000
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   EC                 // Normal Reading(ECh = -20 degrees C)
   00                 // Normal Maximum (00h = 0 degrees C)
   BA                 // Normal Minimum (BAh = -70 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degrees C)
   00                 // Upper critical (00h = 0 degrees C)
   00                 // Upper non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degrees C)
   00                 // Lower critical (00h = 0 degrees C)
   00                 // Lower non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CE                 // Type/Length Code
   'Agg Thrm Mgn 2'   // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'P4000'
_REC_LEN    003E

   // Sensor Record Header
   0068               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   CA                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask   --[u][c,nc]=0000
   0000               // Deassertion Event Mask --[u][c,nc]=0000
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   EC                 // Normal Reading(ECh = -20 degrees C)
   00                 // Normal Maximum (00h = 0 degrees C)
   BA                 // Normal Minimum (BAh = -70 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degrees C)
   00                 // Upper critical (00h = 0 degrees C)
   00                 // Upper non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degrees C)
   00                 // Lower critical (00h = 0 degrees C)
   00                 // Lower non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CE                 // Type/Length Code
   'Agg Thrm Mgn 3'   // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'P4000'
_REC_LEN    003E

   // Sensor Record Header
   0069               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   CB                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask   --[u][c,nc]=0000
   0000               // Deassertion Event Mask --[u][c,nc]=0000
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   EC                 // Normal Reading(ECh = -20 degrees C)
   00                 // Normal Maximum (00h = 0 degrees C)
   BA                 // Normal Minimum (BAh = -70 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degrees C)
   00                 // Upper critical (00h = 0 degrees C)
   00                 // Upper non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degrees C)
   00                 // Lower critical (00h = 0 degrees C)
   00                 // Lower non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CE                 // Type/Length Code
   'Agg Thrm Mgn 4'   // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'P4000'
_REC_LEN    003E

   // Sensor Record Header
   006A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   CC                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask   --[u][c,nc]=0000
   0000               // Deassertion Event Mask --[u][c,nc]=0000
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   EC                 // Normal Reading(ECh = -20 degrees C)
   00                 // Normal Maximum (00h = 0 degrees C)
   BA                 // Normal Minimum (BAh = -70 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degrees C)
   00                 // Upper critical (00h = 0 degrees C)
   00                 // Upper non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degrees C)
   00                 // Lower critical (00h = 0 degrees C)
   00                 // Lower non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CE                 // Type/Length Code
   'Agg Thrm Mgn 5'   // String Bytes

//====================================================================//
//
// Voltage regulator sensors
//
//====================================================================//
_SDR_TYPE   01
_REC_LEN    0039

   // Sensor Record Header
   006B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   34                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D0                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   34                 // M
   00                 // M, Tolerance
   1F                 // B
   40                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   D0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E0                 // Normal Reading (E0h = 11.94 Volt)
   EC                 // Normal Maximum (ECh = 12.56 Volt)
   D5                 // Normal Minimum (D5h = 11.36 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 13.55 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 13.39 Volt)
   F5                 // Upper non-critical (F5h = 13.03 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   C7                 // Lower critical (C7h = 10.64 Volt)
   CD                 // Lower non-critical (CDh = 10.95 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'BB +12.0V'          // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    0038

   // Sensor Record Header
   006C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D1                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   D9                 // M
   00                 // M, Tolerance
   62                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E1                 // Normal Reading (E1h = 4.98 Volt)
   ED                 // Normal Maximum (EDh = 5.24 Volt)
   D6                 // Normal Minimum (D6h = 4.74 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 5.63 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 5.57 Volt)
   F5                 // Upper non-critical (F5h = 5.41 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   C9                 // Lower critical (C9h = 4.46 Volt)
   CF                 // Lower non-critical (CFh = 4.59 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C8                 // Type/Length Code
   'BB +5.0V'         // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    0038

   // Sensor Record Header
   006D               // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D2                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   8F                 // M
   00                 // M, Tolerance
   F6                 // B
   40                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E2                 // Normal Reading (E2h = 3.28 Volt)
   EE                 // Normal Maximum (EEh = 3.45 Volt)
   D7                 // Normal Minimum (D7h = 3.12 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 3.70 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 3.65 Volt)
   F5                 // Upper non-critical (F5h = 3.55 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CB                 // Lower critical (CBh = 2.95 Volt)
   D1                 // Lower non-critical (D1h = 3.04 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C8                 // Type/Length Code
   'BB +3.3V'         // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    003D

   // Sensor Record Header
   006E               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D3                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   D9                 // M
   00                 // M, Tolerance
   62                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E1                 // Normal Reading (E1h = 4.98 Volt)
   ED                 // Normal Maximum (EDh = 5.24 Volt)
   D6                 // Normal Minimum (D6h = 4.74 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 5.63 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 5.57 Volt)
   F5                 // Upper non-critical (F5h = 5.41 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   C9                 // Lower critical (C9h = 4.46 Volt)
   CF                 // Lower non-critical (CFh = 4.59 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'BB +5.0V STBY'    // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    003C

   // Sensor Record Header
   006F               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D4                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1 (signed 2¡¦s complement)
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   8F                 // M (-139)
   00                 // M, Tolerance
   F6                 // B (-114)
   40                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp (-4), B exp (3)
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E2                 // Normal Reading (E2h = 3.28 Volt)
   EE                 // Normal Maximum (EEh = 3.45 Volt)
   D7                 // Normal Minimum (D7h = 3.12 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 3.70 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 3.65 Volt)
   F5                 // Upper non-critical (F5h = 3.55 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CB                 // Lower critical (CBh = 2.95 Volt)
   D1                 // Lower non-critical (D1h = 3.04 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM used for filtering [7:5]= 1 Median [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'BB +3.3V AUX'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_1'
_REC_LEN    0040

   // Sensor Record Header
   0070               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D6                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3B                 // M
   00                 // M, Tolerance
   55                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   CF                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   B1                 // Normal Reading (B1h = 1.05 Volt)
   EF                 // Normal Maximum (EFh = 1.41 Volt)
   73                 // Normal Minimum (73h = 0.68 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.51 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.49 Volt)
   F5                 // Upper non-critical (F5h = 1.45 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   6D                 // Lower critical (6Dh = 0.64 Volt)
   70                 // Lower non-critical (70h = 0.66 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.05V P1Vccp' // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_2'
_REC_LEN    0040

   // Sensor Record Header
   0071               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D7                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3B                 // M
   00                 // M, Tolerance
   55                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   CF                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   B1                 // Normal Reading (B1h = 1.05 Volt)
   EF                 // Normal Maximum (EFh = 1.41 Volt)
   73                 // Normal Minimum (73h = 0.68 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.51 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.49 Volt)
   F5                 // Upper non-critical (F5h = 1.45 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   6D                 // Lower critical (6Dh = 0.64 Volt)
   70                 // Lower non-critical (70h = 0.66 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.05V P2Vccp' // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_1'
_REC_LEN    0040

   // Sensor Record Header
   0072               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D8                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   44                 // M
   00                 // M, Tolerance
   C9                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E4                 // Normal Reading (E4h = 1.50 Volt)
   EF                 // Normal Maximum (EFh = 1.57 Volt)
   D9                 // Normal Minimum (D9h = 1.42 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.68 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.66 Volt)
   F5                 // Upper non-critical (F5h = 1.61 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CD                 // Lower critical (CDh = 1.34 Volt)
   D4                 // Lower non-critical (D4h = 1.39 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.5 P1DDR AB' // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_1'
_REC_LEN    0040

   // Sensor Record Header
   0073               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D9                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   44                 // M
   00                 // M, Tolerance
   C9                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E4                 // Normal Reading (E4h = 1.50 Volt)
   EF                 // Normal Maximum (EFh = 1.57 Volt)
   D9                 // Normal Minimum (D9h = 1.42 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.68 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.66 Volt)
   F5                 // Upper non-critical (F5h = 1.61 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CD                 // Lower critical (CDh = 1.34 Volt)
   D4                 // Lower non-critical (D4h = 1.39 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.5 P1DDR CD' // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_2'
_REC_LEN    0040

   // Sensor Record Header
   0074               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   DA                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   44                 // M
   00                 // M, Tolerance
   C9                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E4                 // Normal Reading (E4h = 1.50 Volt)
   EF                 // Normal Maximum (EFh = 1.57 Volt)
   D9                 // Normal Minimum (D9h = 1.42 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.68 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.66 Volt)
   F5                 // Upper non-critical (F5h = 1.61 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CD                 // Lower critical (CDh = 1.34 Volt)
   D4                 // Lower non-critical (D4h = 1.39 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.5 P2DDR AB' // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_2'
_REC_LEN    0040

   // Sensor Record Header
   0075               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   DB                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   44                 // M
   00                 // M, Tolerance
   C9                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E4                 // Normal Reading (E4h = 1.50 Volt)
   EF                 // Normal Maximum (EFh = 1.57 Volt)
   D9                 // Normal Minimum (D9h = 1.42 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.68 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.66 Volt)
   F5                 // Upper non-critical (F5h = 1.61 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CD                 // Lower critical (CDh = 1.34 Volt)
   D4                 // Lower non-critical (D4h = 1.39 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.5 P2DDR CD' // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    003C

   // Sensor Record Header
   0076               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   DC                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   53                 // M
   00                 // M, Tolerance
   7C                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E9                 // Normal Reading (E9h = 1.80 Volt)
   EF                 // Normal Maximum (EFh = 1.85 Volt)
   E2                 // Normal Minimum (E2h = 1.74 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.98 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.96 Volt)
   F5                 // Upper non-critical (F5h = 1.90 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   D6                 // Lower critical (D6h = 1.64 Volt)
   DD                 // Lower non-critical (DDh = 1.70 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CC                 // Type/Length Code
   'BB +1.8V AUX'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    003D

   // Sensor Record Header
   0077               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   DD                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   FF                 // M
   40                 // M, Tolerance
   86                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   B1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   DA                 // Normal Reading (DAh = 1.10 Volt)
   EF                 // Normal Maximum (EFh = 1.21 Volt)
   C4                 // Normal Minimum (C4h = 0.99 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.29 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.28 Volt)
   F5                 // Upper non-critical (F5h = 1.24 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   BA                 // Lower critical (BAh = 0.94 Volt)
   BF                 // Lower non-critical (BFh = 0.96 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CD                 // Type/Length Code
   'BB +1.1V STBY'    // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    0037

   // Sensor Record Header
   0078               // Record ID
   51                 // SDR Version
   01                 // Record Type
   32                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   DE                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   80                 // M
   00                 // M, Tolerance
   DF                 // B
   40                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E7                 // Normal Reading (E7h = 3.00 Volt)
   F3                 // Normal Maximum (F3h = 3.16 Volt)
   C4                 // Normal Minimum (C4h = 2.56 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 3.31 Volt)
   00                 // Sensor Minimum Reading (00h = 0.05 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0.05 Volt)
   A9                 // Lower critical (A9h = 2.21 Volt)
   C3                 // Lower non-critical (C3h = 2.54 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM used for filtering [7:5]= 1 Median [4:0]=5 Sample Count
   C7                 // Type/Length Code
   'BB VBAT'          // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_1'
_REC_LEN    0040

   // Sensor Record Header
   0079               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   E4                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3D                 // M
   00                 // M, Tolerance
   15                 // B
   80                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E4                 // Normal Reading (E4h = 1.34 Volt)
   EF                 // Normal Maximum (EFh = 1.41 Volt)
   D9                 // Normal Minimum (D9h = 1.27 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.51 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.49 Volt)
   F5                 // Upper non-critical (F5h = 1.45 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CD                 // Lower critical (CDh = 1.20 Volt)
   D4                 // Lower non-critical (D4h = 1.24 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.35 P1LV AB' // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_1'
_REC_LEN    0040

   // Sensor Record Header
   007A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   E5                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3D                 // M
   00                 // M, Tolerance
   15                 // B
   80                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E4                 // Normal Reading (E4h = 1.34 Volt)
   EF                 // Normal Maximum (EFh = 1.41 Volt)
   D9                 // Normal Minimum (D9h = 1.27 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.51 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.49 Volt)
   F5                 // Upper non-critical (F5h = 1.45 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CD                 // Lower critical (CDh = 1.20 Volt)
   D4                 // Lower non-critical (D4h = 1.24 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.35 P1LV CD' // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_2'
_REC_LEN    0040

   // Sensor Record Header
   007B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   E6                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3D                 // M
   00                 // M, Tolerance
   15                 // B
   80                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E4                 // Normal Reading (E4h = 1.34 Volt)
   EF                 // Normal Maximum (EFh = 1.41 Volt)
   D9                 // Normal Minimum (D9h = 1.27 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.51 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.49 Volt)
   F5                 // Upper non-critical (F5h = 1.45 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CD                 // Lower critical (CDh = 1.20 Volt)
   D4                 // Lower non-critical (D4h = 1.24 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.35 P2LV AB' // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_2'
_REC_LEN    0040

   // Sensor Record Header
   007C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   E7                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3D                 // M
   00                 // M, Tolerance
   15                 // B
   80                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E4                 // Normal Reading (E4h = 1.34 Volt)
   EF                 // Normal Maximum (EFh = 1.41 Volt)
   D9                 // Normal Minimum (D9h = 1.27 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.51 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.49 Volt)
   F5                 // Upper non-critical (F5h = 1.45 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CD                 // Lower critical (CDh = 1.20 Volt)
   D4                 // Lower non-critical (D4h = 1.24 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.35 P2LV CD' // String Bytes

//====================================================================//
//
// Hot-swap backplane (HSBP) sensors
//
//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_1_BP4'
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    002C

   // Sensor Record Header
   007D               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F0                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 0 Status'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_1_BP4'
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    002C

   // Sensor Record Header
   007E               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F1                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 1 Status'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_1_BP4'
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    002C

   // Sensor Record Header
   007F               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F2                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 2 Status'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_1_BP4'
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    002C

   // Sensor Record Header
   0080               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F3                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 3 Status'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    002C

   // Sensor Record Header
   0081               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F4                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 4 Status'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    002C

   // Sensor Record Header
   0082               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F5                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 5 Status'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    002C

   // Sensor Record Header
   0083               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F6                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 6 Status'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    002C

   // Sensor Record Header
   0084               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F7                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 7 Status'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_2_BP4'
_SDR_TAG    'HSBP_2_BP8'
_REC_LEN    002C

   // Sensor Record Header
   0085               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F8                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   02                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 8 Status'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_2_BP4'
_SDR_TAG    'HSBP_2_BP8'
_REC_LEN    002C

   // Sensor Record Header
   0086               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F9                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   02                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 9 Status'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_2_BP4'
_SDR_TAG    'HSBP_2_BP8'
_REC_LEN    002D

   // Sensor Record Header
   0087               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   FA                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   02                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 10 Status'    // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_2_BP4'
_SDR_TAG    'HSBP_2_BP8'
_REC_LEN    002D

   // Sensor Record Header
   0088               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   FB                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   02                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 11 Status'    // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_2_BP8'
_REC_LEN    002D

   // Sensor Record Header
   0089               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   FC                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   02                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 12 Status'    // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_2_BP8'
_REC_LEN    002D

   // Sensor Record Header
   008A               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   FD                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   02                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 13 Status'    // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_2_BP8'
_REC_LEN    002D

   // Sensor Record Header
   008B               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   FE                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   02                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 14 Status'    // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_2_BP8'
_REC_LEN    002D

   // Sensor Record Header
   008C               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   60                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   02                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 15 Status'    // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_3_BP4'
_SDR_TAG    'HSBP_3_BP8'
_REC_LEN    002D

   // Sensor Record Header
   008D               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   61                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   03                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 16 Status'    // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_3_BP4'
_SDR_TAG    'HSBP_3_BP8'
_REC_LEN    002D

   // Sensor Record Header
   008E               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   62                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   03                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 17 Status'    // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_3_BP4'
_SDR_TAG    'HSBP_3_BP8'
_REC_LEN    002D

   // Sensor Record Header
   008F               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   63                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   03                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 18 Status'    // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_3_BP4'
_SDR_TAG    'HSBP_3_BP8'
_REC_LEN    002D

   // Sensor Record Header
   0090               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   64                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   03                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 19 Status'    // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_3_BP8'
_REC_LEN    002D

   // Sensor Record Header
   0091               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   65                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   03                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 20 Status'    // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_3_BP8'
_REC_LEN    002D

   // Sensor Record Header
   0092               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   66                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   03                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 21 Status'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_3_BP8'
_REC_LEN    002D

   // Sensor Record Header
   0093               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   67                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   03                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 22 Status'    // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_3_BP8'
_REC_LEN    002D

   // Sensor Record Header
   0094               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   68                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   03                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 23 Status'     // String Bytes

//====================================================================//
// Management Engine (ME controller) records
//====================================================================//
_SDR_TYPE   03
_REC_LEN    001E

   // Sensor Record Header
   0095               // Record ID
   51                 // SDR Version
   03                 // Record Type
   19                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   17                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   01                 // Entity Instance
   DC                 // Sensor type
   75                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'SPS FW Health'    // String Bytes
   
//====================================================================//
_SDR_TYPE   03
_REC_LEN    001D

   // Sensor Record Header
   0096               // Record ID
   51                 // SDR Version
   03                 // Record Type
   18                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   18                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   01                 // Entity Instance
   DC                 // Sensor type
   72                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'NM Exception'     // String Bytes

//====================================================================//
_SDR_TYPE   03
_REC_LEN    001A

   // Sensor Record Header
   0097               // Record ID
   51                 // SDR Version
   03                 // Record Type
   15                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   19                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   01                 // Entity Instance
   DC                 // Sensor type
   73                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'NM Health'        // String Bytes

//====================================================================//
_SDR_TYPE   02
_REC_LEN    002F

   // Sensor Record Header
   0098               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   1A                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   01                 // Entity Instance
   41                 // Sensor Initialization
   C3                 // Sensor Capabilities
   DC                 // Sensor Type
   74                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0700               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0000               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'NM Capabilities'  // String Bytes

//====================================================================//
_SDR_TYPE   03
_REC_LEN    001D

   // Sensor Record Header
   0099               // Record ID
   51                 // SDR Version
   03                 // Record Type
   18                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Channel Number / Sensor Owner LUN
   1B                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   01                 // Entity Instance
   DC                 // Sensor Type
   72                 // Event / Reading Base Type
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'NM Threshold'     // String Bytes
   
//====================================================================//
// FSC Record Type = 0Dh (NM discovery)
//====================================================================//
_SDR_TYPE      C0
_REC_LEN       0010

   // Sensor Record Header
   009A               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0B                 // Record Length

   // Record Body Bytes
   570100          // Manufacturer ID
   0D                 // Record subtype - NM Discovery
   01                 // Version number of record subtype
   2C                 // NM Device Slave Address ([7:1] - 7-bit address; [0] - reserved)
   60                 // [7:4] - channel number (6 for secondary IPMB) [3:2] - reserved [1:0] - sensor owner LUN)
   19                 // Node Manager Health Event sensor
   18                 // Node Manager Exception Event sensor
   1A                 // Node Manager Operational Capabilities sensor
   1B                 // Node Manager Threshold Exceeded sensor

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_1'
_REC_LEN    0036

   // Sensor Record Header
   009B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   31                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   34                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   63                 // Sensor Initialization
   B8                 // Sensor Capabilities
   0C                 // Sensor Type -- Memory
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask   --[u][c,nc]=0000
   0000               // Deassertion Event Mask --[u][c,nc]=0000
   3F3F               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=3F3F
   01                 // Sensor Units 1
   00                 // Sensor Units 2 -- Degrees C
   00                 // Sensor Units 3
   00                 // Linearization
   05                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   F0                 // R exp, B exp
   00                 // Analog characteristic flags
   //------------------------------------------------------------------//
   00                 // Normal Reading
   00                 // Normal Maximum
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   00                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical
   00                 // Upper non-critical
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C6                 // Type/Length Code
   'P1 MTT'         // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_2'
_REC_LEN    0036

   // Sensor Record Header
   009C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   31                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   35                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   02                 // Entity Instance
   63                 // Sensor Initialization
   B8                 // Sensor Capabilities
   0C                 // Sensor Type -- Memory
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask   --[u][c,nc]=0000
   0000               // Deassertion Event Mask --[u][c,nc]=0000
   3F3F               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=3F3F
   01                 // Sensor Units 1
   00                 // Sensor Units 2 -- Degrees C
   00                 // Sensor Units 3
   00                 // Linearization
   05                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   F0                 // R exp, B exp
   00                 // Analog characteristic flags
   //------------------------------------------------------------------//
   00                 // Normal Reading
   00                 // Normal Maximum
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   00                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical
   00                 // Upper non-critical
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C6                 // Type/Length Code
   'P2 MTT'         // String Bytes
   
//====================================================================//
// BIOS owned sensor records
//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   009D               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   01                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   01                 // Entity Instance
   0C                 // Sensor Type
   0B                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mem Rdnc Sensor'  // Memory Redundancy State

//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   009E               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   02                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID = Memory
   01                 // Entity Instance
   0C                 // Sensor Type
   09                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mem Conf Sensor'  // Memory configuration failed
   
//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   009F               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   02                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID = Memory Device
   02                 // Entity Instance
   0C                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mmry ECC Sensor'   // Memory ECC Error Sensor

//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   00A0               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   03                 // Sensor Number

   // Record Body Bytes
   30                 // Entity ID = PCI
   01                 // Entity Instance
   13                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCI Lgcy Sensor'   // Legacy PCI Sensor

//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   00A1               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   04                 // Sensor Number

   // Record Body Bytes
   31                 // Entity ID = PCI Express
   01                 // Entity Instance
   13                 // Sensor Type
   70                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCIe Fat Sensor'  // PCI Express Fatal Error Sensor

//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   00A2               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   05                 // Sensor Number

   // Record Body Bytes
   31                 // Entity ID = PCI Express
   02                 // Entity Instance
   13                 // Sensor Type
   71                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCIe Cor Sensor'  // PCI Express Correctable Error Sensor

//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   00A3               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   06                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID-BIOS POST
   02                 // Entity Instance
   0F                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'POST Err Sensor'  // POST Error Sensor
   
//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   00A4               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   06                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID
   03                 // Entity Instance
   13                 // Sensor Type
   72                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'QPI Corr Sensor'  // QPI Correctable Event Sensor

//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   00A5               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   07                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID
   04                 // Entity Instance
   13                 // Sensor Type
   73                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'QPI Fatl Sensor'   //  QPI Fatal/Uncorrectable Errors
   
//====================================================================//
_SDR_TYPE   03
_REC_LEN    001F

   // Sensor Record Header
   00A6               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1A                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   08                 // Sensor Number

   // Record Body Bytes
   31                 // Entity ID = PCI Express
   03                 // Entity Instance
   19                 // Sensor Type
   75                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Chipset Sensor'   // Chipset Proprietary Errors

//====================================================================//
_SDR_TYPE   03
_REC_LEN    001F

   // Sensor Record Header
   00A7               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1A                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   09                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID
   05                 // Entity Instance
   13                 // Sensor Type
   77                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'QPI Link Width'   // QPI Link Width Reduced

//====================================================================//
_SDR_TYPE   03
_REC_LEN    001F

   // Sensor Record Header
   00A8               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1A                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   10                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID = Memory Device
   03                 // Entity Instance
   0C                 // Sensor Type
   7F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Mem err Sensor'   //Memory Error Extension

//====================================================================//
_SDR_TYPE   03
_REC_LEN    001D

   // Sensor Record Header
   00A9               // Record ID
   51                 // SDR Version
   03                 // Record Type
   18                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   11                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   06                 // Entity Instance
   0C                 // Sensor Type
   0B                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'Sparing Rdnc'     // Sparing Redundancy State

//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   00AA               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   12                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   07                 // Entity Instance
   0C                 // Sensor Type
   09                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Rdnc Mod Sensor'  // Memory Redundancy Configuration

//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   00AB               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   13                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID = Memory Device
   04                 // Entity Instance
   0C                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mmry Parity Err'  // Memory Parity Error

//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   00AC               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   14                 // Sensor Number

   // Record Body Bytes
   31                 // Entity ID = PCI Express
   04                 // Entity Instance
   13                 // Sensor Type
   76                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCIe Fat Sensor'  // PCI Express Fatal Error Sensor

//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   00AD               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   17                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID
   08                 // Entity Instance
   13                 // Sensor Type
   74                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'QPI Fatl Sensor'  // QPI Fatal/Uncorrectable Errors

//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   00AE               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   83                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   09                 // Entity Instance
   12                 // Sensor Type
   6F                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'BIOS Evt Sensor'  // BIOS Boot Event Sensor

//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   00AF               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   83                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   0A                 // Entity Instance
   12                 // Sensor Type
   6F                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'BIOS Evt Sensor'  // BIOS Boot Event Sensor

//====================================================================//
// SDR Type 11 Records
//====================================================================//
_SDR_TYPE   11
_REC_LEN    0019

   // Sensor Record Header
   00B0               // Record ID
   51                 // SDR Version
   11                 // Record Type
   14                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   00                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   07                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // OEM
   C9                 // Type/Length Code
   'Baseboard'        // String Bytes

//====================================================================//
_SDR_TYPE   11
_REC_LEN    001B

   // Sensor Record Header
   00B1               // Record ID
   51                 // SDR Version
   11                 // Record Type
   16                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   04                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   0C                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // OEM
   CB                 // Type/Length Code
   'front panel'      // String Bytes

//====================================================================//
_SDR_TYPE   11
_SDR_TAG    '460_PS1'
_SDR_TAG    '750_PS1'
_SDR_TAG    '1200_PS1'
_REC_LEN    0020
 
   // Sensor Record Header
   00B2               // Record ID
   51                 // SDR Version
   11                 // Record Type
   1B                 // Record Length
   
   // Record Key Bytes
   20                 // Device Access Address
   02                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number
   
   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   0A                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // Reserved for OEM use
   D0                 // Type/Length Code
   'Pwr Supply 1 FRU' // String Bytes

//====================================================================//
_SDR_TYPE   11
_SDR_TAG    '460_PS2'
_SDR_TAG    '750_PS2'
_SDR_TAG    '1200_PS2'
_REC_LEN    0020

   // Sensor Record Header
   00B3               // Record ID
   51                 // SDR Version
   11                 // Record Type
   1B                 // Record Length
   
   // Record Key Bytes
   20                 // Device Access Address
   03                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number
   
   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   0A                 // FRU Entity ID
   02                 // FRU Entity Instance
   00                 // Reserved for OEM use
   D0                 // Type/Length Code
   'Pwr Supply 2 FRU' // String Bytes

//====================================================================//
_SDR_TYPE   11
_SDR_TAG    'HSBP_1_BP4'
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    001E

   // Sensor Record Header
   00B4               // Record ID
   51                 // SDR Version
   11                 // Record Type
   19                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   05                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   0F                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // OEM
   CE                 // Type/Length Code
   'HS Backplane 1'   // String Bytes

//====================================================================//
_SDR_TYPE   11
_SDR_TAG    'HSBP_2_BP4'
_SDR_TAG    'HSBP_2_BP8'
_REC_LEN    001E

   // Sensor Record Header
   00B5               // Record ID
   51                 // SDR Version
   11                 // Record Type
   19                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   06                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   0F                 // FRU Entity ID
   02                 // FRU Entity Instance
   00                 // OEM
   CE                 // Type/Length Code
   'HS Backplane 2'   // String Bytes

//====================================================================//
_SDR_TYPE   11
_SDR_TAG    'HSBP_3_BP4'
_SDR_TAG    'HSBP_3_BP8'
_REC_LEN    001E

   // Sensor Record Header
   00B6               // Record ID
   51                 // SDR Version
   11                 // Record Type
   19                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   07                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   0F                 // FRU Entity ID
   03                 // FRU Entity Instance
   00                 // OEM
   CE                 // Type/Length Code
   'HS Backplane 3'   // String Bytes

//====================================================================//
// SDR Type 12 Records
//====================================================================//
_SDR_TYPE   12
_REC_LEN    0020

   // Sensor Record Header
   00B7               // Record ID
   51                 // SDR Version
   12                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   20                 // Device Slave Address
   00                 // Channel Number

   // Record Body Bytes
   08                 // Power state notification
   BF                 // Device capabilities
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   07                 // Entity ID
   01                 // Entity instance
   00                 // OEM
   D0                 // Type/Length Code
   'Basbrd Mgmt Ctlr' // String Bytes

//====================================================================//
_SDR_TYPE   12
_REC_LEN    0012

   // Sensor Record Header
   00B8               // Record ID
   51                 // SDR Version
   12                 // Record Type
   0D                 // Record Length

   // Record Key Bytes
   2C                 // Device Slave Address
   06                 // Channel number

   // Record Body Bytes
   24                 // Power State Notification
   21                 // Device Capabilities
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   2E                 // Entity ID
   01                 // Entity Instance
   00                 // OEM
   C2                 // Type/Length Code
   'ME'               // String Bytes


//====================================================================//
// Thermal Profile Data, Close Loop
//====================================================================//

//====================================================================//
//
// SDR Type C0/02 Record For Power Unit Map
//
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'PS_REDUNDANCY'
_REC_LEN    000E

   // Sensor Record Header
   00B9               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   09                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   02                 // Record Subtype Value
   02                 // Power Unit Redundancy sensor number
   00                 // Bits [7:1]-Reserved; Bit[0]-1=No monitorable supplies present
   01                 // The number of present and operational
   50                 // Power Supply Status 1 Sensor Number
   51                 // Power Supply Status 2 Sensor Number

//====================================================================//
//
// SDR Type C0/05 Record For Fan Redundancy Map SDR Record
//
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0018

   // Sensor Record Header
   00BA               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   13                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   05                 // Record Subtype Value*******   Fan Redundancy Map SDR Record   **********

   // Fan Redundancy Map Record
   0C                 // Fan Redundancy Sensor Number
   00                 // Flags; [7:1]-Reserved; [0]-persistently stored event state, 1= store this event state persistently
   0404               // Failed Event State Mask
   01                 // Redundant Fan Count
   30                 // System Fan 1 Speed Sensor
   40                 // System Fan 1 Presence Sensor
   31                 // System Fan 2 Speed Sensor
   41                 // System Fan 2 Presence Sensor
   32                 // System Fan 3 Speed Sensor
   42                 // System Fan 3 Presence Sensor
   33                 // System Fan 4 Speed Sensor
   43                 // System Fan 4 Presense Sensor
   34                 // System Fan 5 Speed Sensor
   44                 // System Fan 5 Presense Sensor

//====================================================================//
//
// SDR Type C0/05 Records For Fan Redundancy Map SDR Record
//
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'FCT'
_SDR_TAG    'FCT2'
_REC_LEN    001A

   // Sensor Record Header
   00BB               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   05                 // Record Subtype Value*******   Fan Redundancy Map SDR Record   **********

   // Fan Redundancy Map Record
   0C                 // Fan Redundancy Sensor Number
   00                 // Flags; [7:1]-Reserved; [0]-persistently stored event state, 1= store this event state persistently
   0404               // Failed Event State Mask
   01                 // Redundant Fan Count
   30                 // System Fan 1 Speed Sensor
   40                 // System Fan 1 Presence Sensor
   31                 // System Fan 2 Speed Sensor
   41                 // System Fan 2 Presence Sensor
   32                 // System Fan 3 Speed Sensor
   42                 // System Fan 3 Presence Sensor
   33                 // System Fan 4 Speed Sensor
   43                 // System Fan 4 Presense Sensor
   34                 // System Fan 5 Speed Sensor
   44                 // System Fan 5 Presense Sensor
   35                 // System Fan 6 Speed Sensor
   45                 // System Fan 6 Presense Sensor

//====================================================================//
//
// SDR Type C0/05 Records For Fan Redundancy Map SDR Record
//
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'FAN_REDUN_FLAG'
_REC_LEN    001A

   // Sensor Record Header
   00BC               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   15                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   05                 // Record Subtype Value*******   Fan Redundancy Map SDR Record   **********

   // Fan Redundancy Map Record
   0C                 // Fan Redundancy Sensor Number
   00                 // Flags; [7:1]-Reserved; [0]-persistently stored event state, 1= store this event state persistently
   0404               // Failed Event State Mask
   01                 // Redundant Fan Count
   30                 // System Fan 1 Speed Sensor
   00                 // System Fan 1 Presence Sensor
   31                 // System Fan 2 Speed Sensor
   00                 // System Fan 2 Presence Sensor
   32                 // System Fan 3 Speed Sensor
   00                 // System Fan 3 Presence Sensor
   33                 // System Fan 4 Speed Sensor
   00                 // System Fan 4 Presense Sensor
   34                 // System Fan 5 Speed Sensor
   00                 // System Fan 5 Presense Sensor
   35                 // System Fan 6 Speed Sensor
   00                 // System Fan 6 Presense Sensor

//====================================================================//
//
// SDR Type C0/09 Records For Voltage Sensor Scaling
//
//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0034

   // Sensor Record Header
   00BD               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   2F                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   09                 // Record sub-type - Voltage Sensor Scaling

   // Voltage Sensor Scaling Record
   0E                 // Number of entries following
   D0                 // Voltage Sensor Number
   B80A               // Scale Factor (LSB MSB)
   D1                 // Voltage Sensor Number
   9D0A               // Scale Factor (LSB MSB)
   D2                 // Voltage Sensor Number
   980A               // Scale Factor (LSB MSB)
   D3                 // Voltage Sensor Number
   9D0A               // Scale Factor (LSB MSB)
   D4                 // Voltage Sensor Number
   980A               // Scale Factor (LSB MSB)
   D6                 // Voltage Sensor Number
   1A10               // Scale Factor (LSB MSB)
   D7                 // Voltage Sensor Number
   1A10               // Scale Factor (LSB MSB)
   D8                 // Voltage Sensor Number
   7F0E               // Scale Factor (LSB MSB)
   D9                 // Voltage Sensor Number
   7F0E               // Scale Factor (LSB MSB)
   DA                 // Voltage Sensor Number
   7F0E               // Scale Factor (LSB MSB)
   DB                 // Voltage Sensor Number
   7F0E               // Scale Factor (LSB MSB)
   DC                 // Voltage Sensor Number
   510C               // Scale Factor (LSB MSB)
   DD                 // Voltage Sensor Number
   DB12               // Scale Factor (LSB MSB)
   DE                 // Voltage Sensor Number
   CA09               // Scale Factor (LSB MSB)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0016

   // Sensor Record Header
   00BE               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   11                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   09                 // Record sub-type - Voltage Sensor Scaling

   // Voltage Sensor Scaling Record
   04                 // Number of entries following
   E4                 // Voltage Sensor Number
   1A10               // Scale Factor (LSB MSB)
   E5                 // Voltage Sensor Number
   1A10               // Scale Factor (LSB MSB)
   E6                 // Voltage Sensor Number
   1A10               // Scale Factor (LSB MSB)
   E7                 // Voltage Sensor Number
   1A10               // Scale Factor (LSB MSB)

//====================================================================//
//
// SDR Type C0/0A Records For Fan Sensor Scaling SDR Record
//
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_REC_LEN    001D

   // Sensor Record Header
   00BF               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   18                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record Subtype Value*******   Fan Sensor Scaling SDR Record   **********

   // Fan Sensor Scaling Record
   00                 // Return Format; Bit 0=Fan 0, Bit 1=Fan 1; etc. 0=RPM, 1=Period(***TBD***)
   00                 // Number of tach Pulses Per Revolution: Bit 0=Fan 0, Bit 1=Fan 1, etc.; 0=2 Pulses/Rev, 1=1 Pulse/Rev(***TBD***)
   740E               // Placeholder for System Fan 1(SN:0x30), Max RPM: 3700RPM == 740E (the order is LSB, MSB)
   B414               // Placeholder for System Fan 2(SN:0x31), Max RPM: 5300RPM == B414 (the order is LSB, MSB)
   0001               // Null(SN:0x32)
   0001               // Null(SN:0x33)
   0001               // Null(SN:0x34)
   0001               // Null(SN:0x35)
   0001               // Null(SN:0x36)
   0001               // Null(SN:0x37)
   0001               // Null(SN:0x38)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001D

   // Sensor Record Header
   00C0               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   18                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record Subtype Value*******   Fan Sensor Scaling SDR Record   **********

   // Fan Sensor Scaling Record
   00                 // Return Format; Bit 0=Fan 0, Bit 1=Fan 1; etc. 0=RPM, 1=Period(***TBD***)
   00                 // Number of tach Pulses Per Revolution: Bit 0=Fan 0, Bit 1=Fan 1, etc.; 0=2 Pulses/Rev, 1=1 Pulse/Rev(***TBD***)
   3421               // Placeholder for System Fan 1(SN:0x30), Max RPM: 8500RPM == 3421 (the order is LSB, MSB)
   3421               // Placeholder for System Fan 2(SN:0x31), Max RPM: 8500RPM == 3421 (the order is LSB, MSB)
   3421               // Placeholder for System Fan 3(SN:0x32), Max RPM: 8500RPM == 3421 (the order is LSB, MSB)
   3421               // Placeholder for System Fan 4(SN:0x33), Max RPM: 8500RPM == 3421 (the order is LSB, MSB)
   3421               // Placeholder for System Fan 5(SN:0x34), Max RPM: 8500RPM == 3421 (the order is LSB, MSB)
   0001               // Null(SN:0x35)
   0001               // Null(SN:0x36)
   0001               // Null(SN:0x37)
   0001               // Null(SN:0x38)
   
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    001D

   // Sensor Record Header
   00C1               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   18                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record Subtype Value*******   Fan Sensor Scaling SDR Record   **********

   // Fan Sensor Scaling Record
   00                 // Return Format; Bit 0=Fan 0, Bit 1=Fan 1; etc. 0=RPM, 1=Period(***TBD***)
   00                 // Number of tach Pulses Per Revolution: Bit 0=Fan 0, Bit 1=Fan 1, etc.; 0=2 Pulses/Rev, 1=1 Pulse/Rev(***TBD***)
   740E               // Placeholder for System Fan 1(SN:0x30), Max RPM: 3700RPM == 740E (the order is LSB, MSB)
   B414               // Placeholder for System Fan 2(SN:0x31), Max RPM: 5300RPM == B414 (the order is LSB, MSB)
   0001               // Null(SN:0x32)
   0001               // Null(SN:0x33)
   0001               // Null(SN:0x34)
   0001               // Null(SN:0x35)
   A861               // Placeholder for Processor Fan 1(SN:0x36), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for Processor Fan 2(SN:0x37), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   0001               // Null(SN:0x38)
   
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    001D

   // Sensor Record Header
   00C2               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   18                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record Subtype Value*******   Fan Sensor Scaling SDR Record   **********

   // Fan Sensor Scaling Record
   00                 // Return Format; Bit 0=Fan 0, Bit 1=Fan 1; etc. 0=RPM, 1=Period(***TBD***)
   00                 // Number of tach Pulses Per Revolution: Bit 0=Fan 0, Bit 1=Fan 1, etc.; 0=2 Pulses/Rev, 1=1 Pulse/Rev(***TBD***)
   A861               // Placeholder for System Fan 1(SN:0x30), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 2(SN:0x31), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 3(SN:0x32), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 4(SN:0x33), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 5(SN:0x34), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 6(SN:0x35), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for Processor Fan 1(SN:0x36), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for Processor Fan 2(SN:0x37), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for rear Fan(SN:0x38), Max RPM: 25000RPM == A861 (the order is LSB, MSB)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'FCT'
_REC_LEN    001D

   // Sensor Record Header
   00C3               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   18                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record Subtype Value*******   Fan Sensor Scaling SDR Record   **********

   // Fan Sensor Scaling Record
   00                 // Return Format; Bit 0=Fan 0, Bit 1=Fan 1; etc. 0=RPM, 1=Period(***TBD***)
   00                 // Number of tach Pulses Per Revolution: Bit 0=Fan 0, Bit 1=Fan 1, etc.; 0=2 Pulses/Rev, 1=1 Pulse/Rev(***TBD***)
   3421               // Placeholder for System Fan 1(SN:0x30), Max RPM: 8500RPM == 3421 (the order is LSB, MSB)
   3421               // Placeholder for System Fan 2(SN:0x31), Max RPM: 8500RPM == 3421 (the order is LSB, MSB)
   3421               // Placeholder for System Fan 3(SN:0x32), Max RPM: 8500RPM == 3421 (the order is LSB, MSB)
   3421               // Placeholder for System Fan 4(SN:0x33), Max RPM: 8500RPM == 3421 (the order is LSB, MSB)
   3421               // Placeholder for System Fan 5(SN:0x34), Max RPM: 8500RPM == 3421 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 6(SN:0x35), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for Processor Fan 1(SN:0x36), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for Processor Fan 2(SN:0x37), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for rear Fan(SN:0x38), Max RPM: 25000RPM == A861 (the order is LSB, MSB)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'FCT2'
_REC_LEN    001D

   // Sensor Record Header
   00C4               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   18                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record Subtype Value*******   Fan Sensor Scaling SDR Record   **********

   // Fan Sensor Scaling Record
   00                 // Return Format; Bit 0=Fan 0, Bit 1=Fan 1; etc. 0=RPM, 1=Period(***TBD***)
   00                 // Number of tach Pulses Per Revolution: Bit 0=Fan 0, Bit 1=Fan 1, etc.; 0=2 Pulses/Rev, 1=1 Pulse/Rev(***TBD***)
   3421               // Placeholder for System Fan 1(SN:0x30), Max RPM: 8500RPM == 3421 (the order is LSB, MSB)
   3421               // Placeholder for System Fan 2(SN:0x31), Max RPM: 8500RPM == 3421 (the order is LSB, MSB)
   3421               // Placeholder for System Fan 3(SN:0x32), Max RPM: 8500RPM == 3421 (the order is LSB, MSB)
   3421               // Placeholder for System Fan 4(SN:0x33), Max RPM: 8500RPM == 3421 (the order is LSB, MSB)
   3421               // Placeholder for System Fan 5(SN:0x34), Max RPM: 8500RPM == 3421 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 6(SN:0x35), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for Processor Fan 1(SN:0x36), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   0001               // Null(SN:0x37)
   A861               // Placeholder for rear Fan(SN:0x38), Max RPM: 25000RPM == A861 (the order is LSB, MSB)

//====================================================================//
// Global Stepwise and Global Clamp Headers
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_SDR_TAG    'P4000_ACTIVE'
_SDR_TAG    'P4000'
_REC_LEN    0017

   // Sensor Record Header
   00C5           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   74             // Clamp Header ID
   74             // Temperature Sensor Number -- (P1 Therm Margin)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   FC             // Temperature (FCh = -4 degree C)
   01             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'PROC_2'
_REC_LEN    0017

   // Sensor Record Header
   00C6           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   75             // Clamp Header ID
   75             // Temperature Sensor Number -- (P2 Therm Margin)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   FC             // Temperature (FCh = -4 degree C)
   11             // Clamp Flags [7:4] - CPU Number = 1; [3:1] - Reserved=0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_SDR_TAG    'P4000_ACTIVE'
_SDR_TAG    'P4000'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00C7           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   B0             // Clamp Header ID
   B0             // Temperature Sensor Number -- (DIMM Thrm Mrgn 1)
   00             // Entity Presence Sensor Number -- (NA)
   00             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   F8             // Temperature (F8h = -8 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_SDR_TAG    'P4000_ACTIVE'
_SDR_TAG    'P4000'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00C8           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   B1             // Clamp Header ID
   B1             // Temperature Sensor Number -- (DIMM Thrm Mrgn 2)
   00             // Entity Presence Sensor Number -- (NA)
   00             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   F8             // Temperature (F8h = -8 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'PROC_2'
_REC_LEN    0017

   // Sensor Record Header
   00C9           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   B2             // Clamp Header ID
   B2             // Temperature Sensor Number -- (DIMM Thrm Mrgn 3)
   00             // Entity Presence Sensor Number -- (NA)
   00             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   F8             // Temperature (F8h = -8 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'PROC_2'
_REC_LEN    0017

   // Sensor Record Header
   00CA           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   B3             // Clamp Header ID
   B3             // Temperature Sensor Number -- (DIMM Thrm Mrgn 4)
   00             // Entity Presence Sensor Number -- (NA)
   00             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   F8             // Temperature (F8h = -8 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_SDR_TAG    'P4000_ACTIVE'
_SDR_TAG    'P4000'
_REC_LEN    0017

   // Sensor Record Header
   00CB           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   20             // Clamp Header ID
   20             // Temperature Sensor Number -- (BB EDGE Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   28             // Temperature (28h = 40 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_SDR_TAG    'P4000_ACTIVE'
_SDR_TAG    'P4000'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00CC           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   24             // Clamp Header ID
   24             // Temperature Sensor Number -- (BB CPU1 VR Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   55             // Temperature (55h = 85 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_SDR_TAG    'P4000_ACTIVE'
_SDR_TAG    'P4000'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00CD           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   23             // Clamp Header ID
   23             // Temperature Sensor Number -- (BB BMC Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   5C             // Temperature (5Ch = 92 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_SDR_TAG    'P4000_ACTIVE'
_SDR_TAG    'P4000'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00CE           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   25             // Clamp Header ID
   25             // Temperature Sensor Number -- (BB MEM VR Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   64             // Temperature (64h = 100 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_SDR_TAG    'P4000_ACTIVE'
_SDR_TAG    'P4000'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00CF           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   2F             // Clamp Header ID
   2F             // Temperature Sensor Number -- (LAN NIC Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   69             // Temperature (69h = 105 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_SDR_TAG    'P4000_ACTIVE'
_SDR_TAG    'P4000'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00D0           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   22             // Clamp Header ID
   22             // Temperature Sensor Number -- (SSB Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   53             // Temperature (53h = 83 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'HSBP_1_BP4'
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    0017

   // Sensor Record Header
   00D1           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   29             // Clamp Header ID
   29             // Temperature Sensor Number -- (HSBP 1 Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   5A             // Temperature (5Ah = 90 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'HSBP_2_BP4'
_SDR_TAG    'HSBP_2_BP8'
_REC_LEN    0017

   // Sensor Record Header
   00D2           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   2A             // Clamp Header ID
   2A             // Temperature Sensor Number -- (HSBP 2 Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   5A             // Temperature (5Ah = 90 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'HSBP_3_BP4'
_SDR_TAG    'HSBP_3_BP8'
_REC_LEN    0017

   // Sensor Record Header
   00D3           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   2B             // Clamp Header ID
   2B             // Temperature Sensor Number -- (HSBP 3 Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   5A             // Temperature (5Ah = 90 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_SDR_TAG    'P4000_ACTIVE'
_SDR_TAG    'P4000'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00D4           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   83             // Clamp Header ID
   83             // Temperature Sensor Number -- (P1 DTS Therm Mgn)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   FA             // Temperature (FAh = -6 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (Use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'PROC_2'
_REC_LEN    0017

   // Sensor Record Header
   00D5           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   84             // Clamp Header ID
   84             // Temperature Sensor Number -- (P2 DTS Therm Mgn)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   FA             // Temperature (FAh = -6 degree C)
   10             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (Use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'EATEMP'
_REC_LEN    0017

   // Sensor Record Header
   00D6           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   2E             // Clamp Header ID
   2E             // Temperature Sensor Number -- (Exit Air Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   44             // Temperature (44h = 68 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)
   
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '460_PS1'
_SDR_TAG    '750_PS1'
_SDR_TAG    '1200_PS1'
_REC_LEN    0017

   // Sensor Record Header
   00D7           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   5C             // Clamp Header ID
   5C             // Temperature Sensor Number -- (PS1 Temperature)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   2D             // Temperature (2Dh = 45 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)
   
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '460_PS2'
_SDR_TAG    '750_PS2'
_SDR_TAG    '1200_PS2'
_REC_LEN    0017

   // Sensor Record Header
   00D8           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   5D             // Clamp Header ID
   5D             // Temperature Sensor Number -- (PS1 Temperature)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   2D             // Temperature (2Dh = 45 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)
   
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_SDR_TAG    'P4000_ACTIVE'
_SDR_TAG    'P4000'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00D9           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   94             // Clamp Header ID
   74             // Temperature Sensor Number -- (P1 Therm Margin)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   F9             // Temperature (F9h = -7 degree C)
   01             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 1 (use TControl)
   
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'PROC_2'
_REC_LEN    0017

   // Sensor Record Header
   00DA           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   95             // Clamp Header ID
   75             // Temperature Sensor Number -- (P1 Therm Margin)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   F9             // Temperature (F9h = -7 degree C)
   11             // Clamp Flags [7:4] - CPU Number = 1; [3:1] - Reserved=0; [0] - Temp Source = 1 (use TControl)
   
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_SDR_TAG    'P4000_ACTIVE'
_SDR_TAG    'P4000'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00DB           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   64             // Clamp Header ID
   74             // Temperature Sensor Number -- (P1 Therm Margin)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   20             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   F8             // Temperature (F8h = -8 degree C)
   01             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 1 (use TControl)
   
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'PROC_2'
_REC_LEN    0017

   // Sensor Record Header
   00DC           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   65             // Clamp Header ID
   75             // Temperature Sensor Number -- (P1 Therm Margin)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   20             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   F8             // Temperature (F8h = -8 degree C)
   11             // Clamp Flags [7:4] - CPU Number = 1; [3:1] - Reserved=0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
// Global Stepwise Header Record
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_SDR_TAG    'P4000_ACTIVE'
_SDR_TAG    'P4000'
_REC_LEN    0013

   // Sensor Record Header
   00DD           // Record ID
   51             // SDR Version
   C0             // Record Type
   0E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   01             // FSC Record Type (01h = Global Stepwise Header Records)

   // Global Stepwise Header Record
   00             // Stepwise Header ID
   21             // Temperature Sensor Number -- (Front Panel Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   50             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 2; [2:0]-Positive Hysteresis = 0

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0013

   // Sensor Record Header
   00DE           // Record ID
   51             // SDR Version
   C0             // Record Type
   0E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   01             // FSC Record Type (01h = Global Stepwise Header Records)

   // Global Stepwise Header Record
   01             // Stepwise Header ID
   20             // Temperature Sensor Number -- (BB EDGE Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   50             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 2; [2:0]-Positive Hysteresis = 0
   
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    0013

   // Sensor Record Header
   00DF           // Record ID
   51             // SDR Version
   C0             // Record Type
   0E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   11             // FSC Record Type ([7:5] Reserved. Value 0h; [4] 0 = Byte 7 is sensor number. 1= Byte 7 is domain mask ; [3:0] Value 01h = Global Stepwise Header Records)

   // Global Stepwise Header Record
   02             // Stepwise Header ID
   02             // Domain mask  -- (Domain 1)
   00             // Entity Presence Sensor Number -- (NA)
   00             // Sensor Disabled Control Value
   00             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   00             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 0; [2:0]-Positive Hysteresis = 0

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0013

   // Sensor Record Header
   00E0           // Record ID
   51             // SDR Version
   C0             // Record Type
   0E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   11             // FSC Record Type ([7:5] Reserved. Value 0h; [4] 0 = Byte 7 is sensor number. 1= Byte 7 is domain mask ; [3:0] Value 01h = Global Stepwise Header Records)

   // Global Stepwise Header Record
   03             // Stepwise Header ID
   04             // Domain mask  -- (Domain 2)
   00             // Entity Presence Sensor Number -- (NA)
   00             // Sensor Disabled Control Value
   00             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   00             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 0; [2:0]-Positive Hysteresis = 0

// Add More Stepwise Header Records Here (up to 64 bytes total record length)

//====================================================================//
// Minimum Stepwise Linear Tables
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    003B

   // Sensor Record Header
   00E1           // Record ID
   51             // SDR Version
   C0             // Record Type
   36             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   00             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   19             // 25%
   1B             // 27C
   20             // 32%
   23             // 35C
   31             // 49%
   25             // 37C
   36             // 54%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   01             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   1A             // 26%
   1B             // 27C
   23             // 35%
   23             // 35C
   34             // 52%
   25             // 37C
   3A             // 58%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   02             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   1E             // 30%
   1B             // 27C
   2A             // 42%
   23             // 35C
   3A             // 58%
   25             // 37C
   3E             // 62%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   03             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   28             // 40%
   1B             // 27C
   34             // 52%
   23             // 35C
   46             // 70%
   25             // 37C
   49             // 73%
   2F             // 47C
   64             // 100%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    003B

   // Sensor Record Header
   00E2           // Record ID
   51             // SDR Version
   C0             // Record Type
   36             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   04             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   13             // 19%
   1B             // 27C
   13             // 19%
   23             // 35C
   1E             // 30%
   25             // 37C
   21             // 33%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   05             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   13             // 19%
   1B             // 27C
   13             // 19%
   23             // 35C
   1F             // 31%
   25             // 37C
   22             // 34%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   06             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   14             // 20%
   1B             // 27C
   19             // 25%
   23             // 35C
   21             // 33%
   25             // 37C
   23             // 35%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   07             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   14             // 20%
   1B             // 27C
   19             // 25%
   23             // 35C
   21             // 33%
   25             // 37C
   23             // 35%
   2F             // 47C
   64             // 100%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    003B

   // Sensor Record Header
   00E3           // Record ID
   51             // SDR Version
   C0             // Record Type
   36             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   09             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   1B             // 27%
   1B             // 27C
   1E             // 30%
   23             // 35C
   34             // 52%
   25             // 37C
   37             // 55%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   0A             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   1B             // 27%
   1B             // 27C
   1E             // 30%
   23             // 35C
   34             // 52%
   25             // 37C
   37             // 55%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   0B             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   1E             // 30%
   1B             // 27C
   28             // 40%
   23             // 35C
   37             // 55%
   25             // 37C
   3C             // 60%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   0C             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   22             // 34%
   1B             // 27C
   28             // 40%
   23             // 35C
   3C             // 60%
   25             // 37C
   41             // 65%
   2F             // 47C
   64             // 100%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    003B

   // Sensor Record Header
   00E4           // Record ID
   51             // SDR Version
   C0             // Record Type
   36             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   0D             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   1E             // 30%
   1B             // 27C
   1E             // 30%
   23             // 35C
   23             // 35%
   25             // 37C
   28             // 40%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   0E             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   1E             // 30%
   1B             // 27C
   1E             // 30%
   23             // 35C
   23             // 35%
   25             // 37C
   28             // 40%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   0F             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   1E             // 30%
   1B             // 27C
   1E             // 30%
   23             // 35C
   25             // 37%
   25             // 37C
   2E             // 46%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   10             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   28             // 40%
   1B             // 27C
   28             // 40%
   23             // 35C
   2E             // 46%
   25             // 37C
   30             // 48%
   2F             // 47C
   64             // 100%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    003B

   // Sensor Record Header
   00E5           // Record ID
   51             // SDR Version
   C0             // Record Type
   36             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   12             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   29             // 41%
   1B             // 27C
   32             // 50%
   23             // 35C
   43             // 67%
   25             // 37C
   49             // 73%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   13             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   37             // 55%
   1B             // 27C
   43             // 67%
   23             // 35C
   55             // 85%
   25             // 37C
   58             // 88%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   14             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   14             // 20%
   1B             // 27C
   17             // 23%
   23             // 35C
   1F             // 31%
   25             // 37C
   22             // 34%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   15             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   14             // 20%
   1B             // 27C
   19             // 25%
   23             // 35C
   21             // 33%
   25             // 37C
   23             // 35%
   2F             // 47C
   64             // 100%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    003B

   // Sensor Record Header
   00E6           // Record ID
   51             // SDR Version
   C0             // Record Type
   36             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   16             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   2A             // 42%
   1B             // 27C
   2D             // 45%
   23             // 35C
   43             // 67%
   25             // 37C
   46             // 70%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   17             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   31             // 49%
   1B             // 27C
   37             // 55%
   23             // 35C
   4B             // 75%
   25             // 37C
   50             // 80%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   18             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   1E             // 30%
   1B             // 27C
   23             // 35%
   23             // 35C
   28             // 40%
   25             // 37C
   32             // 50%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   19             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   28             // 40%
   1B             // 27C
   2D             // 45%
   23             // 35C
   35             // 53%
   25             // 37C
   3C             // 60%
   2F             // 47C
   64             // 100%
   
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    003B

   // Sensor Record Header
   00E7           // Record ID
   51             // SDR Version
   C0             // Record Type
   36             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   1A             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   1E             // 30%
   1B             // 27C
   1E             // 30%
   23             // 35C
   1E             // 30%
   25             // 37C
   1E             // 30%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   1B             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   1E             // 30%
   1B             // 27C
   1E             // 30%
   23             // 35C
   1E             // 30%
   25             // 37C
   1E             // 30%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   1C             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   1E             // 30%
   1B             // 27C
   1E             // 30%
   23             // 35C
   1E             // 30%
   25             // 37C
   1E             // 30%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   1D             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   1E             // 30%
   1B             // 27C
   1E             // 30%
   23             // 35C
   1E             // 30%
   25             // 37C
   1E             // 30%
   2F             // 47C
   64             // 100%
   
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    0015

   // Sensor Record Header
   00E8           // Record ID
   51             // SDR Version
   C0             // Record Type
   10             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)
   
   // Global Stepwise Curve Record
   20             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   13             // 19C
   0A             // 10%
   28             // 40C
   19             // 25%
   50             // 80C
   37             // 55%
   64             // 100C
   46             // 70%
   
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0015

   // Sensor Record Header
   00E9           // Record ID
   51             // SDR Version
   C0             // Record Type
   10             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)
   
   // Global Stepwise Curve Record
   21             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   19             // 25C
   0A             // 10%
   28             // 40C
   12             // 18%
   50             // 80C
   2D             // 45%
   64             // 100C
   3C             // 60%
   
//====================================================================//
// Maximum Stepwise Linear Tables
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    0017

   // Sensor Record Header
   00EA           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   08             // Stepwise Curve ID
   85             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   64             // 100%
   1B             // 27C
   64             // 100%
   23             // 35C
   64             // 100%
   25             // 37C
   64             // 100%
   2F             // 47C
   64             // 100%
   
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0017

   // Sensor Record Header
   00EB           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   11             // Stepwise Curve ID
   85             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   64             // 100%
   1B             // 27C
   64             // 100%
   23             // 35C
   64             // 100%
   25             // 37C
   64             // 100%
   2F             // 47C
   64             // 100%
   
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    0017

   // Sensor Record Header
   00EC           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   1E             // Stepwise Curve ID
   85             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   11             // 17C
   64             // 100%
   1B             // 27C
   64             // 100%
   23             // 35C
   64             // 100%
   25             // 37C
   64             // 100%
   2F             // 47C
   64             // 100%
   

//====================================================================//
// Other Stepwise Linear Tables
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_REC_LEN    001D

   // Sensor Record Header
   00ED           // Record ID
   51             // SDR Version
   C0             // Record Type
   18             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   5B             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   1E             // 30C
   19             // 25%
   78             // 120C
   64             // 100%

   // Global Stepwise Curve Record
   5C             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   1E             // 30C
   20             // 32%
   70             // 112C
   64             // 100%

   // Global Stepwise Curve Record
   5D             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   1E             // 30C
   33             // 51%
   59             // 89C
   64             // 100%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_MR'
_REC_LEN    001D

   // Sensor Record Header
   00EE           // Record ID
   51             // SDR Version
   C0             // Record Type
   18             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   5E             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   1E             // 30C
   19             // 25%
   4B             // 75C
   64             // 100%

   // Global Stepwise Curve Record
   5F             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   1E             // 30C
   20             // 32%
   47             // 71C
   64             // 100%

   // Global Stepwise Curve Record
   60             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   1E             // 30C
   33             // 51%
   3C             // 60C
   64             // 100%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_FR'
_REC_LEN    001D

   // Sensor Record Header
   00EF           // Record ID
   51             // SDR Version
   C0             // Record Type
   18             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)
   
   // Global Stepwise Curve Record
   61             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   1E             // 30C
   19             // 25%
   3C             // 60C
   64             // 100%

   // Global Stepwise Curve Record
   62             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   1E             // 30C
   20             // 32%
   3A             // 58C
   64             // 100%

   // Global Stepwise Curve Record
   63             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   1E             // 30C
   33             // 51%
   32             // 50C
   64             // 100%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_SDR_TAG    'OTHER_MR'
_SDR_TAG    'OTHER_FR'
_REC_LEN    0011

   // Sensor Record Header
   00F0           // Record ID
   51             // SDR Version
   C0             // Record Type
   0C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   64             // Stepwise Curve ID
   82             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   1E             // 30C
   64             // 100%
   64             // 100C
   64             // 100%

//====================================================================//
// FSC Record Type = 03h (Fan Sensor Domain Map Record)
// Intel(R) Server Chassis P4000M Non Redundant Fan passive heatsink SKU
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_BASE'
_REC_LEN    0012

   // Sensor Record Header
   00F1           // Record ID
   51             // SDR Version
   C0             // Record Type
   0D             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   03             // FSC Record Type (03h = Fan Sensor Domain Map)

   // Domain Fan Configuration
   01             // [7:4]-Domain Number = 0; [3:0]-Count of sensor numbers = 1
   30             // Fan Sensor Number 1 (30h = System Fan 1)
   11             // [7:4]-Domain Number = 1; [3:0]-Count of sensor numbers = 1
   31             // Fan Sensor Number 2 (31h = System Fan 2)
   22             // [7:4]-Domain Number = 2; [3:0]-Count of sensor numbers = 2
   A0             // PS Fan (A0h = Power Supply 1 Fan1)
   A4             // PS Fan (A4h = Power Supply 2 Fan1)

//====================================================================//
// FSC Record Type = 03h (Fan Sensor Domain Map Record)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0018

   // Sensor Record Header
   00F2           // Record ID
   51             // SDR Version
   C0             // Record Type
   13             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   03             // FSC Record Type (03h = Fan Sensor Domain Map)

   // Domain Fan Configuration
   01             // [7:4]-Domain Number = 0; [3:0]-Count of sensor numbers = 1
   30             // Fan Sensor Number 1 (30h = System Fan 1)
   11             // [7:4]-Domain Number = 1; [3:0]-Count of sensor numbers = 1
   31             // Fan Sensor Number 2 (31h = System Fan 2)
   21             // [7:4]-Domain Number = 2; [3:0]-Count of sensor numbers = 1
   32             // Fan Sensor Number 3 (32h = System Fan 3)
   31             // [7:4]-Domain Number = 3; [3:0]-Count of sensor numbers = 1
   33             // Fan Sensor Number 4 (33h = System Fan 4)
   41             // [7:4]-Domain Number = 4; [3:0]-Count of sensor numbers = 1
   34             // Fan Sensor Number 5 (34h = System Fan 5)
   52             // [7:4]-Domain Number = 5; [3:0]-Count of sensor numbers = 2
   A0             // PS Fan (A0h = Power Supply 1 Fan1)
   A4             // PS Fan (A4h = Power Supply 2 Fan1)

//====================================================================//
// FSC Record Type = 03h (Fan Sensor Domain Map Record)
// Intel(R) Server Chassis P4000M Non Redundant Fan 150w active SKU
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    0016

   // Sensor Record Header
   00F3           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   03             // FSC Record Type (03h = Fan Sensor Domain Map)

   // Domain Fan Configuration
   01             // [7:4]-Domain Number = 0; [3:0]-Count of sensor numbers = 1
   30             // Fan Sensor Number 1 (30h = System Fan 1)
   11             // [7:4]-Domain Number = 1; [3:0]-Count of sensor numbers = 1
   31             // Fan Sensor Number 2 (31h = System Fan 2)
   61             // [7:4]-Domain Number = 6; [3:0]-Count of sensor numbers = 1
   36             // Fan Sensor Number 3 (36h = Processor 1 Fan)
   71             // [7:4]-Domain Number = 7; [3:0]-Count of sensor numbers = 1
   37             // Fan Sensor Number 4 (37h = Processor 2 Fan
   22             // [7:4]-Domain Number = 2; [3:0]-Count of sensor numbers = 2
   A0             // PS Fan (A0h = Power Supply 1 Fan1)
   A4             // PS Fan (A4h = Power Supply 2 Fan1)
   
//====================================================================//
// FSC Record Type = 03h (Fan Sensor Domain Map Record)
// Other Chassis
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    001C

   // Sensor Record Header
   00F4           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   03             // FSC Record Type (03h = Fan Sensor Domain Map)

   // Domain Fan Configuration
   01             // [7:4]-Domain Number = 0; [3:0]-Count of sensor numbers = 1
   30             // Fan Sensor Number 1 (30h = System Fan 1)
   12             // [7:4]-Domain Number = 1; [3:0]-Count of sensor numbers = 2
   31             // Fan Sensor Number 2 (31h = System Fan 2)
   38             // Fan Sensor Number 9 (38h = Real Fan)
   21             // [7:4]-Domain Number = 2; [3:0]-Count of sensor numbers = 1
   32             // Fan Sensor Number 3 (32h = System Fan 3)
   31             // [7:4]-Domain Number = 3; [3:0]-Count of sensor numbers = 1
   33             // Fan Sensor Number 4 (33h = System Fan 4)
   41             // [7:4]-Domain Number = 4; [3:0]-Count of sensor numbers = 1
   34             // Fan Sensor Number 5 (34h = System Fan 5)
   51             // [7:4]-Domain Number = 5; [3:0]-Count of sensor numbers = 1
   35             // Fan Sensor Number 6 (35h = System Fan 6)
   61             // [7:4]-Domain Number = 6; [3:0]-Count of sensor numbers = 1
   36             // Fan Sensor Number 7 (36h = Processor 1 Fan)
   71             // [7:4]-Domain Number = 7; [3:0]-Count of sensor numbers = 1
   37             // Fan Sensor Number 8 (37h = Processor 2 Fan)

//====================================================================//
// Domain 0
//====================================================================//
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Intel(R) Server Chassis P4000M Non Redundant Fan passive heatsink SKU, Domain 0
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_BASE'
_REC_LEN    001B

   // Sensor Record Header
   00F5           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   01             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   00             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID
  
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_BASE'
_REC_LEN    001B

   // Sensor Record Header
   00F6           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   04             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   01             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_BASE'
_REC_LEN    001B

   // Sensor Record Header
   00F7           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   10             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   02             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_BASE'
_REC_LEN    001B

   // Sensor Record Header
   00F8           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   40             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   03             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID
   
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_BASE'
_REC_LEN    001B

   // Sensor Record Header
   00F9           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   0A             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   12             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_BASE'
_REC_LEN    001B

   // Sensor Record Header
   00FA           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   A0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   13             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID
   
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Intel(R) Server Chassis P4000M Non Redundant Fan passive heatsink SKU, Domain 0
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_BASE'
_REC_LEN    001F

   // Sensor Record Header
   00FB           // Record ID
   51             // SDR Version
   C0             // Record Type
   1A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support
   
   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   B1            // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID
   
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Intel(R) Server Chassis P4000M Non Redundant Fan 150w active SKU, Domain 0
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_ACTIVE'
_REC_LEN    001B

   // Sensor Record Header
   00FC           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   01             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   00             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_ACTIVE'
_REC_LEN    001B

   // Sensor Record Header
   00FD           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   04             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   01             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_ACTIVE'
_REC_LEN    001B

   // Sensor Record Header
   00FE           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   10             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   02             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_ACTIVE'
_REC_LEN    001B

   // Sensor Record Header
   00FF           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   40             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   03             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID
   
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_ACTIVE'
_REC_LEN    001B

   // Sensor Record Header
   0100           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   0A             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   12             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_ACTIVE'
_REC_LEN    001B

   // Sensor Record Header
   0101           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   A0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   13             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Intel(R) Server Chassis P4000M Non Redundant Fan 150w active SKU, Domain 0
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    001F

   // Sensor Record Header
   0102           // Record ID
   51             // SDR Version
   C0             // Record Type
   1A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support
   
   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   B1            // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID
   
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU, Domain 0
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   0103           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   01             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   09             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   0104           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   04             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0A             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID
   
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   0105           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   10             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0B             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   0106           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   40             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0C             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   0107           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   0A             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   16             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   0108           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   A0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   17             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU, Domain 0
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   0109           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support
   
   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID

//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU, Domain 0
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0016

   // Sensor Record Header
   010A           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   64             // Domain 0 Fan Failure Value (64h = 100% PWM)
   50             // Domain 1 Fan Failure Value (50h = 80% PWM)
   FF             // Domain 2 Fan Failure Value (FFh = No Change)
   FF             // Domain 3 Fan Failure Value (FFh = No Change)
   FF             // Domain 4 Fan Failure Value (FFh = No Change)
   FF             // Domain 5 Fan Failure Value (FFh = No Change)
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)

//====================================================================//
// Domain 1
//====================================================================//
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Intel(R) Server Chassis P4000M Non Redundant Fan passive heatsink SKU, Domain 1
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_BASE'
_REC_LEN    001B

   // Sensor Record Header
   010B           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   01             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   12             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   04             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_BASE'
_REC_LEN    001B

   // Sensor Record Header
   010C           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   04             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   12             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   05             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_BASE'
_REC_LEN    001B

   // Sensor Record Header
   010D           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   10             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   12             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   06             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_BASE'
_REC_LEN    001B

   // Sensor Record Header
   010E           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   40             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   12             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   07             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_BASE'
_REC_LEN    001B

   // Sensor Record Header
   010F           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   0A             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   12             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   14             // Stepwise Curve ID
   
   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID
   
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_BASE'
_REC_LEN    001B

   // Sensor Record Header
   0110           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   A0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   12             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   15             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Intel(R) Server Chassis P4000M Non Redundant Fan passive heatsink SKU, Domain 1
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_BASE'
_REC_LEN    0027

   // Sensor Record Header
   0111           // Record ID
   51             // SDR Version
   C0             // Record Type
   22             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support
                  
   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   64             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   65             // Clamp ID

//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Intel(R) Server Chassis P4000M Non Redundant Fan 150w active SKU, Domain 1
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_ACTIVE'
_REC_LEN    001B

   // Sensor Record Header
   0112           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   01             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   12             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   04             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_ACTIVE'
_REC_LEN    001B

   // Sensor Record Header
   0113           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   04             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   12             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   05             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_ACTIVE'
_REC_LEN    001B

   // Sensor Record Header
   0114           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   10             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   12             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   06             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_ACTIVE'
_REC_LEN    001B

   // Sensor Record Header
   0115           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   40             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   12             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   07             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_ACTIVE'
_REC_LEN    001B

   // Sensor Record Header
   0116           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   0A             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   12             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   14             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_ACTIVE'
_REC_LEN    001B

   // Sensor Record Header
   0117           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   A0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   12             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   15             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID
   
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Intel(R) Server Chassis P4000M Non Redundant Fan 150w active SKU, Domain 1
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG 'P4000_ACTIVE'
_REC_LEN    0027

   // Sensor Record Header
   0118           // Record ID
   51             // SDR Version
   C0             // Record Type
   22             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support
    
   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   64             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   65             // Clamp ID
   
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU, Domain 1
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   0119           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   01             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   09             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   011A           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   04             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0A             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   011B           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   10             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0B             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   011C           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   40             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0C             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   011D           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   0A             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   16             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   011E           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   A0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   17             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID
   
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU, Domain 1
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0027

   // Sensor Record Header
   011F           // Record ID
   51             // SDR Version
   C0             // Record Type
   22             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   64             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   65             // Clamp ID

//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU, Domain 1
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0016

   // Sensor Record Header
   0120           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   50             // Domain 0 Fan Failure Value (50h = 80% PWM)
   64             // Domain 1 Fan Failure Value (64h = 100% PWM)
   50             // Domain 2 Fan Failure Value (50h = 80% PWM)
   FF             // Domain 3 Fan Failure Value (FFh = No Change)
   FF             // Domain 4 Fan Failure Value (FFh = No Change)
   FF             // Domain 5 Fan Failure Value (FFh = No Change)
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)

//====================================================================//
// Domain 2
//====================================================================//
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU, Domain 2
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   0121           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   01             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0D             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   0122           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   04             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0E             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   0123           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   10             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0F             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   0124           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   40             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   10             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID
   
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   0125           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   0A             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   18             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   0126           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   A0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   19             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU, Domain 2
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0027

   // Sensor Record Header
   0127           // Record ID
   51             // SDR Version
   C0             // Record Type
   22             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   64             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   65             // Clamp ID

//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// FSC Sub-record Type = 05h (Fans Off)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU, Domain 2
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0016

   // Sensor Record Header
   0128           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   FF             // Domain 0 Fan Failure Value (FFh = No Change)
   50             // Domain 1 Fan Failure Value (50h = 80% PWM)
   64             // Domain 2 Fan Failure Value (64h = 100% PWM)
   50             // Domain 3 Fan Failure Value (50h = 80% PWM)
   FF             // Domain 4 Fan Failure Value (FFh = No Change)
   FF             // Domain 5 Fan Failure Value (FFh = No Change)
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)
   
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 05h (Fans Off)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU, Domain 2
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0012

   // Sensor Record Header
   0129           // Record ID
   51             // SDR Version
   C0             // Record Type
   0D             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Fans Off Sub-Record
   05             // FSC Sub-Record Type (05h = Fans Off)
   CA             // Sensor Number Controlling Operation (CAh = Agg Thrm Mgn 3)
   EC             // Fans Off Control Value (ECh = -20 Degrees)
   08             // Hysteresis (08h = 8)
   1E             // Fans Off PWM (1Eh = 30%)

//====================================================================//
// Domain 3
//====================================================================//
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU, Domain 3
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   012A           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   01             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0D             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   012B           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   04             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0E             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   012C           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   10             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0F             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   012D           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   40             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   10             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   012E           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   0A             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   18             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   012F           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   A0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   19             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU, Domain 3
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0027

   // Sensor Record Header
   0130           // Record ID
   51             // SDR Version
   C0             // Record Type
   22             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   64             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   65             // Clamp ID
   
   
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU, Domain 3
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0016

   // Sensor Record Header
   0131           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   FF             // Domain 0 Fan Failure Value (FFh = No Change)
   FF             // Domain 1 Fan Failure Value (FFh = No Change)
   3C             // Domain 2 Fan Failure Value (3Ch = 60% PWM)
   64             // Domain 3 Fan Failure Value (64h = 100% PWM)
   50             // Domain 4 Fan Failure Value (50h = 80% PWM)
   FF             // Domain 5 Fan Failure Value (FFh = No Change)
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)
   
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 05h (Fans Off)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU, Domain 3
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0012

   // Sensor Record Header
   0132           // Record ID
   51             // SDR Version
   C0             // Record Type
   0D             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   FF             // Fan Profile Support

   // Fans Off Sub-Record
   05             // FSC Sub-Record Type (05h = Fans Off)
   CB             // Sensor Number Controlling Operation (CBh = Agg Thrm Mgn 4)
   EC             // Fans Off Control Value (ECh = -20 Degrees)
   08             // Hysteresis (08h = 8)
   1E             // Fans Off PWM (1Eh = 30%)

//====================================================================//
// Domain 4
//====================================================================//
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU, Domain 4
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   0133           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   10             // Domain Mask
   01             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0D             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   0134           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   10             // Domain Mask
   04             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0E             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   0135           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   10             // Domain Mask
   10             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0F             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   0136           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   10             // Domain Mask
   40             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   10             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   0137           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   10             // Domain Mask
   0A             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   18             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   // Sensor Record Header
   0138           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   10             // Domain Mask
   A0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   FF             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   19             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID
   
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU, Domain 4
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0021

   // Sensor Record Header
   0139           // Record ID
   51             // SDR Version
   C0             // Record Type
   1C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   10             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   65             // Clamp ID
   
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU, Domain 4
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0016

   // Sensor Record Header
   013A           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   10             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   FF             // Domain 0 Fan Failure Value (FFh = No Change)
   FF             // Domain 1 Fan Failure Value (FFh = No Change)
   FF             // Domain 2 Fan Failure Value (FFh = No Change)
   50             // Domain 3 Fan Failure Value (50h = 80% PWM)
   64             // Domain 4 Fan Failure Value (64h = 100% PWM)
   FF             // Domain 5 Fan Failure Value (FFh = No Change)
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)

//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 05h (Fans Off)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU, Domain 4
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0012

   // Sensor Record Header
   013B           // Record ID
   51             // SDR Version
   C0             // Record Type
   0D             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   10             // Domain Mask
   FF             // Fan Profile Support

   // Fans Off Sub-Record
   05             // FSC Sub-Record Type (05h = Fans Off)
   CC             // Sensor Number Controlling Operation (CCh = Agg Thrm Mgn 5)
   EC             // Fans Off Control Value (ECh = -20 Degrees)
   08             // Hysteresis (08h = 8)
   1E             // Fans Off PWM (1Eh = 30%)

//====================================================================//
// Domain 5
//====================================================================//
// None

//====================================================================//
// Domain 6
//====================================================================//
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Intel(R) Server Chassis P4000M Non Redundant Fan 150w active SKU, Domain 6
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    001B

   // Sensor Record Header
   013C           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   40             // Domain Mask
   55             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   1A             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   1E             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    001B

   // Sensor Record Header
   013D           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   40             // Domain Mask
   AA             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   1B             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   1E             // Stepwise Curve ID
   
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Intel(R) Server Chassis P4000M Non Redundant Fan 150w active SKU, Domain 6
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    0011

   // Sensor Record Header
   013E           // Record ID
   51             // SDR Version
   C0             // Record Type
   0C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   40             // Domain Mask
   FF             // Fan Profile Support
   
   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   94             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   64             // Clamp ID
   
//====================================================================//
// Domain 7
//====================================================================//
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Intel(R) Server Chassis P4000M Non Redundant Fan 150w active SKU, Domain 7
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    001B

   // Sensor Record Header
   013F           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   80             // Domain Mask
   55             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   1C             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   1E             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    001B

   // Sensor Record Header
   0140           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   80             // Domain Mask
   AA             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   1D             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   1E             // Stepwise Curve ID
   
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Intel(R) Server Chassis P4000M Non Redundant Fan 150w active SKU, Domain 7
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    0013

   // Sensor Record Header
   0141           // Record ID
   51             // SDR Version
   C0             // Record Type
   0E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   80             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   95             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   65             // Clamp ID
   
//====================================================================//
// PS Domain
//====================================================================//
//====================================================================//
// FSC Record Type = 18h (Power Supply Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU, PS Domain
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0018

   // Sensor Record Header
   0142           // Record ID
   51             // SDR Version
   C0             // Record Type
   13             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   18             // FSC Record Type (18h = Power Supply Record)
   20             // Domain Mask
   FF             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   0A             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   FF             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   03             // Stepwise Header ID
   21             // Stepwise Curve ID
   
//====================================================================//
// FSC Record Type = 18h (Power Supply Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU, PS Domain
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    000F

   // Sensor Record Header
   0143           // Record ID
   51             // SDR Version
   C0             // Record Type
   0A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   18             // FSC Record Type (18h = Power Supply Record)
   20             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID

//====================================================================//
// FSC Record Type = 18h (Power Supply Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU, PS Domain
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0016

   // Sensor Record Header
   0144           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   18             // FSC Record Type (18h = Power Supply Record)
   20             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   FF             // Domain 0 Fan Failure Value (FFh = No Change)
   FF             // Domain 1 Fan Failure Value (FFh = No Change)
   FF             // Domain 2 Fan Failure Value (FFh = No Change)
   FF             // Domain 3 Fan Failure Value (FFh = No Change)
   FF             // Domain 4 Fan Failure Value (FFh = No Change)
   FF             // Domain 5 Fan Failure Value (FFh = No Change)
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)

//====================================================================//
// FSC Record Type = 18h (Power Supply Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Intel(R) Server Chassis P4000M Non Redundant Fan passive heatsink SKU, PS Domain
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_REC_LEN    0018

   // Sensor Record Header
   0145           // Record ID
   51             // SDR Version
   C0             // Record Type
   13             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   18             // FSC Record Type (18h = Power Supply Record)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   0A             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   FF             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   02             // Stepwise Header ID
   20             // Stepwise Curve ID
   
//====================================================================//
// FSC Record Type = 18h (Power Supply Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Intel(R) Server Chassis P4000M Non Redundant Fan passive heatsink SKU, PS Domain
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_REC_LEN    000F

   // Sensor Record Header
   0146           // Record ID
   51             // SDR Version
   C0             // Record Type
   0A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   18             // FSC Record Type (18h = Power Supply Record)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID

//====================================================================//
// FSC Record Type = 18h (Power Supply Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Intel(R) Server Chassis P4000M Non Redundant Fan 150w active SKU, PS Domain
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    0018

   // Sensor Record Header
   0147           // Record ID
   51             // SDR Version
   C0             // Record Type
   13             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   18             // FSC Record Type (18h = Power Supply Record)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   0A             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   FF             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   02             // Stepwise Header ID
   20             // Stepwise Curve ID
   
//====================================================================//
// FSC Record Type = 18h (Power Supply Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Intel(R) Server Chassis P4000M Non Redundant Fan 150w active SKU, PS Domain
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    000F

   // Sensor Record Header
   0148           // Record ID
   51             // SDR Version
   C0             // Record Type
   0A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   18             // FSC Record Type (18h = Power Supply Record)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID

//====================================================================//
// FCT/SHIP/FCT2
//====================================================================//
//====================================================================//
// Domain All
// FSC Record Type = 08h (Fan Sensor Domain Map Record)
// FSC Sub-record Type = 01h (Domain Configuration)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'SHIP'
_SDR_TAG    'FCT'
_SDR_TAG    'FCT2'
_REC_LEN    0015

   // Sensor Record Header
   0149           // Record ID
   51             // SDR Version
   C0             // Record Type
   10             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask
   FF             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   64             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

//====================================================================//
// OTHER Chassis
//====================================================================//
//====================================================================//
// FSC Record Type = 08h (Fan Sensor Domain Map Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_REC_LEN    001B

   // Sensor Record Header
   014A           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost
   
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5B             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_REC_LEN    001B

   // Sensor Record Header
   014B           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask
   30             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost
   
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5C             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_REC_LEN    001B

   // Sensor Record Header
   014C           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask
   C0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost
   
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5D             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_MR'
_REC_LEN    001B

   // Sensor Record Header
   014D           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost
   
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5E             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_MR'
_REC_LEN    001B

   // Sensor Record Header
   014E           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask
   30             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost
   
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5F             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_MR'
_REC_LEN    001B

   // Sensor Record Header
   014F           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask
   C0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost
   
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   60             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_FR'
_REC_LEN    001B

   // Sensor Record Header
   0150           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost
   
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   61             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_FR'
_REC_LEN    001B

   // Sensor Record Header
   0151           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask
   30             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost
   
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   62             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_FR'
_REC_LEN    001B

   // Sensor Record Header
   0152           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask
   C0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost
   
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   63             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID

//====================================================================//
// Domain 0
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_SDR_TAG    'OTHER_MR'
_SDR_TAG    'OTHER_FR'
_REC_LEN    0023

   // Sensor Record Header
   0153           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID
   
//====================================================================//
// Domain 1
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_SDR_TAG    'OTHER_MR'
_SDR_TAG    'OTHER_FR'
_REC_LEN    0023

   // Sensor Record Header
   0154           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID
   
//====================================================================//
// Domain 2
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_SDR_TAG    'OTHER_MR'
_SDR_TAG    'OTHER_FR'
_REC_LEN    0023

   // Sensor Record Header
   0155           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID
   
//====================================================================//
// Domain 3
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_SDR_TAG    'OTHER_MR'
_SDR_TAG    'OTHER_FR'
_REC_LEN    0023

   // Sensor Record Header
   0156           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID
   
//====================================================================//
// Domain 4
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_SDR_TAG    'OTHER_MR'
_SDR_TAG    'OTHER_FR'
_REC_LEN    0023

   // Sensor Record Header
   0157           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   10             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID
   
//====================================================================//
// Domain 5
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_SDR_TAG    'OTHER_MR'
_SDR_TAG    'OTHER_FR'
_REC_LEN    0023

   // Sensor Record Header
   0158           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   20             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID
   
//====================================================================//
// Domain 6
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_SDR_TAG    'OTHER_MR'
_SDR_TAG    'OTHER_FR'
_REC_LEN    0023

   // Sensor Record Header
   0159           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   40             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID
   
//====================================================================//
// Domain 7
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_SDR_TAG    'OTHER_MR'
_SDR_TAG    'OTHER_FR'
_REC_LEN    0023

   // Sensor Record Header
   015A           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   80             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

//====================================================================//
//
// SDR Type C0/0E Chassis ID and FAN FRU LED Mapping
//
//====================================================================//

//====================================================================//
// For Intel(R) Server Chassis P4000M Non Redundant Fan passive heatsink SKU
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_REC_LEN    0011

    // Sensor Record Header
   015B           // Record ID
   51             // SDR Version
   C0             // Record Type
   0C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0E             // Record Subtype Value (Chassis ID & FRU LED Mapping)
   01             // Record Version
   00             // Chassis ID number = 00 (P4000_BASE)
   // LED mapping sub-records
   01             // LED Group = 1 (Fan Fault LED)
   02             // Number of mapping pairs = 2
   30             // 1st fan sensor number = 0x30
   2C             // 1st fan fault LED GPIO number = 44
   31             // 2nd fan sensor number = 0x31
   2D             // 2nd fan fault LED GPIO number = 45

//====================================================================//
// For Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0017

    // Sensor Record Header
   015C           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0E             // Record Subtype Value (Chassis ID & FRU LED Mapping)
   01             // Record Version
   00             // Chassis ID number = 00 (P4000)
   // LED mapping sub-records
   01             // LED Group = 1 (Fan Fault LED)
   05             // Number of mapping pairs = 5
   30             // 1st fan sensor number = 0x30
   2C             // 1st fan fault LED GPIO number = 44
   31             // 2nd fan sensor number = 0x31
   2D             // 2nd fan fault LED GPIO number = 45
   32             // 3rd fan sensor number = 0x32
   2E             // 3rd fan fault LED GPIO number = 46
   33             // 4th fan sensor number = 0x33
   2F             // 4th fan fault LED GPIO number = 47
   34             // 5th fan sensor number = 0x34
   30             // 5th fan fault LED GPIO number = 48
   
//====================================================================//
// For Intel(R) Server Chassis P4000M Non Redundant Fan 150w active SKU
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    0015

    // Sensor Record Header
   015D           // Record ID
   51             // SDR Version
   C0             // Record Type
   10             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0E             // Record Subtype Value (Chassis ID & FRU LED Mapping)
   01             // Record Version
   00             // Chassis ID number = 00 (P4000_ACTIVE)
   // LED mapping sub-records
   01             // LED Group = 1 (Fan Fault LED)
   04             // Number of mapping pairs = 4
   30             // 1st fan sensor number = 0x30
   2C             // 1st fan fault LED GPIO number = 44
   31             // 2nd fan sensor number = 0x31
   2D             // 2nd fan fault LED GPIO number = 45
   36             // CPU1 fan sensor number = 0x36
   32             // CPU1 fan fault LED GPIO number = 50
   37             // CPU2 fan sensor number = 0x37
   33             // CPU2 fan fault LED GPIO number = 51

//====================================================================//
// For Other Chassis
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    001F

    // Sensor Record Header
   015E           // Record ID
   51             // SDR Version
   C0             // Record Type
   1A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0E             // Record Subtype Value (Chassis ID & FRU LED Mapping)
   01             // Record Version
   00             // Chassis ID number = 00 (OTHER)
   // LED mapping sub-records
   01             // LED Group = 1 (Fan Fault LED)
   09             // Number of mapping pairs = 9
   30             // 1st fan sensor number = 0x30
   2C             // 1st fan fault LED GPIO number = 44
   31             // 2nd fan sensor number = 0x31
   2D             // 2nd fan fault LED GPIO number = 45
   32             // 3rd fan sensor number = 0x32
   2E             // 3rd fan fault LED GPIO number = 46
   33             // 4th fan sensor number = 0x33
   2F             // 4th fan fault LED GPIO number = 47
   34             // 5th fan sensor number = 0x34
   30             // 5th fan fault LED GPIO number = 48
   35             // 6th fan sensor number = 0x35
   31             // 6th fan fault LED GPIO number = 49
   36             // CPU1 fan sensor number = 0x36
   32             // CPU1 fan fault LED GPIO number = 50
   37             // CPU2 fan sensor number = 0x37
   33             // CPU2 fan fault LED GPIO number = 51
   38             // Rear fan sensor number = 0x38
   47             // Rear fan fault LED GPIO number = 71

//====================================================================//
// For FCT
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'FCT'
_REC_LEN    001F

    // Sensor Record Header
   015F           // Record ID
   51             // SDR Version
   C0             // Record Type
   1A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0E             // Record Subtype Value (Chassis ID & FRU LED Mapping)
   01             // Record Version
   00             // Chassis ID number = 00 (FCT)
   // LED mapping sub-records
   01             // LED Group = 1 (Fan Fault LED)
   09             // Number of mapping pairs = 9
   30             // 1st fan sensor number = 0x30
   2C             // 1st fan fault LED GPIO number = 44
   31             // 2nd fan sensor number = 0x31
   2D             // 2nd fan fault LED GPIO number = 45
   32             // 3rd fan sensor number = 0x32
   2E             // 3rd fan fault LED GPIO number = 46
   33             // 4th fan sensor number = 0x33
   2F             // 4th fan fault LED GPIO number = 47
   34             // 5th fan sensor number = 0x34
   30             // 5th fan fault LED GPIO number = 48
   35             // 6th fan sensor number = 0x35
   31             // 6th fan fault LED GPIO number = 49
   36             // CPU1 fan sensor number = 0x36
   32             // CPU1 fan fault LED GPIO number = 50
   37             // CPU2 fan sensor number = 0x37
   33             // CPU2 fan fault LED GPIO number = 51
   38             // Rear fan sensor number = 0x38
   47             // Rear fan fault LED GPIO number = 71

//====================================================================//
// For FCT2
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'FCT2'
_REC_LEN    001D

    // Sensor Record Header
   0160           // Record ID
   51             // SDR Version
   C0             // Record Type
   18             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0E             // Record Subtype Value (Chassis ID & FRU LED Mapping)
   01             // Record Version
   00             // Chassis ID number = 00 (FCT2)
   // LED mapping sub-records
   01             // LED Group = 1 (Fan Fault LED)
   08             // Number of mapping pairs = 8
   30             // 1st fan sensor number = 0x30
   2C             // 1st fan fault LED GPIO number = 44
   31             // 2nd fan sensor number = 0x31
   2D             // 2nd fan fault LED GPIO number = 45
   32             // 3rd fan sensor number = 0x32
   2E             // 3rd fan fault LED GPIO number = 46
   33             // 4th fan sensor number = 0x33
   2F             // 4th fan fault LED GPIO number = 47
   34             // 5th fan sensor number = 0x34
   30             // 5th fan fault LED GPIO number = 48
   35             // 6th fan sensor number = 0x35
   31             // 6th fan fault LED GPIO number = 49
   36             // CPU1 fan sensor number = 0x36
   32             // CPU1 fan fault LED GPIO number = 50
   38             // Rear fan sensor number = 0x38
   47             // Rear fan fault LED GPIO number = 71
   
//====================================================================//
//
// FSC Record Type = 11h (System Airflow Formula)
//
//====================================================================//

//====================================================================//
// Intel(R) Server Chassis P4000M Non Redundant Fan passive heatsink SKU.
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_REC_LEN    001B


   //Sensor Record Header
   0161               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   16                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   11                 // Record sub-type (11h = System air flow)
   01                 // Domain mask (Domains 0)
   5500               // Correction Factor 1 (5500h = 85 units of .01)
   1F00               // Correction Factor 2 (1F00h = 31 units of .01)
   13                 // PWM for Correction Factor 1 (13h = 19%)
   64                 // PWM for Correction Factor 2 (64h = 100%)
   96                 // Max CFM of Fan (96h = 150)
   01                 // Quantity of fans in this equation

   02                 // Domain mask (Domains 1)
   5500               // Correction Factor 1 (5500h = 85 units of .01)
   1F00               // Correction Factor 2 (1F00h = 31 units of .01)
   13                 // PWM for Correction Factor 1 (13h = 19%)
   64                 // PWM for Correction Factor 2 (64h = 100%)
   DC                 // Max CFM of Fan (DCh = 220)
   01                 // Quantity of fans in this equation
   
//====================================================================//
// Intel(R) Server Chassis P4000M Non Redundant Fan 150w active SKU.
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    001B


   //Sensor Record Header
   0162               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   16                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   11                 // Record sub-type (11h = System air flow)
   01                 // Domain mask (Domains 0)
   5500               // Correction Factor 1 (5500h = 85 units of .01)
   1F00               // Correction Factor 2 (1F00h = 31 units of .01)
   13                 // PWM for Correction Factor 1 (13h = 19%)
   64                 // PWM for Correction Factor 2 (64h = 100%)
   96                 // Max CFM of Fan (96h = 150)
   01                 // Quantity of fans in this equation

   02                 // Domain mask (Domains 1)
   5500               // Correction Factor 1 (5500h = 85 units of .01)
   1F00               // Correction Factor 2 (1F00h = 31 units of .01)
   13                 // PWM for Correction Factor 1 (13h = 19%)
   64                 // PWM for Correction Factor 2 (64h = 100%)
   DC                 // Max CFM of Fan (DCh = 220)
   01                 // Quantity of fans in this equation

//====================================================================/
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU.
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0036


   //Sensor Record Header
   0163               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   31                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   11                 // Record sub-type (11h = System air flow)
   01                 // Domain mask (Domains 0)
   3200               // Correction Factor 1 (3200h = 50 units of .01)
   1C00               // Correction Factor 2 (1C00h = 28 units of .01)
   19                 // PWM for Correction Factor 1 (19h = 25%)
   64                 // PWM for Correction Factor 2 (64h = 100%)
   6D                 // Max CFM of Fan (6Dh = 109)
   01                 // Quantity of fans in this equation

   02                 // Domain mask (Domains 1)
   3200               // Correction Factor 1 (3200h = 50 units of .01)
   1C00               // Correction Factor 2 (1C00h = 28 units of .01)
   19                 // PWM for Correction Factor 1 (19h = 25%)
   64                 // PWM for Correction Factor 2 (64h = 100%)
   6D                 // Max CFM of Fan (6Dh = 109)
   01                 // Quantity of fans in this equation

   04                 // Domain mask (Domains 2)
   3200               // Correction Factor 1 (3200h = 50 units of .01)
   1C00               // Correction Factor 2 (1C00h = 28 units of .01)
   19                 // PWM for Correction Factor 1 (19h = 25%)
   64                 // PWM for Correction Factor 2 (64h = 100%)
   6D                 // Max CFM of Fan (6Dh = 109)
   01                 // Quantity of fans in this equation

   08                 // Domain mask (Domains 3)
   3200               // Correction Factor 1 (3200h = 50 units of .01)
   1C00               // Correction Factor 2 (1C00h = 28 units of .01)
   19                 // PWM for Correction Factor 1 (19h = 25%)
   64                 // PWM for Correction Factor 2 (64h = 100%)
   6D                 // Max CFM of Fan (6Dh = 109)
   01                 // Quantity of fans in this equation

   10                 // Domain mask (Domains 4)
   3200               // Correction Factor 1 (3200h = 50 units of .01)
   1C00               // Correction Factor 2 (1C00h = 28 units of .01)
   19                 // PWM for Correction Factor 1 (19h = 25%)
   64                 // PWM for Correction Factor 2 (64h = 100%)
   6D                 // Max CFM of Fan (6Dh = 109)
   01                 // Quantity of fans in this equation

//====================================================================//
//
// FSC Record Type = 12h (Aggregate Sensor Configuration Record)
//
//====================================================================//

//====================================================================//
// Intel(R) Server Chassis P4000M Non Redundant Fan passive heatsink SKU.
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_REC_LEN    001B

   //Sensor Record Header
   0164               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   16                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   12                 // Record sub-type (12h = Aggregate Sensor Configuration)
   C8                 // Aggregate sensor number (C8h = Aggregate Thermal Margin 1)
   08                 // Number of input pairs to follow
   22                 // Input 1 sensor number (22h = SSB Temp)
   49                 // Input 1 margin reference value (49h = 73)
   23                 // Input 2 sensor number (23h = BB BMC Temp)
   52                 // Input 2 margin reference value (52h = 82)
   25                 // Input 3 sensor number (25h = BB MEM VR Temp)
   5A                 // Input 3 margin reference value (5Ah = 90)
   2F                 // Input 4 sensor number (2Fh = LAN NIC Temp)
   64                 // Input 4 margin reference value (64h = 100)
   B1                 // Input 5 sensor number (B1h = DIMM Thrm Mrgn 2)
   FB                 // Input 5 margin reference value (FBh = -5)
   B2                 // Input 6 sensor number (B2h = DIMM Thrm Mrgn 3)
   FB                 // Input 6 margin reference value (FBh = -5)
   29                 // Input 7 sensor number (29h = HSBP 1 Temp)
   50                 // Input 7 margin reference value (50h = 80)
   2A                 // Input 8 sensor number (2Ah = HSBP 2 Temp)
   50                 // Input 8 margin reference value (50h = 80)

//=========================================================
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_REC_LEN    001F

   //Sensor Record Header
   0165               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   12                 // Record Subtype (12h = Aggregate Sensor Configuration)
   C9                 // Aggregate sensor number (C9h = Aggregate Thermal Margin 2)
   0A                 // Number of input pairs to follow
   B0                 // Input 1 sensor number (B0h = DIMM Thrm Mrgn 1)
   FB                 // Input 1 margin reference value (FBh = -5)
   B1                 // Input 2 sensor number (B1h = DIMM Thrm Mrgn 2)
   FB                 // Input 2 margin reference value (FBh = -5)
   B2                 // Input 3 sensor number (B2h = DIMM Thrm Mrgn 3)
   FB                 // Input 3 margin reference value (FBh = -5)
   B3                 // Input 4 sensor number (B3h = DIMM Thrm Mrgn 4)
   FB                 // Input 4 margin reference value (FBh = -5)
   74                 // Input 5 sensor number (74h = P1 Therm Margin)
   F1                 // Input 5 margin reference value (F1h = -15)
   75                 // Input 6 sensor number (75h = P2 Therm Margin)
   F1                 // Input 6 margin reference value (F1h = -15)
   24                 // Input 7 sensor number (24h = BB CPU1 VR Temp)
   4B                 // Input 7 margin reference value (4Bh = 75)
   25                 // Input 8 sensor number (25h = BB MEM VR Temp)
   5A                 // Input 8 margin reference value (5Ah = 90)
   2A                 // Input 9 sensor number (2Ah = HSBP 2 Temp)
   50                 // Input 9 margin reference value (50h = 80)
   21                 // Input 10 sensor number (21h = Front Panel Temp)
   32                 // Input 10 margin reference value (32h = 50)
   
//====================================================================//
// Intel(R) Server Chassis P4000M Non Redundant Fan 150w active SKU.
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    001B

   //Sensor Record Header
   0166               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   16                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   12                 // Record sub-type (12h = Aggregate Sensor Configuration)
   C8                 // Aggregate sensor number (C8h = Aggregate Thermal Margin 1)
   08                 // Number of input pairs to follow
   22                 // Input 1 sensor number (22h = SSB Temp)
   49                 // Input 1 margin reference value (49h = 73)
   23                 // Input 2 sensor number (23h = BB BMC Temp)
   52                 // Input 2 margin reference value (52h = 82)
   25                 // Input 3 sensor number (25h = BB MEM VR Temp)
   5A                 // Input 3 margin reference value (5Ah = 90)
   2F                 // Input 4 sensor number (2Fh = LAN NIC Temp)
   64                 // Input 4 margin reference value (64h = 100)
   B1                 // Input 5 sensor number (B1h = DIMM Thrm Mrgn 2)
   FB                 // Input 5 margin reference value (FBh = -5)
   B2                 // Input 6 sensor number (B2h = DIMM Thrm Mrgn 3)
   FB                 // Input 6 margin reference value (FBh = -5)
   29                 // Input 7 sensor number (29h = HSBP 1 Temp)
   50                 // Input 7 margin reference value (50h = 80)
   2A                 // Input 8 sensor number (2Ah = HSBP 2 Temp)
   50                 // Input 8 margin reference value (50h = 80)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    001F

   //Sensor Record Header
   0167               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1A                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   12                 // Record Subtype (12h = Aggregate Sensor Configuration)
   C9                 // Aggregate sensor number (C9h = Aggregate Thermal Margin 2)
   0A                 // Number of input pairs to follow
   B0                 // Input 1 sensor number (B0h = DIMM Thrm Mrgn 1)
   FB                 // Input 1 margin reference value (FBh = -5)
   B1                 // Input 2 sensor number (B1h = DIMM Thrm Mrgn 2)
   FB                 // Input 2 margin reference value (FBh = -5)
   B2                 // Input 3 sensor number (B2h = DIMM Thrm Mrgn 3)
   FB                 // Input 3 margin reference value (FBh = -5)
   B3                 // Input 4 sensor number (B3h = DIMM Thrm Mrgn 4)
   FB                 // Input 4 margin reference value (FBh = -5)
   74                 // Input 5 sensor number (74h = P1 Therm Margin)
   F1                 // Input 5 margin reference value (F1h = -15)
   75                 // Input 6 sensor number (75h = P2 Therm Margin)
   F1                 // Input 6 margin reference value (F1h = -15)
   24                 // Input 7 sensor number (24h = BB CPU1 VR Temp)
   4B                 // Input 7 margin reference value (4Bh = 75)
   25                 // Input 8 sensor number (25h = BB MEM VR Temp)
   5A                 // Input 8 margin reference value (5Ah = 90)
   2A                 // Input 9 sensor number (2Ah = HSBP 2 Temp)
   50                 // Input 9 margin reference value (50h = 80)
   21                 // Input 10 sensor number (21h = Front Panel Temp)
   32                 // Input 10 margin reference value (32h = 50)

//====================================================================//
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU.
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0019

   //Sensor Record Header
   0168               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   14                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   12                 // Record Subtype (12h = Aggregate Sensor Configuration)
   C8                 // Aggregate sensor number (C8h = Aggregate Thermal Margin 1)
   07                 // Number of input pairs to follow
   22                 // Input 1 sensor number (22h = SSB Temp)
   49                 // Input 1 margin reference value (49h = 73)
   23                 // Input 2 sensor number (23h = BB BMC Temp)
   52                 // Input 2 margin reference value (52h = 82)
   2F                 // Input 3 sensor number (2Fh = LAN NIC Temp)
   5F                 // Input 3 margin reference value (5Fh = 95)
   25                 // Input 4 sensor number (25h = BB MEM VR Temp)
   5A                 // Input 4 margin reference value (5Ah = 90)
   29                 // Input 5 sensor number (29h = HSBP 1 Temp)
   50                 // Input 5 margin reference value (50h = 80)
   2A                 // Input 6 sensor number (2Ah = HSBP 2 Temp)
   50                 // Input 6 margin reference value (50h = 80)
   21                 // Input 7 sensor number (21h = Front Panel Temp)
   32                 // Input 7 margin reference value (32h = 50)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   //Sensor Record Header
   0169               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   16                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   12                 // Record Subtype (12h = Aggregate Sensor Configuration)
   C9                 // Aggregate sensor number (C9h = Aggregate Thermal Margin 2)
   08                 // Number of input pairs to follow
   22                 // Input 1 sensor number (22h = SSB Temp)
   49                 // Input 1 margin reference value (49h = 73)
   23                 // Input 2 sensor number (23h = BB BMC Temp)
   52                 // Input 2 margin reference value (52h = 82)
   2F                 // Input 3 sensor number (2Fh = LAN NIC Temp)
   5F                 // Input 3 margin reference value (5Fh = 95)
   25                 // Input 4 sensor number (25h = BB MEM VR Temp)
   5A                 // Input 4 margin reference value (5Ah = 90)
   B1                 // Input 5 sensor number (B1h = DIMM Thrm Mrgn 2)
   00                 // Input 5 margin reference value (00h = 0)
   B2                 // Input 6 sensor number (B2h = DIMM Thrm Mrgn 3)
   00                 // Input 6 margin reference value (00h = 0)
   29                 // Input 7 sensor number (29h = HSBP 1 Temp)
   50                 // Input 7 margin reference value (50h = 80)
   21                 // Input 8 sensor number (21h = HSBP 2 Temp)
   32                 // Input 8 margin reference value (32h = 50)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   //Sensor Record Header
   016A               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   16                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   12                 // Record Subtype (12h = Aggregate Sensor Configuration)
   CA                 // Aggregate sensor number (CAh = Aggregate Thermal Margin 3)
   08                 // Number of input pairs to follow
   74                 // Input 1 sensor number (74h = P1 Therm Margin)
   F1                 // Input 1 margin reference value (F1h = -15)
   75                 // Input 2 sensor number (75h = P2 Therm Margin)
   F1                 // Input 2 margin reference value (F1h = -15)
   B2                 // Input 3 sensor number (B2h = DIMM Thrm Mrgn 3)
   00                 // Input 3 margin reference value (00h = 0)
   B1                 // Input 4 sensor number (B1h = DIMM Thrm Mrgn 2)
   00                 // Input 4 margin reference value (00h = 0)
   24                 // Input 5 sensor number (24h = BB CPU1 VR Temp)
   4B                 // Input 5 margin reference value (4Bh = 75)
   29                 // Input 6 sensor number (29h = BB MEM VR Temp)
   50                 // Input 6 margin reference value (50h = 80)
   2A                 // Input 7 sensor number (2Ah = HSBP 1 Temp)
   50                 // Input 7 margin reference value (50h = 80)
   21                 // Input 8 sensor number (21h = HSBP 2 Temp)
   32                 // Input 8 margin reference value (32h = 50)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    001B

   //Sensor Record Header
   016B               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   16                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   12                 // Record Subtype (12h = Aggregate Sensor Configuration)
   CB                 // Aggregate sensor number (CBh = Aggregate Thermal Margin 4)
   08                 // Number of input pairs to follow
   74                 // Input 1 sensor number (74h = P1 Therm Margin)
   F1                 // Input 1 margin reference value (F1h = -15)
   75                 // Input 2 sensor number (75h = P2 Therm Margin)
   F1                 // Input 2 margin reference value (F1h = -15)
   B0                 // Input 3 sensor number (B0h = DIMM Thrm Mrgn 1)
   00                 // Input 3 margin reference value (00h = 0)
   B3                 // Input 4 sensor number (B3h = DIMM Thrm Mrgn 4)
   00                 // Input 4 margin reference value (00h = 0)
   24                 // Input 5 sensor number (24h = BB CPU1 VR Temp)
   4B                 // Input 5 margin reference value (4Bh = 75)
   29                 // Input 6 sensor number (29h = BB MEM VR Temp)
   50                 // Input 6 margin reference value (50h = 80)
   2A                 // Input 7 sensor number (2Ah = HSBP 1 Temp)
   50                 // Input 7 margin reference value (50h = 80)
   21                 // Input 8 sensor number (21h = HSBP 2 Temp)
   32                 // Input 8 margin reference value (32h = 50)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    0019

   //Sensor Record Header
   016C               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   14                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   12                 // Record Subtype (12h = Aggregate Sensor Configuration)
   CC                 // Aggregate sensor number (CCh = Aggregate Thermal Margin 5)
   07                 // Number of input pairs to follow
   75                 // Input 1 sensor number (75h = P2 Therm Margin)
   F1                 // Input 1 margin reference value (F1h = -15)
   B0                 // Input 2 sensor number (B0h = DIMM Thrm Mrgn 1)
   00                 // Input 2 margin reference value (00h = 0)
   B3                 // Input 3 sensor number (B3h = DIMM Thrm Mrgn 4)
   00                 // Input 3 margin reference value (00h = 0)
   24                 // Input 4 sensor number (24h = BB CPU1 VR Temp)
   4B                 // Input 4 margin reference value (4Bh = 75)
   29                 // Input 5 sensor number (29h = HSBP 1 Temp)
   50                 // Input 5 margin reference value (50h = 80)
   2A                 // Input 6 sensor number (2Ah = HSBP 2 Temp)
   50                 // Input 6 margin reference value (50h = 80)
   21                 // Input 7 sensor number (21h = Front Panel Temp)
   32                 // Input 7 margin reference value (32h = 50)

//====================================================================//
//
// FSC Record Type = 13h (DIMM Air Velocity Record)
//
//====================================================================//

//====================================================================//
// Intel(R) Server Chassis P4000M Non Redundant Fan passive heatsink SKU.
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_BASE'
_REC_LEN    002D

   // Sensor Record Header
   016D               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   28                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   13                 // Record Subtype (13h = DIMM Air Velocity)

   B0                 // DIMM aggregate sensor number (B0h = DIMM Thrm Mrgn 1)
   02                 // Domain bit mask (02h = Domain 1)
   1E                 // Reference PWM % 1 (1Eh = 30%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   08                 // PWM 1 Velocity (08h = 8)
   14                 // PWM 2 Velocity (14h = 20)
   1E                 // PWM 3 Velocity (1Eh = 30)
   07                 // Smoothing coefficient (07h = 7)

   B1                 // DIMM aggregate sensor number (B1h = DIMM Thrm Mrgn 2)
   03                 // Domain bit mask (03h = Domain 0 & 1)
   1E                 // Reference PWM % 1 (1Eh = 30%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   08                 // PWM 1 Velocity (08h = 8)
   14                 // PWM 2 Velocity (14h = 20)
   1E                 // PWM 3 Velocity (1Eh = 30)
   07                 // Smoothing coefficient (07h = 7)

   B2                 // DIMM aggregate sensor number (B2h = DIMM Thrm Mrgn 3)
   03                 // Domain bit mask (03h = Domain 0 & 1)
   1E                 // Reference PWM % 1 (1Eh = 30%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   08                 // PWM 1 Velocity (08h = 8)
   14                 // PWM 2 Velocity (14h = 20)
   1E                 // PWM 3 Velocity (1Eh = 30)
   07                 // Smoothing coefficient (07h = 7)

   B3                 // DIMM aggregate sensor number (B3h = DIMM Thrm Mrgn 4)
   02                 // Domain bit mask (2h = Domain 1)
   1E                 // Reference PWM % 1 (1Eh = 30%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   08                 // PWM 1 Velocity (08h = 8)
   14                 // PWM 2 Velocity (14h = 20)
   1E                 // PWM 3 Velocity (1Eh = 30)
   07                 // Smoothing coefficient (07h = 7)
   
//====================================================================//
// Intel(R) Server Chassis P4000M Non Redundant Fan 150w active SKU.
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000_ACTIVE'
_REC_LEN    002D

   // Sensor Record Header
   016E               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   28                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   13                 // Record Subtype (13h = DIMM Air Velocity)

   B0                 // DIMM aggregate sensor number (B0h = DIMM Thrm Mrgn 1)
   02                 // Domain bit mask (02h = Domain 1)
   1E                 // Reference PWM % 1 (1Eh = 30%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   08                 // PWM 1 Velocity (08h = 8)
   14                 // PWM 2 Velocity (14h = 20)
   1E                 // PWM 3 Velocity (1Eh = 30)
   07                 // Smoothing coefficient (07h = 7)

   B1                 // DIMM aggregate sensor number (B1h = DIMM Thrm Mrgn 2)
   03                 // Domain bit mask (03h = Domain 0 & 1)
   1E                 // Reference PWM % 1 (1Eh = 30%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   08                 // PWM 1 Velocity (08h = 8)
   14                 // PWM 2 Velocity (14h = 20)
   1E                 // PWM 3 Velocity (1Eh = 30)
   07                 // Smoothing coefficient (07h = 7)

   B2                 // DIMM aggregate sensor number (B2h = DIMM Thrm Mrgn 3)
   03                 // Domain bit mask (03h = Domain 0 & 1)
   1E                 // Reference PWM % 1 (1Eh = 30%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   08                 // PWM 1 Velocity (08h = 8)
   14                 // PWM 2 Velocity (14h = 20)
   1E                 // PWM 3 Velocity (1Eh = 30)
   07                 // Smoothing coefficient (07h = 7)

   B3                 // DIMM aggregate sensor number (B3h = DIMM Thrm Mrgn 4)
   02                 // Domain bit mask (2h = Domain 1)
   1E                 // Reference PWM % 1 (1Eh = 30%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   08                 // PWM 1 Velocity (08h = 8)
   14                 // PWM 2 Velocity (14h = 20)
   1E                 // PWM 3 Velocity (1Eh = 30)
   07                 // Smoothing coefficient (07h = 7)

//====================================================================//
// Intel(R) Server Chassis P4000M Redundant Fan passive heatsink SKU.
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'P4000'
_REC_LEN    002D

   // Sensor Record Header
   016F               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   28                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   13                 // Record Subtype (13h = DIMM Air Velocity)

   B0                 // DIMM aggregate sensor number (B0h = DIMM Thrm Mrgn 1)
   0C                 // Domain bit mask (0Ch = Domain 2 & 3)
   28                 // Reference PWM % 1 (28h = 40%)
   46                 // Reference PWM % 2 (46h = 70%)
   64                 // Reference PWM % 3 (64h = 100%)
   0A                 // PWM 1 Velocity (0Ah = 10)
   13                 // PWM 2 Velocity (13h = 19)
   1E                 // PWM 3 Velocity (1Eh = 30)
   07                 // Smoothing coefficient (07h = 7)

   B1                 // DIMM aggregate sensor number (B1h = DIMM Thrm Mrgn 2)
   02                 // Domain bit mask (02h = Domain 1)
   28                 // Reference PWM % 1 (28h = 40%)
   46                 // Reference PWM % 2 (46h = 70%)
   64                 // Reference PWM % 3 (64h = 100%)
   0A                 // PWM 1 Velocity (0Ah = 10)
   13                 // PWM 2 Velocity (13h = 19)
   1E                 // PWM 3 Velocity (1Eh = 30)
   07                 // Smoothing coefficient (07h = 7)

   B2                 // DIMM aggregate sensor number (B2h = DIMM Thrm Mrgn 3)
   06                 // Domain bit mask (06h = Domain 1 & 2)
   28                 // Reference PWM % 1 (28h = 40%)
   46                 // Reference PWM % 2 (46h = 70%)
   64                 // Reference PWM % 3 (64h = 100%)
   0A                 // PWM 1 Velocity (0Ah = 10)
   13                 // PWM 2 Velocity (13h = 19)
   1E                 // PWM 3 Velocity (1Eh = 30)
   07                 // Smoothing coefficient (07h = 7)

   B3                 // DIMM aggregate sensor number (B3h = DIMM Thrm Mrgn 4)
   18                 // Domain bit mask (18h = Domain 3 & 4)
   28                 // Reference PWM % 1 (28h = 40%)
   46                 // Reference PWM % 2 (46h = 70%)
   64                 // Reference PWM % 3 (64h = 100%)
   0A                 // PWM 1 Velocity (0Ah = 10)
   13                 // PWM 2 Velocity (13h = 19)
   1E                 // PWM 3 Velocity (1Eh = 30)
   07                 // Smoothing coefficient (07h = 7)

//====================================================================//
// Other chassis.
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    002D

   // Sensor Record Header
   0170               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   28                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   13                 // Record Subtype (13h = DIMM Air Velocity)

   B0                 // DIMM aggregate sensor number (B0h = DIMM Thrm Mrgn 1)
   FF                 // Domain bit mask (FFh = Domain 0 to 7)
   00                 // Reference PWM % 1 (00h = 0%)
   32                 // Reference PWM % 2 (32h = 50%)
   64                 // Reference PWM % 3 (64h = 100%)
   0A                 // PWM 1 Velocity (0Ah = 10)
   0A                 // PWM 2 Velocity (0Ah = 10)
   0A                 // PWM 3 Velocity (0Ah = 10)
   07                 // Smoothing coefficient (07h = 7)

   B1                 // DIMM aggregate sensor number (B1h = DIMM Thrm Mrgn 2)
   FF                 // Domain bit mask (FFh = Domain 0 to 7)
   00                 // Reference PWM % 1 (00h = 0%)
   32                 // Reference PWM % 2 (32h = 50%)
   64                 // Reference PWM % 3 (64h = 100%)
   0A                 // PWM 1 Velocity (0Ah = 10)
   0A                 // PWM 2 Velocity (0Ah = 10)
   0A                 // PWM 3 Velocity (0Ah = 10)
   07                 // Smoothing coefficient (07h = 7)

   B2                 // DIMM aggregate sensor number (B2h = DIMM Thrm Mrgn 3)
   FF                 // Domain bit mask (FFh = Domain 0 to 7)
   00                 // Reference PWM % 1 (00h = 0%)
   32                 // Reference PWM % 2 (32h = 50%)
   64                 // Reference PWM % 3 (64h = 100%)
   0A                 // PWM 1 Velocity (0Ah = 10)
   0A                 // PWM 2 Velocity (0Ah = 10)
   0A                 // PWM 3 Velocity (0Ah = 10)
   07                 // Smoothing coefficient (07h = 7)

   B3                 // DIMM aggregate sensor number (B3h = DIMM Thrm Mrgn 4)
   FF                 // Domain bit mask (FFh = Domain 0 to 7)
   00                 // Reference PWM % 1 (00h = 0%)
   32                 // Reference PWM % 2 (32h = 50%)
   64                 // Reference PWM % 3 (64h = 100%)
   0A                 // PWM 1 Velocity (0Ah = 10)
   0A                 // PWM 2 Velocity (0Ah = 10)
   0A                 // PWM 3 Velocity (0Ah = 10)
   07                 // Smoothing coefficient (07h = 7)

//====================================================================//
// SDR Version Records
//====================================================================//

// SDR Version Record (first letter of 'SDR')
//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0015

   // Sensor Record Header
   0171               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   10                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   'SDR File 1.09'    // String Bytes

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0018

   // Sensor Record Header
   0172               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   13                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   'SDR Package 1.09' // String Bytes
)                     // End of SDR File
