================================================================================
Intel(R) Server Board S2400GP Family
Intel(R) Server System P4000GP Family Firmware Update Package
for Intel(R) Deployment Assistant, Intel(R) One Boot Flash Update Utility, 
The embedded EFI Shell, Windows* Preboot Execution Environment 
================================================================================
Intel Enterprise Platform & Services Division - Marketing
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================
DATE    : Sep. 28, 2012
TO      : Intel(R) Server Board S2400GP Family
	  Intel(R) Server System P4000GP Family customers
SUBJECT : Release Notes for System Firmware Update Package 
================================================================================
                              ABOUT THIS RELEASE
================================================================================
BIOS   : 01.06.0002
ME     : 02.01.05.107
BMC    : 1.16.4010
FRUSDR : 1.05
================================================================================
                           Support Platforms and Dependency
================================================================================
Processors supported: 
Intel(R) Xeon processor E5-2600/2400 series

Microcode update versions:
Intel(R) Xeon processor E5-2600/2400 series C0 stepping: 0x80000513 CPUID = 0x206D5
Intel(R) Xeon processor E5-2600/2400 series C1 stepping: 0x80000619 CPUID = 0x206D6
Intel(R) Xeon processor E5-2600/2400 series C2 stepping: 0x8000070D CPUID = 0x206D7

Production boards:
  Product		    Fab Version	      
  S2400GP		    Fab2 or above     

Before update to the BIOS/ME/BMC/FRUSDR contained in the package, please check in BIOS 
set up menu and verify your board has below BIOS/ME/BMC/FRUSDR versions installed:

  - BIOS 01.02.2002, or later Version
  - ME 02.01.05.69 or later Version
  - BMC 01.00.2812 or later Version
  - FRUSDR 09 or later version

The following update process must be followed to ensure a trouble free update.
1.	BMC firmware to 1.00 or later
2.	BIOS 01.01.1002 or later
3.	Manageability Engine (ME) firmware 02.01.05.69 or later
4.	Latest FRU/SDR package specific to the baseboard.

================================================================================
                  System Firmware Update Package Usage instructions                   
================================================================================
This package can be updated using one of the following methods:
 - The embedded UEFI shell
 - Intel(R) Deployment Assistant
 - Windows* or Linux* operating system using Intel(R) One-boot Flash Update (OFU)
   V11.0 Build 10 or later)
 - Windows* Preboot Execution Environment (WinPE)

To Update from the embedded EFI Shell

update system firmware from Intel server EFI shell by the following steps:
- Download Intel server system firmware update package from http://www.intel.com/support/
- Unzip package and copy all files to root folder in USB disk on key 
- Insert USB disk on key to server USB port
- Reboot server, system will start BIOS/BMC/FRUSDR update automatically

  If case for some reason or you didn't put unzipped package under root folder of USB key, 
  you can do it by:
- Reboot server to EFI shell manually
- Run command "map -r" in EFI shell to mount USB disk on key
- Run command "fs0:" to change folder to USB disk on key, USB key may also mount to
  fs1:. The number of "fs" is dependent on the result of command "map -r"
- Change folder to the folder storing the firmware package
- Run command "startup.nsh" to start firmware update process

Please refer to "EFI_Instructions.pdf" in this firmware package for a quick guide to 
use the EFI commands

To Update from Intel(R) Deployment Assistant (IDA)

The Intel(R) Deployment Assistant software is easy to use and is present on the 
"Intel(R) Server Deployment & Management" DVD shipped with the system.
User can download the latest version IDA CD ISO image from http://www.intel.com/support/
To use the IDA CD to update the system firmware:
- Boot server with IDA CD
- Select "Get System Updates" 
- Choose one of the three options 

  . From http://www.intel.com/support/
    Automatically downloads the latest Firmware Update Package from Intel 
    It requires Internet connection
    Enter your local IP address and proxy configuration
    Click "Next" to start the download and update process

  . From my network
    Download the latest Firmware Update Package from http://www.intel.com/support/ and copy 
    it to a Windows* shared folder
    Enter your local IP address, the Windows* file server name, and a
    Windows user name and password
    Select the firmware package in pop-up window
    Click "Next" to start the update process

  . From USB Disk on Key or Hard Disk
    Download the latest Firmware Update Package from http://www.intel.com/support/ and copy it 
    to a USB key, then insert the key into the server USB port
    Click "Browse"
    Select the firmware package in pop-up window
    Click "Next" to start the update process
    
  Note: The Firmware Update Package is in the ZIP file format. Do not unzip 
        before copying to a Windows* shared folder or USB disk.

To update from Windows* and Linux* or operating systems using the Intel(R) One Boot
Flash Update Utility (OFU)

Intel(R) One boot Flash Update utility can be downloaded from http://www.intel.com/support/
and it is part of the "BIOS, Firmware Update & Configuration Utilities" for 
Windows* and Linux*. Please refer to Intel OFU user guide about the details of 
installation and usage of OFU.

Use OFU to update system firmware by the following steps:
- Install OFU on Windows* or Linux* system
- Download the latest firmware update package from http://www.intel.com/support/
- Unzip package to a folder
- Run the following command in Windows* command line/Linux* terminal window:
  <OFU install folder name>:\flashupdt -u  <package folder name>\flashupdt.cfg
                       
To update from Windows* Preboot Execution Environment (WinPE)

The System Firmware Update Package can be inserted to Windows* PE customized image 
for creating a bootable Windows* PE CD. User is able to update system firmware from 
customized WinPE CD by the following steps:
- Boot server with customized WinPE CD
- Run script "WinPE21_x64_Update.bat" or "WinPE20_x86_Update.bat" 
  (name may be varied depends on your own customization)
  
Note:
1. The Intel(R) OFU utility is case sensitive. Therefore, when you transfer the 
Firmware Update Package using USB key from a Microsoft Windows* system to a Linux
environment, you must first extract under the Linux* environment. Otherwise, you 
will need to mount the USB key manually with 'vfat' option under Linux to avoid 
conversion from upper case to lower case and vice versa.

2. To make Intel(R) OFU utility run properly under x86 or x64 OS, you have to read
OFU releaenotes on known issues for OFU installation.

3. In this SFUP package, Intel only provide batch file "WinPE_x86_Update.bat"
for WinPE2.0 32 bit solution "WinPE_x64_Update.bat" for WinPE2.1/3.0 64 bit 
solution as an example. Please refer to white paper "White Paper-Intel Server 
Utilities Procedure for WinPE.pdf" for details on building your own customized 
WinPE CD.

4. Windows PE 2.0 - built from Windows Vista SP1 32bit or EM64T
5. Windows PE 2.1 - built from Windows Vista SP1 or Windows Server 2008, EM64T
6. Windows PE 3.1 - built from Windows Server 2008R2, EM64T
7. Microsoft IPMI driver is loaded by default from WinPE CD, if you want to use 
Intel IPMI driver instead of MS IPMI driver for firmware update, you can un-install
Microsoft IPMI driver by:
                Devicesetup.exe ¨Cv remove *IPI0001
                Note: IPI0001 is the device ID for Microsoft IPMI driver.

=================================================================================   
 	            BIOS changes since 01.03.0002
=================================================================================  
Others:
- Add fix to avoid the potential issues by limiting the PCIe slot speed to Gen2 unless
  the add-in adapters are PCIe Gen 3 qualified on the Intel?Server Platforms.

- Fixed: Remove NUMA setup option in Intel(R) Server Board S1400SP.            
- Fixed: IO_MOD/SAS_MOD slot number is displayed incorrectly in Microsoft* Windows* 2008.      
- Fixed: When the PCIe slot option ROM is set to disabled in BIOS setup, the option RoM is still enabled. 
- Fixed: WHEAHCT Logo Test fails in some Microsoft* Windows* certification.                
- Fixed: BIOS Setup screen may hang when loading efi image.
- Fixed: Some USB devices can not be recognized in Bios USB configuration page.

Others:
 - Update onboard SATA and SAS RAID option rom versions 
 - Update MRC rev. to 01.00.00.18
 - Display RAID configuration page in Quite Boot Mode when option rom is dispatched
 - Add PCIe Performance Tuning Knobs setup items
 - Add warnings in post screen when showing the capacity of the onboard RAID controller
 - Add memory 1866Mhz support for some platforms
 - Add fix in SMM hook in the runtime service
 
- Fixed: User privilege of RMM4's channel3 mismatch with BIOS setup.
- Fixed: Abnormal items will be displayed in PCIe slot OPROM control page after 
         pressing F9 and then discard changes.
- Fixed: Onboard NIC can not be disabled through BIOS setup on Intel(R) Server board S2600IP.
- Fixed: There is "unknown device" in boot order when USB floppy plugs.

Others:
- Add Intel(R) Server Board S1400SP support.
- Fix some compatbile issue on memory Dimms with Atmel sensor.
- Update processor microcode.

- Fixed: There are some error information in smbios type 178 on some platform.
- Fixed: BIOS Server Management Screen is not compliant with specification.
- Fixed: No Type 10 information within the SMBIOS table.
- Fixed: Only Serial port B could be found under Serial Port Config on some product.
- Fixed: Fix a bug in redirecting a Microsoft* Windows* OS ISO image file to another 
         system from a remote client. 
- Fixed: Can not disable NIC1 port1 in BIOS setup on Intel Server Board(R) S1400SP.
- Fixed: Some failures in SMBIOS Type 8 and Type 10 structure.
- Fixed: No ACPI S1 peripheral wake support under Red Hat* Linux 6.2 on Intel Server 
         Board(R) S4600LH.
- Fixed: Workaround for SDR Version incorrect in some cases.

Others:
- Add enable/Disable Option for PCIe option Rom.
- Add support socket 3 and 4 in Legacy VGA socket on Intel Server Board(R) S4600LH.
- Add PCIE CTLE setting on Intel Server Board(R) S1400SP.

================================================================================
	            ME changes since 02.01.05.91
================================================================================
- Fixed: FW may hang in initialization state after the update of entire ME
         region is interrupted by AC loss. 
         - None of the available ME resets (AC cycle or Global Reset or Power
           Button Override) can get ME out of the error condition, only
           reflashing ME image. 
- Fixed: FW may become unresponsive after switching from Recovery to
         Operational (e.g. during Direct Update).
         - Global Reset or Power Button Override can’t get ME out of the error
           condition. 

================================================================================
                    BMC Changes since release 1.10.3560
================================================================================
- Fixed: System power statistics shows N/A on EWS.
         - Power statistics were not available via Web interface when the PMBUS
           cable was connected.
- Fixed: Update power supply firmware for selected supplies to handle a PSON
         strobing issue which was causing problems on some systems.

- Fixed: S2600CO: Update SDR to version 1.09. 
- Fixed: W2600CR and S2600IP: Update SDR oto version 1.09. 
- Fixed: S2400GP: Update SDR to version 1.06. 
- Fixed: S2600GL/S2600GZ: Update SDR to version 1.05
- Fixed: S2400BB and S1400FP: Update SDR to current distro.
- Fixed: Corrects an issue where the BMC was generating incorrect SEL events.
         - The BMC will not generate SEL events for CPU presence when it starts
           up or after an SDR update, per requirement to exclude such events.
- Fixed: After enable lan failover, lan1 IPv6 address getting re-assigned by
         DHCPv6
- Fixed: RMM4 remote console port forwarding issue
         - Add support for handling network configurations with NAT/Port
           Forwarding between the browser and the BMC.
- Fixed: Embedded Web Server Sensor Readings are not correctly displayed after
         a SDR update and reset or a DC cycle.
         - Was requiring an AC power cycle or a BMC Cold Reset before the
           sensor were displayed correctly.

- Fixed: S4600LH: Added another Platform ID (S4600LH DP).
- Fixed: S2400LP: Added SAS module Temp to this platform.
- Fixed: S4600LH: Update to FRUSDR17.
- Fixed: S1600JP: Update FRUSDR from version 0.05 to version 0.07.
- Fixed: Added power-state fixes for the following conditions:
         - Chassis power-off when i2c connection to PCH fails, now supports
           4-second power button shutdown
         - Allows user to configure OEM PEF to perform graceful shutdown if
           they wish. Default remains immediate hard-shutdown.
- Fixed: Power Statistics displays 0w instead of Not Applicable on Embedded
         Web Server page with a Non PMBus power supply
- Fixed: Issue command of "Enter Firmware Transfer Mode" through RMCP(IOL)
         interface, the completion code is successful.
         - Firmware transfer mode commands are now disabled over
           IOL/RMCP/RMCPP and will fail with 0xD4.
- Fixed: When Onboard NIC 1 is disabled, it also disables the RMM NIC and
         should not

- Fixed: For S2600JF and S2600WP:
         1. Add sensor # 2D to monitor address 0x90 on i2c bus 2.
         2. Add sensor # 28 to monitor address 0x94 on i2c bus 2.
         3. Alter sensor monitor code for 240VA Fault.
- Fixed: Re-enable 1600W PSU and update FW to version 0.9.53 for S3F and 00A
         PSU Models
- Fixed: S4600LH: Updated from FRUSDR15 to FRUSDR16 package
- Fixed: Remove Intel branding from virtual front panel background image.
         - Since this image is outside of the scope of Embedded Web Server OEM
           updates, we have removed the Intel branding so that OEMs can rebrand
           everything with only the EWS OEM updates.
- Fixed: S2400EP: RGMII_IBMC_RMM4_TXD_0 and RGMII_IBMC_RMM4_TXD_1 failing
         ringback specification and is non-monotonic
- Fixed: The last 8 bytes of OEM data of SEL record retrieved by IHC are
         different from SELVIEWER or Embedded Web Server SEL.
- Fixed: SMI timeout will not be triggered when low for 2 minutes.
- Fixed: Local Control Panel: Reboot system twice, the boot option still boot
         to NetBoot.
         - Boot option configured by LCP config menu will no longer permanently
           change the selection. It will now be applicable only for the next
           boot.
- Fixed: After BMC or FRUSDR update, power unit redundancy lost asserted and
         deasserted event generated in SEL
- Fixed: Power unit redundancy has been lost -Asserted/Deasserted" events
         occurred after BMC reset via Cold Reset/Enter-Exit Firmware Transfer
         Mode commands.
- Fixed: S1600JP: Execute "Get CR Configuration" command with 450W mini-ERP PS
         gets unexpected response.
         - The 450W mini-ERP power supply used with S1600JP does not support
           Cold Redundancy. The Get/Set CR Configuration commands have been
           changed to return 0x81 for S1600JP.
- Fixed: Remove power supply will trigger a unexpected 03-A/C lost deasserted
         log in SEL.
- Fixed: Status LED is blinking green and 01-redund lost can not be recovered
         after removing any one 460W power supply and insert 750W power supply.
- Fixed: BMC Automatic Update of HSBP FW Unstable and Impacting BIK Factory
- Fixed: MTT sensor scaling is incorrect in all SDR files.
         - Corrected for S4600LH
- Fixed: Random Temp and Voltage events logged in SEL during factory SEL Check
- Fixed: IPMITOOL cannot get chassis ID LED status if we use web console to
         turn chassis ID LED on or off.
- Fixed: IPMItool identify LED with wrong status
- Fixed: IPMI to get chassis ID LED results is not same as "Manually press to
         light on Chassis identify LED"
         - The Chassis Identification fields of the Get Chassis Status response
           were not set properly for all methods of turning on the ID LED. This
           change adds the status to all methods of turning the ID LED On/Off.
- Fixed: IPMI Chassis Control Power Down incorrectly initiates a clean shutdown
         of OS
         - The Chassis Control command to power off the chassis was implemented
           with the Power Button press. This started a Graceful shutdown
           instead of an immediate one. This change causes the Chassis Control
           command for power down to immediately power down.

- Fixed: Updated S1400SP SDR to FRUSDR0.05 package
         - Changed SAS module address to 0x98
- Fixed: Updated S1400FP SDR to FRUSDR0.04 package
- Fixed: Updated S1600JP SDR to 0.07 package
         - Corrected the slave address for Full Height Full Length riser
           temperature device
         - Added new temperature sensors for new SAS module
- Fixed: Updated S2400BB SDR to FRUSDR1.00 package
- Fixed: Updated S2400GP SDR to FRUSDR1.05 package
- Fixed: Updated S2400LP SDR to FRUSDR1.08 package
- Fixed: Updated S2400SC SDR to FRUSDR1.05 package
- Fixed: Updated S2600IP SDR to FRUSDR1.08 package
- Fixed: Updated W2600CR SDR to FRUSDR1.08 package
- Fixed: Updated S4600LH SDR to FRUSDR0.15 package
         - Updated BB DDR Voltage SDR records
         - Added filtering logic
- Fixed: Added S4600LH baseboard FRU files for all the supported SKUs
         - S4600LH ROW with Intel(R) Ethernet Controller 10 Gigabit X540
         - S4600LH ROW with Intel(R) Ethernet Controller I350-AM4
         - S4600LH LAN with Intel(R) Ethernet Controller 10 Gigabit X540
- Fixed: S1600JP: Changed Mac0 Drive strength to conform to SI/EAs requirement

- Fixed: Green status LED keeps blinking after rearming the Power Unit
         Redundancy sensor.
         - When using manual rearmed sensor with deassertions disabled, status
           LED would not go back to green.
- Fixed: After issuing a turn off KVM services command, Launch Console button
         allows KVM to be launched, but KVM is not available, it will pop-up
         "Socket Error" message
- Fixed: In LCP, all the SEL entries are displaying in EVT MENU but it should
         not display informational events.
         - Only current active events in the system need to be displayed when
           the EVT menu item is selected for LCD.
- Fixed: Incorrect event "Redundancy regained " when PSU plugged in but no AC
         power applied.
- Fixed: BMC does not use a consistent IPv6 DUID

- Fixed: Updated S2400BB FRUSDR
- Fixed: Updated S4600LH to FRUSDR14 release
- Fixed: ADM1276 fails to respond after NACK.
         - Workaround developed and applied.
- Fixed: S2600CO customer SKU showing System Fan RPM 0.
- Fixed: S4600LH After CATERR the system halts instead of rebooting
- Fixed: S4600LH SMI timeout not triggered after 2 minutes
- Fixed: S4600LH Fan fault LEDs not working for system fan 7 to 11
- Fixed: Vlan help page of Embedded Web Server shows incorrect info.
         - Changed help page to align with functionality.
- Fixed: Typo errors found in Embedded Web Server
         -Virtual Front Panel help, IPv6 Network Setting Page, Alerts help
- Fixed: Onboard VGA cannot setup to highest resolution (1920x1080 up)
- Fixed: BMC FAN PWM freq reduced to 11KHz from 22KHz
         - Did not affect fan speed control functionality
- Fixed: S4600LH DIMM thermal trips on P3 and P4 being incorrectly reported
- Fixed: S4600LH Processor DIMM Thermal Margin sensor reading unavailable when
         in a 2 processor configuration
- Fixed: The description of NM Exception event is incorrect on Embedded Web
         Server.
- Fixed: With Intel(R) RAID Expander RES2SV240 connected, Drive "locate" action
         needs 10 to 30 seconds before the drive is blinking
- Added: Detect the node presence in chassis. Provide an OEM command to respond
         with data that indicates which nodes are populated in a multiple node
         system.

- Fixed: Updated S1400FP FRUSDR
- Fixed: Updated S4600LH FRUSDR zip file to version 13
- Fixed: Corrects S4600LH Fan tach calculation based on the fan scaling record
- Fixed: S1400SP Set MAC0 drive strength to improve Signal Integrity
- Fixed: Seeing all DIMM thermal margin sersors failing and providing a invalid
         reading
- Fixed: S1400FP The status LED is solid amber for longer than expected after
         an AC power cycle
- Fixed: S4600LH DIMM Mapping information on DIMM Thermal Trip event is
         incorrect but correct on Embedded Web Server DIMM Information.
- Fixed: S1400SP shows no socket present in CPU information page of EWS.
- Fixed: There are two 2 NMI assertion SEL events occurring when NMI pulse is
         generated.
- Fixed: S2400BB The fan fault LED did not light with a broken fan installed
- Fixed: Default LCD banner text when server with normal health is displaying
         some junk characters at the end.
- Fixed: LCD - After selecting Error as the banner, with Server Health as
         normal, the banner text is displaying as "No Error" instead of "System
         Health OK"
- Fixed: LCD - SN [Server Name] displays different values at VIEW menu and
         when SN selected as a banner.
- Fixed: LCD default screen after power on is incorrect
- Fixed: System reset instead of powering off when power button was pressed
- Fixed: No response to IPMI commands after an AC power cycle when LAN failover
         enabled with DHCP
- Added: Implements IPMI command extension to permit user to set a custom text
         string to display as the banner text on the LCD. Can also be set via
         BIOS in setup.

================================================================================
                    FRUSDR Changes since release 1.02
================================================================================    
- Follow Granite Pass FSC config sheet Rev (2.9).
- S2400GP.sdr: Modify "front panel" FRU Entity ID from 0x07 change to 0x0C.
- S2400GP.sdr: Modify "front panel" FRU Entity Instance from 0x37 change to 0x01.
- S2400GP.sdr: Modify "Baseboard" FRU Entity Instance from 0x36 change to 0x01.
- S2400GP.sdr: Modify "SAS Module" FRU Entity Instance from 0x31 change to 0x01.
- S2400GP.sdr: Add SDR Type 11 Record "Pwr Supply 1 FRU".
- S2400GP.sdr: Add SDR Type 11 Record "Pwr Supply 2 FRU".
- S2400GP.sdr: Add SDR Type 11 Record "HS Backplane 1".
- S2400GP.sdr: Add SDR Type 11 Record "HS Backplane 2".
- S2400GP.sdr: Add SDR Type 11 Record "HS Backplane 3".
- Follow Granite Pass FSC config sheet Rev (3.0).
- Update FRUSDR utility Version 11.0 Build 9.
- S2400GP.sdr: Modify HDD number.
- S2400GP.sdr: Add SAS Module Presence.
- Follow Granite Pass FSC config sheet Rev (3.1).
- Update FRUSDR utility Version 11.0 Build 11.
- S2400GP.sdr: Power unit redundancy sensor "Capabilities" change to 00.

=============================================================================
                            LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products. 
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation may 
have patents or pending patent applications, trademarks, copyrights, or other 
intellectual property rights that relate to the presented subject matter.  
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any 
such patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product 
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 
*Other names and brands are the property of their respective owners.
Copyright (c) 2012 Intel Corporation.

A portion of this firmware is open source code, which falls under the
GPL 2.0 license.  

[END OF RELEASE NOTES]
