Intel® Graphics Media Accelerator 600
Graphics Controller Diagnostic Utility
Version 3.0.1
Diagnostic Utility Release Notes

PV 1.0 Version 3.0.1 (Intel® Graphics Media Accelerator 600)

April 7, 2011

DISCLAIMER: Information in this document is provided in connection with Intel products. No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. Except as provided in Intel’s Terms and Conditions of Sale for such products, Intel assumes no liability whatsoever, and Intel disclaims any express or implied warranty relating to sale and/or use of Intel products, including liability or warranties relating to fitness for a particular purpose, merchantability or infringement of any patent, copyright or other intellectual property right. Intel products are not intended for use in medical, lifesaving, or life-sustaining applications.
Intel may make changes to specifications and product descriptions at any time, without notice.
Contact your local Intel sales office or your distributor to obtain the latest specifications and before placing your product order.
* Other brands and names are the property of their respective owners.
Copyright © Intel Corporation 1999-2009
NOTICE: The Intel® Graphics Media Accelerator 600 may contain design defects or errors described as “known issues” which may cause the product to deviate from expected performance. Current characterized known issues are documented in this update.

Revision History

Date | Revision | Version | Platforms | Draft/Changes
April 7 , 2011 | PV 1.0 (Intel Graphics Media Accelerator 600 ) | 3.0.1 | Intel Graphics Media Accelerator 600 | Fully Functional

Build 1 | Features Added, Diagnostics Utility
N/A | Diagnostic Utility | Initial release supporting Intel Oaktrail platform.
Build 1 | Resolved Issues, Diagnostics Utility
Tibet | Diagnostic Utility | None.
Build 1 | Open Issues, Diagnostics Utility
Known Issue | Diagnostic Utility | If OEM Diagnostics has been executed, the system must be rebooted prior to executing the VESA utility.