*++
;
;Copyright (c) 2009-2012, LAPIS SEMICONDUCTOR CO., LTD.  All rights reserved.
;
;Module Name:
;
;    iohsata.INF
;
;Abstract:
;    INF file for installing SATA device driver
;
;--*/

[Version]
CatalogFile=iohsata.cat
signature="$Windows NT$"
Class=hdc
ClassGuid={4D36E96A-E325-11CE-BFC1-08002BE10318}
Provider=%INTEL%
DriverVer=11/26/2012, 2.7.0.0

[SourceDisksNames]
1 = %DiskId1%,iohsata.sys,,

[SourceDisksFiles]
iohsata.sys = 1

[DestinationDirs]
DefaultDestDir = 12

[DriverFiles_XP]
iohsata.sys,,,0x20

[Manufacturer]
%INTEL%=OKISEMI,NTx86.5.1

[OKISEMI]
%PCI\VEN_8086&DEV_880B.DeviceDesc%=IOHSATA, PCI\VEN_8086&DEV_880B&CC_010601

[OKISEMI.NTx86.5.1]
%PCI\VEN_8086&DEV_880B.DeviceDesc%=IOHSATA, PCI\VEN_8086&DEV_880B&CC_010601

[IOHSATA]
CopyFiles=DriverFiles_XP

[IOHSATA.Services]
AddService = IOHSATA, 0x00000002, IOHSATA_Service_Inst, Miniport_EventLog_Inst

[IOHSATA_Service_Inst]
DisplayName=%IOHSATA.SvcDesc%
ServiceType    = 1      ; SERVICE_KERNEL_DRIVER
StartType      = 0      ; SERVICE_BOOT_START
ErrorControl   = 1      ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\iohsata.sys
LoadOrderGroup = SCSI Miniport
AddReg         = IOHSATA_Addreg
AddReg         = bus_type_ide

[IOHSATA_Addreg]
HKR, "Parameters\PnpInterface", "5", 0x00010001, 0x00000001
HKR, "Parameters\Device", "MaximumSGList", 0x00010001, 0x00000020
HKR, "Parameters\Device", "NumberOfRequests", 0x00010001, 0x40
HKLM,"System\CurrentControlSet\Services\Disk","TimeOutValue",0x00010001,0x00000014
HKR, "Parameters\Device", "DriverParameters", 0x00000000, "ForceResetOnResume=0;ForcePowerStateTransition=0;EnableActivityLED=0;FlushCacheThreshold=50;ForceRemovable=0;BlowHPA=0;SetModeTimeoutOnResume=30"

[Miniport_EventLog_Inst]
AddReg = Miniport_EventLog_AddReg

[Miniport_EventLog_AddReg]
HKR,,EventMessageFile,%REG_EXPAND_SZ%,%11%%IOLOGMSGDLL%
HKR,,TypesSupported,%REG_DWORD%,7

;*************************************************************
;These addreg sections should be used for non-SCSI miniports
;to indicate what STORAGE_BUS_TYPE they actually do support.

[bus_type_ide]
HKR, "Parameters", "BusType", 0x00010001, 0x00000003

[Strings]
INTEL="Intel"
PCI\VEN_8086&DEV_880B.DeviceDesc="Intel(R) Platform Controller Hub EG20T SATA AHCI Controller - 880B"
IOHSATA.SvcDesc="SCSI Miniport Driver for Intel(R) Platform Controller Hub EG20T AHCI SATA Controller"
DiskId1="Intel(R) Platform Controller Hub EG20T SATA AHCI Driver Installation Disk"

REG_EXPAND_SZ=0x00020000
REG_DWORD=0x00010001
IOLOGMSGDLL="\IoLogMsg.dll"