================================================================================
Intel(R) Server Platform S1200BT System Firmware Update Package for 
Intel(R) Deployment Assistant, Intel(R) One Boot Flash Update Utility, 
The embedded EFI Shell, Windows* Preboot Execution Environment 
================================================================================
Intel Enterprise Platform & Services Division - Marketing
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================
DATE    : Aug 10, 2012
TO      : Intel(R) Server Board S1200BTL/S1200BTLRM
SUBJECT : Release Notes for System Firmware Update Package 
================================================================================
                              ABOUT THIS RELEASE
================================================================================
BIOS   : S1200BT.86B.02.00.0040.092620121113
ME     : ME_02_02_00_049
BMC    : 1.15
FRUSDR : 1.16

Note: There is no separate firmware of the Hot-Swap Backplane FUP4X35HSBP for 
Intel(R) Server Board S1200BT server system. The Hot-Swap Backplane firmware 
is integrated into the BMC firmware.

Note: - IDA and OFU doesn¡¯t support ME downgrade from 02.02.00.036 or higher version 
        to 02.00.09.032 or lower version. EFI shell is applicable to do ME Downgrade
      - When updating BMC in IDA, IDA shows the ¡°Release level in the package¡± for 
        BMC version in Hex. E.g: 1.14 as 1.0e

================================================================================
                           Support Platforms and Dependency
================================================================================
This update package is for Intel(R) Server Board S1200BTL/S1200BTLRM and
			   Intel(R) Server System R1304BTLSFAN and
                           Intel(R) Server System R1304BTLSHBN and
                           Intel(R) Server System P4304BTLSFCN and
			   Intel(R) Server System P4304BTLSHCN.

Intel(R) Server Platform S1200BT family Processors supported: 
  Intel(R) Xeon(R) Processor E3-1200 series, 
  2nd Generation of Intel(R) Core(TM) i3 processor,
  Intel(R) Xeon processor E3-1200V2 series and
  3rd Generation of Intel(R) Core(TM) i3 processor.
  
Microcode update versions:
CPUID     Version      Status
Intel(R) Xeon processor E3-1200 series D1   stepping: 0x00000028 CPUID = 0x206a6 
Intel(R) Xeon processor E3-1200 series D2   stepping: 0x00000028 CPUID = 0x206a7 
Intel(R) Xeon processor E3-1200 series Q0   stepping: 0x00000028 CPUID = 0x206a7
Intel(R) Xeon processor E3-1200V2 series B0 stepping: 0x0000000C CPUID = 0x306a2
Intel(R) Xeon processor E3-1200V2 series C0 stepping: 0x00000007 CPUID = 0x306a4
Intel(R) Xeon processor E3-1200V2 series K0 stepping: 0x00000009 CPUID = 0x306a5
Intel(R) Xeon processor E3-1200V2 series D0 stepping: 0x00000004 CPUID = 0x306a6
Intel(R) Xeon processor E3-1200V2 series E0 stepping: 0x00000010 CPUID = 0x306a8
Intel(R) Xeon processor E3-1200V2 series E1 stepping: 0x00000015 CPUID = 0x206a9

On-Board Component Option ROM Versions:
	Integrated BMC Matrox VGA (S1200BTL) : VBE BIOS V3.8
	SM712 Video Option ROM (S1200BTS)  : v2.24.03r
	Intel Rapid Storage Technology     : v11.0.0.1339
	ESRT2 SWRAID (Legacy) Option ROM   : A.10.02251631I
	Intel iSCSI Boot Oprom             : v2.7.53
	82579 EEPROM Version               : v1.0
	82579 PXE Version                  : Intel(R) Boot Agent GE v1.3.65
	82574L PXE Version                 : Intel(R) Boot Agent GE v1.3.65
	Memory Reference Code Version      : v1.2.0
	TXT Framework BIOS Reference Code  : V1.0.0  
	SNB ACPI Reference Code Version    : V1.2.0
	System Agent Reference Code Version: V1.2.0
	Intel(R) SPS ME Firmware Package   : ME_02_02_00_049
      
================================================================================
                  System Firmware Update Package Usage instructions                   
================================================================================
This package can be updated using one of the following methods:
 - The embedded EFI shell
 - Intel(R) Deployment Assistant
 - Windows* or Linux* operating system using Intel(R) One-boot Flash Update (OFU)
   v11.0Build 10 or later)
 - Windows* Preboot Execution Environment (WinPE)

To Update from the embedded EFI Shell

Update system firmware from Intel server EFI shell by the following steps:
- Download Intel server system firmware update package from support.intel.com
- Unzip package and copy all files to root folder in USB disk on key 
- Insert USB disk on key to server USB port
- Reboot server, system will start BIOS/BMC/FRUSDR update automatically

  In case for some reason or you didn't put unzipped package under root folder of USB key, 
  you can do it by:
- Reboot server to EFI shell manually
- Run command "map -r" in EFI shell to mount USB disk on key
- Run command "fs0:" to change folder to USB disk on key, USB key may also mount to
  fs1:. The number of "fs" is dependent on the result of command "map -r"
- Change folder to the folder storing the firmware package
- Run command "startup.nsh" to start firmware update process


Please refer to "EFI_Instructions.pdf" in this firmware package for a quick guide to 
use the of EFI commands

To Update from Intel(R) Deployment Assistant (IDA)

The Intel(R) Deployment Assistant software is easy to use and is present on the 
"Intel(R) Server Deployment toolkit" CD shipped with the system.
User can download the latest version IDA CD ISO image from http://downloadcenter.intel.com/
To use the IDA CD to update the system firmware:
- Boot server with IDA CD
- Select "Get System Updates" 
- Choose one of the three options 

  . From http://downloadcenter.intel.com/
    Automatically downloads the latest Firmware Update Package from Intel 
    It requires Internet connection
    Enter your local IP address and proxy configuration
    Click "Next" to start the download and update process

  . From my network
    Download the latest Firmware Update Package from http://downloadcenter.intel.com/ and copy 
    it to a Windows* shared folder
    Enter your local IP address, the Windows* file server name, and a
    Windows user name and password
    Select the firmware package in pop-up window
    Click "Next" to start the update process

  . From USB Disk on Key or Hard Disk
    Download the latest Firmware Update Package from http://downloadcenter.intel.com/ and copy it 
    to a USB key, then insert the key into the server USB port
    Click "Browse"
    Select the firmware package in pop-up window
    Click "Next" to start the update process
    
  Note: The Firmware Update Package is in the ZIP file format. Do not unzip 
        before copying to a Windows* shared folder or USB disk.

To update from Windows* and Linux* or operating systems using the Intel(R) One Boot
Flash Update Utility (OFU)

Intel(R) One boot Flash Update utility can be downloaded from http://downloadcenter.intel.com/
and it is part of the "BIOS, Firmware Update & Configuration Utilities" for 
Windows* and Linux*. Please refer to Intel OFU user guide about the details of 
installation and usage of OFU.

Use OFU to update system firmware by the following steps:
- Install OFU on Windows* or Linux* system
- Download the latest firmware update package from http://downloadcenter.intel.com/
- Unzip package to a folder
- Run the following command in Windows* command line/Linux* terminal window:
  <OFU install folder name>:\flashupdt -u  <package folder name>\flashupdt.cfg
                       
To update from Windows* Preboot Execution Environment (WinPE)

The System Firmware Update Package can be inserted to Windows* PE customized image 
for creating a bootable Windows* PE CD. User is able to update system firmware from 
customized WinPE CD by the following steps:
- Boot server with customized WinPE CD
- Run script "WinPE21_x64_Update.bat" or "WinPE20_x86_Update.bat" 
  (name may be varied depends on your own customization)
  
Note:
1. The Intel(R) OFU utility is case sensitive. Therefore, when you transfer the 
Firmware Update Package using USB key from a Microsoft Windows* system to a Linux
environment, you must first extract under the Linux* environment. Otherwise, you 
will need to mount the USB key manually with 'vfat' option under Linux to avoid 
conversion from upper case to lower case and vice versa.

2. To make Intel(R) OFU utility run properly under x86 or x64 OS, you have to read
OFU release notes on known issues for OFU installation.

3. In this SFUP package, Intel only provide batch file "WinPE_x86_Update.bat"
for WinPE2.0 32 bit solution "WinPE_x64_Update.bat" for WinPE2.1/3.0 64 bit 
solution as an example. Please refer to white paper "White Paper-Intel Server 
Utilities Procedure for WinPE.pdf" for details on building your own customized 
WinPE CD.

4. Windows PE 2.0 - built from Windows Vista SP1 32bit or EM64T
5. Windows PE 2.1 - built from Windows Vista SP1 or Windows Server 2008, EM64T
6. Windows PE 3.0 - built from Windows Server 2008R2, EM64T
7. Microsoft IPMI driver is loaded by default from WinPE CD, if you want to use 
Intel IPMI driver instead of MS IPMI driver for firmware update, you can un-install
Microsoft IPMI driver by:
                Devicesetup.exe ¨Cv remove *IPI0001
                Note: IPI0001 is the device ID for Microsoft IPMI driver.

Warning: 
!!Do NOT reboot or shut down power from your system during following software update!!

Warning: 
!!The firmware for S1200BTL,S1200BTLRM and S1200BTS are different and BIOS0038 is just for S1200BTLRM.

Warning: 
!!BIOS R0038 and above cannot be downgraded to BIOS R0037 or earlier version On BTP RM SKU. 

================================================================================
                               BIOS Change in release R0040
================================================================================
- Fixed: NIC1 will be changed to disabled in BIOS after updating to BIOS R02.00.0037 on Intel(R) Server Board S1200BTL and Intel(R) Server Board S1200BTS.
- Fixed: HECI initialization failure when ME running in recovery mode.
- Fixed: Setup items "Intel VT for directed I/O" and "Console redirection" cannot 
         be updated through load default command line "iflash32.efi /rd."
- Fixed: HDDs LED amber blinking on Intel(R) Server System R1304BTLSHBN.

Other:
- Updated Microcode to revision 0x15 for Intel(R) Xeon processor E3-1200V2 series E1.
- Updated Microcode to revision 0x28 for Intel(R) Xeon processor E3-1200 series D2 and Intel(R) Xeon processor E3-1200 series Q0.
- Remove CPU Core Frequency in BIOS setup.

================================================================================
                               BIOS Change in release R0038
================================================================================
- Added: Support Intel(R) Server Board S1200BTLRM SKU

================================================================================
                               BIOS Change in release R0037
================================================================================
- Fixed: It's countdown from 65535 seconds after auto reboot when UEFI install 
  OS w2k8 R2 64bit.
- Fixed: The IFlash32 /rd switch does not work on BTP.
- Fixed: Sync Romely implementation mechanism about function key(F2) show time 
  to user during entering setup engine.
- Fixed: Raise SMI calls fail for Any BIOS variables in OS GUID Partition.
- Fixed: Unable to get Server Management variables on BTP using SysCfg.
- Fixed: Keep the variable Maximum value unchanged compared to the previous 
  release R0035.

Other:
- Added: New setup option onboard NIC disable/Enable.  
- Added: The support to modify boot orders using some third party tool.
- Added: New setup option to Show CPU Core Ratio in Setup Menu.
- Added: New feature "Power on Password".
- Added: Update ME FW to SPS_02.02.00.049.

================================================================================
                              BIOS Change in release R0035
================================================================================
- Fixed: Errors logged in SEL when certain add-in video cards were installed.
- Fixed: SAS module RMS2AF040 is not detected when Intel(R) E3-1200V2 series 
  processors are installed.
- Fixed: When memory is installed in dual mode, BIOS setup reports the memory 
  as Independent mode.
- Fixed: 4k sector HDD's set as non-bootable causes the system to take 10 
  minutes to boot.
- Fixed: Intel(R) RAID controller RS5DB080 cannot be detected in the UEFI 
  environment when EFI optimized Boot is enabled in BIOS setup.
- Fixed: With Front Panel Lockout enabled in BIOS setup, the front panel NMI 
  button is still functional.
- Fixed: Server Management Settings cannot be configured using the SysCfg 
  utility.

================================================================================
                               BIOS Change in Release R0032
================================================================================
- Fixed: ME might enter recovery mode after some specific scenario on Intel(R) 
  Server Board S1200BTS.
- Fixed: Console redirection item is not shown correctly in BIOS setup page.
- Fixed: A bug relate to NMI function.
- Fixed: Adaptec 6445 compatible issue with Intel(R) Server Board S1200BTL.
- Fixed: Integrated BMC and RMM4 NIC settings in BIOS setup are gone after 
  load default.

Other:
- Update Intel(R) Rapid Storage Option Rom to the version v10.6.0.1091
================================================================================
                               BIOS Change in Release R0030
================================================================================
- Fixed: Incorrect error message in BIOS setup Error Manager after flashing the 
  BIOS.
- Fixed: With TXT enabled, a USB keyboard may become non-functional after as USB 
  flash drive is inserted/removed.
- Fixed: RMM4 password cannot be set in BIOS Setup.
- Fixed: When multiple USB devices are connected via a hub, some USB devices may 
  not be detected by BIOS.

Other:
- Added:	 Enabled ACPI S3 capability.

================================================================================
                               BIOS Change in Release R0029
================================================================================
- Fixed: SMBIOS flash data will be lost after a BIOS update. 
- Fixed: System hangs when getting SMBIOS flash data after the second reboot. 
- Fixed: DMIedit utility cannot write Board S/N and PBA in EFIx64 and Microsoft* 
  Windows*.

Other:

- Update: Microcode to revision 18.

================================================================================
                               BIOS Change in Release R0028
================================================================================
- Fixed: Hotplug not supported under AHCI mode.
- Fixed: System doesn't reboot properly with EUP LOT6 enabled.
- Fixed: Intel (R) RAID Controller RS2BL040 in S1200BTL: Pressing Ctrl+G will 
  not display RAID BIOS Console 2.
- Fixed: Microsoft* Windows* 2008 R2 cannot be installed properly with the NIC 
  ROM disabled.
- Fixed: Ambient temperature reading is incorrect.
- Fixed: When CTRL+I is pressed via remote console with Console Redirection 
  enabled, the system will hang.

Other:
- Update: Processor microcode to version 17.
- Added:  Intel (R) TXT support.
    
================================================================================
                               BIOS Change in Release R0027
================================================================================
- Fixed: System may hang during OS reboot testing.
- Fixed: SMBIOS Type 17 memory total width variable is incorrect.

Other: 
- Change: S1200BTSE SIO clock changed from 24MHz to 48MHz


================================================================================
                               BIOS Change in Release R0025
================================================================================
- Fixed: The video output during OS installation is larger than the intended 
  video resolution.
- Fixed: The system cannot be awakened on LAN from ACPI S1 sleep state.
- Fixed: After setting BIOS defaults and with the Admin password set, the Admin 
  password is not required to enter BIOS setup after the first reboot.
- Fixed: The Error Manager in BIOS setup incorrectly displays "B6A3--DXE boot 
  services driver Unrecognized" when a USB optical device is attached.
- Fixed: Installing Linux RHEL6* in AHCI mode creates errors in the dmesg log.
- Fixed: The BMC version number is not being correctly displayed in BIOS Setup.
- Fixed: Fan Speeds are not correctly displayed in BIOS setup on S1200BTS.

Other:
- Updated: SM712 OPRom to version 2.24.03p.
- Added:   NVRAM recovery feature. 
 
================================================================================
                               BIOS changes in release R0024
================================================================================
- Fixed: Server Active Console is not available on the remote console.
- Fixed: Bios settings cannot be changed after running 'syscfg /bldfs' to load 
  Bios defaults.
- Fixed: Microsoft Windows 2008* R2 64 bit fails to load when using an LSI* 
  20320 RAID adapter.
- Fixed: BIOS Admin password gets cleared after loading BIOS defaults <F9>.

Other:
- Updated: Fan Speed Control.
- Enabled: Global reset after ME update.
- Updated: SM712 VBIOS to version2.24.03n

================================================================================
                      BIOS Changes in release R0022
================================================================================
- Fixed: System hangs when there is only one hard disk in the boot order device 
  type.
- Fixed: System Acoustics and Performance: Selectable options are incorrect.
- Fixed: SE Video has no output from slot5 using a VGA video card.
- Fixed: Admin Password is cleared after loading BIOS defaults.
- Fixed: Cannot boot from a USB device that emulates a CD-ROM.
- Fixed: The Help Text descriptions of BIOS items are not consistent. 
- Fixed: ME update displays 0.0.0.0 in BIOS setup after update.
- Fixed: System Boot Timeout is incorrect; the default should be zero.
- Fixed: Microsoft* Windows* installation to iSCSI target fails. 

================================================================================
                      BIOS Changes in release R0018
================================================================================
- Fixed: The Serial Port Console Redirection cannot be set to enabled.
- Fixed: Console redirection is non-functional after ME update.

Other:
- Update: Intel(R) Xeon processor E3-1200 series D2 stepping Microcode(uCode) to v14.
================================================================================
                      BIOS Changes in release R0016
================================================================================

- Initial production BIOS release for the Intel(R) Server Board S1200BT.

===============================================================================
                            ME Changes in release 02_02_00_049
===============================================================================
- Fixed: ME does not recognize proper CPU ID when host change power state from
         SX to S0.
- Fixed: When ME FW met an exception during platform power state transition,
         the platform could not finalize the transition (host will hang).
- Fixed: ME FW may reset itself during host reset when there is no receiver on
         IPMBus for IPMI messages generated by ME.
- Fixed: ME FW may reset itself during host reset with power cycle.
- Fixed: When ME FW configuration on flash is wrong ME may permanently stay in
         transitioning between Operational and Recovery instead of staying in
         Recovery after few tries.
- Fixed: NM power limiting functionality is not working on Intel(R) Xeon(R)
         processor E5-4600/2600/2400/1600/1400 v2 product families with 17
         watts TDP power.
- Added: This release contains fixes in the ME recovery boot loader section.

===============================================================================
                      ME Changes in release 02_02_00_036
===============================================================================
- Fixed: Sometimes the platform is not booting when the Operational image is
         corrupted, ME is not responding.
- Fixed: MEInfo does not show ME features set when ME is in Recovery mode. Also
         Recovery image version is not shown.
- Fixed: HECI reset is not properly supported when ME is in Recovery Mode.
- Fixed: NM does not support DCMI1.1 commands defined in IPMI-spec.
- Fixed: VHD dynamic fusing is not working as expected.
- Fixed: When ME FW configured for operating in All Sx states and platform
         powered up from G3 to S5 power mode. ME FW will stuck during ME reset
         executed in recovery mode.
- Fixed: Get ME-BIOS Interface Version (HECI command) is not implemented in
         Recovery mode.
- Fixed: After Direct Update (without ME reset) Get FW Version HECI command
         returns version of the former image.
- Fixed: General NM Presets configuration in FITc application does not contain
         all S1200BT options.
- Fixed: There are power flow scenarios where ME recovery jumper does not reset
         ME configuration to factory defaults. The jumper is supposed to cause
         ME to enter recovery boot loader code and reset ME firmware
         configuration to factory defaults. The later sometimes does not occur.
- Fixed: Firmware Heartbeat in HECI-1 Extended FW Status register is not
         incremented as it is described in "ME-BIOS-SPS Firmware Interface
         Specification".
- Fixed: After sending the "ME Reset to defaults" IPMI command ME stops
         responding to IPMI commands for 8 seconds.
- Fixed: When Diagnostics service is enabled and Diagnostics Console is
         disconnected switching to Recovery via IPMI or HECI commands takes
         about 5 seconds.
- Fixed: Diagnostics console Compliance Test 1.2. "BIOS HECI Initialization
         message" gives unspecified state of "HECI Initialization message".
- Fixed: In case when flash erase limit has been reached ME generates ME
         Firmware Health event with the event data 3 equal to 0xD5 instead of
         0x01.
- Fixed: Resuming platform after S3 state fails on Intel(R) Xeon(R) processor
         E5-4600/2600/2400/1600/1400 v2 product families, also Dynamic Fusing
         will fail during Sx -> S0 transition.
- Fixed: If ME reset will be performed after AC cycle, then HMRFPO_LOCK HECI
         message will return invalid Nonce causing Direct Update failure.
- Fixed: If invalid image will be used for Direct Update and global reset will
         be issued for ME reset, then ME will state in Recovery mode and
         repairing broken image using Direct Update will fail (HMRFPO_LOCK HECI
         message will return invalid Nonce).
- Fixed: Active policy with Policy Exception Actions = 1 (Shutdown system) may
         sometimes unexpectedly shutdown platform even when power is properly
         capped.
- Fixed: Power Sensor Address set to 0x10 instead of 0x20 in Alert Immediate NM
         Health Event.
- Fixed: Power Reading polling is not working when Scan Period is set to 250 ms
         for BMC set as a Power Reading source.
- Fixed: Node Manager Exception Events are sent after every Correction Time.
         This behavior can cause SEL overflow.
- Fixed: Unexpected shutdown during aggressive policy operation. Sometimes
         aggressive policy could cause platform shutdown even if power limit
         was reached.
- Fixed: Node Manager Exception Event "Policy Correction Time Exceeded" comes
         after double correction time instead of one correction time.
- Added: Thermal policies support was added in current release.
- Added: This release contains fixes in the ME recovery boot loader section.
================================================================================
                      ME Changes in release ME_02_00_09_032
================================================================================
Issue Fixed:
- Sometimes, when ME is configured for operating in all Sx states and while
  platform is performing transition from G3 to S5 and later from S5 to S0, ME
  could be unexpectedly reset.
- Unexpected ME reset could appear during NM communication with some specific
  PSU, as a result of which the CPU throttling statistics could be violated.

================================================================================
                      ME Changes in release SPS_02_00_08_015_0
================================================================================
- Initial production ME release for the Intel(R) Server Board S1200BTL


===============================================================================
                           BMC Changes in release 1.14
===============================================================================
 

- Fixed: There is a typo error in BMC WebUI help document for "Alert Email" 
	 sub-menu
- Fixed: Can't disable an exist user in EWS
- Fixed: Encounter IPMI Error Code 6 or 204 when add or delete users through BMC 
	 WebUI
- Fixed: BMC NVRAM corrupt after DHCP configuration

===============================================================================
                           BMC Changes in release 1.13
===============================================================================
- Fixed: rKVM/Remote media client not tracking source port forwards
- Fixed: Cannot ping SUT with VLAN IP after AC Cycle and completed POST.
- Fixed: Diagnostic tests are unclear what they are supposed to do
- Fixed: OEM Timestamp and OEM Non Timestamped events not decoded correctly in
         Embedded Web Console and Embedded Web Console SEL dumps
- Fixed: Embedded Web Console SEL display page does not display the specific
         DIMM, CPU, and PCIE information for all DIMM, CPU, and PCIE faults
- Fixed: The BIOS does not save the BMC RMM4 IP configuration if NIC1 IP
         configuration also changed
- Fixed: In the Embedded Web Console, if the sensor is in "N/A" status, the
         indicative string is "OK" and should be "Unknown".
================================================================================
			BMC Changes in release 1.12
================================================================================
- Upgrade HSBP Firmware to 00.12
Issue Fixed:
 - Mount ISO image to RMM4 may cause "error reading video data" issue on S1200BT
   when using some network switches
   
================================================================================
			BMC Changes in release 1.10
================================================================================
Issue Fixed:
 - SEL keeps reporting rebuild/remap in progress,Deasserted/Asserted,and finally 
   fills up the SEL
 - HSBP PSOC FW reports drive presence not correct
 - The Connection to RMM4 from IASC will lost sometimes

================================================================================
			BMC Changes in release 1.09
================================================================================
Issue Fixed:
 - Remove UNC and UC threshold for VBAT sensor.

================================================================================
			BMC Changes in release 1.08
================================================================================
Issue Fixed:
- System Fan RPM 0 after running sometime on Intel(R) Server System R1304BTLSHBN.

================================================================================
                     BMC Changes in release 1.07
================================================================================
Issue Fixed:
 - BMC user SOL payload enable/disable status can't be saved across BMC reset issue.
 - HSBP PSOC FW reported drive presence not correct issue.
 
================================================================================
                     BMC Changes in release 1.05
================================================================================
Issue Fixed:
- Integrated BMC SMBus ACK hold time delay issue.
 
================================================================================
                     BMC Changes in release 1.04
================================================================================
Issue Fixed:
- Fixed 4 HSBP problems via including HSBP 0.6

================================================================================
                     BMC Changes in release 1.04
================================================================================
Issue Fixed:
- Fixed 4 HSBP problems via including HSBP 0.6

================================================================================
                     BMC Changes in release 1.03
================================================================================
Issues Fixed:
- Initial production BMC release for the Intel(R) Server Board S1200BTL.

================================================================================
		     FRUSDR Changes in release 1.15
================================================================================
Feature Added:
- Support Board S1200BTM.
- Update FRUSDR utility to FRUSDR11.0-Build12.
- Add BTP_BMC_RM.fru file into the package.

================================================================================
		     FRUSDR Changes in release 1.14
================================================================================
Feature Added:
- Add PV_VCC_SENSOR(0xE0) to support Intel(R) Xeon(R) E3-1200V2 Processors.
- Correct the comment for BB +3V Vbat record.

================================================================================
		    FRUSDR Changes in release 1.13
================================================================================
Feature Added:
- Add different stepping to support Intel(R) Xeon(R) E3-1200V2 Processors.
Issue Fixed:
- Cannot detect "Intel(R) Xeon(R) E3-1200V2 Processors" during the processing of FRUSDR update

=================================================================================
		   FRUSDR Changes in release 1.12
=================================================================================
- Add Intel(R) Xeon(R) E3-1200V2 Processors detection.

================================================================================
		     FRUSDR Changes in release 1.11
================================================================================
Feature Added:
- Divide sensor number 04h record into two, one is with chassis intrusion event mask, another is not.
  
================================================================================
		     FRUSDR Changes in release 1.10
================================================================================
Feature Added:
- Add Front Panel NMI tag
- Modify sensor type and event reading type for Mem P1 Thermal Trip.
- Add auto-detection for the next generation processor

================================================================================
		     FRUSDR Changes in release 1.09
================================================================================
Issue Fixed:
- Fan sensor multiplier for the 3rd party chassis.
- Remove displaying the prompt if no front panel sensor is detected.

================================================================================
		     FRUSDR Changes in release 1.08
================================================================================
Issue Fixed: 
 - 3V VBat upper critical/non-critical threshold value to FFh/FEh.

================================================================================
                     FRUSDR Changes in release 1.07
================================================================================
Issue Fixed:
- Add checking prod id mechanism.
- Correct OTHER chassis referring to front panel for stepwise.
- Modify fan speed range for 3rd party chassis.
- Update SDR as per Bromolow FSC Config Sheet.xls(v2.0).
- Change display for board name to S1200BTL and chassis code name.
- Modify Node Manager discovery record to support Node Manager Capabilities 
  and Threshold sensor.

=================================================================================
                    FRUSDR Changes in release 1.05
=================================================================================
Issue Fixed:
- Modify entity instance for entity id 07 to identical.

=================================================================================
                    FRUSDR Changes in release 1.04
=================================================================================
Issue Fixed:
- Change P4304XXSHBN domain 3 stepwise fan speed control value.
- Change HSBP target temperature for clamping to 52 degree.
- Add an OEM Node Manager Discovery record for SDR.
- Update SDR as per Bromolow FSC Config Sheet.xls(v1.9).

=================================================================================
                   FRUSDR Changes in release 1.03
=================================================================================
Issue Fixed:
- Unique the entity instance for each entity id.
- Add a condition for CPU fan shouldn't install for R1304XXS chassis detection.
- Update FRUSDR utility to FRUSDR10.0-Build05.
- Change file name to align BMC version.

================================================================================
                    FRUSDR Changes in release 11
================================================================================    
Issues Fixed:
- Switch sensor number for Board Inlet Temperature and iBMC Board Temperature sensor.
- Update P4304XXSFCN System Fan4.
- Remove chassis intrusion sensor for R1304XXS.

================================================================================
                    FRUSDR Changes in release 10
================================================================================    
Issues Fixed:
- Initial production FRU/SDR release for the Intel(R) Server Board S1200BTL.

=============================================================================
                            LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products. 
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation may 
have patents or pending patent applications, trademarks, copyrights, or other 
intellectual property rights that relate to the presented subject matter.  
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any 
such patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product 
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 
*Other names and brands are the property of their respective owners.
Copyright (c) 2012 Intel Corporation.

A portion of this firmware is open source code, which falls under the
GPL 2.0 license.  

[END OF RELEASE NOTES]
