This release note and the software that accompanies it are copyright (c) 2012, Intel Corporation or its suppliers, and may only be installed and used in accordance with the license that accompanies the software.

This Software is furnished under license and may only be used or copied in accordance with the terms of that license. No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. The Software is subject to change without notice, and should not be construed as a commitment by Intel Corporation or its suppliers to market, license, sell or support any product or technology. Unless otherwise provided for in the license under which this Software is provided, the Software is provided AS IS, with no warranties of any kind, express or implied. Except as expressly permitted by the Software license, neither Intel Corporation nor its suppliers assumes any responsibility or liability for any errors or inaccuracies that may appear herein. Except as expressly permitted by the Software license, no part of the Software may be reproduced, stored in a retrieval system, transmitted in any form, or distributed by any means without the express written consent of Intel Corporation.

========================
Supported RAID Expanders
========================
This download supports Intel(R) RAID Expander RES2CV360-R, please verify that this utility has been tested with the RAID card you have chosen to use by checking the drivers web page for your controller at http://support.intel.com.

===================
Package Information
===================
Firmware Version v0.13.0.6
MFG Version 1.03

==========
Attention!
==========
N/A

==================
Known Restrictions
==================
1) Firmware upgrade requires the expander connected to proper Intel(R) SAS/RAID Host Bus Adapter (HBA), see below for the HBA compatibility list.

SAS Host Bus Adapter Compatibilty:
Intel(R) Integrated RAID Module RMS25JB040, RMS25JB080, RMS25KB040, RMSKB080, RMS2LL040, and RMS2LL080.
Intel(R) RAID controller RS25GB008

RAID Host Bus Adapter Compatibilty:
Intel(R) Integrated RAID Module RMS25PB080, RMS25PB040,RMT3PB080, RMS25CB080, RMS25CB040, RMT3CB080, RMS25CB080N and RMS25PB080N
Intel(R) RAID controller RS25AB080, RS25SB008, RS25DB080 and RS25NB008

On-board SAS Controller Compatibilty:
On-board SATA/SAS Capable Controller based on Intel(R) C600 chipset in Intel(R) Rapid Storage Technology enterprise (RSTe) mode. SAS feautre needs be be enabled by proper Intel(R) RAID C600 upgrade keys.

2) Firmware upgrade also requires proper operating system to perform.
Firmware upgrade through SAS host bus adapter is supported under Windows, Linux, and UEFI (EFI 2.0).
Firmware upgrade through RAID host bus adapter is supported under windows and Linux.
Firmware upgrade through On-board SATA/SAS Capable Controller is supported under Linux only.

=======================
Contents on the package 
=======================
The following files are included in this zip:

Name:								Description:
RES2CV360-R_FW0.13.0.6_MFG1.03_Update_Package.txt		This file
Windows\*							Windows update utility and support files including Firmware binary
Linux\*								Linux update utility and support files including Firmware binary
UEFI\*								UEFI update utility and support files including Firmware binary
License_v2.pdf							License Agreement
COPYING.NEWLIB.txt						License Agreement


==========================
Installation instructions:
==========================

Refer to the readme file under each sub folder for firmware upgrading instructions on different operation systems.

=============
Fixes/Updates 
=============
MFG
v.80
- Initial release

v.85
- Fixed connector type for ports 4-11 & 16-19

v1.0
- Initial release

v1.01
- Fix expander cascading

v1.02
- Only report front panel temp sensor

v1.03
- Increase Tx output on phy 0 -11 (External) to support up to 6 meter cables

FW
v0.13.0.3
- Initial release
- Supports element pages for Temperature, Cooling, Voltage, and Power Supplies
- Changed slot mapping to match PAS, A D & C are external connections, Drive backplanes should be connected to F, I, E, H, D, & G respectively for slot mapping 0 - 23
- FSC based off front pannel temperature sensor (If FP is not installed fans will run at full speed)

v0.13.0.4
- Add function to automatically create OEM page with SAS & Enclosure ID if not present.

v0.13.0.5
- Fix expander cascading
- Add power supply shut down command
- Fix fan rpm reporting

v0.13.0.6
- Add front panel over temp indication

