This release note and the software that accompanies it are copyright (c) 2013, Intel Corporation or its suppliers, and may only be installed and used in accordance with the license that accompanies the software.

This Software is furnished under license and may only be used or copied in accordance with the terms of that license. No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. The Software is subject to change without notice, and should not be construed as a commitment by Intel Corporation or its suppliers to market, license, sell or support any product or technology. Unless otherwise provided for in the license under which this Software is provided, the Software is provided AS IS, with no warranties of any kind, express or implied. Except as expressly permitted by the Software license, neither Intel Corporation nor its suppliers assumes any responsibility or liability for any errors or inaccuracies that may appear herein. Except as expressly permitted by the Software license, no part of the Software may be reproduced, stored in a retrieval system, transmitted in any form, or distributed by any means without the express written consent of Intel Corporation.

==========================
Supported RAID Controllers
==========================
This download supports Intel(R) RAID controllers using SAS software stack (RS2SG244, RS2WG160, RS2BL080, RS2BL080DE, RS2BL040, RS2MB044, RS2PI008, RS2PI008DE, RMS2MH080, RT3WB080, RS2VB080, RS2VB040), please verify that this utility has been tested with the RAID card you have chosen to use by checking the drivers web page for your controller at http://support.intel.com.

===================
Package Information
===================
Flash package = v12.13.0-0154 (firmware 2.130.383-2315)

==========
Attention!
==========
Intel recommends to loading Factory Default setting after the firmware upgrade which will not affect data on any existing array. To do so:
1. Reboot the system and login to the RAID BIOS Console. 
2. Select the controller and select 'Adapter Properties'->'Next'
3. Set the 'Set Factory Defaults' setting to 'Yes' and submit the change.
4. Reboot the system (the default settings are applied).
5. Re-configure to the desired settings in RAID Web Console2.

==================
Known Restrictions
==================
1) This download does NOT support EFI v1.1 environment. Please use the EFI shell command “ver" to identify the EFI version.
2) When 2 or more VDs are created, VD cache settings must be the same.

=======================
Contents on the package
=======================
The following files are included in this zip:

Name:							Description:
IR3_2108SASHWR_FWPKG-v12.13.0-0154_readme.txt		This file
COPYING.NEWLIB.txt					License Agreement
License_v2.pdf						License Agreement
MR410p.rom 						Firmware binary
update.bat						DOS firmware update batch file
update.nsh						UEFI firmware update batch file
CmdTool2\DOS\*						DOS update utility and support files 
CmdTool2\FreeBSD\*					FreeBSD update utility and support files
CmdTool2\Linux\*					Linux update utility and support files
CmdTool2\Solaris\*					Solaris update utility and support files
CmdTool2\UEFI\*						UEFI update utility and support files
CmdTool2\Windows\*					Windows update utility and support files


==========================
Installation instructions:
==========================

UEFI (EFI 2.0) instructions for updating RAID Firmware:
-----------------
   1. Download and extract all files to a local drive.
   2. Boot the target system to EFI shell. 
   3. Change directory to the local drive and directory containing the flash update files and the firmware image file.
   4. Type "update.nsh" or "efi\cmdtool2 -adpfwflash -f MR410p.rom -noverchk -aall"
   5. Wait for the flash to complete. Do NOT reboot the system during the update.

DOS instructions for updating RAID Firmware:
-----------------
   1. Download and extract all files to a local drive.
   2. Boot the target system to DOS. 
   3. Change directory to the local drive and directory containing the flash update files and the firmware image file.
   4. Type "update.bat" or "dos\cmdtool2 -adpfwflash -f MR410p.rom -aall"
   5. Wait for the flash to complete. Do NOT reboot the system during the update.

Windows and Linux instructions for updating RAID Firmware:
-----------------
The firmware update may be run from Within Windows or Linux using the appropriate versions of CmdTool2.
  In Windows, unzip the utility into the same directory as the rom file by typing 
      "cmdtool2 -adpfwflash -f MR410p.rom -aall". 
  The Linux CmdTool2 by running the rpm and then calling the utility from /opt/MegaRAID/CmdTool2 as 
      "./CmdTool2 -AdpFwFlash -f MR410p.rom -aall"

You can also use RAID Web Console 2 to update the RAID firmware. For more detail, please refer to the Intel(R) RAID Software User's Guide.

=============
Fixes/Updates 
=============
Package v12.13.0-0154
 Firmware - 2.130.383-2315
 - Invalid target ID after new logical drive creation
 - Support for mutlipath topology is broken
 - OEM on iMR FW update caused card to FW fault state and card cannot boot to OS
 - During Reconstruction (R0->R5) when system reboots the reconstruction doesnt resume. System hangs Megamon hit
 - OEM Rack BMC see clock stetching on I2C bus
 - adapterOperations.alarmControl is being set to 1 even if controller doesnot have alarm on board
 - Drive temperature is shown very high on Falcon
 - 9260-16i's drive locate/fault LED header doesn't work
 - Firmware halts when flashing components other than app.rom for OEM=9
 - PL library and files checkin for PL version 5.38
 - Not able to flash both 9265-8i and 9285-8e card with 5.3 patch 1 firmware.However, it is ok on 9266-8i
 - Dont interpret the cachecade BVD flags if the volume is created with old FW which does not support cachecade
 - Data Corruption during Raid Level Migration
 - MR5.4 - DATA Corruption - offline drive becomes automatically online during Raid Level Migration
 - Bad disk being serviced hung Linux boot for 2 hours
 - VD is degraded(automatically) after raid level migration R1 TO R5 (adding one drive)
 - Firmware enters megamon by system reboot after changing MFC OEM to 6
 - Set the Recovery mode page (WriteRetryCount and recoveryTimeLimit)

 - Current Access policy is not getting updated for iMR
 - Unable to open "Set Patrol Read Properties" in MSM with 2008-iMR
 - Data Corruption during Raid Level Migration
 - Add support for Ringbuffer and Dq compilation
 - disableHII: Needs to be updated from nvdata into MFCD
 - 9240-4i on BCM RX67Q-6S motherboard is not getting required memory resources on boot, on Linux it waits 5 minutes, resets the
 - multi path with Consistency Check LED behavior problem
 - Address Action Item SCGCQ00340495 (Check coding standard for structure OfuRequestState)
 - Unable to enable ocr using application due to FW ocr setting taking precedence
 - Support for mutlipath topology is broken
 - Bad disk being serviced hung Linux boot for 2 hours
 - During Reconstruction (R0->R5) when system reboots the reconstruction doesnt resume. System hangs Megamon hit
 - Auto Foreign import fails when controller is booted with pinned cache.
 - Provide the count of LBAs that are present in the sata bbm table
 - Enable or disable 512E using Applications
 - Fail the IO in case the medium error recovery is taking more time
 FCODE - 4.12.05.00
 UEFI_Driver - 0x05270000
 BIOS - 3.27.00
 Hii - 01.36.00
 - Hii enter black screen/timeout when user switching between fields/form sub_form and during Pd rebuild
 - Remove debug message which is not applicable for non Mercury customers
 NVDATA - 2.09.03-0045
 - Change the showSgpio activity to 0
 - Need OEM's "showSgpioActivity" setting set back to 0
 - Code review: correcting the delivery error
 WebBIOS - 6.0-51-e_47_Rel
 - Change BBU Mode description for Liberator batteries.
 PCLI - 4.04.20
 Medusa_Expander - SAS2XFW-25.05.04.00_MFGIMG-25.05.04.00
 ROMENV - 1.08
 BootBlockCommon - 09.250.01.219
 BootBlock - 2.02.00.00-0000

Package v12.12.0-0139
 Firmware 2.130.373-2022
 - If VD is secured while reconstruction is going on does not stay secured once reconstruction is done
 - Battery continually stating Battery Yearly Deep Discharge Relearn Pending. Please Initiate a manual Relearn
 - System hang on IBM machine with a critical boot message
 - Event (MR_EVT_CTRL_RESETNOW_DONE ) is not generated after OFU is completed
 - EEPROM corruption(BQ2060 errata) due to corrupted value of design Capacity written in FCC for iBBU07
 - INVALID SGL causes dump into montask, OCR does not recover. MonTask: line 377 in file ../../dm/mpt2/mptrec.c & MonTask: line
 - Firmware upgrade/downgrade not possible due to missing env stamping
 - Megamon issue when disabling the drive security on a MR controller with spun down FDE drives
 - OFU is not happening when tried to upgrade firmware
 - Flash of package with OFU request
 - Code review: With the new approach for CtrlOFUPossibleSet/Get() shutdown path broken
 - Copyback on a drive hits kill adapter
 - Firmware fails to return proper value when flashed same firmware image with different stamping with OFU request.
 - Data Corruption during Raid Level Migration
 - Code Review Defect: Correct the error in copy back path smart errors path
 - Controller always enter HSM when it is set to HCOE
 - PD clear operation is not handle correctly with spun drive drives
 - Out-of-bounds access (OVERRUN_STATIC) of an array "ar" in pdCopyBackSpinupCallBack
 - Out of bound access in LDBBMListInit
 - GetConnectorIndex() Out of bound array access
 - Not able to flash both 9265-8i and 9285-8e card with 5.3 patch 1 firmware.However, it is ok on 9266-8i
 - Out-of-bounds access (OVERRUN_STATIC) of an array "nvInfo->lockKeyBlob.keyCheck" in displayNvKeyInfo
 - Out-of-bounds access (OVERRUN_STATIC) of an array "ar" in pdDcmdRebuildCB
 - Multiple switch cases are not handles correctly in debug functions
 - Dont interpret the cachecade BVD flags if the volume is created with old FW which does not support cachecade
 - Unable to enable ocr using application due to FW ocr setting taking precedence
 - Support for mutlipath topology is broken
 - Improve foreign config import for iMR with mixed JBOD/RAID settings
 - Add NVDATA support to make 512 Emulated drive support as configurable for customers
 - iBBU07 - SOH bad will be declared for low capacity battery before starting learn cycle
 - iBBU07: EEPROM and register values will be updated to revised values at first boot after FW flash
 FCODE 4.12.05.00
 UEFI Driver 0x05210000
 - UEFI Driver fails SCT Test
 - Enhance critical boot message handling
 - UEFI Driver should check pMRCtrlInfo ->maxHANodes with > 1 to determine HAMR
 BIOS 3.26.00
 HII 1.33.00
 - Allows to select Cachecade VD as Boot device
 - HII will not allow config to be cleared no drives attached
 - HII while in safe mode locks up when entering View drive
 - HII: Disables all requirement for human input at boot time
 - Add MFI State error string for the new MFI stat error codes
 - Remove 'Adaptive Read Ahead' option from every MegaRAID management utility
 NVDATA 2.09.03-0041
 - Code review: correcting the delivery error
 - Disable emergencyspare for a customer
 WebBIOS 6.0-51-e_47-Rel
 PCLI 4.04.20
 MR 2108V FW Medusa Release SAS2XFW-25.05.04.00_MFGIMG-25.05.04.00
 ROMENV 1.08
 BootBlockCommon 09.250.01.219
 BootBlock 2.02.00.00-0000

Package v12.12.0-0124
 Firmware 2.130.363-1846
 - Battery continually stating Battery Yearly Deep Discharge Relearn Pending
 - System hang on OEM machine with a critical boot message
 - Code Review Defect: Correct the error in copy back path smart errors path
 - Controller always enter HSM when it is set to HCOE
 - Add NVDATA support to make 512 Emulated drive support as configurable for customers
 MR FCODE Driver release
 Signed UEFI Driver 0x05180000 (for Win 8 Secure Boot)
 BIOS 3.25
 HII 1.32.00
 - Manage SSD Caching is showing all the VD's in the list in HII.
 NVDATA  2.09.03-0039
 - Added enable512eSupport parameter in MR PARAMS PAGE in nvdata
 WebBIOS 6.0-51-e_47-Rel
 - Change BBU Mode description for Liberator batteries.
 PCLI 4.04.20
 MR 2108V FW Medusa Release SAS2XFW-25.05.04.00_MFGIMG-25.05.04.00
 ROMENV 1.08
 BootBlockCommon 09.250.01.219
 BootBlock 2.02.00.00-0000

v12.12.0-0111
Fixed Native configuration is no longer supported message in post
Fixed FW quiesces IO when LC starts on BBU even in "WB always" mode
Fixed Patrol Reads on SSD drives
Fixed Implemented the limited band charging
Fixed Megamon during Injecting errors to VD with 512e PDs on iMR controller
Fixed Native configuration is no longer supported message in post
Fixed CRC errors during TSOC communication
Fixed Update BBU eeprom offset 0x08 and 0x09 

v12.12.0-0102
Fixed Reboot Causes HSP to Revert to Unconfigured Good 
Fixed Adding/Removing FoD key causes Legacy BIOS to stop and not continue 
Fixed Amber LED flashes during copyback after rebuilding degraded VD 
Fixed recon starting and progressing in 1.21 HII 
Fixed R5/R6 enabled using FOD and do a OCR on controller;R5 VD comes up as foreign once OCR is done 
Fixed Querying SMART / PFA Status Returns All Zeros in Sense Data 
Fixed Clearing excess drive error 
Fixed FW fails to create configuration and utilites fail to report the VD size after the reconstruction. 
Fixed HDD powersave options still shown in Ctrl Info,VD info & VD creation menus of HII becase FW reports it supports PS 
Fixed SATA FDE disk not recognized as FDE, SAS model is 
Fixed Secured Drives Counts as Two Physical Drives 
Fixed Megamon during import of FC from MR to iMR contoller 
Fixed Battery is < 623mAH and LUNS in writeback mode 
Fixed Upon OCR, Recon Ghost LD needs to be created before WJ processing 
Fixed If you enable security on controller using FOD and create secure VD it goes missing upon reboot. 
Fixed 'clear' tasks on disks always show 0% complete when doing 'init' task on RAID volume 
Fixed BBU Charging gets disabled when Transparent Relearn fails to start due to low capacity 
Fixed PD other error counter never increments 
Fixed compilation issue 
Fixed Error message pop out in HII when set to factory default. 
Fixed Windows blue screen while in background rebuild process 
Fixed cannot auto rebuild while we put a clean - JBOD 
Fixed After OCR+reboot, user is asked to hit enter to ack the activated FOD features on OEM system. 
Added Change EDV values in iBBU07 to improve accuracy with aging batery packs 
Fixed while running IOs on VD using a cachecade WB VD FW goes to megamon 
Fixed Data curruption while running I/O's on R0 VD with CC r1 VD present. 
Fixed HII/HII browser sluggishness is seen when exiting browser, going to EFI WebBIOS, and then going back to HII browser 
Fixed IMR-Web Bios shown Configured drives option in Manage power save settings 
Fixed Grammatical error in WebBIOS. 
Fixed In WebBIOS, Drive Group Definition screen, enclosures should not be selectable in the Drives column 
Fixed In EFI-WebBIOS, the white bars do not match up under VD properties page. 

v12.12.0-0091
Added	CacheCade Pro 2.0
Added	support for RS2VB080, RS2VB040, RS2SG244, RS2WG160
Fixed	Port forward to main stream liberator maintenance
Fixed	disableOnlinePFKChange should be disabled for OEM. ELF doesn't show up for OEM
Fixed	Advanced features key have to be re-entered
Fixed	Controller does not work with pci set to nomsi in kdump kernel
Fixed	OEM requests qty of prints to be reduced in fw log for ibbu i2c communication retries
Fixed	HWR: 10M09: OEM requests ibbu i2c communication retries to be displayed in fw log
Fixed	10M09: HWR: Battery failed message during learn cycle
Fixed	CSET: BT1680: SATA workaround handles LBA incorrectly for 6-byte read CDB - (SCGCQ00213383)
Fixed	Code review defect to checkin merge double copy
Fixed	Intermittent RAID key failure during power-on
Fixed	HWR: 10M09: too many messages in fw log "ArDiskTypeMisMatch : SAS_SATA_MIXING_VIOLATION¡±
Fixed	Potential DI issue while running the IO on degraded R5 VDs with 32 drives.
Fixed	HWR: 10M09: Patrol Read fails on R1 with around 2000 double medium errors
Fixed	HWR: 10M09: additional reboot required after updating ibbu FCC to design capacity
Fixed	 MR bios show "adapter at baseport is not repoonding" intermittence
Fixed	wrong slot # reported by megaraid compared to physical slot for EG disk
Fixed	FoD features will not activate or deactivate
Fixed	Logical Unit ID (VPD page 0x83) changed after foreign import
Fixed	SL1:LSI Mega RAID SAS-MFI BIOS Register state 0xF0010002
Fixed	LDBBM entries are incorrect after foreign import
Fixed	UnconfigGood PD fails to kick in as EHS (Emergency Hot Spare)
Fixed	R1 rebuild hangs at 50% mark after CC is run
Fixed	Enable PCI capability Bit for VPD exsupport.
Fixed	10M09: MR: Multibit ECC error with customer Liberator MR board and vmware ESXi5.0
Fixed	Disk performance disparity between WB controller cache on and off on system disks
Fixed	10M09: Older ibbu batteries display 65K capacity and are marked SOH bad
Fixed	Enabling security causes the config to be missing, and a configured FDE array to be seen as foreign on reboot.
Fixed	 M1015 Dimmer Switch - all Dimmer Switches must be disabled by Default
Fixed	10M09: Request FW to not mark ibbu battery as bad when very high capacity is detected
Fixed	Pulling VD 0 from an R60 and rebooting, 2 foreign configs when array 0
Fixed	Fw broke into MegaMon while writing a test file to a VD (R6) from a non MR disk.
Fixed	TDA 5015 Batteries Not Charging
Fixed	Alarm sounds with online VD's after flashing latest 10M09 Patch 16 firmware (2.120.163-1343)
Fixed	HWR: 10M09: No data is copied to target array after more than 15 secs
Fixed	HWR: 10M09: unexpected Power State Change events occur
Fixed	HWR 10M09 can't sustain at least 950 MBps performance with Cache Flush setting 1 sec
Fixed	10M09: HWR: Battery failed message during learn cycle
Fixed	10M09: HWR: FW automatically starts learn cycles on ibbu08 every reboot
Fixed	M1015 Dimmer Switch - all Dimmer Switches must be disabled by Default
Fixed	Change Niwot/BBU-08 support Firmware Mode5 WB capacity from 960mAh to 674mAh for low power DDR-2
Fixed	dummyd-efect version upgrade
Fixed	MegaCli prematurely returns exit 0x0 status on drive firmware flash
Fixed	10M09 P16 set properties command fails
Fixed	Sepaton noticed additional fan speed event messages every 2 minutes
Fixed	HWR: FW seems to incorrectly mark ibbu's SOH bad (iBBU07, ibbu05, ibbu01)
Fixed	HWR: 10M09: DelaySOD is not working on customer Liberator boards
Fixed	HWR: 10M09: configuration becomes foreign after fw fails 3-4 attempts to access raid key during boot
Fixed	Liberator FW 10M09 cause system (sles11sp1/rhel6) reset while lspci -vvx
Fixed	HWR: 10M09: extended retries of write verify command causes driver timeout
Fixed	BBUmode incorrectly set
Fixed	"Non-Transparent" learns seen with Mode 3

v12.12.0-0051
1) Fixed No event is generated when fan in enclosure fails 
2) Fixed Medium error handling fixes for >2TB 
3) Fixed PCR 235 Warning for High Error Counts 
4) Fixed Add SGPIO for Medusa 

v12.12.0-0048
1) Fixed firmware incomplete Writes During Power Fail and Recovery due to controller due to discarded controller cached data.
2) Fixed MegaRaid FW does not wait at post, code added to handle this condition.
3) Fixed (HSAXXXX) The new event can't be logged. 
4) Fized Red LED is lit on the next empty slot in an AIC/Xtor JBOD if the empy slot is immediatly after an array member 
5) Fixed MR FW reports "Unexpected sense, Invalid field in CDB" for LOG SENSE command sent to Seagate drives 
6) Fixed Label of Virtual Disk not provided by Drive Identify Command 
7) Fixed SMART predictive failure detection takes longer in 10M09 than 10M06 
8) Fixed Firmware Incompleted Writes During Power Fail and Recovery 
9) Fixed Enable/disable of HDD cache doesn't appear to work 
10) Fixed HWR: Fw log should indicate if a created/existing VD is already initialized 
11) Fixed MegaCli -AdpAllInfo shows BBU is not supported for Castor cards 
12) Fixed DC found when rebuild is progressing on R1 VD with media error under IO. 
13) Fixed Unable to import a Foreign Configuration
14) Fixed Power save mode hangs firmware causing driver to send kill adpter command
15) FIxed Liberator FW 10M09 cause system (sles11sp1/rhel6) reset while lspci -vvxxx is used
16) Fixed FW doesn't detect the iBBU08 if it is remotely mounting with OEM's Castor controller
17) Fixed FW revision is not displayed in the Bios' controller list
18) Fixed Remove JBOD message from BIOS POST if FW doesnt support it
19) Fixed Provide mechanism to bypass settings delayPOST and envDelaySOD
20) Fixed With multipath setting, found data miscompare while IOs across 2 enclosures
21) Fixed I/O miscompares when issue OCR.
22) Fixed Liberator FW 10M09 cause system (sles11sp1/rhel6) reset while lspci -vvxxx is used
23) Fixed Inconsistent drive state after drives are changed to different slots.
24) Fixed Controller hit montask during BGI
25) Fixed FW hit montask at pd.c when rebuilding from raid 6
26) Fixed Clear configured with SSC degraded causing FW went to mon_tsk()
27) Fixed Configured PDs become not supported PDs, LDs dropping offline. 
28) Fixed Controller reports "phy is bad" for single port with any SATA device 
29) Fixed HSP commissioned alarm beep goes away after reboot 
30) Fixed Application has advanced software options listed. This needs to be removed for OEM 
31) Fixed sscd show 0 byte in debugger and MSM 
32) Fixed ekms bios is not enable 
33) Fixed FW aborts the recovery resulting SES not responding 
34) Fixed Drive comes up as unconfigured bad while running power cycle and error injection script 
35) Fixed DateOfFirstuse is Incorrectly Causing BBU Deep Discharge Requirement 

v12.12.0-0036
1) Fixed FW causes Fatal Error when HSP drive responded with Sense 0x02 for Write/Verify or TUR. 
2) Fixed Machine Check with particular motherboard. 
3) Fixed Provide the chip version/revision for MegaRAID controllers thru CmdTool2 
4) Fixed After a complete and successfully recalibrate cycle the request to a relearn is still on 
5) Fixed After FW downgrade eventlog is corrupted
6) Fixed Tape Device LTO-05 loads unexpectedly on SAS2108 and SAS2008 chip based MR adapters 
7) Fixed Some LED are still not working according to OEM SPEC with latest NVDATA 
8) Fixed intermittent RAID key authentication issue was occurring on boot up 
9) Fixed PL version 05.00.28.00 check in 
10) Fixed ESXi installation fails on RAID1/RAID0 cluster of two SSDs 
11) Fixed Intermittent initialization failure (Fault code 0x01) SDRAM ReadEye calibration 
12) Fixed sas address not programmed correctly for OEM Wasat boards 
13) Fixed Copy back does not start in a case of revertible HSP 
14) Fixed Field cant flash back from 10M08 to 10M04 successfully, requires Debugger 
15) Fixed SFO 2108 ROMB reports a non-functional Local Disk as "Operable" 
16) Fixed HSA0297 Command timeout happens in Electra + 600GB SAS HDD during the system power-on. 
17) Fixed RAID-0 Volumes Disappeared After RAID Creation - intermittent 
18) Fixed Disable VPD for specific SSVID
19) Added BBU AEN Change for 6G SAS controllers
20) Added ability to RESET expander from behind MegaSAS

v12.9.0-0046
1) Fixed - CmdTool2 -AdpAllInfo unexpectedly indicate "BBU Supported" for non HWR card.
2) Fixed - After replacing an OEM expander, all the virtual drives are gone if the system is rebooted
3) Fixed - Warning with RWC2 using Intel RES2SV240 Expander card with Hardware RAID cards
4) Fixed - RAID Failed to Rebuild After Reboot with New Drive Insert
5) Fixed - config loss due to lost device insertion post processing callback.

v12.9.0-0044
1) Fixed - Phy 0-3 should be rate limited to SAS 1 speeds for old chip sping.
2) Added - Change NVDATA settings (xml files) for iMR product 
3) Added - Add new xml file for Inspur 
4) Added - Add new ID for ASUS MR product 
5) Added - Revise new iMR NVDATA 
6) Added - Add New Customer IDs to iMR & MR 
7) Added - Add CustomerIDs to 2108 MR (add a new xml file to 10M06 and later stream) 

v12.9.0-0037
1) Fixed - LDBBM fix for mr - imr imports
2) Fixed - LDBBM table getting re-initialized
3) Fixed - PCI VPD data is not populated
4) Fixed - VPD should contain VD Vendor Spec field for Battery type BBU07/BBU08
5) Fixed - LDBBM entries getting corrupted after import from MR to iMR

v2.70.03-0862
1) Fixed Fw error during R50 9per per span rebuild. 
2) Fixed >2TB : DATA TLB ERROR Exception is hit while creation of VD. 
3) Fixed Change nvdata version stretagy to reflect corresponding train 
4) Fixed Dummy defect to checkin the Liberator B4/ Falcon B2 downgrade scenarios 
5) Fixed PL5 SAS_DISC_DS_MAX_ENCLOSURES_EXCEED 
6) Fixed DC is hit on VIEWs after OCR during rebuild. 
7) Fixed DI Issue : LDBBM entries are lost after REBOOT/OCR 
8) Fixed 6919982 Activity LEDs are backwards 
9) Fixed "DDF_ConfigReadPd" Error is shown in FW print on creating config OR during boot. 
10) Fixed FW hit mon task after connect cable to enclosure. 
11) Fixed Dummy defect to check in ieee changes 
12) Fixed No OCR after controller halt for OEM specific Sentinel change 
13) Fixed >2TB iMR: PR fails to detect medium errors 
14) Fixed >2TB : PR fails to find any medium errors on all RAID levels. 
15) Fixed Pl merge 05.00.07.00 
16) Fixed Sentinel Testing:Copy pattern to R0, reboot and doing CC will result in MegaMon 
17) Fixed All applications hangs when pdlist command is executed with 2TB SATA Drives. 
18) Fixed DATA TLB ERROR Exception is hit while creation of VD on SATA PDs 
19) Fixed Rebuild does not progress on a 2.2TB drive(restarts once it reaches 2%) 
20) Fixed DI Issue : FW fails to populate valid LDBBM entries. 
21) Fixed Sentinel testing: fw broke into MegaMon when test file is read (R0 and R1) 
22) Fixed Sentinel file gets corrupted on VDs with non default stripe size 
23) Fixed Dummy defect to check in B2 downgrade scenario changes for Falcon 
24) Fixed Sentinel testing: Megamon hit at reboot after copying pattern to R0,R1,R5,R6(4 drive) 
25) Fixed fw hits megamon on PD command timeout 
26) Fixed iMR Drake Controller doesn't auto rebuild drives on McCave Backplane 
27) Fixed DF365856 >2TB SATA drives are reported as only having 2TB capacity 
28) Fixed FW went to mon_tsk() when running heavy IO's + Rebuilding 
29) Fixed IO fail when running on 16 VDs. 
30) Fixed iMR PL5 FW removes pds when failing redundant path 
31) Fixed OEM changes for Sentinel 
32) Fixed (RW LSIP200062530) Dummy defect to checkin the Liberator B4/ Falcon B2 downgrade scenarios 
33) Fixed FW crashed when you Pull/Push SATA and SSD Drive with SAS Drive Present. 
34) Fixed FW breaks to MonTask: line 2771 in file ../../dm/mpt2/mptcmd. 
35) Fixed VD goes offline with command timeout on PDs in MP 
36) Fixed FW breaks into MegaMon during boot if unconfigured SATA drives are present in a Shea enclosure 
37) Fixed >2TB : DC is hit on R1/R5 VDs 
38) Fixed > 2TB : Drive comes up as foreign even when there is no config. 
39) Fixed DI Issue : CC/rebuild fails to detect the medium error. 
40) Fixed Support for snapshot is missing in Special handling of Pattern.  
41) Fixed Sentinel testing: Drive drop during cc after rebuild, and also during reconstruction 
42) Fixed >2TB: iMR Drive comes up as foreign after clearing config and reboot 
43) Fixed An un-configured PD comes up as configured after reboot. 
44) Fixed Sentinel file (read) causes specific drive model to fail 
45) Fixed >2TB-iMR-hotplug enclosure,debugger hit montask line 199 
46) Fixed CC fails to detect Media errors for above 2TB VD size 
47) Fixed >2TB : DI Issue : LDBBM entries are lost after REBOOT/OCR 
48) Fixed >2TB : DC is hit on PRL 11 using >2TB drives ST33000650NS 
49) Fixed Cascaded enclosures go missing when reconnecting enclosures to import foreign config. 

v2.60.03-0829
1) Fixed Fix DATA TLB exception while updating DDF
2) Fixed Check in PL 2.20 which has permenant fix for alignement exception

v2.40.03-0787
1) Fixed Patrol Read wrongly detects medium error on disk location slot 3 at phy 0
2) Fixed Patrol Read detects media error after full initialization.
3) Added Change NVDATA to Enable exposeEnclosureDevices.
4) Fixed change the slot mapping starting offset
5) Fixed Assertion failure during rebuild unsuspend on RAID 60 disk group with 16 VDs
6) Fixed FW breakes into Megamon when Rebuild is going on, by clearing the suspension bit before changing pd rebuild state active.
7) Fixed Data Miscompare while running Heavy I/O and Rebuild simultaneouly.
8) Fixed SAS Topology Error thrown on connecting 6Gig Enclosure to External Port.
9) Fixed PD getting offline while runing IO overnight on SAS Drives connected directly to controller.
10) Fixed SAS topology error: SMP function failed
11) Fixed PD state changes to Foreign instead of Rebuild after running heavy IO for 3 days
12) Added Reducing Device Qdepth to 64 
13) Fixed Direct Cache is hit when adapter reset is triggered during rebuild on RAID6.
14) Fixed FW breaks into "MonTask: line 4972 in file ../../raid/raidpci.c
15) Fixed FW crashed while booting.
16) Fixed Timestamp is not saved everytime after adapter reset occurs

v2.0.03-0725
1) Fixed Offline foreign VDs get target ID of 255 causing resolution & discovery issues   
 
v2.0.03-0673
1) Fixed Unable to read White text on Gray background in uEFI WB   
2) Fixed System hang with multiple controllers   
3) Fixed RBC some of the buttons are out of range on VD property window   
4) Fixed System PD is taken count when creating array using auto configuration   
5) Fixed RBC shows blank grey screen when selecting 2nd adapter each time RBC is launched   
6) Fixed Data miscompare on Raid 5 WB LD when error injection script is ran   
7) Fixed Foreign config handling issue with automated script.   
8) Fixed Small IO size Seq reads with low QD performing lower than Gen 1 card   
9) Fixed CC on R1 VD didn't correct every inconsistencies the first time it ran   
10) Fixed Degraded PR11 to any RaidLevel allows to remove only offline drives   
11) Fixed Length of parameter list defined in Mode Select (Page19) is not set properly.   
12) Fixed Length of parameter list defined in Mode Select (Page08) is not set properly.   
13) Fixed mode parameter length is hard coded for caching page   
14) Fixed set factory defaults should clear persistent nvdata   
15) Fixed rebuid Not Kick In during Cycle enclosure power while running I/O   
16) Fixed 4 drive inconsistent PRL 11 VD is markd consistent after single drive rebuild.   
17) Fixed GetLDDistribution fails when importing R10 from IR to HWR   
18) Fixed Evt #34 "Not enough controller memory" generated during adapter diagnostics   
19) Fixed SGPIO In Critical, In Failed and PFA Missing   
20) Fixed Change nvdata page 12 and 13 similar to Gen1 nvdata   
21) Fixed Failed I2C send diag cmd due to transfer of less than requested parameter list   
22) Fixed Auto rebuild fails when unsecured SED inserted in the hot slot of a secured VD   
23) Fixed Auto rebuild failure on secured SED when inserted in the hot slot of unsecure VD   
24) Fixed Firmware crashes when SSU gets an 06/3f/01 check condition during DISM   
25) Fixed F/W crash on reboot after flashing the drives.   
26) Fixed Line index being used for CMe reassigns is wrong   
27) Fixed FW breaks into "Fatal firmware error: Line 2578 in ../../dm/mpt2/mptcmd.c" mon_tasks while pull <--> push to rebuild SATA PDs   
28) Fixed external port LEDs not illuminated when links are active   
29) Fixed SATA medium error recovery leads to PL hard reset and FW crash   
30) Fixed FW crash with invalid SGL during SATA medium error recovery   
31) Fixed FW crash running multi-path script with power cycle enclosure overnight   
32) Fixed FW hangs during SATA uncorrectable medium recovery   
33) Fixed Phy error counters not updated in SAS Phy Page   
34) Fixed FW crash in Multipath config with Gen 2 & Gen 1 mix enclosures   
35) Fixed FW crash - MPTREC:Target Reset Does not Complete All the Commands   
36) Fixed FW crash with SSD SATA drives connected to the controller card   
37) Fixed FW crash when removing cable from enclosure.   
38) Fixed PL reset due to PD command timeouts while running I/O on a 4-span R50   
39) Fixed Discovery issue with SATA drives with FW package 12.0.1-0034/-0038   
40) Fixed PL fails to handle correctly a bad SATA drive during discovery   
41) Fixed FW keeps hitting Fault 5841 during removing <--> inserting one path with rebuilding PDs in multipath SAS environment   
42) Fixed Update FW code to work with revision B3 (and above) 2108 devices   
43) Fixed FW hangs when SATA drive with Alta is connected to Red Devil   
44) Fixed Foreign configuration not detected after pinned cache discarded   
45) Fixed reinsert the drive and report wrong slot number on RWC2 v3.04-05   
46) Fixed Rebuild fails to start on PD (part of RAID array) after pull/push operation.   
47) Fixed Pull/push of rebuilding drive causes foreign config. Internal backplane server only.   
48) Fixed PDs get associated with enclosure 0xff until comminication w/ SEP restored   
49) Fixed Battery missing POST message has incorrect formatting   
50) Fixed FW crash due to pincache issue   
51) Fixed sbbm table is not imported from SWR to HWR controller   
52) Fixed FDE changes to make it TCG compliant   
53) Fixed FW writes invalid inquiry data.   
54) Fixed product name gets truncated when its length is >25   
55) Fixed RAID controller returned string(OPROM PnP header) does not return the controller name   
56) Removed Ctrl E which is used to skip OpROM Execution   
57) Fixed check consistency on R1 VD did not correct every inconsistencies   
58) Fixed controller emits many "F/W Initializing Devices 8" messages issue   
59) Updated current Megaraid boot device node name   
60) Fixed allocate mem for one entry when message list is not null and controller handle is null   
61) Fixed EFI Driver does not set cmdStatus on DCMD failure   
62) Removed Gen1 from Gen2 UEFI Driver support   
63) Fixed Controller fails with Invalid SAS Topology error at POST when two enclosures are chained   
 
v2.0.03-0654 - Initial release 

*Third-party trademarks are the property of their respective owners.

