This release note and the software that accompanies it are copyright (c) 2013, Intel Corporation or its suppliers, and may only be installed and used in accordance with the license that accompanies the software.

This Software is furnished under license and may only be used or copied in accordance with the terms of that license. No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. The Software is subject to change without notice, and should not be construed as a commitment by Intel Corporation or its suppliers to market, license, sell or support any product or technology. Unless otherwise provided for in the license under which this Software is provided, the Software is provided AS IS, with no warranties of any kind, express or implied. Except as expressly permitted by the Software license, neither Intel Corporation nor its suppliers assumes any responsibility or liability for any errors or inaccuracies that may appear herein. Except as expressly permitted by the Software license, no part of the Software may be reproduced, stored in a retrieval system, transmitted in any form, or distributed by any means without the express written consent of Intel Corporation.

==========================
Supported RAID Controllers
==========================
This download supports Intel(R) RAID controllers using SAS software stack (RCS25ZB040, RCS25ZB040LX, RMS25PB080, RMS25PB040,RMT3PB080, RMS25CB080, RMS25CB040, RMT3CB080, RMS25CB080N, RMS25PB080N, RS25AB080, RS25SB008, RS25DB080, RS25NB008, RS2VB080, RS2VB040, RT3WB080, RS2WC040, RS2WC080, RS2SG244, RS2WG160, RMS2MH080, RMS2AF080, RMS2AF040, RS2MB044, RS2BL080, RS2BL080DE, RS2BL040, RS2PI008DE, RS2PI008, SRCSASJV, SRCSASRB, SRCSATAWB, SROMBSASFC, SROMBSASMP2, SROMBSASMR, SRCSASPH16I, SRCSASBB8I, SRCSASLS4I, SRCSAS18E, SRCSAS144E, SROMBSAS18E), please ensure that this utility has been tested with the RAID card you have chosen to use by checking the drivers web page for your controller at http://support.intel.com.

===================
Package Information
===================
version =13.04.03.01
OS supported = Solaris 11
This package can be installed on all x86 and x64 systems.

=========
Attention
=========
1)RWC2 uses 5571 or 3071 as multicast listening ports, please make sure these ports are NOT blocked by firewall utility for RWC2 remote connection.

2)From MR5.3 RWC2 is added with 256 bit encryption and this option is disabled by default from factory.
The end user(s) who needs to enable 256 bit encryption is\are expected to perform the below steps

    .   Go to <RWC2_HOME>\ StrongSSLEncryption.ini
    .   Modify the property SSL_STRONG_ENCRYPTION to .ENABLE.
    .   Restart the RWC2 Framework

Warning : Please be aware that enabling 256bit encryption would restrict the user from communicating with the previous versions of RWC2 due to the higher Vs lower bit encryption
handshake in the communication channel.


==================
Known Restrictions
==================
1) The RWC2 service,Framework will not start upon reboot if the /opt file system is mounted on a separate partition. This is because these services currently depend only on the network service which starts even before the other file systems are getting mounted.
2) The icons on the start menu will not appear immediately after the installation or upgrade of the package. The user has to logout and then login to use the icons.
3) In Solaris, location of Systemlog will depend upon the configuration available in the /etc/syslog.conf. 
4) SNMP Trap integration is not done for this release. Additional steps has to be performed after installing Solaris SAS SNMP Agent, 
	a) Edit LSI_StorSNMP.ini file located under /etc/lsi_mrdsnmp
	b) Search for the following line and change Y to N at the end of the line.
		## Dat File Name    ###  Trap Dest. File Name##
		/etc/lsi_mrdsnmp/sas/sas_mib.dat 
		etc/lsi_mrdsnmp/sas/sas_TrapDestination.conf  N
5)While using MSM, user can observe some kind of delay/freeze in the following scenario
Scenario: When the user is trying to perform "Full initialization" on a particular Virtual Drive (VD) (or) all VD.s in MSM.
Reason behind delay/freeze: While issuing a "Full initialization" command MSM performs a check whether the VD belongs to OS drive (or) not to make sure we are not allowing the u
ser to perform initialization on the OS drive. During this operation, especially in Solaris x86/SPARC underlying layers will perform a check to see if the OS VPD page data and t
he FW LD VPD data is matching (or) not. During this check the latency is introduced because of which MSM is observing a slight delay/freeze at the GUI level.


=======================
Contents on the package
=======================
This package includes the Java Runtime Environment files as well as the RaidWebConsole2 installation files.


=========================
Installation Instructions
=========================
Summary of Installation Steps:

1. Extract the files from the tar.gz. Note the package also contains the Java Runtime Environment (JRE) files that must be installed.

2. From the unpacked files, run ./install.sh. The installation path cannot be changed. Most files are installed to /opt/RaidWebConsole2 with additional files added to /var and /etc.

WARNING: 
If the *.sh files in the packages have Windows line breaks. Run the 'tr' command to convert the scripts before you install RWC2.

$> tr -d '\15\32' < existing_file_name > new_file_name
$> chmod a+x new_file_name

3. This package supports only Complete installation mode.

======
	1. While installation the user has to provide the "y" option wherever the installation scripts prompts for the same.

	2. To shutdown RWC2 Framework service, run "svcadm disable -t RWC2Framework".

	3. To startup the framework service run "svcadm enable RWC2Framework".
	
	4.If the service is in "maintenance" state, use "svcadm clear RWC2Framework"

	5. To check for the status of RWC2 services execute the command "svcs -a | grep -i RWC2".

Prerequisites to run RWC2 remote admin:
======================================
	1. Configure the system with valid IP address. Make sure there is no IP address conflict with in the sub network.

	2. Ports such as 3071 and 5571 are open and available for RWC2 framework communication.

	3. Disable all security manager and firewall.

	4. Configure the multicasting, make sure class D multicast IP addresses are registered (at least 229.111.112.12 should be register for RWC2 to work), if not create static route using the following command: "Route add 229.111.112.12 dev eth1"

	5. Install RWC2, if already installed then restart RWC2 framework.


===========================
Uninstallation Instructions
===========================
The product can be uninstalled by executing the "uninstaller.sh" file located in /opt/RaidWebConsole2 directory. While uninstallaion the user has to provide the "y" option wherever the uninstallation scripts prompts for the same.

Notes:
	1. To shutdown RWC2 Framework service, run "svcadm disable -t RWC2Framework".

	2. To startup the framework service run "svcadm enable RWC2Framework".
	
	3.If the service is in "maintenance" state, use "svcadm clear RWC2Framework"

	4. To check for the status of RWC2 services execute the command "svcs -a | grep -i RWC2".


=============================
SNMP Agent Usage Instructions
=============================
1. SNMP MIB:
------------
After installing SNMP Agent package, the MIB file "LSI-AdapterSAS.mib" is installed under /etc/lsi_mrdsnmp/sas directory. The MIB file for SAS IR "LSI-AdapterSASIR.mib" is installed under /etc/lsi_mrdsnmp/sasir directory.

2. Starting/Stopping/Status of SNMP Agent:
------------------------------------------

1.) Following commands are used to start/stop the net-snmpd daemon
	Start	: # svcadm enable svc:/application/management/net-snmp
	Stop	: # svcadm disable svc:/application/management/net-snmp
	restart	: # svcadm restart svc:/application/management/net-snmp
	Status	: # svcs svc:/application/management/net-snmp
NOTE: online indicates the net-snmpd is started.
      disabled indicates the net-snmpd is stopped.
 
2.) Following commands are used to start/stop SAS SNMP Agent daemon
	Start	: #/etc/init.d/lsi_mrdsnmpd start
	Stop	: #/etc/init.d/lsi_mrdsnmpd stop
	restart	: #/etc/init.d/lsi_mrdsnmpd restart
	Status	: #/etc/init.d/lsi_mrdsnmpd status

3.Configuring snmpd.conf:
-------------------------

By default, snmp queries (walk,get) can be executed from any remote machine without any snmpd.conf file changes. To quickly add a new community and client access , please follow the following steps

1. stop the SMA service,by executing the following command
	# svcadm disable svc:/application/management/net-snmp
	
2. Adding readonly and readwrite community names,

To add readonly community name and client/hostname/ipaddress Under "SECTION: Access Control Setup" in 
/etc/net-snmp/snmp/snmpd.conf file is shown below.

Following is an excerpt from the /etc/net-snmp/snmp/snmpd.conf file

###########################################################################
#
# SECTION: Access Control Setup
#
#   This section defines who is allowed to talk to your running
#   snmp agent.

# rocommunity: a SNMPv1/SNMPv2c read-only access community name
#   arguments:  community [default|hostname|network/bits] [oid]

rwcommunity snmpclient 172.28.157.149
###########################################################################

Similarly, To add readwrite community name and client/hostname/ipaddress Under "SECTION: Access Control Setup" in  /etc/net-snmp/snmp/snmpd.conf file is shown below.

Following is an excerpt from the /etc/net-snmp/snmp/snmpd.conf file

###########################################################################
#
# SECTION: Access Control Setup
#
#   This section defines who is allowed to talk to your running
#   snmp agent.

# rocommunity: a SNMPv1/SNMPv2c read-only access community name
#   arguments:  community [default|hostname|network/bits] [oid]

rwcommunity snmpclient 172.28.157.149
###########################################################################

3. start the net-snmpd daemon, by executing the following command
	# svcadm enable svc:/application/management/net-snmp

NOTE: Refer "man snmpd.conf" command for more information on configuring snmpd.conf file.

4.Configuring SNMP Traps:
-------------------------
To receive SNMP traps, the following steps needs to be followed,

1.) stop SNMP Agent by executing the following command,
	#/etc/init.d/lsi_mrdsnmpd stop

2.) Edit /etc/lsi_mrdsnmp/sas/sas_TrapDestination.conf file & add ipaddress as shown below
#################################################
# Agent Service needs the IP addresses to sent trap
# The trap destination may be specified in this file or
# using snmpd.conf file. Following indicators can be set
# on "TrapDestInd" to instruct the agent to pick the IPs
# as the destination.
# 1 - IPs only from snmpd.conf
# 2 - IPs from this file only
# 3 - IPs from both the files
#################################################
TrapDestInd 2
#############Trap Destination IP##################
127.0.0.1   public
172.28.157.149 public
#################################################

3.) start SNMP Agent by executing the following command,
	#/etc/init.d/lsi_mrdsnmpd start

5.Configuring SNMP Traps:
-------------------------

To receive SNMP traps, the following steps need to be followed

1.) stop IR SNMP Agent by executing the following command,
	#/etc/init.d/lsi_mrdsnmpd stop

2.) Edit /etc/lsi_mrdsnmp/sasir/sas_ir_TrapDestination.conf file & add ipaddress as shown below
#################################################
# Agent Service needs the IP addresses to sent trap
# The trap destination may be specified in this file or
# using snmpd.conf file. Following indicators can be set
# on "TrapDestInd" to instruct the agent to pick the IPs
# as the destination.
# 1 - IPs only from snmpd.conf
# 2 - IPs from this file only
# 3 - IPs from both the files
#################################################
TrapDestInd 2
#############Trap Destination IP##################
127.0.0.1   public
172.28.157.149 public
#################################################

3. If in case, 'TrapDestInd' above is set to 1, IP addresses shall be taken from '/etc/net-snmp/snmp/snmpd.conf' in the following format:
'com2sec snmpclient 172.28.157.149 public'
'Trapsink' and 'TrapCommunity' tokens are supported for sending customised SNMP traps.

4. start LSI SAS SNMP Agent by executing the following command,
	#/etc/init.d/lsi_mrdsnmpd start


6.References:
-------------
Please visit http://docs.sun.com/app/docs/doc/817-3000/introduction-1?a=view for more information on Solaris System Management Agent.

7. RWC2 Performance improvement
-------------------------------

Symptoms
a. RWC2 slow/hung during large configurations.
b. RWC2 slow while running the TAS tool.
c. Out of Memory Error.

For better performance of RWC2, when subjected to any heap-intensive (say heavy IOs) or computational tasks, 
improve the heap by including the following command "-Xms1024m -Xmx1024m",where 
1024m           Size of the heap allocated. The specified size is dependent on the machine's Hardware configuration.
-Xms1024m	Sets the initial size of the Java heap to 1024 Mbytes
-Xmx1024m	Sets the maximum heap size to 1024 Mbytes

1. Goto product home folder (/opt/RaidWebConsole2).
2. Open startupui.sh file in editable mode.
3. Include the command -Xms1024m -Xmx1024m after "./jre/bin/java",
   effectively:
   LD_LIBRARY_PATH=$RWC2_HOME/lib ./jre/bin/java -Xms1024m -Xmx1024m -DVENUS=true....
   
8. Logo and Splash Screen Customization(Channel Customers)
-----------------------------------------------------------
   
   In order to help system builders  redistribute RWC2 with their own logo and splash screen, 
   user can provide the customized Logo & Splash screen file name by editing the file "msm.properties", present in  <installation-directory\RaidWebConsole2> folder.
     
   In the file "msm.properties" there are two key values which have no entry. 
   Following are the keys:
   
   CHANNELLOGO=
   CHANNELSPLASHSCREEN=
   
   By default there are no values assigned for both these "Keys" and hence RWC2 uses the default
   LSI Logo and Splash screen.
   
   When system builders like to customize the Logo and Splash screen, they need to provide the Logo & Splash screen file name against these entries. Following are the steps which need to 
   be followed to provide the filenames:
   
   1)	Open the file "msm.properties" in <installation-directory\RaidWebConsole2> folder.
   2)	Make the entry for Logo file against the key "CHANNELLOGO"
   3)	Make the entry for Splash screen file against the key "CHANNELSPLASHSCREEN"
   4)	Save the file
   5)	Place the 2 images in <installation-directory\RaidWebConsole2> folder.
   6)	Start the application.
   
   Notes:
   1)	File names for both entries should not have any spaces.	
   For eg: valid file name would be: logo_test_1.png or  LogoTest1.png or  
   TEST_SPLASH_FILE.jpg
   2)	 Logo image dimensions should not be more than 160 * 85 i.e width * height.
   3)	 Splash screen image dimensions should not be more than  390 * 260 i.e width * height.
   
    After making above changes, when user logs into RWC2, user should see changes with new splash screen and logo in RWC2.


============
Known Issues
============
1) When changing virtual disk properties, initial values for 'Write Policy' or for 'Write Thru for failed/missing Battery' may be different from the currently set values. Always check that the correct 'Write Policy' setting is selected before clicking 'Go' button.

2) Service management facility is introduced into the Solaris package by which the services will start and stop automatically if the system reboots.

3)Latest RaidWebConsole2 for Windows/Linux/Solaris is using an expired SSL certification (it was expired in Aug 18, 2009).Though RWC2 is not a Web-based application, RWC2 uses
the Socket connection over SSL to handshakes only with the legitimate clients of its own using the proprietary key files which were generated using java's key tool with the limi
ted life time. Though it has been identified as an issue as the key was expired, this is not a constraint to end-user anymore. The renewal of "vivaldikey" , "server.cert"  and
"server.key"  needs to be done with both client and Framework i.e. if we renew the key in both the client and Framework the latest version of the RWC2 will not work with earlier
 versions of the Framework which implies a limitation in the deployment environment. In RaidWebConsole2 RWC2 GUI, MegaPopup acts as Client and Framework act as Server.

4)SCGCQ00320645		(RW LSIP200229458) (RW LSIP200224028) MSM will not install or uninstall correctly without Run as Administrator being sel
5)SCGCQ00320633		The pop up window to Dismiss Alerts Pop up hides behind ,difficult for the user to locate.


=============
Fixes/Updates
=============
13.04.03.01 (MR5.7)
Defects:
- SWR - User can login MSM without giving the credentials in SLES 11 SP2 64 bit in THOR_RX300_S7 Server
- MSM is not dynamically reporting configuration changes and events when connected to VMWare

13.04.03.00
Defects:
- System logs contains junk characters  in event description when system locale is set to Japanese.
- MSM 13.04.02.01/Loss of connection occurrs will connected to a server and accidetly put in an IP that does not exist
- Update Controller Firmware dialog disappears sometimes.
- Invader: MSM is not showing drop down list to change the Cachecade VD properties
- MSM not sending emails for events that occur on VMWare host
- MSM displays incorrect "Date of Manufacture" for BBU
- MSM 13.04.02.01/MSM is not showing the estimated time left during a rebuild under show progress.
- MegaRAID CacheVault Unlimited (Unsupported) Factory Installed (Unsupported) on an IBM controller in Advanced Software Options
- Incorrect data in view server profile
- MSM provides conflicting messages in popups for patrol read possibilities
- MSM:PR property settings windows does not pop up in Win server 2012 OS
- Latest release MSM_13.04.02.01 flicker way too long during auto refresh
- MSM is not response  and display NA when pull out multiple drive and put back for rebuild

13.04.02.01
Defects:
- Invader: MSM is not showing drop down list to change the Cachecade VD properties
- CC 2.2: MSM shows the tape device type as "Unknown" and device ID as "0"
- VD name displayed incorrect in server profile.
- MSM Framework hangs on creating more than three globalhotspares in Solaris sparc 10 OS
- MSM no longer reports External Port A or B and Position 1 or 2 on the errors 
- Title missing for popup with text message a test email was sent to selected recipients
- Unable to resume rebuild in MSM
- MSM reports failure to run instant secure erase on a locked FDE drive
- MSM in peer server is not refreshing After configuration related operations

13.04.02.00
Enhancements:
- NMR1.5 HSW merge to MR5.7 HSW
- Nytro XD 1.5 storCLI commands to be merged with MR 5.7
- Removal of VD creation date info in MSM/RWC2
- Add Support for OEM HA-DAS product
Defects:
- MSM - RWC2 Individual event descriptions for MR_Monitor are unclear and out of order
- MSM 12.08.03.03 with BGI progress
- CC2.2: MSM is showing irrelevant message pop up when trying flash 16MB image
- WDMSM: Somtimes wrong Storelib version is displayed under server info for MSM on ESX.
- MSM - RWC2 Individual event descriptions for MR_Monitor are unclear and out of order
- MSM should not show Elapsed Secs for PD/VD progresses
- Progress bar is not completely updating to 100% in copyback.
- PERC9: MSM provides an option to create the virtual drive of strip size 8KB
- Wrong spanned drive group size is displayed in MSM
- Start patrol read option is missing in a particular scenario
- iMR_MSM:Online capacity expansion is not successful after rebuild of global hot spare

13.04.00.00
Enhancements:
- Rebuild time reset
- Red Hat Enterprise Linux 5.9 Support
- VMware 5.0 Update 2 Support
- Need to validate the absolute value on Controller set time
- Add Support for OEM HA-DAS product
Defects:
- After clear configuration from any of the server,Refresh of device tree is taking more time.

13.01.04.00 (MR5.6)
Defects:
- MSM discovery host does not work
- After clear configuration from any of the server,Refresh of device tree is taking more time.
- Server Profile information is not alligned properly in MSM Dashboard for SPARC10
- Invalid entries in MSM resource files

13.01.03.00
Defects
- Wrong nextlearntime is shown for BBU in snmp util and HP openview.
- Not able to select SAS,SATA PD's after selecting and deselecting SSD's as part of the Drive Group.
- VD informations are not aligned properly in solaris sparc 11.
- MSM: Recon option on Odd numbered drive R0 not allowed.
- MSM discovery host does not work
- CSA-1.5 MSM-"Selected FW version" shows wrongly while updating firmware (7mb rom  file of 2161) from MSM
- SWR: MSM displays incorrect VD creation time.
- Text not displayed properly in advanced properties of BBU page.
- CSA1.5: MSM : Alt+g+c+t is not displaying pop up window for set patrol read properties.
- MSM is showing junk characters in preserved cache window

13.01.02.00
Defects:
- MR5.6 Linux 32/64 bit MSM is not packaged with JRE1.7
- MSM- not displaying the complete serial no. for IBM, toshiba drives and Expander
- MSM: when flashing a MR controller, MSM reports it will flash iMR FW in the same package
- Windows 2012 is unable to discover VMWare through MSM
- MSM Fails to Discover ESXi servers.
- iMR_Fury_6.1:MSM - MSM framework crashed during Foreign config import

13.01.01.00
Defects:
- MR 5.6 Alpha: MSM is unable to create a snapshot view
- MSM still prompt user when trying to Uninstall MSM using the "silent" option
- MSM's BBU Advanced Properties page have text that are truncated
- Host Name and OS Name were not displayed for ESXi servers
- Set virtual drive properties dailog is not closing when we click on Ok button
- RAID 10 not listed for IR2 in MSM
- Host name and Right Click option not visible IR2/IR controller
- MACON:  ssd drive temperature is shown in negative value.
- "Create VD" tab is missing on specific scenario
- Windows 2012 is unable to discover VMWare through MSM
- MSM: MR5.6 is missing the 256 bit encryption US export policy and local_policy jar files in jre1.7
- (RW LSIP200223243) macon: the media error count in pd proerties page dosent change unless we do a manual refresh
- HAMR: MSM show Domain ID instead of server name when only node exist in cluster
- HAMR: MSM did not have a help file for configure a shared VD
- iMr_Hamlin_MSM:Prepare for removal option is not coming for DIF/SED drives in MSM
- iMR_Hamlin_MSM:4K drive size not shown proper in MSM profile summary
- MR-MSM: on starting manual learn cycle on supercap, warning message shows that learn cycle takes upto 8 hours.
- iMR_Hamlin_MSM:"Instant secure erase" option is enabled for FDE/SED drives in JBOD state

13.01.00.00
Enhancements:
- MSM Japanese Translation
- Improve MSM response time - early work
- MSM to display entire HA cluster in a a single pane - early work
- MSM: Add support to load CIMPlugin in Linux 64-bit client
- Add MSM StartUI icon
- NMR1.0 HSW merge to MR5.6 HSW

12.08.03.02 (MR5.4)
1) RWC212.01.03.00 reporting time does not converge correctly on the 24 hour clock.
2) Linux: Readme Changes were Missing
3) Error when loading the Intel_adaptersas MIB
4) IBM PE: RWC2 Doesn't Illustrate a Hotspare on the Logical Tab
5) Intel RWC2 - windows version 12.01.03.01  is displaying INTEL  corporation License in the installer
6) RWC2 not showing the boot time events on SWR setup
7) RWC2 message for controller in safe mode is not grammatically correct
8) IN LDAP LOGIN WITH USERNAME AS LDAP\ADMINISTRATOR,FULL ACCESS MODE LOGIN IS NOT ALLOWED.
9) RWC2's BBU status still show as "Optimal" when there is a Fatal error 3 that says "SOH Bad"
10) RWC2 is showing wrong parity size for R50 Virtual disk
11) RWC2-IR2-Exception while creating R10 >1TB in simple configuration mode with odd number of drives[12.08.03.00]
12) In RWC2 BBU Properties page the sentence next to Design Mode has too many spaces inbetween some of the words.
13) RAID1E  Volume Creation Fails with odd number of drives in IR Card-Gen-1
14) RWC2 doesn't generate AEN if Smaller size PD is added for Rebuild.

12.08.03.01
Defects:
1) IN LDAP LOGIN WITH USERNAME AS LDAP\ADMINISTRATOR,FULL ACCESS MODE LOGIN IS NOT ALLOWED.
2) RWC2 displays mis-match BBU learn cycle time in Advanced Properties window
3) RWC2 does not displays information for SuperCap
4) AFTER LDAP LOGIN TO REMOTE SERVER FROM LOCAL SERVER,RWC2 DISPLAYS RAID CONTROLLER CARD OF LOCAL SERVER.
5) RWC2 reports BBU mode as 4 when it is set to mode 5
6) Incorrect server information displayed when RWC2 servers are discovered using IP list option
7) RWC2 allows selection of Full Init for R6 PI enabled VD during creation when normal drive group also present
8) BBU Retention Time Icon is confusing the user

12.08.03.00
Defects:
1) In Dashboard Background operations panel for More details link, the cursor is not changing to hand symbol
2) Controller SAS address SNMP query returning no response
3) Raid10 was not listed for IR2 Card in Windows
4) CLOSING BRACKET MISSING FOR CONTROLLER NAME IN FORIEGN CONFIGURATION WIZARD.
5) RWC2 always change the Write Policy to Write Back with BBU
6) RWC2 showing “Cached?Logical drive property name and value separately
7) RWC2 (12.08.02.00) Readme file needs update
8) Logical drive properties alignment is not proper if user select Enable SSD caching while creating VD.
9) AFTER DISABLING RWC2 FRAMEWORK SERVICE,FRAMEWORK SERVICE IS GOING TO MAINTAINENCE STATE IN SOLARIS SPARC 10.
10) MR monitor plugin: after reboot initial pop up is not displaying.
11) CONFIGURE HOST BUTTON HANGS THAT IS INTIRN CAUSING RWC2 BUTTON TO HANG
12) IR2 : Raid10 Volume creation throws Exception through simple mode.
13) RWC2 incorrectly allows selection of Full Init for R6 PI enabled VD during creation.
14) Remove the PR:INTELP200229508 from the readme Enhancements section as it is removed from MR5.4
15) Assign Dedicated Hotspare- Finding difficulty to differentiate between individual spans (UX design issue)

12.08.02.00
Defects:
1) View only option in RWC2 allows operations like consistency check and Initialize operation
2) RWC2 BBU Advanced Properties page does not show correct information for BBU after BBU is replaced
3) INSTALL.SH FILE IS NOT WORKING,WHEN IT IS KEPT UNDER A FOLDER IN SOLAIS SPARC 10.
4) RWC2 needs to change the Boot Error Handling Property text
5) VMWare RWC2 Allows Operations in View Mode
6) In mib file “cacheFlushInterval?property name shows as “cacheFlushInteval?
7) CSA_RWC2: TTY log shows Device Intr as Unknown
8) EVENT ID'S IN SAVED RWC2 LOGS ARE NOT MATCHING WITH ACTUAL RWC2 LOGS.
9) JUNK CHARCTERS ARE DISPLAYED IN README FILE.
10) For headless mode, the dialog box's size is improper
11) The ‘Device Intr?field is displayed as ‘Unknown?in TTY Logs
12) Pd Serial Number displayed with junk characters.
13) Scrambled content shown  when click on "MANAGE MEGARAID ADVANCED SOFTWARE OPTIONS" for resolution > 1024x768
14) AFTER DISABLING RWC2 FRAMEWORK SERVICE,FRAMEWORK SERVICE IS GOING TO MAINTAINENCE STATE.
15) RWC2 does not give warning when creating CC VD with more than 512GB capacity
16) A new column adding automatically in RWC2 Log when click on 'Rollback to current log' menu
17) CREATION OF SPAN IS NOT ALLOWED WHEN THE SECOND SPAN IS REMOVED.
18) iMR: There is no trap message for SpinUPDelay/SpinupDriveCount

12.08.00.01
Defects:
1) RWC2 Login screen shows OS as 'unknown' for Windows 8
2) RWC2 getting uninstalled while it is still running.
3) Drive Icon is missing during foreign import for VD
4) RWC2 still shows copywrite as 2010
5) Scope-209989 BBUredesign code Check in
6) Drive Icon is missing during foreign import for SSD in CC VD
7) INFO events having the wrong default Alert Delivery Methods

12.08.00.00
Enhancements:
1) Get rid of dependency on 3rd party libs
2) Redesign battery related pages in MR utilities
3) Windows 8 support for MegaRAID SAS products
4) Allow the Customer to change email port in RWC2
5) RHEL 6.3 support for MegaRAID SAS products
6) Citrix XenServer 6.0 support for MegaRAID SAS products
7) VMware ESXi 5.1 Support for MegaRAID SAS products
Defects:
1) Unable to login Citrix- RWC2, shows Error Message as Invalid Username or Password!
2) RWC2 need to allows use to change the email port
3) Performance improvement on ESXi discovery part
4) RWC2 need to allows use to change the email port
5) 64 bit RWC2 is having issues, while firing DCMD'd
6) Unable to display “Advanced MegaRAID software options?window upon clicking link on dashboard
7) Add Windows 8 support to INTEL Windows SNMP
8) Readme file changes for Citrix XenServer 6.0 support
9) (CSCtx53112) RWC2 reports BBU on 2008M-8i falcon controller for ESX 4.1 U2

12.05.03.00
Defects:
1) RWC2 displays Protected CacheCade feature RWC2

12.05.02.01
Defects:
1) Copy Back Progress String needs to be Modified as a Replace Drive in Progress panels for TB and Invader Cards.
2) Wireshark logs says SSLV2 for latest RWC2 v-12.05.01.00

12.05.02.00
Defects:
1)MR5.3 RWC2: Flash size in the controller property is shown as NA for WD card
2)UG drive shows emergency hotspare status when Emergency Hotspare for UG drives is disabled.
3)Dummy Defect - Resolving compilation error due to merge.
4)RWC2 12.05.01.00 cannot update latest firmware image due to change in package size
5)RWC2 deletes the VD when select to discard cache from the access blocked VD
6)RWC2 allows user to create SSC VD with more than 512GB but does not provide any warning message
7)SNMP Services do Not Restart after System Reboot.
8)MR5.3 SNMP/RWC2: SNMP displays invalid values for some of the WD attributes
9)SSL_STRONG_ENCRYPTION enabled by default
10)RWC2 Does not Allow Configuring DS3 when  DS1 and DS2 is disabled and DS3 is Enabled
11)Serial Number displayed wrong while SNMP query for ThunderBolt Controller
12)Unable to start PR with Set PR Properties when one of the VDs is in degraded state.
13)LDAP Settings not getting saved When RWC2 is relaunched.
14)mfcdefaults should not be NULL check codition is not required for populating Manage power save settings Menu in RWC2
15)MR5.3 RWC2: NVRAM size is displayed as NA though NVRAM is present
16)SSL Security needs to be modify
17)OCR becomes disabled when changing controller rates in RWC2
18)Defect to check-in modified readme file for Linux SNMP-IR agent
19)Mib version is showing different from the version mentioned in release note.
20)RWC2 12.05.01.00/Is displaying copyback in certain areas and should say replace drive.
21)RWC2 is displaying Copyback in events, string to be changed to Replace Drive Operation

12.05.01.00
Defects:
1)Prepopulated CacheCade VD Name is using different format between VD0 and VD1.
2)Error when loading the lsi_adaptersas MIB
3)MR5.3: Misspelling of 'acyivation' in RWC2's "Activate MR Advance Software..." Window
4)RWC2 CC2.0 warning message is not valid with RAID0 in WB mode
5)Prepopulated CacheCade VD name is larger than 15 characters allowed.

12.05.00.00
Defects:
1)Full init option is available from RWC2 when creating a PI enabled R60 VD
2) RWC2/UG drive shows emergency hotspare status when Emergency Hotspare for UG drives is disabled.
3)RWC2 local mode installation can connec to another system with complete installation
4)RWC2 crashed on Windows 2008 R2 when doing a refresh
5)RWC2 monitor configure alert menu has restore default option which does not function correcly.
6)RWC2 reports "Login failed: Exception while login!" when logging into VMWare ESXi 5.0 server
7)5.3 Alpha RWC2 on Linux fails to set CC schedule: "The requested command has invalid arguments"
8)RWC2 does not allow start PR on optimal VD, while another VD is rebuild state.
9)(Defer Unable to display CopyRight String in Windows SNMP
RWC2 displays invalid VD number in the AEN when SSD caching is disable on the VD
11)RWC2 does not sort the events by date/time correctly
12)RWC2 fails to restore SSD Caching back to original "Enabled" state after loading original configuration file.
13) Enclosure Position number is incorrect in RWC2 after hotplug enclosure to port 4-7
14)Remaining Capacity for SuperCaP in SNMP-MIB is different than in RWC2
15)Pause for password at boot time cannot be disabled from RWC2
16)Enabled pause for password at boot time is not reported by RWC2 without restarting the app

12.02.01.01
Defects:
1)SNMPWalk displaying OID's of only one controller and Copyright is not displayed.
2)PD serial numbers are showing incorrect.
3)RWC2 error message for medium error is not clear on which port/drive is having the medium error
4)Copyright is missing in SNMP walk.
5)lsi_mrdsnmd service does not stop .
6)SNMP Crashes with querying of CopyRightinfo .
7)RWC2 always displays "0-0-0" for "Diagnostics Complete Date" on DIF drives

12.02.01.00
Enhancements:
1)Get rid of dependency on 3rd party libs
2)Limit lower boundary of SSL encryption to 128bit
3)Use SSLv3 or hire protocols in RWC2
4)SLES 11 SP2 support for MegaRAID SAS products
5)RHEL 5.8 support for MegaRAID SAS products
6)RWC2 Support for Solaris 11
7)Port RWC2 to JRE 7 for Solaris
8)RWC2 Popup Installation in /etc/profile should change
for Solaris 11
Defects:
 RWC2 showing "Battery State" as Operational for Non-Operational battery also

12.01.03.01
Defects:
1)RWC2 alert emails are missing strings to identify the FW package version and FW version

12.01.03.00
Defects:
1)RWC2 shows two instances under Windows 2008 Uninstall window
2)Required Multilingual User Interface (MUI) support on e-mail functionality
4)RWC2/Two different clients are able to login to the same server at the same time in NAT environment
5)RWC2 cannot configure alerts from Client over NAT
6)RWC2 does not connect to local server
7)RWC2 12.01.02.02\Unable to send email after putting in SMTP server
8)Install RWC2 12.01.02.02 and found log with errors

12.01.02.02
Defects
1)RWC2 will not install or uninstall correctly without Run as Administrator being selected
2)RWC2-ESXi Server does not discovery not successful via RWC2

12.01.02.01
Defects
1)Need to update the readme file appropriately  for receiving the SNMP traps in Solaris Sparc
2)RWC2 over NAT incurs major performance hit
3)The word "periodically" is misspell in the warning message for "Disable Automatic Learn Cycle"
4)RWC2 Next Learn cycle not showing correct value for DayLightSaving time Zone
5)RWC2/SSM: Not displaying the power properties in DG page for spanned DG
6)SNMP query fails to report the updated adapter task rates(cc rate, recon rate,rebuild rate and bgi rate).
8)Physical tab and controller properties are disappearing from RWC2 After creating VD for IR2 controller
9)If you enable security on controller using FOD and create secure VD it goes missing upon reboot
10)Enclosure Position number is incorrect in RWC2 after hotplug enclosure to port 4-7
11)RWC2 does not allow user to disable "Use LDAP Login"
12)RWC2 is causing Memory Leak in javaw.exe
13)Pressing OK button in the Manage SSD Caching it brings up the Update Controller Firmware option
14)RWC2 event log shows incomplete onboard "disk device ID"
15)RWC2 issue with email (SMTP) when multiple email recipients are set
16)RWC2 stops refreshing after drives are inserted or removed
17)Enclosure information is missing in SNMP walk
18)RWC2 JLogger showing wrong rescheduled time value for the "Periodic Battery Relearn was missed" event
19)SNMP queries not getting refreshed once enclosure is connected/removed.
20)RWC2 installer allows to proceed without entering LDAP details when"Do you wish to specify LDAP details" is selected
21)Warning message for BBU manual learn cycle contains misspell word
22)RWC2 reports "Battery is not being discharged" when the battery is discharging and "Operational" when in "Relearn"
23)JBOD drive creation didn't get update in RWC2 logical view

12.01.02.00
Defects
1)BBU next learn cycle did not get detected by RWC2
2)RWC2 should not display 65535 minutes estimated recharge time when not charging
3)RWC2 'Cannot create configuration: 3'
4)RWC2 does not display PD properties and Mouse Right Click not working  for SATA PD in SPARC OS
5)SNMP for RHEL crashes with lsi_mrdsnmpd Service restart and enclosure push/pull .
6)Cannot reconstruct partial degrade R6 to R5
7)macon: on changing the rebuild rate the cache flush interval is also getting changed.
8)macon: the media error count in pd properties page doesn’t change unless we do a manual refresh
9)don’t allow user to set properties for TMMC nontransparent battery.
10)RWC2 fails to discover ESXi server
11)Defect created for Re-Scoped PR "-Real Time Scheduler for Relearn" code check in

12.01.01.00
Defects:
1)RWC2 show a PRL11 as a R1 instead of R10 with treatR1EAsR10 enabled.
2)Calendar  needs to be implement more user friendly in BBU set properties Enable mode.
3)Manual and Automatic Panels are scrambling in the BBU Set Properties disable mode.
4)RWC2 allows user to select a PI enabled VD as Snapshot repository for non PI enabled VD
5)Resolve the known limitation of RWC2 on ESXi server - Event logging feature
6)Initial events are not logging on RWC2 - JLogger for ESXi server.
7)When Patrol Read is disabled, RWC2 does not gray out "Start Patrol Read"
8)No option to disable data protection on the spanned Drive Group but there is for single Drive Group.
9)SNMP shows incorrect Serial Number of Physical Drive
10)In MIB file "stripe size" parameter description is not correct which gives user a wrong interpretation for its value
11)- Device interface parameter values are not coming properly in MIB browser
12)- Raid level Qualifier parameter name is not coming correctly in MIB browser description.
13)- SNMP: Operation support description is not proper in MIB browser.
14)Unable to set  CC, Patrolread ,BGI,Rebuild,Reconstruction Rates during SNMP query.
15)Instructions in readme file for receiving traps is inappropriate for SLES11.
16)SNMP Memory Leak
17)Set Learn Cycle Properties popup will not allow pressing OK to exit message
18)RWC2 Array creation wizard chooses write back always as it's default choice as opposed to write thru

12.01.00.00
Enhancements:
1)	Request for RWC2 to display drive Serial number 
2)	add event ID to RWC2 email alerts           
3)	Real Time Scheduler for Relearn 
4)	SNMP to add missing drive properties
5)	Change for SNMP agent to be able to send the trap to non default community
6)	SLES 11 SP2 support for MegaRAID SAS products
7)	RHEL 6.2 support for MegaRAID SAS products
8)	OEL & OEL UEK 5.6, 5.7, 6.0 & 6.1 support for MegaRAID SAS products
9)	WD controller specific attributes for SNMP
10)	WD SNMP: Add DFF specific attributes
11)	WD SNMP: Support SNMP Traps for WD events
12)	Report the new Events for DFF temperature and power throttling
Defects:
1)	Delivering all changes done for 11M08_CCoH
2)	Drive SN & FW information is missing >> 
3)	SNMP trap for custom community support for MegaRAID controllers >> Subbu asked me to fix it as part of the defect
4)	Defect to resolve version no conflicts of SNMP DC and Agent >> Used to resolve the version number conflicts with 2011 Q4 SNMP builds

11.12.01.01
Defects:
1)Incorrect Exception thrown when RWC2 services are stopped in remote server
2)LDAP: Provide login access mode based on user group privileges
3)Unable to launch RWC2 in "Full Access" when Computer is assigned to multiple Groups in LDAP

11.12.01.00
Defects:
1)RWC2 is not able to save the configuration of the events when the machine is not in network in all the platforms
2)LDAP: Update "Welcome<loggedInUser> <accessMode>" string in RWC2 mainscreen
3)LDAP discovery not happening when IP address of RWC2 server is changed after registering it to AD
4)LDAP: Save LDAP credentials while switching RWC2 server from host view screen using Manage -> Server option
5)RWC2 Windows Installer: Add LDAP Support in RWC2 installer
6)RWC2 Generic: Host view screen not getting updated after connection to first server is lost
7)LDAP: Add RWC2 windows LDAP installer support in RWC2
8)LDAP Cosmetic changes

11.12.00.00
Enhancements:
1)LDAP services support
2)LSI SNMP agent cannot send traps to a custom port
3)RWC2 support selectable NIC ports for Email Notification function
4)RWC2 needs to remove references to EKMs
5)Customer is requesting us to add host SAS address in the controller properties in RWC2
6)Show progress indicator during controller FW update

11.08.03.00
Enhancements:
PERC 8.1:  End to End Data Protection (EEDP)
Defects:
RWC2 reports wrong location for LBA over 2 TB
RWC2 : PCI ID contents of event ID 0”Firmware initialization started?is incorrect.
RWC2 : Unable to report the event in /var/log/messages.
PD Reset warning event message is not getting generated in RWC2 for SATA PD only      
RWC2 show blank  the description in event
RWC2 : Displayed Month is incorrect during Oct-Nov when PatrolRead, CC is running.
RWC2 JLogger always showing PHY value as 0
Getting empty events in RWC2 when SAS data cable is inserted or removed from controller
RWC2 upgrade fails due to CLI version difference in Linux
RWC2 needs to update the Suppport Link and Help Link from http://www.LSICorp.com to http://www.LSI.com
Invader:- Flashing 16MB FW with RWC2 hits PROGRAM(SRR0/1,ESR) exception
Maximum allowed unconfig good drives on a controller displays a decimal number RWC2 has some typing errors in making unconfig good
RWC2 has many typing, grammar and description errors in simple creation of VDs.
MACON: megacli gets  installed on installing RWC2 instead of CmdTool


11.08.02.07
Defects:
RWC2 is allowing dimmer switch features for IBM
Readme file has some junk letters in RWC2 and RWC2 in 11.08.02.03 builds
Default value for Disk Cache Policy during VD creation changes after first VD is created.
Snapshot feature set to  take the snapshot for every reboot  is not generating the snapshot view.
Can't create VD with HSP if trying to create VD using simple mode with different PD size in RWC2

11.08.02.06
Defects:
Doesn't allow to create DHSP with specific application	

11.08.02.05
Defects:
Learn Properties Dialog box does not complete message
RWC2 is not supposed to check the popup status if it is not installed
RWC2 has some typing errors in making unconfig good
RWC2 : Severity Level of Event is not changeable.
Battery Predictive Failure message displays twice in RWC2 / Reported as "not Required"
RWC2 : Fails to login to other RWC2 client.
Readme file has some junk letters in RWC2 and RWC2 in 11.08.02.03 builds
RWC2 JLogger always showing PHY value as 0
Getting empty events in RWC2 when SAS data cable is inserted or removed from controller
Needs attention at status properties under dashboard tab in RWC2 is showing irrespective of VD/PD state
Suspend all operation in RWC2 under group show progress is not suspending PR
RWC2 show blank  the description in event                      
In the Event description field on remote RWC2 for the ESXi 5.0 server inaccurate progress is report

11.08.02.04
Defects:
SNMP Trap Alert should be sent when one phy connector between Liberator card and SAS expander is degraded

11.08.02.03
Defects:
RWC2 Unexpected Sense PD info CDB value is not proper
Invalid timestamp for boot time events
RWC2 does not allowing the Patrol Read to resume if suspended previously
RWC2 : When PR Stop after suspend, RWC2 Show Progress shows PR suspended
Controller time synch up with System time if the skew is more than 90 sec

11.08.02.02
Defects:
RWC2 reports incorrect "0" for the passes for dignostic test.
RWC2 : Fails to retreive events during OS shutdown, boot up.
Invader:- When running the Erase function Suspend all option is enabled in RWC2.
RWC2: Suspend All button is enabled even after suspending all the supported BG operations
RWC2: During upgrade of RWC2 8.32.00 to 8.33.00 pop is appearing .
RWC2: uninstallation of RWC2 8.33.0000 prompts for reboot.
RWC2 Unexpected Sense PD info CDB value is not proper
Duplicate SLIR Defect: Bios Version not displayed correctly in Solaris SPARC
RWC2 does not list the access policy and power state Properties for Blocked WT Virtual Drives.

11.08.02.01
Defects:
IMR:When using 11.08-01 RWC2 to convert from JBOD to Unconfigured good FW hits Montask

11.08.02.00
Defects:
Link to LSI.com needs to be updated
Max Power Save mode can not be enabled on Drive Groups with RWC2 or CLI
Unable to get updated remaining capaciity and voltage info  when selecting BBU refresh properties with supercap
Menu name "Manage MegaRaid Advanced Options" needs to be renamed for IBM.
MR Monitor logs are getting cleared when logged off and logged in to RWC2 11.08.01.00
Cannot schedule Patrol Read in RWC2
Unable to set learn cycle properties from the BBU menu with supercap
Unable to get updated remaining capaciity and voltage info  when selecting BBU refresh properties with supercap
the foreign drives comes under the DG.
when high contrast is set in windows,in manage advanced software window all the activated sotware options dosent come.
when high contrast is set in windows, the contents in the dashboard dosent come.
Dummy defect: RWC2 doesn't recieve AENs from ESXi 4.x machines
Installing RWC2 in windows does not create the entry in Add/remove programs  list of Control panel.

11.08.01.00
Enhancements:
12 Gb/s functionality
USB offload implementation
Defects:
Max Power Save mode can not be enabled on Drive Groups with RWC2 or CLI
Unable to create Volume for Gen1 card in Advance mode in all platforms
RWC2 should report that Forced WB VDs are not affected when controller detects BBU disabled
VD capacity display misaligned in RWC2 in RHEL
RWC2 kernel related events not logging in the RWC2 log
In Configure Alerts, we can’t configure the Alert Delivery Method
RWC2 : Fails to provide event log info from ID 386 and above to Windows app log.

11.08.00.01
Enhancements:
Update RWC2 installer to a later version
Defects:
The test email, and we assume others that RWC2 will send is in breach of RFC2821
DSIII: RWC2 did not show the current setting when change controller PS setting
RWC2: Unable to install RWC2 11M08 Build 11.08.00.00 due to install script error
RWC2 failed to upgrade to local mode
DSIII-Should not allow to select PS policy at create VD for mfc bit x08
RWC2 11.08.00.00 installation does not show all numeric values available to user
DSIII:Mercury Select Power Save during create VD  should be disable for Mercury controller
Running "Uninstaller.sh"  or clicking uninstaller icon does not uninstall RWC2_11.08.00-00 application in local mode
Dummy defect to resolve the merge conflicts
RWC2 not displaying remaining capacity while creating VD and not allowing to create VD if clicked on DG on SWR.
RWC2 "create virtual drive" button is enabled even after creating maximum 8 VD's on SWR.
MACON: on lauching RWC2 the create VD icon is disabled
macon: option to save TTY log comes for swr controller.
Macon:SCU: Events are not comming in both RWC2 and Storelib Test.
SWR:Macon: Set PatrolRead properties option not available in RWC2/RWC2
Needs 10M06 RWC2 patch that includes addtional device tree fix to take care of SEP multi port display issue
SNMP:TMM01 BBU FW version  shown wrongly in HP Openview Browser
RWC2:MR Monitor logs are not updating in NAT Environment
Email notification from RWC2 having the minimum details
SNMP:TMM01 BBU FW version  shown wrongly in HP Openview Browser
MegaRAID controllers where lsi_mrdsnmpmain is chewing up 100% CPU apparently in a "busy wait"
Memory usage of SNMP service increases linearly (memory leak) when storeLib reports events continuously.

Update RWC2 with Oracle JRE v.16u24
RWC2 in NAT Environments
Provide native 64 bit Linux RWC2
Update MR SAS LSI applications for VMWare ESXi MN Release

11.06.00.03
1) RWC2 "create virtual drive" button is enabled even after creating maximum 8 VD's on SWR.
2) RWC2 v11.06.00-0200 Host server IP not resolved - 127.0.0.1
3) RWC2: Intel RWC2 not see the licence agreement in Solaris X86
4) RWC2 require to reboot system when do upgrade or uninstall
5) RWC2 11.06.00.0200 can not be opened after upgrading from RWC2 11.05.01.0200
6) RWC2: instead of RWC2, "RWC2" is mentioned in solaris read me file .
7) Macon:"Start Patrol Read" is disabled in RWC2 if rebuild in progress (i.e PR cannot be started on non rebuild drives)
8) macon: option to save TTY log comes for swr controller.
9) MACON: RWC2 changes its default write policy for the sencond VD while creating 2 vd's in same time.


11.06.00.02
Enhancements:
1) Need OEM license agreement in their version of RWC2 
Defects:
1): MACON: under "manage" the option to start init/cc is active when there are no vd's.
2): Macon: RWC2 throws wrong error message on startin PR while rebuild is in progress for spanned array(raid10)
3): MACON: the server profile page is not alligned properly.
4): macon: option to save TTY log comes for swr controller.
5): MACON: RWC2 changes its default write policy for the sencond VD while creating 2 vd's in same time.
6): MACON: Set VD properties not available in RWC2 for VDs in RWC2 
7): MACON: update firmware option is enabled for the SWR controller in dashboard.
8): MACON: option "suspend patrol read" dosent work in group show progress window
9): SWR:Macon: Group Consistency Check Tab is not displayed for SWR controller
10): RAID Web Console Version 2-9.00-00 doesn't invoke properly on RHEL5 ; hangs
11): Cannot migrate R6 to R5 if use all the drive
12): After enclosure element event, RWC2 must manually be refreshed to show new enclosure element status
13): (HSA0xxx)RWC2 : When install RWC2 v8.31-00 by silent installation, the login screen with IP 127.0.0.1 appears.
14): 11M05 : SNMP packages gets installed along with VMware RWC2 installation on ESX 4.1
15): Cisco-ESXi4.1 and ESX4.1 on Alpline/Drake cannot be managed by remote RWC2 Client
16): RWC2 on guest OS intermittently has issues showing event/progress updates
17): ESXi- Simultaneous 64VDs Initialization does not work

11.06.00.01
1. Framework not getting started in SLES 10 SP4 x64
2. RWC2 11.06 under the section for Operating System it displays No Data available when connecting to the ESXi 5.0 server
3. RWC2 11.06.00 RWC2 log messages are not proper 
4. MR Monitor plugin: MR monitor crashes after full init starts
5. MR monitor plugin: mr monitor displays "%" symbol when full init starts.
6. MR Monitor plugin: Reconstruction Rate is not shown in MR monitor log.
7. Connector name is not displaying on popup log, system log and email notification

11.05.01.00
1. Dummy defect to check-in changes in CimPlugin
2. (RW LSIP200123954) (RW LSIP200122654) (RW LSIP200121781) RWC2 only allows the first 16 JBOD to be convert to Unconfigured
3. (Defer LSIP200097351) RWC2 showing pd clear progress in dashboard while doing full init on VD
4. a connected RWC2 GUI client (client only v8.16-01) is unable to configure email alerts from the Tools menu

11.05.00.02
1) Defect to checkin 'fullFGDisallow' implementation in group initialization dialog
2) (RW LSIP200139478) RWC2 Create Snapshot dialog shows big virtual drive list box
3) Enclosure temperatures are reported 20 deg C higher than actual temperature.
4) (RW LSIP200139183) RWC2 :Advanced Software Options link  to external website is not working
5) Open RWC2 will cause RWC2 to perform a PHY set on Phy 17 with speed 255
6) RWC2 is ignoring the option "This server requires authentication".
7) RWC2 does not show correct date in pop up Windows(Alerts)
8) PD labelling is not proper in the RWC2 event logs.
9) SWR: Macon -In RWC2 from Manage option  unable to select the virtual drives for intilisation.
10) Unsupported feature Access policy has been observed in VD Properties Panel for IR and WH controllers
11) Unable to Clear Controller Configuration in RWC2 11.05.00.00
12) RWC2 IT Support: Unsupported fields to be addressed in RWC2 

11.05.00.01
Defects:
1) Cache Offload support revF - RWC2 does not display Capacitance.
2) Defect to checkin 'fullFGDisallow' implementation
3) RWC2 reports incorrect number of eligible JBOD drives for conversion.
4) RWC2 Unable to update controller firmware
5) CacheOffload : RWC2 VD property does not get refresshed , not showing proper write policy when battery is removed.
6) CacheOffload : reason for difference in write policy shows blank space when pinned cache is present.
7) CacheOffload :Enable SSD caching windows popup on non cachecade controller.
8) CacheOffload : CaheOffload related events are not comming in RWC2 
9) RWC2 Windows complete installed able to detect and connect to  SLES RWC2 local

11.05.00.00
Defects:
1):Dummy Defect: Error code 0x5015 when attempting to flash incorrect package on WH board using RWC2 
2): RWC2 UX document is not as per PR
3): RWC2 does not grey out remaining disks when 16 disks are selected to convert to unconfigured good from JBOD.
4):Typo "Configured Shiled" in RWC2 log window
5):Dummy defect for IBM Enclosure PR
6): RWC2 Support for IT2 FW
7): RWC2 does not show all ongoing operations on PD
8): RWC2 Create Snapshot dialog shows big virtual drive list box
9): RWC2 Advanced Software Options link  to external website is not working
10): RWC2 is unable to show the progress information of copyback operation.
11): RWC2 : There is no proper update on progress bar  in dash board while running some operation
12):In RWC2 Enclosure properties are not as per PR
13): RWC2 8.17.01 fails to set the link speed with Keyboard only, mouse ok.
14):Can not do reconstruction from 11R6 to PRL11 by adding one more drive
15): Linux RWC2 Installation does not show all numeric options

11.02.00.00
Enhancements:
1) SW licensing. Support FoD for PF activations on MegaRAID
2) Add new Event to notify "Patrol Read Aborted" in MegaRAID FW.
Defects:
1): when RWC2 is launched select "go to" tab ,here all the entities are enabled.
2):Dummy Defect: Error code 0x5015 when attempting to flash incorrect package on WH board using RWC2 
3):CDROM  icon does not remove after disconnected the cdrom from the controller.
4): RWC2 : Under background operations in dash board , the progress for VD erase shows twice for a single operation.
5): RWC2 is not allowing user to login in Local Mode
6):When you try to create configuration on iMR controller with just JBOD drives present it does not work.
7): RWC2 Create Snapshot dialog shows big virtual drive list box
8):Cannot change Link Speed in RWC2 for Solaris
9): RWC2 :Advanced Software Options link  to external website is not working
10): RWC2 : There is no proper update on progress bar  in dash board while running some operation
11):Unable to change link speed using keyboard in RWC2
12):RWC2: Abort option is not showing for suspended Copy back
13):(RW LSIP200124997) HII not showing property "SSD Cache"
14):Dummy Defect for chekin new image
15):EHSP:Foreign drives showing as emergnecy hotspare eligible
16):(RW LSIP200120735) Disk Cache Policy fails to change when SSD drive becomes part of HDD drive group.
17):Copyback operation suspend Resume functionality not working properly
18):This defect is to check-in the PR changes:LSIP200122937,LSIP200122938
19):Dummy defect to resolve the merge conflicts
20):After reboot or refresh suspended Rebuild or copyback operations is not showing in" show progress" window
21):This defect is to resolve the merge changes
22):Cacheoffload - Battery type and Firmware version needs to be displayed.
23):Resume all is not coming up after OCR
24):SNMP not working properly in RWC2 build 8.15-04 in SPARC

11.20-01
1):RWC2 missing warning box When assign a Dif drive to a Non Pi VD
2):Dummy defect to fix the merge issues
3):Battery state option in RWC2 is not as per UX document
4):For Patrol read Suspend Resume buttons not available
5):Battery retention time is not as per UX document in RWC2
6):BBU temperature shows "high" in RWC2 but all other application shows normal.
7):Battery replacement field in RWC2 is not as per UX
8):Parity Size calculation for RAID 50 is wrong in RWC2.
9):Dummy Defect for chekin new image
10):For Rebuild operation after performing suspend suspendall is not grayed out in RWC2
11):Device tree not getting updated after rebuild complete and changing unconfigured bad to good
12):Cacheoffload - Battery type and Firmware version needs to be displayed.
13):CLI Payload which is incorporated with the RWC2 is not the 11M02 CLI Payload.

11.20-00
1):: RWC2 not showing BBU
2):RWC2 fails to select PDs seperately.
3):BBU status option is missing in SNMP
4):MRmonitor prints wrong string for commisioned Hot Spare
5):Defect to resolve the merge conflicts
6):Unable to create new virtual drive using free capacity on existing drive group in RWC2
7):RWC2 : resume/suspend option for Reconstruction is present.
8):snmp: Rebuilded online PD showing as Emergencyspare
9):Emergency hotspare field shows "ineligible" for eligible PDs for EHS
10):PD/VD Progress panels in Dashboard are not removed after passing the operations
11):Disk Cache Policy is shown as "Enabled" in RWC2
12):Diagnostics complete time string should be changed to diagnostics complete date in RWC2.
13):RWC2: "Resume All" is not enabled on suspending the BGI
14):Exception error when create Simple config with mix drive and DIF option
15):SNMP: PD property Emergencyspare shows wrong value for eligible EHS PDs
16):Emergency hotspare properties getting disabled after change any controller property
17):Shielded PD state is shown as null in RWC2.
18):RWC2 : RWC2 Dashboard , does not show PD or VD erase progress in "Background Operation" tab.
19):RWC2 : Group progress still shows the progress bar of the PR operation which got aborted , and application hangs
20):RWC2 not able to import DIF config
21):RWC2: "Abort All" is not getting disabled after "Suspend all"
22):Unable to create spanned volume in RWC2
23):RWC2: Suspend All showing for Initialization
24):Mirror data is shown as Redundant data in SNMP

9.00.00
1) Fixed refresh issue while rebuild on HSP is aborted 
2) Fixed label issue in configure alerts
3) Fixed power savings not working for 1078 boards.
4) Fixed Special character seen at the end of battery type

8.16-01
1) not able to set adjustable task rates through RWC2
2) RWC2 does not refresh and display created RAID volume in Logical View for IR RAID

8.15-04
1) Fixed break mirror / join mirror is still there in RWC2 8.15.03
2) Fixed RWC2:Unable to Receive MRMonitor events 8.15-03 SLES 10 SP3
3) Fixed In the "Set PR properties", when the PR has been started manually, there is a grammatical error of the text.
4) Fixed RWC2:Configure Host shows wrong IP Address in Login Screen
5) Fixed RWC2 not updating pd properties properly
6) Fixed Join Mirror option is coming in RWC2
7) Fixed Show progress is not refreshing automatically while copyback is going on.
8) Fixed iMR-RWC2 hangs after hotplug enclosure
9) Fixed RWC2: JBOD to unconfigured drive conversion window does not grey out drives beyond 16
10) Fixed IMR - Logical view shows JBOD drives in RWC2
11) Fixed RWC2 Install Problems on Windows 2008 w/ Terminal Services
12) Fixed Pd not showing in Logical Tab after deleting the VD.
13) Fixed TB : Vivaldi shows in-correct values against 'capacity used' and 'capacity remaining' while start CC on repo' VD
14) Fixed CDROM id does not display properly on RWC2 under the event
15) Fixed mrmonitor crashes in Ver 8.15-2
16) Fixed RWC2 GUI fails to refresh on changing system settings for "High contrast

8.05-04
1) Change ˇ°CacheCadeˇ± to ˇ°CacheCade ¨C SSD Cachingˇ± in WebBIOS, RWC2 and CLI
2) Fixed BBU battery properties are not being displayed properly in Linux
3) Fixed User cannot set BBU properties.
4) Fixed Starting Patrol read immediately after CC or Init displays patrol read disable popup
6) Fixed Repeated and non-functional mnemonics in the 'change security screen' in RWC2
7) Fixed RWC2 - Discovery of Hosts happen forever.
8) Fixed RWC2: Single click VD create tab becomes disable after creating one VD
9) Fixed RWC2is displaying SSC and SSCD incorrectly in Foreign Configuration Wizard
10) Fixed Close button missing in Tips to Login GUI
11) Fixed Repeated and non-functional mnemonics in the 'enable security screen' in RWC2
13) Fixed RWC2 fails to discover all the available servers in the subnet even when discovery for remote hosts is enabled.
14) Fixed RWC2 Dashboard screen malformation for resolution 800x600. No Scroll to view
15) Fixed RWC2 Server Profile details different from UX.
16) Fixed Aphrodite: Create Config Wizard does not close even after we press cancel.
17) Fixed RWC2 Operation progress window not updated sometimes
18) Fixed Aphrodite: Mismatch in IP addresses after Sorting in the Host View Screen
19) Fixed 'Enable security' screen ouot of scope in Linux
20) Fixed RWC2 gives an Error when a Pd participating in Vd is made offline when it is in online state.
21) Fixed RWC2 gives an Error when a Pd participating in Vd is made offline when it is in online state.
23) Fixed RWC2 Does not display all VDs being cached to SSCD.
24) Fixed RWC2 - Health of the VD is not reflected on clicking on Server button.
25) Fixed RWC2 Background opereations progress (on VD) count is not updating autometically
26) Fixed RWC2 Background opereations progress count (on PD and VD) is not updating autometically
27) Fixed Spacing issue in RWC2 tooltips screen
28) Fixed Spell Errors in RWC2 tooltips screen
29) Fixed RWC2 Dashboard, enable alarm/ disable alarm does not get updated. Needs refresh
30) Fixed RWC2 Find Next Option pop up does not give the correct message
31) Fixed RWC2 PD operation does not have percentage progress tab
32) Fixed RWC2 does not show popup for invalid username/passwordwhen logging into a remote host with wrong credentials
33) Fixed Framework service exists even for client installation of RWC2 in Linux
34) Fixed Status of controller is not getting refreshed autometically with the change in VD state
35) Fixed RWC2 Manuall start rebuild on PD gives error 0x4
36) Fixed No context sensitive help files present for RWC2 linux
37) Fixed RWC2 fails to make an offline drive online: throws error 0x4
38) Fixed RWC2 Host view GUI get corrupted in resolution 800x600 in Linux
39) Fixed mnemonics to enter the new drive security key in the 'change security screen' in RWC2-6.11-01 is closing the screen itself

6.90-04
1) Fixed RWC2 GUI refresh along with Monitor log updatation fails intermittently on windows-vista 64bit
2) Fixed In RWC2 PRLL VD expansion fails with no message
3) Fixed not able to "restore defaults" in "change individual event" window.

6.50-12
1) Fixed OS main GUI (Desktop) comes blank after Installing RWC2 and rebooting the system.
2) Fixed "prepare for removal" option is absent for FDE.
3) Fixed cannot delete RAID 1.
4) Fixed RWC2 provides option to enable snapshot on VD as repository when it is offline.
5) Fixed RWC2 'show progress' window fails to auto-update VD's BGI progress.
6) Fixed RWC2 shows 'Virtual drive spin down: Enabled' against controller properties.
7) Fixed the capacity used field in repository properties is displaying wrong values.
8) Fixed Cannot create RAID5 due to improper screen if language is set to French or Japanese.
9) Fixed Headings of a few windows appear as English and a few appears as Jananese or French.
10) Fixed UserName, Password & Start up are in English
11) Fixed Mixing of Jpanese-English and English-French in Monitor Event Log
12) Fixed While Creation of VD next,back,help and cancel buttons coming in English.
13) Fixed Strings are displaying in English

5.00-10
1) Fixed initialization cannot be aborted   
2) Fixed RWC2 closes when cancel button is clicked from the manage tab, server option   
3) Fixed show progress window does not show abort button to abort initialization   
4) Fixed RWC2 Create VD Default Settings Incorrect   
5) Fixed SNMP displays incorrect SAS-IR MIB File version while querying   
6) Fixed RWC2 Offers Option to Configure SWR Volumes with Read Ahead   
7) Fixed start initialization button does not greyed out ,when already the initialization is running   
8) Fixed wrong ARCH in sassnmp pkginfo file   
9) Fixed after reboot popup function does not work   
10) Fixed no module named displayed on RHEL 5.3 32-bit   
11) Fixed debug message displayed in console   
 
3.04-07
1) Fixed when network connection is unstable, error message keeps outputting it to start.log   
2) Fixed RWC2 Not Supported for VMWare   
3) Fixed RWC2- Does not allow Reconstruction of Degraded VD.   
4) Fixed BBU times to empty & time to full are 65535 minutes   
5) Fixed RWC2 does not allow to configure 22 drive Raid1   
6) Fixed Selection of  SED as DHSP is blocked in adv. wizard for unsecure SED VD creation   
7) Fixed RWC2 shows a "No foreign config found" error msg after secured disks import   
8) Fixed "Security Key" needs to change to "Passphrase" in "Unlock Foreign Drive" window   
9) Fixed RWC2 DG property for secured is not updated w/o a rescan   
10) Updated RWC2 Readme File   
11) Fixed RWC2 sees System PDs with a status of "Direct" while other apps see a status of "System"   
 
3.04-05
1) Fixed RWC2 2.35-01 shows Win 2008 x86 OS as 'Windows Vista'   
2) Fixed RWC2 framework Solaris SPARC crash when flash FW from remote client   
3) Fixed RWC2 3.04-03 Linux: RWC2 pop ups have some unneeded characters   
4) Fixed RWC2 Framework is not loading the storelib library because it could not detect the controllers present in SPARC Solaris OS   
5) Fixed Can not create VD when asking to create more VD   
6) Fixed RWC2 2.07 Startup fails in DSA installed RHEL5 32 bit Snap7 (1/12)   
7) Fixed Simple and advanced config wizard screen doesnt display the RAID string properly on IR2 controller   
8) Fixed Discard Pinned Cache alert has junk characters   
9) Fixed RWC2 GUI shows "Windows 2008 Server" as "Windows Vista".   
10) Fixed RWC2 sees System PDs with a status of "Direct" while other apps see a status of "System"   
11) Fixed System OS volume is permanently lost after creating a VD   
12) Fixed FDE terms in RWC2 are incorrect   
13) Fixed Storelibtest detect two same controlller in SPARC Solaris   
14) Fixed RWC2 Warning on SLES 11 Install   
15) Fixed RWC2 Display junk character when connect to Sun internal Backplane server   
16) Fixed RWC2 Server properties displaying wrong OS information   
17) Fixed RWC2 displays junk characters when rescanned for a second foreign config   
18) Fixed RWC2 dispalys Vista as the OS on a W2K8 install   
19) Fixed Audit : Documentation for RWC2 does not list Firefox required   
20) Fixed RWC2 3.04-03: R10 displayed as R1E in Advanced Import Foreign Configuration Screen   
21) Fixed RWC2 throws "invalid input parameter" error after importing multiple foreign configs.   
22) Fixed In VD details window text are not properly arranged   
23) Fixed RWC2- Allows to select hot spare for RAID0.   
24) Fixed Can not create Raid volume with "Always WB" in SLES9-SP4_X64   
25) Fixed 'DG settings' page fails to sort drives in 'Drive' & 'Capacity'   
26) Fixed Using RWC2 you can not reconstruct 2 drive R0 to 4 Drive PRL 11.   
27) Fixed Simple Config: Creation of R1 with more than 2 drives throws exception   
28) Fixed 'Create VD' option no exists in 'Free capacity node' from device tree   
29) Fixed Simple config allows 'Free capacity' after VD creation   
30) Fixed IR: "Next" button is not enabled after creating R0 using "Advanced" configuration   
31) Fixed Advanced config allows to create '0 Bytes' size VD   
32) Fixed RWC2- GUI gets corrupted while creating more then 16vd's.   
33) Fixed RWC2- Simple config-- R1 space and no. of VD;s not correct   
34) Fixed No Dialogue message when press 'cancel' button or 'Escape' key in 'Simple' config window   
35) Fixed Chunk Charater in Advance option of Create Virtual Drive-Drive group settings window.   
36) Fixed SWR- Not able to create R5 with Hot Spare option using Simple config in RWC2   
37) Fixed RWC2- Unsupported Raid levels shown for SWR card.   
38) Fixed 'Initial focus' & 'Default button' (Next) fails to work after using 'Back' key   
39) Fixed Advanced config fails to create VD with partial space and different policy settings   
40) Fixed RWC2 2.35-01 shows Win 2008 x86 OS as 'Windows Vista'   
41) Fixed In tree view window of RWC2 (solaris) , two instance of SASIR card as well as drives can be seen   
42) Fixed Advanced config disabled 'RAID level' option after removed DG   
43) Fixed RWC2 does not give the dedicated HS option with FDE controller encrypted array and FDE encrypted array   
44) Fixed RWC2 shows same 'VD default name' for two VDs   
45) Fixed Cosmetic issue in Graphical view of Enclosure   
46) Fixed RWC2 3.03-00 returned "cannot create Virtual Disk: Invalid input parameters for creating Virtual Disk!" msg using Always WB   
47) Fixed RWC2 GUI shows "Windows 2008 Server" as "Windows Vista".   
48) Fixed RWC2- Does not connect to Remote CIMMOM ( VM Ware)   
49) Fixed Advanced config, allows to create more than 16VDs from single DG   
50) Fixed 'Simple' config fails to show the maximum size   
51) Fixed Tab/Shift+Tab/Hot key issue in 'Select unconfigured drives' in Advanced config   
52) Fixed Utilities set Disk cache policy to disabled when VD is created   
53) Fixed 'Simple' not shows 'DG & VD setting' page after chose 'Use free capacity on an existing DG' option   
54) Fixed Advanced config fails to show DG settings page   
55) Fixed RWC2-- More than 4 PD can be added to create PRL11 even though it is not supported   
56) Fixed RWC2- Spanned DG name not as per CR   
57) Fixed An Error message is generated, when tried to create a VD with different parameters other than default values   
58) Fixed 'Drive Group' from 'VD settings' page shows controller info   
59) Fixed RAID1E not supported on an IR controller.   
60) Fixed RWC2 fails to create R1 with HSP while using Simple Config wizard.   
61) Fixed Cannot create VD after selecting Spanned option in Advanced config   
62) Fixed RWC2 fails to update VD properties while creating VD.   
63) Fixed 'Remove' button not working as per scenario A & B from UX design   
64) Fixed IR: RWC2 allows user to select partial VD size from a Disk Group on IR controller   
65) Fixed Mnemonics in RWC2 in simple and Advance options of create VD in not working   
66) Fixed Advanced config shows '-ve' size against free capacity   
67) Fixed VD creation fails when add PDs one by one to DG   
68) Fixed Advanced config shows wrong info against 'hotspare' and same VD# for two VDs   
69) Fixed RWC2 fails to fast initialise a SASIR VD created using Advanced config.   
70) Fixed RWC2- Advanced config shows size of Partila R1 (4 drives) as 0bytes   
71) Fixed Dedicated Hotspare related issues   
72) Fixed Auto config snapshot remains despite of pulling out back of the config   
73) Fixed Simple Config: HotSpare checkbox gets enabled for RAID0   
74) Fixed Issue in 'Add PD' check in 'Reconstruction' wizard   
75) Fixed 'Initial focus' & 'Default button' (Create virtual drive) fails to work in 'VD settings' page   
76) Fixed IR: No R1E to select from Raid Level combo list in RWC2   
77) Fixed PRL11 not supported in Advanced config   
78) Fixed GUI issue when try to remove DGs from DG settings page   
79) Fixed RWC2 incorrectly states FDE drive as Non-FDE during global hotspare creation.   
80) Fixed RWC2- Advanced Config-- Back Next not working.   
81) Fixed 'Drive type mixing' not available in 'Simple' config   
82) Fixed RWC2 4.01-01 does not show CIM plugin version   
83) Fixed RWC2 gives option for creating more VD even though there are no free PD's   
84) Fixed IR: Unable to Create more than one array from RWC2 for IR controller   
85) Fixed 'RAID level' drop box not shows RAID order as per UX design   
86) Fixed Advanced config fails to change size if switch between GB/MB/KB Units   
87) Fixed Remove the redundant function isEncryptionSupported and isEncryptionEnabled methods   
88) Fixed RWC2 - Operation Tab remains inactive for free capacity selection.   
89) Fixed Issue when creating VD in TB size in Advanced config   
90) Fixed RWC2 does not show proper 'default name' against VD   
91) Fixed Advanced config shows '0' against 'Total capacity' in Summary screen   
92) Fixed unable to reconstruct from 5PD R5 to 8PD PRL11 in RWC2   
93) Fixed IR: With only 1 drive available, Raild Level box shows R0 to select, in "Advanced" configuration.   
94) Fixed SWR- Not able to create R1 using Simple config in RWC2   
95) Fixed Default write cache policy is NOT Write back in 3.03-00   
96) Fixed 'Simple' config creates VD using different stripe size   
97) Fixed Capacity not shows sizes in ascending or descending order in simple config   
98) Fixed RWC2 shows option for create VD even though there are no UG PD's   
99) Fixed Advanced config allows to create lesser size VDs beyond RWC2 minimum size limit   
100) Fixed RWC2- Advanced Config. VD created shown in wrong DG.   
101) Fixed Drive Security Drop Down Box does not get updated appropriately   
102) Fixed Simple & Advanced config shows hotkey(Alt+l) for cancel key   
103) Fixed Summary screen shows 'No' against HS when VD has 'HS'   
104) Fixed No warning message for 'Space wastage' in 'Simple' config   
105) Fixed 'Advanced' config not page not shows the default stripe size from MFC   
106) Fixed RWC2- Simple config window has no heading.   
107) Fixed RWC2- GUI gets corrupted in after removing VD while creating.   
108) Fixed Can not create 64 VD using Guide Config   
109) Fixed Unable to create 2nd VD after creating the first for SASIR Gen1.   
110) Fixed RWC2 throws exception for simple config with hole present   
111) Fixed IR: RWC2 allows to create DiskGroup with 11drives for R0.   
112) Fixed IR: "Advanced" configuration displays R5 & Spanned Volumes (00,50,60) in RaidLevel combo box   
113) Fixed RWC2- DG not shown in Advanced config page.   
114) Fixed RWC2- "Confirm Enable Security" Pop up does not fit in the Screen   
115) Fixed GUI issue while moving capacity tab in 'Select Unconfigured drives'   
116) Fixed Advanced config shows commands against 'Drive security method' combo box   
117) Fixed Max limitations for Advanced VD creation Page   
118) Fixed RWC2 - Create Config while rebuilt is in progress thorws error.   
119) Fixed RWC2 2.07 Startup fails in DSA installed RHEL5 32 bit Snap7 (1/12)   
120) Fixed IR: Using "Simple" configuration, no arrays can be created using any number of drives   
121) Fixed RWC2 logical view shows HS PDs twice after created in Advanced config   
122) Fixed Add HS support not available for span RAID levels   
123) Fixed Advanced config allows to add HS for RAID00   
124) Fixed Issue in MB Units in Advanced config when creating VD   
125) Fixed IR: "Simple" configuration displays R5 & R6 in Raid Level combo box for IR controller   
126) Fixed IR: 'Drive Security Method' is enabled in RWC2 for IR controller   
127) Fixed RWC2 shows create VD page when there are no free PDs and no DG with free space   
128) Fixed RWC2- DG size not shown shown properly whle creaing VD.   
129) Fixed IR: VD parameters are changable in RWC2 for IR controller   
130) Fixed Simple config not shows name for 'DG and VD setting' page   
131) Fixed RWC2 allows to add more than 2 PD's for R1 in a 1068 card. PRL 11 not supported   
132) Fixed RWC2- Create more VD's fail when in particular case.   
133) Fixed RWC2- Advanced Config-- SAS drives remain disabled after even selecting Cntrl Encryption
134) Fixed Advanced config shows 'Create more VD' dialogue box when DG has less than '1MB' free space   
135) Fixed Intermittent GUI issues from 'CreateVD' option   
136) Fixed "Select" option for Drive security is active for the 1068 controller card even with non FDE drives   
137) Fixed RWC2- Simple config mnemonics not working.   
138) Fixed Wrong Default button after canceling warning in config wizard in RWC2.   
139) Fixed RWC2- SAS/SATA mix option does not chk RAID level allowed   
140) Fixed RWC2- Dedicted hot spare shown for both spans in the GUI   
141) Fixed Size issue while updating VD in 'VD settings' page   
142) Fixed RWC2 allows create VD thru free capacity when VD reconstruction is in progress   
143) Fixed RWC2- Closing the config window gives blank msg!   
144) Fixed RWC2- 4Drive R1 shown as RAID17 in summary page.   
145) Fixed Junk characters displayed with GUID for foreign config import.   
146) Fixed RWC2- Gives option to create more VD's after R0 of all PD is made.   
147) Fixed 'Next' button disabled once 'Back' from VD settings to DG settings page   
148) Fixed Advanced config fails to show existing DGs information in DG & VD settings page   
149) Fixed Advanced config fails to create HS in two different scenarios   
150) Fixed RWC2 shows 'Create VD' and 'Configuration' options   
151) Fixed Advanced config fails to create R1 with full space   
152) Fixed RWC2- Cannot Create configuration. Throws exception when controler is selected.   
153) Fixed RWC2- Cannot create R10 with 3 spans.   
154) Fixed Drive group allows to create 3PD R1 DG   
155) Fixed Error when change to WB policy in RWC2   
156) Fixed RWC2 Server properties displaying wrong OS information   
157) Fixed RWC2 dispalys Vista as the OS on a W2K8 install   
158) Fixed Simple Config: Wrong capacities displayed for R1   
159) Fixed RWC2- (MFC=useFDEonly=1) Still RWC2 shows option to create Controller based Encrypted VD. 
160) Fixed 'RAID level' disabled after adding PDs one by one in DG settings page   
161) Fixed Initial focus not working in simple config   
162) Fixed Advanced config not allows to create more than 16VDs from DG   
163) Fixed RWC2 pull down menu cannot set the Solid State Drive(SSD) Guard.   
164) Fixed RWC2- Some strings do not match according to UX   
165) Fixed Advanced config fails to create 3PD R6   
166) Fixed Hotkey conflict in 'VD settings' page and leads to config error   
167) Fixed RWC2- (MFC=allowedDeviceTypes=0(SAS/SATA) to 1 i.e SAS only, config wizard shows SATA   
168) Fixed Default setting in RWC2 3.3-00 is conflict with Ctrl_R, it should be WB, NRA, DIO   
169) Fixed 'Create VD' shows available capacity in the size of Kbytes   
170) Fixed RWC2- Config does not show the pop up "Do you want to create mord VD"   
171) Fixed RWC2- VD creation from a VD under rebuild fails with Error code: 0x32   
172) Fixed Simple Config: Implement the logic for missing RAID levels.   
173) Fixed RWC2- DG size goes to more than max allowd in the scroll option.   
174) Fixed Drive groups are not listed for selecting DHS as per CR 71084.   
175) Fixed RWC2- String RAID shown twice in Crate VD advance Config page   
176) Fixed DG settings page fails to disable 'Drive security method' when encryption is not available   
177) Fixed RWC2- Icon not shown for pop up msgs   
178) Fixed RAID6 not available under 'Simple' configuration   
179) Fixed RWC2- Does not show the RIAD icon in create config wizard.   
180) Fixed IR: Unable to create multiple Drive Groups on IR controller using RWC2

2.92-01
1) Change default setting to disable HDD write cache   
2) Added comments for cache setting during array creation   
3) Added the BBUGood variable for BBU status display   
4) Fixed RWC2 continuously executed stop/start of the network service   
5) Fixe RWC2 shows "Windows 2008 Server" as "Windows Vista".   
6) Fixed Popup.exe forced to go down by the IO trafic fragility test in DoS Attack   
7) Fixed RWC2 display SWR driver version as FW version.   
8) Added Japanese Email Alert   
9) Fixed Controllers on the VMware Server system cannot be recognized by RWC2   
 
2.91-03
1) Fixed typo in global hot spare coverage warning dialog box   
2) Added SMARTer support for SSD.   
3) Added ability to set VD size with "TB"   
4) Fixed RWC2 max VD exceeded issue   
 
2.91-01
1) Fixed RWC2 ALT+A does not work in Reconst screen   
2) Fixed controller Properties corruption when user changes controller setting.   
3) Fixed RWC2 Junk Chars displayed in the warning msg of Foreign config import screen   
4) Fixed typo in Global Hot Spare coverage warning dialog box   
5) Fixed RWC2 scan for Foreign Config does not work with a drive in Spun Down State.   
6) Fixed "Write-Thru for failed/missing battery" setting displayed incorrectly in RWC2
7) Fixed failure to create Global Hot Spare during rebuild on R1 & raid 6 together.

2.90-02
1) Fixed "Concurrent" option of "Scheduled Consistency Check" is invalid
2) Fixed RWC2 Framework Service on SLES10 Must Be Restarted to Connect from Remote Windows Machine
3) Fixed RWC2 services fails on every reboot on a standalone server
4) Fixed Change Security Key Settings Next Button Disabled
5) Fixed Upgrading from RWC2 2.77 to 2.90 Failure
6) Fixed 64k stripe size option for SWR 
7) Fixed RWC2 CIM plug-in to get loaded on RHEL5 system
8) Fixed Scheduled Consistency Check" stops unexpectedly.
9) Fixed RWC2 is not allowing to configure Global Hotspare when more that one VD is present
10) Fixed Remove status dots in physical & logical views
11) Fixed RWC2 under RHEL 5.1 EM64T doesn't see any RAID controller
12) Added more users support for RWC2 FULL access under Linux
13) Fixed RWC2 GUI gets corrupted  with a ' NULL PTR Exception' when connected to remote RAID Server.

2.64-00
N/A

2.63-00
1) Fixed RAID controller internal time shift issue which cause constant battery relearn

2.34-00
1. Fixed "Write Through for failed/missing Battery" setting sticking to 'No'.
2. Added capability of changing physical disk status from 'Unconfigured Bad' to 'Unconfigured Good'
3. Added capability of manually starting battery relearn
4. Added SNMP Agent installation
5. Added Server Only (no GUI, remote management only) installation option for Linux
6. Fixed RWC2 version in the Support information section shows incorrect value on Windows.
7. Fixed RWC2 does not delete the 'Installation Folder' after uninstallation.
8. Fixed Resolve accesibility issues with RWC2
9. Fixed unable to connect to RWC2 on VMWARE from remote client
10. Fixed failure to install RWC2 on VMWARE
11. Fixed popup alerts being lost when no user is logged on to Windows
12. Fixed Popup does not work on Linux for local user
13. Fixed Pop Up error message when install RWC2 on VMWARE
14. Fixed RWC2 version in the Support information section shows incorrect value on Windows.

2.19-00
1. Adding SRCSASJV, SRCSASRB, SRCSATAWB and SROMBSASFC support

1.19-00
1. Adding Forced Write Back Mode feature support
2. Monitor support for email

1.18-00
1. Change RWCII graphics to be Intel 3.0

1.15-00
1. Fixed RWC2 failed to remove "RAID Web Console 2" Directory from "C:\Program Files\"
2. Fixed 'Unconfigured Good' PD appears inside a R0 array after the disk is pulled out and reinserted. 
3. Fixed "Disk Cache Policy" could not change without error.
4. Fixed Blocked graphical representation of enclosure in "Graphical View" tab of enclosure
5. Operation panel should not visible if no operation available
6. Fixed Failed to load saved log file.
7. Fixed right click on Controller fails to display available operations.
8. Fixed the garble occurs to a message of RWC2.
9. Fixed the RBC and RWC2 is not consistence display info
10. Fixed RWC2 allows you to start an Init on the RAID LD that your OS is installed.
11. Displayed GMT time for Event date and time.
12. The making location of the "popuplog.log" file.
13. Foreign configuration will be merged and displayed with other native configuration
14. Implementation of default Write Policy depends on existing/non-existing BBU
15. RWC2 can be lunched without any extra authentication from any other trusted application
16. Close button has been added in the show progress window. On clicking, the show progress window closes.
17. System supports to display CDROM and Tape under Port and displays their properties in Property tab.
18. Handle AEN for Enclosure so that enclosure property should automatically refreshed if it will get enclosure specific AEN.
19. Include date and time in alert notification
20. Remove newline in alertStringsSpec.xml file
21. Set a reference to a filelogger object when loading the alertstrings library

1.13-07
1. Fixed Unistallation of RWC2 is possible without warning when the initial login screen is kept open.
2. Fixed RWC2 can't be started on Linux by local user
3. Enable WB without battery
4. Fixed RWC2 return error when a unconfigured bad  perform a prepare for removal.
5. Fixed RWC2 display wrong bbu even a bbu is installed in ZCR controller.
7. Fixed "Guided" and "Auto" Config fails to create redundant array with more than 2 free PDs available.
8. Fixed Popup doesn't work on Linux for a local user other than root.
9. Fixed Popup function error
11. Added Logging when you reboot server without operating in RWC2.
12. Fixed Installer upgrade process where when RWC2 is running it fails actually failed to upgrade the components.
13. Fixed MegaRAID Storage Manager Client Hang up.
14. Fixed RWC2 does not read FW MFC data when create new configuration.
15. Improved Error severity reporting and thread synchronization issue reporting in this release of Monitor.
16. Fixed the Event Notification application to un-register with FW when applications exit.
17. Added Event Notification Application replies back to FW.
18. Added a New server.pem file which does not require password.
19. Added Monitor support for email.
20. Fixed RWC2 to read FW MFC data when creating a new configuration.
21. Fixed Invalid Options are appearing on right mouse button clicking on "Port".
22. Fixed RWC2 to diplay "About" GUI under Help to show Product name and version properly.
23. Fixed Uninstalling RWC2 fails to remove corresponding files and directories.
24. Fixed Build display to correctly show build numbers.
25. Fixed issue with RWC2 create Ded HSP to allow only HDD's that are bigger than or equal to the max capacity drive of the array.
26. Fixed exception error when clicking on Tool-Mail configurator with Win2003 Japanese version.
27. Fixed Mail alert function error.
28. Fixed incorrect parameter of ID99 message.

1.13-01
1) Fixed Intel(r) Embedded Server RAID - RAID 5 (SWR5) While creating partial 2nd LD, RWC2 configuration wizard displays array0 as array7
2) Fixed Failure to import Save RAID configuration file during a Rebuild operation.
3) Fixed Failure of Guided and "Auto" Config to create redundant array with more than 2 free PDs available.
4) Fixed Failure of RWC2 to start Installation process when no "C:\" drive present in the system

1.11-01
1) Fixed Assigning long VD name is not displying the VD size unless rescan is performed
2) Fixed Attempt to create Config encounters error "Command failed by Operating System" and AEN updation stops
3) Fixed SWR / After upgrading to the latest driver, R10 can not be configured in OS level.
4) Fixed The number of Fans and Power Supplies is different from Log
5) Fixed RWC2 shows incorrect detail messages.
6) Fixed RWC2 could not display Graphical View, Correctly.
7) Fixed RWC2: when making Dedicated HS, it shows max 10 arrays even if we have more than 10 arrays.
8) Fixed 'Locate VD' & 'Stop Locating VD' options available against VD with PD outside an enclosure.
9) Fixed Upgrading RWC2 from ver 1.08-00 to 1.08-01 fails to start Popup service in Windows env.

1.08-01
1) Fixed Automatic starting sequence of the Popup function set by RWC2 installer is unjust
2) Fixed ENA pop-up message boxes are not consistent in size when displaying either Critical or Fatal asynchronous event messages.
3) Fixed Popup application crashes if you have events generating very fast.

1.08-00
1) Fixed When the Rebuild is in progress on JBOD (with EP107) then you go to Hibernation mode, in the nextrecovery you cannot resume the Rebuild.  If user try to activate the external, MRMonitor service will become Application Error. This problem is not 100% reprodeuceable.
2) Fixed RWC2 not reporting double media errors correctly.
3) Fixed Rebooting system pops up error msg with Popup service failing to get auto-started.

1.07-00.
1) Fixed Creating a R0 VD spanning over two R0 array displays "RAID 00" as the applicable raid level.
2) Fixed Port number against PD displayed incorrectly while assigning it as a HSP.
3) Fixed Popup service fails to start & stop automatically after installing & uninstalling respectively
4) Fixed Creation RAID level selection screen non-descrptive syntax
5) Fixed X16/PT SRSM doesn't warn that data will be lost before starting initialization
6) Fixed Junk characters displayed  when importing foreign configuration.


*Third-party trademarks are the property of their respective owners.