This release note and the software that accompanies it are copyright (c) 2013, Intel Corporation or its suppliers, and may only be installed and used in accordance with the license that accompanies the software.

This Software is furnished under license and may only be used or copied in accordance with the terms of that license. No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. The Software is subject to change without notice, and should not be construed as a commitment by Intel Corporation or its suppliers to market, license, sell or support any product or technology. Unless otherwise provided for in the license under which this Software is provided, the Software is provided AS IS, with no warranties of any kind, express or implied. Except as expressly permitted by the Software license, neither Intel Corporation nor its suppliers assumes any responsibility or liability for any errors or inaccuracies that may appear herein. Except as expressly permitted by the Software license, no part of the Software may be reproduced, stored in a retrieval system, transmitted in any form, or distributed by any means without the express written consent of Intel Corporation.

==========================
Supported RAID Controllers
==========================
This download supports Intel(R) RAID controllers using SAS software stack (RCS25ZB040, RCS25ZB040LX), please verify that this utility has been tested with the RAID card you have chosen to use by checking the drivers web page for your controller at http://support.intel.com.

===================
Package Information
===================
Flash package = v23.13.0-0056 (firmware version 3.200.25-2490)

==========
Attention!
==========
Intel recommends to loading Factory Default setting after the firmware upgrade which will not affect data on any existing array. To do so:
1. Reboot the system and login to the RAID BIOS Console. 
2. Select the controller and select 'Adapter Properties'->'Next'
3. Set the 'Set Factory Defaults' setting to 'Yes' and submit the change.
4. Reboot the system (the default settings are applied).
5. Re-configure to the desired settings in RAID Web Console2.

==================
Known Restrictions
==================
1) This download does NOT support EFI v1.1 environment. Please use the EFI shell command “ver" which will display the EFI version, to identify the EFI version.
2) When 2 or more VDs are created, VD cache settings must be the same.


=======================
Contents on the package 
=======================
The following files are included in this zip:

Name:								Description:
ir3_2208NMR_FWPKG-v23.13.0-0056_readme.txt			This file
NMR15p.rom							Firmware binary
update.bat							DOS firmware update batch file
update.nsh							UEFI firmware update batch file
CmdTool2\DOS\*							DOS update utility and support files 
CmdTool2\FreeBSD\*						FreeBSD update utility and support files
CmdTool2\Linux\*						Linux update utility and support files
CmdTool2\Solaris\*						Solaris update utility and support files
CmdTool2\UEFI\*							UEFI update utility and support files
CmdTool2\Windows\*						Windows update utility and support files
License_v2.pdf							License Agreement
COPYING.NEWLIB.txt						License Agreement


==========================
Installation instructions:
==========================

UEFI (EFI 2.0) instructions for updating RAID Firmware:
-----------------
   1. Download and extract all files to a local drive.
   2. Boot the target system to EFI shell. 
   3. Change directory to the local drive and directory containing the flash update files and the firmware image file.
   4. Type "update.nsh" or "efi\cmdtool2 -adpfwflash -f NMR15p.rom -noverchk -aall"
   5. Wait for the flash to complete. Do NOT reboot the system during the update.

Windows and Linux instructions for updating RAID Firmware:
-----------------
The firmware update may be run from Within Windows or Linux using the appropriate versions of CmdTool2.
  In Windows, unzip the utility into the same directory as the rom file by typing 
      "cmdtool2 -adpfwflash -f NMR15p.rom -aall". 
  The Linux CmdTool2 by running the rpm and then calling the utility from /opt/MegaRAID/CmdTool2 as 
      "./CmdTool2 -AdpFwFlash -f NMR15p.rom -aall"

DOS instructions for updating RAID Firmware:
-----------------
   1. Download and extract all files to a local drive.
   2. Boot the target system to DOS. 
   3. Change directory to the local drive and directory containing the flash update files and the firmware image file.
   4. Type "update.bat" or "dos\cmdtool2 -adpfwflash -f NMR15p.rom -aall"
   5. Wait for the flash to complete. Do NOT reboot the system during the update.

You can also use RAID Web Console 2 to update the RAID firmware. For more detail, please refer to the Intel(R) RAID Software User's Guide.

=============
Package Details/Fixes/Updates 
=============
23.13.0-0056 (NMR 1.5patch)
 Firmware v3.200.25-2490
 - Reboot fails after upgrade of FW from older FW(2210) to newer FW(2477).
 
23.13.0-0046 (NMR 1.5)
 Firmware v3.200.25-2480
 - After foreign config import VD properties are not reporting in the MSM
 - NMR1.5-Critical event OCR observed during OS bootup in OEM-specific server
 - CSA1.5 IntelZiaBeach: DFF moved to JBOD state after enabling JBOD from mfc settings of the controller
 - CSA1.5 IntelZiaBeach:2 out of 14 PD's are not configuring to JBOD state even though all PD's are in Unconfigured Good state
 - CSA 1.5: Source VD goes offline while copying large file from one VD to another VD (associated to Nytro Cache)
 - fixed in release order
 - MR_DCMD_CTRL_IO_METRICS_GET should return MFI_STAT_IO_METRICS_DISABLED if Io metrics collection is not enabled.
 Cache Offload v3.200.14-2073
 - CSA1.5-Firmware crash observed after introducing lock out, pull the power cable
 BIOS - v5.35.00
 Hii - v01.32.00
 PCLI - v05.02-01
 WebBIOS - v6.5-18-e_0-Rel
 - CSA1.5 :WEBBIOS hangs during source vd creation
 - CSA1.5 :WebBios Virtual Drive Erase option is not working for all the 3 variants of VD Erase!
 - CSA1.5 :WebBIOS 'Drive Erase' option for VD is not displaying the 'Delete VD option after Erase' checkbox option missing
 NVDATA - v2.1108.03-0090
 Bootblock - v2.06.00.01-0000
 Common Bootblock - v07.26.05.219


23.6.1-0004 (NMR 1.0) - Initial Release
 Firmware v3.200.15-2221
 Cache Offload v3.200.14-1825
 BIOS - v5.35.00
 Hii - v01.32.00
 PCLI - v05.02-01
 WebBIOS - v6.5-8-e_0-Rel
 NVDATA - v2.1108.03-0088
 Bootblock - v2.06.00.01-0000
 Common Bootblock - v07.26.05.219


*Third-party trademarks are the property of their respective owners.

