//****************************************************************************
//                          Intel Corporation
//                    Jones Farm, Hillsboro, Oregon
//                           (503) 696-8080
//
//                Intel Corporation Proprietary Information
//     Copyright (c) 2010 - 2013 Intel Corporation, All Rights Reserved
//****************************************************************************
//
//
// File Header Information
//

_LF_NAME       'Rainbow Pass SDR File'
_LF_VERSION    '1.05'
_LF_FMT_VER    '1.50'
_IPMI_VERSION  '2.00'

//
// SDR Header Information
//

_SDR (
_START_ADDR     0000
_DATA_LEN       0000
_NVS_TYPE       'IMBDEVICE'
_DEV_BUS        FF
_DEV_ADDRESS    20

//====================================================================//
// (1) Chassis related TAG
//====================================================================//
//_SDR_TAG    'UPS_4HDD'               // SDRs for Union Peak S Default SKU
//_SDR_TAG    'UPS_8HDD'               // SDRs for Union Peak S Default SKU
//_SDR_TAG    'OTHER'                  // SDRs for OTHER chassis
//_SDR_TAG    'OTHER_SR'               // SDRs for OTHER(Slow Ramp) chassis
//_SDR_TAG    'OTHER_MR'               // SDRs for OTHER(Medium Ramp) chassis
//_SDR_TAG    'OTHER_FR'               // SDRs for OTHER(Fast Ramp) chassis
//_SDR_TAG    'R1000_SAS'              // SDRs for Buffalo Peak 21 with SAS Module
//_SDR_TAG    'R1000_NOSAS'            // SDRs for Buffalo Peak 21 no SAS Module
//_SDR_TAG    'UPS_4SAS'               // SDRs for UPS 4x3.5HDD with SAS Module
//_SDR_TAG    'UPS_4NOSAS'             // SDRs for UPS 4x3.5HDD no SAS Module
//_SDR_TAG    'UPS_4FIXSAS'            // SDRs for UPS 4x3.5HDD Fix with SAS Module
//_SDR_TAG    'UPS_4FIXNOSAS'          // SDRs for UPS 4x3.5HDD Fix no SAS Module
//_SDR_TAG    'UPS_8X35SAS'            // SDRs for UPS 8x3.5HDD with SAS Module
//_SDR_TAG    'UPS_8X35NOSAS'          // SDRs for UPS 8x3.5HDD no SAS Module			

//====================================================================//
// (2) Processor related sensors
//====================================================================//
// _SDR_TAG     'PROC_1'                // SDRs for Processor 1

//====================================================================//
// (3) Temperature sensors
//====================================================================//
// _SDR_TAG    'FP_TEMP'                // SDR for Front Panel Temp
// _SDR_TAG    'EATEMP'                 // SDR for Exit Air Temp
// _SDR_TAG    'SYS_AIRFLOW'                 // SDR for System Airflow

//====================================================================//
// (4) Fan sensors
//====================================================================//
// _SDR_TAG   'PROC1_FAN'               // Processor Fan 1
// _SDR_TAG   'OTHER_FAN_1'             // System Fan 1
// _SDR_TAG   'OTHER_FAN_2'             // System Fan 2
// _SDR_TAG   'OTHER_FAN_3'             // System Fan 3
// _SDR_TAG   'OTHER_FAN_4'             // System Fan 4
// _SDR_TAG   'R1000_FAN_1'              // System Fan 1 (System Fans (1U BP21") - 3 Fixed Fans)
// _SDR_TAG   'R1000_FAN_2'              // System Fan 2 (System Fans (1U BP21") - 3 Fixed Fans)
// _SDR_TAG   'R1000_FAN_3'              // System Fan 3 (System Fans (1U BP21") - 3 Fixed Fans)
// _SDR_TAG   'UPS_4HDD_FAN_4'          // System Fan 4 (System Fans (4U UPS 4 HDD))
// _SDR_TAG   'UPS_4HDD_PROC_FAN'       // Processor Fan 1 (System Fans (4U UPS 4 HDD))
// _SDR_TAG   'UPS_8HDD_FAN_1'          // System Fan 4 (System Fans (4U UPS 8 HDD both 3.5&2.5) )
// _SDR_TAG   'UPS_8HDD_FAN_4'          // System Fan 4 (System Fans (4U UPS 8 HDD both 3.5&2.5) )
// _SDR_TAG   'UPS_8HDD_PROC_FAN'       // Processor Fan 1 (System Fans (4U UPS 8 HDD both 3.5&2.5) )

//====================================================================//
// (5) Chassis Intrusion
//====================================================================//
// _SDR_TAG    'CHASSIS_INTRU'          // Physical Security sensor
// _SDR_TAG    'NO_CHASSIS_INTRU'       // no Physical Security sensor

//====================================================================//
// (6) OTher device sensors
//====================================================================//
// _SDR_TAG    'HSBP_1_BP4'             // SDR for 4 port HSBP 1
// _SDR_TAG    'HSBP_1_BP8'             // SDR for 8 port HSBP 1
// _SDR_TAG    'IO_MODULE'              // SDR for I/O
// _SDR_TAG    'IO_MODULE_FRU'          // SDR for I/O
// _SDR_TAG    'SAS_MODULE'             // SDR for SAS
// _SDR_TAG    'SAS_MODULE_FRU'         // SDR for SAS

//====================================================================//
// (7) Power Supply related sensors
//====================================================================//
// _SDR_TAG    'PS_REDUNDANCY'         // Redundant Power Supply
// _SDR_TAG    '350_PS'                // 350W Power Supply 1.
// _SDR_TAG    '500_PS'                // 500W Power Supply 1.
// _SDR_TAG    '460_PS'                // 460W Power Supply 1.
// _SDR_TAG    '500_PS2'               // 500W Power Supply 2.
// _SDR_TAG    '460_PS2'               // 460W Power Supply 2.

//====================================================================//
// (8) Factory sensors
//====================================================================//
// _SDR_TAG     'SHIP'                  // SDRs for Shippings
// _SDR_TAG     'FCT'                   // SDRs for FCT
// _SDR_TAG     'FCT2'                  // SDRs for FCT2

//====================================================================//
// (9) Others
//====================================================================//
// _SDR_TAG    'FP_NMI'                 // SDRs for NMI

//====================================================================//
_SDR_TYPE   02
_REC_LEN    002F

   // Sensor Record Header
   0001               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   01                 // Sensor Number

   // Record Body Bytes
   15                 // Entity ID - power management / power distribution board
   01                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   40                 // Sensor Capabilities
   09                 // Sensor Type - power unit
   6F                 // Event / Reading Base Type
   7100               // Assertion Event Mask   --Power down/A/C lost/Soft power control failure/Power unit failure =7100
   7100               // Deassertion Event Mask --Power down/A/C lost/Soft power control failure/Power unit failure =7100
   7100               // Reading Mask & Settable / Readable Threshold Masks --Power down/A/C lost/Soft power control failure/Power unit failure =7100
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Pwr Unit Status'  // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PS_REDUNDANCY'
_REC_LEN    002F

   // Sensor Record Header
   0002               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   02                 // Sensor Number

   // Record Body Bytes
   15                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   09                 // Sensor Type
   0B                 // Event / Reading Base Type
   FF00               // Assertion Event Mask   --Redundancy regained/Non-red: suff res from redund/Redundancy lost/Redundancy degraded/Non-red: suff from insuff/Non-red: insufficient/Redun degrade from full/Redun degrade from non-redundant=FF00
   0000               // Deassertion Event Mask --Redundancy regained/Non-red: suff res from redund/Redundancy lost/Redundancy degraded/Non-red: suff from insuff/Non-red: insufficient/Redun degrade from full/Redun degrade from non-redundant=FF00
   FF00               // Reading Mask & Settable / Readable Threshold Masks
                      //--Redundancy regained/Non-red: suff res from redund/Redundancy lost/Redundancy degraded/Non-red: suff from insuff/Non-red: insufficient/Redun degrade from full/Redun degrade from non-redundant=FF00
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Pwr Unit Redund'  // String Bytes

//====================================================================//
_SDR_TYPE   02
_REC_LEN    002D

   // Sensor Record Header
   0003               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   03                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   23                 // Sensor Type
   6F                 // Event / Reading Base Type
   0F01               // Assertion Event Mask   --Timer expired, status only/Hard reset/Power down/Power cycle/Timer interrupt =0F01
   0000               // Deassertion Event Mask --No Deassertion =0000
   0F01               // Reading Mask & Settable / Readable Threshold Masks --Timer expired, status only/Hard reset/Power down/Power cycle/Timer interrupt =0F01
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'IPMI Watchdog'    // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'CHASSIS_INTRU'
_REC_LEN    002E

   // Sensor Record Header
   0004               // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   04                 // Sensor Number

   // Record Body Bytes
   17                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   05                 // Sensor Type
   6F                 // Event / Reading Base Type
   1100               // Assertion Event Mask   --Chassis intrusion/LAN leash lost 1 =1100
   1100               // Deassertion Event Mask --Chassis intrusion/LAN leash lost 1 =1100
   1100               // Reading Mask & Settable / Readable Threshold Masks --Chassis intrusion/LAN leash lost 1 =1100
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Physical Scrty'   // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'NO_CHASSIS_INTRU'
_REC_LEN    002E

   // Sensor Record Header
   0005               // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   04                 // Sensor Number

   // Record Body Bytes
   17                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   05                 // Sensor Type
   6F                 // Event / Reading Base Type
   1000               // Assertion Event Mask   -- LAN leash lost =1000
   1000               // Deassertion Event Mask -- LAN leash lost =1000
   1000               // Reading Mask & Settable / Readable Threshold Masks -- LAN leash lost =1000
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Physical Scrty'   // String Bytes
   
//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'FP_NMI'
_REC_LEN    002F

   // Sensor Record Header
   0006               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   05                 // Sensor Number

   // Record Body Bytes
   0C                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   13                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Assertion Event Mask   --Front panel NMI/diagnostic interrupt = 0100
   0000               // Deassertion Event Mask --No Deassertion =0000
   0100               // Reading Mask & Settable / Readable Threshold Masks --Front panel NMI/diagnostic interrupt = 0100
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'FP NMI Diag Int'  // String Bytes

//====================================================================//
_SDR_TYPE   02
_REC_LEN    002B

   // Sensor Record Header
   0007               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   06                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   41                 // Sensor Capabilities
   F3                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --State asserted =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'SMI Timeout'      // String Bytes

//====================================================================//
_SDR_TYPE   02
_REC_LEN    0030

   // Sensor Record Header
   0008               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   07                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   10                 // Sensor Type
   6F                 // Event / Reading Base Type
   0400               // Assertion Event Mask  --Log area reset / cleared =0400
   0000               // Deassertion Event Mask --N/A
   0400               // Reading Mask & Settable / Readable Threshold Masks --Log area reset / cleared =0400
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'System Event Log' // String Bytes

//====================================================================//
_SDR_TYPE   02
_REC_LEN    002C

   // Sensor Record Header
   0009               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   08                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   12                 // Sensor Type
   6F                 // Event / Reading Base Type
   1000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   1000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'System Event'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_REC_LEN    0026

   // Sensor Record Header
   000A               // Record ID
   51                 // SDR Version
   02                 // Record Type
   21                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   09                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   14                 // Sensor Type
   6F                 // Event / Reading Base Type
   0500               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0500               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C6                 // Type/Length Code
   'Button'           // String Bytes

//====================================================================//   
_SDR_TYPE      02
_REC_LEN       002C

   // Sensor Record Header
   000B               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0A                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   28                 // Sensor Type
   6F                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'BMC Watchdog'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_REC_LEN    002B

   // Sensor Record Header
   000C               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0B                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   02                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --State asserted =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'VR Watchdog'      // String Bytes

//====================================================================//
_SDR_TYPE   02
_REC_LEN    002E

   // Sensor Record Header
   000E               // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0D                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   01                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --State asserted =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PCH Therm Trip'   // String Bytes

_SDR_TYPE   02
_SDR_TAG    'IO_MODULE'
_REC_LEN    002F

   // Sensor Record Header
   000F               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0E                 // Sensor Number

   // Record Body Bytes
   2C                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   15                 // Sensor Type
   08                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'IO Mod Presence'  // String Bytes

_SDR_TYPE   02
_SDR_TAG    'SAS_MODULE'
_REC_LEN    0030

   // Sensor Record Header
   0010              // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0F                 // Sensor Number

   // Record Body Bytes
   2C                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   15                 // Sensor Type
   08                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'SAS Mod Presence' // String Bytes

//====================================================================//
_SDR_TYPE   02
_REC_LEN    002D

   // Sensor Record Header
   F00F               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   10                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   28                 // Sensor Type
   6F                 // Event / Reading Base Type
   1000               // Assertion Event Mask   --State asserted =1000
   0000               // Deassertion Event Mask --State asserted =0000
   1000               // Reading Mask & Settable / Readable Threshold Masks --State asserted =1000
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'BMC FW Health'    // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SYS_AIRFLOW'
_REC_LEN    003E

   // Sensor Record Header
   F010               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   11                 // Sensor Number

   // Record Body Bytes
   17                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   63                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   11                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   02                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   5A                 // Nominal Reading
   B4                 // Normal Maximum
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   //------------------------------------------------------------------//
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'System Airflow'   // String Bytes

//====================================================================//
_SDR_TYPE   03   
_REC_LEN    0021

   // Sensor Record Header
   0011               // Record ID
   51                 // SDR Version
   03                 // Record Type 
   1C                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   12                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   2B                 // Sensor type 
   70                 // Event/Reading Type Code 
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code 
   'FW Update Status' // String Bytes


//====================================================================//
//
// Baseboard and chassis related temperature related sensors
//
//====================================================================//
_SDR_TYPE   01
_REC_LEN    003C

   // Sensor Record Header
   0012               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   20                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type -- (Temperature)
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- (Degrees C)
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   3A                 // Normal Reading (3Ah = 58 degrees C)
   69                 // Normal Maximum (69h = 105 degrees C)
   0A                 // Normal Minimum (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   73                 // Upper critical (73h = 115 degrees C)
   6E                 // Upper non-critical (6Eh = 110 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (00h = 0 degrees C)
   05                 // Lower non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'BB EDGE Temp'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'FP_TEMP'
_REC_LEN    0040

   // Sensor Record Header
   0013               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   21                 // Sensor Number 

   // Record Body Bytes
   40                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   FE                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   1E                 // Normal Reading (1Eh = 30 degrees C)
   2F                 // Normal Maximum (2Fh = 47 degrees C)
   0C                 // Normal Minimum (0Ch = 12 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   39                 // Upper critical (39h = 57 degrees C)
   34                 // Upper non-critical (34h = 52 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   02                 // Lower critical (02h = 2 degrees C)
   07                 // Lower non-critical (07h = 7 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   D0                 // Type/Length Code
   'Front Panel Temp' // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    0038

   // Sensor Record Header
   0014               // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   22                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type -- (Temperature)
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- (Degrees C)
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   34                 // Normal Reading (34h = 52 degrees C)
   5D                 // Normal Maximum (5Dh = 93 degrees C)
   0A                 // Normal Minimum (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   67                 // Upper critical (67h = 103 degrees C)
   62                 // Upper non-critical (62h = 98 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (00h = 0 degrees C)
   05                 // Lower non-critical (05h = 05 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C8                 // Type/Length Code
   'PCH Temp'         // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    003B

   // Sensor Record Header
   0015               // Record ID
   51                 // SDR Version
   01                 // Record Type
   36                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   23                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type -- (Temperature)
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- (Degrees C)
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   3A                 // Normal Reading (3Ah = 58 degrees C)
   69                 // Normal Maximum (69h = 105 degrees C)
   0A                 // Normal Minimum (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   73                 // Upper critical (73h = 115 degrees C)
   6E                 // Upper non-critical (6Eh = 110 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (00h = 0 degrees C)
   05                 // Lower non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'BB BMC Temp'      // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    003E

   // Sensor Record Header
   0016               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   24                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type -- (Temperature)
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- (Degrees C)
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   3A                 // Normal Reading (3Ah = 58 degrees C)
   69                 // Normal Maximum (69h = 105 degrees C)
   0A                 // Normal Minimum (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   73                 // Upper critical (73h = 115 degrees C)
   6E                 // Upper non-critical (6Eh = 110 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (00h = 0 degrees C)
   05                 // Lower non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'BB CPU VR Temp'    // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'IO_MODULE'
_REC_LEN    003C

   // Sensor Record Header
   0018               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   26                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   28                 // Normal Reading (28h = 40 degrees C)
   46                 // Normal Maximum (46h = 70 degrees C)
   0A                 // Normal Minimum (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   50                 // Upper critical (50h = 80 degrees C)
   4B                 // Upper non-critical (4Bh = 75 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (00h =0 degrees C)
   05                 // Lower non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CC                 // Type/Length Code
   'I/O Mod Temp'     // String Bytes
   
//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'HSBP_1_BP4'
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    003B

   // Sensor Record Header
   0019               // Record ID
   51                 // SDR Version
   01                 // Record Type
   36                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   29                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   7D                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask    --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask  --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   3A                 // Normal Reading (3Ah = 58 degrees C)
   69                 // Normal Maximum (69h = 105 degrees C)
   0A                 // Normal Minimum (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   73                 // Upper critical (73h = 115 degrees C)
   6E                 // Upper non-critical (6Eh = 110 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (00h = 0 degrees C)
   05                 // Lower non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type Length Code
   'HSBP 1 Temp'      // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SAS_MODULE'
_REC_LEN    003C

   // Sensor Record Header
   001C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   2D                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   39                 // Normal Reading 
   68                 // Normal Maximum 
   0A                 // Normal Minimum 
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading 
   80                 // Sensor Minimum Reading 
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   72                 // Upper critical 
   6D                 // Upper non-critical 
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical 
   05                 // Lower non-critical 
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CC                 // Type/Length Code
   'SAS Mod Temp'     // String Bytes
   
//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'EATEMP'
_REC_LEN    003D

   // Sensor Record Header
   001D               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   2E                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type -- (Temperature)
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask   --[u,l][c,nc]=0000
   0000               // Deassertion Event Mask --[u,l][c,nc]=0000
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- (Degrees C)
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   28                 // Normal Reading (28h = 40 degrees C)
   46                 // Normal Maximum (46h = 70 degrees C)
   0A                 // Normal Minimum (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   55                 // Upper critical (55h = 85 degrees C)
   50                 // Upper non-critical (50h = 80 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (00h = 0 degrees C)
   05                 // Lower non-critical (05h = 05 degrees C)
   //------------------------------------------------------------------//
   04                 // Positive hysteresis value
   04                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   47                 // OEM
   CD                 // Type/Length Code
   'Exit Air Temp'    // String Bytes

//====================================================================//
//
// Fan tachometer sensors
//
//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_1'
_REC_LEN    003C

   // Sensor Record Header
   001F               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   30                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   82                 // Normal Reading (82h == 12750 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   05                 // Normal Minimum (05h == 500 RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 25000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   01                 // Lower critical (01h == 175 RPM)
   04                 // Lower non-critical (04h == 400 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 1'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'R1000_FAN_1'
_REC_LEN    003C

   // Sensor Record Header
   0020               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   30                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   84                 // Normal Reading 
   FF                 // Normal Maximum 
   0A                 // Normal Minimum 
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading 
   00                 // Sensor Minimum Reading 
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   04                 // Lower critical 
   06                 // Lower non-critical 
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 1'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'UPS_8HDD_FAN_1'
_REC_LEN    003C

   // Sensor Record Header
   F022               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   30                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   19                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   92                 // Normal Reading 
   FF                 // Normal Maximum 
   26                 // Normal Minimum 
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading 
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable 
   00                 // Upper critical 
   00                 // Upper non-critical
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable 
   1B                 // Lower critical
   1E                 // Lower non-critical 
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 1'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_2'
_REC_LEN    003C

   // Sensor Record Header
   0022               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   31                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   03                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   82                 // Normal Reading (82h == 12750 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   05                 // Normal Minimum (05h == 500 RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 25000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   01                 // Lower critical (01h == 175 RPM)
   04                 // Lower non-critical (04h == 400 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 2'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'R1000_FAN_2'
_REC_LEN    003C

   // Sensor Record Header
   0023               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   31                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   03                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   84                 // Normal Reading 
   FF                 // Normal Maximum 
   0A                 // Normal Minimum 
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading 
   00                 // Sensor Minimum Reading 
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   04                 // Lower critical 
   06                 // Lower non-critical 
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 2'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_3'
_REC_LEN    003C

   // Sensor Record Header
   0025               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   32                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   04                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   82                 // Normal Reading (82h == 12750 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   05                 // Normal Minimum (05h == 500 RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 25000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   01                 // Lower critical (01h == 175 RPM)
   04                 // Lower non-critical (04h == 400 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 3'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'R1000_FAN_3'
_REC_LEN    003C

   // Sensor Record Header
   0026               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   32                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   04                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   84                 // Normal Reading 
   FF                 // Normal Maximum 
   0A                 // Normal Minimum 
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading 
   00                 // Sensor Minimum Reading 
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   04                 // Lower critical 
   06                 // Lower non-critical 
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 3'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_4'
_REC_LEN    003C

   // Sensor Record Header
   0027               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   33                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   05                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   82                 // Normal Reading (82h == 12750 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   05                 // Normal Minimum (05h == 500 RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 25000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   01                 // Lower critical (01h == 175 RPM)
   04                 // Lower non-critical (04h == 400 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 4'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'UPS_4HDD_FAN_4'
_REC_LEN    003C

   // Sensor Record Header
   0028               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   33                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   05                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   18                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   89                 // Normal Reading 
   FF                 // Normal Maximum 
   14                 // Normal Minimum 
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading 
   00                 // Sensor Minimum Reading 
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   06                 // Lower critical 
   09                 // Lower non-critical 
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 4'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'UPS_8HDD_FAN_4'
_REC_LEN    003C

   // Sensor Record Header
   0029               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   33                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   05                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   18                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   89                 // Normal Reading 
   FF                 // Normal Maximum 
   14                 // Normal Minimum 
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading 
   00                 // Sensor Minimum Reading 
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   06                 // Lower critical 
   09                 // Lower non-critical 
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 4'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'UPS_4HDD_PROC_FAN'
_REC_LEN    003D

   // Sensor Record Header
   002A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   36                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   08                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   0C                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   A7                 // Normal Reading 
   FF                 // Normal Maximum 
   4F                 // Normal Minimum 
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading 
   00                 // Sensor Minimum Reading 
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   37                 // Lower critical 
   3F                 // Lower non-critical 
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   03                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'Processor Fan'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC1_FAN'
_REC_LEN    003D

   // Sensor Record Header
   002C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   36                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   08                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   82                 // Normal Reading (82h == 12750 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   05                 // Normal Minimum (05h == 500 RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 25000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   01                 // Lower critical (01h == 175 RPM)
   04                 // Lower non-critical (04h == 400 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   03                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'Processor Fan'  // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'UPS_8HDD_PROC_FAN'
_REC_LEN    003D

   // Sensor Record Header
   F02C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   36                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   08                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   0C                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   A7                 // Normal Reading 
   FF                 // Normal Maximum 
   4F                 // Normal Minimum 
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading 
   00                 // Sensor Minimum Reading 
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   37                 // Lower critical 
   3F                 // Lower non-critical 
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   03                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'Processor Fan'     // String Bytes

//====================================================================//
//
// Power supply sensors (Only supported with PMBus enabled power supplies)
//
//====================================================================//
_SDR_TYPE   02
_SDR_TAG    '350_PS'
_SDR_TAG    '500_PS'
_SDR_TAG    '460_PS'
_REC_LEN    002A

   // Sensor Record Header
   0035               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   50                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   08                 // Sensor Type
   6F                 // Event / Reading Base Type
   4F00               // Assertion Event Mask   --Presence/Failure/Predictive Failure/A/C lost/Configuration error =4F00
   4F00               // Deassertion Event Mask --Presence/Failure/Predictive Failure/A/C lost/Configuration error =4F00
   4F00               // Reading Mask & Settable / Readable Threshold Masks --Presence/Failure/Predictive Failure/A/C lost/Configuration error =4F00
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'PS1 Status'       // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    '500_PS2'
_SDR_TAG    '460_PS2'
_REC_LEN    002A

   // Sensor Record Header
   0036               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   51                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   08                 // Sensor Type
   6F                 // Event / Reading Base Type
   4F00               // Assertion Event Mask   --Presence/Failure/Predictive Failure/A/C lost/Configuration error =4F00
   4F00               // Deassertion Event Mask --Presence/Failure/Predictive Failure/A/C lost/Configuration error =4F00
   4F00               // Reading Mask & Settable / Readable Threshold Masks --Presence/Failure/Predictive Failure/A/C lost/Configuration error =4F00
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'PS2 Status'       // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '500_PS'
_REC_LEN    003C

   // Sensor Record Header
   0037               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   54                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   04                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   66                 // Nomnal Reading 
   CC                 // Normal Maximum 
   00                 // Normal Minimum 
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading 
   00                 // Sensor Minimum Reading 
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   E6                 // Upper critical 
   D9                 // Upper non-critical 
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'PS1 Power In'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '460_PS'
_REC_LEN    003C

   // Sensor Record Header
   0038               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   54                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   04                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   68                 // Nomnal Reading 
   D0                 // Normal Maximum 
   00                 // Normal Minimum 
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading 
   00                 // Sensor Minimum Reading 
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   E9                 // Upper critical 
   DC                 // Upper non-critical 
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'PS1 Power In'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '350_PS'
_REC_LEN    003C

   // Sensor Record Header
   0039               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   54                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   07                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   5E                 // Nomnal Reading (5Eh=658.0Watt)
   BC                 // Normal Maximum (BCh=1316.0Watt)
   00                 // Normal Minimum (00h=0Watt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh=1785.0Watt)
   00                 // Sensor Minimum Reading (00h=0.0Watt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   FA                 // Upper critical (FAh=1750.0Watt)
   DB                 // Upper non-critical (DBh=1533.0Watt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'PS1 Power In'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '500_PS2'
_REC_LEN    003C

   // Sensor Record Header
   003B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   55                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   04                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   66                 // Nomnal Reading (66h=408.0Watt)
   CC                 // Normal Maximum (CCh=816.0Watt)
   00                 // Normal Minimum (00h=0Watt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh=1020.0Watt)
   00                 // Sensor Minimum Reading (00h=0.0Watt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   E6                 // Upper critical (E6h=920.0Watt)
   D9                 // Upper non-critical (D9h=868.0Watt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'PS2 Power In'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '460_PS2'
_REC_LEN    003C

   // Sensor Record Header
   003C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   55                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   04                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   68                 // Nomnal Reading 
   D0                 // Normal Maximum 
   00                 // Normal Minimum 
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading 
   00                 // Sensor Minimum Reading 
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   E9                 // Upper critical 
   DC                 // Upper non-critical 
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'PS2 Power In'     // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '500_PS'
_REC_LEN    003E

   // Sensor Record Header
   003D               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   58                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   32                 // Normal Reading (32h = 50 %)
   64                 // Normal Maximum (64h = 100 %)
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   70                 // Upper critical 
   64                 // Upper non-critical (64h = 100.0 %)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical  (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysterisis value
   00                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS1 Curr Out %'   // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '460_PS'
_REC_LEN    003E

   // Sensor Record Header
   003E               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   58                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   32                 // Normal Reading (32h = 50 %)
   64                 // Normal Maximum (64h = 100 %)
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   70                 // Upper critical (70h = 112.0 %)
   64                 // Upper non-critical (64h = 100.0 %)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical  (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysterisis value
   00                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS1 Curr Out %'   // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '500_PS2'
_REC_LEN    003E

   // Sensor Record Header
   0041               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   59                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   32                 // Normal Reading (32h = 50 %)
   64                 // Normal Maximum (64h = 100 %)
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   70                 // Upper critical (70h = 112.0 %)
   64                 // Upper non-critical (64h = 100.0 %)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical  (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysterisis value
   00                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS2 Curr Out %'   // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '460_PS2'
_REC_LEN    003E

   // Sensor Record Header
   0042               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   59                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   32                 // Normal Reading 
   64                 // Normal Maximum 
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   70                 // Upper critical 
   64                 // Upper non-critical 
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical  (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysterisis value
   00                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS2 Curr Out %'   // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '350_PS'
_SDR_TAG    '500_PS'
_SDR_TAG    '460_PS'
_REC_LEN    003F

   // Sensor Record Header
   0043               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   5C                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   01                 // Sensor Type -- Temp
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- Degrees C
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   19                 // Normal Reading 
   32                 // Normal Maximum 
   05                 // Normal Minimum 
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   3C                 // Upper critical 
   37                 // Upper non-critical 
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CF                 // Type/Length Code
   'PS1 Temperature'  // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '500_PS2'
_SDR_TAG    '460_PS2'
_REC_LEN    003F

   // Sensor Record Header
   0044               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   5D                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   01                 // Sensor Type -- Temp
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- Degrees C
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   19                 // Normal Reading 
   32                 // Normal Maximum 
   05                 // Normal Minimum 
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   3C                 // Upper critical 
   37                 // Upper non-critical 
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CF                 // Type/Length Code
   'PS2 Temperature'  // String Bytes
//====================================================================//
//
// Backplane Status
//
//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_1_BP4'
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    002B

   // Sensor Record Header
   0045               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   69                 // Sensor Number

   // Record Body Bytes
   16                 // Entity ID - chassis back panel board
   01                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   40                 // Sensor Capabilities
   16                 // Sensor Type - microcontroller
   0A                 // Event / Reading Base Type
   1000               // Assertion Event Mask   -- transition to Off Line =1000
   1000               // Deassertion Event Mask -- transition to Off Line =1000
   1000               // Reading Mask & Settable / Readable Threshold Masks --transition to Off Line =1000
   00                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'HSC1 Status'      // String Bytes

//====================================================================//
//
// Processor (CPU) & DIMM sensors
//
//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROC_1'
_REC_LEN    0029

   // Sensor Record Header
   0048               // Record ID
   51                 // SDR Version
   02                 // Record Type
   24                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   70                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   6F                 // Event / Reading Base Type
   8200               // Assertion Event Mask   --Thermal trip/Presence/Processor disabled =8200
   8200               // Deassertion Event Mask --Thermal trip/Presence/Processor disabled =8200
   8201               // Reading Mask & Settable / Readable Threshold Masks --Thermal trip/Presence/Processor disabled=8201
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'P1 Status'        // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_1'
_REC_LEN    003F

   // Sensor Record Header
   004A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   74                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   F1                 // Normal Reading (F1h = -15 degree C)
   00                 // Normal Maximum (00h = 0 degree C)
   BA                 // Normal Minimum (BAh = -70 degree C)
   //------------------------------------------------------------------//
   00                 // Sensor Maximum Reading (00h = 0 degree C)
   80                 // Sensor Minimum Reading (80h = -128 degree C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degree C)
   00                 // Upper critical (00h = 0 degree C)
   00                 // Upper non-critical (00h = 0 degree C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degree C)
   00                 // Lower critical (00h = 0 degree C)
   00                 // Lower non-critical (00h = 0 degree C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CF                 // Type/Length Code
   'P1 Therm Margin'  // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_1'
_REC_LEN    003F

   // Sensor Record Header
   004C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   78                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   00                 // Normal Reading (00h = 0 %)
   14                 // Normal Maximum (14h = 20 %)
   00                 // Normal Minimum (00h = 0 %)
   //------------------------------------------------------------------//
   64                 // Sensor Maximum Reading (64h = 100 %)
   00                 // Sensor Minimum Reading (00h = 0 %)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 %)
   32                 // Upper critical (32h = 50 %)
   1E                 // Upper non-critical (1Eh = 30 %)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 %)
   00                 // Lower critical (00h = 0 %)
   00                 // Lower non-critical (00h = 0 %)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'P1 Therm Ctrl %'  // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROC_1'
_REC_LEN    0027

   // Sensor Record Header
   004E               // Record ID
   51                 // SDR Version
   02                 // Record Type
   22                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   7C                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   41                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --State asserted =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C7                 // Type/Length Code
   'P1 ERR2'          // String Bytes

//====================================================================//
_SDR_TYPE   02
_REC_LEN    0026

   // Sensor Record Header
   0050               // Record ID
   51                 // SDR Version
   02                 // Record Type
   21                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   80                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C6                 // Type/Length Code
   'CATERR'           // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROC_1'
_REC_LEN    002F

   // Sensor Record Header
   0051               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   81                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'P1 ICC Mismatch' // String Bytes

//====================================================================//
_SDR_TYPE   02
_REC_LEN    002B

   // Sensor Record Header
   0052               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   82                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'CPU Missing'      // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_1'
_REC_LEN    0040

   // Sensor Record Header
   0053               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   83                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   F1                 // Normal Reading (F1h = -15 degree C)
   00                 // Normal Maximum (00h = 0 degree C)
   BA                 // Normal Minimum (BAh = -70 degree C)
   //------------------------------------------------------------------//
   00                 // Sensor Maximum Reading (00h = 0 degree C)
   80                 // Sensor Minimum Reading (80h = -128 degree C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degree C)
   0F                 // Upper critical (0Fh = 15 degree C)
   0A                 // Upper non-critical (0Ah = 10 degree C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degree C)
   00                 // Lower critical (00h = 0 degree C)
   00                 // Lower non-critical (00h = 0 degree C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   D0                 // Type/Length Code
   'P1 DTS Therm Mgn' // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROC_1'
_REC_LEN    002A

   // Sensor Record Header
   0056               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   90                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   01                 // Sensor Type
   05                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --Limit exceeded =0200
   0200               // Deassertion Event Mask --Limit exceeded =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --Limit exceeded =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'P1 VRD Hot'       // String Bytes

//====================================================================//
//
// Power supply fan tachometer sensors
//
//====================================================================//
_SDR_TYPE   02
_SDR_TAG    '500_PS'
_SDR_TAG    '460_PS'
_REC_LEN    002C

   // Sensor Record Header
   005C               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   A0                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0B                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   00                 // Sensor Capabilities -- Manual Rearm
   04                 // Sensor Type - Fan
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Mask
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'PS1 Fan Fail'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    '500_PS2'
_SDR_TAG    '460_PS2'
_REC_LEN    002C

   // Sensor Record Header
   005F               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   A4                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0D                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   00                 // Sensor Capabilities -- Manual Rearm
   04                 // Sensor Type - Fan
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Mask
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'PS2 Fan Fail'     // String Bytes

//====================================================================//
//
// Memory thermal margin sensors
//
//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_1'
_REC_LEN    0040

   // Sensor Record Header
   0062               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   B0                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   EC                 // Normal Reading(ECh = -20 degrees C)
   00                 // Normal Maximum (00h = 0 degrees C)
   BA                 // Normal Minimum (BAh = -70 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degrees C)
   0A                 // Upper critical (0Ah = 10 degrees C)
   05                 // Upper non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degrees C)
   00                 // Lower critical (00h = 0 degrees C)
   00                 // Lower non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   D0                 // Type/Length Code
   'DIMM Thrm Mrgn 1' // String Bytes

//====================================================================//
//
// Memory thermal trip sensors
//
//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROC_1'
_REC_LEN    0030

   // Sensor Record Header
   0066               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   C0                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   0C                 // Sensor Type
   6F                 // Event / Reading Base Type
   0004               // Assertion Event Mask   --State asserted =0004
   0004               // Deassertion Event Mask --State asserted =0004
   0004               // Reading Mask & Settable / Readable Threshold Masks --State asserted =0004
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'P1 Mem Thrm Trip' // String Bytes

//====================================================================//
//
// Global aggregate thermal margin sensors
//
//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'UPS_4HDD'
_SDR_TAG    'UPS_8HDD'
_REC_LEN    003E

   // Sensor Record Header
   0068               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   C8                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask   --[u][c,nc]=0000
   0000               // Deassertion Event Mask --[u][c,nc]=0000
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   EC                 // Normal Reading(ECh = -20 degrees C)
   00                 // Normal Maximum (00h = 0 degrees C)
   BA                 // Normal Minimum (BAh = -70 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degrees C)
   00                 // Upper critical (00h = 0 degrees C)
   00                 // Upper non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degrees C)
   00                 // Lower critical (00h = 0 degrees C)
   00                 // Lower non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CE                 // Type/Length Code
   'Agg Thrm Mgn 1'   // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'UPS_8HDD'
_REC_LEN    003E

   // Sensor Record Header
   006A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   CA                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask   --[u][c,nc]=0000
   0000               // Deassertion Event Mask --[u][c,nc]=0000
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   EC                 // Normal Reading(ECh = -20 degrees C)
   00                 // Normal Maximum (00h = 0 degrees C)
   BA                 // Normal Minimum (BAh = -70 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degrees C)
   00                 // Upper critical (00h = 0 degrees C)
   00                 // Upper non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degrees C)
   00                 // Lower critical (00h = 0 degrees C)
   00                 // Lower non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CE                 // Type/Length Code
   'Agg Thrm Mgn 3'   // String Bytes

//====================================================================//
//
// Voltage regulator sensors
//
//====================================================================//
_SDR_TYPE   01
_REC_LEN    0039

   // Sensor Record Header
   006D               // Record ID
   51                 // SDR Version
   01                 // Record Type
   34                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D0                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   34                 // M
   00                 // M, Tolerance
   1F                 // B
   40                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   D0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E0                 // Normal Reading 
   EC                 // Normal Maximum 
   D5                 // Normal Minimum 
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading 
   00                 // Sensor Minimum Reading 
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable 
   FC                 // Upper critical 
   F5                 // Upper non-critical 
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable 
   C7                 // Lower critical 
   CD                 // Lower non-critical 
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'BB +12.0V'        // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    0039

   // Sensor Record Header
   006E               // Record ID
   51                 // SDR Version
   01                 // Record Type
   34                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D1                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   D9                 // M
   00                 // M, Tolerance
   62                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E1                 // Normal Reading 
   ED                 // Normal Maximum 
   D6                 // Normal Minimum 
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading 
   00                 // Sensor Minimum Reading 
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable 
   FC                 // Upper critical 
   F5                 // Upper non-critical 
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable 
   C9                 // Lower critical 
   CF                 // Lower non-critical 
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'BB +5.0V1'        // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    0038

   // Sensor Record Header
   006F               // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D2                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   8F                 // M
   00                 // M, Tolerance
   F6                 // B
   40                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E2                 // Normal Reading 
   EE                 // Normal Maximum 
   D7                 // Normal Minimum 
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading 
   00                 // Sensor Minimum Reading 
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable 
   FC                 // Upper critical 
   F5                 // Upper non-critical 
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable 
   CB                 // Lower critical 
   D1                 // Lower non-critical 
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C8                 // Type/Length Code
   'BB +3.3V'         // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    0039

   // Sensor Record Header
   0070               // Record ID
   51                 // SDR Version
   01                 // Record Type
   34                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D3                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   D9                 // M
   00                 // M, Tolerance
   62                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E1                 // Normal Reading 
   ED                 // Normal Maximum 
   D6                 // Normal Minimum 
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading 
   00                 // Sensor Minimum Reading 
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable 
   FC                 // Upper critical 
   F5                 // Upper non-critical 
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable 
   C9                 // Lower critical 
   CF                 // Lower non-critical 
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'BB +5.0V2'        // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    003C

   // Sensor Record Header
   0076               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D5                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   34                 // M
   00                 // M, Tolerance
   1F                 // B
   40                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   D0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E0                 // Normal Reading 
   EC                 // Normal Maximum 
   D5                 // Normal Minimum 
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading 
   00                 // Sensor Minimum Reading 
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable 
   FC                 // Upper critical 
   F5                 // Upper non-critical 
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable 
   C7                 // Lower critical 
   CD                 // Lower non-critical 
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'BB +12.0V V2' // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_1'
_REC_LEN    003E

   // Sensor Record Header
   0072               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D6                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   53                 // M
   00                 // M, Tolerance
   7C                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E8                 // Normal Reading 
   EF                 // Normal Maximum 
   E2                 // Normal Minimum 
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading 
   00                 // Sensor Minimum Reading 
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable 
   FC                 // Upper critical 
   F5                 // Upper non-critical 
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable 
   D2                 // Lower critical 
   D7                 // Lower non-critical 
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'BB +1.75V Vccp'   // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_1'
_REC_LEN    003D

   // Sensor Record Header
   FF74               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D8                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   44                 // M
   00                 // M, Tolerance
   C9                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E4                 // Normal Reading (E4h = 1.50 Volt)
   EF                 // Normal Maximum (EFh = 1.57 Volt)
   D9                 // Normal Minimum (D9h = 1.42 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.68 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.66 Volt)
   F5                 // Upper non-critical (F5h = 1.61 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CD                 // Lower critical (CDh = 1.34 Volt)
   D4                 // Lower non-critical (D4h = 1.39 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'BB +1.5 P1DDR' // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    0037

   // Sensor Record Header
   007A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   32                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   DE                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[u,l][c,nc]=0530
   0500               // Deassertion Event Mask   --[u,l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=0303
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   80                 // M
   00                 // M, Tolerance
   DF                 // B
   40                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E7                 // Normal Reading 
   F3                 // Normal Maximum 
   C4                 // Normal Minimum 
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading 
   00                 // Sensor Minimum Reading 
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable 
   A9                 // Lower critical 
   C3                 // Lower non-critical 
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM used for filtering [7:5]= 1 Median [4:0]=5 Sample Count
   C7                 // Type/Length Code
   'BB VBAT'          // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    003D

   // Sensor Record Header
   F031               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   E2                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3C                 // M
   00                 // M, Tolerance
   C1                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   B1                 // Normal Reading 
   EF                 // Normal Maximum 
   62                 // Normal Minimum 
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading 
   00                 // Sensor Minimum Reading 
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable 
   FC                 // Upper critical 
   F5                 // Upper non-critical 
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable 
   5C                 // Lower critical 
   5F                 // Lower non-critical 
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'BB +1.05V PCH'    // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    003D

   // Sensor Record Header
   F032               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   E3                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3C                 // M
   00                 // M, Tolerance
   C1                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   B1                 // Normal Reading 
   EF                 // Normal Maximum 
   62                 // Normal Minimum 
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.16 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.15 Volt)
   F5                 // Upper non-critical (F5h = 1.12 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable 
   5C                 // Lower critical 
   5F                 // Lower non-critical 
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'BB +1.05V AUX'    // String Bytes

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROC_1'
_REC_LEN    003D

   // Sensor Record Header
   007B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   E4                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3D                 // M
   00                 // M, Tolerance
   15                 // B
   80                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E4                 // Normal Reading (E4h = 1.34 Volt)
   EF                 // Normal Maximum (EFh = 1.41 Volt)
   D9                 // Normal Minimum (D9h = 1.27 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.51 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.49 Volt)
   F5                 // Upper non-critical (F5h = 1.45 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CD                 // Lower critical (CDh = 1.20 Volt)
   D4                 // Lower non-critical (D4h = 1.24 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'BB +1.35V MEM' // String Bytes

//====================================================================//
_SDR_TYPE   01
_REC_LEN    003C

   // Sensor Record Header
   F033               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   E8                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask      --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   34                 // M
   00                 // M, Tolerance
   1F                 // B
   40                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   D0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E0                 // Normal Reading 
   EC                 // Normal Maximum 
   D5                 // Normal Minimum 
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading 
   00                 // Sensor Minimum Reading 
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable 
   FC                 // Upper critical 
   F5                 // Upper non-critical 
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable 
   C7                 // Lower critical 
   CD                 // Lower non-critical 
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'BB +12.0V V1'     // String Bytes

//====================================================================//
//
// Hot-swap backplane (HSBP) sensors
//
//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_1_BP4'
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    002C

   // Sensor Record Header
   F086               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F0                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 0 Status'     // String Bytes
   
_SDR_TYPE   02
_SDR_TAG    'HSBP_1_BP4'
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    002C

   // Sensor Record Header
   007F               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F1                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 1 Status'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_1_BP4'
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    002C

   // Sensor Record Header
   0080               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F2                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 2 Status'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_1_BP4'
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    002C

   // Sensor Record Header
   0081               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F3                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 3 Status'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    002C

   // Sensor Record Header
   0082               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F4                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 4 Status'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    002C

   // Sensor Record Header
   0083               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F5                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 5 Status'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    002C

   // Sensor Record Header
   0084               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F6                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 6 Status'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    002C

   // Sensor Record Header
   0085               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F7                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 7 Status'     // String Bytes

//====================================================================//
// Management Engine (ME controller) records
//====================================================================//
_SDR_TYPE   03
_SDR_TAG    'RPSKU'
_SDR_TAG    'RPSESKU'
_REC_LEN    001E

   // Sensor Record Header
   0097               // Record ID
   51                 // SDR Version
   03                 // Record Type
   19                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   17                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   01                 // Entity Instance
   DC                 // Sensor type
   75                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'SPS FW Health'    // String Bytes

//====================================================================//
_SDR_TYPE   03
_SDR_TAG    'RPSKU'
_REC_LEN    001D

   // Sensor Record Header
   0098               // Record ID
   51                 // SDR Version
   03                 // Record Type
   18                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   18                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   01                 // Entity Instance
   DC                 // Sensor type
   72                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'NM Exception'     // String Bytes

//====================================================================//
// FSC Record Type = 0Dh (NM discovery)
// Intel(R) Server Chassis BP15 Non-Redundant.
//====================================================================//
_SDR_TYPE      C0
_REC_LEN       0010

   // Sensor Record Header
   009C               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0B                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0D                 // Record subtype - NM Discovery
   01                 // Version number of record subtype
   2C                 // NM Device Slave Address ([7:1] - 7-bit address; [0] - reserved)
   60                 // [7:4] - channel number (6 for secondary IPMB) [3:2] - reserved [1:0] - sensor owner LUN)
   25                 // Node Manager Health Event sensor
   24                 // Node Manager Exception Event sensor
   26                 // Node Manager Operational Capabilities sensor
   27                 // Node Manager Threshold Exceeded sensor

//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'RPSKU'
_SDR_TAG    'RPSESKU'
_REC_LEN    0036

   // Sensor Record Header
   009D               // Record ID
   51                 // SDR Version
   01                 // Record Type
   31                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   34                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   63                 // Sensor Initialization
   B8                 // Sensor Capabilities
   0C                 // Sensor Type -- Memory
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask   --[u][c,nc]=0000
   0000               // Deassertion Event Mask --[u][c,nc]=0000
   3F3F               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=3F3F
   01                 // Sensor Units 1
   00                 // Sensor Units 2 -- Degrees C
   00                 // Sensor Units 3
   00                 // Linearization
   05                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   F0                 // R exp, B exp
   00                 // Analog characteristic flags
   //------------------------------------------------------------------//
   00                 // Normal Reading 
   00                 // Normal Maximum 
   00                 // Normal Minimum 
   //------------------------------------------------------------------//
   00                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical
   00                 // Upper non-critical 
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C6                 // Type/Length Code
   'P1 MTT'           // String Bytes

//====================================================================//
//
// BIOS Recovery Mode Status
//
//====================================================================//
_SDR_TYPE 03 
_REC_LEN 0020

    // Sensor Record Header
    F151 // Record ID
    51 // SDR Version
    03 // Record Type 
    1B // Record Length

    // Record Key Bytes
    33 // Sensor Owner ID
    00 // Sensor Owner LUN
    15 // Sensor Number

    // Record Body Bytes
    22 // Entity ID
    01 // Entity Instance
    0F // Sensor type 
    70 // Event/Reading Type Code 
    0000 // Sensor Record Sharing
    00 // Reserved
    00 // OEM
    CF // Type/Length Code 
    'BIOS Recov Mode' // String Bytes

//====================================================================//
// BIOS owned sensor records
//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   009F               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   02                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID = Memory Device
   01                 // Entity Instance
   0C                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mmry ECC Sensor'  // Memory ECC Error Sensor

//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   00A0               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   03                 // Sensor Number

   // Record Body Bytes
   30                 // Entity ID = PCI
   01                 // Entity Instance
   13                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCI Lgcy Sensor'  // Legacy PCI Sensor

//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   00A1               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   04                 // Sensor Number

   // Record Body Bytes
   31                 // Entity ID = PCI Express
   01                 // Entity Instance
   13                 // Sensor Type
   70                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCIe Fat Sensor'  // PCI Express Fatal Error Sensor

//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   00A6               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   14                 // Sensor Number

   // Record Body Bytes
   31                 // Entity ID = PCI Express
   04                 // Entity Instance
   13                 // Sensor Type
   70                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCIe Fat Sensor'  // PCI Express Fatal Error Sensor
   
//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   00A2               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   05                 // Sensor Number

   // Record Body Bytes
   31                 // Entity ID = PCI Express
   02                 // Entity Instance
   13                 // Sensor Type
   71                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCIe Cor Sensor'  // PCI Express Correctable Error Sensor

//====================================================================//
// SDR Type 03 - Event Only Record for BIOS Boot Events
//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   00A7               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   83                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   03                 // Entity Instance
   12                 // Sensor Type
   6F                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'BIOS Evt Sensor'  // BIOS Boot Event Sensor

//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   00A8               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   83                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   04                 // Entity Instance
   12                 // Sensor Type
   6F                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'BIOS Evt Sensor'  // BIOS Boot Event Sensor

//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   00A3               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   06                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID-BIOS POST
   01                 // Entity Instance
   0F                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'POST Err Sensor'  // POST Error Sensor

//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   00AA               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   02                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID = Memory
   02                 // Entity Instance
   0C                 // Sensor Type
   09                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mem Conf Sensor'  // Memory configuration failed

//====================================================================//
_SDR_TYPE   03
_REC_LEN    001F

   // Sensor Record Header
   00AC               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1A                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   10                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID = Memory Device
   03                 // Entity Instance
   0C                 // Sensor Type
   7F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Mem err Sensor'   //Memory Error Extension

//====================================================================//
// SDR Type 11 Records
//====================================================================//
_SDR_TYPE   11
_REC_LEN    0019

   // Sensor Record Header
   00B1               // Record ID
   51                 // SDR Version
   11                 // Record Type
   14                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   00                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   07                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // OEM
   C9                 // Type/Length Code
   'Baseboard'        // String Bytes

//====================================================================//
_SDR_TYPE   11
_REC_LEN    001B

   // Sensor Record Header
   00B2               // Record ID
   51                 // SDR Version
   11                 // Record Type
   16                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   04                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   0C                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // OEM
   CB                 // Type/Length Code
   'front panel'      // String Bytes
   
//====================================================================//
_SDR_TYPE   11
_SDR_TAG    'IO_MODULE_FRU'
_REC_LEN    0019

   // Sensor Record Header
   00B3               // Record ID
   51                 // SDR Version
   11                 // Record Type
   14                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   09                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   2C                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // OEM
   C9                 // Type/Length Code
   'IO Module'        // String Bytes

//====================================================================//
_SDR_TYPE   11
_SDR_TAG    'SAS_MODULE_FRU'
_REC_LEN    001A

   // Sensor Record Header
   00B4               // Record ID
   51                 // SDR Version
   11                 // Record Type
   15                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   0A                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   33                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // OEM
   CA                 // Type/Length Code
   'SAS Module'       // String Bytes 

//=========================================================
_SDR_TYPE   11
_SDR_TAG   'HSBP1_TEMP'
_REC_LEN    0015

   // Sensor Record Header
   F0A3               // Record ID
   51                 // SDR Version
   11                 // Record Type
   10                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   05                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   07                 // FRU Entity ID
   37                 // FRU Entity Instance
   00                 // OEM
   C5                 // Type/Length Code
   'HSBP1'            // String Bytes  

//=========================================================
_SDR_TYPE   11
_SDR_TAG   'PS1'
_REC_LEN    0013

   // Sensor Record Header
   F0A6               // Record ID
   51                 // SDR Version
   11                 // Record Type
   0E                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   02                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   07                 // FRU Entity ID
   35                 // FRU Entity Instance
   00                 // OEM
   C3                 // Type/Length Code
   'PS1'              // String Bytes   
   
//=========================================================
_SDR_TYPE   11
_SDR_TAG   'PS2'
_REC_LEN    0013

   // Sensor Record Header
   F0A7               // Record ID
   51                 // SDR Version
   11                 // Record Type
   0E                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   03                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   07                 // FRU Entity ID
   36                 // FRU Entity Instance
   00                 // OEM
   C3                 // Type/Length Code
   'PS2'              // String Bytes     

//====================================================================//
// SDR Type 12 Records
//====================================================================//
_SDR_TYPE   12
_REC_LEN    0020

   // Sensor Record Header
   00B5               // Record ID
   51                 // SDR Version
   12                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   20                 // Device Slave Address
   00                 // Channel Number

   // Record Body Bytes
   08                 // Power state notification
   BF                 // Device capabilities
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   07                 // Entity ID
   01                 // Entity instance
   00                 // OEM
   D0                 // Type/Length Code
   'Basbrd Mgmt Ctlr' // String Bytes

//====================================================================//
_SDR_TYPE   12
_SDR_TAG    'RPSKU'
_SDR_TAG    'RPSESKU'
_REC_LEN    0012

   // Sensor Record Header
   00B6               // Record ID
   51                 // SDR Version
   12                 // Record Type
   0D                 // Record Length

   // Record Key Bytes
   2C                 // Device Slave Address
   06                 // Channel number

   // Record Body Bytes
   24                 // Power State Notification
   21                 // Device Capabilities
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   2E                 // Entity ID
   01                 // Entity Instance
   00                 // OEM
   C2                 // Type/Length Code
   'ME'               // String Bytes

//====================================================================//
// Thermal Profile Data, Close Loop
//====================================================================//
//====================================================================//
//
// SDR Type C0/02 Record For Power Unit Map 
//
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'PS_REDUNDANCY'
_REC_LEN    000E

   // Sensor Record Header
   00B7               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   09                 // Record Length
   
   // Record Body Bytes
   570100             // Manufacturer ID
   02                 // Record Subtype Value
   02                 // Power Unit Redundancy sensor number
   00                 // Bits [7:1]-Reserved; Bit[0]-1=No monitorable supplies present
   01                 // The number of present and operational
   50                 // Power Supply Status 1 Sensor Number
   51                 // Power Supply Status 2 Sensor Number

//====================================================================//
//
// SDR Type C0/09 Records For Voltage Sensor Scaling
//
//====================================================================//
_SDR_TYPE   C0
_REC_LEN    002B

   // Sensor Record Header
   00BA               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   26                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   09                 // Record sub-type - Voltage Sensor Scaling

   // Voltage Sensor Scaling Record
   0B                 // Number of entries following
   D0                 // Voltage Sensor Number
   B80A               // Scale Factor (LSB MSB)
   D1                 // Voltage Sensor Number
   9D0A               // Scale Factor (LSB MSB)
   D2                 // Voltage Sensor Number
   980A               // Scale Factor (LSB MSB)
   D3                 // Voltage Sensor Number
   9D0A               // Scale Factor (LSB MSB)
   E8                 // Voltage Sensor Number
   B80A               // Scale Factor (LSB MSB)
   D5                 // Voltage Sensor Number
   B80A               // Scale Factor (LSB MSB)
   D6                 // Voltage Sensor Number
   510C               // Scale Factor (LSB MSB)
   DE                 // Voltage Sensor Number
   CA09               // Scale Factor (LSB MSB)
   E2                 // Voltage Sensor Number
   1A10               // Scale Factor (LSB MSB)
   E3                 // Voltage Sensor Number
   1A10               // Scale Factor (LSB MSB)
   E4                 // Voltage Sensor Number
   1A10               // Scale Factor (LSB MSB)

//====================================================================//
//
// SDR Type C0/0A Record For Fan Sensor Scaling SDR Record
//
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0019

   // Sensor Record Header
   00BE               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   14                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record Subtype Value*******   Fan Sensor Scaling SDR Record   **********

   // Fan Sensor Scaling Record
   00                 // Return Format; Bit 0=Fan 0, Bit 1=Fan 1; etc. 0=RPM, 1=Period(***TBD***)
   00                 // Number of tach Pulses Per Revolution: Bit 0=Fan 0, Bit 1=Fan 1, etc.; 0=2 Pulses/Rev, 1=1 Pulse/Rev(***TBD***)
   A861               // Placeholder for System Fan 1(SN:0x30), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 2(SN:0x31), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 3(SN:0x32), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 4(SN:0x33), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   0001               // Null(SN:0x34)
   0001               // Null(SN:0x35)
   A861               // Placeholder for Processor Fan 1(SN:0x36), Max RPM: 25000RPM == A861 (the order is LSB, MSB)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    0019

   // Sensor Record Header
   F1BD               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   14                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record Subtype Value*******   Fan Sensor Scaling SDR Record   **********

   // Fan Sensor Scaling Record
   00                 // Return Format; Bit 0=Fan 0, Bit 1=Fan 1; etc. 0=RPM, 1=Period(***TBD***)
   00                 // Number of tach Pulses Per Revolution: Bit 0=Fan 0, Bit 1=Fan 1, etc.; 0=2 Pulses/Rev, 1=1 Pulse/Rev(***TBD***)
   A861               // Placeholder for System Fan 1(SN:0x30), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 2(SN:0x31), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 3(SN:0x32), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   0001               // Null(SN:0x33)
   0001               // Null(SN:0x34)
   0001               // Null(SN:0x35)
   0001               // Null(SN:0x36)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4HDD'
_REC_LEN    0019

   // Sensor Record Header
   F2BD               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   14                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record Subtype Value*******   Fan Sensor Scaling SDR Record   **********

   // Fan Sensor Scaling Record
   00                 // Return Format; Bit 0=Fan 0, Bit 1=Fan 1; etc. 0=RPM, 1=Period(***TBD***)
   00                 // Number of tach Pulses Per Revolution: Bit 0=Fan 0, Bit 1=Fan 1, etc.; 0=2 Pulses/Rev, 1=1 Pulse/Rev(***TBD***)
   0001               // Null(SN:0x30)
   0001               // Null(SN:0x31)
   0001               // Null(SN:0x32)
   9C18               // Placeholder for System Fan 4(SN:0x33), Max RPM: 6300RPM == 9C18 (the order is LSB, MSB)
   0001               // Null(SN:0x34)
   0001               // Null(SN:0x35)
   800C               // Placeholder for Processor Fan 1(SN:0x36), Max RPM: 800CRPM == 3200 (the order is LSB, MSB)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8HDD'
_REC_LEN    0019

   // Sensor Record Header
   F3BD               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   14                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record Subtype Value*******   Fan Sensor Scaling SDR Record   **********

   // Fan Sensor Scaling Record
   00                 // Return Format; Bit 0=Fan 0, Bit 1=Fan 1; etc. 0=RPM, 1=Period(***TBD***)
   00                 // Number of tach Pulses Per Revolution: Bit 0=Fan 0, Bit 1=Fan 1, etc.; 0=2 Pulses/Rev, 1=1 Pulse/Rev(***TBD***)
   C819               // Placeholder for System Fan 1(SN:0x30), Max RPM: 6600RPM == C819 (the order is LSB, MSB)
   0001               // Null(SN:0x31)
   0001               // Null(SN:0x32)
   9C18               // Placeholder for System Fan 4(SN:0x33), Max RPM: 6300RPM == 9C18 (the order is LSB, MSB)
   0001               // Null(SN:0x34)
   0001               // Null(SN:0x35)
   800C               // Placeholder for Processor Fan 1(SN:0x36), Max RPM: 3200RPM == 800C (the order is LSB, MSB)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'FCT'
_REC_LEN    001D

   // Sensor Record Header
   00BF               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   18                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record Subtype Value*******   Fan Sensor Scaling SDR Record   **********

   // Fan Sensor Scaling Record
   00                 // Return Format; Bit 0=Fan 0, Bit 1=Fan 1; etc. 0=RPM, 1=Period(***TBD***)
   00                 // Number of tach Pulses Per Revolution: Bit 0=Fan 0, Bit 1=Fan 1, etc.; 0=2 Pulses/Rev, 1=1 Pulse/Rev(***TBD***)
   A861               // Placeholder for System Fan 1(SN:0x30), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 2(SN:0x31), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 3(SN:0x32), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 4(SN:0x33), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   0001               // Null(SN:0x34)
   0001               // Null(SN:0x35)
   A861               // Placeholder for Processor Fan 1(SN:0x36), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   0001               // Null(SN:0x37)
   0001               // Null(SN:0x38)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'FCT2'
_REC_LEN    001D

   // Sensor Record Header
   00C0               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   18                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record Subtype Value*******   Fan Sensor Scaling SDR Record   **********

   // Fan Sensor Scaling Record
   00                 // Return Format; Bit 0=Fan 0, Bit 1=Fan 1; etc. 0=RPM, 1=Period(***TBD***)
   00                 // Number of tach Pulses Per Revolution: Bit 0=Fan 0, Bit 1=Fan 1, etc.; 0=2 Pulses/Rev, 1=1 Pulse/Rev(***TBD***)
   0001               // Null(SN:0x30)
   0001               // Null(SN:0x31)
   0001               // Null(SN:0x32)
   0001               // Null(SN:0x33)
   0001               // Null(SN:0x34)
   0001               // Null(SN:0x35)
   A861               // Placeholder for Processor Fan 1(SN:0x36), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   0001               // Null(SN:0x37)
   0001               // Null(SN:0x38)

//====================================================================//
//
// Global Stepwise and Global Clamp Headers
//
//====================================================================//
//====================================================================//
// Global Clamp Header Record
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000'
_SDR_TAG    'UPS_4HDD'
_SDR_TAG    'UPS_8HDD'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00C1           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length
   
   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   74             // Clamp Header ID
   74             // Temperature Sensor Number -- (P1 Therm Margin)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value 
   64             // Sensor Fail Control Value 
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   00             // Temperature (00h = 0 degree C)
   01             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000'
_SDR_TAG    'UPS_4HDD'
_SDR_TAG    'UPS_8HDD'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00C3           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length
   
   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)
   
   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   B0             // Clamp Header ID
   B0             // Temperature Sensor Number -- (DIMM Thrm Mrgn 1)
   00             // Entity Presence Sensor Number -- (NA)
   00             // Sensor Disabled Control Value 
   64             // Sensor Fail Control Value 
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   F8             // Temperature (F8h = -8 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000'
_SDR_TAG    'UPS_4HDD'
_SDR_TAG    'UPS_8HDD'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00C7           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length
   
   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)
   
   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   20             // Clamp Header ID
   20             // Temperature Sensor Number -- (BB EDGE Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value 
   64             // Sensor Fail Control Value 
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   28             // Temperature (28h = 40 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000'
_SDR_TAG    'UPS_4HDD'
_SDR_TAG    'UPS_8HDD'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00C8           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length
   
   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)
   
   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   24             // Clamp Header ID
   24             // Temperature Sensor Number -- (BB CPU1 VR Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value 
   64             // Sensor Fail Control Value 
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   55             // Temperature (55h = 85 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000'
_SDR_TAG    'UPS_4HDD'
_SDR_TAG    'UPS_8HDD'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00C9           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length
   
   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)
   
   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   23             // Clamp Header ID
   23             // Temperature Sensor Number -- (BB BMC Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value 
   64             // Sensor Fail Control Value 
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   58             // Temperature (58h = 88 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000'
_SDR_TAG    'UPS_4HDD'
_SDR_TAG    'UPS_8HDD'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00CC           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length
   
   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)
   
   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   22             // Clamp Header ID
   22             // Temperature Sensor Number -- (PCH Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value 
   64             // Sensor Fail Control Value 
   39             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   53             // Temperature (53h = 83 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'HSBP_1_BP4'
_SDR_TAG    'HSBP_1_BP8'
_REC_LEN    0017

   // Sensor Record Header
   00CD           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length
   
   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)
   
   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   29             // Clamp Header ID
   29             // Temperature Sensor Number -- (HSBP 1 Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value 
   64             // Sensor Fail Control Value 
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   32             // Temperature (32h = 50 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'IO_MODULE'
_REC_LEN    0017

   // Sensor Record Header
   00D0           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length
   
   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)
   
   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   26             // Clamp Header ID
   26             // Temperature Sensor Number -- (I/O Mod Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value 
   64             // Sensor Fail Control Value 
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   3C             // Temperature (3Ch = 60 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'SAS_MODULE'
_REC_LEN    0017

   // Sensor Record Header
   00D1           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length
   
   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)
   
   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   2D             // Clamp Header ID
   2D             // Temperature Sensor Number -- (SAS Mod Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value 
   64             // Sensor Fail Control Value 
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   50             // Temperature (50h = 80 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)
   
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000'
_SDR_TAG    'UPS_4HDD'
_SDR_TAG    'UPS_8HDD'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00D2           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length
   
   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)
   
   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   83             // Clamp Header ID
   83             // Temperature Sensor Number -- (P1 DTS Therm Mgn)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value 
   64             // Sensor Fail Control Value 
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   FA             // Temperature (FAh = -6 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'EATEMP'
_REC_LEN    0017

   // Sensor Record Header
   00D4           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length
   
   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)
   
   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   2E             // Clamp Header ID
   2E             // Temperature Sensor Number -- (Exit Air Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value 
   64             // Sensor Fail Control Value 
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   2B             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 3
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   40             // Temperature (40h = 64 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000'
_SDR_TAG    'UPS_4HDD'
_SDR_TAG    'UPS_8HDD'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00D5           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length
   
   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)
   
   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   5C             // Clamp Header ID
   5C             // Temperature Sensor Number -- (PSU1 Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value 
   64             // Sensor Fail Control Value 
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   35             // Temperature (35h = 53 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000'
_SDR_TAG    'UPS_4HDD'
_SDR_TAG    'UPS_8HDD'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00D6           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length
   
   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)
   
   // Global Clamp Header Record
   // Clamp Type Temperature Sensor sub-record
   5D             // Clamp Header ID
   5D             // Temperature Sensor Number -- (PSU2 Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value 
   64             // Sensor Fail Control Value 
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   35             // Temperature (35h = 53 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'PROC_1'
_REC_LEN    0017

   // Sensor Record Header
   00D8           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length
   
   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   93             // Clamp Header ID
   74             // Temperature Sensor Number -- (P1 Therm Margin)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value 
   64             // Sensor Fail Control Value 
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   18             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 3; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   00             // Temperature (00h = 0 degree C)
   01             // Clamp Flags [7:4] - CPU Number = 1; [3:1] - Reserved=0; [0] - Temp Source = 1 (use TControl)

//======================================================================//
_SDR_TYPE   C0
_SDR_TAG    'PROC_1'
_REC_LEN    0017

   // Sensor Record Header
   E0AA           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length
   
   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   63             // Clamp Header ID
   74             // Temperature Sensor Number -- (P1 Therm Margin)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value 
   64             // Sensor Fail Control Value 
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   18             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 3; [2:0]-Positive Hysteresis = 0
   20             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   FD             // Temperature (FDh = -3 degree C)
   01             // Clamp Flags [7:4] - CPU Number = 1; [3:1] - Reserved=0; [0] - Temp Source = 1 (use TControl)

//======================================================================//
_SDR_TYPE   C0
_SDR_TAG    'PROC_1'
_REC_LEN    0017

   // Sensor Record Header
   E0AB           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length
   
   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   53             // Clamp Header ID
   74             // Temperature Sensor Number -- (P1 Therm Margin)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value 
   64             // Sensor Fail Control Value 
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   18             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 3; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   FC             // Temperature (FCh = -4 degree C)
   01             // Clamp Flags [7:4] - CPU Number = 1; [3:1] - Reserved=0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
// Global Stepwise Header Record
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000'
_SDR_TAG    'UPS_4HDD'
_SDR_TAG    'UPS_8HDD'
_REC_LEN    0013

   // Sensor Record Header
   00D9           // Record ID
   51             // SDR Version
   C0             // Record Type
   0E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   01             // FSC Record Type (01h = Global Stepwise Header Records)

   // Global Stepwise Header Record
   00             // Stepwise Header ID
   21             // Temperature Sensor Number -- (Front Panel Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value 
   64             // Sensor Fail Control Value 
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   50             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 2; [2:0]-Positive Hysteresis = 0

   // Global Stepwise Header Record
   // Add More Stepwise Header Records Here (up to 64 bytes total record length)   

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000'
_SDR_TAG    'UPS_4HDD'
_SDR_TAG    'UPS_8HDD'
_SDR_TAG    'OTHER'
_REC_LEN    0013

   // Sensor Record Header
   00DA           // Record ID
   51             // SDR Version
   C0             // Record Type
   0E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   01             // FSC Record Type (01h = Global Stepwise Header Records)

   // Global Stepwise Header Record
   01             // Stepwise Header ID
   20             // Temperature Sensor Number -- (BB EDGE Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value 
   64             // Sensor Fail Control Value 
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   50             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 2; [2:0]-Positive Hysteresis = 0

   // Global Stepwise Header Record
   // Add More Stepwise Header Records Here (up to 64 bytes total record length)

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000'
_SDR_TAG    'UPS_8HDD'
_REC_LEN    0013

   // Sensor Record Header
   00DB           // Record ID
   51             // SDR Version
   C0             // Record Type
   0E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   11             // FSC Record Type (11h = Global Stepwise Header Records)

   // Global Stepwise Header Record
   02             // Stepwise Header ID
   08             // Temperature Sensor Number -- (PS1)
   00             // Entity Presence Sensor Number -- (NA)
   00             // Sensor Disabled Control Value 
   00             // Sensor Fail Control Value 
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   00             // Sleep State and Hysteresis [7:6]-Supported in S1; [5:3]-Negative Hysteresis = 0; [2:0]-Positive Hysteresis = 0

   // Global Stepwise Header Record
   // Add More Stepwise Header Records Here (up to 64 bytes total record length)

//====================================================================//
// Minimum Stepwise Linear Tables
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_SAS'
_REC_LEN    003B

   // Sensor Record Header
   00DD           // Record ID
   51             // SDR Version
   C0             // Record Type
   36             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   00             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   14             // 20C
   19             // 25%
   1E             // 30C
   19             // 25%
   24             // 36C
   1E             // 30%
   26             // 38C
   23             // 35%
   32             // 50C
   64             // 100%

   // Global Stepwise Curve Record
   01             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   14             // 20C
   19             // 25%
   1E             // 30C
   19             // 25%
   24             // 36C
   23             // 35%
   26             // 38C
   28             // 40%
   32             // 50C
   64             // 100%

   // Global Stepwise Curve Record
   02             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   14             // 20C
   19             // 25%
   1E             // 30C
   19             // 25%
   24             // 36C
   21             // 33%
   26             // 38C
   25             // 37%
   32             // 50C
   64             // 100%
   
   // Global Stepwise Curve Record
   03             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   14             // 20C
   19             // 25%
   1C             // 28C
   28             // 40%
   24             // 36C
   2D             // 45%
   26             // 38C
   32             // 50%
   32             // 50C
   64             // 100%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_NOSAS'
_REC_LEN    003B

   // Sensor Record Header
   00DE           // Record ID
   51             // SDR Version
   C0             // Record Type
   36             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   04             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   14             // 20C
   19             // 25%
   1E             // 30C
   19             // 25%
   24             // 36C
   1E             // 30%
   26             // 38C
   23             // 35%
   32             // 50C
   64             // 100%

   // Global Stepwise Curve Record
   05             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   14             // 20C
   19             // 25%
   1E             // 30C
   19             // 25%
   24             // 36C
   23             // 35%
   26             // 38C
   28             // 40%
   32             // 50C
   64             // 100%

   // Global Stepwise Curve Record
   06             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   14             // 20C
   19             // 25%
   1C             // 28C
   23             // 35%
   24             // 36C
   28             // 40%
   26             // 38C
   2D             // 45%
   32             // 50C
   64             // 100%

   // Global Stepwise Curve Record
   07             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   14             // 20C
   23             // 35%
   1C             // 28C
   2D             // 45%
   24             // 36C
   37             // 55%
   26             // 38C
   3C             // 60%
   32             // 50C
   64             // 100%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXSAS'
_REC_LEN    003B

   // Sensor Record Header
   00E0           // Record ID
   51             // SDR Version
   C0             // Record Type
   36             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   0E             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   11             // 17C
   19             // 25%
   1B             // 27C
   19             // 25%
   25             // 37C
   23             // 35%
   2A             // 42C
   28             // 40%
   2F             // 47C
   64             // 100%
   
   // Global Stepwise Curve Record
   0F             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   11             // 17C
   1E             // 30%
   1B             // 27C
   1E             // 30%
   25             // 37C
   23             // 35%
   2A             // 42C
   28             // 40%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   10             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   11             // 17C
   1B             // 27%
   1B             // 27C
   1C             // 28%
   25             // 37C
   37             // 55%
   2A             // 42C
   41             // 65%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   11             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   11             // 17C
   28             // 40%
   1B             // 27C
   2D             // 45%
   25             // 37C
   3C             // 60%
   2A             // 42C
   46             // 70%
   2F             // 47C
   64             // 100%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXNOSAS'
_REC_LEN    003B

   // Sensor Record Header
   00E1           // Record ID
   51             // SDR Version
   C0             // Record Type
   36             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   12             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   11             // 17C
   14             // 20%
   1B             // 27C
   14             // 20%
   25             // 37C
   1E             // 30%
   2A             // 42C
   23             // 35%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   13             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   11             // 17C
   19             // 25%
   1B             // 27C
   19             // 25%
   25             // 37C
   1E             // 30%
   2A             // 42C
   23             // 35%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   14             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   11             // 17C
   16             // 22%
   1B             // 27C
   17             // 23%
   25             // 37C
   24             // 36%
   2A             // 42C
   29             // 41%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   15             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   11             // 17C
   23             // 35%
   1B             // 27C
   28             // 40%
   25             // 37C
   2F             // 47%
   2A             // 42C
   34             // 52%
   2F             // 47C
   64             // 100%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXNOSAS'
_REC_LEN    0023

   // Sensor Record Header
   0FE1           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   2C             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   11             // 17C
   1C             // 28%
   1B             // 27C
   26             // 38%
   25             // 37C
   3F             // 63%
   2A             // 42C
   4B             // 75%
   2F             // 47C
   64             // 100%


   // Global Stepwise Curve Record
   2D             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   11             // 17C
   37             // 55%
   1B             // 27C
   41             // 65%
   25             // 37C
   50             // 80%
   2A             // 42C
   5A             // 90%
   2F             // 47C
   64             // 100%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4SAS'
_REC_LEN    003B

   // Sensor Record Header
   00E2           // Record ID
   51             // SDR Version
   C0             // Record Type
   36             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   16             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   11             // 17C
   23             // 35%
   1B             // 27C
   23             // 35%
   25             // 37C
   28             // 40%
   2A             // 42C
   2D             // 45%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   17             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   11             // 17C
   28             // 40%
   1B             // 27C
   28             // 40%
   25             // 37C
   2D             // 45%
   2A             // 42C
   32             // 50%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   18             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   11             // 17C
   16             // 22%
   1B             // 27C
   2A             // 42%
   25             // 37C
   3E             // 62%
   2A             // 42C
   48             // 72%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   19             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   11             // 17C
   1B             // 27%
   1B             // 27C
   2E             // 46%
   25             // 37C
   42             // 66%
   2A             // 42C
   4B             // 75%
   2F             // 47C
   64             // 100%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4NOSAS'
_REC_LEN    003B

   // Sensor Record Header
   00E3           // Record ID
   51             // SDR Version
   C0             // Record Type
   36             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   1A             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   11             // 17C
   1E             // 30%
   1B             // 27C
   1E             // 30%
   25             // 37C
   23             // 35%
   2A             // 42C
   28             // 40%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   1B             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   11             // 17C
   23             // 35%
   1B             // 27C
   23             // 35%
   25             // 37C
   28             // 40%
   2A             // 42C
   2D             // 45%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   1C             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   11             // 17C
   1C             // 28%
   1B             // 27C
   2A             // 42%
   25             // 37C
   4C             // 76%
   2A             // 42C
   51             // 81%
   2F             // 47C
   64             // 100%

   // Global Stepwise Curve Record
   1D             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   11             // 17C
   2D             // 45%
   1B             // 27C
   36             // 54%
   25             // 37C
   50             // 80%
   2A             // 42C
   5A             // 90%
   2F             // 47C
   64             // 100%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35SAS'
_REC_LEN    003B

   // Sensor Record Header
   F0E4           // Record ID
   51             // SDR Version
   C0             // Record Type
   36             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   1E             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   13             // 19C
   16             // 22%
   1D             // 29C
   1B             // 27%
   27             // 39C
   2A             // 42%
   2C             // 44C
   30             // 48%
   31             // 49C
   37             // 55%

   // Global Stepwise Curve Record
   1F             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   13             // 19C
   16             // 22%
   1D             // 29C
   1F             // 31%
   27             // 39C
   2C             // 44%
   2C             // 44C
   32             // 50%
   31             // 49C
   38             // 56%

   // Global Stepwise Curve Record
   20             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   13             // 19C
   0C             // 12%
   1D             // 29C
   0E             // 14%
   27             // 39C
   22             // 34%
   2C             // 44C
   2B             // 43%
   31             // 49C
   33             // 51%

   // Global Stepwise Curve Record
   21             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   13             // 19C
   0C             // 12%
   1D             // 29C
   13             // 19%
   27             // 39C
   25             // 37%
   2C             // 44C
   2D             // 45%
   31             // 49C
   35             // 53%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35SAS'
_REC_LEN    0023

   // Sensor Record Header
   F1E4           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   22             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   13             // 19C
   11             // 17%
   1D             // 29C
   13             // 19%
   27             // 39C
   27             // 39%
   2C             // 44C
   30             // 48%
   31             // 49C
   64             // 100%

   // Global Stepwise Curve Record
   23             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   13             // 19C
   11             // 17%
   1D             // 29C
   18             // 24%
   27             // 39C
   2A             // 42%
   2C             // 44C
   32             // 50%
   31             // 49C
   64             // 100%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35NOSAS'
_REC_LEN    003B

   // Sensor Record Header
   F0E5           // Record ID
   51             // SDR Version
   C0             // Record Type
   36             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   24             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   13             // 19C
   16             // 22%
   1D             // 29C
   1B             // 27%
   27             // 39C
   2A             // 42%
   2C             // 44C
   30             // 48%
   31             // 49C
   37             // 55%

   // Global Stepwise Curve Record
   25             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   13             // 19C
   16             // 22%
   1D             // 29C
   1F             // 31%
   27             // 39C
   2C             // 44%
   2C             // 44C
   32             // 50%
   31             // 49C
   38             // 56%

   // Global Stepwise Curve Record
   26             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   13             // 19C
   0C             // 12%
   1D             // 29C
   0E             // 14%
   27             // 39C
   22             // 34%
   2C             // 44C
   2B             // 43%
   31             // 49C
   33             // 51%

   // Global Stepwise Curve Record
   27             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   13             // 19C
   0C             // 12%
   1D             // 29C
   13             // 19%
   27             // 39C
   25             // 37%
   2C             // 44C
   2D             // 45%
   31             // 49C
   35             // 53%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35NOSAS'
_REC_LEN    0023

   // Sensor Record Header
   F0F5           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   28             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   13             // 19C
   11             // 17%
   1D             // 29C
   13             // 19%
   27             // 39C
   27             // 39%
   2C             // 44C
   30             // 48%
   31             // 49C
   64             // 100%

   // Global Stepwise Curve Record
   29             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   13             // 19C
   11             // 17%
   1D             // 29C
   18             // 24%
   27             // 39C
   2A             // 42%
   2C             // 44C
   32             // 50%
   31             // 49C
   64             // 100%

_SDR_TYPE   C0
_SDR_TAG    'R1000_SAS'
_SDR_TAG    'R1000_NOSAS'
_SDR_TAG    'UPS_8X35SAS'
_SDR_TAG    'UPS_8X35NOSAS'
_REC_LEN    0017

   // Sensor Record Header
   F1E7           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   37             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   14             // 20C
   14             // 20%
   28             // 40C
   1E             // 30%
   3C             // 60C
   2D             // 45%
   50             // 80C
   41             // 65%
   64             // 100C
   64             // 100%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0023

   // Sensor Record Header
   00E4           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   5B             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   1E             // 30C
   19             // 25%
   3C             // 60C
   32             // 50%

   // Global Stepwise Curve Record
   5C             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   1E             // 30C
   20             // 32%
   3C             // 60C
   39             // 57%

   // Global Stepwise Curve Record
   5D             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   1E             // 30C
   33             // 51%
   3C             // 60C
   4C             // 76%

   // Global Stepwise Curve Record
   5E             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   1E             // 30C
   19             // 25%
   3C             // 60C
   4B             // 75%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0023

   // Sensor Record Header
   00E5           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   // Global Stepwise Curve Record
   5F             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   1E             // 30C
   20             // 32%
   3C             // 60C
   52             // 82%

   // Global Stepwise Curve Record
   60             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   1E             // 30C
   33             // 51%
   3C             // 60C
   64             // 100%

    // Global Stepwise Curve Record
   61             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   1E             // 30C
   33             // 51%
   3C             // 60C
   64             // 100%

   // Global Stepwise Curve Record
   62             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   1E             // 30C
   20             // 32%
   3C             // 60C
   64             // 100%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0011

   // Sensor Record Header
   00E6           // Record ID
   51             // SDR Version
   C0             // Record Type
   0C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   63             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   1E             // 30C
   33             // 51%
   3C             // 60C
   64             // 100%
   
//====================================================================//
// Maximum Stepwise Linear Tables
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_SAS'
_SDR_TAG    'R1000_NOSAS'
_REC_LEN    0023

   // Sensor Record Header
   00E7           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   08             // Stepwise Curve ID
   85             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   0F             // 15C
   64             // 100%
   1C             // 28C
   64             // 100%
   24             // 36C
   64             // 100%
   26             // 38C
   64             // 100%
   32             // 50C
   64             // 100%
   

   // Global Stepwise Curve Record
   09             // Stepwise Curve ID
   85             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   0F             // 15C
   64             // 100%
   1C             // 28C
   64             // 100%
   24             // 36C
   64             // 100%
   26             // 38C
   64             // 100%
   32             // 50C
   64             // 100%

_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXSAS'
_SDR_TAG    'UPS_4FIXNOSAS'
_SDR_TAG    'UPS_4SAS'
_SDR_TAG    'UPS_4NOSAS'
_SDR_TAG    'UPS_8X35SAS'
_SDR_TAG    'UPS_8X35NOSAS'
_REC_LEN    0017

   // Sensor Record Header
   F0E7           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   2A             // Stepwise Curve ID
   85             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   13             // 19C
   64             // 100%
   1D             // 29C
   64             // 100%
   27             // 39C
   64             // 100%
   2C             // 44C
   64             // 100%
   31             // 49C
   64             // 100%

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0011

   // Sensor Record Header
   F2E7           // Record ID
   51             // SDR Version
   C0             // Record Type
   0C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   64             // Stepwise Curve ID
   82             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count 
   1E             // 30C
   64             // 100%
   3C             // 60C
   64             // 100%

//====================================================================//
//
// FSC Record Type = 03h (Fan Sensor Domain Map Record)
//
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_SAS'
_SDR_TAG    'R1000_NOSAS'
_REC_LEN    0013

   // Sensor Record Header
   00E9           // Record ID
   51             // SDR Version
   C0             // Record Type
   0E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   03             // FSC Record Type (03h = Fan Sensor Domain Map)

   // Domain Fan Configuration
   01             // [7:4]-Domain Number = 0; [3:0]-Count of sensor numbers = 1
   31             // Fan Sensor Number 2 (31h = System Fan 2)
   21             // [7:4]-Domain Number = 2; [3:0]-Count of sensor numbers = 1
   30             // Fan Sensor Number 1 (30h = System Fan 1)
   31             // [7:4]-Domain Number = 3; [3:0]-Count of sensor numbers = 1
   32             // Fan Sensor Number 3 (32h = System Fan 3)
   61             // [7:4]-Domain Number = 3; [3:0]-Count of sensor numbers = 2
   A0             // Fan Sensor Number 2 (A0h = PS1 Fan Fail) 

//====================================================================//
//
// FSC Record Type = 03h (Fan Sensor Domain Map Record)
//
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXSAS'
_SDR_TAG    'UPS_4FIXNOSAS'
_SDR_TAG    'UPS_4SAS'
_SDR_TAG    'UPS_4NOSAS'
_REC_LEN    000F

   // Sensor Record Header
   00EA           // Record ID
   51             // SDR Version
   C0             // Record Type
   0A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   03             // FSC Record Type (03h = Fan Sensor Domain Map)

   // Domain Fan Configuration
   01             // [7:4]-Domain Number = 0; [3:0]-Count of sensor numbers = 1
   36             // Fan Sensor Number 7 (36h = Processor 1 Fan)
   11             // [7:4]-Domain Number = 1; [3:0]-Count of sensor numbers = 1
   33             // Fan Sensor Number 4 (33h = System Fan 4)

//====================================================================//
//
// FSC Record Type = 03h (Fan Sensor Domain Map Record)
//
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35SAS'
_SDR_TAG    'UPS_8X35NOSAS'
_REC_LEN    0014

   // Sensor Record Header
   F2EA           // Record ID
   51             // SDR Version
   C0             // Record Type
   0F             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   03             // FSC Record Type (03h = Fan Sensor Domain Map)

   01             // [7:4]-Domain Number = 0; [3:0]-Count of sensor numbers = 1
   36             // Fan Sensor Number 7 (36h = Processor 1 Fan)
   11             // [7:4]-Domain Number = 1; [3:0]-Count of sensor numbers = 1   
   33             // Fan Sensor Number 4 (33h = System Fan 4) 
   21             // [7:4]-Domain Number = 2; [3:0]-Count of sensor numbers = 1
   30             // Fan Sensor Number 1 (30h = System Fan 1)
   62             // [7:4]-Domain Number = 3; [3:0]-Count of sensor numbers = 2
   A0             // Fan Sensor Number 1 (A0h = PS1 Fan Fail)  
   A4             // Fan Sensor Number 2 (A4h = PS2 Fan Fail)

//====================================================================//
//
// FSC Record Type = 03h (Fan Sensor Domain Map Record)
//
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0014

   // Sensor Record Header
   00EB           // Record ID
   51             // SDR Version
   C0             // Record Type
   0F             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   03             // FSC Record Type (03h = Fan Sensor Domain Map)

   // Domain Fan Configuration
   02             // [7:4]-Domain Number = 0; [3:0]-Count of sensor numbers = 2
   30             // Fan Sensor Number 1 (30h = System Fan 1) 
   36             // Fan Sensor Number 7 (36h = Processor 1 Fan)
   11             // [7:4]-Domain Number = 1; [3:0]-Count of sensor numbers = 2
   33             // Fan Sensor Number 4 (33h = System Fan 4)
   21             // [7:4]-Domain Number = 2; [3:0]-Count of sensor numbers = 1
   31             // Fan Sensor Number 2 (31h = System Fan 2)
   31             // [7:4]-Domain Number = 3; [3:0]-Count of sensor numbers = 1
   32             // Fan Sensor Number 3 (32h = System Fan 3)

//====================================================================//
// Domain 0
//====================================================================//
//====================================================================//
// Domain 0
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_SAS'
_REC_LEN    001C

   // Sensor Record Header
   00EC           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   FF             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   00             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_SAS'
_REC_LEN    001C

   // Sensor Record Header
   00ED           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   F0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   FF             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   01             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
// Domain 0
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_SAS'
_REC_LEN    001F

   // Sensor Record Header
   00F2           // Record ID
   51             // SDR Version
   C0             // Record Type
   1A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   63             // Clamp ID
//====================================================================//
// Domain 0
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 05h (Fans Off)
//====================================================================//

//====================================================================//
// Domain 0
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_NOSAS'
_REC_LEN    001C

   // Sensor Record Header
   00F3           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   FF             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   04             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_NOSAS'
_REC_LEN    001C

   // Sensor Record Header
   00F4           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   F0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   FF             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   05             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
// Domain 0
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_NOSAS'
_REC_LEN    001D

   // Sensor Record Header
   00F9           // Record ID
   51             // SDR Version
   C0             // Record Type
   18             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   63             // Clamp ID
//====================================================================//
// Domain 0
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXSAS'
_REC_LEN    001C

   // Sensor Record Header
   00FA           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0E             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXSAS'
_REC_LEN    001C

   // Sensor Record Header
   00FB           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   F0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0F             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
// Domain 0
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXSAS'
_REC_LEN    001B

   // Sensor Record Header
   00FC           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   63             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID

//====================================================================//
// Domain 0
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXNOSAS'
_REC_LEN    001C

   // Sensor Record Header
   00FD           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   12             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXNOSAS'
_REC_LEN    001C

   // Sensor Record Header
   00FE           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   F0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   13             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
// Domain 0
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXNOSAS'
_REC_LEN    001B

   // Sensor Record Header
   00FF           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   63             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID

//====================================================================//
// Domain 0
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4SAS'
_REC_LEN    001C

   // Sensor Record Header
   0F01           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   16             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4SAS'
_REC_LEN    001C

   // Sensor Record Header
   0F02           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   F0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   17             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
// Domain 0
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4SAS'
_REC_LEN    001D

   // Sensor Record Header
   0F03           // Record ID
   51             // SDR Version
   C0             // Record Type
   18             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   63             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID
//====================================================================//
// Domain 0
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4NOSAS'
_REC_LEN    001C

   // Sensor Record Header
   0F04           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   1A             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4NOSAS'
_REC_LEN    001C

   // Sensor Record Header
   0F05           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   F0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   1B             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
// Domain 0
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4NOSAS'
_REC_LEN    001D

   // Sensor Record Header
   0F06           // Record ID
   51             // SDR Version
   C0             // Record Type
   18            // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   63             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID
//====================================================================//
// Domain 0
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35SAS'
_REC_LEN    001C

   // Sensor Record Header
   0F08           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   1E             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35SAS'
_REC_LEN    001C

   // Sensor Record Header
   0F09           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   F0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   1F             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
// Domain 0
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35SAS'
_REC_LEN    0021

   // Sensor Record Header
   0F0A           // Record ID
   51             // SDR Version
   C0             // Record Type
   1C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   53             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID

//====================================================================//
// Domain 0
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35NOSAS'
_REC_LEN    001C

   // Sensor Record Header
   0F0B           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   24             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35NOSAS'
_REC_LEN    001C

   // Sensor Record Header
   0F0C           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   F0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   25             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
// Domain 0
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35NOSAS'
_REC_LEN    0021

   // Sensor Record Header
   0F0D           // Record ID
   51             // SDR Version
   C0             // Record Type
   1C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   53             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID

//====================================================================//
// Domain 1
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXSAS'
_REC_LEN    001C

   // Sensor Record Header
   0F0E           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   16             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   10             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXSAS'
_REC_LEN    001C

   // Sensor Record Header
   0F0F           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   F0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   16             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
// Domain 1
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXSAS'
_REC_LEN    0019

   // Sensor Record Header
   0F10           // Record ID
   51             // SDR Version
   C0             // Record Type
   14             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   93             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID

//====================================================================//
// Domain 1
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 05h (Fans Off)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXSAS'
_REC_LEN    0012

   // Sensor Record Header
   0F11           // Record ID
   51             // SDR Version
   C0             // Record Type
   0D             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support
   
   // Fans Off Sub-Record
   05             // FSC Sub-Record Type (05h = Fans Off)
   C8             // Sensor Number Controlling Operation (C8h = Agg Thrm Mgn 2)
   EC             // Fans Off Control Value (ECh = -20 Degrees)
   0A             // Hysteresis (0Ah = 10)
   16             // Fans Off PWM (16h = 22%)

//====================================================================//
// Domain 1
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXNOSAS'
_REC_LEN    001C

   // Sensor Record Header
   0F12           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   05             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   16             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   14             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXNOSAS'
_REC_LEN    001C

   // Sensor Record Header
   0F13           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   50             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   16             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   15             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXNOSAS'
_REC_LEN    001C

   // Sensor Record Header
   AF13           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   0A             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   16             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2C             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXNOSAS'
_REC_LEN    001C

   // Sensor Record Header
   AF14           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   A0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   16             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2D             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
// Domain 1
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXNOSAS'
_REC_LEN    0019

   // Sensor Record Header
   0F14           // Record ID
   51             // SDR Version
   C0             // Record Type
   14             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   93             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID

//====================================================================//
// Domain 1
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 05h (Fans Off)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXNOSAS'
_REC_LEN    0012

   // Sensor Record Header
   0F15           // Record ID
   51             // SDR Version
   C0             // Record Type
   0D             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support
   
   // Fans Off Sub-Record
   05             // FSC Sub-Record Type (05h = Fans Off)
   C8             // Sensor Number Controlling Operation (C8h = Agg Thrm Mgn 2)
   EC             // Fans Off Control Value (ECh = -20 Degrees)
   0A             // Hysteresis (0Ah = 10)
   16             // Fans Off PWM (16h = 22%)

//====================================================================//
// Domain 1
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4SAS'
_REC_LEN    001C

   // Sensor Record Header
   0F16           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   16             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   18             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4SAS'
_REC_LEN    001C

   // Sensor Record Header
   0F17           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   F0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   16             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   19             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
// Domain 1
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4SAS'
_REC_LEN    001B

   // Sensor Record Header
   0F18           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   93             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID
//====================================================================//
// Domain 1
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 05h (Fans Off)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4SAS'
_REC_LEN    0012

   // Sensor Record Header
   0F19           // Record ID
   51             // SDR Version
   C0             // Record Type
   0D             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support
   
   // Fans Off Sub-Record
   05             // FSC Sub-Record Type (05h = Fans Off)
   C8             // Sensor Number Controlling Operation (C8h = Agg Thrm Mgn 2)
   EC             // Fans Off Control Value (ECh = -20 Degrees)
   0A             // Hysteresis (0Ah = 10)
   16             // Fans Off PWM (16h = 22%)

//====================================================================//
// Domain 1
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4NOSAS'
_REC_LEN    001C

   // Sensor Record Header
   0F1A           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   16             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   1C             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4NOSAS'
_REC_LEN    001C

   // Sensor Record Header
   0F1B           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   F0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   16             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   1D             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
// Domain 1
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4NOSAS'
_REC_LEN    001B

   // Sensor Record Header
   0F1C           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   93             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID
//====================================================================//
// Domain 1
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 05h (Fans Off)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4NOSAS'
_REC_LEN    0012

   // Sensor Record Header
   0F1D           // Record ID
   51             // SDR Version
   C0             // Record Type
   0D             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support
   
   // Fans Off Sub-Record
   05             // FSC Sub-Record Type (05h = Fans Off)
   C8             // Sensor Number Controlling Operation (C8h = Agg Thrm Mgn 2)
   EC             // Fans Off Control Value (ECh = -20 Degrees)
   0A             // Hysteresis (0Ah = 10)
   16             // Fans Off PWM (16h = 22%)

//====================================================================//
// Domain 1
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35SAS'
_REC_LEN    001C

   // Sensor Record Header
   FF08           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   16             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   1E             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35SAS'
_REC_LEN    001C

   // Sensor Record Header
   FF09           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   F0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   16             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   1F             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
// Domain 1
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35SAS'
_REC_LEN    001F

   // Sensor Record Header
   FF0A           // Record ID
   51             // SDR Version
   C0             // Record Type
   1A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   93             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID

//====================================================================//
// Domain 1
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35NOSAS'
_REC_LEN    001C

   // Sensor Record Header
   FF0B           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   16             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   24             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35NOSAS'
_REC_LEN    001C

   // Sensor Record Header
   FF0C           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   F0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   16             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   25             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
// Domain 1
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35NOSAS'
_REC_LEN    001F

   // Sensor Record Header
   FF0D           // Record ID
   51             // SDR Version
   C0             // Record Type
   1A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   93             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID

//====================================================================//
// Domain 1
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 05h (Fans Off)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35NOSAS'
_SDR_TAG    'UPS_8X35SAS'
_REC_LEN    0012

   // Sensor Record Header
   DF23           // Record ID
   51             // SDR Version
   C0             // Record Type
   0D             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support
   
   // Fans Off Sub-Record
   05             // FSC Sub-Record Type (05h = Fans Off)
   C8             // Sensor Number Controlling Operation (C8h = Agg Thrm Mgn 2)
   EC             // Fans Off Control Value (ECh = -20 Degrees)
   0A             // Hysteresis (0Ah = 10)
   16             // Fans Off PWM (16h = 22%)

//====================================================================//
// Domain 2
//====================================================================//
//====================================================================//
// Domain 2
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_SAS'
_REC_LEN    001C

   // Sensor Record Header
   0F24           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   FF             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   02             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   09             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_SAS'
_REC_LEN    001C

   // Sensor Record Header
   0F25           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   F0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   FF             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   03             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   09             // Stepwise Curve ID

//====================================================================//
// Domain 2
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_SAS'
_REC_LEN    0019

   // Sensor Record Header
   0F28           // Record ID
   51             // SDR Version
   C0             // Record Type
   14             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   63             // Clamp ID

//====================================================================//
// Domain 2
//====================================================================//
//====================================================================//
// Domain 2
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_NOSAS'
_REC_LEN    001C

   // Sensor Record Header
   0F29           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   FF             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   06             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   09             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_NOSAS'
_REC_LEN    001C

   // Sensor Record Header
   0F2A           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   F0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   FF             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   07             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   09             // Stepwise Curve ID

//====================================================================//
// Domain 2
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_NOSAS'
_REC_LEN    0019

   // Sensor Record Header
   0F2D           // Record ID
   51             // SDR Version
   C0             // Record Type
   14             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   63             // Clamp ID
//====================================================================//
// Domain 2
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35SAS'
_REC_LEN    001C

   // Sensor Record Header
   DD1E           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   05             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   0A             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   20             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35SAS'
_REC_LEN    001C

   // Sensor Record Header
   DD1F           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   50             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   0A             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   21             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
// Domain 2
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35SAS'
_REC_LEN    001C

   // Sensor Record Header
   DF20           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   0A             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   0A             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   22             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35SAS'
_REC_LEN    001C

   // Sensor Record Header
   DF21           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   A0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   0A             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   23             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
// Domain 2
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35SAS'
_REC_LEN    001D

   // Sensor Record Header
   DF22           // Record ID
   51             // SDR Version
   C0             // Record Type
   18             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID

//====================================================================//
// Domain 2
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35NOSAS'
_REC_LEN    001C

   // Sensor Record Header
   DF1E           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   05             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   0A             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   26             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35NOSAS'
_REC_LEN    001C

   // Sensor Record Header
   DF1F           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   50             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   0A             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   27             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
// Domain 2
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35NOSAS'
_REC_LEN    001C

   // Sensor Record Header
   DF2A           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   0A             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   0A             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   28             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35NOSAS'
_REC_LEN    001C

   // Sensor Record Header
   DF2B           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   A0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   0A             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   29             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
// Domain 2
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35NOSAS'
_REC_LEN    001D

   // Sensor Record Header
   DF2C           // Record ID
   51             // SDR Version
   C0             // Record Type
   18             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID

//====================================================================//
// Domain 2
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 05h (Fans Off)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35NOSAS'
_SDR_TAG    'UPS_8X35SAS'
_REC_LEN    0012

   // Sensor Record Header
   DF2D           // Record ID
   51             // SDR Version
   C0             // Record Type
   0D             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   FF             // Fan Profile Support
   
   // Fans Off Sub-Record
   05             // FSC Sub-Record Type (05h = Fans Off)
   CA             // Sensor Number Controlling Operation (CAh = Agg Thrm Mgn 2)
   EC             // Fans Off Control Value (ECh = -20 Degrees)
   0A             // Hysteresis (0Ah = 10)
   0A             // Fans Off PWM (0Ah = 10%)

//====================================================================//
// Domain 3
//====================================================================//
//====================================================================//
// Domain 3
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_SAS'
_REC_LEN    001C

   // Sensor Record Header
   0F2E           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   FF             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   00             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_SAS'
_REC_LEN    001C

   // Sensor Record Header
   0F2F           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   F0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   FF             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   01             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
// Domain 3
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_SAS'
_REC_LEN    001F

   // Sensor Record Header
   0F32           // Record ID
   51             // SDR Version
   C0             // Record Type
   1A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   63             // Clamp ID
//====================================================================//
// Domain 3
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_NOSAS'
_REC_LEN    001C

   // Sensor Record Header
   0F34           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   FF             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   04             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_NOSAS'
_REC_LEN    001C

   // Sensor Record Header
   0F35           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   F0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   FF             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   05             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
// Domain 3
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_NOSAS'
_REC_LEN    001D

   // Sensor Record Header
   0F38           // Record ID
   51             // SDR Version
   C0             // Record Type
   18             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   63             // Clamp ID

//====================================================================//
// Domain PS
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 05h (Fans Off)
//====================================================================//


//====================================================================//
// Domain PS
// FSC Record Type = 18h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_SAS'
_SDR_TAG    'R1000_NOSAS'
_REC_LEN    001C

   // Sensor Record Header
   0F39           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   18             // FSC Record Type (08h = Main Domain)
   40             // Domain Mask
   FF             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   FF             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   02             // Stepwise Header ID
   37             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//====================================================================//
// Domain PS
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_SAS'
_SDR_TAG    'R1000_NOSAS'
_REC_LEN    0015

   // Sensor Record Header
   0F3A           // Record ID
   51             // SDR Version
   C0             // Record Type
   10             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   18             // FSC Record Type (08h = Main Domain)
   40             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID

//====================================================================//
// Domain PS
// FSC Record Type = 18h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35SAS'
_SDR_TAG    'UPS_8X35NOSAS'
_REC_LEN    001C

   // Sensor Record Header
   0F3D           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   18             // FSC Record Type (08h = Main Domain)
   40             // Domain Mask
   FF             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   0A             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   02             // Stepwise Header ID
   37             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   2A             // Stepwise Curve ID

//====================================================================//
// Domain PS
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35SAS'
_SDR_TAG    'UPS_8X35NOSAS'
_REC_LEN    0013

   // Sensor Record Header
   0F3E           // Record ID
   51             // SDR Version
   C0             // Record Type
   0E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   18             // FSC Record Type (08h = Main Domain)
   40             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   93             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID

//====================================================================//
// FCT/SHIP/FCT2
//====================================================================//
//====================================================================//
// Domain All
// FSC Record Type = 08h (Fan Sensor Domain Map Record)
// FSC Sub-record Type = 01h (Domain Configuration)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'SHIP'
_SDR_TAG    'FCT'
_SDR_TAG    'FCT2'
_REC_LEN    0015

   // Sensor Record Header
   0128           // Record ID
   51             // SDR Version
   C0             // Record Type
   10             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask
   FF             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   64             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost   

   // Clamp Sub-Record

//====================================================================//
// OTHER Chassis
//====================================================================//
//====================================================================//
// FSC Record Type = 08h (Fan Sensor Domain Map Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_REC_LEN    001B

   // Sensor Record Header
   0129           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost
                  
   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5B             // Stepwise Curve ID

   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_REC_LEN    001B

   // Sensor Record Header
   012A           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask
   30             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost
                  
   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5C             // Stepwise Curve ID

   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_REC_LEN    001B

   // Sensor Record Header
   012B           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask
   C0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost
                  
   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5D             // Stepwise Curve ID

   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_MR'
_REC_LEN    001B

   // Sensor Record Header
   012C           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost
                  
   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5E             // Stepwise Curve ID

   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_MR'
_REC_LEN    001B

   // Sensor Record Header
   012D           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask
   30             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost
                  
   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5F             // Stepwise Curve ID

   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_MR'
_REC_LEN    001B

   // Sensor Record Header
   012E           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask
   C0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost
                  
   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   60             // Stepwise Curve ID

   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID
   
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_FR'
_REC_LEN    001B

   // Sensor Record Header
   012F           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost
                  
   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   61             // Stepwise Curve ID

   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_FR'
_REC_LEN    001B

   // Sensor Record Header
   0130           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask
   30             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost
                  
   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   62             // Stepwise Curve ID

   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_FR'
_REC_LEN    001B

   // Sensor Record Header
   0131           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask
   C0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost
                  
   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   63             // Stepwise Curve ID

   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID

//====================================================================//
// Domain 0
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_SDR_TAG    'OTHER_MR'
_SDR_TAG    'OTHER_FR'
_REC_LEN    001F

   // Sensor Record Header
   0132           // Record ID
   51             // SDR Version
   C0             // Record Type
   1A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support
   
   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID

//====================================================================//
// Domain 1
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_SDR_TAG    'OTHER_MR'
_SDR_TAG    'OTHER_FR'
_REC_LEN    001F

   // Sensor Record Header
   0133           // Record ID
   51             // SDR Version
   C0             // Record Type
   1A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support
   
   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID

//====================================================================//
// Domain 2
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_SDR_TAG    'OTHER_MR'
_SDR_TAG    'OTHER_FR'
_REC_LEN    001F

   // Sensor Record Header
   0134           // Record ID
   51             // SDR Version
   C0             // Record Type
   1A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   FF             // Fan Profile Support
   
   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID

//====================================================================//
// Domain 3
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_SDR_TAG    'OTHER_MR'
_SDR_TAG    'OTHER_FR'
_REC_LEN    001F

   // Sensor Record Header
   0135           // Record ID
   51             // SDR Version
   C0             // Record Type
   1A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   FF             // Fan Profile Support
   
   // Clamp Sub-Record
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID
   
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID

   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID

//====================================================================//
//
// FSC Record Type = 11h (System Airflow Formula)
//
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R1000_SAS'
_SDR_TAG    'R1000_NOSAS'
_REC_LEN    0024


   //Sensor Record Header
   013F               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1F                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   11                 // Record sub-type (11h = System air flow)
   
   01                 // Domain mask (Domains 0)
   7700               // Correction Factor 1 
   4700               // Correction Factor 2 
   14                 // PWM for Correction Factor 1 
   64                 // PWM for Correction Factor 2 (64h = 100%)
   1E                 // Max CFM of Fan 
   01                 // Quantity of fans in this equation
   
   04                 // Domain mask (Domains 2)
   7700               // Correction Factor 1 
   4700               // Correction Factor 2 
   14                 // PWM for Correction Factor 1 
   64                 // PWM for Correction Factor 2 (64h = 100%)
   18                 // Max CFM of Fan 
   01                 // Quantity of fans in this equation

   08                 // Domain mask (Domains 2)
   7700               // Correction Factor 1 
   4700               // Correction Factor 2 
   14                 // PWM for Correction Factor 1 
   64                 // PWM for Correction Factor 2 (64h = 100%)
   1E                 // Max CFM of Fan 
   01                 // Quantity of fans in this equation

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXSAS'
_SDR_TAG    'UPS_4FIXNOSAS'
_SDR_TAG    'UPS_4SAS'
_SDR_TAG    'UPS_4NOSAS'
_REC_LEN    0012


   //Sensor Record Header
   0140               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0D                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   11                 // Record sub-type (11h = System air flow)
   
   03                 // Domain mask (Domains 0)
   2D00               // Correction Factor 1 
   3200               // Correction Factor 2 
   16                 // PWM for Correction Factor 1 
   64                 // PWM for Correction Factor 2 (64h = 100%)
   82                 // Max CFM of Fan 
   01                 // Quantity of fans in this equation

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35SAS'
_SDR_TAG    'UPS_8X35NOSAS'
_REC_LEN    0012


   //Sensor Record Header
   A140               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0D                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   11                 // Record sub-type (11h = System air flow)
   
   07                 // Domain mask (Domains 0)
   2D00               // Correction Factor 1 
   3200               // Correction Factor 2 
   16                 // PWM for Correction Factor 1 
   64                 // PWM for Correction Factor 2 (64h = 100%)
   82                 // Max CFM of Fan 
   01                 // Quantity of fans in this equation

//====================================================================//
//
// FSC Record Type = 12h (Aggregate Sensor Configuration Record)
//
//====================================================================//
//=========================================================
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXSAS'
_SDR_TAG    'UPS_4SAS'
_REC_LEN    0017

   //Sensor Record Header
   0142               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   12                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   12                 // Record Subtype (12h = Aggregate Sensor Configuration)
   C8                 // Aggregate sensor number 
   06                 // Number of input pairs to follow
   74                 // Input 1 sensor number 
   00                 // Input 1 margin reference value 
   B0                 // Input 2 sensor number 
   00                 // Input 2 margin reference value 
   22                 // Input 3 sensor number 
   50                 // Input 3 margin reference value 
   2D                 // Input 4 sensor number 
   5F                 // Input 4 margin reference value 
   23                 // Input 5 sensor number 
   1E                 // Input 5 margin reference value 
   2E                 // Input 6 sensor number 
   2D                 // Input 6 margin reference value 

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_4FIXNOSAS'
_SDR_TAG    'UPS_4NOSAS'
_REC_LEN    0017

   //Sensor Record Header
   0143               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   12                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   12                 // Record Subtype (12h = Aggregate Sensor Configuration)
   C8                 // Aggregate sensor number 
   06                 // Number of input pairs to follow
   74                 // Input 1 sensor number 
   00                 // Input 1 margin reference value 
   B0                 // Input 2 sensor number 
   00                 // Input 2 margin reference value 
   22                 // Input 3 sensor number 
   50                 // Input 3 margin reference value 
   24                 // Input 4 sensor number 
   5F                 // Input 4 margin reference value 
   23                 // Input 5 sensor number 
   1E                 // Input 5 margin reference value 
   2E                 // Input 6 sensor number 
   2D                 // Input 6 margin reference value

//=========================================================
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35SAS'
_SDR_TAG    'UPS_8X35NOSAS'
_REC_LEN    0019

   //Sensor Record Header
   F142               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   14                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   12                 // Record Subtype (12h = Aggregate Sensor Configuration)
   C8                 // Aggregate sensor number 
   07                 // Number of input pairs to follow
   74                 // Input 1 sensor number 
   00                 // Input 1 margin reference value 
   B0                 // Input 2 sensor number 
   00                 // Input 2 margin reference value 
   24                 // Input 3 sensor number 
   1E                 // Input 3 margin reference value 
   2E                 // Input 4 sensor number 
   40                 // Input 4 margin reference value 
   5C                 // Input 5 sensor number 
   2D                 // Input 5 margin reference value 
   5D                 // Input 6 sensor number 
   2D                 // Input 6 margin reference value 
   2E                 // Input 7 sensor number 
   2D                 // Input 7 margin reference value 

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'UPS_8X35SAS'
_SDR_TAG    'UPS_8X35NOSAS'
_REC_LEN    0015

   //Sensor Record Header
   F143               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   10                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   12                 // Record Subtype (12h = Aggregate Sensor Configuration)
   CA                 // Aggregate sensor number 
   05                 // Number of input pairs to follow
   74                 // Input 1 sensor number 
   00                 // Input 1 margin reference value 
   B0                 // Input 2 sensor number 
   00                 // Input 2 margin reference value 
   23                 // Input 3 sensor number 
   1E                 // Input 3 margin reference value 
   22                 // Input 4 sensor number 
   50                 // Input 4 margin reference value 
   2E                 // Input 5 sensor number 
   2D                 // Input 5 margin reference value 

//====================================================================//
// SDR Version Records
//====================================================================//

// SDR Version Record (first letter of 'SDR')
//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0015

   // Sensor Record Header
   014B               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   10                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   'SDR File 1.05'    // String Bytes

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0018

   // Sensor Record Header
   014C               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   13                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   'SDR Package 1.05' // String Bytes
)                     // End of SDR File
