================================================================================
Intel(R) Xeon(R) Processor-Based Server BIOS Development
================================================================================
INTEL Enterprise Products and Services Division
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================
DATE    : November 15, 2013
TO      : Multi-Core Intel(R) Xeon(R) Processor-Based Server Platform customers
SUBJECT : BIOS Release notes for version R01.03.0005
================================================================================
                           LEGAL INFORMATION
================================================================================

INFORMATION IN THIS DOCUMENT IS PROVIDED IN CONNECTION WITH INTEL PRODUCTS. NO 
LICENSE, EXPRESS OR IMPLIED, BY ESTOPPEL OR OTHERWISE, TO ANY INTELLECTUAL 
PROPERTY RIGHTS IS GRANTED BY THIS DOCUMENT. EXCEPT AS PROVIDED IN INTEL'S TERMS 
AND CONDITIONS OF SALE FOR SUCH PRODUCTS, INTEL ASSUMES NO LIABILITY WHATSOEVER 
AND INTEL DISCLAIMS ANY EXPRESS OR IMPLIED WARRANTY, RELATING TO SALE AND/OR USE 
OF INTEL PRODUCTS INCLUDING LIABILITY OR WARRANTIES RELATING TO FITNESS FOR A 
PARTICULAR PURPOSE, MERCHANTABILITY, OR INFRINGEMENT OF ANY PATENT, COPYRIGHT OR 
OTHER INTELLECTUAL PROPERTY RIGHT. 

A "Mission Critical Application" is any application in which failure of the Intel 
Product could result, directly or indirectly, in personal injury or death. SHOULD 
YOU PURCHASE OR USE INTEL'S PRODUCTS FOR ANY SUCH MISSION CRITICAL APPLICATION, 
YOU SHALL INDEMNIFY AND HOLD INTEL AND ITS SUBSIDIARIES, SUBCONTRACTORS AND 
AFFILIATES, AND THE DIRECTORS, OFFICERS, AND EMPLOYEES OF EACH, HARMLESS AGAINST 
ALL CLAIMS COSTS, DAMAGES, AND EXPENSES AND REASONABLE ATTORNEYS' FEES ARISING OUT 
OF, DIRECTLY OR INDIRECTLY, ANY CLAIM OF PRODUCT LIABILITY, PERSONAL INJURY, OR 
DEATH ARISING IN ANY WAY OUT OF SUCH MISSION CRITICAL APPLICATION, WHETHER OR NOT 
INTEL OR ITS SUBCONTRACTOR WAS NEGLIGENT IN THE DESIGN, MANUFACTURE, OR WARNING OF 
THE INTEL PRODUCT OR ANY OF ITS PARTS. 

Intel may make changes to specifications and product descriptions at any time, 
without notice. Designers must not rely on the absence or characteristics of any 
features or instructions marked "reserved" or "undefined". Intel reserves these for 
future definition and shall have no responsibility whatsoever for conflicts or 
incompatibilities arising from future changes to them. The information here is 
subject to change without notice. Do not finalize a design with this information. 

The products described in this document may contain design defects or errors known 
as errata which may cause the product to deviate from published specifications. 
Current characterized errata are available on request. 

Contact your local Intel sales office or your distributor to obtain the latest 
specifications and before placing your product order. 

Copies of documents which have an order number and are referenced in this document, 
or other Intel literature, may be obtained by calling 1-800-548-4725, 
or go to: http://www.intel.com/design/literature.htm

Intel is a registered trademark of Intel Corporation. 

*Other names and brands are the property of their respective owners.

Copyright (C) 2013 Intel Corporation.

================================================================================
                              ABOUT THIS RELEASE
================================================================================
Build Version : S1200RP.86B.01.03.0005
Build Dater   : November 21, 2013

================================================================================
                           BIOS COMPONENTS/CONTENTS
================================================================================
Processors supported: 
Intel(R) Xeon processor E3-1200 V3 series

Microcode update versions:
Intel(R) Xeon processor E3-1200 V3 series A0 stepping: 0xffff0014  CPUID = 0x306C1   
Intel(R) Xeon processor E3-1200 V3 series B0 stepping: 0xffff0006  CPUID = 0x306C2   
Intel(R) Xeon processor E3-1200 V3 series C0 stepping: 0x00000009  CPUID = 0x306C3   

On-Board Component Option ROM Versions:
Integrated Matrox VGA               : VBE BIOS V3.8 SQ
PXE Option ROM                      : Intel(R) Boot Agent XE v1.4.10
iSCSI Option ROM                    : Intel(R) iSCSI Remote Boot version 2.7.137
SATA RAID Option ROM - RSTe         : 3.7
UEFI SATA RAID Option ROM - RSTe    : 3.7
ESRT II FOR SATA                    : A.11.11191606
Legacy Processor Video              : 2170 
UEFI Processor Video driver         : 5.2.1002 

Memory Reference Code Version       : 1.5.0.1
Management Engine Firmware Version  : 3.0.4.209

================================================================================
                       SYSTEM FIRMWARE REQUIREMENTS
================================================================================
BIOS Update Utility: 
  UEFI iFlash32 V12.0 build06 or later.
  
  Product   Fab Version	  BMC	   FRUSDR    
S1200V3RPL  G62251-302	  1.03	     1.03
S1200V3RPS  G62252-302    1.03	     1.03
	    G62252-305    1.03	     1.03
S1200V3RPO  G62253-302    1.03	     1.03
	    G62253-305    1.03	     1.03
S1200V3RPM  G62254-302    1.03	     1.03

================================================================================
                           INSTALLATION NOTES
================================================================================

WARNING:  It is very important to follow these instructions as they are written.
Failure to update using the proper procedure may cause damage to your system.

UEFI iFlash32 
   1.  Boot the system to EFI Shell
   2.  Copy IFlash32.efi and BIOS.CAP file to a USB Flash Drive
       ( Do not use the *Rec.CAP file as it will clear the NVRAM and should
         only be used for Recovery - See Recovery Instructions below )
   3.  Map the respective storage device in the system with the command
	   Shell> map -r
   4.  Change the Shell to mapped device file system
	   Example: Shell> fs0: (or fs1:)
   5.  Run the IFlash32 utility at the prompt
	   fs0:\> IFlash32 [File Name] /u /ni
   6. Either reboot the system and
      6a. Go into BIOS setup <F2>, reset defaults <F9> and save <f10> or
      6b. After the BIOS update and before rebooting, run: fS0:> Iflash32 -rd
   7.  Reboot system.

================================================================================
                        BIOS RECOVERY INSTRUCTIONS
================================================================================

The Recovery process can be initiated by setting the recovery jumper. (called 
BIOS Recovery Boot Jumper)
 
A BIOS recovery can be accomplished from the backup BIOS region or USB Mass Storage device. 
Please note that recovery from USB floppy is not supported on this platform. 
 
The recovery media must contain the following files under the root directory:
   1.  DNL.ROM (optional)
   2.  UEFI iFlash32 (including IFlash32.efi and ipmi.efi )
   3.  *Rec.CAP
   4.  Startup.nsh (update accordingly to use proper *Rec.CAP file)
 
BIOS starts the recovery process by first loading and booting to the recovery image from the 
backup BIOS region or file (DNL.ROM) on the root directory of the recovery media (USB disk).

This process takes place before any video or console is available. Once the system boots 
to recovery image, it will boot automatically into EFI Shell to invoke the Startup.nsh 
script and start the flash update application (IFlash32.efi). IFlash32.efi requires the 
supporting BIOS Capsule image file (*Rec.CAP). After the update is complete, there will 
be a message displayed stating that the "BIOS has been updated successfully" indicating 
the recovery process is finished. The User should then switch the recovery jumper back to
normal operation and restart the system by performing a power cycle.
 
The following steps demonstrate this recovery process:
   1.  Power OFF the system.
   2.  Insert recovery media.(Optional if the backup BIOS region works)
   3.  Switch the recovery jumper. Details regarding the jumper ID and location
       can be obtained from the Product Board TPS.
   4.  Power ON the system.
   5.  The BIOS POST screen will appear displaying the progress and system automatically 
       boots to the EFI SHELL.
   6.  Startup.nsh file executes, and initiates the flash update (IFlash32.efi)
       with new capsule file (*Rec.CAP). The regular IFlash message will be displayed at
       the end of the process, once the flash update succeeds.
   7.  Power OFF the system, and revert the recovery jumper position to "normal".
   8.  Power ON the system. 
   9.  Do *NOT* interrupt the BIOS POST during the first boot.


================================================================================
                            KNOWN ISSUES/WORKAROUNDS
================================================================================
- If you want to install Linux* SUSE* 11 SP2 or boot to a pre-installed Linux* SUSE* 11 
  SP2 OS, USB 3.0 support will need to be disabled in BIOS setup -> USB Configuration tab. 

================================================================================
                                R01.03.0005
================================================================================
- Fixed: PCIe device lost issue on slot4.

================================================================================
                                R01.03.0004
================================================================================
- Fixed: System can't boot into an OS or UEFI using Intel(R) Pentium(R) processors.
- Fixed: Red Hat* Linux* RHEL 6.4 32bit cannot be installed with 1GB DIMMs installed.
- Fixed: Corrected help text for "USB 3.0 support".
- Fixed: RAID mode incorrectly listed as "RST" - changed to "RSTe".
- Fixed: "9266" error is reported with certain add-in video adapters.

Other:
Added:	 TXT ACM V1.3 integration.
Updated: Video BIOS updated to version 2170

================================================================================
                                R01.02.0004
================================================================================
- Fixed: Signed driver check test fails due to an unknown device found in Windows 2012 WHQL
         (Windows Hardware Quality Labs) certification.

================================================================================
                                R01.02.0002
================================================================================
- Fixed: Memory DIMM will sometimes starts throttling, even in good thermal conditions.
- Fixed: System can't wake up from S3 via power button/USB device/Lan.
- Fixed: System power consumption cannot be limited by Node Manager.
- Fixed: BIOS version is not be updated accordingly in server management remote console.

Other:
 - Updated RSTe UEFI/Legacy OPROM to 3.7
    
================================================================================
                                R01.01.0006
================================================================================
- First production BIOS release.
 

[END OF RELEASE NOTES]
