This release note and the software that accompanies it are copyright (c) 2014, Intel Corporation or its suppliers, and may only be installed and used in accordance with the license that accompanies the software.

This Software is furnished under license and may only be used or copied in accordance with the terms of that license. No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. The Software is subject to change without notice, and should not be construed as a commitment by Intel Corporation or its suppliers to market, license, sell or support any product or technology. Unless otherwise provided for in the license under which this Software is provided, the Software is provided AS IS, with no warranties of any kind, express or implied. Except as expressly permitted by the Software license, neither Intel Corporation nor its suppliers assumes any responsibility or liability for any errors or inaccuracies that may appear herein. Except as expressly permitted by the Software license, no part of the Software may be reproduced, stored in a retrieval system, transmitted in any form, or distributed by any means without the express written consent of Intel Corporation.

==========================
Supported RAID Controllers
==========================
This download supports Intel(R) RAID controllers using SAS software stack (RS2WC080, RS2WC040, RMS2AF080 and RMS2AF040), please verify that this utility has been tested with the RAID card you have chosen to use by checking the drivers web page for your controller at http://support.intel.com.

===================
Package Information
===================
Flash package = v20.12.1-0168 (firmware 2.130.394-3028)

==========
Attention!
==========
Intel recommends to loading Factory Default setting after the firmware upgrade which will not affect data on any existing array. To do so:
1. Reboot the system and login to the RAID BIOS Console. 
2. Select the controller and select 'Adapter Properties'->'Next'
3. Set the 'Set Factory Defaults' setting to 'Yes' and submit the change.
4. Reboot the system (the default settings are applied).
5. Re-configure to the desired settings in RAID Web Console2.

==================
Known Restrictions
==================
1) This download does NOT support EFI v1.1 environment. Please use the EFI shell command "ver" to identify the EFI version.
2) When 2 or more VDs are created, VD cache settings must be the same.

=======================
Contents on the package
=======================
The following files are included in this zip:

Name:							Description:
COPYING.NEWLIB.txt					License Agreement
IMR411p.rom						Firmware binary
ir3_2008SASHWR_FWPKG-v20.12.1-0168_readme.txt		This file
License_v2.pdf						License Agreement
update.bat						DOS firmware update batch file
update.nsh						UEFI firmware update batch file
CmdTool2\DOS\*						DOS update utility and support files 
CmdTool2\FreeBSD\*					FreeBSD update utility and support files
CmdTool2\Linux\*					Linux update utility and support files
CmdTool2\Solaris\*					Solaris update utility and support files
CmdTool2\UEFI\*						UEFI update utility and support files
CmdTool2\Windows\*					Windows update utility and support files


==========================
Installation instructions:
==========================
UEFI (EFI 2.0) instructions for updating RAID Firmware:
-----------------
   1. Download and extract all files to a local drive.
   2. Boot the target system to EFI shell. 
   3. Change directory to the local drive and directory containing the flash update files and the firmware image file.
   4. Type "update.nsh" or "efi\cmdtool2 -adpfwflash -f IMR411p.rom -aall"
   5. Wait for the flash to complete. Do NOT reboot the system during the update.

DOS instructions for updating RAID Firmware:
-----------------
   1. Download and extract all files to a local drive.
   2. Boot the target system to DOS. 
   3. Change directory to the local drive and directory containing the flash update files and the firmware image file.
   4. Type "update.bat" or "dos\cmdtool2 -adpfwflash -f IMR411p.rom -aall"
   5. Wait for the flash to complete. Do NOT reboot the system during the update.

Windows and Linux instructions for updating RAID Firmware:
-----------------
The firmware update may be run from Within Windows or Linux using the appropriate versions of CmdTool2.
  In Windows, unzip the utility into the same directory as the rom file by typing 
      "cmdtool2 -adpfwflash -f IMR411p.rom -aall". 
  The Linux CmdTool2 by running the rpm and then calling the utility from /opt/MegaRAID/CmdTool2 as 
      "./CmdTool2 -AdpFwFlash -f IMR411p.rom -aall"

You can also use RAID Web Console 2 to update the RAID firmware. For more detail, please refer to the Intel(r) RAID Software User's Guide.

=============
Package Details/Fixes/Updates  
=============
Package - 20.12.1-0168 (4.11 Patch)
 Firmware 2.130.394-3028
  SCGCQ00426160 - MegaRAID iMR FW with "enableReducedFeatureSet=1" issue
  SCGCQ00475764 - after the newest image is installed, servers often will not boot.
  SCGCQ00475589 - FW sending wrong configuration data during boot msg pending state
  SCGCQ00466496 - Not able to change the properties of MSM.
  SCGCQ00463043 - Upgrading from Software RAID to 9260-8i causes Alarm to sound
  SCGCQ00455655 - Error in MR_DCMD_CTRL_EVENT_COUNT/SL_DIR_READ
  SCGCQ00454839 - MSM log warning: Controller booted in headless mode with errors
  SCGCQ00426916 - Data Corruption with R5 cachedIO mode
  SCGCQ00349837 - Sequential Read performance is less on CacheCade associated LD's.
  SCGCQ00467839 - Montask occurs when running host i/o and parallel OOB command
  SCGCQ00464657 - Generic point release MR4.9 :VPD output of lspci vvxxx showing [RV] Reserved: checksum bad, 86 byte(s) reserved
  SCGCQ00450935 - When pinned cache present VD property not changing from WB to WT.
  SCGCQ00440568 - 9260-8i(SAS2108) hitting OOB SRAT timeout for a long time causing OOB commands to fail
  SCGCQ00584561 - Check-in Pl version 5.0.42.0 -- Improve STP connection timing behavior with idle connections
  SCGCQ00558885 - Checking-in new PL version :05.00.41
  SCGCQ00488348 - To check-in new PL version 5.00.40.00
  SCGCQ00427464 - Discard preserved cache takes excessive time or hangs
  SCGCQ00458860 - Controller always gives an event MR_EVT_CTRL_BOOT_HEADLESS_MODE_HAD_ERRORS if controller is set in HSM mode.
  SCGCQ00457324 - Montask occurs when running host i/o and parallel OOB command
  SCGCQ00455014 - PDs go online without VD created & App doesn't allow any VD creation on passing a wrong parameter in Spanned VD.
  SCGCQ00456152 - To Disable the logging of event MR_EVT_PD_EMERGENCY_SPARE_COMMISSIONED_REMINDER
  SCGCQ00479336 - EEprom CRC error is detected when WebBIOS is running
  SCGCQ00491037 - STP Passthrough Support through OOB
  SCGCQ00471180 - FW is not declaring the battery bad if learn cycles fail continuously
  SCGCQ00467625 - Validate the requested blocks for SCSI VERIFY commands on RAID volumes
  SCGCQ00451971 - see 9261-8i emergency spare being commissioned
  SCGCQ00437904 - Data Miscompare found while running I/O overnight with degraded virtual drives
  SCGCQ00456777 - FW halts when you have pinned cahce and remove VD form the configuration.
  SCGCQ00458859 - FW halts when you have pinned cahce and remove VD form the configuration.
  SCGCQ00462516 - Card Running iMR Machine Checks when Requesting Host Memory
  SCGCQ00478812 - Minimum Capacity needed for relearn is incorrect in 2208 MR FW
  SCGCQ00558100 - Incorrect variable type in MR Read/Modify/Write path
  SCGCQ00558115 - RM_SataBBMTotalCount always return 0
  SCGCQ00558947 - FW Automatically detect backplane SGPIO type to set the driveactivityLED parameter
  SCGCQ00559344 - Setting the ASO key with storcli 1.02.08 (MegaCli 8.07.06) fails with an error code 3 on Windows or Linux if the MB BIOS PCI
  SCGCQ00451982 - Discard preserved cache takes excessive time or hangs
  SCGCQ00433403 - During rebuild on PRL11 CacheCade VD and rebuild on RAID6 Source VD IO integrity error is seen.
  SCGCQ00433391 - IO integrity error seen after Source VD associated with CacheCade VD is forcibly unblocked
  SCGCQ00579790 - LDBBM on RAID6 not eligible
  SCGCQ00458879 - PCIe core has received a PCIe request that it does not support
  SCGCQ00459017 - Firmware returns asc value as 0 when failing IOs with medium errors
  SCGCQ00475895 - Firmware hits Montask when drive is pulled after changing the volume property from read ahead to no read ahead.
  SCGCQ00476387 - Faulty protocol used for changing the Disk Write Cache Policy
  SCGCQ00487207 - BU SOH bad message be posted after exhauting retry attempts. Stop monitoring battery once SOH bad is declared
  SCGCQ00487654 - RHEL6.4 Kernel crash after reboot
  SCGCQ00488061 - Medium error correction event is not logged during CC
  SCGCQ00558908 - Firmware Version 2.130.383-2912 is hitting MonTask at line 1209 in file ../../raid/1078dma.c
  SCGCQ00449634 - Source VD gets blocked on OCR after one PD removal from R0 WB CCVD and reuse of that PD in creating another CCVD.
  SCGCQ00447651 - Data Corruption seen when IOs are in progress and cachecade PD is marked as missing and reused to create another SSC VD.
  SCGCQ00433563 - Sequential Read performance is less on CacheCade associated LD's.
  SCGCQ00433409 - When a Cachecade PD marked as missing is reused to make Cachecade VD IO integrity error is observed.
  SCGCQ00434393 - Saved Release Note DataSLIB returning bad data as good data after host reboots
  SCGCQ00458876 - (Vital Product Data) needs to identify PCB hardware level
  SCGCQ00476060 - Validate the requested blocks for SCSI VERIFY commands on RAID volumes
  SCGCQ00476108 - If a BOOT Passphrase is enabled with SafeStor "MegaCli adpbios dsply a0" will display "BIOS will Stop on error" even if any other mode is set.
  SCGCQ00488447 - Update the events
  SCGCQ00558950 - Firmware is not updating recovery timer as intended
  SCGCQ00484210 - "chip paused" causes high service time on all drives
  SCGCQ00450646 - 9260-8i(SAS2108) hitting OOB SRAT timeout for a long time causing OOB commands to fail
  SCGCQ00583755 - Raid configuration loss after reboot - PDs in POWERSAVE
  SCGCQ00487664 - Code Review: Call DDF_discardInvalidPds only if DS3 is enabled
  SCGCQ00558924 - Upgrading from Software RAID to 9260-8i causes Alarm to sound
  SCGCQ00479291 - system black screen during S1 Sleep test
 NVDATA 3.09.03-0054
 BootBlock 2.02.00.00-0001  
 ROMENV 1.08
 WebBIOS 4.0-60-e_49-Rel
 PCLI 03.02.20
  SCGCQ00477036 - UEFI driver issue with platforms when user having 2TB or 4TB VD
  SCGCQ00484087 - platfrom has UEFI hang when SATA is connected 
  SCGCQ00492562 - Disable Debug print in UEFI Driver
  SCGCQ00492563 - Block IO tests from SCT IHV test suite failed
  SCGCQ00484115 - ATA PT: Follow UEFI Spec on interpreting In and Out Transfer Length that upper layer sends
 UEFI_Driver 0x05290000
 Hii 1.38.00
  SCGCQ00492564 - Obtain the Physical Slot number from the PCI Bridge to which the Controller is connected.
 BIOS 4.37.00
  SCGCQ00455591 - Memory access issue for when loading Ctrl R
  SCGCQ00455597 - Memory allocation: Allocate only two 64k
 FCODE 4.14.05.00

Package - v20.12.1-015 (MR4.11)
 Firmware - 2.130.394-2550
  SCGCQ00395533 - CC schedule is changed to an unjust date by "Configuration Clear"
  SCGCQ00349837 - Sequential Read performance is less on CacheCade associated LD's.
  SCGCQ00396335 - 9260-16i's drive locate/fault LED header is not working properly.
  SCGCQ00361312 - MR4.7 FW reports detected problem with iBBU07 charging circuit
  SCGCQ00360938 - When attempting to secure LD during RLM, receive option to secure LD, LD not secured (message incorrect/misleading.)
  SCGCQ00392840 - Prevent overtemp warnings while charging
  SCGCQ00399692 - Modify MR fw to eliminate four second window where drive swap is not recognized.
  SCGCQ00406955 - Prevent data correction in pagefil.sys to happen during Check Consistency after heavy I/O test.
  SCGCQ00422473 - When a Cachecade PD marked as missing is reused to make Cachecade VD IO integrity error is observed.
  SCGCQ00432851 - Saved Release Note DataSLIB returning bad data as good data after host reboots
  SCGCQ00436896 - Minimum Capacity needed for relearn is incorrect in 2208 MR FW
  SCGCQ00447652 - Potential data integrity issue seen when IOs are in progress and cachecade PD is marked as missing and reused to create another SSC VD.
  SCGCQ00448732 - Card Running iMR Machine Checks when Requesting Host Memory
  SCGCQ00449871 - Verify drive reinsertion within/before drive-removal-delay setting -verify discovery (Without IO)
  SCGCQ00414148 - Firmware returns invalid data in OOB packet
  SCGCQ00437920 - Data Miscompare found while running I/O overnight with degraded virtual drives
  SCGCQ00439197 - Potential data integrity issue with R5 cachedIO mode
  SCGCQ00421933 - IO integrity error seen after Source VD associated with CacheCade VD is forcibly unblocked
  SCGCQ00423725 - Sequential Read performance is less on CacheCade associated LD's.
  SCGCQ00421891 - Assertion failure in ../../raid/raidpci.c at line 8323 while running IO with cable pull/push.
  SCGCQ00421960 - During rebuild on PRL11 CacheCade VD and rebuild on RAID6 Source VD IO integrity error is seen.
  SCGCQ00450056 - Source VD gets blocked on OCR after one PD removal from R0 WB CCVD and reuse of that PD in creating another CCVD.
  SCGCQ00338466	- Not able to flash both 9265-8i and 9285-8e card with 5.3 patch 1 firmware
  SCGCQ00340840	- Don't interpret the cachecade BVD flags if the volume is created with old FW which does not support cachecade.
  SCGCQ00357643	- Possible data integrity issue during Raid Level Migration
  SCGCQ00359356	- Offline drive becomes automatically online during Raid Level Migration
  SCGCQ00363555	- Bad disk being serviced hung Linux boot for 2 hours
  SCGCQ00365307	- Offline drive becomes automatically online during Raid Level Migration
  SCGCQ00369276	- VD is degraded(automatically) after raid level migration R1 TO R5 (adding one drive)
  SCGCQ00369346	- VD is degraded(automatically) after raid level migration R1 TO R5 (adding one drive)
  SCGCQ00374525	- Firmware enters megamon by system reboot after changing MFC OEM
  SCGCQ00307050	- Not able to flash both 9265-8i and 9285-8e card with 5.3 patch 1 firmware.However, it is ok on 9266-8i.
  SCGCQ00338490	- Invalid target ID after new logical drive creation
  SCGCQ00341791	- Support for mutlipath topology is broken
  SCGCQ00361303	- on iMR FW update caused card to FW fault state and card cannot boot to OS.
  SCGCQ00371477	- During Reconstruction (R0->R5) when system reboots the reconstruction doesnt resume. System hangs Megamon hit
  SCGCQ00375250	- BMC see clock stetching on I2C bus
  SCGCQ00375854	- adapterOperations.alarmControl is being set to 1 even if controller doesnot have alarm on board
  SCGCQ00384381	- Drive temperature is shown very high on 9240
  SCGCQ00391094	- 9260-16i's drive locate/fault LED header doesn't work
  SCGCQ00392062	- Firmware halts when flashing components other than app.rom for OEM
  SCGCQ00392063	- PL library and files checkin for PL version 5.38
  SCGCQ00363619	- Set the Recovery mode page (WriteRetryCount and recoveryTimeLimit)
 BIOS - 4.36.00
 FCODE - 4.12.05.00
 UEFI_Driver - 0x05270000
 HII - 1.37.00
  SCGCQ00395508 - System with SSD HDD will pop up an error message after creating VD via HII
 PCLI - 03.02.20
 WebBIOS - 4.0-60-e_49-Rel
  SCGCQ00386062: Unable to read the correct value of controller property "Boot Error Handling" after changing
 NVDATA - 3.09.03-0052
  SCGCQ00393134: Change the showSgpio activity to 0
  SCGCQ00350995: Requested changes from Channel Factory Defaults for MFC values
  SCGCQ00411296: iMR FW NVDATA change for global fault/activity LED
 BootBlock - 2.02.00.00-0001
 ROMENV 1.08

Package v20.11.1-0135 (MR4.10p)
 Firmware - 2.130.384-2166
  SCGCQ00341980 - Current Access policy is not getting updated for iMR
  SCGCQ00353935 - Add support for Ringbuffer and Dq compilation
  SCGCQ00356925 - disableHII: Needs to be updated from nvdata into MFCD
  SCGCQ00357046 - 9240-4i on particular motherboard is not getting required memory resources on boot
  SCGCQ00349562 - Unable to open "Set Patrol Read Properties" in MSM with 2008-iMR
  SCGCQ00362340 - multi path with Consistency Check LED behavior problem
  SCGCQ00342405 - Enable or disable 512E using Applications
  SCGCQ00342397 - Provide the count of LBAs that are present in the sata bbm table.
  SCGCQ00350996 - Fail the IO in case the medium error recovery is taking more time.
  SCGCQ00359200 - offline drive becomes automatically online during Raid Level Migration
  SCGCQ00371803 - During Reconstruction (R0->R5) when system reboots the reconstruction doesnt resume. System hangs.
  SCGCQ00358361 - Bad disk being serviced hung Linux boot for 2 hours
  SCGCQ00373802 - Auto Foreign import fails when controller is booted with pinned cache.
 FCODE - 4.12.05.00
 UEFI_Driver - 0x05270000
  SCGCQ00347171 - MR: on having pinned cache on OEM controller, the option to invoke storage dosent come.
  SCGCQ00369636 - UEFI: Settime only when FW time is not set; DHP: Return appropriate health status when there is no critical boot message
  SCGCQ00340581 - UEFI Driver should check pMRCtrlInfo ->maxHANodes with > 1
  SCGCQ00318101 - Timed critical boot message under UEFI mode
  SCGCQ00347492 - UEFI: Retry read capacity if scsi status is not success
  SCGCQ00310476 - Load HII when user responds to critical boot message by pressing C
 BIOS - 4.35.00
 Hii - 01.36.00
  SCGCQ00268038 - Hii enter black screen/timeout when user switching between fields/form sub_form and during Pd rebuild.
  SCGCQ00364156 - Remove debug message which is not applicable for non Mercury customers
 NVDATA - 3.09.03-0045
 WebBIOS - 4.0-59-e_48-Rel
 PCLI - 03.02.20
 BootBlock - 2.02.00.00-0001
 ROMENV - 1.08

Package v20.10.1-0126 (MR4.9)
 Firmware 2.130.374-2023
  SCGCQ00262426 - If VD is secured while reconstruction is going on does not stay secured once reconstruction is done.
  SCGCQ00313883 - Battery continually stating Battery Yearly Deep Discharge Relearn Pending. Please Initiate a manual Relearn
  SCGCQ00319537 - System hang on IBM machine with a critical boot message
  SCGCQ00327006 - Event (MR_EVT_CTRL_RESETNOW_DONE ) is not generated after OFU is completed
  SCGCQ00329851 - EEPROM corruption(BQ2060 errata) due to corrupted value of design Capacity written in FCC for iBBU07
  SCGCQ00332181 - INVALID SGL causes dump into montask, OCR does not recover. MonTask: line 377 in file ../../dm/mpt2/mptrec.c & MonTask: line
  SCGCQ00333679 - reverting the changes of SCGCQ00295604
  SCGCQ00333696 - EEPROM corruption(BQ2060 errata) due to corrupted value of design Capacity written in FCC for iBBU07
  SCGCQ00334032 - Code review checkin
  SCGCQ00335607 - Firmware upgrade/downgrade not possible due to missing env stamping
  SCGCQ00336716 - Megamon issue when disabling the drive security on a MR controller with spun down FDE drives.
  SCGCQ00337894 - OFU is not happening when tried to upgrade firmware.
  SCGCQ00338008 - Flash of package with OFU request
  SCGCQ00345497 - Code review: With the new approach for CtrlOFUPossibleSet/Get() shutdown path broken
  SCGCQ00346275 - Copyback on a drive hits kill adapter
  SCGCQ00347253 - Firmware fails to return proper value when flashed same firmware image with different stamping with OFU request.
  SCGCQ00353344 - Data Corruption during Raid Level Migration
  SCGCQ00335935 - Coverity Defect fixes
  SCGCQ00286152 - GetConnectorIndex() Out of bound array access
  SCGCQ00334889 - Multiple switch cases are not handles correctly in debug functions
  SCGCQ00314781 - Controller always enter HSM when it is set to HCOE
  SCGCQ00317767 - Code Review Defect: Correct the error in copy back path smart errors path
  SCGCQ00333346 - Dont interpret the cachecade BVD flags if the volume is created with old FW which does not support cachecade.
  SCGCQ00340772 - Address Action Item SCGCQ00340495 (Check coding standard for structure OfuRequestState)
  SCGCQ00332658 - Out-of-bounds access (OVERRUN_STATIC) of an array "ar" in pdCopyBackSpinupCallBack
  SCGCQ00332651 - Out-of-bounds access (OVERRUN_STATIC) of an array "nvInfo->lockKeyBlob.keyCheck" in displayNvKeyInfo
  SCGCQ00329070 - Coverity Defect
  SCGCQ00315029 - PD clear operation is not handle correctly with spun drive drives
  SCGCQ00332588 - Fix coverity defects 10216 and 10425 (overrun and potential NULL pointer access)
  SCGCQ00307050 - Not able to flash both 9265-8i and 9285-8e card with 5.3 patch 1 firmware.However, it is ok on 9266-8i.
  SCGCQ00353322 - Unable to enable ocr using application due to FW ocr setting taking precedence
  SCGCQ00328109 - Out of bound access in LDBBMListInit
  SCGCQ00337060 - Coverity Defects
  SCGCQ00341791 - Support for mutlipath topology is broken
  SCGCQ00330344 - FW halts with a a kill adaptor on performing an onffline of the drive under copyback. line 1188 in file ../../raid/1078dma.c
  SCGCQ00332099 - Out-of-bounds access (OVERRUN_STATIC) of an array "ar" in pdDcmdRebuildCB
  SCGCQ00302600 - Added more debug information
  SCGCQ00307949 - True FW Online update for Liberator
  SCGCQ00307950 - BGI is in endless loop continuously restarting after completion
  SCGCQ00308988 - Improve foreign config import for iMR with mixed JBOD/RAID settings
  SCGCQ00314258 - Need the ability to determine what disk a logical LBA associate with on the fly, api call/algorithim/etc. on Liberator
  SCGCQ00323446 - Add NVDATA support to make 512 Emulated drive support as configurable for customers.
  SCGCQ00345203 - megacli reports battery pack is missing on hot insertion
  SCGCQ00314965 - iBBU07 - SOH bad will be declared for low capacity battery before starting learn cycle
  SCGCQ00307956 - iBBU07: EEPROM and register values will be updated to revised values at first boot after FW flash.
 BIOS - 4.34.00
 UEFI Driver 0x05210000
  SCGCQ00262858	- Debug message is shown from EFI app choice prompt
  SCGCQ00308870	- EFI Driver 518\When disconnecting the driver in EFI, I am still able to exectue the EFI utility menu.
  SCGCQ00312683	- UEFI Driver not timing out in 3 mins when FW is in undefined state
  SCGCQ00320619	- UEFI: Build Device Path and Get Next Target function of SCSI Pass Thru is not returning correct EFI status for certain cases
  SCGCQ00335617	- Drives are reporting timeout on Write Buffer cmd 
  SCGCQ00339371	- UEFI Driver fails SCT Test
  SCGCQ00343869	- Enhance critical boot message handling
  SCGCQ00338066	- UEFI - HAMR: Fire LD list query based on maxHANodes
  SCGCQ00338782	- If SetOptions is called for Invader dont show EFI WebBIOS and EFI CLI option
  SCGCQ00340581	- UEFI Driver should check pMRCtrlInfo ->maxHANodes with > 1 to determine HAMR
 HII 1.33.00
  SCGCQ00318010 - Allows to select Cachecade VD as Boot device
  SCGCQ00319005 - HII will not allow config to be cleared no drives attached
  SCGCQ00319010 - HII while in safe mode locks up when entering View drive
  SCGCQ00293056 - HII: LSIP200198414/LSIP200229508/LSIP200231613: Disables all requirement for human input at boot time
  SCGCQ00317934 - Add MFI State error string for the new MFI stat error codes
  SCGCQ00317991 - Remove 'Adaptive Read Ahead' option from every MegaRAID management utility (PR: SCGCQ00295908)
 FCODE 4.12.05.00
 NVDATA 3.09.03-0045
 - Code review: correcting the delivery error
 - Disable emergencyspare for a customer
 WebBIOS 4.0-59-e_48-Rel
 PCLI 03.02.20
 ROMENV 1.08
 BootBlock 2.02.00.00-0001

Package v20.10.1-0119 (MR4.8)
 Firmware 2.130.364-1847
  SCGCQ00308820 - Bbumode is 5 instead of 0 for iBBU07
  SCGCQ00311062 - Fatal firmware error: Line 1842 during FC import
  SCGCQ00284536 - 9260 controller VD goes offline during Slow/Full/Foreground Initialize with 3TB Seagate SED SAS drives
  SCGCQ00301160 - Limited band Charging for all OEMs
  SCGCQ00298687 - Code Review defect to handle SA_INVALID_FIELD_IN_CDB
  SCGCQ00292830 - FW correctly removes entries in the SBBM table by properly shifting the entries to the right.
  SCGCQ00292943 - Allocate BBLog for iMR Initally during boot up
  SCGCQ00295474 - BBU mode is set to 5 for BBU07 in ctrl-h
  SCGCQ00294981 - FW Montask on every boot
  SCGCQ00252606 - Drive fails after I/O timeout and subsequent target reset during continuous firmware flash.
  SCGCQ00284230 - Megamon during Injecting errors to VD with 512e PDs on iMR controller
  SCGCQ00295130 - spare pointer is incorrectly used in MR_CONFIG_DATA
  SCGCQ00290512 - Checked in the review comment for SCGCQ00286613
  SCGCQ00313883 - Battery continually stating Battery Yearly Deep Discharge Relearn Pending. Please Initiate a manual Relearn
  SCGCQ00319537 - System hang on OEM machine with a critical boot message
  SCGCQ00263446 - Support SGPIO SideBand with/without Activity
  SCGCQ00296744 - enable Emergency hotspare capability for channel
  SCGCQ00323446 - Add NVDATA support to make 512 Emulated drive support as configurable for customers.
  SCGCQ00286613 - ER corresponding to LSIP200230920
  SCGCQ00290530 - Band Gap charging for iBBU08
  SCGCQ00288679 - ER corresponding to LSIP200122939
  SCGCQ00290531 - Learn Improvement - Do not take Command block if there is no LD for which cache policy will change
 NVDATA 3.09.03-0045
   SCGCQ00324305 - Added enable512eSupport parameter in MR PARAMS PAGE in nvdata
 MR FCODE Driver release
 Signed UEFI Driver 0x05180000 (for Win 8 Secure Boot)
 BIOS 4.31.00
 HII 1.31.00
   SCGCQ00293398 - Can not enable SSD caching in HII
 WebBIOS 4.0-59-e_48-Rel
  SCGCQ00295052 - Change BBU Mode description for Liberator batteries. 
 PCLI 03.02.20
 ROMENV 1.08
 BootBlock 2.02.00.00-0001

v20.10.1-0107
Fixed Native configuration is no longer supported message in post
Fixed Patrol Reads on SSD drives
Fixed Implemented the limited band charging
Fixed Megamon during Injecting errors to VD with 512e PDs on iMR controller
Fixed Native configuration is no longer supported message in post
Fixed CRC errors during TSOC communication
Fixed iMR FW : Fail to read the header info from CFI Flash ROM during repeated system reboot. 

v20.10.1-0096
Fixed FW failes to create configuration and utilites fail to report the VD size after the reconstruction.
Fixed BJW STC - Error message pop out in Hatteras HII when set to factory default.
Fixed Megamon during import of FC from MR to iMR contoller

v20.10.1-0077
Fixed CSET: BT1680: SATA workaround handles LBA incorrectly for 6-byte read CDB 
Fixed Bios prints extra lines for press Ctrl_G to enter bios when you have some configuration errors
Fixed BT750 workaround code is not disabled in all the path
Fixed TB BIOS : Overwrites invalid address and force system to fail the boot.

v20.10.1-0051
1) Fix FW issue related to currentSSCSize.

v20.10.1-0044
1) Fixed No event is generated when fan in enclosure fails 
2) Fixed Medium error handling fixes for >2TB 
3) Fixed PCR 235 Warning for High Error Counts 
4) Fixed Add SGPIO for Medusa 

v20.10.1-0020
1) Fixed FW causes Fatal Error when HSP drive responded with Sense 0x02 for Write/Verify or TUR. 
2) Fixed Machine Check with particular motherboard. 
3) Fixed Provide the chip version/revision for MegaRAID controllers thru CmdTool2 
4) Fixed After a complete and successfully recalibrate cycle the request to a relearn is still on 
5) Fixed After FW downgrade eventlog is corrupted
6) Fixed Tape Device LTO-05 loads unexpectedly on SAS2108 and SAS2008 chip based MR adapters 
7) Fixed Some LED are still not working according to OEM SPEC with latest NVDATA 
8) Fixed intermittent RAID key authentication issue was occurring on boot up 
9) Fixed PL version 05.00.28.00 check in 
10) Fixed ESXi installation fails on RAID1/RAID0 cluster of two SSDs 
11) Fixed Intermittent initialization failure (Fault code 0x01) SDRAM ReadEye calibration 
12) Fixed sas address not programmed correctly for OEM Wasat boards 
13) Fixed Copy back does not start in a case of revertible HSP 
14) Fixed Field cant flash back from 10M08 to 10M04 successfully, requires Debugger 
15) Fixed SFO 2108 ROMB reports a non-functional Local Disk as "Operable" 
16) Fixed HSA0297 Command timeout happens in Electra + 600GB SAS HDD during the system power-on. 
17) Fixed RAID-0 Volumes Disappeared After RAID Creation - intermittent 
18) Fixed Disable VPD for specific SSVID
19) Added BBU AEN Change for 6G SAS controllers
20) Added ability to RESET expander from behind MegaSAS

v20.7.1-0016
1) Fixed - After replacing a 3rd party expander card, all the virtual drives are gone if the system is rebooted 
2) Fixed - Warning with RWC2 using Intel(R) RES2SV240 Expander Card with Intel MegaRAID cards 
3) Fixed - Fix config loss due to lost device insertion post processing callback during NEM replacement
4) Fixed - Phy 0-3 should be rate limited to SAS 1 speeds for old chip sping.
5) Added - Change NVDATA settings (xml files) for iMR product 
6) Added - Add new xml file for Inspur 
7) Added - Add new ID for ASUS MR product 
8) Added - Revise new iMR NVDATA 
9) Added - Add New Customer IDs to iMR & MR 
10) Added - Add CustomerIDs to 2108 MR (add a new xml file to 10M06 and later stream) 

v2.70.04-0862
1) Fixed Fw error during R50 9per per span rebuild. 
2) Fixed >2TB : DATA TLB ERROR Exception is hit while creation of VD. 
3) Fixed Change nvdata version stretagy to reflect corresponding train 
4) Fixed Dummy defect to checkin the Liberator B4/ Falcon B2 downgrade scenarios 
5) Fixed PL5 SAS_DISC_DS_MAX_ENCLOSURES_EXCEED 
6) Fixed DC is hit on VIEWs after OCR during rebuild. 
7) Fixed DI Issue : LDBBM entries are lost after REBOOT/OCR 
8) Fixed 6919982 Activity LEDs are backwards 
9) Fixed "DDF_ConfigReadPd" Error is shown in FW print on creating config OR during boot. 
10) Fixed FW hit mon task after connect cable to enclosure. 
11) Fixed Dummy defect to check in ieee changes 
12) Fixed No OCR after controller halt for OEM specific Sentinel change 
13) Fixed >2TB iMR: PR fails to detect medium errors 
14) Fixed >2TB : PR fails to find any medium errors on all RAID levels. 
15) Fixed Pl merge 05.00.07.00 
16) Fixed Sentinel Testing:Copy pattern to R0, reboot and doing CC will result in MegaMon 
17) Fixed All applications hangs when pdlist command is executed with 2TB SATA Drives. 
18) Fixed DATA TLB ERROR Exception is hit while creation of VD on SATA PDs 
19) Fixed Rebuild does not progress on a 2.2TB drive(restarts once it reaches 2%) 
20) Fixed DI Issue : FW fails to populate valid LDBBM entries. 
21) Fixed Sentinel testing: fw broke into MegaMon when test file is read (R0 and R1) 
22) Fixed Sentinel file gets corrupted on VDs with non default stripe size 
23) Fixed Dummy defect to check in B2 downgrade scenario changes for Falcon 
24) Fixed Sentinel testing: Megamon hit at reboot after copying pattern to R0,R1,R5,R6(4 drive) 
25) Fixed fw hits megamon on PD command timeout 
26) Fixed iMR Drake Controller doesn't auto rebuild drives on McCave Backplane 
27) Fixed DF365856 >2TB SATA drives are reported as only having 2TB capacity 
28) Fixed FW went to mon_tsk() when running heavy IO's + Rebuilding 
29) Fixed IO fail when running on 16 VDs. 
30) Fixed iMR PL5 FW removes pds when failing redundant path 
31) Fixed OEM changes for Sentinel 
32) Fixed (RW LSIP200062530) Dummy defect to checkin the Liberator B4/ Falcon B2 downgrade scenarios 
33) Fixed FW crashed when you Pull/Push SATA and SSD Drive with SAS Drive Present. 
34) Fixed FW breaks to MonTask: line 2771 in file ../../dm/mpt2/mptcmd. 
35) Fixed VD goes offline with command timeout on PDs in MP 
36) Fixed FW breaks into MegaMon during boot if unconfigured SATA drives are present in a Shea enclosure 
37) Fixed >2TB : DC is hit on R1/R5 VDs 
38) Fixed > 2TB : Drive comes up as foreign even when there is no config. 
39) Fixed DI Issue : CC/rebuild fails to detect the medium error. 
40) Fixed Support for snapshot is missing in Special handling of Pattern.  
41) Fixed Sentinel testing: Drive drop during cc after rebuild, and also during reconstruction 
42) Fixed >2TB: iMR Drive comes up as foreign after clearing config and reboot 
43) Fixed An un-configured PD comes up as configured after reboot. 
44) Fixed Sentinel file (read) causes specific drive model to fail 
45) Fixed >2TB-iMR-hotplug enclosure,debugger hit montask line 199 
46) Fixed CC fails to detect Media errors for above 2TB VD size 
47) Fixed >2TB : DI Issue : LDBBM entries are lost after REBOOT/OCR 
48) Fixed >2TB : DC is hit on PRL 11 using >2TB drives ST33000650NS 
49) Fixed Cascaded enclosures go missing when reconnecting enclosures to import foreign config.

v2.60.04-0829
1) Fixed Fix DATA TLB exception while updating DDF
2) Fixed Check in PL 2.20 which has permenant fix for alignement exception

v2.40.04-0787
1) Fixed Patrol Read wrongly detects medium error after full initialization.
2) Fixed Update MFC defaults in NVDATA
3) Fixed Change NVDATA to Enable exposeEnclosureDevices
4) Fixed change the slot mapping starting offset
5) Fixed Controller Properties Incorrectly Validated
6) Fixed HDD power save option is enabled by default for particular OEMs, and attempting to disable feature will not work

*Third-party trademarks are the property of their respective owners.

