//****************************************************************************
//                            INTEL CONFIDENTIAL
//                     Copyright 2012 Intel Corporation
//                           All Rights Reserved.
//
// The source code contained or described herein and all documents related to
// the source code ("Material") are owned by Intel Corporation or its
// suppliers or licensors. Title to the Material remains with Intel
// Corporation or its suppliers and licensors. The Material contains trade
// secrets and proprietary and confidential information of Intel or its
// suppliers and licensors. The Material is protected by worldwide copyright
// and trade secret laws and treaty provisions. No part of the Material may be
// used, copied, reproduced, modified, published, uploaded, posted,
// transmitted, distributed, or disclosed in any way without Intel's prior
// express written permission.
//
// No license under any patent, copyright, trade secret or other intellectual
// property right is granted to or conferred upon you by disclosure or
// delivery of the Materials, either expressly, by implication, inducement,
// estoppel or otherwise. Any license under such intellectual property rights
// must be express and approved by Intel in writing.
//
//****************************************************************************
//
//  Date:  October 16, 2012
//  Description:  Field Replaceable Unit (FRU) data file for the Intel
//  Server Board
//
//****************************************************************************


_LF_NAME       'SVRBD-ROW_P.fru' // Name for this load file
_LF_VERSION    '0.03'            // Version of this load file
_LF_FMT_VER    '1.50'            // Version of the load file format
_IPMI_VERSION  '2.00'            // IPMI format version

_FRU (
_FRU_TITLE     'Serverboard FRU' // FRU Title
_START_ADDR    0000              // Start Address
_DATA_LEN      0138              // Data Length
_NVS_TYPE      'IMBDEVICE'       // Non-volatile Storage Type
_DEV_ID        00                // Device ID
_DEV_BUS       FF                // Device Bus

_SEE_COMMON
   01                            // Common Header Format Version
   01                            // Internal Use Area Starting Offset (in multiples of 8 bytes)
   02                            // Chassis Info Area Starting Offset (in multiples of 8 bytes)
   10                            // Board Info Area Starting Offset (in multiples of 8 bytes)
   1A                            // Product Info Area Starting Offset (in multiples of 8 bytes)
   00                            // MultiRecord Area Starting Offset (in multiples of 8 bytes)
   00                            // Pad
   D2                            // Common Header Checksum

_SEE_INTERNAL
   01                            // Internal Use Format Version
   00                            // Intel reserves the right to relocate and redefine these fields
   00                            // without prior notification
   00
   00
   00
   00
   01

_SEE_CHASSIS
   01                 // Chassis Info Area Format Version Bit Fields
   0E                 // Chassis Info Area Length (in multiples of 8 bytes)
   17                 // Chassis Type (Main Server Chassis)
   D2                 // Chassis Part Number
   '..................'
   D2                 // Chassis Serial Number
   '..................'
   DF                 // Custom Chassis Info type/length byte for AM1 (For Microsoft WHQL use)
   '...............................'
   DF                 // Custom Chassis Info type/length byte for AM2 (For OEM use)
   '...............................'
   C1                 // End of field marker

_SEE_BOARD
   01                             // Board Info Area Format Version Bit Fields
   0A                             // Board Info Area Length (in multiples of 8 bytes)
   00                             // Language Code
   000000                         // Mfg. Date/Time
   D1                             // Board Manufacturer (17 Bytes)
   'Intel Corporation'
   CB                             // Board Product Name
   'SVRBD-ROW_P'
   CC                             // Board Serial Number (12 Bytes)
   '............'                 // Variable Field Entered by Test
   CA                             // Board Part Number (Contains the PBA# @10 bytes)
   '..........'                   // Variable Field Entered by Test
   CC                             // FRU File version ID string
   'FRU Ver 0.03'                 // FRU Ver 0.02
   C1                             // End of field marker

_SEE_PRODUCT
   01                 // Product Info Area Format Version Bit Fields
   0D                 // Product Info Area Length (in multiples of 8 bytes),WILL
   00                 // Language Code
   D1                 // Product Manufacturer Name
   'Intel Corporation'
   C7                 // Product Name
   'S4600LH'
   CA                 // Product Part Number (Contains the Top Assembly (TA)#)
   '..........'
   D4                 // Product Version (Available for OEM use)
   '....................'
   CC                 // Product Serial Number
   '............'
   D4                 // Asset Tag (Available for OEM use)
   '....................'
   C0                 // FRU File ID (Not used)
   C1                 // End of field marker

}