This release note and the software that accompanies it are copyright (c) 2014, Intel Corporation or its suppliers, and may only be installed and used in accordance with the license that accompanies the software.

This Software is furnished under license and may only be used or copied in accordance with the terms of that license. No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. The Software is subject to change without notice, and should not be construed as a commitment by Intel Corporation or its suppliers to market, license, sell or support any product or technology. Unless otherwise provided for in the license under which this Software is provided, the Software is provided AS IS, with no warranties of any kind, express or implied. Except as expressly permitted by the Software license, neither Intel Corporation nor its suppliers assumes any responsibility or liability for any errors or inaccuracies that may appear herein. Except as expressly permitted by the Software license, no part of the Software may be reproduced, stored in a retrieval system, transmitted in any form, or distributed by any means without the express written consent of Intel Corporation.

==========================
Supported RAID Controllers
==========================
This download supports Intel(R) RAID controllers using MR software stack (RS3DC040, RS3DC080), please verify that this utility has been tested with the RAID card you have chosen to use by checking the drivers web page for your controller at http://support.intel.com.

===================
Package Information
===================
Flash package = v24.2.1-0021

==========
Attention!
==========
The EFI StorCLI tool and update script will only work with 'Boot Mode' set to 'UEFI' or 'EFI Optimized Boot' set to 'Enabled' in system F2 setup.

Intel recommends to loading Factory Default setting after the firmware upgrade which will not affect data on any existing array. To do so:
1. Reboot the system and login to the RAID BIOS Console. 
2. Select the controller and select 'Adapter Properties'->'Next'
3. Set the 'Set Factory Defaults' setting to 'Yes' and submit the change.
4. Reboot the system (the default settings are applied).
5. Re-configure to the desired settings in RAID Web Console2.

==================
Known Restrictions
==================
1) The EFI StorCLI tool and update script will only work with 'Boot Mode' set to 'UEFI' or 'EFI Optimized Boot' set to 'Enabled' in system F2 setup.
2) This download does NOT support EFI v1.1 environment. Please use the EFI shell command “ver" which will display the EFI version, to identify the EFI version.
3) When 2 or more VDs are created, VD cache settings must be the same.

=======================
Contents on the package 
=======================
The following files are included in this zip:

Name:							Description:
COPYING.NEWLIB.txt					License Agreement
3108-IMR_FWPKG-v24.2.1-0021_readme.txt			This file
MR62.rom						Firmware binary
License_v2.pdf						License Agreement
update.nsh						UEFI firmware update batch file
StorCLI\EFI\*						UEFI update utility and support files
StorCLI\FreeBSD\*					FreeBSD update utility and support files
StorCLI\Linux\*						Linux update utility and support files
StorCLI\Solaris\*					Solaris update utility and support files
StorCLI\Sparc\*						Sparc update utility and support files
StorCLI\Ubuntu\*					Ubuntu update utility and support files
StorCLI\Vmware\*					Vmware update utility and support files
StorCLI\Vmware-MN\*					Vmware-MN update utility and support files
StorCLI\Windows\*					Windows update utility and support files


==========================
Installation instructions:
==========================

UEFI shell instructions for updating RAID Firmware:
-----------------
   1. Download and extract all files to a USB flash drive.
   2. Set 'Boot Mode' to 'UEFI' in BIOS F2 setup (Note: in Romley and older systems, set 'EFI Optimized Boot' to 'Enabled') 
   3. Boot the target system to EFI shell. 
   4. Change directory to the local drive and directory containing the flash update files and the firmware image file.
   5. Type "update.nsh" and press <Enter> to execute the command
   6. Wait for the flash to complete. Do NOT reboot the system during the update.

You can also use RAID Web Console 2 or OS version of StorCLI to update the RAID firmware.  For more detail, please refer to the Intel(R) RAID Software User's Guide.

=============================
Package Details/Fixes/Updates 
=============================
Package: 24.2.1-0021 (MR 6.2)
 Firmware 4.220.40-3267
  SCGCQ00651072 - Battery learn cycle continues to more than one cycle even FW has marked it as bad in previous reboot
  SCGCQ00645802 - DIS mismatch while running system reboot script with dirty data in DDR
  SCGCQ00644122 - Optimize onfi descriptor setting for offload
  SCGCQ00637239 - FW crash while launching Ctrl+R
  SCGCQ00612786 - Assertion failure in double DIP power cycle test case
  SCGCQ00604253 - Elapsed time of Patrol Read in tty log is incorrect
  SCGCQ00602839 - Elapsed time of Reconstruction is incorrect
  SCGCQ00598917 - Firmware not taking "SMARTerEnabled" from NVDATA
  SCGCQ00598825 - Rebuild triggered on an incompatible blocksize PD
  SCGCQ00573764 - Upgrade 3108 MR FW failing
  SCGCQ00569093 - PD erase does not work with SATA SSDs
  SCGCQ00558985 - Diagnostics failed after Drives goes to shield state
  SCGCQ00549095 - The DQlog.bin is getting corrupted after restarting the service of MRDiag
  SCGCQ00546653 - protect the removal of the device when the device is still under initialization
  SCGCQ00527932 - BIOS is not getting updated with the DISM progress
  SCGCQ00527416 - Running out of free entries in task list due to recursive addition of tasks
  SCGCQ00527397 - Wrong information of PD erase progress is shown by the firmware.
  SCGCQ00527241 - DM_DISM_LOG_SENSE state is not present in DISM
  SCGCQ00524801 - PI enabled VD is importing successfully even though "prevent PI Import" option is enabled
  SCGCQ00524040 - Change the CRC filed size
  SCGCQ00518855 - Fix the learn issue at powerup
  SCGCQ00505401 - LSI_MR Controllers fails to set "FACTORY SETTINGS"
  SCGCQ00503341 - VD's switch from Write Back with BBU to Write Through when an OCR is issued and BBU gets disabled.
  SCGCQ00503309 - Fix scheduling of hostspare correctly
  SCGCQ00503257 - seen DC error while running io's on 6.2 in Dev pull-push setup
  SCGCQ00499700 - chaos fails on R6 VD after importing failed R5 VD and one of R1 CacheCade drive
  SCGCQ00499455 - Defect fix for MSM does not show Create cachecade option
  SCGCQ00495896 - To fix task list overflow issue on max config setup
  SCGCQ00452322 - FW throws "MPT_LogDiscoveryErrors: SAS_TOPOLOGY_MAX_TOPO_PHYS_EXCEED" when connect 2 in multi-path
  SCGCQ00457909 - Assertion failure in ../../raid/raidpci.c at line 10522
  SCGCQ00461907 - Read VPD error message on 3108
  SCGCQ00464372 - Configurable drives count in iMR reflected wrongly to applications
  SCGCQ00466545 - wrong error code displayed and wrong error message for copyback command
  SCGCQ00466936 - FW hits to MonTask: while running enclosure power cycle with 4K drives
  SCGCQ00469174 - Issue with supercap energy calculations
  SCGCQ00470287 - modify scap energy calculation
  SCGCQ00471823 - directly attached SATA drive is not detected by controller
  SCGCQ00472614 - Dual Context to Single Context switching does not toggle when Cobra expanders are cascaded with EDFB enabled PHY's.
  SCGCQ00473420 - Defect fix for Montask observed while installing OS on JBOD
  SCGCQ00476945 - Controller Hangs during execution of Storcli command ''/c0 delete termlog''
  SCGCQ00477266 - Battery retention test failure during continuous loop test when there was power failure during erase
  SCGCQ00477667 - Battery Enable (BBE) is asserted even when BBU/Supercap not present or even when all LDs are in WT mode
  SCGCQ00485545 - TM timeout during enclosure pull while running heavy IO
  SCGCQ00486810 - Learn is not completing at powerup
  SCGCQ00487215 - 3TB Seagate PD size being reported as 2TB in Apps/Firmware
  SCGCQ00493312 - Controller Reset due to Fatal Error with RAID6/60 configuration
  SCGCQ00494704 - Elapsed Seconds displayed in firmware logs for background operations progress is improper
  SCGCQ00384656 - Kill adapter observed while running IOs on JBODs and VDs
  SCGCQ00614723 - CME handling of Invader
  SCGCQ00599798 - Issue with Global Hot Spare assignment
  SCGCQ00596434 - Drives connected through enclosure showing wrong slot numbers.
  SCGCQ00580415 - issue with MR 24.1.1-003 with JBOD Mode enabled
  SCGCQ00557580 - (null) noticed while PD pull-push testing.
  SCGCQ00554546 - SMPpassthru is not happening through storlib.
  SCGCQ00551614 - System Reboots after issuing the OCR and kernel panic is observed
  SCGCQ00524812 - on breaking multipath while drives are spinning up results in montask
  SCGCQ00523544 - Initialize invalid interrupt as part of intInitialize function
  SCGCQ00518692 - OEM server hangs after enabling EKM and rebooting.
  SCGCQ00505537 - Associating cachecade VD to a secured VD from Storcli does not fail.
  SCGCQ00496454 - Offload fails after corrupting BMT1 and BBT 2 address location
  SCGCQ00496422 - Adding the log event corresponding to ER   SCGCQ00493492
  SCGCQ00435204 - BGI kicks in on 5R5 but shows no progress at any point of time.
  SCGCQ00446327 - Defect fix for Unable create R0 in HII with 4K drives
  SCGCQ00451805 - FW-FW hit 'MonTask: line 243 in file ../../raid/1078in' while issuing OS reboot command on 9340 controller
  SCGCQ00470310 - CPLD input GPIO 21 driving when supercap is present and not present
  SCGCQ00472407 - Pinned cache gets flushed even after memory battery problem occurs.
  SCGCQ00474617 - VD erase restarts instead of resuming after reboot.
  SCGCQ00477301 - Fix the cset issue
  SCGCQ00478707 - Cache Memory Size of controller Information is ZERO
  SCGCQ00484448 - Data Corruption observed while running FPIO on VDs; making-breaking multipath in overnight loop.
  SCGCQ00486766 - Config loss after OCR during creation of config - when the drives are still spinning up
  SCGCQ00486982 - Added an event to notify the user when command times out on PD
  SCGCQ00487803 - FDE/SED drives does not reflect as FDE/SED drives.
  SCGCQ00605077 - "Corrected medium error" event is logged for uncorrectable medium errors during PR
  SCGCQ00530495 - To declare block bad at the earliest for the safer side the number of error correction bits shall be reduced
  SCGCQ00504346 - Re-enable EKMS for OEM
  SCGCQ00421822 - System reboots continuously after flashing Firmware in Solaris _11
  SCGCQ00460033 - MonTask: line 7193 in file ../../bbu/onfi.c
  SCGCQ00461733 - Kill adapter observed on large setup on enquiring Controller properties while drives spinning up from powersave.
  SCGCQ00463368 - coverity tool reported issue 13545(Wrong sizeof argument)
  SCGCQ00465561 - restore and flushing cache to PD are not reliable when 1st image of NF mem is corrupted
  SCGCQ00470502 - Firmware is allow to create slices in cachecade drivegroup using SMIS utility.
  SCGCQ00474005 - EKMS feature for OEM is disabled
  SCGCQ00474734 - max temperature bytes read from VPD is should be swapped before using
  SCGCQ00477996 - MR_6.2_DISM: FW hung due to DISM discovery failure on pulling the enclosure cable on reboot after running adpbattest.
  SCGCQ00488780 - Controller alarm continues to beep after transitioning VD from degraded to optimal state.
  SCGCQ00494084 - Handle OEM fault LED behavoir
  SCGCQ00556570 - MR6.2_iMR_fury_DM_Issue_TUR
  SCGCQ00524903 - In enclosure management page for DELL ,it shows some junk data in HII
  SCGCQ00501356 - Controller Reset due to Fatal Error with RAID6/60 configuration
  SCGCQ00402933 - CME logic using overlaid fields in c->rec
  SCGCQ00460254 - Montask appears on running IO's on 64VD's while changing LD policies
  SCGCQ00465672 - Enable OCR by default on GCA builds
  SCGCQ00480503 - MR: on FW init, controller post adapter base port missing
  SCGCQ00495361 - Invalid "Elapsed Seconds" value for FGI
  SCGCQ00531106 - Rebuild and Consistency Check aren't progressed when it is executed by CTL+R
  SCGCQ00518734 - Latest API changes in mr.h breaks FW compilation in mrdebug.c
  SCGCQ00464536 - Build Issue using GNUmakefile for MR and iMR
  SCGCQ00524913 - Storcli command to reset the boot ld on controller fails
  SCGCQ00506335 - boot block compile fails because of an erroneous macro definition
  SCGCQ00468366 - DATA TLB error faced while powercycle the enclosure during controller initialization 
  SCGCQ00490696 - foreign import fails if degraded VD is present in import
  SCGCQ00415512 - Toolbox Console Text Display Tool
  SCGCQ00451314 - Porting of the PR "spin up changes to accommodate multiple power domains simultaneously" to Invader.
  SCGCQ00460871 - Validate the requested blocks for SCSI VERIFY commands on RAID volumes
  SCGCQ00466819 - IOCInit multiple Reply Descriptor Post Queue addresses
  SCGCQ00471500 - Firmware Change for Pre-boot management tool & boot capability for SPARC
  SCGCQ00477817 - add reserved fields to IO Unit Page 7 for future use
  SCGCQ00481549 - Disable thermal throttle changes
  SCGCQ00493492 - Identifying the DDR, ONFI flash and SCap combination
  SCGCQ00518786 - SGPIO back plane requires ramdon slot number support.
  SCGCQ00595486 - Increase PCIe Receiver Margin
  SCGCQ00595487 - Increase margin in PCIe Rx Serdes
  SCGCQ00438437 - obsolete SAS IO Unit Control _TRANSMIT_PORT_SELECT_SIGNAL
  SCGCQ00471293 - obsolete "Limit SATA max rate to 1.5 Gbps"
  SCGCQ00490725 - Debug Queue Implementation and Support as part of enhanced MR Diagnostic support
  SCGCQ00573397 - Increase the support for 32 slots
  SCGCQ00585068 - Add Critical event in FW to indicate that an INIT operation was halted due to reboot or other failure
  SCGCQ00593824 - Update code to modify GG and VPD at powerup
  SCGCQ00468085 - Implement throttle mechanism to prevent thermal run away
  SCGCQ00472399 - Change hash algorithm for cache row hash from a bit mask to a modulo
  SCGCQ00556564 - DIS feature
  SCGCQ00469990 - Signed images for FWDownload
  SCGCQ00342679 - Don't interpret the cachecade BVD flags if the volume is created with old FW which does not support cachecade.
  SCGCQ00359329 - Code-review action item for removing and updating names for AEN dism.
  SCGCQ00454419 - Patrol Read - no progress
  SCGCQ00462259 - WB Logical disks are moving to WT after corrupting BMT1,BBT1 and reboot.
  SCGCQ00462309 - Deep Learn is not invoked in new battery, when the system is reboot before the first learn completes
  SCGCQ00462327 - Transparent Learn Cycle is rescheduled even though it is not completed
  SCGCQ00469037 - TFM error handling : Cache policy change for WB to WT if supercap is faulty
  SCGCQ00469755 - Intermittent SEP errors on iMR and MR controllers
  SCGCQ00471540 - When Cachecade LD is deleted invalid LD details is shown in the Cachecade size changed event.
  SCGCQ00473330 - Hotspare Recovery Doesn't Start after Inserting Failed Drives
  SCGCQ00478032 - FW sending wrong configuration data during boot msg pending state
  SCGCQ00479443 - Upgrading from Software RAID to 9260-8i causes Alarm to sound
  SCGCQ00482660 - ONFI_BBM Dev test build: FwTermLog does not preserve information before powerup. 
  SCGCQ00483590 - iMR TB Data loss when reconstructing from 1 drive R0 to 2 drive R1 with reboot
  SCGCQ00484771 - incorrectly uses a slot offset value to enumerate HDD.
  SCGCQ00485259 - In case of a certain OEM iMR shows R5 enabled.
  SCGCQ00492432 - MSM log warning: Controller booted in headless mode with errors
  SCGCQ00495888 - Set the Recovery mode page (WriteRetryCount and recoveryTimeLimit)
  SCGCQ00498734 - If VD is secured while reconstruction is going on does not stay secured once reconstruction is done.
  SCGCQ00498742 - SEAGATE hotspare drives remain spun up on LSI FW 12.12.0-0079
  SCGCQ00498946 - Firmware is not updating recovery timer as intended
  SCGCQ00502953 - Call DDF_discardInvalidPds only if DS3 is enabled
  SCGCQ00518879 - LSI_MR Controllers fails to set "FACTORY SETTINGS"
  SCGCQ00521513 - Controller Reset due to Fatal Error with RAID6/60 configuration
  SCGCQ00521758 - VPD output of lspci –vvxxx showing [RV] Reserved: checksum bad, 86 byte(s) reserved
  SCGCQ00523958 - Multi-stripe size in each raid level of R1,r5,r6 with SAS, DIF, 4K pinned cache offline vd import cause Montask
  SCGCQ00523962 - Remove memory module on MR controller to downgrade to iMR does not work
  SCGCQ00523970 - HII critical message form/Extra character "r" with configuration not supported critical message.
  SCGCQ00523976 - Fw defect in PdStateSet()
  SCGCQ00524442 - Controller Reset due to Fatal Error with RAID6/60 configuration
  SCGCQ00524493 - Correct how the SCL high and low period values are calculated for the I2C to run at 400Khz
  SCGCQ00524494 - For new spin up code get persistent devId for drives that are connected via internal back plane.
  SCGCQ00526284 - Controller Reset due to Fatal Error with RAID6/60 configuration
  SCGCQ00526632 - Drive security mode switching in MSM
  SCGCQ00526633 - Unable to create another Virtual Drive when pulling first drive (degrading) in partial Virtual Drive where all drives are configured
  SCGCQ00549320 - Baseboard Management Controller (BMC): STP passthru command failure
  SCGCQ00552443 - External Key management security for iMR
  SCGCQ00552444 - Re-keying a controller with External Key Management(EKM) security enabled, results in a corrupted key ID.
  SCGCQ00554050 - Performing an online firmware update or Online Controller Reset(OCR) on a controller with External Key Management(EKM) enabled, results in all secured drives marked as foreign.
  SCGCQ00558051 - MR 4K Validation : 4K VD assigned to 512K CacheCade
  SCGCQ00559254 - Re-keying in External Key Management mode followed by disabling security and enabling LKM results in a bail out while creating a Virtual Drive
  SCGCQ00562800 - VD goes offline when we start reconstruction on 32 Drive R0 VD
  SCGCQ00566690 - Raise priority of pci config trap interrupt to critical
  SCGCQ00567036 - Not seeing the correct Boot Message when the connection to the External Key Management server is down
  SCGCQ00575842 - Switching to Local Key Management Mode(LKM) after a rekey in External Key Management(EKM) rekey without rebooting results in HII saying key incorrect but Firmware says key was created.
  SCGCQ00575843 - On a controller with Local Key Management(LKM) enabled, user is asked to enter the security key to unlock and import a foreign, locked and External Key Management(EKM) enabled drive.
  SCGCQ00579499 - FwTermLog does not preserve information before powerup. 
  SCGCQ00579847 - Implement I2C Slave Address for Sideband Management
  SCGCQ00580752 - Defect Fix for VPD and inquiry callback issues in DISM
  SCGCQ00580771 - spin up tracker dequeue is not handled for case in which TUR error happens even after MAX retries
  SCGCQ00588963 - Too many unexpected sense AEN raised by CC during CME recovery on R5
  SCGCQ00588964 - Too many unexpected sense AEN raised by CC during CME recovery on R5
  SCGCQ00588973 - Fix GNU make file compilation
  SCGCQ00588977 - Routines to inject bit error in NF and ecc error in DDR for ONFI
  SCGCQ00588978 - Mismatch in LD id and target ID during set/reset boot device
  SCGCQ00588979 - Mismatch in LD id and target ID during set/reset boot device
  SCGCQ00593826 - Adding test routine for the bad block loop test for PR   SCGCQ00423195
  SCGCQ00595783 - SMART poll needs to issue log sense with page control set to current/ cumulative value
  SCGCQ00597425 - FW breaks if wrong security key is entered
  SCGCQ00604028 - on breaking the multipath in loop while drives are spinning up will result in montask
  SCGCQ00604030 - FW hangs while creating 64 VDs on the controller with SLES11 SP2 PPC64
  SCGCQ00604033 - While running reconstruction from R1 to 4 drive PRL11 with IO,FW hits to MonTask: line 1270 in file ../../raid/1078dm
  SCGCQ00604041 - Static analysis tool defect
  SCGCQ00604042 - Static Analysis Tool defects
  SCGCQ00609872 - CLI Reporting of TMM VPD
  SCGCQ00610801 - Rebuild triggered on an incompatible blocksize PD
  SCGCQ00610813 - Issue with Global Hot Spare assignment
  SCGCQ00610824 - Elapsed time of Reconstruction is incorrect
  SCGCQ00610834 - Elapsed time of Patrol Read in tty log is incorrect
  SCGCQ00610846 - "Corrected medium error" event is logged for uncorrectable medium errors during PR
  SCGCQ00612226 - Increase margin in PCIe Rx Serdes
  SCGCQ00612228 - Increase PCIe Receiver Margin
  SCGCQ00620118 - Liberator Card loses its boot VD after many reboots
  SCGCQ00635628 - Cache policy of Virtual Drives(VD) does not change to Write Through(WT) mode even after detecting a bad supercap.
  SCGCQ00638288 - RAID configured on PD been erased with Normal or Thorough will lost after system reboot/reset
  SCGCQ00646479 - Defect fix for kenel panic with iMR Fury with Free BSD driver
  SCGCQ00651117 - Hitting montask line 1930 in file ../../bbu/onfi.c while running FP IO's on degraded VD's
  SCGCQ00335860 - Cachecade configurations could not be created.
  SCGCQ00462330 - Deep learn doesn't start when it is requested during relaxing.
  SCGCQ00469041 - Write policy changed from WT to WB when the battery/Supercap is declared as bad
  SCGCQ00471509 - Firmware crash seen while doing continuous sas cable pull
  SCGCQ00471542 - Invalid "mode select(Page=0a)" issued during disk initialization phase.
  SCGCQ00477967 - Defect fix for Montask observed while installing OS on JBOD
  SCGCQ00478050 - Firmware returns asc value as 0 when failing IOs with medium errors
  SCGCQ00482662 - display BMU fw version in battery design info
  SCGCQ00482663 - Break Mirror for R10 should not be allowed
  SCGCQ00486553 - Medium error correction event is not logged during CC
  SCGCQ00498748 - 9240-4i on BCM RX67Q-6S motherboard is not getting required memory resources on boot
  SCGCQ00503258 - foreign import fails if degraded VD is present in import
  SCGCQ00504804 - L2/L3 cache error on reboot
  SCGCQ00514666 - search for one wire devices prints are masked after the boot
  SCGCQ00518020 - VPD info can't be retrieved for OEM enclosure
  SCGCQ00523959 - If a BOOT Passphrase is enabled with SafeStor "MegaCli adpbios dsply a0" will display "BIOS will Stop on error" even if any other mode is set.
  SCGCQ00523972 - Profile based VD creation - [Partial RAID options blocked until system reboot]
  SCGCQ00523975 - Hard coded values should be removed in TFM module
  SCGCQ00524802 - Fix repeated prints issue
  SCGCQ00559253 - A data TLB error occurs when the External Key Management Server(EKMS) is down and drive security is changed from External Key Management(EKM) mode to Local Key Management(LKM) mode.
  SCGCQ00563824 - HII & Ctrl-R: BGI operation still running on RAID0 VD even after PI protection disabled
  SCGCQ00575844 - Getting a non informative message when trying to import a Virtual Drive after a re-key without reboot
  SCGCQ00577296 - Deep learn will not start immediately when Relative State of Charge (RSOC) of battery is equal to 95%.
  SCGCQ00593485 - Raid configuration loss after reboot - PDs in POWERSAVE
  SCGCQ00600939 - Fix the learn issue at powerup
  SCGCQ00603399 - Faulty protocol used for changing the Disk Write Cache Policy
  SCGCQ00604029 - on breaking the multipath in loop while drives are spinning up will result in montask
  SCGCQ00604031 - FW- FW hangs while creating 64 VDs on the controller with SLES11 SP2 PPC64
  SCGCQ00604038 - Static Analysis Tool defects
  SCGCQ00604039 - Static Analysis Tool defects
  SCGCQ00604074 - Enabling DQ support bit in FW
  SCGCQ00610444 - The restore successful and unsuccessful prints to be handled properly
  SCGCQ00614828 - not enough bs found during double Dip power cycle Test
  SCGCQ00615002 - Montask in divert.c seen when injecting 64K consecutive errors on R0 VD, Patrol Read running in background.
  SCGCQ00615537 - Single image support for ONFI
  SCGCQ00635323 - Assertion failure (not enough BS found) in double DIP power cycle test case
  SCGCQ00651115 - DC observed upon performing OCR on a degraded R1 (AWB).
  SCGCQ00450647 - 9260-8i(SAS2108) hitting OOB SRAT timeout for a long time causing OOB commands to fail
  SCGCQ00470568 - modify scap energy calculation
  SCGCQ00483575 - wrong error code displayed and wrong error message for copyback command
  SCGCQ00485096 - Bad or Missing TMM boot message is changed to Critical error
  SCGCQ00498752 - 9260-16i's drive locate/fault LED header doesn't work
  SCGCQ00518011 - MR Controller does OCR due to Temp Buffer overflow
  SCGCQ00523459 - The Firmware does not change the Virtual Drives's from Write Through to Write Back after a battery manual learn cycle is complete
  SCGCQ00554074 - SLES 11.3 x64 Halts when Loading Kernel During Warm Reboot Stress
  SCGCQ00555052 - Initialize invalid interrupt as part of intInitialize function
  SCGCQ00567037 - Switching the security mode from External Key Management(EKM) to Local Key Management(LKM) on iMR controller will result in a corrupted controller key.
  SCGCQ00595833 - SMART poll needs to issue log sense with page control set to current/ cumulative value
  SCGCQ00604043 - Static Analysis Tool defects
  SCGCQ00617625 - Power removal of enclosure FW hits to MonTask: line 4056 in file ../../bbu/onfiBBM.c
  SCGCQ00359282 - Multiple interposer drives will not be detected by MegaRAID firmware.
  SCGCQ00454415 - Infinite retry happens on Test Unit command when HDD didn't respond to TU command during the initialization.
  SCGCQ00462149 - Secondary RAID key data page read failure 6 seen on some controllers and key vault combination
  SCGCQ00478428 - StorCLI_F showed firmware download failed but really took
  SCGCQ00481856 - Assertion failure in ../../raid/raidpci.c at line 10522
  SCGCQ00484769 - FW Crash when using SCSI Passthrough SCSI_READ_10(0x28) to read 512 bytes on a RAID5 Native 4K drive.
  SCGCQ00492431 - When pinned cache present VD property not changing from WB to WT.
  SCGCQ00492433 - PDs go online without VD created & App doesn't allow any VD creation on passing a wrong parameter in Spanned VD.
  SCGCQ00497659 - Customer is hitting an ECC error
  SCGCQ00521514 - Invader: Cache Memory Size of controller Information is ZERO
  SCGCQ00554312 - Incorrect variable type in MR Read/Modify/Write path
  SCGCQ00598504 - StorCLI_F showed firmware download failed but really took
  SCGCQ00617620 - cache restore failure message displayed though cache restore was successful
  SCGCQ00372236 - System hanged after pulling out drives from a 8Raid-6 array during OCR in Debian OS
  SCGCQ00454381 - Change SES Green/Amber LED behaviour for OEM ACHILLES JBOD enclosure.
  SCGCQ00597426 - FW breaks if wrong security key is entered
  SCGCQ00366030 - While executing path-failover test with an SATA-SSD drive behind an interposer, the device is marked failed.
  SCGCQ00454368 - Card Running iMR Machine Checks when Requesting Host Memory
  SCGCQ00456776 - iMR FW update caused card to FW fault state and card cannot boot to OS.
  SCGCQ00479292 - system black screen during S1 Sleep test
  SCGCQ00490892 - Firmware Crash during Controller StartUp when large number of drives are connected
 UEFI_Driver 0x06030501
  SCGCQ00478652 - Block IO tests from SCT IHV test suite failed
  SCGCQ00479003 - Disable Debug print in UEFI Driver
  SCGCQ00498925 - Not able to boot into BIOS boot menu
  SCGCQ00518791 - In IsValidHandle() - Free the buffer if status is not EFI success for LocateHandle
  SCGCQ00493654 - Memory Leak issue in UEFI driver when reconnect happens
  SCGCQ00483847 - Remove private GUID and use EFI_KMS_PROTOCOL_GUID defined in UEFI 2.3.1 spec
  SCGCQ00479016 - Disable Debug print in UEFI Driver
  SCGCQ00484085 - UEFI hang when SATA is connected
  SCGCQ00484086 - UEFI hang when SATA is connected
  SCGCQ00579837 - UEFI Driver should calculate checksum before setting bios data (MR_BIOS_DATA)
  SCGCQ00468948 - Uninstall HII CAP and Driver Health formset if platform calls Start again without calling GetHealthStatus
  SCGCQ00477828 - 9240/9260/9270 UEFI driver issue with RD640/RD440 platforms when user having 2TB or 4TB VD
  SCGCQ00477705 - 9240/9260/9270 UEFI driver issue with RD640/RD440 platforms when user having 2TB or 4TB VD
  SCGCQ00484113 - Follow UEFI Spec on interpreting In and Out Transfer Length that upper layer sends
  SCGCQ00478692 - Block IO tests from SCT IHV test suite failed
  SCGCQ00484114 - Follow UEFI Spec on interpreting In and Out Transfer Length that upper layer sends
 Hii 03.05.11.03
  SCGCQ00470101 - Allow user to edit VD size (that is free form input) as it is cumbersome to modify the size using +/-
  SCGCQ00471830 - Save and Restore Configuration – MR
  SCGCQ00556209 - Transition a Thunderbolt MR controller to run in iMR mode = Controller fail in HII After Memory removed
  SCGCQ00556811 - When controller is in safe mode the PD menu displays inaccurate text and hangs when clicking a PD
  SCGCQ00579816 - HII\EKM-LKM without reboot should show proper message
  SCGCQ00452128 - HII cannot assign partial space less than 1 GB
  SCGCQ00573871 - fixing code review defects (AIM version + UCM GUID + deallocation)
  SCGCQ00529287 - Profile Based Raid1 Creation fails as invalid arguments
  SCGCQ00502940 - Naming inconsistency in option present in Create VD and Create VD - Advanced
  SCGCQ00482092 - condition checking is not right
  SCGCQ00474402 - Allows user to select EKM mode when supportEKM is set to 0
  SCGCQ00485401 - Using 84 PD encl when clicking on HW, Advanced then Enclosure Management, it completely freezes the system
  SCGCQ00571353 - Allow user to select RAID level when controller has other VD + error handling
  SCGCQ00569098 - Enter security key for locked drives screen, press down to get to OK, OK will show up again on right
  SCGCQ00473204 - unable to show UF003 as well the first two forms + XML special character handling
  SCGCQ00486457 - fixing memory leak of 128 drive enclosure implementation
  SCGCQ00556839 - Able to select EKM even when the EKM FOD key is removed from the system.
  SCGCQ00505566 - Drop down option to set phy linkspeed tp 12 Gbps in HII browser is not available.
  SCGCQ00473186 - Save and Restore Configuration - MR w/ Premium Features (SED and Cachecade)
  SCGCQ00501111 - Issues when trying to change EKM security key from change security key option.
  SCGCQ00523869 - EKMS is down but it is still possible to select drive security in MSM and HII during creation.
  SCGCQ00524969 - Going from LKM to EKM asks for a Current Security key Identifier and Security key.
  SCGCQ00527700 - Update the latest API change in HEFU
  SCGCQ00571359 - UCM Phase 1: Typo "Clear Configuration" -> "Clear Configuration"
  SCGCQ00500945 - EXPAND operation fails in HII for prl11
  SCGCQ00494431 - Streamline the usage of max PD in limited configuration path (alias UCM)
  SCGCQ00494214 - Help content for Free space in Select Drive group is inappropriate
  SCGCQ00485932 - UCM Simple Configuration: Allow Clear Config always + Suppress Checkbox (Uf002.PDs) when VD count is >0
  SCGCQ00575062 - added a while loop and take care of the multiple PD Groups scenario.
  SCGCQ00574041 - AIM (Agentless Inventory Manager) Issues
  SCGCQ00481284 - Typos in help content for profile VD for Write Policy
  SCGCQ00472196 - Profile based VD creation path incorrectly showing protect VD/secure VD checkbox when user clicks on drive selection criteria
  SCGCQ00471209 - config using 8PDs/16 partial VDs and all stripe sizes and HSPs does not restore
  SCGCQ00487936 - After creating a VD with UCM tool the manual configuration PD section still shows configured PDs as UG, and duplicates
  SCGCQ00495236 - Controller not seen in HII Browsercan after switching from EFI WebBIOS
  SCGCQ00505591 - Checking the Enclosure Management settings in HII causes the system to reboot.
  SCGCQ00475217 - Request to support 128 drives wihin single enclosure
  SCGCQ00468930 - UCM Phase 2 support
  SCGCQ00571579 - (Implemented) - Create a formset with classGUID that customer has provided. 
  SCGCQ00481277 - Request to change the help content for write policy in create VD form
  SCGCQ00415456 - Obtain the Physical Slot number from the PCI Bridge to which the Controller is connected.
  SCGCQ00557522 - System hang observed when the "PdInfo.userDataBlockSize" is set to 0
  SCGCQ00476607 - HII cannot assign partial space less than 1 GB
  SCGCQ00629813 - RSOD during POST after enabling SecureBoot - HEFU.ROM should report exact size of .EFI image
  SCGCQ00482099 - Typos in help content for profile VD for Write Policy
  SCGCQ00498521 - HII cannot create a VD using unconfigured good drives as long as PD locate is set on the drives
  SCGCQ00477863 - Obtain the Physical Slot number from the PCI Bridge to which the Controller is connected.
 BIOS 6.14.05.0
  SCGCQ00479507 - Getting memory conflict during boot 
  SCGCQ00455591 - Memory access issue when loading Ctrl R
  SCGCQ00495471 - OOB function corrupts EBDA area used by other server function
  SCGCQ00552308 - not allocating memory correctly when MR and iMR are in the same system
  SCGCQ00493680 - Optimize reading IO port in INT15h path
  SCGCQ00482283 - System reboots during IO because FW didn't receive permanent host memory from OpROM
  SCGCQ00503046 - OpROM is displaying incorrect value for the number of INT13h device it supports
  SCGCQ00559094 - Provide an option to limit the max number of INT 13h devices presented to system BIOS
  SCGCQ00466276 - Check the controller status bit in the function which hooks INT15
  SCGCQ00455597 - Allocate only two 64k
  SCGCQ00454086 - Add boundary checking when allocating EBDA and PMM memory for BIOS post.
  SCGCQ00504752 - OpROM is displaying incorrect value for the number of INT13h device it supports
  SCGCQ00460724 - Memory access issue for Mercury when loading Ctrl R
  SCGCQ00460725 - Memory allocation: Allocate only two 64k
  SCGCQ00501253 - OOB function corrupts EBDA area used by other server function
 Ctrl-R 5.03-0005
  SCGCQ00485184 - Change Emergency Spare to NONE with enable emergency on Smarter checked will fail with error=03
  SCGCQ00487220 - ctrl-r dosent list all the drives to do replace drive.
  SCGCQ00487602 - Power savings button not enabled on Ctrl-R
  SCGCQ00490688 - ctrl-H doesn't list the drives to do replace drive while doing copyback in PD MGmt Screen
  SCGCQ00490789 - Selecting "Manage Link Speed" in CTL+R causes Fatal Error with SAS 9343-4i
  SCGCQ00493479 - Implemented the safe mode in Ctrl-R
  SCGCQ00518579 - Unable to make R10 through Ctrl R using 4k drives
  SCGCQ00593396 - Default (Initial) setting of VD doesn't reflect MFC's setting
  SCGCQ00606717 - /c0/pall show and Linkspeed information is not in same in Ctrl-R.
  SCGCQ00601637 - Changes in BIOS mode (pause on error) to be in sync
  SCGCQ00601691 - Need to display controller memory in Control-R
  SCGCQ00568108 - showing "BIOS Mode" in both the pages of ctrl mgmt
  SCGCQ00568688 - Help content is not updated with the Key stroke added
  SCGCQ00573077 - VD Erase will be disabled in Ctrl+R when Initialization on particular VD
  SCGCQ00579583 - Write policy is not added with writeback with BBu when MFC is set
 BootBlock 3.02.00.00-0000
  SCGCQ00288393 - iMR boot Block code initial changes
  SCGCQ00322313 - Errbios load fails on Fury adapters
  SCGCQ00337925 - Merged 6.0 boot block changes to 6.1
  SCGCQ00313425 - Bootblock is using NVRAM data even if NVRAM is uninitialized
  SCGCQ00371801 - Configure chip reset to link down
  SCGCQ00375108 - Added the code to enable OCM RMW errors
  SCGCQ00505902 - Coherency bit is disabled in SRAM TLBs
 NVDATA 3.1310.00-0070
  Numerous changes for specific customers
 FCODE 4.16.08.00
  SCGCQ00553069 - PCLI(1.07.05) Sparc: Command "cli set securitykey=L
  SCGCQ00471703 - Fcode CLI support for Invader (MR only)
  SCGCQ00486355 - Define and use capability bit to identify the StorCLI
 PCLI 1.07.05
 ROMENV 1.09

----------------------------------------------------------
Package: 24.1.1-0006 (MR 6.1)
 Firmware 4.210.50-3015
  SCGCQ00383439 - fix for the defect - 4k drives display wrong value of Coerced size.
  SCGCQ00573649 - JBOD mode drive cannot be set as Bootdrive when Only JBOD Mode drive exist in MR6.1
  SCGCQ00563950 - Fix for Infinite retries of command for sense code 0B/47/03
  SCGCQ00523831 - controller does not boot after Cache Offload
  SCGCQ00521575 - (Resolved) - LSI BIOS POST displays F/W initialized percentage greater than 100% i.e 106%
  SCGCQ00452322 - FW throws "MPT_LogDiscoveryErrors: SAS_TOPOLOGY_MAX_TOPO_PHYS_EXCEED" when connect 2 enclosures in multi-path
  SCGCQ00448575 - Fix coverity defect 13424
  SCGCQ00448009 - Defect Fix for Exception in Core 0
  SCGCQ00440474 - MISCOMPARES FOUND DURING COPYBACK
  SCGCQ00433521 - boards have issue in bootup after the wait time was increased in finding the ONFI flash configuration
  SCGCQ00426148 - Fix the unhandled interrupt by minimizing the critical interrupt
  SCGCQ00422673 - FW hit Montask with line 782, L2/L3 cache error when one drive is pulled out from enclosure
  SCGCQ00421805 - Changes to SMARTerEnabled and SSDSMARTerEnabled are not reflected in controller properties
  SCGCQ00420102 - fw breaks into montask on transporting ONFI module from 4i contoller
  SCGCQ00419935 - Change IO time out value to 20 seconds for FW initiated IOs
  SCGCQ00415989 - Modify the code to support tty dump in interrupt context
  SCGCQ00413690 - MSM freezes until full initialization completes when configuration created
  SCGCQ00349837 - Sequential Read performance is less on CacheCade associated LD's.
  SCGCQ00567996 - ECC Errors in tty logs
  SCGCQ00550456 - removing the cset   SCGCQ00550153: Identifying the DDR, ONFI flash and SCap combination
  SCGCQ00456094 - Data Corruption seen upon OCR after injecting Medium Error on Metadata of one Drive of R0 WB CCVD
  SCGCQ00455015 - Unblock 4G DDR support for OEM controllers
  SCGCQ00454330 - Capacitance value as 0% for Supercap FBU03 even though capacitor is fully charged
  SCGCQ00451378 - Data corruption on Raid 6 volume while running smash raw io on 63 volume
  SCGCQ00448581 - Coverity Defect Fix
  SCGCQ00442609 - NVCache fails on sCapMaxESRThreshold exceeds after a battery relearn
  SCGCQ00435532 - CC SRAM optimization using overlapped sections in SRAM
  SCGCQ00433463 - Insertion of the boot messages and the evets for montoring the ONFI backup capacity.
  SCGCQ00427452 - Indifference between MR.H and FW implementation for lockKeyLength
  SCGCQ00427326 - Boot block Version is not displayed in CTRL+R
  SCGCQ00421908 - Remove NO_RETENTION flag as it is not used
  SCGCQ00418459 - Assertion failure observed after reconstruction over from R0 to R5
  SCGCQ00408827 - Raise priority of pci config trap interrupt to critical
  SCGCQ00396609 - Remove 4K toggle code to enable 4K support PR in 6.1.
  SCGCQ00558428 - Rebuild and Consistency Check aren't processed when it is executed by CTL+R
  SCGCQ00455583 - Memory battery problem seen while corrupting both the banks at alternative address in 8G Ptolemy.
  SCGCQ00452094 - Small Sequential Reads and Writes are lower than TB
  SCGCQ00450489 - replacePack bit is set to 1, still FW gives the battery(FBU03) status as optimal when apps queries the status
  SCGCQ00446931 - Firmware Version incorrectly displayed
  SCGCQ00446104 - MR: on doing cache offload and restore, the data loss is seen
  SCGCQ00427451 - bootMsgPending.needsEKM bit is not set when FW needs a key
  SCGCQ00423468 - ONFI: Reducing the onfi initialize time from 7sec to 2sec
  SCGCQ00422566 - Foreign config import fails with pinned cache when VD is migrated from one controller to another controller
  SCGCQ00415034 - Watchdog timer excetpion in core 1
  SCGCQ00413263 - Online R6 VD became offline after another R5 VD was removed during IO with a CC2.0 VD
  SCGCQ00412599 - Configuring SBR for operating DDR at 800MHz does not work
  SCGCQ00412591 - Removal of CacheCade VD causes Hang during foreign import reports Command block Data structure issue
  SCGCQ00408922 - Enable watchdog timer
  SCGCQ00396711 - FirmWare hitting Montask with PL fault(0000d115) while trying to create R5 vd on 3drives powersavemode
  SCGCQ00396324 - Defect fix for Montask ../../raid/mem.c at line 280
  SCGCQ00442641 - Defect fix for VD rebuild doesnot kickin and goes to foreign state after reboot
  SCGCQ00435715 - Loss or corruption of meta data information declares nvcache as bad and move from WB to WT
  SCGCQ00417354 - Firmware broke @ 639 in file ../../raid/routines for reading the puctured LBAs due to Reference Tag in PI enabled LDs.
  SCGCQ00415844 - Defect Fix for Montask Observed during cable pull/push
  SCGCQ00414361 - Inverted check for flush completion in L3CacheFlushAll
  SCGCQ00451974 - Unit attention for a FP IO is not handled
  SCGCQ00447956 - Recon progress shows improper estimated time left .
  SCGCQ00436260 - To resolve Failure of skinny compilation
  SCGCQ00415677 - Two different VDs getting same target IDs on MR controller and FW hangs
  SCGCQ00391804 - Firmware crash (MonTask: line 416 in file ../../dm/mpt2/mptrec.c) on reboot after installing ESX4.1U3 on VD
  SCGCQ00390068 - ONFI error hit when 4K sector PDs were used in CacheCade testing.
  SCGCQ00411644 - PD state changes from JBOD to Unconfigured Good across reboots for certain PDs
  SCGCQ00392627 - verification of error cases handling issues
  SCGCQ00434812 - Rebuild starts automatically on drive with foreign config after reboot
  SCGCQ00436221 - For certain OS versions, returning ASCQ=0 for TUR for an offline VD casues the storage stack to keep issuing SSU and TUR commands
  SCGCQ00441021 - Term log capture to include the RAID-Key phase of the boot
  SCGCQ00567340 - Add event in FW to indicate that an INIT operation was halted due to reboot or other failure 
  SCGCQ00394433 - Invader Boot Volumes
  SCGCQ00447612 - Cobra EDFB write performance not scaling to 6400MB/s for IOs > 32k
  SCGCQ00434810 - Enable OCR by default in all pre-GCA builds for OEM 
  SCGCQ00395865 - Transition of defect id   SCGCQ00393644 from MR_FW_SAS3_6.0 to MR_FW_SAS3_6.1
  SCGCQ00413395 - Sequential Read performance is less on CacheCade associated LD's.
  SCGCQ00420689 - BBU Charging gets disabled when Transparent Relearn fails to start due to low capacity
  SCGCQ00420710 - Implementing code review comments
  SCGCQ00420713 - Ability to power off and on individual HDD
  SCGCQ00420732 - Implementing code review comments for code collaborator review #14994
  SCGCQ00420739 - Firmware is sending totalElapsedSecs value as 0 for LD and PD progresses
  SCGCQ00420745 - 5.7 ‘Static Code Analysis Tool’ changes
  SCGCQ00420749 - MonTask: line 281 in file ../../raid/mem.c if running megacli AdpDiag
  SCGCQ00420767 - ‘Static Code Analysis Tool’ warnings 10071, 10100, 10162, 10174, 10288, 10332, 10361, 10363, 10503
  SCGCQ00433405 - Auto Foreign import fails when controller is booted with pinned cache.
  SCGCQ00434144 - Alarm continues to sound after copy-back is done, across reboot, from an unconfigured good drive that is used as an emergency spare.
  SCGCQ00434149 - Change RAID controller FW bad battery warning message that comes up during POST.
  SCGCQ00434151 - Setting the ASO key with storcli 1.02.08 (MegaCli 8.07.06) fails with an error code 3 on Windows or Linux if the MB BIOS PCI
  SCGCQ00434185 - Application could not make a JBOD bootable without a VD present
  SCGCQ00435943 - user is able to associate a DIF enabled VD to Cachecade
  SCGCQ00449870 - static variable used in PD Progress and LD Progress function which may affect multiple progresses running at the same time.
  SCGCQ00549466 - Cache Memory Size of controller Information is ZERO
  SCGCQ00549468 - Controller Reset due to Fatal Error with RAID6/60 configuration
  SCGCQ00550153 - Identifying the DDR, ONFI flash and SCap combination
  SCGCQ00550337 - Baseboard Management Controller (BMC): STP passthru command failure
  SCGCQ00556151 - SLES 11.3 x64 Halts when Loading Kernel During Warm Reboot Stress
  SCGCQ00558049 - MR 4K Validation : 4K VD assigned to 512K CacheCade
  SCGCQ00562722 - MR_6.2 Storlib : SMPpassthru is not happening through storlib.
  SCGCQ00562793 - Unable to create another Virtual Drive when pulling first drive (degrading) in partial Virtual Drive where all drives are configured
  SCGCQ00571048 - Elapsed Seconds displayed in firmware logs for background operations progress is improper
  SCGCQ00384606 - Assertion failure in ../../raid/raidpci.c at line 10011 , while running IO with medium errors on arrays.
  SCGCQ00420692 - The reliability and error recovery of the SuperCap firmware was improved.
  SCGCQ00420747 - ‘Static Code Analysis Tool’ code changes
  SCGCQ00420750 - ‘Static Code Analysis Tool’ Fixes: 10463, 10513, 10591, 10592
  SCGCQ00420760 - Delete VD while PR still in progress cause debugger to loop. Reboot the system, debugger still loops
  SCGCQ00423453 - Adding check to prevent WT->WB property update for SSC VD when enableSSCWB is 0
  SCGCQ00434184 - Skinny firmware does not progress background operations with certain systems when using WebBIOS in legacy mode
  SCGCQ00454467 - Stressing test on degrade raid with UNC drives or rebuilding on UNC drives will cause firmware hang
  SCGCQ00498743 - Don't interpret the cachecade BVD flags if the volume is created with old FW which does not support cachecade.
  SCGCQ00518877 - LSI_MR Controllers fails to set "FACTORY SETTINGS"
  SCGCQ00562792 - Incorrect variable type in MR Read/Modify/Write path
  SCGCQ00394788 - Firmware blocked firmware download to interposer
  SCGCQ00420686 - Firmware returns invalid data in OOB packet
  SCGCQ00420716 - T-bolt firmware : ECC memory error boot message and event log enhancement.
  SCGCQ00420757 - "Question value mismatch with Option Value" message in HII's Controller Management when in Safe Mode with pin cache
  SCGCQ00420764 - Grammatical spacing error in bios message at POST
  SCGCQ00420771 - HII /When user has a critical message and the conrtoller is in Safe Mode, going into CTRL mang will result an error msg
  SCGCQ00433450 - FW halts when you have pinned cahce and remove VD form the configuration.
  SCGCQ00452019 - Virtual drive configurations go missing during firmware upgrade from 5.3 to 5.7
  SCGCQ00454364 - OEM facing with incorrect SAS HDD's indication, MSM shows 2X drives connected
  SCGCQ00458466 - ONFI Coverity defects : 13414,13415,13416,13417,13418,13419,13420,13421,13422
  SCGCQ00558941 - Running out of free entries in task list due to recursive addition of tasks
  SCGCQ00420725 - 4K sector support - iMR, analyze all remaining hard-coded instances of "512"
  SCGCQ00434153 - Disable Band Gap feature for select customers
  SCGCQ00441739 - Allow Type2 DIF drive as JBOD drives
  SCGCQ00450979 - Incase of HW failure move to WT mode and also error case handling of flash tables
  SCGCQ00420724 - Port latency outlier fixes to FW (from legacy PR137246)
  SCGCQ00420753 - Fix code collaborator coding standard related comments for Review #18196.
  SCGCQ00432857 - Saved Release Note DataSLIB returning bad data as good data after host reboots
  SCGCQ00417871 - montask hit at the line "Fatal firmware error: Line 1057 in ../../dm/src/dm.c while running copyback
  SCGCQ00420744 - Provide Fastpath as a standard offering for TB based controllers
  SCGCQ00434156 - OEM- StorCli should not allow turning on JBOD in MR mode
  SCGCQ00436903 - Minimum Capacity needed for relearn is incorrect in 2208 MR FW
 UEFI_Driver 0x06010600
  SCGCQ00478652 - Block IO tests from SCT IHV test suite failed
  SCGCQ00435384 - UEFI System hang if controller FW is in fault state
  SCGCQ00404216 - Add 3008 device ID for iMR product.
  SCGCQ00392836 - LSI to Support Remote Key Management
  SCGCQ00436609 - add PnPID's for 3004 and 3108
  SCGCQ00479016 - Disable Debug print in UEFI Driver
  SCGCQ00484085 - platfrom has UEFI hang when SATA is connected
  SCGCQ00477705 - 9240/9260/9270 UEFI driver issue with platforms when user having 2TB or 4TB VD
  SCGCQ00484113 - Follow UEFI Spec on interpreting In and Out Transfer Length that upper layer sends
 Hii 03.03.10.00
  SCGCQ00415826 - UCM Driver - unable to create an 8PD R5
  SCGCQ00420950 - empty warning prompt is given when creating a CacheCade VD with forced writeback option
  SCGCQ00421615 - BBU information and propererties are not displayed in HII browser 
  SCGCQ00421618 - HII Manage Foreign Configuration menu is not available when a foreign lockeddrive is present in the configuration.
  SCGCQ00423622 - Tool to generate VFR
  SCGCQ00423659 - UCM - Virtual Drive Configuration summary does not report the "Interface Type"
  SCGCQ00431622 - Navigation issue from Enable Drive Security form
  SCGCQ00422725 - HII doesn not allow user to use the remain free capacity to configure additional VD for R50/R10.
  SCGCQ00427518 - HII failed to allow user to use the remains free capacity for R1 VD with 2 plus TB capacity.
  SCGCQ00431231 - Hii enter black screen/timeout when user switching between fields/form sub_form to create R10 VD
  SCGCQ00432915 - Hii failed to report warning that inappropriate drives are picked to config R10 VD.
  SCGCQ00419159 - New Field "package version" in Controller Management
  SCGCQ00441850 - Profile based configuration help issues
  SCGCQ00443864 - When creating an invalid argument in HII during VD creation and after correction, save is grayed out
  SCGCQ00437500 - Hii failed to report error warning when config 2pds R10 with different drive capacity.
  SCGCQ00452128 - HII cannot assign partial space less than 1 GB
  SCGCQ00472196 - Profile based VD creation path incorrectly showing protect VD/secure VD checkbox when user clicks on drive selection criteria
  SCGCQ00452128 - HII cannot assign partial space less than 1 GB
  SCGCQ00477863 - Obtain the Physical Slot number from the PCI Bridge to which the Controller is connected.
  SCGCQ00482099 - Typos in help content for profile VD for Write Policy
 BIOS 6.13.00.1
  SCGCQ00455591 - Memory access issue for OEM when loading Ctrl R
  SCGCQ00559094 - Provide an option to limit the max number of INT 13h devices presented to system BIOS
  SCGCQ00455597 - Memory allocation: Allocate only two 64k
  SCGCQ00504752 - OpROM is displaying incorrect value for the number of INT13h device it supports
  SCGCQ00501253 - OOB function corrupts EBDA area used by other server function
 Ctrl-R 5.01-0005
  SCGCQ00413334 - Ctrl+R- Shows 'Power Save Mode for Configured drives' as 'Enabled' for iMR Fury controller
  SCGCQ00419980 - CtrlR shows option to create VDs even after configuring 16VDs in one DG.
  SCGCQ00436692 - Implemented the old PR LSIP200082262 with this ER in Ctrl-H
  SCGCQ00442610 - Firmware crashed @Line 244 in ../../raid/1078int.c for entering into CTRL-R with Pinned cache in R60 and R6.
  SCGCQ00461680 - ctrlR display "cache offload" as a premium feature at the place of "safe secure" feature.
  SCGCQ00461965 - Unable to silence the alarm
  SCGCQ00468676 - Aligning with FW for strip calculation for 4K drives
  SCGCQ00461544 - Unable to Activate the Premium feature with PFK in Ctrl+R
  SCGCQ00472563 - not able to create r0 WB cachecade VD in ctrl-R
  SCGCQ00497771 - Selecting "Manage Link Speed" in CTL+R causes Fatal Error with SAS 9343-4i
  SCGCQ00497772 - Power savings button not enabled on Ctrl-R
  SCGCQ00558344 - Boot error handling settings are not consistent for HII and CTL-R
  SCGCQ00558359 - Added a shortcut Ctrl+S which saves the changes and refreshes the page.  
  SCGCQ00565105 - Implemented to list all 4 BIOS modes
 FCODE 4.14.05.00
 NVDATA 3.1310.00-0062
  Numerous changes for specific customers
 BootBlock 3.00.00.00-0009
 ROMENV 1.09

----------------------------------------------------------
Initial Release:
Package: 24.0.2-0013 (MR 6.0.1) 
 Firmware 4.200.20-2839
 UEFI_Driver 0x06000500
 Hii 03.02.11.01
 BIOS 6.12.00
 Ctrl-R 5.00-0007
 BootBlock 3.00.00.00-0009
 NVDATA 3.1304.00-0039
 FCODE 4.12.05.00
 ROMENV 1.09


*Third-party trademarks are the property of their respective owners.


