================================================================================
Intel(R) Server Board S2600GZ/GL, Intel(R) Server System R1000GZ/GL Product Family and
Intel(R) Server System R2000GZ/GL Product Family Firmware Update Package
for Intel(R) Deployment Assistant, Intel(R) One Boot Flash Update Utility, 
The embedded EFI Shell, Windows* Preboot Execution Environment 
================================================================================
Intel(R) Server Boards and Systems
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================
DATE    : 	April , 29 2014
TO      : 	Intel(R) Server Board S2600GZ/GL, Intel(R) Server System R1000GZ/GL 
                Product Family and Intel(R) Server System R2000GZ/GL Product Family
                customers
SUBJECT : Release Notes for System Firmware Update Package 
================================================================================
                              ABOUT THIS RELEASE
================================================================================
BIOS   : 02.02.0002
ME     : 02.01.07.328
BMC    : 01.20.5793
FRUSDR : 1.12
================================================================================
                           Support Platforms and Dependency
================================================================================
Processors supported: 
Intel(R) Xeon processor E5-4600/2600/2400 series
Intel(R) Xeon processor E5-4600/2600/2400 v2 series

Microcode update versions:
Intel(R) Xeon processor E5-4600/2600/2400 series C0 stepping: 0x00000513 CPUID = 0x206D5
Intel(R) Xeon processor E5-4600/2600/2400 series C1 stepping: 0x00000619 CPUID = 0x206D6
Intel(R) Xeon processor E5-4600/2600/2400 series C2 stepping: 0x00000710 CPUID = 0x206D7
Intel(R) Xeon processor E5-4600/2600/2400 v2 series C0/C1 stepping: 0x00000416 CPUID = 0x306e4

Production boards:
  Product		Fab Version	      
  S2600GZ/GL	Fab3 or above     

The following update process must be followed to ensure a trouble free update.
1.	BMC firmware
2.	BIOS
3.	Manageability Engine (ME) firmware
4.	FRUSDR

================================================================================
                  System Firmware Update Package Usage instructions                   
================================================================================
This package can be updated using one of the following methods:
 - The embedded UEFI shell
 - Intel(R) Deployment Assistant
 - Windows* or Linux* operating system using Intel(R) One-boot Flash Update (OFU)
   V11.0 Build 15 or later)
 - Windows* Preboot Execution Environment (WinPE)

To update from the embedded EFI Shell

Update system firmware from Intel server EFI shell by the following steps:
- Download Intel server system firmware update package from http://downloadcenter.intel.com/
- Unzip package and copy all files to root folder in USB flash drive 
- Insert USB flash drive to server USB port
- Reboot server, system will start BIOS/BMC/FRUSDR update automatically

  If the unzipped package is not under the root folder of USB flash drive:
- Reboot server to EFI shell manually
- Run command "map -r" in EFI shell to find the mount point of the USB flash drive
- The USB flash drive may mount to fs0: or fs1: or other. 
- Run command "fs0:" or other to change folder to USB flash drive, 
- Change folder to the folder storing the firmware package
- Run command "startup.nsh" to start firmware update process

Please refer to "EFI_Instructions.pdf" in this firmware package for a quick guide to 
use the EFI commands

To Update from Intel(R) Deployment Assistant (IDA)

The Intel(R) Deployment Assistant software is easy to use and is present on the 
"Intel(R) Server Deployment & Management" DVD shipped with the system.
User can download the latest version IDA CD ISO image from http://downloadcenter.intel.com/
To use the IDA CD to update the system firmware:
- Boot server with IDA CD
- Select "Get System Updates" 
- Choose one of the three options 

  . From http://www.intel.com/support/
    Automatically downloads the latest Firmware Update Package from Intel 
    Requires Internet connection
    Enter your local IP address and proxy configuration
    Click "Next" to start the download and update process

  . From my network
    Download the latest Firmware Update Package from http://downloadcenter.intel.com/ and copy 
    it to a Windows* shared folder
    Enter your local IP address, the Windows* file server name, and a
    Windows user name and password
    Select the firmware package in pop-up window
    Click "Next" to start the update process

  . From USB flash drive or Hard Disk
    Download the latest Firmware Update Package from http://downloadcenter.intel.com/ and copy it 
    to a USB flash drive, then insert the USB flash drive into the server USB port
    Click "Browse"
    Select the firmware package in pop-up window
    Click "Next" to start the update process
    
  Note: The Firmware Update Package is in the ZIP file format. Do not unzip 
        before copying to a Windows* shared folder or USB flash drive.

To update from Windows* and Linux* or operating systems using the Intel(R) One Boot
Flash Update Utility (OFU)

Intel(R) One boot Flash Update utility can be downloaded from http://downloadcenter.intel.com/
and it is part of the "BIOS, Firmware Update & Configuration Utilities" for 
Windows* and Linux*. Please refer to Intel OFU user guide about the details of 
installation and usage of OFU.

Use OFU to update system firmware by the following steps:
- Install OFU on Windows* or Linux* system
- Download the latest firmware update package from http://downloadcenter.intel.com/
- Unzip package to a folder
- Run the following command in Windows* command line/Linux* terminal window:
  <OFU install folder name>:\flashupdt -u  <package folder name>\flashupdt.cfg
                       
To update from Windows* Preboot Execution Environment (WinPE)

The System Firmware Update Package can be inserted to Windows* PE customized image 
for creating a bootable Windows* PE CD. User is able to update system firmware from 
customized WinPE CD by the following steps:
- Boot server with customized WinPE CD
- Run script "WinPE21_x64_Update.bat" or "WinPE20_x86_Update.bat" 
  (name may be varied depends on your own customization)
  
Note:
1. The Intel(R) OFU utility is case sensitive. Therefore, when you transfer the 
Firmware Update Package using USB flash drive from a Microsoft Windows* system to a Linux
environment, you must first extract under the Linux* environment. Otherwise, you 
will need to mount the USB flash drive manually with 'vfat' option under Linux to avoid 
conversion from upper case to lower case and vice versa.

2. To make Intel(R) OFU utility run properly under x86 or x64 OS, you have to read
OFU release notes on known issues for OFU installation.

3. In this SFUP package, Intel only provide batch file "WinPE_x86_Update.bat"
for WinPE2.0 32 bit solution "WinPE_x64_Update.bat" for WinPE2.1/3.0 64 bit 
solution as an example. Please refer to white paper "White Paper-Intel Server 
Utilities Procedure for WinPE.pdf" for details on building your own customized 
WinPE CD.

4. Windows PE 2.0 - built from Windows Vista SP1 32bit or EM64T
5. Windows PE 2.1 - built from Windows Vista SP1 or Windows Server 2008, EM64T
6. Windows PE 3.1 - built from Windows Server 2008R2, EM64T
7. Microsoft IPMI driver is loaded by default from WinPE CD, if you want to use 
Intel IPMI driver instead of MS IPMI driver for firmware update, you can un-install
Microsoft IPMI driver by:
                Devicesetup.exe ¨Cv remove *IPI0001
                Note: IPI0001 is the device ID for Microsoft IPMI driver.

=================================================================================   
 				BIOS 02.02.0002
=================================================================================
- Fixed: The system can't power up after restoring the BIOS default value via removing the
         CMOS battery

================================================================================
                     		ME 2.01.07.328 release
================================================================================
- Fixed: Platform is not able to power on properly after being shut down by NM
         Policy
- Fixed: Global platform power consumption reported by NM Statistics in S5 is
         incorrect
- Fixed: OOB (out-of-band) stress test by issuing the wrong username may cause
         connection to be unavailable
- Fixed: Shutdown action can be interrupted by cold reset when volatile NM
         policy is in use
===============================================================================
                                BMC 01.20.5793
===============================================================================
- Fixed: Cold Redundant Power Supply Configuration Issue, fix it by a DPS 750XB 
         A PSU v100 image.
- Fixed: The Embedded Web Console was showing the incorrect version of ME
         Firmware when the ME was in firmware update mode.
- Fixed: Nothing displayed on the Embedded Web Console while logging in with an
         IPv6 address (stateless ICMPv6 discovery).
- Fixed: BMC Embedded Web Console session not maintained with a power cycle
- Fixed: System does not maintain BMC web console session during power
         state change or system reset.
- Fixed: The Intel(R) Xeon(R) Phi(TM) Coprocessor adapters numbering is not
         consistent with riser slot numbering on server board.
- Fixed: Embedded Web Console SEL text log not decoding BIOS update versions
         correctly.
- Fixed: No video display in BMC KVM when SUT wakes up from S1 or S3 in 
         Windows* 2012.
- Fixed: S2600IP - Intel(R) Xeon(R) Phi(TM) Coprocessor adapter MIC Status 7
         shows as Unknown in some configurations.
- Fixed: S2600GZ - Intel(R) Xeon(R) Phi(TM) Coprocessor adapter MIC Status
         Sensor shows "Unknown" when only 1 MIC card exists in system.
- Fixed: Cannot set link-local gateway for BMC Network Management Interface
         using IPv6.
- Fixed: [X] Web Console not defaulting to English when another non-English
         browser is detected.
- Fixed: Add Cross Frame Options to prevent cross-frame scripting of Embedded
         Web Console
- Fixed: Browser autocomplete enabled before authentication.
- Fixed: SMI Timeout errors not logging IIO Global error registers in Debug Log
- Fixed: BMC LAN connection not working after IP address change.
- Fixed: Multi-node boards with node ID 1111 are not regarded as a single node.
- Fixed: BMC email alerts refused by some servers.
- Fixed: IP address of baseboard management NIC can't be configured
         successfully when dynamic and static IP changed.
- Fixed: The baseboard management NIC can't get a dynamic IP address when the
         VLAN set as enable.
- Fixed: Change to 1600W PSU firmware for an acoustic issue.
- Fixed: POST Error code 0xA6A0 was causing the SEL page to fail to render.
         - Also fixes decode of POST Error code 0x0012 and invalid POST Errors
           causing the SEL page to fail to render.
- Fixed: The ME firmware has 2 minor versions in the update related SEL.
         Updated the OEM command format to support this.
- Added: Support Intel(R) Xeon(R) Phi(TM) Coprocessor adapters in Intel(R)
         Server Boards and Systems.
- Added: Added a button on Web to enable/disable IPMI over LAN.

================================================================================
                                   FRUSDR 1.12
================================================================================    
- Added FRU file for S2600GL and Updated Master.cfg
=============================================================================
                            LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products. 
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation may 
have patents or pending patent applications, trademarks, copyrights, or other 
intellectual property rights that relate to the presented subject matter.  
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any 
such patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product 
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 
*Other names and brands are the property of their respective owners.
Copyright (c) 2014 Intel Corporation.

A portion of this firmware is open source code, which falls under the
GPL 2.0 license.  

[END OF RELEASE NOTES]
