//****************************************************************************
//                   INTEL CORPORATION PROPRIETARY INFORMATION
//       This software is supplied under the terms of a license agreement or
//       nondisclosure agreement with Intel Corporation and may not be copied
//       or disclosed except in accordance with the terms of that agreement.
//         Copyright (c) 2013 - 2014 Intel Corporation. All Rights Reserved.
//****************************************************************************
//
// Data in this file is based on the S2600GZ/GL rev 7.1 FSC SDR spreadsheet.
//
// SDR tag usage

//====================================================================//
// (1) Chassis related TAG
//====================================================================//
// Chassis support tags:
//		R1000           = Supported 1U chassis
//		R2000           = Supported 2U chassis
//		R2224           = Supported 2U chassis(3 * 2U 8X2.5 HSBP)
//		R2312           = Supported 2U chassis(2U 12X3.5 HSBP)
//		R2XXX           = Supported 2U chassis(1 * 2U 8X2.5 HSBP or 2 * 2U 8X2.5 HSBP or 2U 8X3.5 HSBP)
//		R2AUXCOOL       = Supported 2U chassis w/ PCIe card thermal sensor
//              R2000FAMILY     = supported 2U chassis (All)
//		OTHER           = Supported OTHER chassis
//		OTHER_SR        = Supported OTHER(Slow Ramp) chassis
//		OTHER_MR        = Supported OTHER(Medium Ramp) chassis
//		OTHER_FR        = Supported OTHER(Fast Ramp) chassis
//		TEST_PLATE      = Open test plate
//
//====================================================================//
// (2) Processor related sensors
//====================================================================//
// Processor support tags:
//      PROCESSOR_2     = Second CPU in a dual processor system
//
//====================================================================//
// (3) HSBP device
//====================================================================//
// Hot Swap Backplane (HSBP) tags:
//		HSBP1_1U8X25    = F1U8X25HSBP
//		HSBP1_1U4X35    = FR1304HSBP
//		HSBP1_2U8X25    = FXX8X25HSBP
//		HSBP1_2U8X25DP  = FXX8X25DPBP
//		HSBP1_2U8X35    = F2U8X35HSBP
//		HSBP1_2U12X35   = F2U12X35HSBP
//		HSBP2_2U8X25    = 2nd FXX8X25HSBP
//		HSBP3_2U8X25    = 3rd FXX8X25HSBP
//
//====================================================================//
// (4) Fan sensors
//====================================================================//
//  Fan tags:
//      OTHER_FAN_1A        = System Fan 1A
//      OTHER_FAN_1B        = System Fan 1B
//      OTHER_FAN_2A        = System Fan 2A
//      OTHER_FAN_2B        = System Fan 2B
//      OTHER_FAN_3A        = System Fan 3A
//      OTHER_FAN_3B        = System Fan 3B
//      OTHER_FAN_4A        = System Fan 4A
//      OTHER_FAN_4B        = System Fan 4B
//      OTHER_FAN_5A        = System Fan 5A
//      OTHER_FAN_5B        = System Fan 5B
//      OTHER_FAN_6A        = System Fan 6A
//      OTHER_FAN_6B        = System Fan 6B
//      OTHER_PROC1_FAN     = Processor Fan 1
//      OTHER_PROC2_FAN     = Processor Fan 2
//====================================================================//
// (5) Power Supply related sensors
//====================================================================//
//  Power supply tags:
//      PS1_460W        = 460 Watt power supply module 1
//      PS1_750W        = 750 Watt power supply module 1
//      PS2_460W        = 460 Watt power supply module 2
//      PS2_750W        = 750 Watt power supply module 2
//      REDUNDANT_PS    = 2 power supplies installed so power redundancy sensor is supported
//      
//====================================================================//
// (6) Others
//====================================================================//
// Miscellanious support tags:
//      NON_STORE_FP    = Non-Storage Front panel temperature sensor
//      STORE_FP_V1     = Unmodified Storage Front panel temperature sensor
//      STORE_FP_V2     = Modified Storage Front panel temperature sensor
//      NO_INTRUSION    = Chassis does not support a intrusion switch
//      INTRUSION       = Chassis does support an intrusion switch
//      FP_NMI          = Front panel NMI button
//      R1000_RED_FAN   = R1000 Chassis supports fan redundancy
//      R2000_RED_FAN   = R2000 Chassis supports fan redundancy
//	RISER_1_FRU     = Riser 1 FRU device detected
//	RISER_2_FRU     = Riser 2 FRU device detected
//      FCT             = Functional Test (manufacturing)
//      FOQM            = Functional Outgoing Manufacturing Test (manufacturing)
//      SHIPPING        = Default shipping configuration which the baseboard should leave the factory with
//		NOT_USED        = Record is currently not used and will not be installed

//
// File Header Information
//

_LF_NAME       'S2600GZ.SDR'
_LF_VERSION    '1.13'
_LF_FMT_VER    '1.50'
_IPMI_VERSION  '2.00'

//
// SDR Header Information
//

_SDR (
_START_ADDR    0000
_DATA_LEN      0000
_NVS_TYPE      'IMBDEVICE'
_DEV_BUS       FF
_DEV_ADDRESS   20


//*****************************************************************************
//
// Miscellaneous core sensor data records 
//
//*****************************************************************************


_SDR_TYPE   02
_REC_LEN    002F

   // Sensor Record Header
   0100           // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   01                 // Sensor Number

   // Record Body Bytes
   15                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   09                 // Sensor Type
   6F                 // Event / Reading Base Type
   7500               // Assertion Event Mask
   7500               // Deassertion Event Mask
   7500               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Pwr Unit Status'  // String Bytes


_SDR_TYPE   02
_SDR_TAG    'REDUNDANT_PS'
_REC_LEN    002F

   // Sensor Record Header
   0200           // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   02                 // Sensor Number

   // Record Body Bytes
   15                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   09                 // Sensor Type
   0B                 // Event / Reading Base Type
   FF00               // Assertion Event Mask
   FF00               // Deassertion Event Mask (No Deassertion events)
   FF00               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Pwr Unit Redund'  // String Bytes   


_SDR_TYPE   02
_REC_LEN    002D

   // Sensor Record Header
   0300           // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   03                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   23                 // Sensor Type
   6F                 // Event / Reading Base Type
   0F01               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0F01               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'IPMI Watchdog'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'NO_INTRUSION'
_SDR_TAG    'SHIPPING'
_REC_LEN    002E

   // Sensor Record Header
   0400           // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   04                 // Sensor Number

   // Record Body Bytes
   17                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   05                 // Sensor Type
   6F                 // Event / Reading Base Type
   1000               // Assertion Event Mask
   1000               // Deassertion Event Mask
   1000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Physical Scrty'   // String Bytes


_SDR_TYPE   02
_SDR_TAG    'INTRUSION'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    002E

   // Sensor Record Header
   0500           // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   04                 // Sensor Number

   // Record Body Bytes
   17                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   05                 // Sensor Type
   6F                 // Event / Reading Base Type
   1100               // Assertion Event Mask
   1100               // Deassertion Event Mask
   1100               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Physical Scrty'   // String Bytes


_SDR_TYPE   02
_SDR_TAG    'FP_NMI'
_REC_LEN    002F

   // Sensor Record Header
   0600           // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   05                 // Sensor Number 

   // Record Body Bytes
   0C                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   13                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0100               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'FP NMI Diag Int'  // String Bytes


_SDR_TYPE   02
_REC_LEN    002B

   // Sensor Record Header
   0700           // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   06                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   F3                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'SMI Timeout'      // String Bytes


_SDR_TYPE   02
_REC_LEN    0030

   // Sensor Record Header
   0800           // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   07                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   10                 // Sensor Type
   6F                 // Event / Reading Base Type
   0400               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0400               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'System Event Log' // String Bytes


_SDR_TYPE   02
_REC_LEN    002C

   // Sensor Record Header
   0900           // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   08                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   12                 // Sensor Type
   6F                 // Event / Reading Base Type
   1000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   1000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'System Event'     // String Bytes


_SDR_TYPE   02
_REC_LEN    0026

   // Sensor Record Header
   0A00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   21                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   09                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   14                 // Sensor Type
   6F                 // Event / Reading Base Type
   0500               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0500               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C6                 // Type/Length Code
   'Button'           // String Bytes


_SDR_TYPE      03
_REC_LEN       001D

   // Sensor Record Header
   0B00           // Record ID
   51                 // SDR Version
   03                 // Record Type
   18                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0A                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   28                 // Sensor type
   03                 // Event/Reading Type Code
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'BMC Watchdog'     // String Bytes


_SDR_TYPE   02
_REC_LEN    002B

   // Sensor Record Header
   0C00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0B                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   02                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'VR Watchdog'      // String Bytes


_SDR_TYPE   02
_SDR_TAG    'R1000_RED_FAN'
_SDR_TAG    'R2000_RED_FAN'
_REC_LEN    002E

   // Sensor Record Header
   0D00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0C                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   04                 // Sensor Type
   0B                 // Event / Reading Base Type
   FF00               // Assertion Event Mask
   FF00               // Deassertion Event Mask
   FF00               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00				  // Reserved
   00	              // Reserved
   00       	      // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Fan Redundancy'   // String Bytes


_SDR_TYPE   02
_REC_LEN    002E

   // Sensor Record Header
   0E00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0D                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   01                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'SSB Therm Trip'   // String Bytes


_SDR_TYPE   02
_REC_LEN    002F

   // Sensor Record Header
   0F00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0E                 // Sensor Number

   // Record Body Bytes
   2C                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   15                 // Sensor Type
   08                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'IO Mod Presence'  // String Bytes
 
  
_SDR_TYPE   02
_REC_LEN    0030

   // Sensor Record Header
   1000           // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0F                 // Sensor Number

   // Record Body Bytes
   2C                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   15                 // Sensor Type
   08                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'SAS Mod Presence' // String Bytes


_SDR_TYPE   02
_REC_LEN    002D

   // Sensor Record Header
   1100           // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   10                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   28                 // Sensor Type
   6F                 // Event / Reading Base Type
   1000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   1000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'BMC FW Health'    // String Bytes


_SDR_TYPE   01
_REC_LEN    003E

   // Sensor Record Header
   1200           // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   11                 // Sensor Number

   // Record Body Bytes
   17                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   63                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   11                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   02                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   00                 // Analog characteristic flags
   00                 // Nominal Reading
   00                 // Normal Maximum
   00                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'System Airflow'   // String Bytes


_SDR_TYPE   03
_REC_LEN    0021

   // Sensor Record Header
   1300           // Record ID
   51                 // SDR Version
   03                 // Record Type
   1C                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   12                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   2B                 // Sensor type
   70                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'FW Update Status' // String Bytes


//*****************************************************************************
//
// Baseboard and chassis related temperature related sensors
//
//*****************************************************************************


_SDR_TYPE   01
_REC_LEN    003D

   // Sensor Record Header
   1400           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   20                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   3A                 // Nominal Reading
   69                 // Normal Maximum
   0A                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   73                 // Upper critical
   6E                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   05                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CD                 // Type/Length Code
   'BB P1 VR Temp'	  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'NON_STORE_FP'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    0040

   // Sensor Record Header
   1500           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   21                 // Sensor Number

   // Record Body Bytes
   0C                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   1C                 // Nominal Reading
   2D                 // Normal Maximum
   0A                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   37                 // Upper critical
   32                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   05                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   D0                 // Type/Length Code
   'Front Panel Temp' // String Bytes

_SDR_TYPE   01
_SDR_TAG    'STORE_FP_V1'
_REC_LEN    0040

   // Sensor Record Header
   1600           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   21                 // Sensor Number

   // Record Body Bytes
   0C                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   F8                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   29                 // Nominal Reading
   3F                 // Normal Maximum
   12                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   49                 // Upper critical
   44                 // Upper non-critical
   00                 // Lower non-recoverable
   08                 // Lower critical
   0D                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   D0                 // Type/Length Code
   'Front Panel Temp' // String Bytes

_SDR_TYPE   01
_SDR_TAG    'STORE_FP_V2'
_REC_LEN    0040

   // Sensor Record Header
   1700           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   21                 // Sensor Number

   // Record Body Bytes
   0C                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   F8                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   29                 // Nominal Reading
   3F                 // Normal Maximum
   12                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   49                 // Upper critical
   44                 // Upper non-critical
   00                 // Lower non-recoverable
   08                 // Lower critical
   0D                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   D0                 // Type/Length Code
   'Front Panel Temp' // String Bytes

_SDR_TYPE   01
_REC_LEN    0038

   // Sensor Record Header
   1800           // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   22                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   34                 // Nominal Reading
   5D                 // Normal Maximum
   0A                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   67                 // Upper critical
   62                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   05                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   C8                 // Type/Length Code
   'SSB Temp'		  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    003D

   // Sensor Record Header
   1900           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   23                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   3A                 // Nominal Reading
   69                 // Normal Maximum
   0A                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   73                 // Upper critical
   6E                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   05                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CD                 // Type/Length Code
   'BB P2 VR Temp'	  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    003D

   // Sensor Record Header
   1A00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   24                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   3A                 // Nominal Reading
   69                 // Normal Maximum
   0A                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   73                 // Upper critical
   6E                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   05                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CD                 // Type/Length Code
   'BB Vtt 2 Temp'	  // String Bytes


_SDR_TYPE   01
_REC_LEN    003D

   // Sensor Record Header
   1B00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   25                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   3A                 // Nominal Reading
   69                 // Normal Maximum
   0A                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   73                 // Upper critical
   6E                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   05                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CD                 // Type/Length Code
   'BB Vtt 1 Temp'	  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'IO_MODULE'
_SDR_TAG    'FCT'
_REC_LEN    003C

   // Sensor Record Header
   1C00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   26                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   28                 // Nominal Reading
   46                 // Normal Maximum
   0A                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   50                 // Upper critical
   4B                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   05                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CC                 // Type/Length Code
   'I/O Mod Temp'	  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'HSBP1_1U4x35'
_SDR_TAG    'HSBP1_1U8X25'
_SDR_TAG    'HSBP1_2U8X25'
_SDR_TAG    'HSBP1_2U8X25DP'
_SDR_TAG    'HSBP1_2U8X35'
_SDR_TAG    'HSBP1_2U12X35'
_REC_LEN    003B

   // Sensor Record Header
   1D00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   36                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   29                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   3A                 // Nominal Reading
   69                 // Normal Maximum
   0A                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   73                 // Upper critical
   6E                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   05                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CB                 // Type/Length Code
   'HSBP 1 Temp'      // String Bytes


_SDR_TYPE   01
_SDR_TAG    'HSBP2_2U8X25'
_REC_LEN    003B

   // Sensor Record Header
   1E00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   36                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   2A                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   3A                 // Nominal Reading
   69                 // Normal Maximum
   0A                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   73                 // Upper critical
   6E                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   05                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CB                 // Type/Length Code
   'HSBP 2 Temp'      // String Bytes


_SDR_TYPE   01
_SDR_TAG    'HSBP3_2U8X25'
_REC_LEN    003B

   // Sensor Record Header
   1F00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   36                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   2B                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   3A                 // Nominal Reading
   69                 // Normal Maximum
   0A                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   73                 // Upper critical
   6E                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   05                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CB                 // Type/Length Code
   'HSBP 3 Temp'      // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SAS_MODULE'
_SDR_TAG    'FCT'
_REC_LEN    003C

   // Sensor Record Header
   2000           // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   2D                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   28                 // Nominal Reading
   46                 // Normal Maximum
   0A                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   50                 // Upper critical
   4B                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   05                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CC                 // Type/Length Code
   'SAS Mod Temp'	  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PS1_460W'
_SDR_TAG    'PS1_750W'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   2100           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   2E                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0030               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   28                 // Nominal Reading
   46                 // Normal Maximum
   0A                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   55                 // Upper critical
   50                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   05                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Exit Air Temp'    // String Bytes


_SDR_TYPE   01
_REC_LEN    003C

   // Sensor Record Header
   2200           // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   2F                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   3C                 // Nominal Reading
   6E                 // Normal Maximum
   0A                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   78                 // Upper critical
   73                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   05                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM (25h is Modal Filtering with 5 samples)
   CC                 // Type/Length Code
   'LAN NIC Temp'     // String Bytes


//*****************************************************************************
//
// Fan tachometer sensors
//
//*****************************************************************************


_SDR_TYPE   01
_SDR_TAG    'R1000'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   2300           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   30                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3E                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   93                 // Nominal Reading
   FF                 // Normal Maximum
   27                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   1B                 // Lower critical
   1F                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 1A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'R1000'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   2400           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   31                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3C                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   94                 // Nominal Reading
   FF                 // Normal Maximum
   29                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   1C                 // Lower critical
   21                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 1B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'R1000'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   2500           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   32                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   03                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3E                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   93                 // Nominal Reading
   FF                 // Normal Maximum
   27                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   1B                 // Lower critical
   1F                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 2A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'R1000'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   2600           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   33                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   04                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3C                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   94                 // Nominal Reading
   FF                 // Normal Maximum
   29                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   1C                 // Lower critical
   21                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 2B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'R1000'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   2700           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   34                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   05                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3E                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   93                 // Nominal Reading
   FF                 // Normal Maximum
   27                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   1B                 // Lower critical
   1F                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 3A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'R1000'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   2800           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   35                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   06                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3C                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   94                 // Nominal Reading
   FF                 // Normal Maximum
   29                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   1C                 // Lower critical
   21                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 3B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'R1000'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   2900           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   36                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   07                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3E                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   93                 // Nominal Reading
   FF                 // Normal Maximum
   27                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   1B                 // Lower critical
   1F                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 4A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'R1000'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   2A00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   37                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   08                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3C                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   94                 // Nominal Reading
   FF                 // Normal Maximum
   29                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   1C                 // Lower critical
   21                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 4B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'R1000'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   2B00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   38                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   09                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3E                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   93                 // Nominal Reading
   FF                 // Normal Maximum
   27                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   1B                 // Lower critical
   1F                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 5A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'R1000'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   2C00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   39                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0A                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3C                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   94                 // Nominal Reading
   FF                 // Normal Maximum
   29                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   1C                 // Lower critical
   21                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 5B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'R1000'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   2D00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   3A                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0B                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3E                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   93                 // Nominal Reading
   FF                 // Normal Maximum
   27                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   1B                 // Lower critical
   1F                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 6A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'R1000'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   2E00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   3B                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0C                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3C                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   94                 // Nominal Reading
   FF                 // Normal Maximum
   29                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   1C                 // Lower critical
   21                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 6B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'R2000'
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    003C

   // Sensor Record Header
   2F00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   30                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   31                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   99                 // Nominal Reading
   FF                 // Normal Maximum
   33                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   23                 // Lower critical
   28                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 1'     // String Bytes


_SDR_TYPE   01
_SDR_TAG    'R2000'
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    003C

   // Sensor Record Header
   3000           // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   32                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   31                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   99                 // Nominal Reading
   FF                 // Normal Maximum
   33                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   23                 // Lower critical
   28                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 2'     // String Bytes


_SDR_TYPE   01
_SDR_TAG    'R2000'
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    003C

   // Sensor Record Header
   3100           // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   34                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   03                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   31                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   99                 // Nominal Reading
   FF                 // Normal Maximum
   33                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   23                 // Lower critical
   28                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 3'     // String Bytes


_SDR_TYPE   01
_SDR_TAG    'R2000'
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    003C

   // Sensor Record Header
   3200           // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   36                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   04                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   31                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   99                 // Nominal Reading
   FF                 // Normal Maximum
   33                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   23                 // Lower critical
   28                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 4'     // String Bytes


_SDR_TYPE   01
_SDR_TAG    'R2000'
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    003C

   // Sensor Record Header
   3300           // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   38                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   05                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   31                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   99                 // Nominal Reading
   FF                 // Normal Maximum
   33                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   23                 // Lower critical
   28                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'System Fan 5'     // String Bytes


   
_SDR_TYPE   01
_SDR_TAG    'NOT_USED'
_REC_LEN    003F

   // Sensor Record Header
   3400           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   3C                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   31                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   8E                 // Nominal Reading
   FF                 // Normal Maximum
   1E                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   15                 // Lower critical
   18                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CF                 // Type/Length Code
   'Processor 1 Fan'  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'NOT_USED'
_REC_LEN    003F

   // Sensor Record Header
   3500           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   3D                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   31                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   8E                 // Nominal Reading
   FF                 // Normal Maximum
   1E                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   15                 // Lower critical
   18                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CF                 // Type/Length Code
   'Processor 2 Fan'  // String Bytes



_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_1A'
_REC_LEN    003D

   // Sensor Record Header
   3600           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   30                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   05                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 1A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_1B'
_REC_LEN    003D

   // Sensor Record Header
   3700           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   31                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   05                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 1B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_2A'
_REC_LEN    003D

   // Sensor Record Header
   3800           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   32                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   03                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   05                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 2A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_2B'
_REC_LEN    003D

   // Sensor Record Header
   3900           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   33                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   04                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   05                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 2B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_3A'
_REC_LEN    003D

   // Sensor Record Header
   3A00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   34                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   05                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   05                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 3A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_3B'
_REC_LEN    003D

   // Sensor Record Header
   3B00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   35                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   06                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   05                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 3B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_4A'
_REC_LEN    003D

   // Sensor Record Header
   3C00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   36                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   07                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   05                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 4A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_4B'
_REC_LEN    003D

   // Sensor Record Header
   3D00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   37                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   08                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   05                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 4B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_5A'
_REC_LEN    003D

   // Sensor Record Header
   3E00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   38                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   09                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   05                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 5A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_5B'
_REC_LEN    003D

   // Sensor Record Header
   3F00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   39                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0A                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   05                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 5B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_6A'
_REC_LEN    003D

   // Sensor Record Header
   4000           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   3A                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0B                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   05                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 6A'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_6B'
_REC_LEN    003D

   // Sensor Record Header
   4100           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   3B                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0C                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   05                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 6B'    // String Bytes

_SDR_TYPE   01
_SDR_TAG    'OTHER_PROC1_FAN'
_REC_LEN    003F

   // Sensor Record Header
   4200           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   3C                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   05                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CF                 // Type/Length Code
   'Processor 1 Fan'  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_PROC2_FAN'
_REC_LEN    003F

   // Sensor Record Header
   4300           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   3D                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   05                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CF                 // Type/Length Code
   'Processor 2 Fan'  // String Bytes

//*****************************************************************************
//
// Fan presence sensors (Only supported with hot-swappable fans)
//
//*****************************************************************************


_SDR_TYPE   02
_SDR_TAG    'R2000_HS_FAN'
_REC_LEN    002D

   // Sensor Record Header
   4400           // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   40                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   04                 // Sensor Type
   08                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Fan 1 Present'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'R2000_HS_FAN'
_REC_LEN    002D

   // Sensor Record Header
   4500           // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   41                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   04                 // Sensor Type
   08                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Fan 2 Present'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'R2000_HS_FAN'
_REC_LEN    002D

   // Sensor Record Header
   4600           // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   42                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   03                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   04                 // Sensor Type
   08                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Fan 3 Present'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'R2000_HS_FAN'
_REC_LEN    002D

   // Sensor Record Header
   4700           // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   43                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   04                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   04                 // Sensor Type
   08                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Fan 4 Present'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'R2000_HS_FAN'
_REC_LEN    002D

   // Sensor Record Header
   4800           // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   44                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   05                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   04                 // Sensor Type
   08                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Fan 5 Present'    // String Bytes


//*****************************************************************************
//
// Power supply sensors (Only supported with PMBus enabled power supplies)
//
//*****************************************************************************


_SDR_TYPE   02
_SDR_TAG    'PS1_460W'
_SDR_TAG    'PS1_750W'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    002A

   // Sensor Record Header
   4900           // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   50                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   08                 // Sensor Type
   6F                 // Event / Reading Base Type 
   4F00               // Assertion Event Mask
   4F00               // Deassertion Event Mask
   4F00               // Reading Mask &  Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'PS1 Status'       // String Bytes


_SDR_TYPE   02
_SDR_TAG    'PS2_460W'
_SDR_TAG    'PS2_750W'
_SDR_TAG    'FCT'
_REC_LEN    002A


   // Sensor Record Header
   4A00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   51                 // Sensor Number ok

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   08                 // Sensor Type
   6F                 // Event / Reading Base Type
   4F00               // Assertion Event Mask
   4F00               // Deassertion Event Mask
   4F00               // Reading Mask &  Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00          		  // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'PS2 Status'       // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PS1_460W'
_REC_LEN    003F

   // Sensor Record Header
   4B00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   54                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   03                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   56                 // Nominal Reading
   AC                 // Normal Maximum
   00                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   CC                 // Upper critical
   BC                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS1 Input Power'  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PS2_460W'
_REC_LEN    003F

   // Sensor Record Header
   4C00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   55                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   03                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   56                 // Nominal Reading
   AC                 // Normal Maximum
   00                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   CC                 // Upper critical
   BC                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS2 Input Power'  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PS1_750W'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003F

   // Sensor Record Header
   4D00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   54                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   04                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   66                 // Nominal Reading
   CC                 // Normal Maximum
   00                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   E6                 // Upper critical
   D9                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS1 Input Power'  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PS2_750W'
_SDR_TAG    'FCT'
_REC_LEN    003F

   // Sensor Record Header
   4E00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   55                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   04                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   66                 // Nominal Reading
   CC                 // Normal Maximum
   00                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   E6                 // Upper critical
   D9                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS2 Input Power'  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PS1_460W'
_REC_LEN    003E

   // Sensor Record Header
   4F00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   58                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   32                 // Nominal Reading
   64                 // Normal Maximum
   00                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   76                 // Upper critical
   64                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS1 Curr Out %'   // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PS2_460W'
_REC_LEN    003E

   // Sensor Record Header
   5000           // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   59                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   32                 // Nominal Reading
   64                 // Normal Maximum
   00                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   76                 // Upper critical
   64                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS2 Curr Out %'   // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PS1_750W'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003E

   // Sensor Record Header
   5100           // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   58                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   32                 // Nominal Reading
   64                 // Normal Maximum
   00                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   76                 // Upper critical
   64                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS1 Curr Out %'   // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PS2_750W'
_SDR_TAG    'FCT'
_REC_LEN    003E

   // Sensor Record Header
   5200           // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   59                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   32                 // Nominal Reading
   64                 // Normal Maximum
   00                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   76                 // Upper critical
   64                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS2 Curr Out %'   // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PS1_460W'
_REC_LEN    003F

   // Sensor Record Header
   5300           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   5C                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   1E                 // Nominal Reading
   3C                 // Normal Maximum
   05                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   46                 // Upper critical
   41                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS1 Temperature'  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PS2_460W'
_REC_LEN    003F

   // Sensor Record Header
   5400           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   5D                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   1E                 // Nominal Reading
   3C                 // Normal Maximum
   05                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   46                 // Upper critical
   41                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS2 Temperature'  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PS1_750W'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003F

   // Sensor Record Header
   5500           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   5C                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   1E                 // Nominal Reading
   3C                 // Normal Maximum
   05                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   46                 // Upper critical
   41                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS1 Temperature'  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PS2_750W'
_SDR_TAG    'FCT'
_REC_LEN    003F

   // Sensor Record Header
   5600           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   5D                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   1E                 // Nominal Reading
   3C                 // Normal Maximum
   05                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   46                 // Upper critical
   41                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS2 Temperature'  // String Bytes


//*****************************************************************************
//
// Additional hot-swap backplane (HSBP) hard disk drive status sensors
//
//*****************************************************************************


_SDR_TYPE   02
_SDR_TAG    'HSBP2_2U8X25'
_REC_LEN    002D

   // Sensor Record Header
   5700           // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   60                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   13                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 15 Status'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP3_2U8X25'
_REC_LEN    002D

   // Sensor Record Header
   5800           // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   61                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   11                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 16 Status'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP3_2U8X25'
_REC_LEN    002D

   // Sensor Record Header
   5900           // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   62                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   12                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 17 Status'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP3_2U8X25'
_REC_LEN    002D

   // Sensor Record Header
   5A00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   63                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   13                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 18 Status'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP3_2U8X25'
_REC_LEN    002D

   // Sensor Record Header
   5B00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   64                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   14                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 19 Status'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP3_2U8X25'
_REC_LEN    002D

   // Sensor Record Header
   5C00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   65                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   15                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 20 Status'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP3_2U8X25'
_REC_LEN    002D

   // Sensor Record Header
   5D00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   66                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   16                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 21 Status'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP3_2U8X25'
_REC_LEN    002D

   // Sensor Record Header
   5E00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   67                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   17                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 22 Status'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP3_2U8X25'
_REC_LEN    002D

   // Sensor Record Header
   5F00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   68                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   18                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 23 Status'    // String Bytes


//*****************************************************************************
//
// Processor (CPU) sensors
//
//*****************************************************************************


_SDR_TYPE   02
_REC_LEN    0029

   // Sensor Record Header
   6000           // Record ID
  51                 // SDR Version
   02                 // Record Type
   24                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   70                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   6F                 // Event / Reading Base Type
   8200               // Assertion Event Mask
   8200               // Deassertion Event Mask
   8200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'P1 Status'        // String Bytes


_SDR_TYPE   02
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0029

   // Sensor Record Header
   6100           // Record ID
   51                 // SDR Version
   02                 // Record Type
   24                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   71                 // Sensor Number ok

   // Record Body Bytes
   03                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   6F                 // Event / Reading Base Type
   8200               // Assertion Event Mask
   8200               // Deassertion Event Mask
   8200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'P2 Status'        // String Bytes


_SDR_TYPE   01
_REC_LEN    003F

   // Sensor Record Header
   6200           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   74                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   F1                 // Nominal Reading
   00                 // Normal Maximum
   BA                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'P1 Therm Margin'  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    003F

   // Sensor Record Header
   6300           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   75                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   F1                 // Nominal Reading
   00                 // Normal Maximum
   BA                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'P2 Therm Margin'  // String Bytes


_SDR_TYPE   01
_REC_LEN    003F

   // Sensor Record Header
   6400           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   78                 // Sensor Number 

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   00                 // Nominal Reading
   14                 // Normal Maximum
   00                 // Normal Minimum
   64                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   32                 // Upper critical
   1E                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'P1 Therm Ctrl %'  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    003F

   // Sensor Record Header
   6500           // Record ID
  51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   79                 // Sensor Number 

   // Record Body Bytes
   03                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   00                 // Nominal Reading
   14                 // Normal Maximum
   00                 // Normal Minimum
   64                 // Sensor Maximum Reading          
   00                 // Sensor Minimum Reading          
   00                 // Upper non-recoverable           
   32                 // Upper critical
   1E                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'P2 Therm Ctrl %'  // String Bytes


_SDR_TYPE   02
_REC_LEN    0027

   // Sensor Record Header
   6600           // Record ID
   51                 // SDR Version
   02                 // Record Type
   22                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   7C                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   41                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C7                 // Type/Length Code
   'P1 ERR2'		  // String Bytes


_SDR_TYPE   02
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0027

   // Sensor Record Header
   6700           // Record ID
   51                 // SDR Version
   02                 // Record Type
   22                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   7D                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   41                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C7                 // Type/Length Code
   'P2 ERR2'		  // String Bytes


_SDR_TYPE   02
_REC_LEN    0026

   // Sensor Record Header
   6800           // Record ID
   51                 // SDR Version
   02                 // Record Type
   21                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   80                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C6                 // Type/Length Code
   'CATERR'           // String Bytes


_SDR_TYPE   02
_REC_LEN    0030

   // Sensor Record Header
   6900           // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   81                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'P1 MSID Mismatch' // String Bytes


_SDR_TYPE   02
_REC_LEN    002B

   // Sensor Record Header
   6A00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   82                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'CPU Missing'      // String Bytes
 

_SDR_TYPE   01
_REC_LEN    0040

   // Sensor Record Header
   6B00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   83                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   F1                 // Normal Reading
   00                 // Normal Maximum
   BA                 // Normal Minimum
   00                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   0F                 // Upper critical
   0A                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   D0                 // Type/Length Code
   'P1 DTS Therm Mgn' // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0040

   // Sensor Record Header
   6C00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   84                 // Sensor Number

	 // Record Body Byte
   03                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   F1                 // Normal Reading
   00                 // Normal Maximum
   BA                 // Normal Minimum
   00                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   0F                 // Upper critical
   0A                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   D0                 // Type/Length Code
   'P2 DTS Therm Mgn' // String Bytes  


_SDR_TYPE   02
_SDR_TAG    'PROCESSOR_2'
_REC_LEN    0030

   // Sensor Record Header
   6D00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   87                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'P2 MSID Mismatch' // String Bytes


//*****************************************************************************
//
// Voltage regulator sensors
//
//*****************************************************************************


_SDR_TYPE   02
_REC_LEN    002A

   // Sensor Record Header
   6E00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   90                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   01                 // Sensor Type
   05                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'P1 VRD Hot'       // String Bytes


_SDR_TYPE   02
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    002A

   // Sensor Record Header
   6F00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   91                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   01                 // Sensor Type
   05                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'P2 VRD Hot'       // String Bytes


_SDR_TYPE   02
_REC_LEN    0030

   // Sensor Record Header
   7000           // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   94                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   01                 // Sensor Type
   05                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'P1 Mem01 VRD Hot' // String Bytes


_SDR_TYPE   02
_REC_LEN    0030

   // Sensor Record Header
   7100           // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   95                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   01                 // Sensor Type
   05                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'P1 Mem23 VRD Hot' // String Bytes


_SDR_TYPE   02
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0030

   // Sensor Record Header
   7200           // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   96                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   01                 // Sensor Type
   05                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'P2 Mem01 VRD Hot' // String Bytes


_SDR_TYPE   02
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0030

   // Sensor Record Header
   7300           // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   97                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   01                 // Sensor Type
   05                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'P2 Mem23 VRD Hot' // String Bytes


//*****************************************************************************
//
// Power supply fan tachometer sensors
//
//*****************************************************************************
   
//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PS1_460W'
_SDR_TAG    'PS1_750W'
_REC_LEN    002C

   // Sensor Record Header
   7400           // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   A0                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   00                 // Sensor Capabilities -- Manual Rearm
   04                 // Sensor Type - Fan
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Mask
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'PS1 Fan Fail'     // String Bytes

//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PS2_460W'
_SDR_TAG    'PS2_750W'
_REC_LEN    002C

   // Sensor Record Header
   7500           // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   A4                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   00                 // Sensor Capabilities -- Manual Rearm
   04                 // Sensor Type - Fan
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Mask
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'PS2 Fan Fail'     // String Bytes



//*****************************************************************************
//
// Memory thermal margin sensors
//
//*****************************************************************************


_SDR_TYPE   01
_REC_LEN    0040

   // Sensor Record Header
   7600           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   B0                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   EC                 // Nominal Reading
   00                 // Normal Maximum
   BA                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   0A                 // Upper critical
   05                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM used for filtering [7:5]= 1 Median [4:0]=5 Sample Count
   D0                 // Type/Length Code
   'DIMM Thrm Mrgn 1' // String Bytes


_SDR_TYPE   01
_REC_LEN    0040

   // Sensor Record Header
   7700           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   B1                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   EC                 // Nominal Reading
   00                 // Normal Maximum
   BA                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   0A                 // Upper critical
   05                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM used for filtering [7:5]= 1 Median [4:0]=5 Sample Count
   D0                 // Type/Length Code
   'DIMM Thrm Mrgn 2' // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_REC_LEN    0040

   // Sensor Record Header
   7800           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   B2                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   EC                 // Nominal Reading
   00                 // Normal Maximum
   BA                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   0A                 // Upper critical
   05                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM used for filtering [7:5]= 1 Median [4:0]=5 Sample Count
   D0                 // Type/Length Code
   'DIMM Thrm Mrgn 3' // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_REC_LEN    0040

   // Sensor Record Header
   7900           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   B3                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   EC                 // Nominal Reading
   00                 // Normal Maximum
   BA                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   0A                 // Upper critical
   05                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM used for filtering [7:5]= 1 Median [4:0]=5 Sample Count
   D0                 // Type/Length Code
   'DIMM Thrm Mrgn 4' // String Bytes

   
//*****************************************************************************
//
// Memory thermal trip sensors
//
//*****************************************************************************


_SDR_TYPE   02
_REC_LEN    0030

   // Sensor Record Header
   7A00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   C0                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   0C                 // Sensor Type
   6F                 // Event / Reading Base Type
   0004               // Assertion Event Mask
   0004               // Deassertion Event Mask
   0004               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'Mem P1 Thrm Trip' // String Bytes


_SDR_TYPE   02
_SDR_TAG    'PROCESSOR_2'
_REC_LEN    0030

   // Sensor Record Header
   7B00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   C1                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   0C                 // Sensor Type
   6F                 // Event / Reading Base Type
   0004               // Assertion Event Mask
   0004               // Deassertion Event Mask
   0004               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'Mem P2 Thrm Trip' // String Bytes 


//*****************************************************************************
//
// Global aggregate thermal margin sensors
//
//*****************************************************************************


_SDR_TYPE   01
_SDR_TAG    'R1000'
_SDR_TAG    'R2000'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003F

   // Sensor Record Header
   7C00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   C8                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   EC                 // Nominal Reading
   00                 // Normal Maximum
   BA                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM used for filtering [7:5]= 1 Median [4:0]=5 Sample Count
   CF                 // Type/Length Code
   'Agg Therm Mgn 1'  // String Bytes
  
 
//*****************************************************************************
//
// Voltage sensors
//
//*****************************************************************************


_SDR_TYPE   01
_REC_LEN    0039

   // Sensor Record Header
   7D00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   34                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D0                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   34                 // M
   00                 // M, Tolerance
   1F                 // B
   40                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   D0                 // R exp, B exp
   07                 // Analog characteristic flags
   E0                 // Normal Reading
   EC                 // Normal Maximum
   D5                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   FC                 // Upper critical
   F5                 // Upper non-critical
   00                 // Lower non-recoverable
   C7                 // Lower critical
   CD                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'BB +12.0V'        // String Bytes


_SDR_TYPE   01
_REC_LEN    0038

   // Sensor Record Header
   7E00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D1                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   D9                 // M
   00                 // M, Tolerance
   62                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   E1                 // Normal Reading
   ED                 // Normal Maximum
   D6                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   FC                 // Upper critical
   F5                 // Upper non-critical
   00                 // Lower non-recoverable
   C7                 // Lower critical
   CD                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C8                 // Type/Length Code
   'BB +5.0V'         // String Bytes


_SDR_TYPE   01
_REC_LEN    0038

   // Sensor Record Header
   7F00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D2                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   8F                 // M
   00                 // M, Tolerance
   F6                 // B
   40                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   E2                 // Normal Reading
   EE                 // Normal Maximum
   D7                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   FC                 // Upper critical
   F5                 // Upper non-critical
   00                 // Lower non-recoverable
   CB                 // Lower critical
   D1                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C8                 // Type/Length Code
   'BB +3.3V'         // String Bytes


_SDR_TYPE   01
_REC_LEN    003D

   // Sensor Record Header
   8000           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D3                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   D9                 // M
   00                 // M, Tolerance
   62                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   E1                 // Normal Reading
   ED                 // Normal Maximum
   D6                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   FC                 // Upper critical
   F5                 // Upper non-critical
   00                 // Lower non-recoverable
   C9                 // Lower critical
   CF                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CD                 // Type/Length Code
   'BB +5.0V STBY'    // String Bytes


_SDR_TYPE   01
_REC_LEN    003C

   // Sensor Record Header
   8100           // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D4                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   8F                 // M
   00                 // M, Tolerance
   F6                 // B
   40                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   E2                 // Normal Reading
   EE                 // Normal Maximum
   D7                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   FC                 // Upper critical
   F5                 // Upper non-critical
   00                 // Lower non-recoverable
   CB                 // Lower critical
   D1                 // Lower non-critical
   01                 // Positive hysterisis value
   01                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM used for filtering [7:5]= 1 Median [4:0]=5 Sample Count
   CC                 // Type/Length Code
   'BB +3.3V AUX'     // String Bytes


_SDR_TYPE   01
_REC_LEN    003F

   // Sensor Record Header
   8200           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D6                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3C                 // M
   00                 // M, Tolerance
   C1                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   B1                 // Normal Reading
   EF                 // Normal Maximum
   62                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   FC                 // Upper critical
   F5                 // Upper non-critical
   00                 // Lower non-recoverable
   5B                 // Lower critical
   5D                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'BB +1.05Vccp P1'  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    003F

   // Sensor Record Header
   8300           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D7                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3C                 // M
   00                 // M, Tolerance
   C1                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   B1                 // Normal Reading
   EF                 // Normal Maximum
   62                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   FC                 // Upper critical
   F5                 // Upper non-critical
   00                 // Lower non-recoverable
   5B                 // Lower critical
   5D                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'BB +1.05Vccp P2'  // String Bytes


_SDR_TYPE   01
_REC_LEN    0040

   // Sensor Record Header
   8400           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D8                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   44                 // M
   00                 // M, Tolerance
   C9                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   E4                 // Normal Reading
   EF                 // Normal Maximum
   D9                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   FC                 // Upper critical
   F5                 // Upper non-critical
   00                 // Lower non-recoverable
   CD                 // Lower critical
   D4                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.5 P1MEM AB' // String Bytes


_SDR_TYPE   01
_REC_LEN    0040

   // Sensor Record Header
   8500           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D9                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   44                 // M
   00                 // M, Tolerance
   C9                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   E4                 // Normal Reading
   EF                 // Normal Maximum
   D9                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   FC                 // Upper critical
   F5                 // Upper non-critical
   00                 // Lower non-recoverable
   CD                 // Lower critical
   D4                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.5 P1MEM CD' // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0040

   // Sensor Record Header
   8600           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   DA                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   44                 // M
   00                 // M, Tolerance
   C9                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   E4                 // Normal Reading
   EF                 // Normal Maximum
   D9                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   FC                 // Upper critical
   F5                 // Upper non-critical
   00                 // Lower non-recoverable
   CD                 // Lower critical
   D4                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.5 P2MEM AB' // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0040

   // Sensor Record Header
   8700           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   DB                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   44                 // M
   00                 // M, Tolerance
   C9                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   E4                 // Normal Reading
   EF                 // Normal Maximum
   D9                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   FC                 // Upper critical
   F5                 // Upper non-critical
   00                 // Lower non-recoverable
   CD                 // Lower critical
   D4                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.5 P2MEM CD' // String Bytes


_SDR_TYPE   01
_REC_LEN    003C

   // Sensor Record Header
   8800           // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   DC                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   53                 // M
   00                 // M, Tolerance
   7C                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   E9                 // Normal Reading
   EF                 // Normal Maximum
   E2                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   FC                 // Upper critical
   F5                 // Upper non-critical
   00                 // Lower non-recoverable
   D6                 // Lower critical
   DD                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CC                 // Type/Length Code
   'BB +1.8V AUX'     // String Bytes


_SDR_TYPE   01
_REC_LEN    003D

   // Sensor Record Header
   8900           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   DD                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   FF                 // M
   40                 // M, Tolerance
   86                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   B1                 // R exp, B exp
   07                 // Analog characteristic flags
   DA                 // Normal Reading
   EF                 // Normal Maximum
   C4                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   FC                 // Upper critical
   F5                 // Upper non-critical
   00                 // Lower non-recoverable
   BA                 // Lower critical
   BF                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CD                 // Type/Length Code
   'BB +1.1V STBY'    // String Bytes


_SDR_TYPE   01
_REC_LEN    003D

   // Sensor Record Header
   8A00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   DE                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   80                 // M
   00                 // M, Tolerance
   DF                 // B
   40                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   E7                 // Normal Reading
   F3                 // Normal Maximum
   C4                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   A9                 // Lower critical
   C3                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM used for filtering [7:5]= 1 Median [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'BB +3.3V Vbat'    // String Bytes


_SDR_TYPE   01
_REC_LEN    0040

   // Sensor Record Header
   8B00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   E4                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3D                 // M
   00                 // M, Tolerance
   15                 // B
   80                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   E4                 // Normal Reading
   EF                 // Normal Maximum
   D9                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   FC                 // Upper critical
   F5                 // Upper non-critical
   00                 // Lower non-recoverable
   CD                 // Lower critical
   D4                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.35 P1LV AB' // String Bytes


_SDR_TYPE   01
_REC_LEN    0040

   // Sensor Record Header
   8C00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   E5                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3D                 // M
   00                 // M, Tolerance
   15                 // B
   80                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   E4                 // Normal Reading
   EF                 // Normal Maximum
   D9                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   FC                 // Upper critical
   F5                 // Upper non-critical
   00                 // Lower non-recoverable
   CD                 // Lower critical
   D4                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.35 P1LV CD' // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0040

   // Sensor Record Header
   8D00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   E6                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3D                 // M
   00                 // M, Tolerance
   15                 // B
   80                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   E4                 // Normal Reading
   EF                 // Normal Maximum
   D9                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   FC                 // Upper critical
   F5                 // Upper non-critical
   00                 // Lower non-recoverable
   CD                 // Lower critical
   D4                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.35 P2LV AB' // String Bytes


_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0040

   // Sensor Record Header
   8E00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   E7                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3D                 // M
   00                 // M, Tolerance
   15                 // B
   80                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   E4                 // Normal Reading
   EF                 // Normal Maximum
   D9                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   FC                 // Upper critical
   F5                 // Upper non-critical
   00                 // Lower non-recoverable
   CD                 // Lower critical
   D4                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.35 P2LV CD' // String Bytes


_SDR_TYPE   01
_SDR_TAG    'RISER_1_FRU'
_REC_LEN    0040

   // Sensor Record Header
   8F00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   EA                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   0420               // Assertion Event Mask
   0400               // Deassertion Event Mask
   0202               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   91                 // M
   00                 // M, Tolerance
   7F                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   E2                 // Normal Reading
   EE                 // Normal Maximum
   93                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   64                 // Lower critical (~2 V)
   8F                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +3.3 RSR1 PGD' // String Bytes


_SDR_TYPE   01
_SDR_TAG    'RISER_2_FRU'
_REC_LEN    0040

   // Sensor Record Header
   9000           // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   EB                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   0420               // Assertion Event Mask
   0400               // Deassertion Event Mask
   0202               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   91                 // M
   00                 // M, Tolerance
   7F                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   E2                 // Normal Reading
   EE                 // Normal Maximum
   93                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   64                 // Lower critical (~2 V)
   8F                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +3.3 RSR2 PGD' // String Bytes 


//*****************************************************************************
//
// Hot-swap backplane (HSBP) sensors
//
//*****************************************************************************


_SDR_TYPE   02
_SDR_TAG    'HSBP1_1U8X25'
_SDR_TAG    'HSBP1_1U4X35'
_SDR_TAG    'HSBP1_2U8X25'
_SDR_TAG    'HSBP1_2U8X25DP'
_SDR_TAG    'HSBP1_2U8X35'
_SDR_TAG    'HSBP1_2U12X35'
_REC_LEN    002C

   // Sensor Record Header
   9100           // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F0                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 0 Status'     // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP1_1U8X25'
_SDR_TAG    'HSBP1_1U4X35'
_SDR_TAG    'HSBP1_2U8X25'
_SDR_TAG    'HSBP1_2U8X25DP'
_SDR_TAG    'HSBP1_2U8X35'
_SDR_TAG    'HSBP1_2U12X35'
_REC_LEN    002C

   // Sensor Record Header
   9200           // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F1                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 1 Status'     // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP1_1U8X25'
_SDR_TAG    'HSBP1_1U4X35'
_SDR_TAG    'HSBP1_2U8X25'
_SDR_TAG    'HSBP1_2U8X25DP'
_SDR_TAG    'HSBP1_2U8X35'
_SDR_TAG    'HSBP1_2U12X35'
_REC_LEN    002C

   // Sensor Record Header
   9300           // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F2                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 2 Status'     // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP1_1U8X25'
_SDR_TAG    'HSBP1_1U4X35'
_SDR_TAG    'HSBP1_2U8X25'
_SDR_TAG    'HSBP1_2U8X25DP'
_SDR_TAG    'HSBP1_2U8X35'
_SDR_TAG    'HSBP1_2U12X35'
_REC_LEN    002C

   // Sensor Record Header
   9400           // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F3                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 3 Status'     // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP1_1U8X25'
_SDR_TAG    'HSBP1_2U8X25'
_SDR_TAG    'HSBP1_2U8X25DP'
_SDR_TAG    'HSBP1_2U8X35'
_SDR_TAG    'HSBP1_2U12X35'
_REC_LEN    002C

   // Sensor Record Header
   9500           // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F4                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 4 Status'     // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP1_1U8X25'
_SDR_TAG    'HSBP1_2U8X25'
_SDR_TAG    'HSBP1_2U8X25DP'
_SDR_TAG    'HSBP1_2U8X35'
_SDR_TAG    'HSBP1_2U12X35'
_REC_LEN    002C

   // Sensor Record Header
   9600           // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F5                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 5 Status'     // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP1_1U8X25'
_SDR_TAG    'HSBP1_2U8X25'
_SDR_TAG    'HSBP1_2U8X25DP'
_SDR_TAG    'HSBP1_2U8X35'
_SDR_TAG    'HSBP1_2U12X35'
_REC_LEN    002C

   // Sensor Record Header
   9700           // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F6                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 6 Status'     // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP1_1U8X25'
_SDR_TAG    'HSBP1_2U8X25'
_SDR_TAG    'HSBP1_2U8X25DP'
_SDR_TAG    'HSBP1_2U8X35'
_SDR_TAG    'HSBP1_2U12X35'
_REC_LEN    002C

   // Sensor Record Header
   9800           // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F7                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 7 Status'     // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP1_2U12X35'
_SDR_TAG    'HSBP2_2U8X25'
_REC_LEN    002C

   // Sensor Record Header
   9900           // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F8                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 8 Status'     // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP1_2U12X35'
_SDR_TAG    'HSBP2_2U8X25'
_REC_LEN    002C

   // Sensor Record Header
   9A00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F9                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 9 Status'     // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP1_2U12X35'
_SDR_TAG    'HSBP2_2U8X25'
_REC_LEN    002D

   // Sensor Record Header
   9B00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   FA                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 10 Status'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP1_2U12X35'
_SDR_TAG    'HSBP2_2U8X25'
_REC_LEN    002D

   // Sensor Record Header
   9C00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   FB                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 11 Status'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP2_2U8X25'
_REC_LEN    002D

   // Sensor Record Header
   9D00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   FC                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 12 Status'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP2_2U8X25'
_REC_LEN    002D

   // Sensor Record Header
   9E00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   FD                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 13 Status'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'HSBP2_2U8X25'
_REC_LEN    002D

   // Sensor Record Header
   9F00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   FE                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'HDD 14 Status'    // String Bytes


//*****************************************************************************
//
//  SDR Type 3 Manageability Engine (ME controller) Records
//
//*****************************************************************************


_SDR_TYPE   03
_REC_LEN    001E

   // Sensor Record Header
   A000           // Record ID
   51                 // SDR Version
   03                 // Record Type
   19                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   17                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   02                 // Entity Instance
   DC                 // Sensor type
   75                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'SPS FW Health'    // String Bytes


_SDR_TYPE   03
_REC_LEN    001D

   // Sensor Record Header
   A100           // Record ID
   51                 // SDR Version
   03                 // Record Type
   18                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   18                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   02                 // Entity Instance
   DC                 // Sensor type
   72                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'NM Exception'     // String Bytes


_SDR_TYPE   03
_REC_LEN    001A

   // Sensor Record Header
   A200           // Record ID
   51                 // SDR Version
   03                 // Record Type
   15                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   19                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   02                 // Entity Instance
   DC                 // Sensor type
   73                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'NM Health'        // String Bytes


_SDR_TYPE   02
_REC_LEN    002F

   // Sensor Record Header
   A300           // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   1A                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   02                 // Entity Instance
   41                 // Sensor Initialization
   C3                 // Sensor Capabilities
   DC                 // Sensor Type
   74                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0700               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0000               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'NM Capabilities'  // String Bytes


_SDR_TYPE   03
_REC_LEN    001D

   // Sensor Record Header
   A400           // Record ID
   51                 // SDR Version
   03                 // Record Type
   18                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Channel Number / Sensor Owner LUN
   1B                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   02                 // Entity Instance
   DC                 // Sensor Type
   72                 // Event / Reading Base Type
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'NM Threshold'     // String Bytes


_SDR_TYPE      C0
_REC_LEN       0010

   // Sensor Record Header
   A500           // Record ID
  51                 // SDR Version
   C0                 // Record Type
   0B                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0D                 // Record subtype - NM Discovery
   01                 // Version number of record subtype
   2C                 // NM Device Slave Address ([7:1] - 7-bit address; [0] - reserved)
   60                 // [7:4] - channel number (6 for secondary IPMB) [3:2] - reserved [1:0] - sensor owner LUN)
   19                 // Node Manager Health Event sensor
   18                 // Node Manager Exception Event sensor
   1A                 // Node Manager Operational Capabilities sensor
   1B                 // Node Manager Threshold Exceeded sensor


_SDR_TYPE   01
_REC_LEN    0038

   // Sensor Record Header
   A600           // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   34                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   63                 // Sensor Initialization
   B8                 // Sensor Capabilities
   0C                 // Sensor Type -- Memory
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   3F3F               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2 -- Degrees C
   00                 // Sensor Units 3
   00                 // Linearization
   05                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   F0                 // R exp, B exp
   00                 // Analog characteristic flags
   00                 // Normal Reading 
   00                 // Normal Maximum 
   00                 // Normal Minimum 
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical
   00                 // Upper non-critical 
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C8                 // Type/Length Code
   'MTT CPU1'         // String Bytes


_SDR_TYPE   01
_REC_LEN    0038

   // Sensor Record Header
   A700           // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   35                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   02                 // Entity Instance
   63                 // Sensor Initialization
   B8                 // Sensor Capabilities
   0C                 // Sensor Type -- Memory
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   3F3F               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2 -- Degrees C
   00                 // Sensor Units 3
   00                 // Linearization
   05                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   F0                 // R exp, B exp
   00                 // Analog characteristic flags
   00                 // Normal Reading 
   00                 // Normal Maximum 
   00                 // Normal Minimum 
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical
   00                 // Upper non-critical 
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C8                 // Type/Length Code
   'MTT CPU2'         // String Bytes
//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PS1_460W'
_SDR_TAG    'PS1_750W'
_REC_LEN    002B

   // Sensor Record Header
   A701               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   66                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   27                 // Sensor Initialization
   40                 // Sensor Capabilities
   08                 // Sensor Type
   6F                 // Event / Reading Base Type
   2000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   2000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0000               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'PSU1 Status'  // String Bytes
   
//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PS2_460W'
_SDR_TAG    'PS2_750W'
_REC_LEN    002B

   // Sensor Record Header
   A702               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   67                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   27                 // Sensor Initialization
   40                 // Sensor Capabilities
   08                 // Sensor Type
   6F                 // Event / Reading Base Type
   2000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   2000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0000               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'PSU2 Status'  // String Bytes
   
_SDR_TYPE   01
_REC_LEN    003C

   // Sensor Record Header
   A800           // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   C4                 // Sensor Number

   // Record Body Bytes
   D0                 // Entity ID
   00                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask   --[u][c,nc]=0000
   0000               // Deassertion Event Mask --[u][c,nc]=0000
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   F1                 // Normal Reading(ECh = -20 degrees C)
   00                 // Normal Maximum (00h = 0 degrees C)
   BA                 // Normal Minimum (BAh = -70 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degrees C)
   00                 // Upper critical (00h = 0 degrees C)
   00                 // Upper non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degrees C)
   00                 // Lower critical (00h = 0 degrees C)
   00                 // Lower non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CC                 // Type/Length Code
   'MIC 1 Margin'     // String Bytes

_SDR_TYPE   01
_REC_LEN    003C

   // Sensor Record Header
   A900           // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   C5                 // Sensor Number

   // Record Body Bytes
   D0                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask   --[u][c,nc]=0000
   0000               // Deassertion Event Mask --[u][c,nc]=0000
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   F1                 // Normal Reading(ECh = -20 degrees C)
   00                 // Normal Maximum (00h = 0 degrees C)
   BA                 // Normal Minimum (BAh = -70 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degrees C)
   00                 // Upper critical (00h = 0 degrees C)
   00                 // Upper non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degrees C)
   00                 // Lower critical (00h = 0 degrees C)
   00                 // Lower non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CC                 // Type/Length Code
   'MIC 2 Margin'     // String Bytes

_SDR_TYPE   02
_REC_LEN    002C

   // Sensor Record Header
   AA00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   A2                 // Sensor Number

   // Record Body Bytes
   D0                 // Entity ID
   00                 // Entity Instance
   2C                 // Sensor Initialization
   40                 // Sensor Capabilities
   C0                 // Sensor Type
   70                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   7F00               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'MIC 1 Status'     // String Bytes

_SDR_TYPE   02
_REC_LEN    002C

   // Sensor Record Header
   AB00           // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   A3                 // Sensor Number

   // Record Body Bytes
   D0                 // Entity ID
   01                 // Entity Instance
   2C                 // Sensor Initialization
   40                 // Sensor Capabilities
   C0                 // Sensor Type
   70                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   7F00               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'MIC 2 Status'     // String Bytes

//*****************************************************************************
//
// SDR Type 3 BIOS Sensor Data Records
//
//*****************************************************************************


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   AC00           // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   01                 // Sensor Number

   // Record Body Bytes
   22                 // Entity ID = Processor/Memory Module
   01                 // Entity Instance
   0C                 // Sensor Type
   0B                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mem Rdnc Sensor'  // Memory Redundancy State


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   AD00           // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   02                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID = Memory Device
   01                 // Entity Instance
   0C                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mmry ECC Sensor'   // Memory ECC Error Sensor


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   AE00           // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   03                 // Sensor Number

   // Record Body Bytes
   30                 // Entity ID = PCI
   01                 // Entity Instance
   13                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCI Lgcy Sensor'   // Legacy PCI Sensor


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   AF00           // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   04                 // Sensor Number

   // Record Body Bytes
   31                 // Entity ID = PCI Express
   01                 // Entity Instance
   13                 // Sensor Type
   70                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCIe Fat Sensor'  // PCI Express Fatal Error Sensor


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   B000           // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   05                 // Sensor Number

   // Record Body Bytes
   31                 // Entity ID = PCI Express
   01                 // Entity Instance
   13                 // Sensor Type
   71                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCIe Cor Sensor'  // PCI Express Correctable Error Sensor


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   B100           // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   06                 // Sensor Number

   // Record Body Bytes
   22                 // Entity ID System Firmware (BIOS)
   01                 // Entity Instance
   0F                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'POST Err Sensor'  // POST Error Sensor


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   B200           // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   06                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID
   01                 // Entity Instance
   13                 // Sensor Type
   72                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'QPI Corr Sensor'  // QPI Correctable Event Sensor


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   B300           // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   07                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID
   01                 // Entity Instance
   13                 // Sensor Type
   73                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'QPI Fatl Sensor'   //  QPI Fatal/Uncorrectable Errors


_SDR_TYPE   03
_REC_LEN    001F

   // Sensor Record Header
   B400           // Record ID
   51                 // SDR Version
   03                 // Record Type
   1A                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   08                 // Sensor Number

   // Record Body Bytes
   31                 // Entity ID = PCI Express
   01                 // Entity Instance
   19                 // Sensor Type
   75                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Chipset Sensor'   // Chipset Proprietary Errors

_SDR_TYPE   03
_REC_LEN    001F

   // Sensor Record Header
   B500           // Record ID
   51                 // SDR Version
   03                 // Record Type
   1A                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   09                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID
   05                 // Entity Instance
   13                 // Sensor Type
   77                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'QPI Link Width'   // QPI Link Width Reduced

_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   B600           // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   02                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID = Memory
   01                 // Entity Instance
   0C                 // Sensor Type
   09                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mem Conf Sensor'  // Memory configuration failed

//====================================================================//
_SDR_TYPE   03
_REC_LEN    001D

   // Sensor Record Header
   B700           // Record ID
   51                 // SDR Version
   03                 // Record Type
   18                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   11                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   01                 // Entity Instance
   0C                 // Sensor Type
   0B                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'Sparing Rdnc'     // Sparing Redundancy State


_SDR_TYPE   03
_REC_LEN    001F

   // Sensor Record Header
   B800           // Record ID
   51                 // SDR Version
   03                 // Record Type
   1A                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   10                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID = Memory Device
   01                 // Entity Instance
   0C                 // Sensor Type
   7F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Mem err Sensor'   //Memory Error Extension


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   B900           // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   12                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   01                 // Entity Instance
   0C                 // Sensor Type
   09                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Rdnc Mod Sensor'  // Memory Redundancy Configuration


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   BA00           // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   13                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID = Memory Device
   01                 // Entity Instance
   0C                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mmry Parity Err'  // Memory Parity Error

_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   BB00           // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   14                 // Sensor Number

   // Record Body Bytes
   31                 // Entity ID = PCI Express
   01                 // Entity Instance
   13                 // Sensor Type
   76                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCIe Fat Sensor'  // PCI Express Fatal Error Sensor

_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   BC00           // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   17                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID
   01                 // Entity Instance
   13                 // Sensor Type
   74                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'QPI Fatl Sensor'  // QPI Fatal/Uncorrectable Errors


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   BD00           // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   83                 // Sensor Number

   // Record Body Bytes
   22                 // Entity ID = System Firmware (BIOS)
   01                 // Entity Instance
   12                 // Sensor Type
   6F                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'BIOS Evt Sensor'  // BIOS Boot Event Sensor

_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   BE00           // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   83                 // Sensor Number

   // Record Body Bytes
   22                 // Entity ID = System Firmware (BIOS)
   01                 // Entity Instance
   12                 // Sensor Type
   6F                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'BIOS Evt Sensor'  // BIOS Boot Event Sensor

_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   BF00           // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   83                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   01                 // Entity Instance
   12                 // Sensor Type
   6F                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'BIOS Evt Sensor'  // BIOS Boot Event Sensor


//*******************************************************
//
// SDR Type 11 FRU Device Locator Records
//
//*******************************************************


_SDR_TYPE   11
_REC_LEN    0019

   // Sensor Record Header
   C000           // Record ID
   51                 // SDR Version
   11                 // Record Type
   14                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   00                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   07                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // OEM
   C9                 // Type/Length Code
   'Baseboard'        // String Bytes


_SDR_TYPE   11
_SDR_TAG    'PS1_460W'
_SDR_TAG    'PS1_750W'
_REC_LEN    0020
 
   // Sensor Record Header
   C100           // Record ID
   51                 // SDR Version
   11                 // Record Type
   1B                 // Record Length
   // Record Key Bytes
   20                 // Device Access Address
   02                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number
   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   0A                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // Reserved for OEM use
   D0                 // Type/Length Code
   'Pwr Supply 1 FRU' // String Bytes


_SDR_TYPE   11
_SDR_TAG    'PS2_460W'
_SDR_TAG    'PS2_750W'
_REC_LEN    0020

   // Sensor Record Header
   C200           // Record ID
   51                 // SDR Version
   11                 // Record Type
   1B                 // Record Length
   // Record Key Bytes
   20                 // Device Access Address
   03                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number
   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   0A                 // FRU Entity ID
   02                 // FRU Entity Instance
   00                 // Reserved for OEM use
   D0                 // Type/Length Code
   'Pwr Supply 2 FRU' // String Bytes


_SDR_TYPE   11
_REC_LEN    001B

   // Sensor Record Header
   C300           // Record ID
   51                 // SDR Version
   11                 // Record Type
   16                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   04                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   0C                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // OEM
   CB                 // Type/Length Code
   'Front Panel'      // String Bytes


_SDR_TYPE   11
_SDR_TAG    'HSBP1_1U8X25'
_SDR_TAG    'HSBP1_1U4X35'
_SDR_TAG    'HSBP1_2U8X25'
_SDR_TAG    'HSBP1_2U8X25DP'
_SDR_TAG    'HSBP1_2U8X35'
_SDR_TAG    'HSBP1_2U12X35'
_REC_LEN    001E

   // Sensor Record Header
   C400           // Record ID
   51                 // SDR Version
   11                 // Record Type
   19                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   05                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   0F                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // OEM
   CE                 // Type/Length Code
   'HS Backplane 1'   // String Bytes


_SDR_TYPE   11
_SDR_TAG    'HSBP2_2U8X25'
_REC_LEN    001E

   // Sensor Record Header
   C500           // Record ID
   51                 // SDR Version
   11                 // Record Type
   19                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   06                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   0F                 // FRU Entity ID
   02                 // FRU Entity Instance
   00                 // OEM
   CE                 // Type/Length Code
   'HS Backplane 2'   // String Bytes


_SDR_TYPE   11
_SDR_TAG    'HSBP3_2U8X25'
_REC_LEN    001E

   // Sensor Record Header
   C600           // Record ID
   51                 // SDR Version
   11                 // Record Type
   19                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   07                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   0F                 // FRU Entity ID
   03                 // FRU Entity Instance
   00                 // OEM
   CE                 // Type/Length Code
   'HS Backplane 3'   // String Bytes


_SDR_TYPE   11
_SDR_TAG    'IO_MODULE_FRU'
_SDR_TAG    'FCT'
_REC_LEN    0019

   // Sensor Record Header
   C700           // Record ID
   51                 // SDR Version
   11                 // Record Type
   14                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   09                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   2C                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // OEM
   C9                 // Type/Length Code
   'IO Module'        // String Bytes
   
_SDR_TYPE   11
_SDR_TAG    'SAS_MODULE_FRU'
_SDR_TAG    'FCT'
_REC_LEN    001A

   // Sensor Record Header
   C800           // Record ID
   51                 // SDR Version
   11                 // Record Type
   15                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   0A                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   33                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // OEM
   CA                 // Type/Length Code
   'SAS Module'       // String Bytes   

   
//*******************************************************
//
// SDR Type 12 Management Controller Records
//
//*******************************************************


_SDR_TYPE   12
_REC_LEN    0020

   // Sensor Record Header
   C900           // Record ID
   51                 // SDR Version
   12                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   20                 // Device Slave Address
   00                 // Channel Number

   // Record Body Bytes
   08                 // Power state notification
   BF                 // Device capabilities
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   07                 // Entity ID
   01                 // Entity instance
   00                 // OEM
   D0                 // Type/Length Code
   'Basbrd Mgmt Ctlr' // String Bytes


_SDR_TYPE   12
_REC_LEN    001B

   // Sensor Record Header
   CA00           // Record ID
   51                 // SDR Version
   12                 // Record Type
   16                 // Record Length

   // Record Key Bytes
   2C                 // Device Slave Address
   06                 // Channel number

   // Record Body Bytes
   24                 // Power State Notification
   21                 // Device Capabilities
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   2E                 // Entity ID
   02                 // Entity Instance
   00                 // OEM
   CB                 // Type/Length Code
   'Mgmt Engine'      // String Bytes


//*******************************************************
//
// SDR Type C0/02 Record For Power Unit Map 
//
//*******************************************************


_SDR_TYPE   C0
_SDR_TAG    'REDUNDANT_PS'
_REC_LEN    000E

   // Sensor Record Header
   CB00           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   09                 // Record Length
   
   // Record Body Bytes
   570100             // Manufacturer ID
   02                 // Record Subtype Value
   02                 // Power Unit Redundancy sensor number
   00                 // Bits [7:1]-Reserved; Bit[0]-1=No monitorable supplies present
   01                 // The number of present and operational
   50                 // Power Supply Status 1 Sensor Number
   51                 // Power Supply Status 2 Sensor Number


//*******************************************************
//
// SDR Type C0/05 Record For R2000 Fan Redundancy Map
//
//*******************************************************


_SDR_TYPE   C0
_SDR_TAG    'R2000_RED_FAN'
_REC_LEN    0018

   // Sensor Record Header
   CC00           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   13                 // Record Length
   
   // Record Body Bytes
   570100             // Manufacturer ID
   05                 // Record Subtype Value
   
   //Fan Redundancy Map Record
   0C                 // Fan Redundancy Sensor Number
   00                 // Flags; [7:1]-Reserved; [0]-persistently stored event state, 1= store tis event state persistently
   0404               // Failed Event State Mask
   01                 // Redundant Fan Count
   30                 // Fan Speed Sensor #1
   40                 // Fan Presence Sensor #1
   32                 // Fan Speed Sensor #2
   41                 // Fan Presence Sensor #2
   34                 // Fan Speed Sensor #3
   42                 // Fan Presence Sensor #3   
   36                 // Fan Speed Sensor #4
   43                 // Fan Presence Sensor #4
   38                 // Fan Speed Sensor #5
   44                 // Fan Presence Sensor #5

//*******************************************************
//
// SDR Type C0/05 Record For R1000 Fan Redundancy Map
//
//*******************************************************


_SDR_TYPE   C0
_SDR_TAG    'R1000_RED_FAN'
_REC_LEN    0026

   // Sensor Record Header
   CD00           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   21                 // Record Length
   
   // Record Body Bytes
   570100             // Manufacturer ID
   05                 // Record Subtype Value
   
   //Fan Redundancy Map Record
   0C                 // Fan Redundancy Sensor Number
   00                 // Flags; [7:1]-Reserved; [0]-persistently stored event state, 1= store tis event state persistently
   0404               // Failed Event State Mask
   01                 // Redundant Fan Count
   30                 // Fan Speed Sensor #1
   00                 // Fan Presence Sensor #1
   31                 // Fan Speed Sensor #2
   00                 // Fan Presence Sensor #2
   32                 // Fan Speed Sensor #3
   00                 // Fan Presence Sensor #3
   33                 // Fan Speed Sensor #4
   00                 // Fan Presence Sensor #4
   34                 // Fan Speed Sensor #5
   00                 // Fan Presence Sensor #5   
   35                 // Fan Speed Sensor #6
   00                 // Fan Presence Sensor #6   
   36                 // Fan Speed Sensor #7
   00                 // Fan Presence Sensor #7
   37                 // Fan Speed Sensor #8
   00                 // Fan Presence Sensor #8
   38                 // Fan Speed Sensor #9
   00                 // Fan Presence Sensor #9
   39                 // Fan Speed Sensor 10#
   00                 // Fan Presence Sensor #10
   3A                 // Fan Speed Sensor 11#
   00                 // Fan Presence Sensor #11
   3B                 // Fan Speed Sensor 12#
   00                 // Fan Presence Sensor #12


//*******************************************************
//
// SDR Type C0/09 Records For Voltage Sensor Scaling
//
//*******************************************************


_SDR_TYPE   C0
_REC_LEN    0040

   // Sensor Record Header
   CE00           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   3B                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   09                 // Record sub-type - Voltage Sensor Scaling
   12                 // Number of entries following
   D0                 // Voltage Sensor Number
   A60A               // Scale Factor (LSB MSB)
   D1                 // Voltage Sensor Number
   8C0A               // Scale Factor (LSB MSB)
   D2                 // Voltage Sensor Number
   870A               // Scale Factor (LSB MSB)
   D3                 // Voltage Sensor Number
   8C0A               // Scale Factor (LSB MSB)
   D4                 // Voltage Sensor Number
   870A               // Scale Factor (LSB MSB)
   D6                 // Voltage Sensor Number
   0010               // Scale Factor (LSB MSB)
   D7                 // Voltage Sensor Number
   0010               // Scale Factor (LSB MSB)
   D8                 // Voltage Sensor Number
   670E               // Scale Factor (LSB MSB)
   D9                 // Voltage Sensor Number
   670E               // Scale Factor (LSB MSB)
   DA                 // Voltage Sensor Number
   670E               // Scale Factor (LSB MSB)
   DB                 // Voltage Sensor Number
   670E               // Scale Factor (LSB MSB)
   DC                 // Voltage Sensor Number
   3D0C               // Scale Factor (LSB MSB)
   DD                 // Voltage Sensor Number
   BD12               // Scale Factor (LSB MSB)
   DE                 // Voltage Sensor Number
   CA09               // Scale Factor (LSB MSB)
   E4                 // Voltage Sensor Number
   0010               // Scale Factor (LSB MSB)
   E5                 // Voltage Sensor Number
   0010               // Scale Factor (LSB MSB)
   E6                 // Voltage Sensor Number
   0010               // Scale Factor (LSB MSB)
   E7                 // Voltage Sensor Number
   0010               // Scale Factor (LSB MSB)
 
 
//*****************************************************************************
//
// Additional SDR Type C0/09 Records For Voltage Sensor Scaling
//
// Must be broken up from above due to 64 byte OEM SDR length limitation
//
//*****************************************************************************


_SDR_TYPE   C0
_REC_LEN    0010

   // Sensor Record Header
   CF00           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0B                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   09                 // Record sub-type - Voltage Sensor Scaling
   02                 // Number of entries following
   EA                 // Voltage Sensor Number
   870A               // Scale Factor (LSB MSB)
   EB                 // Voltage Sensor Number
   870A               // Scale Factor (LSB MSB)


//*****************************************************************************
//
// SDR Type C0/0A Records For Fan Sensor Scaling
//
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R1000'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    0027

  //Sensor Record Header
   D000           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   22                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record sub-type - Fan Sensor Scaling
   00                 // Format - Bit fields, 1 == Raw time, 0 = RPM
   00                 // Pulses Per Revolution - Bit Field - 1 == 1 PPR, 0 == 2 PPR
   803E               // Sys Fan 1A Max RPM (Sensor 30) **(M = 3E)**
   283C               // Sys Fan 1B Max RPM (Sensor 31) **(M = 3C)**
   803E               // Sys Fan 2A Max RPM (Sensor 32) **(M = 3E)**
   283C               // Sys Fan 2B Max RPM (Sensor 33) **(M = 3C)**
   803E               // Sys Fan 3A Max RPM (Sensor 34) **(M = 3E)**
   283C               // Sys Fan 3B Max RPM (Sensor 35) **(M = 3C)**
   803E               // Sys Fan 4A Max RPM (Sensor 36) **(M = 3E)**
   283C               // Sys Fan 4B Max RPM (Sensor 37) **(M = 3C)**
   803E               // Sys Fan 5A Max RPM (Sensor 38) **(M = 3E)**
   283C               // Sys Fan 5B Max RPM (Sensor 39) **(M = 3C)**
   803E               // Sys Fan 6A Max RPM (Sensor 3A) **(M = 3E)**
   283C               // Sys Fan 6B Max RPM (Sensor 3B) **(M = 3C)**
   0001               // CPU Fan 01 Max RPM (Sensor 3C) **Not Used**
   0001               // CPU Fan 02 Max RPM (Sensor 3D) **Not Used**


_SDR_TYPE   C0
_SDR_TAG    'R2000'
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    0027

  //Sensor Record Header
   D100           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   22                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record sub-type - Fan Sensor Scaling
   00                 // Format - Bit fields, 1 == Raw time, 0 = RPM
   00                 // Pulses Per Revolution - Bit Field - 1 == 1 PPR, 0 == 2 PPR
   D430               // Sys Fan 1  Max RPM (Sensor 30) **(M = 31)**
   0001               // Sys Fan xx Max RPM (Sensor 31) **Not Used**
   D430               // Sys Fan 2  Max RPM (Sensor 32) **(M = 31)**
   0001               // Sys Fan xx Max RPM (Sensor 33) **Not Used**
   D430               // Sys Fan 3  Max RPM (Sensor 34) **(M = 31)**
   0001               // Sys Fan xx Max RPM (Sensor 35) **Not Used**
   D430               // Sys Fan 4  Max RPM (Sensor 36) **(M = 31)**
   0001               // Sys Fan xx Max RPM (Sensor 37) **Not Used**
   D430               // Sys Fan 5  Max RPM (Sensor 38) **(M = 31)**
   0001               // Sys Fan xx Max RPM (Sensor 39) **Not Used**
   0001               // Sys Fan xx Max RPM (Sensor 3A) **Not Used**
   0001               // Sys Fan xx Max RPM (Sensor 3B) **Not Used**
   0001               // CPU Fan 01 Max RPM (Sensor 3C) **Not Used**
   0001               // CPU Fan 02 Max RPM (Sensor 3D) **Not Used**


_SDR_TYPE   C0
_SDR_TAG    'SHIPPING'
_REC_LEN    0027


  //Sensor Record Header
   D200           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   22                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record sub-type - Fan Sensor Scaling
   00                 // Format - Bit fields, 1 == Raw time, 0 = RPM
   00                 // Pulses Per Revolution - Bit Field - 1 == 1 PPR, 0 == 2 PPR
   803E               // Sys Fan 1A Max RPM (Sensor 30) **(M = 3E)**
   283C               // Sys Fan 1B Max RPM (Sensor 31) **(M = 3C)**
   803E               // Sys Fan 2A Max RPM (Sensor 32) **(M = 3E)**
   283C               // Sys Fan 2B Max RPM (Sensor 33) **(M = 3C)**
   803E               // Sys Fan 3A Max RPM (Sensor 34) **(M = 3E)**
   283C               // Sys Fan 3B Max RPM (Sensor 35) **(M = 3C)**
   803E               // Sys Fan 4A Max RPM (Sensor 36) **(M = 3E)**
   283C               // Sys Fan 4B Max RPM (Sensor 37) **(M = 3C)**
   803E               // Sys Fan 5A Max RPM (Sensor 38) **(M = 3E)**
   283C               // Sys Fan 5B Max RPM (Sensor 39) **(M = 3C)**
   803E               // Sys Fan 6A Max RPM (Sensor 3A) **(M = 3E)**
   283C               // Sys Fan 6B Max RPM (Sensor 3B) **(M = 3C)**
   3421               // CPU Fan 01 Max RPM (Sensor 3C) **(M = 21)**
   3421               // CPU Fan 02 Max RPM (Sensor 3D) **(M = 21)**


_SDR_TYPE   C0
_SDR_TAG    'TEST_PLATE'
_REC_LEN    0027


  //Sensor Record Header
   D300           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   22                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record sub-type - Fan Sensor Scaling
   00                 // Format - Bit fields, 1 == Raw time, 0 = RPM
   00                 // Pulses Per Revolution - Bit Field - 1 == 1 PPR, 0 == 2 PPR
   3421               // Sys Fan 1 Max RPM (Sensor 30) **(M = 21)**
   0100               // Not Used
   3421               // Sys Fan 2 Max RPM (Sensor 32) **(M = 21)**
   0100               // Not Used
   3421               // Sys Fan 3 Max RPM (Sensor 34) **(M = 21)**
   0100               // Not Used
   3421               // Sys Fan 4 Max RPM (Sensor 36) **(M = 21)**
   0100               // Not Used
   0100               // Not Used
   0100               // Not Used
   0100               // Not Used
   0100               // Not Used
   0100               // Not Used
   0100               // Not Used

_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0027


  //Sensor Record Header
   D400           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   22                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record sub-type - Fan Sensor Scaling
   00                 // Format - Bit fields, 1 == Raw time, 0 = RPM
   00                 // Pulses Per Revolution - Bit Field - 1 == 1 PPR, 0 == 2 PPR
   8062               // Sys Fan 1A Max RPM (Sensor 30) **(M = 62)**
   2862               // Sys Fan 1B Max RPM (Sensor 31) **(M = 62)**
   8062               // Sys Fan 2A Max RPM (Sensor 32) **(M = 62)**
   2862               // Sys Fan 2B Max RPM (Sensor 33) **(M = 62)**
   8062               // Sys Fan 3A Max RPM (Sensor 34) **(M = 62)**
   2862               // Sys Fan 3B Max RPM (Sensor 35) **(M = 62)**
   8062               // Sys Fan 4A Max RPM (Sensor 36) **(M = 62)**
   2862               // Sys Fan 4B Max RPM (Sensor 37) **(M = 62)**
   8062               // Sys Fan 5A Max RPM (Sensor 38) **(M = 62)**
   2862               // Sys Fan 5B Max RPM (Sensor 39) **(M = 62)**
   8062               // Sys Fan 6A Max RPM (Sensor 3A) **(M = 62)**
   2862               // Sys Fan 6B Max RPM (Sensor 3B) **(M = 62)**
   3462               // CPU Fan 01 Max RPM (Sensor 3C) **(M = 62)**
   3462               // CPU Fan 02 Max RPM (Sensor 3D) **(M = 62)**

//*****************************************************************************
//
// Fan Speed Control (FSC) configuration records
//
//*****************************************************************************

//====================================================================//
// Global Clamp Header Records
//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   D500           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   74             // Clamp Header ID
   74             // Input Sensor Number -- (P1 Therm Margin)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   38             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   FA             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   FC             // Clamp Temperature
   01             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   D600           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   75             // Clamp Header ID
   75             // Input Sensor Number -- (P2 Therm Margin)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   38             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   FA             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   FC             // Clamp Temperature
   11             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   D700           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   B0             // Clamp Header ID
   B0             // Input Sensor Number -- (DIMM Thrm Mrgn 1)
   00             // Entity Presence Sensor Number
   00             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   FC             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   D800           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   B1             // Clamp Header ID
   B1             // Input Sensor Number -- (DIMM Thrm Mrgn 2)
   00             // Entity Presence Sensor Number
   00             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   FC             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   D900           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   B2             // Clamp Header ID
   B2             // Input Sensor Number -- (DIMM Thrm Mrgn 3)
   00             // Entity Presence Sensor Number
   00             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   FC             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   DA00           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   B3             // Clamp Header ID
   B3             // Input Sensor Number -- (DIMM Thrm Mrgn 4)
   00             // Entity Presence Sensor Number
   00             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   FC             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   DB00           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   20             // Clamp Header ID
   20             // Input Sensor Number -- (BB P1 VR Temp)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   5A             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   DC00           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   23             // Clamp Header ID
   23             // Input Sensor Number -- (BB P2 VR Temp)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   5A             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   DD00           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   24             // Clamp Header ID
   24             // Input Sensor Number -- (BB VTT2 Temp)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   5A             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   DE00           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   25             // Clamp Header ID
   25             // Input Sensor Number -- (BB VTT1 Temp)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   50             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   DF00           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   29             // Clamp Header ID
   29             // Input Sensor Number -- (HSBP 1 Temp)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   4B             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   E000           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   2A             // Clamp Header ID
   2A             // Input Sensor Number -- (HSBP 2 Temp)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   4B             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   E100           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   2B             // Clamp Header ID
   2B             // Input Sensor Number -- (HSBP 3 Temp)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   4B             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   E200           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   22             // Clamp Header ID
   22             // Input Sensor Number -- (PCH Temp)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   55             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   E300           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   26             // Clamp Header ID
   26             // Input Sensor Number -- (I/O Mod Temp)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   3C             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   E400           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   2D             // Clamp Header ID
   2D             // Input Sensor Number -- (SAS Mod Temp)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   50             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   E500           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   2F             // Clamp Header ID
   2F             // Input Sensor Number -- (LAN NIC Temp)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   5F             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   E600           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   5C             // Clamp Header ID
   5C             // Input Sensor Number -- (PSU1 Temp)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   32             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   E700           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   5D             // Clamp Header ID
   5D             // Input Sensor Number -- (PSU2 Temp)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   32             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   E800           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   83             // Clamp Header ID
   83             // Input Sensor Number -- (P1 DTS Margin)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   FA             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   F6             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   E900           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   84             // Clamp Header ID
   84             // Input Sensor Number -- (P2 DTS Margin)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   FA             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   F6             // Clamp Temperature
   10             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   EA00           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   2E             // Clamp Header ID
   2E             // Input Sensor Number -- (Texit)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   46             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   EB00           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   00             // Clamp Header ID
   5C             // Input Sensor Number -- (PSU1 Temp)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   28             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   EC00           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   01             // Clamp Header ID
   5D             // Input Sensor Number -- (PSU2 Temp)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   02             // Clamp Control Coefficient MSB
   28             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   ED00           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   03             // Clamp Header ID
   5C             // Input Sensor Number -- (PSU1 Temp)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   34             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   EE00           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   04             // Clamp Header ID
   5D             // Input Sensor Number -- (PSU2 Temp)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   34             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   EF00           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   94             // Clamp Header ID
   74             // Input Sensor Number -- (P1 Therm Margin)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   F9             // Clamp Temperature
   01             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   F000           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   95             // Clamp Header ID
   75             // Input Sensor Number -- (P2 Therm Margin)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   F9             // Clamp Temperature
   11             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   F100           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   C4             // Clamp Header ID
   C4             // Input Sensor Number -- (MIC 1 Margin)
   00             // Entity Presence Sensor Number
   00             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   96             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   FC             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   F200           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   C5             // Clamp Header ID
   C5             // Input Sensor Number -- (MIC 2 Margin)
   00             // Entity Presence Sensor Number
   00             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   96             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   FC             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   F300           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   96             // Clamp Header ID
   C4             // Input Sensor Number -- (MIC 1 Margin)
   00             // Entity Presence Sensor Number
   00             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   F9             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   F400           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   00             // FSC Record Type (Global Clamp Header Record)

   // Global Clamp Header Record
   97             // Clamp Header ID
   C5             // Input Sensor Number -- (MIC 2 Margin)
   00             // Entity Presence Sensor Number
   00             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   F9             // Clamp Temperature
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved = 0; [0] - Temp Source = 1 (use TControl)


//*****************************************************************************
// FSC Record Type = 01h (Global Stepwise Header Record)
// All Chassis
//*****************************************************************************

//====================================================================//
// Global Stepwise Header Records
//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0013

   // Sensor Record Header
   F500           // Record ID
   51             // SDR Version
   C0             // Record Type
   0E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   01             // FSC Record Type (Global Stepwise Header Record)

   // Global Stepwise Header Record
   00             // Stepwise Header ID
   21             // Input Sensor Number -- (FP)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   50             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0013

   // Sensor Record Header
   F600           // Record ID
   51             // SDR Version
   C0             // Record Type
   0E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   01             // FSC Record Type (Global Stepwise Header Record)

   // Global Stepwise Header Record
   01             // Stepwise Header ID
   20             // Input Sensor Number -- (Baseboard)
   00             // Entity Presence Sensor Number
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   50             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0



//*****************************************************************************
// FSC Record Type = 02h (Global Stepwise Curve Record)
// All Chassis
//*****************************************************************************

//====================================================================//
// Global Step Curve Records
//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   F700           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   00             // Stepwise Curve ID
   05             // Domain max and count
   0F             //  15C
   1E             //  30%
   19             //  25C
   23             //  35%
   23             //  35C
   32             //  50%
   28             //  40C
   4B             //  75%
   2D             //  45C
   64             //  100%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   F800           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   01             // Stepwise Curve ID
   05             // Domain max and count
   0F             //  15C
   1E             //  30%
   19             //  25C
   28             //  40%
   23             //  35C
   3C             //  60%
   28             //  40C
   50             //  80%
   2D             //  45C
   64             //  100%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0015

   // Sensor Record Header
   F900           // Record ID
   51             // SDR Version
   C0             // Record Type
   10             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   02             // Stepwise Curve ID
   04             // Domain max and count
   0F             //  15C
   23             //  35%
   19             //  25C
   2D             //  45%
   21             //  33C
   46             //  70%
   2D             //  45C
   64             //  100%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0013

   // Sensor Record Header
   FA00           // Record ID
   51             // SDR Version
   C0             // Record Type
   0E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   03             // Stepwise Curve ID
   03             // Domain max and count
   0F             //  15C
   28             //  40%
   19             //  25C
   2D             //  45%
   1C             //  28C
   3C             //  60%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   FB00           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   04             // Stepwise Curve ID
   05             // Domain max and count
   0F             //  15C
   14             //  20%
   19             //  25C
   23             //  35%
   23             //  35C
   32             //  50%
   28             //  40C
   5A             //  90%
   2D             //  45C
   5F             //  95%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   FC00           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   05             // Stepwise Curve ID
   05             // Domain max and count
   0F             //  15C
   19             //  25%
   19             //  25C
   28             //  40%
   23             //  35C
   3C             //  60%
   28             //  40C
   5A             //  90%
   2D             //  45C
   64             //  100%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0015

   // Sensor Record Header
   FD00           // Record ID
   51             // SDR Version
   C0             // Record Type
   10             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   06             // Stepwise Curve ID
   04             // Domain max and count
   0F             //  15C
   1E             //  30%
   19             //  25C
   32             //  50%
   21             //  33C
   3C             //  60%
   2D             //  45C
   64             //  100%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0015

   // Sensor Record Header
   FE00           // Record ID
   51             // SDR Version
   C0             // Record Type
   10             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   07             // Stepwise Curve ID
   04             // Domain max and count
   0F             //  15C
   32             //  50%
   19             //  25C
   3C             //  60%
   1C             //  28C
   41             //  65%
   2D             //  45C
   64             //  100%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   FF00           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   08             // Stepwise Curve ID
   85             // Domain max and count
   0F             //  15C
   4B             //  75%
   19             //  25C
   5F             //  95%
   21             //  33C
   64             //  100%
   23             //  35C
   64             //  100%
   2D             //  45C
   64             //  100%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   0001           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   09             // Stepwise Curve ID
   05             // Domain max and count
   0F             //  15C
   46             //  70%
   19             //  25C
   46             //  70%
   1C             //  28C
   46             //  70%
   21             //  33C
   46             //  70%
   23             //  35C
   46             //  70%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0013

   // Sensor Record Header
   0101           // Record ID
   51             // SDR Version
   C0             // Record Type
   0E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   0A             // Stepwise Curve ID
   03             // Domain max and count
   0F             //  15C
   14             //  20%
   19             //  25C
   14             //  20%
   23             //  35C
   14             //  20%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   0201           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   0B             // Stepwise Curve ID
   05             // Domain max and count
   0F             //  15C
   32             //  50%
   19             //  25C
   32             //  50%
   23             //  35C
   32             //  50%
   28             //  40C
   5A             //  90%
   2D             //  45C
   5F             //  95%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   0301           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   0C             // Stepwise Curve ID
   05             // Domain max and count
   0F             //  15C
   3C             //  60%
   19             //  25C
   3C             //  60%
   23             //  35C
   3C             //  60%
   28             //  40C
   5A             //  90%
   2D             //  45C
   64             //  100%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   0401           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   0D             // Stepwise Curve ID
   05             // Domain max and count
   0F             //  15C
   3C             //  60%
   19             //  25C
   3C             //  60%
   21             //  33C
   3C             //  60%
   28             //  40C
   5A             //  90%
   2D             //  45C
   64             //  100%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   0501           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   0E             // Stepwise Curve ID
   05             // Domain max and count
   0F             //  15C
   41             //  65%
   19             //  25C
   41             //  65%
   1C             //  28C
   41             //  65%
   28             //  40C
   5A             //  90%
   2D             //  45C
   64             //  100%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   0601           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   0F             // Stepwise Curve ID
   05             // Domain max and count
   0F             //  15C
   32             //  50%
   19             //  25C
   3C             //  60%
   23             //  35C
   55             //  85%
   28             //  40C
   64             //  100%
   2D             //  45C
   64             //  100%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   0701           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   10             // Stepwise Curve ID
   05             // Domain max and count
   0F             //  15C
   3C             //  60%
   19             //  25C
   46             //  70%
   23             //  35C
   5A             //  90%
   28             //  40C
   64             //  100%
   2D             //  45C
   64             //  100%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   0801           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   11             // Stepwise Curve ID
   05             // Domain max and count
   0F             //  15C
   3C             //  60%
   19             //  25C
   46             //  70%
   21             //  33C
   5A             //  90%
   28             //  40C
   64             //  100%
   2D             //  45C
   64             //  100%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   0901           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   12             // Stepwise Curve ID
   05             // Domain max and count
   0F             //  15C
   41             //  65%
   19             //  25C
   4B             //  75%
   1C             //  28C
   5F             //  95%
   28             //  40C
   64             //  100%
   2D             //  45C
   64             //  100%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0017

   // Sensor Record Header
   0A01           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   13             // Stepwise Curve ID
   85             // Domain max and count
   0F             //  15C
   64             //  100%
   19             //  25C
   64             //  100%
   21             //  33C
   64             //  100%
   23             //  35C
   64             //  100%
   2D             //  45C
   64             //  100%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0011

   // Sensor Record Header
   0B01           // Record ID
   51             // SDR Version
   C0             // Record Type
   0C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   5B             // Stepwise Curve ID
   02             // Domain max and count
   1E             //  30C
   19             //  25%
   3C             //  60C
   32             //  50%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0011

   // Sensor Record Header
   0C01           // Record ID
   51             // SDR Version
   C0             // Record Type
   0C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   5C             // Stepwise Curve ID
   02             // Domain max and count
   1E             //  30C
   20             //  32%
   3C             //  60C
   39             //  57%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0011

   // Sensor Record Header
   0D01           // Record ID
   51             // SDR Version
   C0             // Record Type
   0C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   5D             // Stepwise Curve ID
   02             // Domain max and count
   1E             //  30C
   33             //  51%
   3C             //  60C
   4C             //  76%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0011

   // Sensor Record Header
   0E01           // Record ID
   51             // SDR Version
   C0             // Record Type
   0C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   5E             // Stepwise Curve ID
   02             // Domain max and count
   1E             //  30C
   19             //  25%
   3C             //  60C
   4B             //  75%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0011

   // Sensor Record Header
   0F01           // Record ID
   51             // SDR Version
   C0             // Record Type
   0C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   5F             // Stepwise Curve ID
   02             // Domain max and count
   1E             //  30C
   20             //  32%
   3C             //  60C
   52             //  82%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0011

   // Sensor Record Header
   1001           // Record ID
   51             // SDR Version
   C0             // Record Type
   0C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   60             // Stepwise Curve ID
   02             // Domain max and count
   1E             //  30C
   33             //  51%
   3C             //  60C
   64             //  100%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0011

   // Sensor Record Header
   1101           // Record ID
   51             // SDR Version
   C0             // Record Type
   0C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   61             // Stepwise Curve ID
   02             // Domain max and count
   1E             //  30C
   19             //  25%
   3C             //  60C
   64             //  100%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0011

   // Sensor Record Header
   1201           // Record ID
   51             // SDR Version
   C0             // Record Type
   0C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   62             // Stepwise Curve ID
   02             // Domain max and count
   1E             //  30C
   20             //  32%
   3C             //  60C
   64             //  100%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0011

   // Sensor Record Header
   1301           // Record ID
   51             // SDR Version
   C0             // Record Type
   0C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   63             // Stepwise Curve ID
   02             // Domain max and count
   1E             //  30C
   33             //  51%
   3C             //  60C
   64             //  100%

//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0011

   // Sensor Record Header
   1401           // Record ID
   51             // SDR Version
   C0             // Record Type
   0C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   02             // FSC Record Type (Global Stepwise Curve Record)

   // Global Stepwise Curve Record
   64             // Stepwise Curve ID
   82             // Domain max and count
   1E             //  30C
   64             //  100%
   3C             //  60C
   64             //  100%

// ******************** END OF GLOBAL RECORDS *********************************

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// R1000 Chassis, All Domains, Profiles 0 & 1
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    001C

   // Sensor Record Header
   1501           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   3F             // Domain Mask
   03             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E		  // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   00             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID



//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// R1000 Chassis, All Domains, Profiles 2 & 3
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    001C

   // Sensor Record Header
   1601           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   3F             // Domain Mask
   0C             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E		  // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   01             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID


//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// R1000 Chassis, All Domains, Profiles 4 & 5
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    001C

   // Sensor Record Header
   1701           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   3F             // Domain Mask
   30             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E		  // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   02             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID


//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// R1000 Chassis, All Domains, Profiles 6 & 7
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    001C

   // Sensor Record Header
   1801           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   3F             // Domain Mask
   C0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E		  // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   03             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID



//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// R1000 Chassis, Domain 0, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    0023

   // Sensor Record Header
   1901           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID (74h = 74h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID (B1h = B1h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   20             // Clamp ID (20h = 20h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID (25h = 25h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID (26h = 26h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID (2Dh = 2Dh)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID (2Eh = 2Eh)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID (5Ch = 5Ch)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID (5Dh = 5Dh)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   94             // Clamp ID (94h = 94h)

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// R1000 Chassis, Domain 1, All Profiles
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    0027

   // Sensor Record Header
   1A01           // Record ID
   51             // SDR Version
   C0             // Record Type
   22             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID (74h = 74h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID (B0h = B0h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID (B1h = B1h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   20             // Clamp ID (20h = 20h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID (25h = 25h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID (22h = 22h)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID (26h = 26h)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID (2Dh = 2Dh)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID (2Eh = 2Eh)
   // Clamp Sub-Record 11   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID (5Ch = 5Ch)
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID (5Dh = 5Dh)
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   94             // Clamp ID (94h = 94h)
   

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// R1000 Chassis, Domain 2, All Profiles
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    0023

   // Sensor Record Header
   1B01           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID (83h = 83h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID (B0h = B0h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   20             // Clamp ID (20h = 20h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID (22h = 22h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID (2Fh = 2Fh)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID (2Eh = 2Eh)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID (5Ch = 5Ch)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID (5Dh = 5Dh)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   94             // Clamp ID (94h = 94h)

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// R1000 Chassis, Domain 3, All Profiles
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    0023

   // Sensor Record Header
   1C01           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID (75h = 75h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID (B0h = B0h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID (22h = 22h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID (2Fh = 2Fh)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID (5Ch = 5Ch)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID (5Dh = 5Dh)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID (2Eh = 2Eh)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   95             // Clamp ID (95h = 95h)

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// R1000 Chassis, Domain 4, All Profiles
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    0021

   // Sensor Record Header
   1D01           // Record ID
   51             // SDR Version
   C0             // Record Type
   1C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   10             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID (75h = 75h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID (B2h = B2h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID (24h = 24h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID (5Ch = 5Ch)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID (5Dh = 5Dh)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID (2Eh = 2Eh)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   95             // Clamp ID (95h = 95h)

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// R1000 Chassis, Domain 5, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    001F

   // Sensor Record Header
   1E01           // Record ID
   51             // SDR Version
   C0             // Record Type
   1A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   20             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID (75h = 75h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID (B2h = B2h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID (24h = 24h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID (5Ch = 5Ch)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID (5Dh = 5Dh)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID (2Eh = 2Eh)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   95             // Clamp ID (95h = 95h)

//*****************************************************************************
// FSC Record Type = 18h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// R1000 Chassis, Domain 6 (Power Supply), All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    0029

   // Sensor Record Header
   1F01           // Record ID
   51             // SDR Version
   C0             // Record Type
   24             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   18             // FSC Record Type (18h = Power Supply Main Domain)
   40             // Domain Mask
   FF             // Fan Profile Support
   
   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   00             // Sensor Exclusion Count (0h = No sensors to exclude)
				  // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0A             // Stepwise Curve ID
   
   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID (84h = 84h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID (B2h = B2h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID (24h = 24h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID (2Eh = 2Eh)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   95             // Clamp ID (95h = 95h)


//*****************************************************************************
// FSC Record Type = 13h (DIMM Air Velocity Record)
// R1000 Chassis
//*****************************************************************************

_SDR_TYPE      C0
_SDR_TAG    'R1000'
_REC_LEN       002D

   // Sensor Record Header
   2001           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   28                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   13                 // Record Subtype (13h = DIMM Air Velocity)

   B0                 // DIMM aggregate sensor number (B0h = DIMM Thrm Mrgn 1)
   06		      // Domain bit mask (06h = Domain 1 & 2)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   06                 // PWM 1 Velocity (06h = 06)
   0C                 // PWM 2 Velocity (0Ch = 12)
   0E                 // PWM 3 Velocity (0Eh = 14)
   07                 // Smoothing coefficient (07h = 7)

   B1                 // DIMM aggregate sensor number (B1h = DIMM Thrm Mrgn 2)
   03		          // Domain bit mask (03h = Domain 0 & 1)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   07                 // PWM 1 Velocity (07h = 07)
   0E                 // PWM 2 Velocity (0Eh = 14)
   11                 // PWM 3 Velocity (11h = 17)
   07                 // Smoothing coefficient (07h = 7)

   B2                 // DIMM aggregate sensor number (B2h = DIMM Thrm Mrgn 3)
   30		          // Domain bit mask (30h = Domain 4 & 5)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   05                 // PWM 1 Velocity (05h = 05)
   0A                 // PWM 2 Velocity (0Ah = 10)
   0D                 // PWM 3 Velocity (0Dh = 13)
   07                 // Smoothing coefficient (07h = 7)
  
   B3                 // DIMM aggregate sensor number (B3h = DIMM Thrm Mrgn 4)
   18		          // Domain bit mask (18h = Domain 3 & 4)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   05                 // PWM 1 Velocity (05h = 05)
   0A                 // PWM 2 Velocity (0Ah = 10)
   0D                 // PWM 3 Velocity (0Dh = 13)
   07                 // Smoothing coefficient (07h = 7)


//*****************************************************************************
// FSC Record Type = 12h (Aggregate Sensor Configuration Record)
// R1000 Chassis, Domain 0
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    001B

   //Sensor Record Header
   2101           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   16                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   12                 // Record sub-type (12h = Aggregate Sensor Configuration)
   C8                 // Aggregate sensor number (C8h = Aggregate Thermal Margin 1)
   08		      // Number of input pairs to follow
   26                 // Input 1 sensor number (26h = I/O Module Temp)
   37                 // Input 1 margin reference value (37h = 55)
   B2                 // Input 2 sensor number (B2h = DIMM Thrm Mrgn 3)
   00                 // Input 2 margin reference value (00h = 0)
   75                 // Input 3 sensor number (75h = P2 Therm Mgn)
   FB                 // Input 3 margin reference value (FBh = -5)
   B0                 // Input 4 sensor number (B0h = P1 Dimm Thrm Mrgn)
   00                 // Input 4 margin reference value (00h = 00)
   5C                 // Input 5 sensor number (5Ch = PS1 Temp)
   37                 // Input 5 margin reference value (37h = 55)
   22                 // Input 6 sensor number (22h = SSB Temp)
   55                 // Input 6 margin reference value (55h = 85)
   2E                 // Input 7 sensor number (2Eh = Exit Air Temp)
   41                 // Input 7 margin reference value (41h = 65)
   74                 // Input 8 sensor number (74h = P1 Thrm Mrgn)
   FB                 // Input 8 margin reference value (FBh = -5)
   

//*****************************************************************************
// FSC Record Type = 11h (System Airflow Formula)
// R1000 Chassis, All Domains
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    0012


   //Sensor Record Header
   2201           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0D                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   11                 // Record sub-type (11h = System air flow)
   3F                 // Domain mask (Domains 1-6)
   1D00   	      // Correction Factor 1 LSB first (001Dh = 29 units of .01)
   2A00               // Correction Factor 2 LSB first (002Ah = 42 units of .01)
   14                 // PWM for Correction Factor 1 (14h = 20%)
   64                 // PWM for Correction Factor 2 (64h = 100%)
   20                 // Max CFM of Fan (20h = 32)
   01                 // Quantity of fans in this equation

//*****************************************************************************
// FSC Record Type = 03h (Fan Sensor Domain Map Record)
// R1000 Chassis
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R1000'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    0020

   // Sensor Record Header
   2301           // Record ID
   51             // SDR Version
   C0             // Record Type
   1B             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   03             // FSC Record Type (03h = Fan Sensor Domain Map)

   // Domain Fan Configuration
   02             // [7:4]-Domain Number = 0; [3:0]-Count of sensor numbers = 2
   30             // Fan Sensor Number 1 (30h = System Fan 1)
   31             // Fan Sensor Number 2 (31h = System Fan 2)
   12             // [7:4]-Domain Number = 1; [3:0]-Count of sensor numbers = 2
   32             // Fan Sensor Number 3 (32h = System Fan 3)
   33             // Fan Sensor Number 4 (33h = System Fan 4)
   22             // [7:4]-Domain Number = 2; [3:0]-Count of sensor numbers = 2
   34             // Fan Sensor Number 5 (34h = System Fan 5)
   35             // Fan Sensor Number 6 (35h = System Fan 6)
   32             // [7:4]-Domain Number = 3; [3:0]-Count of sensor numbers = 2
   36             // Fan Sensor Number 7 (36h = System Fan 7)
   37             // Fan Sensor Number 8 (37h = System Fan 8)
   42             // [7:4]-Domain Number = 4; [3:0]-Count of sensor numbers = 2
   38             // Fan Sensor Number 9 (38h = System Fan 9)
   39             // Fan Sensor Number 10 (39h = System Fan 10)
   52             // [7:4]-Domain Number = 5; [3:0]-Count of sensor numbers = 2
   3A             // Fan Sensor Number 11 (3Ah = System Fan 11)
   3B             // Fan Sensor Number 12 (3Bh = System Fan 12)
   62             // [7:4]-Domain Number = 6; [3:0]-Count of sensor numbers = 2
   A0             // Fan Sensor Number 13 (A0h = Power Supply 1 Fan 1)
   A4             // Fan Sensor Number 14 (A4h = Power Supply 2 Fan 1)


//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// FSC Sub-record Type = 05h (Fans Off)
// R1000 Chassis, Domain 0, All Profiles
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    0016

   // Sensor Record Header
   2401           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   64             // Domain 0 Fan Failure Value (64h = 100% PWM)
   64             // Domain 1 Fan Failure Value (64h = 100% PWM)
   50             // Domain 2 Fan Failure Value (50h = 80% PWM)
   50             // Domain 3 Fan Failure Value (50h = 80% PWM)
   FF             // Domain 4 Fan Failure Value (FFh = No Change)
   FF             // Domain 5 Fan Failure Value (FFh = No Change)
   50             // Domain 6 Fan Failure Value (50h = 80% PWM)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)
  

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// R1000 Chassis, Domain 1, All Profiles
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    0016

   // Sensor Record Header
   2501           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   64             // Domain 0 Fan Failure Value (64h = 100% PWM)
   64             // Domain 1 Fan Failure Value (64h = 100% PWM)
   64             // Domain 2 Fan Failure Value (64h = 100% PWM)
   50             // Domain 3 Fan Failure Value (50h = 80% PWM)
   3C             // Domain 4 Fan Failure Value (3Ch = 60% PWM)
   3C             // Domain 5 Fan Failure Value (3Ch = 60% PWM)
   50             // Domain 6 Fan Failure Value (50h = 80% PWM)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)
   
//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// R1000 Chassis, Domain 2, All Profiles
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    0016

   // Sensor Record Header
   2601           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   64             // Domain 0 Fan Failure Value (64h = 100% PWM)
   64             // Domain 1 Fan Failure Value (64h = 100% PWM)
   64             // Domain 2 Fan Failure Value (64h = 100% PWM)
   64             // Domain 3 Fan Failure Value (64h = 100% PWM)
   50             // Domain 4 Fan Failure Value (50h = 80% PWM)
   50             // Domain 5 Fan Failure Value (50h = 80% PWM)
   64             // Domain 6 Fan Failure Value (64h = 100% PWM)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)
   

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// R1000 Chassis, Domain 3, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    0016

   // Sensor Record Header
   2701           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   64             // Domain 0 Fan Failure Value (64h = 100% PWM)
   64             // Domain 1 Fan Failure Value (64h = 100% PWM)
   64             // Domain 2 Fan Failure Value (64h = 100% PWM)
   64             // Domain 3 Fan Failure Value (64h = 100% PWM)
   64             // Domain 4 Fan Failure Value (64h = 100% PWM)
   64             // Domain 5 Fan Failure Value (64h = 100% PWM)
   64             // Domain 6 Fan Failure Value (64h = 100% PWM)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)
   
//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// R1000 Chassis, Domain 4, All Profiles
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    0016

   // Sensor Record Header
   2801           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   10             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   50             // Domain 0 Fan Failure Value (50h = 80% PWM)
   50             // Domain 1 Fan Failure Value (50h = 80% PWM)
   50             // Domain 2 Fan Failure Value (50h = 80% PWM)
   64             // Domain 3 Fan Failure Value (64h = 100% PWM)
   64             // Domain 4 Fan Failure Value (64h = 100% PWM)
   64             // Domain 5 Fan Failure Value (64h = 100% PWM)
   64             // Domain 6 Fan Failure Value (64h = 100% PWM)   
   FF             // Domain 7 Fan Failure Value (FFh = No Change)
   

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// R1000 Chassis, Domain 5, All Profiles
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    0016

   // Sensor Record Header
   2901           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   20             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   3C             // Domain 0 Fan Failure Value (3Ch = 60% PWM)
   3C             // Domain 1 Fan Failure Value (3Ch = 60% PWM)
   50             // Domain 2 Fan Failure Value (50h = 80% PWM)
   50             // Domain 3 Fan Failure Value (50h = 80% PWM)
   64             // Domain 4 Fan Failure Value (64h = 100% PWM)
   64             // Domain 5 Fan Failure Value (64h = 100% PWM)
   64             // Domain 6 Fan Failure Value (64h = 100% PWM)   
   FF             // Domain 7 Fan Failure Value (FFh = No Change)
   

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// R1000 Chassis, Domain 6 (Power Supply), All Profiles
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    0016

   // Sensor Record Header
   2A01           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   18             // FSC Record Type (18h = Power Supply Main Domain)
   40             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   FF             // Domain 0 Fan Failure Value (FFh = No Change)
   3C             // Domain 1 Fan Failure Value (3Ch = 60% PWM)
   50             // Domain 2 Fan Failure Value (50h = 80% PWM)
   50             // Domain 3 Fan Failure Value (50h = 80% PWM)
   64             // Domain 4 Fan Failure Value (64h = 100% PWM)
   64             // Domain 5 Fan Failure Value (64h = 100% PWM)
   64             // Domain 6 Fan Failure Value (64h = 100% PWM)   
   FF             // Domain 7 Fan Failure Value (FFh = No Change)  
 
//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 05h (Fans Off)
// R1000 Chassis, All Domains, All Profiles
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R1000'
_REC_LEN    0012

   // Sensor Record Header
   2B01           // Record ID
   51             // SDR Version
   C0             // Record Type
   0D             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (18h = Power Supply Main Domain)
   3F             // Domain Mask
   0F             // Fan Profile Support

   // Fans Off Sub-Record
   05             // FSC Sub-Record Type (05h = Fans Off)
   C8             // Sensor Number Controlling Operation (C8h = Aggregate Thermal Margin 1)
   EC             // Fans Off Control Value (ECh = -20 Degrees)
   0A             // Hysteresis (0Ah = 10)
   1E             // Fans Off PWM (1Eh = 30%)

// ************ END OF R1000 RECORDS ***************

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// R2000 Chassis, All Domains, Profiles 0 & 1
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R2000'
_REC_LEN    001C

   // Sensor Record Header
   2C01           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   1F             // Domain Mask
   03             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E		  // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   04             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// R2000 Chassis, All Domains, Profiles 2 & 3
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R2000'
_REC_LEN    001C

   // Sensor Record Header
   2D01           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   1F             // Domain Mask
   0C             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E		  // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   05             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// R2000 Chassis, All Domains, Profiles 4 & 5
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R2000'
_REC_LEN    001C

   // Sensor Record Header
   2E01           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   1F             // Domain Mask
   30             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E		  // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   06             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID
   
   
//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// R2000 Chassis, All Domains, Profiles 6 & 7
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R2000'
_REC_LEN    001C

   // Sensor Record Header
   2F01           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   1F             // Domain Mask
   C0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E		  // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   07             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID
   
    
//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// R2000 Chassis, Domain 0, All Profiles
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R2000'
_REC_LEN    0027

   // Sensor Record Header
   3001           // Record ID
   51             // SDR Version
   C0             // Record Type
   22             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID (74h = 74h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID (B1h = B1h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   20             // Clamp ID (20h = 20h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID (25h = 25h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID (26h = 26h)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID (2Dh = 2Dh)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID (2Eh = 2Eh)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID (75h = 75h)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID (5Ch = 5Ch)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID (5Dh = 5Dh)
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   94             // Clamp ID (94h = 94h)
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   95             // Clamp ID (95h = 95h)


//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// R2000 Chassis, Domain 1, All Profiles
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R2000'
_REC_LEN    002F

   // Sensor Record Header
   3101           // Record ID
   51             // SDR Version
   C0             // Record Type
   2A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID (74h = 74h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID (B0h = B0h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID (B1h = B1h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   20             // Clamp ID (20h = 20h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID (25h = 25h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID (2Ah = 2Ah)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID (22h = 22h)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID (26h = 26h)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID (2Dh = 2Dh)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID (2Fh = 2Fh)
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID (2Eh = 2Eh)   
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID (75h = 75h)   
   // Clamp Sub-Record 14
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID (5Ch = 5Ch)   
   // Clamp Sub-Record 15
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID (5Dh = 5Dh)   
   // Clamp Sub-Record 16
   03             // FSC Sub-Record Type (03h = Clamp)
   94             // Clamp ID (94h = 94h)   
   // Clamp Sub-Record 17
   03             // FSC Sub-Record Type (03h = Clamp)
   95             // Clamp ID (95h = 95h)   
   
//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// R2000 Chassis, Domain 2, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2000'
_REC_LEN    0025

   // Sensor Record Header
   3201           // Record ID
   51             // SDR Version
   C0             // Record Type
   20             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID (83h = 83h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID (84h = 84h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID (B0h = B0h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID (2Ah = 2Ah)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID (22h = 22h)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID (2Fh = 2Fh)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID (2Eh = 2Eh)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID (5Ch = 5Ch)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID (5Dh = 5Dh)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   94             // Clamp ID (94h = 94h)
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   95             // Clamp ID (95h = 95h)

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// R2000 Chassis, Domain 3, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2000'
_REC_LEN    002B

   // Sensor Record Header
   3301           // Record ID
   51             // SDR Version
   C0             // Record Type
   26             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID (75h = 75h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID (B2h = B2h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID (24h = 24h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID (2Ah = 2Ah)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   2B             // Clamp ID (2Bh = 2Bh)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID (22h = 22h)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID (2Fh = 2Fh)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID (5Ch = 5Ch)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID (5Dh = 5Dh)
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID (2Eh = 2Eh)
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID (83h = 83h)
   // Clamp Sub-Record 14
   03             // FSC Sub-Record Type (03h = Clamp)
   94             // Clamp ID (94h = 94h)
   // Clamp Sub-Record 15
   03             // FSC Sub-Record Type (03h = Clamp)
   95             // Clamp ID (95h = 95h)

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// R2000 Chassis, Domain 4, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2000'
_REC_LEN    0023

   // Sensor Record Header
   3401           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   10             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID (75h = 75h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID (B2h = B2h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID (24h = 24h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   2B             // Clamp ID (2Bh = 2Bh)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID (5Ch = 5Ch)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID (5Dh = 5Dh)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID (2Eh = 2Eh)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID (74h = 74h)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   94             // Clamp ID (94h = 94h)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   95             // Clamp ID (95h = 95h)

//*****************************************************************************
// FSC Record Type = 18h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// R2000 Chassis, Domain 5 (Power Supply), All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2000'
_REC_LEN    0029

   // Sensor Record Header
   3501           // Record ID
   51             // SDR Version
   C0             // Record Type
   24             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   18             // FSC Record Type (18h = Power Supply Main Domain)
   20             // Domain Mask
   FF             // Fan Profile Support
   
   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   00             // Sensor Exclusion Count (0h = No sensors to exclude)
				  // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0A             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID (84h = 84h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID (B2h = B2h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID (24h = 24h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID (2Eh = 2Eh)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   95             // Clamp ID (95h = 95h)

//*****************************************************************************
// FSC Record Type = 12h (Aggregate Sensor Configuration Record)
// R2000 Chassis, Domain 0
//*****************************************************************************

_SDR_TYPE      C0
_SDR_TAG    'R2000'
_REC_LEN       001B

   //Sensor Record Header
   3601           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   16                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   12                 // Record sub-type (12h = Aggregate Sensor Configuration)
   C8                 // Aggregate sensor number (C8h = Aggregate Thermal Margin 1)
   08		      // Number of input pairs to follow
   26                 // Input 1 sensor number          (26h = I/O Module Temp)
   37                 // Input 1 margin reference value (37h = 55)
   B2                 // Input 2 sensor number          (B2h = P2 DIMM Thrm Mrgn Group 1)
   00                 // Input 2 margin reference value (00h = 0)
   75                 // Input 3 sensor number          (75h = P2 Therm Mgn)
   FB                 // Input 3 margin reference value (FBh = -5)
   B0                 // Input 4 sensor number          (B0h = P1 Dimm Thrm Mrgn Group 1)
   00                 // Input 4 margin reference value (00h = 00)
   5C                 // Input 5 sensor number          (5Ch = PS1 Temp)
   37                 // Input 5 margin reference value (37h = 55)
   22                 // Input 6 sensor number          (22h = SSB Temp)
   55                 // Input 6 margin reference value (55h = 85)
   2E                 // Input 7 sensor number          (2Eh = Exit Air Temp)
   41                 // Input 7 margin reference value (41h = 65)
   74                 // Input 8 sensor number          (74h = P1 Therm Mrgn)
   FB                 // Input 8 margin reference value (FBh = -5)

//*****************************************************************************
// FSC Record Type = 03h (Fan Sensor Domain Map Record)
// R2000 Chassis
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2000'
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    0018

   // Sensor Record Header
   3701           // Record ID
   51             // SDR Version
   C0             // Record Type
   13             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   03             // FSC Record Type (03h = Fan Sensor Domain Map)

   // Domain Fan Configuration
   01             // [7:4]-Domain Number = 0; [3:0]-Count of sensor numbers = 1
   30             // Fan Sensor Number 1 (30h = System Fan 1) 
   11             // [7:4]-Domain Number = 1; [3:0]-Count of sensor numbers = 1
   32             // Fan Sensor Number 2 (32h = System Fan 3)
   21             // [7:4]-Domain Number = 2; [3:0]-Count of sensor numbers = 1
   34             // Fan Sensor Number 3 (34h = System Fan 5)
   31             // [7:4]-Domain Number = 3; [3:0]-Count of sensor numbers = 1
   36             // Fan Sensor Number 4 (36h = System Fan 7)
   41             // [7:4]-Domain Number = 4; [3:0]-Count of sensor numbers = 1
   38             // Fan Sensor Number 5 (38h = System Fan 9) 
   52             // [7:4]-Domain Number = 5; [3:0]-Count of sensor numbers = 2
   A0             // Fan Sensor Number 6 (A0h = Power Supply 1 Fan 1)
   A4             // Fan Sensor Number 7 (A4h = Power Supply 2 Fan 1)

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// R2000 Chassis, Domain 0, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2000'
_REC_LEN    0016

   // Sensor Record Header
   3801           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   64             // Domain 0 Fan Failure Value (64h = 100% PWM)
   64             // Domain 1 Fan Failure Value (64h = 100% PWM)
   50             // Domain 2 Fan Failure Value (50h = 80% PWM)
   50             // Domain 3 Fan Failure Value (50h = 80% PWM)
   FF             // Domain 4 Fan Failure Value (FFh = No Change)
   50             // Domain 5 Fan Failure Value (50h = 80% PWM)
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// R2000 Chassis, Domain 1, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2000'
_REC_LEN    0016

   // Sensor Record Header
   3901           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   64             // Domain 0 Fan Failure Value (64h = 100% PWM)
   64             // Domain 1 Fan Failure Value (64h = 100% PWM)
   64             // Domain 2 Fan Failure Value (64h = 100% PWM)
   50             // Domain 3 Fan Failure Value (50h = 80% PWM)
   3C             // Domain 4 Fan Failure Value (3Ch = 60% PWM)
   50             // Domain 5 Fan Failure Value (50h = 80% PWM)
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)
  
//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// R2000 Chassis, Domain 2, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2000'
_REC_LEN    0016

   // Sensor Record Header
   3A01           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   64             // Domain 0 Fan Failure Value (64h = 100% PWM)
   64             // Domain 1 Fan Failure Value (64h = 100% PWM)
   64             // Domain 2 Fan Failure Value (64h = 100% PWM)
   64             // Domain 3 Fan Failure Value (64h = 100% PWM)
   50             // Domain 4 Fan Failure Value (50h = 80% PWM)
   64             // Domain 5 Fan Failure Value (64h = 100% PWM)
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// R2000 Chassis, Domain 3, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2000'
_REC_LEN    0016

   // Sensor Record Header
   3B01           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   50             // Domain 0 Fan Failure Value (50h = 80% PWM)
   50             // Domain 1 Fan Failure Value (50h = 80% PWM)
   64             // Domain 2 Fan Failure Value (64h = 100% PWM)
   64             // Domain 3 Fan Failure Value (64h = 100% PWM)
   64             // Domain 4 Fan Failure Value (64h = 100% PWM)
   64             // Domain 5 Fan Failure Value (64h = 100% PWM)   
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// R2000 Chassis, Domain 4
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2000'
_REC_LEN    0016

   // Sensor Record Header
   3C01           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   10             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   3C             // Domain 0 Fan Failure Value (3Ch = 60% PWM)
   3C             // Domain 1 Fan Failure Value (3Ch = 60% PWM)
   50             // Domain 2 Fan Failure Value (50h = 80% PWM)
   64             // Domain 3 Fan Failure Value (64h = 100% PWM)
   64             // Domain 4 Fan Failure Value (64h = 100% PWM)
   64             // Domain 5 Fan Failure Value (64h = 100% PWM)   
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// R2000 Chassis, Domain 5 (Power Supply), All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2000'
_REC_LEN    0016

   // Sensor Record Header
   3D01           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   18             // FSC Record Type (18h = Power Supply Main Domain)
   20             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   FF             // Domain 0 Fan Failure Value (FFh = No Change)
   3C             // Domain 1 Fan Failure Value (3Ch = 60% PWM)
   50             // Domain 2 Fan Failure Value (50h = 80% PWM)
   64             // Domain 3 Fan Failure Value (64h = 100% PWM)
   64             // Domain 4 Fan Failure Value (64h = 100% PWM)
   64             // Domain 5 Fan Failure Value (64h = 100% PWM)   
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)


//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 05h (Fans Off)
// R2000 Chassis, All Domains, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2000'
_REC_LEN    0012

   // Sensor Record Header
   3E01           // Record ID
   51             // SDR Version
   C0             // Record Type
   0D             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (18h = Power Supply Main Domain)
   1F             // Domain Mask
   0F             // Fan Profile Support

   // Fans Off Sub-Record
   05             // FSC Sub-Record Type (05h = Fans Off)
   C8             // Sensor Number Controlling Operation (C8h = Aggregate Thermal Margin 1)
   EC             // Fans Off Control Value (ECh = -20 Degrees)
   0A             // Hysteresis (0Ah = 10)
   14             // Fans Off PWM (14h = 20%)

// END OF R2000 RECORDS

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// R2AUXCOOL Chassis, All Domains, Profiles 0 & 1
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    001C

   // Sensor Record Header
   3F01           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   1F             // Domain Mask
   03             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E		  // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   04             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// R2AUXCOOL Chassis, All Domains, Profiles 2 & 3
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    001C

   // Sensor Record Header
   4001           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   1F             // Domain Mask
   0C             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E		  // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   05             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// R2AUXCOOL Chassis, All Domains, Profiles 4 & 5
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    001C

   // Sensor Record Header
   4101           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   1F             // Domain Mask
   30             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E		  // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   06             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID
   
   
//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// R2AUXCOOL Chassis, All Domains, Profiles 6 & 7
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    001C

   // Sensor Record Header
   4201           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   1F             // Domain Mask
   C0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E		  // Sensor Number To Exclude From Fan Boost   
                  
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   07             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID
   
//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// R2AUXCOOL Chassis, Domain 0, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    0021

   // Sensor Record Header
   4301           // Record ID
   51             // SDR Version
   C0             // Record Type
   1C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   83             // Clamp ID (83h = 83h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID (B1h = B1h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   20             // Clamp ID (20h = 20h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID (25h = 25h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID (26h = 26h)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID (2Dh = 2Dh)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID (2Eh = 2Eh)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   00             // Clamp ID (00h = 00h)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   01             // Clamp ID (01h = 01h)

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// R2AUXCOOL Chassis, Domain 1, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    0029

   // Sensor Record Header
   4401           // Record ID
   51             // SDR Version
   C0             // Record Type
   24             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   83             // Clamp ID (83h = 83h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID (B0h = B0h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID (B1h = B1h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   20             // Clamp ID (20h = 20h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID (25h = 25h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID (2Ah = 2Ah)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID (22h = 22h)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID (26h = 26h)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID (2Dh = 2Dh)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID (2Fh = 2Fh)
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID (2Eh = 2Eh)   
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   00             // Clamp ID (00h = 00h)   
   // Clamp Sub-Record 14
   03             // FSC Sub-Record Type (03h = Clamp)
   01             // Clamp ID (01h = 01h)   

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// R2AUXCOOL Chassis, Domain 2, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    0021

   // Sensor Record Header
   4501           // Record ID
   51             // SDR Version
   C0             // Record Type
   1C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   83             // Clamp ID (83h = 83h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   84             // Clamp ID (84h = 84h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID (B0h = B0h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID (2Ah = 2Ah)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID (22h = 22h)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID (2Fh = 2Fh)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID (2Eh = 2Eh)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   00             // Clamp ID (00h = 00h)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   01             // Clamp ID (01h = 01h)

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// R2AUXCOOL Chassis, Domain 3, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    0025

   // Sensor Record Header
   4601           // Record ID
   51             // SDR Version
   C0             // Record Type
   20             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   84             // Clamp ID (84h = 84h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID (B2h = B2h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID (24h = 24h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID (2Ah = 2Ah)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   2B             // Clamp ID (2Bh = 2Bh)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID (22h = 22h)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID (2Fh = 2Fh)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   00             // Clamp ID (00h = 00h)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   01             // Clamp ID (01h = 01h)
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID (2Eh = 2Eh)

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// R2AUXCOOL Chassis, Domain 4, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    001D

   // Sensor Record Header
   4701           // Record ID
   51             // SDR Version
   C0             // Record Type
   18             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   10             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   84             // Clamp ID (84h = 84h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID (B2h = B2h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID (24h = 24h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   2B             // Clamp ID (2Bh = 2Bh)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   00             // Clamp ID (00h = 00h)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   01             // Clamp ID (01h = 01h)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID (2Eh = 2Eh)


//*****************************************************************************
// FSC Record Type = 18h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// R2AUXCOOL Chassis, Domain 5 (Power Supply), All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    0028

   // Sensor Record Header
   4801           // Record ID
   51             // SDR Version
   C0             // Record Type
   23             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   18             // FSC Record Type (18h = Power Supply Main Domain)
   20             // Domain Mask
   FF             // Fan Profile Support
   
   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (0h = No sensors to exclude)
   2E	          // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0A             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   84             // Clamp ID (84h = 84h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID (B2h = B2h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID (24h = 24h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID (2Eh = 2Eh)


//*****************************************************************************
// FSC Record Type = 13h (DIMM Air Velocity Record)
// R2AUXCOOL Chassis
//*****************************************************************************

_SDR_TYPE      C0
_SDR_TAG    'R2AUXCOOL'
_REC_LEN       002D

   // Sensor Record Header
   4901           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   28                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   13                 // Record Subtype (13h = DIMM Air Velocity)

   B0                 // DIMM aggregate sensor number (B0h = DIMM Thrm Mrgn 1)
   06		          // Domain bit mask (06h = Domain 1 & 2)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   07                 // PWM 1 Velocity (07h = 07)
   0E                 // PWM 2 Velocity (0Eh = 14)
   11                 // PWM 3 Velocity (11h = 17)
   07                 // Smoothing coefficient (07h = 7)

   B1                 // DIMM aggregate sensor number (B1h = DIMM Thrm Mrgn 2)
   03		          // Domain bit mask (03h = Domain 0 & 1)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   07                 // PWM 1 Velocity (07h = 07)
   10                 // PWM 2 Velocity (10h = 16)
   14                 // PWM 3 Velocity (14h = 20)
   07                 // Smoothing coefficient (07h = 7)

   B2                 // DIMM aggregate sensor number (B2h = DIMM Thrm Mrgn 3)
   30		          // Domain bit mask (30h = Domain 4 & 5)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   08                 // PWM 1 Velocity (08h = 08)
   11                 // PWM 2 Velocity (11h = 17)
   17                 // PWM 3 Velocity (17h = 23)
   07                 // Smoothing coefficient (07h = 7)
  
   B3                 // DIMM aggregate sensor number (B3h = DIMM Thrm Mrgn 4)
   18		          // Domain bit mask (18h = Domain 3 & 4)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   07                 // PWM 1 Velocity (07h = 07)
   0E                 // PWM 2 Velocity (0Eh = 14)
   11                 // PWM 3 Velocity (11h = 17)
   07                 // Smoothing coefficient (07h = 7)

//*****************************************************************************
// FSC Record Type = 11h (System Airflow Formula)
// R2AUXCOOL Chassis, All Domains
//*****************************************************************************

_SDR_TYPE      C0
_SDR_TAG    'R2AUXCOOL'
_REC_LEN       0012

   //Sensor Record Header
   4A01           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0D                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   11                 // Record sub-type (11h = System air flow)
   1F                 // Domain mask (Domains 0-4)
   2600   	      // Correction Factor 1 LSB first (0026h = 38 units of .01)
   2A00               // Correction Factor 2 LSB first (002Ah = 42 units of .01)
   19                 // PWM for Correction Factor 1 (19h = 25%)
   64                 // PWM for Correction Factor 2 (64h = 100%)
   42                 // Max CFM of Fan (42h = 66)
   01                 // Quantity of fans in this equation


//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// R2AUXCOOL Chassis, Domain 0, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    0016

   // Sensor Record Header
   4B01           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   64             // Domain 0 Fan Failure Value (64h = 100% PWM)
   64             // Domain 1 Fan Failure Value (64h = 100% PWM)
   50             // Domain 2 Fan Failure Value (50h = 80% PWM)
   50             // Domain 3 Fan Failure Value (50h = 80% PWM)
   FF             // Domain 4 Fan Failure Value (FFh = No Change)
   50             // Domain 5 Fan Failure Value (50h = 80% PWM)
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// R2AUXCOOL Chassis, Domain 5 (Power Supply), All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    0016

   // Sensor Record Header
   4C01           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   18             // FSC Record Type (18h = Power Supply Main Domain)
   20             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   FF             // Domain 0 Fan Failure Value (FFh = No Change)
   3C             // Domain 1 Fan Failure Value (3Ch = 60% PWM)
   50             // Domain 2 Fan Failure Value (50h = 80% PWM)
   64             // Domain 3 Fan Failure Value (64h = 100% PWM)
   64             // Domain 4 Fan Failure Value (64h = 100% PWM)
   64             // Domain 5 Fan Failure Value (64h = 100% PWM)   
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// R2AUXCOOL Chassis, Domain 1, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    0016

   // Sensor Record Header
   4D01           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   64             // Domain 0 Fan Failure Value (64h = 100% PWM)
   64             // Domain 1 Fan Failure Value (64h = 100% PWM)
   64             // Domain 2 Fan Failure Value (64h = 100% PWM)
   50             // Domain 3 Fan Failure Value (50h = 80% PWM)
   3C             // Domain 4 Fan Failure Value (3Ch = 60% PWM)
   50             // Domain 5 Fan Failure Value (50h = 80% PWM)
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// R2AUXCOOL Chassis, Domain 2, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    0016

   // Sensor Record Header
   4E01           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   64             // Domain 0 Fan Failure Value (64h = 100% PWM)
   64             // Domain 1 Fan Failure Value (64h = 100% PWM)
   64             // Domain 2 Fan Failure Value (64h = 100% PWM)
   64             // Domain 3 Fan Failure Value (64h = 100% PWM)
   50             // Domain 4 Fan Failure Value (50h = 80% PWM)
   64             // Domain 5 Fan Failure Value (64h = 100% PWM)
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)


//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// R2AUXCOOL Chassis, Domain 3, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    0016

   // Sensor Record Header
   4F01           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   50             // Domain 0 Fan Failure Value (50h = 80% PWM)
   50             // Domain 1 Fan Failure Value (50h = 80% PWM)
   64             // Domain 2 Fan Failure Value (64h = 100% PWM)
   64             // Domain 3 Fan Failure Value (64h = 100% PWM)
   64             // Domain 4 Fan Failure Value (64h = 100% PWM)
   64             // Domain 5 Fan Failure Value (64h = 100% PWM)   
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)


//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// R2AUXCOOL Chassis, Domain 4
//*****************************************************************************


_SDR_TYPE   C0
_SDR_TAG    'R2AUXCOOL'
_REC_LEN    0016

   // Sensor Record Header
   5001           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   10             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   3C             // Domain 0 Fan Failure Value (3Ch = 60% PWM)
   3C             // Domain 1 Fan Failure Value (3Ch = 60% PWM)
   50             // Domain 2 Fan Failure Value (50h = 80% PWM)
   64             // Domain 3 Fan Failure Value (64h = 100% PWM)
   64             // Domain 4 Fan Failure Value (64h = 100% PWM)
   64             // Domain 5 Fan Failure Value (64h = 100% PWM)   
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)



// END OF R2AUXCOOL RECORDS

//*****************************************************************************
// FSC Record Type = 13h (DIMM Air Velocity Record)
// R2XXX Chassis
//*****************************************************************************

_SDR_TYPE      C0
_SDR_TAG    'R2XXX'
_REC_LEN       002D

   // Sensor Record Header
   5101           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   28                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   13                 // Record Subtype (13h = DIMM Air Velocity)

   B0                 // DIMM aggregate sensor number (B0h = DIMM Thrm Mrgn 1)
   06		          // Domain bit mask (06h = Domain 1 & 2)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   07                 // PWM 1 Velocity (07h = 07)
   0E                 // PWM 2 Velocity (0Eh = 14)
   11                 // PWM 3 Velocity (11h = 17)
   07                 // Smoothing coefficient (07h = 7)

   B1                 // DIMM aggregate sensor number (B1h = DIMM Thrm Mrgn 2)
   03		          // Domain bit mask (03h = Domain 0 & 1)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   07                 // PWM 1 Velocity (07h = 07)
   10                 // PWM 2 Velocity (10h = 16)
   14                 // PWM 3 Velocity (14h = 20)
   07                 // Smoothing coefficient (07h = 7)

   B2                 // DIMM aggregate sensor number (B2h = DIMM Thrm Mrgn 3)
   30		          // Domain bit mask (30h = Domain 4 & 5)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   08                 // PWM 1 Velocity (08h = 08)
   11                 // PWM 2 Velocity (11h = 17)
   17                 // PWM 3 Velocity (17h = 23)
   07                 // Smoothing coefficient (07h = 7)
  
   B3                 // DIMM aggregate sensor number (B3h = DIMM Thrm Mrgn 4)
   18		          // Domain bit mask (18h = Domain 3 & 4)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   07                 // PWM 1 Velocity (07h = 07)
   0E                 // PWM 2 Velocity (0Eh = 14)
   11                 // PWM 3 Velocity (11h = 17)
   07                 // Smoothing coefficient (07h = 7)

//*****************************************************************************
// FSC Record Type = 11h (System Airflow Formula)
// R2XXX Chassis, All Domains
//*****************************************************************************


_SDR_TYPE      C0
_SDR_TAG    'R2XXX'
_REC_LEN       0012


   //Sensor Record Header
   5201           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0D                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   11                 // Record sub-type (11h = System air flow)
   1F                 // Domain mask (Domains 0-4)
   2600   		      // Correction Factor 1 LSB first (0026h = 38 units of .01)
   2A00               // Correction Factor 2 LSB first (002Ah = 42 units of .01)
   19                 // PWM for Correction Factor 1 (19h = 25%)
   64                 // PWM for Correction Factor 2 (64h = 100%)
   42                 // Max CFM of Fan (42h = 66)
   01                 // Quantity of fans in this equation

// END OF R2XXX RECORDS

//*****************************************************************************
// FSC Record Type = 13h (DIMM Air Velocity Record)
// R2224 Chassis
//*****************************************************************************

   
_SDR_TYPE      C0
_SDR_TAG    'R2224'
_REC_LEN       002D

   // Sensor Record Header
   5301           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   28                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   13                 // Record Subtype (13h = DIMM Air Velocity)

   B0                 // DIMM aggregate sensor number (B0h = DIMM Thrm Mrgn 1)
   06		          // Domain bit mask (06h = Domain 1 & 2)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   06                 // PWM 1 Velocity (06h = 06)
   0D                 // PWM 2 Velocity (0Dh = 13)
   10                 // PWM 3 Velocity (10h = 16)
   07                 // Smoothing coefficient (07h = 7)

   B1                 // DIMM aggregate sensor number (B1h = DIMM Thrm Mrgn 2)
   03		          // Domain bit mask (03h = Domain 0 & 1)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   07                 // PWM 1 Velocity (07h = 07)
   0E                 // PWM 2 Velocity (0Eh = 14)
   12                 // PWM 3 Velocity (12h = 18)
   07                 // Smoothing coefficient (07h = 7)

   B2                 // DIMM aggregate sensor number (B2h = DIMM Thrm Mrgn 3)
   30		          // Domain bit mask (30h = Domain 4 & 5)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   07                 // PWM 1 Velocity (07h = 07)
   0E                 // PWM 2 Velocity (0Eh = 14)
   14                 // PWM 3 Velocity (14h = 20)
   07                 // Smoothing coefficient (07h = 7)
  
   B3                 // DIMM aggregate sensor number (B3h = DIMM Thrm Mrgn 4)
   18		          // Domain bit mask (18h = Domain 3 & 4)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   05                 // PWM 1 Velocity (05h = 05)
   0B                 // PWM 2 Velocity (0Bh = 11)
   0E                 // PWM 3 Velocity (0Eh = 14)
   07                 // Smoothing coefficient (07h = 7)

//*****************************************************************************
// FSC Record Type = 11h (System Airflow Formula)
// R2224 Chassis, All Domains
//*****************************************************************************

_SDR_TYPE      C0
_SDR_TAG    'R2224'
_REC_LEN       0012


   //Sensor Record Header
   5401           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0D                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   11                 // Record sub-type (11h = System air flow)
   1F                 // Domain mask (Domains 0-4)
   2000   		      // Correction Factor 1 LSB first (0020h = 32 units of .01)
   2200               // Correction Factor 2 LSB first (0022h = 34 units of .01)
   19                 // PWM for Correction Factor 1 (19h = 25%)
   64                 // PWM for Correction Factor 2 (64h = 100%)
   42                 // Max CFM of Fan (42h = 66)
   01                 // Quantity of fans in this equation

// END OF R2224 RECORDS

//*****************************************************************************
// FSC Record Type = 13h (DIMM Air Velocity Record)
// R2312 Chassis
//*****************************************************************************

_SDR_TYPE      C0
_SDR_TAG    'R2312'
_REC_LEN       002D

   // Sensor Record Header
   5501           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   28                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   13                 // Record Subtype (13h = DIMM Air Velocity)

   B0                 // DIMM aggregate sensor number (B0h = DIMM Thrm Mrgn 1)
   06		          // Domain bit mask (06h = Domain 1 & 2)
   28                 // Reference PWM % 1 (28h = 40%)
   46                 // Reference PWM % 2 (46h = 70%)
   64                 // Reference PWM % 3 (64h = 100%)
   08                 // PWM 1 Velocity (08h = 08)
   0D                 // PWM 2 Velocity (0Dh = 13)
   10                 // PWM 3 Velocity (10h = 16)
   07                 // Smoothing coefficient (07h = 7)

   B1                 // DIMM aggregate sensor number (B1h = DIMM Thrm Mrgn 2)
   03		          // Domain bit mask (03h = Domain 0 & 1)
   28                 // Reference PWM % 1 (28h = 40%)
   46                 // Reference PWM % 2 (46h = 70%)
   64                 // Reference PWM % 3 (64h = 100%)
   09                 // PWM 1 Velocity (09h = 09)
   0E                 // PWM 2 Velocity (0Eh = 14)
   12                 // PWM 3 Velocity (12h = 18)
   07                 // Smoothing coefficient (07h = 7)

   B2                 // DIMM aggregate sensor number (B2h = DIMM Thrm Mrgn 3)
   30		          // Domain bit mask (30h = Domain 4 & 5)
   28                 // Reference PWM % 1 (28h = 40%)
   46                 // Reference PWM % 2 (46h = 70%)
   64                 // Reference PWM % 3 (64h = 100%)
   09                 // PWM 1 Velocity (09h = 09)
   0E                 // PWM 2 Velocity (0Eh = 14)
   14                 // PWM 3 Velocity (14h = 20)
   07                 // Smoothing coefficient (07h = 7)
  
   B3                 // DIMM aggregate sensor number (B3h = DIMM Thrm Mrgn 4)
   18		          // Domain bit mask (18h = Domain 3 & 4)
   28                 // Reference PWM % 1 (28h = 40%)
   46                 // Reference PWM % 2 (46h = 70%)
   64                 // Reference PWM % 3 (64h = 100%)
   07                 // PWM 1 Velocity (07h = 07)
   0B                 // PWM 2 Velocity (0Bh = 11)
   0E                 // PWM 3 Velocity (0Eh = 14)
   07                 // Smoothing coefficient (07h = 7)
   
//*****************************************************************************
// FSC Record Type = 11h (System Airflow Formula)
// R2312 Chassis, All Domains
//*****************************************************************************


_SDR_TYPE      C0
_SDR_TAG    'R2312'
_REC_LEN       0012


   //Sensor Record Header
   5601           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0D                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   11                 // Record sub-type (11h = System air flow)
   1F                 // Domain mask (Domains 0-4)
   1800   		      // Correction Factor 1 LSB first (0020h = 24 units of .01)
   1D00               // Correction Factor 2 LSB first (0022h = 29 units of .01)
   19                 // PWM for Correction Factor 1 (19h = 25%)
   64                 // PWM for Correction Factor 2 (64h = 100%)
   42                 // Max CFM of Fan (42h = 66)
   01                 // Quantity of fans in this equation
   
// END OF R2312 RECORDS
   

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Other Chassis, All Domains, All Profiles
//*****************************************************************************
_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0019

   // Sensor Record Header
   5701           // Record ID
   51             // SDR Version
   C0             // Record Type
   14             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask (All Domains)
   FF             // Fan Profile Support 
   
   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   64             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (0h = No sensors to exclude)
   2E		  // Sensor Number To Exclude From Fan Boost   
                  
   // Note that Lower Clipping curve sub-records are defined in the Other Slow Ramp,
   // Medium Ramp, and Fast Ramp sections below.

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID (64h = 100)
   
//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Other Chassis, Domain 0, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    002F

   // Sensor Record Header
   5801           // Record ID
   51             // SDR Version
   C0             // Record Type
   2A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID (B0h = B0h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID (B1h = B1h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID (B2h = B2h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   20             // Clamp ID (20h = 20h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID (24h = 24h)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID (25h = 25h)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID (2Ah = 2Ah)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   2B             // Clamp ID (2Bh = 2Bh)
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID (22h = 22h)
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID (26h = 26h)
   // Clamp Sub-Record 14
   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID (2Dh = 2Dh)
   // Clamp Sub-Record 15
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID (2Fh = 2Fh)
   // Clamp Sub-Record 16
   03             // FSC Sub-Record Type (03h = Clamp)
   83             // Clamp ID (83h = 83h)
   // Clamp Sub-Record 17
   03             // FSC Sub-Record Type (03h = Clamp)
   84             // Clamp ID (84h = 84h)
   

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Other Chassis, Domain 1, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    002F

   // Sensor Record Header
   5901           // Record ID
   51             // SDR Version
   C0             // Record Type
   2A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID (B0h = B0h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID (B1h = B1h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID (B2h = B2h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   20             // Clamp ID (20h = 20h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID (24h = 24h)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID (25h = 25h)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID (2Ah = 2Ah)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   2B             // Clamp ID (2Bh = 2Bh)
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID (22h = 22h)
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID (26h = 26h)
   // Clamp Sub-Record 14
   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID (2Dh = 2Dh)
   // Clamp Sub-Record 15
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID (2Fh = 2Fh)
   // Clamp Sub-Record 16
   03             // FSC Sub-Record Type (03h = Clamp)
   83             // Clamp ID (83h = 83h)
   // Clamp Sub-Record 17
   03             // FSC Sub-Record Type (03h = Clamp)
   84             // Clamp ID (84h = 84h)
   
//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Other Chassis, Domain 2, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    002F

   // Sensor Record Header
   5A01           // Record ID
   51             // SDR Version
   C0             // Record Type
   2A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID (B0h = B0h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID (B1h = B1h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID (B2h = B2h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   20             // Clamp ID (20h = 20h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID (24h = 24h)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID (25h = 25h)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID (2Ah = 2Ah)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   2B             // Clamp ID (2Bh = 2Bh)
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID (22h = 22h)
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID (26h = 26h)
   // Clamp Sub-Record 14
   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID (2Dh = 2Dh)
   // Clamp Sub-Record 15
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID (2Fh = 2Fh)
   // Clamp Sub-Record 16
   03             // FSC Sub-Record Type (03h = Clamp)
   83             // Clamp ID (83h = 83h)
   // Clamp Sub-Record 17
   03             // FSC Sub-Record Type (03h = Clamp)
   84             // Clamp ID (84h = 84h)
   
//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Other Chassis, Domain 3, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    002F

   // Sensor Record Header
   5B01           // Record ID
   51             // SDR Version
   C0             // Record Type
   2A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   08             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID (B0h = B0h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID (B1h = B1h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID (B2h = B2h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   20             // Clamp ID (20h = 20h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID (24h = 24h)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID (25h = 25h)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID (2Ah = 2Ah)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   2B             // Clamp ID (2Bh = 2Bh)
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID (22h = 22h)
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID (26h = 26h)
   // Clamp Sub-Record 14
   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID (2Dh = 2Dh)
   // Clamp Sub-Record 15
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID (2Fh = 2Fh)
   // Clamp Sub-Record 16
   03             // FSC Sub-Record Type (03h = Clamp)
   83             // Clamp ID (83h = 83h)
   // Clamp Sub-Record 17
   03             // FSC Sub-Record Type (03h = Clamp)
   84             // Clamp ID (84h = 84h)
   
//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Other Chassis, Domain 4, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    002F

   // Sensor Record Header
   5C01           // Record ID
   51             // SDR Version
   C0             // Record Type
   2A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   10             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID (B0h = B0h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID (B1h = B1h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID (B2h = B2h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   20             // Clamp ID (20h = 20h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID (24h = 24h)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID (25h = 25h)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID (2Ah = 2Ah)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   2B             // Clamp ID (2Bh = 2Bh)
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID (22h = 22h)
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID (26h = 26h)
   // Clamp Sub-Record 14
   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID (2Dh = 2Dh)
   // Clamp Sub-Record 15
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID (2Fh = 2Fh)
   // Clamp Sub-Record 16
   03             // FSC Sub-Record Type (03h = Clamp)
   83             // Clamp ID (83h = 83h)
   // Clamp Sub-Record 17
   03             // FSC Sub-Record Type (03h = Clamp)
   84             // Clamp ID (84h = 84h)
   
//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Other Chassis, Domain 5, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    002F

   // Sensor Record Header
   5D01           // Record ID
   51             // SDR Version
   C0             // Record Type
   2A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   20             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID (B0h = B0h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID (B1h = B1h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID (B2h = B2h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   20             // Clamp ID (20h = 20h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID (24h = 24h)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID (25h = 25h)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID (2Ah = 2Ah)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   2B             // Clamp ID (2Bh = 2Bh)
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID (22h = 22h)
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID (26h = 26h)
   // Clamp Sub-Record 14
   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID (2Dh = 2Dh)
   // Clamp Sub-Record 15
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID (2Fh = 2Fh)
   // Clamp Sub-Record 16
   03             // FSC Sub-Record Type (03h = Clamp)
   83             // Clamp ID (83h = 83h)
   // Clamp Sub-Record 17
   03             // FSC Sub-Record Type (03h = Clamp)
   84             // Clamp ID (84h = 84h)
   
//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Other Chassis, Domain 6, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    002F

   // Sensor Record Header
   5E01           // Record ID
   51             // SDR Version
   C0             // Record Type
   2A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   40             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID (B0h = B0h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID (B1h = B1h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID (B2h = B2h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   20             // Clamp ID (20h = 20h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID (24h = 24h)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID (25h = 25h)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID (2Ah = 2Ah)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   2B             // Clamp ID (2Bh = 2Bh)
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID (22h = 22h)
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID (26h = 26h)
   // Clamp Sub-Record 14
   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID (2Dh = 2Dh)
   // Clamp Sub-Record 15
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID (2Fh = 2Fh)
   // Clamp Sub-Record 16
   03             // FSC Sub-Record Type (03h = Clamp)
   83             // Clamp ID (83h = 83h)
   // Clamp Sub-Record 17
   03             // FSC Sub-Record Type (03h = Clamp)
   84             // Clamp ID (84h = 84h)
   
//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Other Chassis, Domain 7, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    002F

   // Sensor Record Header
   5F01           // Record ID
   51             // SDR Version
   C0             // Record Type
   2A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   80             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID (B0h = B0h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID (B1h = B1h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID (B2h = B2h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   20             // Clamp ID (20h = 20h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID (24h = 24h)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID (25h = 25h)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID (2Ah = 2Ah)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   2B             // Clamp ID (2Bh = 2Bh)
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID (22h = 22h)
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID (26h = 26h)
   // Clamp Sub-Record 14
   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID (2Dh = 2Dh)
   // Clamp Sub-Record 15
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID (2Fh = 2Fh)
   // Clamp Sub-Record 16
   03             // FSC Sub-Record Type (03h = Clamp)
   83             // Clamp ID (83h = 83h)
   // Clamp Sub-Record 17
   03             // FSC Sub-Record Type (03h = Clamp)
   84             // Clamp ID (84h = 84h)
   
   
//*****************************************************************************
// FSC Record Type = 13h (DIMM Air Velocity Record)
// Other Chassis
//*****************************************************************************

   
_SDR_TYPE      C0
_SDR_TAG    'OTHER'
_REC_LEN       002D

   // Sensor Record Header
   6001           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   28                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   13                 // Record Subtype (13h = DIMM Air Velocity)

   B0                 // DIMM aggregate sensor number (B0h = DIMM Thrm Mrgn 1)
   FF		          // Domain bit mask (FFh = All Domains)
   00                 // Reference PWM % 1 (0h = 0%)
   32                 // Reference PWM % 2 (32h = 50%)
   64                 // Reference PWM % 3 (64h = 100%)
   0A                 // PWM 1 Velocity (0Ah = 10)
   0A                 // PWM 2 Velocity (0Ah = 10)
   0A                 // PWM 3 Velocity (0Ah = 10)
   07                 // Smoothing coefficient (07h = 7)

   B1                 // DIMM aggregate sensor number (B1h = DIMM Thrm Mrgn 2)
   FF		          // Domain bit mask (FFh = All Domains)
   00                 // Reference PWM % 1 (0h = 0%)
   32                 // Reference PWM % 2 (32h = 50%)
   64                 // Reference PWM % 3 (64h = 100%)
   0A                 // PWM 1 Velocity (0Ah = 10)
   0A                 // PWM 2 Velocity (0Ah = 10)
   0A                 // PWM 3 Velocity (0Ah = 10)
   07                 // Smoothing coefficient (07h = 7)

   B2                 // DIMM aggregate sensor number (B2h = DIMM Thrm Mrgn 3)
   FF		          // Domain bit mask (FFh = All Domains)
   00                 // Reference PWM % 1 (0h = 0%)
   32                 // Reference PWM % 2 (32h = 50%)
   64                 // Reference PWM % 3 (64h = 100%)
   0A                 // PWM 1 Velocity (0Ah = 10)
   0A                 // PWM 2 Velocity (0Ah = 10)
   0A                 // PWM 3 Velocity (0Ah = 10)
   07                 // Smoothing coefficient (07h = 7)
  
   B3                 // DIMM aggregate sensor number (B3h = DIMM Thrm Mrgn 4)
   FF		          // Domain bit mask (FFh = All Domains)
   00                 // Reference PWM % 1 (0h = 0%)
   32                 // Reference PWM % 2 (32h = 50%)
   64                 // Reference PWM % 3 (64h = 100%)
   0A                 // PWM 1 Velocity (0Ah = 10)
   0A                 // PWM 2 Velocity (0Ah = 10)
   0A                 // PWM 3 Velocity (0Ah = 10)
   07                 // Smoothing coefficient (07h = 7)
   
//*****************************************************************************
// FSC Record Type = 03h (Fan Sensor Domain Map Record)
// Other Chassis
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0021

   // Sensor Record Header
   6101           // Record ID
   51             // SDR Version
   C0             // Record Type
   1C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   03             // FSC Record Type (03h = Fan Sensor Domain Map)

   // Domain Fan Configuration
   02             // [7:4]-Domain Number = 0; [3:0]-Count of sensor numbers = 2
   30             // Fan Sensor Number 1 (30h = System Fan 1)
   31             // Fan Sensor Number 2 (31h = System Fan 2)
   12             // [7:4]-Domain Number = 1; [3:0]-Count of sensor numbers = 2
   32             // Fan Sensor Number 3 (32h = System Fan 3)
   33             // Fan Sensor Number 4 (33h = System Fan 4)
   22             // [7:4]-Domain Number = 2; [3:0]-Count of sensor numbers = 2
   34             // Fan Sensor Number 5 (34h = System Fan 5)
   35             // Fan Sensor Number 6 (35h = System Fan 6)
   32             // [7:4]-Domain Number = 3; [3:0]-Count of sensor numbers = 2
   36             // Fan Sensor Number 7 (36h = System Fan 7)
   37             // Fan Sensor Number 8 (37h = System Fan 8)
   42             // [7:4]-Domain Number = 4; [3:0]-Count of sensor numbers = 2
   38             // Fan Sensor Number 9 (38h = System Fan 9)
   39             // Fan Sensor Number 10 (39h = System Fan 10)
   52             // [7:4]-Domain Number = 5; [3:0]-Count of sensor numbers = 2
   3A             // Fan Sensor Number 11 (3Ah = System Fan 11)
   3B             // Fan Sensor Number 12 (3Bh = System Fan 12)
   61             // [7:4]-Domain Number = 6; [3:0]-Count of sensor numbers = 1
   3C             // Fan Sensor Number 13 (3Ch = )
   71             // [7:4]-Domain Number = 7; [3:0]-Count of sensor numbers = 1
   3D             // Fan Sensor Number 13 (3Ch = )

//*****************************************************************************
// Main Domain Record, Other & Slow Ramp Configuration, All Domains 
//*****************************************************************************


//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Other Chassis Slow Ramp, All Domains, Profiles 0 & 1 & 2 & 3
//*****************************************************************************
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_REC_LEN    0010

   // Sensor Record Header
   6201           // Record ID
   51             // SDR Version
   C0             // Record Type
   0B             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask (All Domains)
   0F             // Fan Profile Support 
   
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5B             // Stepwise Curve ID (5Bh = 91)
   
//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Other Chassis Slow Ramp, All Domains, Profiles 4 & 5
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_REC_LEN    0010

   // Sensor Record Header
   6301           // Record ID
   51             // SDR Version
   C0             // Record Type
   0B             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask (All Domains)
   30             // Fan Profile Support 
   
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5C             // Stepwise Curve ID (5Ch = 92)


//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Other Chassis Slow Ramp, All Domains, Profiles 6 & 7
//*****************************************************************************
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_REC_LEN    0010

   // Sensor Record Header
   6401           // Record ID
   51             // SDR Version
   C0             // Record Type
   0B             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask (All Domains)
   C0             // Fan Profile Support 
   
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5D             // Stepwise Curve ID (5Dh = 93)

//*****************************************************************************
// Main Domain Record, Other & Med Ramp Configuration, All Domains 
//*****************************************************************************

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Other Chassis Med Ramp, All Domains, Profiles 0 & 1 & 2 & 3
//*****************************************************************************
_SDR_TYPE   C0
_SDR_TAG    'OTHER_MR'
_REC_LEN    0010

   // Sensor Record Header
   6501           // Record ID
   51             // SDR Version
   C0             // Record Type
   0B             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask (All Domains)
   0F             // Fan Profile Support 
   
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5E             // Stepwise Curve ID (5Eh = 94)


//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Other Chassis Med Ramp, All Domains, Profiles 4 & 5
//*****************************************************************************
_SDR_TYPE   C0
_SDR_TAG    'OTHER_MR'
_REC_LEN    0010

   // Sensor Record Header
   6601           // Record ID
   51             // SDR Version
   C0             // Record Type
   0B             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask (All Domains)
   30             // Fan Profile Support 
   
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5F             // Stepwise Curve ID (5Fh = 95)


//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Other Chassis Med Ramp, All Domains, Profiles 6 & 7
//*****************************************************************************
_SDR_TYPE   C0
_SDR_TAG    'OTHER_MR'
_REC_LEN    0010

   // Sensor Record Header
   6701           // Record ID
   51             // SDR Version
   C0             // Record Type
   0B             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask (All Domains)
   C0             // Fan Profile Support 
   
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   60             // Stepwise Curve ID (60h = 96)
   
//*****************************************************************************
// Main Domain Record, Other & Fast Ramp Configuration, All Domains 
//*****************************************************************************

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Other Chassis Fast Ramp, All Domains, Profiles 0 & 1 & 2 & 3
//*****************************************************************************
_SDR_TYPE   C0
_SDR_TAG    'OTHER_FR'
_REC_LEN    0010

   // Sensor Record Header
   6801           // Record ID
   51             // SDR Version
   C0             // Record Type
   0B             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask (All Domains)
   0F             // Fan Profile Support 
                     
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   61             // Stepwise Curve ID (61h = 97)
   

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Other Chassis Fast Ramp, All Domains, Profiles 4 & 5
//*****************************************************************************   
_SDR_TYPE   C0
_SDR_TAG    'OTHER_FR'
_REC_LEN    0010

   // Sensor Record Header
   6901           // Record ID
   51             // SDR Version
   C0             // Record Type
   0B             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask (All Domains)
   30             // Fan Profile Support 
   
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   62             // Stepwise Curve ID (62h = 98)
   

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Other Chassis Fast Ramp, All Domains, Profiles 6 & 7
//*****************************************************************************
_SDR_TYPE   C0
_SDR_TAG    'OTHER_FR'
_REC_LEN    0010

   // Sensor Record Header
   6A01           // Record ID
   51             // SDR Version
   C0             // Record Type
   0B             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask (All Domains)
   C0             // Fan Profile Support 
   
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   63             // Stepwise Curve ID (63h = 99)
      
// END OF OTHER RECORDS

//*****************************************************************************
// Main Domain Record, Shipping & Test Plate Configuration, Domains 0 - 5
// left Domain Configuration cause Shipping & Test Plate full run don't need other config
//*****************************************************************************

//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Shipping SDR, All Domains, All Profiles
//*****************************************************************************   
_SDR_TYPE   C0
_SDR_TAG    'SHIPPING'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    001C

   // Sensor Record Header
   6B01           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask (All Domains)
   FF             // Fan Profile Support 
   
   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   64             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (0h = No sensors to exclude)
   2E		  // Sensor Number To Exclude From Fan Boost
                  
   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   09             // Stepwise Curve ID (09h = 9)
   
   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID (08h = 8)


//*****************************************************************************
// Domain All
// FSC Record Type = 08h (Fan Sensor Domain Map Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'SHIPPING'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    0023

   // Sensor Record Header
   6C01           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask (All Domains)
   FF             // Fan Profile Support (All Profiles)

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   20             // Clamp ID
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID
   
_SDR_TYPE   C0
_SDR_TAG    'SHIPPING'
_REC_LEN    0023

   // Sensor Record Header
   6D01           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   FF             // Domain Mask (All Domains)
   FF             // Fan Profile Support (All Profiles)

   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   2A             // Clamp ID
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   2B             // Clamp ID
   // Clamp Sub-Record 14
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID
   // Clamp Sub-Record 15
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID
   // Clamp Sub-Record 16
   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID
   // Clamp Sub-Record 17
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID
   // Clamp Sub-Record 18
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID
   // Clamp Sub-Record 19
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID
   // Clamp Sub-Record 20
   03             // FSC Sub-Record Type (03h = Clamp)
   83             // Clamp ID
   // Clamp Sub-Record 21
   03             // FSC Sub-Record Type (03h = Clamp)
   84             // Clamp ID
   // Clamp Sub-Record 22
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID

// END OF SHIPPING RECORDS


//====================================================================//
// MIC records
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R2000FAMILY'
_REC_LEN    001C

   // Sensor Record Header
   6E01           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   28             // FSC Record Type ([5]=Profile Bank Select; [4]=PS Domain; [3:0]= 8h Main Domain)
   1F             // Domain Mask
   01             // Profile Mask

   // Domain Configuration
   01             // FSC Sub-record Type (Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost


   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (Stepwise)
   00             // Stepwise Header ID
   04             // Stepwise Curve ID

   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (Stepwise)
   00             // Stepwise Header ID
   13             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R2000FAMILY'
_REC_LEN    001C

   // Sensor Record Header
   6F01           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   28             // FSC Record Type ([5]=Profile Bank Select; [4]=PS Domain; [3:0]= 8h Main Domain)
   1F             // Domain Mask
   02             // Profile Mask

   // Domain Configuration
   01             // FSC Sub-record Type (Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost


   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (Stepwise)
   00             // Stepwise Header ID
   0F             // Stepwise Curve ID

   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (Stepwise)
   00             // Stepwise Header ID
   13             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R2000FAMILY'
_REC_LEN    001C

   // Sensor Record Header
   7001           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   28             // FSC Record Type ([5]=Profile Bank Select; [4]=PS Domain; [3:0]= 8h Main Domain)
   1F             // Domain Mask
   04             // Profile Mask

   // Domain Configuration
   01             // FSC Sub-record Type (Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost


   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (Stepwise)
   00             // Stepwise Header ID
   05             // Stepwise Curve ID

   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (Stepwise)
   00             // Stepwise Header ID
   13             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R2000FAMILY'
_REC_LEN    001C

   // Sensor Record Header
   7101           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   28             // FSC Record Type ([5]=Profile Bank Select; [4]=PS Domain; [3:0]= 8h Main Domain)
   1F             // Domain Mask
   08             // Profile Mask

   // Domain Configuration
   01             // FSC Sub-record Type (Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost


   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (Stepwise)
   00             // Stepwise Header ID
   10             // Stepwise Curve ID

   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (Stepwise)
   00             // Stepwise Header ID
   13             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R2000FAMILY'
_REC_LEN    001C

   // Sensor Record Header
   7201           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   28             // FSC Record Type ([5]=Profile Bank Select; [4]=PS Domain; [3:0]= 8h Main Domain)
   1F             // Domain Mask
   10             // Profile Mask

   // Domain Configuration
   01             // FSC Sub-record Type (Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost


   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (Stepwise)
   00             // Stepwise Header ID
   06             // Stepwise Curve ID

   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (Stepwise)
   00             // Stepwise Header ID
   13             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R2000FAMILY'
_REC_LEN    001C

   // Sensor Record Header
   7301           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   28             // FSC Record Type ([5]=Profile Bank Select; [4]=PS Domain; [3:0]= 8h Main Domain)
   1F             // Domain Mask
   20             // Profile Mask

   // Domain Configuration
   01             // FSC Sub-record Type (Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost


   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (Stepwise)
   00             // Stepwise Header ID
   13             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R2000FAMILY'
_REC_LEN    001C

   // Sensor Record Header
   7401           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   28             // FSC Record Type ([5]=Profile Bank Select; [4]=PS Domain; [3:0]= 8h Main Domain)
   1F             // Domain Mask
   40             // Profile Mask

   // Domain Configuration
   01             // FSC Sub-record Type (Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost


   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (Stepwise)
   00             // Stepwise Header ID
   07             // Stepwise Curve ID

   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (Stepwise)
   00             // Stepwise Header ID
   13             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R2000FAMILY'
_REC_LEN    001C

   // Sensor Record Header
   7501           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   28             // FSC Record Type ([5]=Profile Bank Select; [4]=PS Domain; [3:0]= 8h Main Domain)
   1F             // Domain Mask
   80             // Profile Mask

   // Domain Configuration
   01             // FSC Sub-record Type (Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost


   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (Stepwise)
   00             // Stepwise Header ID
   12             // Stepwise Curve ID

   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (Stepwise)
   00             // Stepwise Header ID
   13             // Stepwise Curve ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R2000FAMILY'
_REC_LEN    002B

   // Sensor Record Header
   7601           // Record ID
   51             // SDR Version
   C0             // Record Type
   26             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   28             // FSC Record Type ([5]=Profile Bank Select; [4]=PS Domain; [3:0]= 8h Main Domain)
   01             // Domain Mask
   FF             // Profile Mask


   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   74             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   B1             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   20             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   25             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   29             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   26             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   2D             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   2E             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   03             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   04             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   94             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   C4             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   C5             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   96             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   97             // Clamp ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R2000FAMILY'
_REC_LEN    0033

   // Sensor Record Header
   7701           // Record ID
   51             // SDR Version
   C0             // Record Type
   2E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   28             // FSC Record Type ([5]=Profile Bank Select; [4]=PS Domain; [3:0]= 8h Main Domain)
   02             // Domain Mask
   FF             // Profile Mask


   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   74             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   B0             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   B1             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   20             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   25             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   29             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   2A             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   22             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   26             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   2D             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   2F             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   2E             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   03             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   04             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   94             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   C4             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   C5             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   96             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   97             // Clamp ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R2000FAMILY'
_REC_LEN    002D

   // Sensor Record Header
   7801           // Record ID
   51             // SDR Version
   C0             // Record Type
   28             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   28             // FSC Record Type ([5]=Profile Bank Select; [4]=PS Domain; [3:0]= 8h Main Domain)
   04             // Domain Mask
   FF             // Profile Mask


   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   74             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   75             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   B0             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   B3             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   2A             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   22             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   2F             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   2E             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   03             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   04             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   94             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   95             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   C4             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   C5             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   96             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   97             // Clamp ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R2000FAMILY'
_REC_LEN    002F

   // Sensor Record Header
   7901           // Record ID
   51             // SDR Version
   C0             // Record Type
   2A             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   28             // FSC Record Type ([5]=Profile Bank Select; [4]=PS Domain; [3:0]= 8h Main Domain)
   08             // Domain Mask
   FF             // Profile Mask


   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   75             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   B2             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   B3             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   23             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   24             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   2A             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   2B             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   22             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   2F             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   03             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   04             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   2E             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   95             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   C4             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   C5             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   96             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   97             // Clamp ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R2000FAMILY'
_REC_LEN    0027

   // Sensor Record Header
   7A01           // Record ID
   51             // SDR Version
   C0             // Record Type
   22             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   28             // FSC Record Type ([5]=Profile Bank Select; [4]=PS Domain; [3:0]= 8h Main Domain)
   10             // Domain Mask
   FF             // Profile Mask


   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   75             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   B2             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   23             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   24             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   2B             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   03             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   04             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   2E             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   95             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   C4             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   C5             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   96             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   97             // Clamp ID

//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'R2000FAMILY'
_REC_LEN    002A

   // Sensor Record Header
   7B01           // Record ID
   51             // SDR Version
   C0             // Record Type
   25             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record)
   02             // FSC version 2
   38             // FSC Record Type ([5]=Profile Bank Select; [4]=PS Domain; [3:0]= 8h Main Domain)
   20             // Domain Mask
   FF             // Profile Mask

   // Domain Configuration
   01             // FSC Sub-record Type (Domain Configuration)
   14             // Normal Control Value
   64             // Ramp Step
   01             // Scan Rate
   64             // Fan Fault Boost Value
   64             // Temperature Threshold Boost Value
   64             // Chassis Cover Boost Value
   01             // Sensor Exclusion Count
   2E             // Sensor Number To Exclude From Fan Boost


   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (Stepwise)
   00             // Stepwise Header ID
   0A             // Stepwise Curve ID

   // Stepwise Sub-Record
   02             // FSC Sub-Record Type (Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   75             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   B2             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   B3             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   23             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   24             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   2E             // Clamp ID

   // Clamp Sub-Record
   03             // FSC Sub-Record Type (Clamp)
   95             // Clamp ID

// ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
// ||||||||||||||||||||||||||||||||
// Add new records above here only!
//
//****************************************************************
// SDR Type C0 Records For File & Package Revisions
//
// NOTE: THESE 2 RECORDS MUST BE THE LAST RECORDS IN THIS FILE!
// If you need to add more records, add them above these records!
//
//****************************************************************


_SDR_TYPE   C0
_REC_LEN    0015

   // Sensor Record Header
   7C01           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   10                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   'SDR File 1.13'    // String Bytes

_SDR_TYPE   C0
_REC_LEN    0018

   // Sensor Record Header
   7D01           // Record ID
   51                 // SDR Version
   C0                 // Record Type
   13                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   'SDR Package 1.13' // String Bytes
)
