================================================================================
Intel(R) Server Board S2600CP Family
Intel(R) Server System P4000CP Family Firmware Update Package
for Intel(R) Deployment Assistant, Intel(R) One Boot Flash Update Utility, 
The embedded EFI Shell, Windows* Preboot Execution Environment 
================================================================================
Intel(R) Server Boards and Systems
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================
DATE    :	May, 27 2014
TO      :	Intel(R) Server Board S2600CP Family
			Intel(R) Server System P4000CP Family customers
SUBJECT : 	Release Notes for System Firmware Update Package 
================================================================================
                              ABOUT THIS RELEASE
================================================================================
BIOS   : 02.03.0003
ME     : 02.01.07.328
BMC    : 1.21.r6038
FRUSDR : 1.11
================================================================================
                           Support Platforms and Dependency
================================================================================
Processors supported: 
Intel(R) Xeon processor E5-4600/2600/2400 series
Intel(R) Xeon processor E5-4600/2600/2400 v2 series

Microcode update versions:
Intel(R) Xeon processor E5-4600/2600/2400 series C0 stepping: 0x00000513 CPUID = 0x206D5
Intel(R) Xeon processor E5-4600/2600/2400 series C1 stepping: 0x00000619 CPUID = 0x206D6
Intel(R) Xeon processor E5-4600/2600/2400 series C2 stepping: 0x00000710 CPUID = 0x206D7
Intel(R) Xeon processor E5-4600/2600/2400 v2 series C0/C1 stepping: 0x00000416 CPUID = 0x306e4

Production boards:
  Product		    Fab Version	      
  S2600CP		    Fab5 or above     

The following update process must be followed to ensure a trouble free update.
1.	BMC firmware
2.	BIOS
3.	Manageability Engine (ME) firmware
4.	FRUSDR
================================================================================
                  System Firmware Update Package Usage instructions                   
================================================================================
This package can be updated using one of the following methods:
 - The embedded UEFI shell
 - Intel(R) Deployment Assistant
 - Windows* or Linux* operating system using Intel(R) One-boot Flash Update (OFU)
   V11.0 Build 15 or later)
 - Windows* Preboot Execution Environment (WinPE)

To update from the embedded EFI Shell

Update system firmware from Intel server EFI shell by the following steps:
- Download Intel server system firmware update package from http://downloadcenter.intel.com/
- Unzip package and copy all files to root folder in USB flash drive 
- Insert USB flash drive to server USB port
- Reboot server, system will start BIOS/BMC/FRUSDR update automatically

  If the unzipped package is not under the root folder of USB flash drive:
- Reboot server to EFI shell manually
- Run command "map -r" in EFI shell to find the mount point of the USB flash drive
- The USB flash drive may mount to fs0: or fs1: or other. 
- Run command "fs0:" or other to change folder to USB flash drive, 
- Change folder to the folder storing the firmware package
- Run command "startup.nsh" to start firmware update process

Please refer to "EFI_Instructions.pdf" in this firmware package for a quick guide to 
use the EFI commands

To Update from Intel(R) Deployment Assistant (IDA)

The Intel(R) Deployment Assistant software is easy to use and is present on the 
"Intel(R) Server Deployment & Management" DVD shipped with the system.
User can download the latest version IDA CD ISO image from http://downloadcenter.intel.com/
To use the IDA CD to update the system firmware:
- Boot server with IDA CD
- Select "Get System Updates" 
- Choose one of the three options 

  . From http://www.intel.com/support/
    Automatically downloads the latest Firmware Update Package from Intel 
    Requires Internet connection
    Enter your local IP address and proxy configuration
    Click "Next" to start the download and update process

  . From my network
    Download the latest Firmware Update Package from http://downloadcenter.intel.com/ and copy 
    it to a Windows* shared folder
    Enter your local IP address, the Windows* file server name, and a
    Windows user name and password
    Select the firmware package in pop-up window
    Click "Next" to start the update process

  . From USB flash drive or Hard Disk
    Download the latest Firmware Update Package from http://downloadcenter.intel.com/ and copy it 
    to a USB flash drive, then insert the USB flash drive into the server USB port
    Click "Browse"
    Select the firmware package in pop-up window
    Click "Next" to start the update process
    
  Note: The Firmware Update Package is in the ZIP file format. Do not unzip 
        before copying to a Windows* shared folder or USB flash drive.

To update from Windows* and Linux* or operating systems using the Intel(R) One Boot
Flash Update Utility (OFU)

Intel(R) One boot Flash Update utility can be downloaded from http://downloadcenter.intel.com/
and it is part of the "BIOS, Firmware Update & Configuration Utilities" for 
Windows* and Linux*. Please refer to Intel OFU user guide about the details of 
installation and usage of OFU.

Use OFU to update system firmware by the following steps:
- Install OFU on Windows* or Linux* system
- Download the latest firmware update package from http://downloadcenter.intel.com/
- Unzip package to a folder
- Run the following command in Windows* command line/Linux* terminal window:
  <OFU install folder name>:\flashupdt -u  <package folder name>\flashupdt.cfg
                       
To update from Windows* Preboot Execution Environment (WinPE)

The System Firmware Update Package can be inserted to Windows* PE customized image 
for creating a bootable Windows* PE CD. User is able to update system firmware from 
customized WinPE CD by the following steps:
- Boot server with customized WinPE CD
- Run script "WinPE21_x64_Update.bat" or "WinPE20_x86_Update.bat" 
  (name may be varied depends on your own customization)
  
Note:
1. The Intel(R) OFU utility is case sensitive. Therefore, when you transfer the 
Firmware Update Package using USB flash drive from a Microsoft Windows* system to a Linux
environment, you must first extract under the Linux* environment. Otherwise, you 
will need to mount the USB flash drive manually with 'vfat' option under Linux to avoid 
conversion from upper case to lower case and vice versa.

2. To make Intel(R) OFU utility run properly under x86 or x64 OS, you have to read
OFU release notes on known issues for OFU installation.

3. In this SFUP package, Intel only provide batch file "WinPE_x86_Update.bat"
for WinPE2.0 32 bit solution "WinPE_x64_Update.bat" for WinPE2.1/3.0 64 bit 
solution as an example. Please refer to white paper "White Paper-Intel Server 
Utilities Procedure for WinPE.pdf" for details on building your own customized 
WinPE CD.

4. Windows PE 2.0 - built from Windows Vista SP1 32bit or EM64T
5. Windows PE 2.1 - built from Windows Vista SP1 or Windows Server 2008, EM64T
6. Windows PE 3.1 - built from Windows Server 2008R2, EM64T
7. Microsoft IPMI driver is loaded by default from WinPE CD, if you want to use 
Intel IPMI driver instead of MS IPMI driver for firmware update, you can un-install
Microsoft IPMI driver by:
                Devicesetup.exe ¨Cv remove *IPI0001
                Note: IPI0001 is the device ID for Microsoft IPMI driver.
				
=================================================================================   
 				      BIOS 02.03.0003
=================================================================================
- This version enhances the protection of certain UEFI variables as described in 
	Intel Security Advisory INTEL-SA-00038
- Add "Memory Performance" option in BIOS Setup
- Fixed: IRQ of 10GigE (on board) is not described by BIOS on S4600LH
- Fixed: System does not reset when memory address parity error
- Fixed: Blank console issue fix for McAfee BIOS
- Fixed: CTLE Settings for S4600LH platforms
- Fixed: System halt after creating RAID with 9750 card
- Fixed: User selected power policy not programmed into MSR 0xB01
- Fixed: ME not reporting SmaRT/CLST events to the SEL.
- Fixed: blank lines in server management screen
- Fixed: Change SMBIOS Type 1 - "SKUNum and Family fields" default from 
   "To be filled by O.E.M" to "00"
- Fixed: Show error "BIOS handoff failed"after installLinux OS under UE
- Fixed: The SMBIOS log has wrong description about Port Type in Type8
- Fixed: Qlogic 4-Port Fiber Channel Cards Configuration does not work
- Fixed: SYSCFG "/bbo" and "/bbosys" not working as expected when "Static Boot Order" Enabled
- Fixed: After setting Admin password to enabled, no password is requested
- Fixed: BIOS needs to support more than 8 NIC boot from PXE
- Fixed: RMS25CB080 -610 board may not be detected on some platforms
- Fixed: IRQ of 10GigE (on board) is not described by BIOS on S4600LH
- Fixed:System does not reset when memory address parity error
- Fixed: CTLE Settings for S4600LH platforms

Others:
- Update processor microcode.
- Update support for additional devices on PCIe Gen 3 qualified list on the 
   Intel(R) Server Platforms for E5-4600/2600/2400 CPUs.
- Restore customized defaults when auto recovering from NVRAM corruption 
- Update reference code (V02.00.00.03)
================================================================================
                     		ME 2.01.07.328 release
================================================================================
- Fixed: Platform is not able to power on properly after being shut down by NM
         Policy
- Fixed: Global platform power consumption reported by NM Statistics in S5 is
         incorrect
- Fixed: OOB (out-of-band) stress test by issuing the wrong username may cause
         connection to be unavailable
- Fixed: Shutdown action can be interrupted by cold reset when volatile NM
         policy is in use
		 
===============================================================================
                            BMC 01.21.6038
===============================================================================
- Fixed: BMC User configuration is corrupted and users cannot be re-created.
- Fixed: The response of getting satellite fw update status is always 01
- Fixed: HSC slots status present sensor showed NA in EWS.
- Fixed: (X) Disk Drive LED - Locating drive is inconsistent in time to illuminate and stop
- Fixed: Hot Plug Fan not changing system status on Fan failure.
- Fixed: EWC Fan sensor readings disappear when filtered and there is a fan failure.
- Fixed: (X) BMC hung after network Scan.
- Fixed: Current power is incorrect on EWS while power down SUT by pressing power button.
- Fixed: Special characters '<>' of FRU info can't be shown in the EWS page.
- Fixed: Recurring temperature alarms on sensor #0x22(SSB).
- Fixed: (X) S600GL/S2600GR - Fail EMC Brownout testing.
- Fixed: DIMM Thrm Mrgn sensor shows "unknown" when just plug DIMM in Channel3 
- Fixed: [X] Updated Java signitures to support new JAVA requirements.
- Fixed: Get SOL Configuration parameters 5 & 6 should not return invalid response.
- Fixed: EWS is incorrectly decoding ME firmware update SEL events.
- Fixed: BMC channle 1 can not ping succesfully and EWS login fail while using static IPV6 address.
- Fixed: Baseboard IP address can't be assigned when IPv6 address set as auto-configuration.
- Fixed: IP address can't be assigned when IPv6 address set as dynamic.
- Fixed: BMC Hangs during first A/C power up.
- Fixed: Reading the PCI Riser temperature sensors for S2600CP was not operating correctly.
- Fixed: CFM calculation failed on PSU removal/insertion.
- Fixed: Enable FPGA logic to preserve PWM registers.
- Fixed: Check in 750AB V8 PSU image per PSU verification team's request
- Fixed: Porting FRU discovery APIs from Grantley where the Auto-Configuration feature requires the operational 
         status of the managed FRUs.
- Fixed: Add the displaying of the PS HW Revison for the PS if update is required or not.

================================================================================
                      FRUSDR Changes in release 1.11
================================================================================    
Issue Fixed:
- None.
Features added:
- Update FRUSDR utility to version 11 build 20.

=============================================================================
                            LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products. 
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation may 
have patents or pending patent applications, trademarks, copyrights, or other 
intellectual property rights that relate to the presented subject matter.  
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any 
such patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product 
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 
*Other names and brands are the property of their respective owners.
Copyright (c) 2014 Intel Corporation.

A portion of this firmware is open source code, which falls under the
GPL 2.0 license.  

[END OF RELEASE NOTES]
