================================================================================
Intel(R) Server Board S2600KP Product Family and Intel(R) Compute Module HNS2600KP Product Family Firmware Update Package for Intel(R) Deployment Assistant, Intel(R) One Boot Flash Update Utility, The embedded EFI Shell, Windows* Preboot Execution Environment 
================================================================================
Intel Enterprise Platform & Services Division - Marketing
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================
DATE    : 	September 18, 2014
TO      : 	Intel(R) Server Board S2600KP Product Family and Intel(R) Compute Module HNS2600KP 
                   Product Family customers
SUBJECT : Release Notes for System Firmware Update Package 
================================================================================
                              ABOUT THIS RELEASE
================================================================================
BIOS:     	01.01.0003
ME:        	03.00.06.274
BMC:     	01.05.6802
FRUSDR:	1.00
================================================================================
                           Support Platforms and Dependency
================================================================================
Processors supported: 
Intel(R) Xeon processor E5-2600 v3 series

Microcode update versions:
Intel(R) Xeon processor E5-2600 V3 series C1 stepping: 0x00000023 CPUID = 0x306f2

Production boards:
  Product		Fab Version	      
  S2600KP		Fab3 (PBA# -350) or above    
  S2600KP	F	Fab3 (PBA# -350) or above 

The following update process must be followed to ensure a trouble free update.
1.	BMC firmware
2.	BIOS
3.	Manageability Engine (ME) firmware
4.	FRUSDR

================================================================================
                  System Firmware Update Package Usage instructions                   
================================================================================
This package can be updated using one of the following methods:
 - The embedded UEFI shell
 - Intel(R) Deployment Assistant
 - Windows* or Linux* operating system using Intel(R) One-boot Flash Update (OFU)
   V11.0 Build 14 or later)
 - Windows* Preboot Execution Environment (WinPE)

To update from the embedded EFI Shell

Update system firmware from Intel server EFI shell by the following steps:
- Download Intel server system firmware update package from http://downloadcenter.intel.com/
- Unzip package and copy all files to root folder in USB flash drive 
- Insert USB flash drive to server USB port
- Reboot server, system will start BIOS/BMC/FRUSDR update automatically

  If the unzipped package is not under the root folder of USB flash drive:
- Reboot server to EFI shell manually
- Run command "map -r" in EFI shell to find the mount point of the USB flash drive
- The USB flash drive may mount to fs0: or fs1: or other. 
- Run command "fs0:" or other to change folder to USB flash drive, 
- Change folder to the folder storing the firmware package
- Run command "startup.nsh" to start firmware update process

Please refer to "EFI_Instructions.pdf" in this firmware package for a quick guide to 
use the EFI commands

To Update from Intel(R) Deployment Assistant (IDA)

The Intel(R) Deployment Assistant software is easy to use and is present on the 
"Intel(R) Server Deployment & Management" DVD shipped with the system.
User can download the latest version IDA CD ISO image from http://downloadcenter.intel.com/
To use the IDA CD to update the system firmware:
- Boot server with IDA CD
- Select "Get System Updates" 
- Choose one of the three options 

  . From http://www.intel.com/support/
    Automatically downloads the latest Firmware Update Package from Intel 
    Requires Internet connection
    Enter your local IP address and proxy configuration
    Click "Next" to start the download and update process

  . From my network
    Download the latest Firmware Update Package from http://downloadcenter.intel.com/ and copy 
    it to a Windows* shared folder
    Enter your local IP address, the Windows* file server name, and a
    Windows user name and password
    Select the firmware package in pop-up window
    Click "Next" to start the update process

  . From USB flash drive or Hard Disk
    Download the latest Firmware Update Package from http://downloadcenter.intel.com/ and copy it 
    to a USB flash drive, then insert the USB flash drive into the server USB port
    Click "Browse"
    Select the firmware package in pop-up window
    Click "Next" to start the update process
    
  Note: 1) The Firmware Update Package is in the ZIP file format. Do not unzip 
        before copying to a Windows* shared folder or USB flash drive.
	2) The IDA will always update backup bios with this FSUP package even if the IDA backup bios check box is not selected.

To update from Windows* and Linux* or operating systems using the Intel(R) One Boot
Flash Update Utility (OFU)

Intel(R) One boot Flash Update utility can be downloaded from http://downloadcenter.intel.com/
and it is part of the "BIOS, Firmware Update & Configuration Utilities" for 
Windows* and Linux*. Please refer to Intel OFU user guide about the details of 
installation and usage of OFU.

Use OFU to update system firmware by the following steps:
- Install OFU on Windows* or Linux* system
- Download the latest firmware update package from http://downloadcenter.intel.com/
- Unzip package to a folder
- Run the following command in Windows* command line/Linux* terminal window:
  <OFU install folder name>:\flashupdt -u  <package folder name>\flashupdt.cfg
                       
To update from Windows* Preboot Execution Environment (WinPE)

The System Firmware Update Package can be inserted to Windows* PE customized image 
for creating a bootable Windows* PE CD. User is able to update system firmware from 
customized WinPE CD by the following steps:
- Boot server with customized WinPE CD
- Run script "WinPE21_x64_Update.bat" or "WinPE20_x86_Update.bat" 
  (name may be varied depends on your own customization)
  
Note:
1. The Intel(R) OFU utility is case sensitive. Therefore, when you transfer the 
Firmware Update Package using USB flash drive from a Microsoft Windows* system to a Linux
environment, you must first extract under the Linux* environment. Otherwise, you 
will need to mount the USB flash drive manually with 'vfat' option under Linux to avoid 
conversion from upper case to lower case and vice versa.

2. To make Intel(R) OFU utility run properly under x86 or x64 OS, you have to read
OFU release notes on known issues for OFU installation.

3. In this SFUP package, Intel only provide batch file "WinPE_x86_Update.bat"
for WinPE2.0 32 bit solution "WinPE_x64_Update.bat" for WinPE2.1/3.0 64 bit 
solution as an example. Please refer to white paper "White Paper-Intel Server 
Utilities Procedure for WinPE.pdf" for details on building your own customized 
WinPE CD.

4. Windows PE 2.0 - built from Windows Vista SP1 32bit or EM64T
5. Windows PE 2.1 - built from Windows Vista SP1 or Windows Server 2008, EM64T
6. Windows PE 3.1 - built from Windows Server 2008R2, EM64T
7. Microsoft IPMI driver is loaded by default from WinPE CD, if you want to use 
Intel IPMI driver instead of MS IPMI driver for firmware update, you can un-install
Microsoft IPMI driver by:
                Devicesetup.exe ¨Cv remove *IPI0001
                Note: IPI0001 is the device ID for Microsoft IPMI driver.
8. If to update backup BIOS region or NVRAM, you need to customize the OFU update 
       scripts (eg.flashupdt.cfg) and add "UpdateBackupBios" or "UpdateNvram" parameter.
 
================================================================================
				BIOS 01.01.0001
================================================================================
EPSD100026796	Setup Server Management Page, Console Redirection item not synchronize with 
SOL change.
EPSD100243718	[SLV_CWP] Wording mistake in 'Legacy Network Device Order' interface.
EPSD100243720	Clone of: [SLV_CWP] Wording mistakes in 'USB Configuration' interface of BIOS 
Setup.
EPSD100026816	Setup menu display will be distorted after changing Console Redirection settings
EPSD100243746	[SLV_TLP] Wording mistake in 'CPU C State Control' interface of BIOS SETUP.
EPSD100243716	[SLV_TLP] Wording mistake in 'Legacy Network Device Order' interface of BIOS 
SETUP.
EPSD100243747	[SLV_TLP] Wording mistake in 'CPU C State Control-C1E Autopromote' interface of 
BIOS SETUP.
EPSD100243755	Clone of: [SLV_CWP] Wording mistake in 'CPU C State Control-C1E Autopromote' 
interface of BIOS SETUP.
EPSD100243763	Clone of: [SLV_CWP] Wording mistake in 'CPU C State Control' interface of BIOS 
SETUP.
EPSD100026816   	Setup menu display will be distorted after changing Console Redirection settings
EPSD100242907   	WCP - CATERR with PCIe SSD card in Riser 1
EPSD100243596	System CATERRs when the Intel SSD PCIe AIC card is installed

================================================================================
                            ME 03.00.06.274
================================================================================
- Fixed: Improper ME FW Health Event is sent when ME is reset to factory defaults with IPMI command 
Force ME Recovery
- Fixed: Sometimes during SMBalert assertion stress test unexpected ME FW reset may be observed.    
- Fixed: SpsFITc and ME FW do not enable configuring MGPIO number greater than 15.
- Fixed: Sometimes unexpected SmaRT&CLST event is send by ME FW during platform AC cycle.    
- Fixed: During Global Reset cycle testing ME Exception: LOADER TIMEOUT may be observed.
- Fixed: Alerts from redundant PSU are not properly masked, so system could be throttled when 	
redundant PSU asserts an error signal. Approx. one second throttling could be observed when 
redundant PSU is unplugged.

===============================================================================
                             BMC 01.05.6802
===============================================================================
-EPSD100241497: BMC cannot be contacted until AC power cycle after restoring defaults
-EPSD100243953: EWS server health page sensor reading show " Not Available" for " PS Fan Fail" sensor.

================================================================================
                             FRUSDR 1.00
================================================================================    
- EPSD100243001: Remove obsolete sensor 0x69 from SDR.
- N/A: Add LAN leash sensor in 2U4N chassis.

=============================================================================
                            LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products. 
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation may 
have patents or pending patent applications, trademarks, copyrights, or other 
intellectual property rights that relate to the presented subject matter.  
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any 
such patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product 
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 
*Other names and brands are the property of their respective owners.
Copyright (c) 2014 Intel Corporation.

A portion of this firmware is open source code, which falls under the
GPL 2.0 license.  

[END OF RELEASE NOTES]
