Intel® Server Board SE7501BR2
The products you are looking for are no longer manufactured by Intel. Additionally, Intel no longer provides interactive support for these products via telephone or e-mail, nor will Intel provide any future content updates or software updates to support new operating systems or improve compatibility with third party devices and software products. THESE PRODUCT SUPPORT DOCUMENTS ARE PROVIDED FOR HISTORICAL REFERENCE ONLY AND ARE SUBJECT TO THE TERMS SET FORTH IN THE "TERMS OF USE" INFORMATION. Information on currently available Intel products is available at www.intel.com and/or developer.intel.com

Identify your product
  Product Discontinuance Announcement

    Intel® will no longer provide interactive support for these products via telephone or e-mail.

    | Product Discontinuation Announcement (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

Software and drivers

Technical specifications
  Technical Product Specifications

    Product overview, including descriptions and diagrams of the integrated features

    | Technical Product Specification (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  Specification update

    An update to the specifications contained in the Technical Product Specification

    | Specification update (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

Installation and use
  4-3-4-4 beep code during POST
    Fully populate memory Bank 1(slots 1A and 1B) before populating other memory banks
  Adaptec* Host RAID supported RAID Levels
    The onboard Adaptec* 7901/7902 SCSI controller supports RAID 0 and RAID 1.
  Adaptec* Host RAID User's Guide

    | Adaptec* Host RAID User's Guide (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  AGP Support on Server Products
    Only the Intel® Server Boards T440BX, S845WD1-E, S875WP1-E, and SE7505VB2 have an AGP slot to allow an AGP video card to be plugged in.
  Authentication of "None" allowed by management utilities
    Download the BMC LAN Fix Utility and the CLI AutoConfig Utility 1.05.
  Clearing Memory Errors During POST
    BIOS > Advanced > Memory Settings > Memory Retest
  Clearing Processor Errors During POST
    BIOS > Main > Processor Settings > Processor Retest
  Error: "Platform IDs don't match in the Boot Block. The update cannot continue."
    Update BMC to 1.11 before updating to BMC 1.14.
  Error: CMOS Checksum Bad
    Clear the CMOS. See the TPS for instructions.
  Error: No Valid Controller Found with a Zero Channel RAID Controller
    Disable the Adaptec* Host* RAID option:
    1. During POST, while the Adaptec* Option ROM is initializing, press the [CTRL+A] key combination.
    2. From the device menu that appears, select a channel and press Enter.
    3. From the Main Options menu, select Disable HostRAID and press Enter. (If the controller has two channels, make sure that steps 1 through 3 are performed for the second channel)
    4. Save and exit.
  Fan Connector placement on the Intel® Server Chassis SC5250-E
    Connect the rear chassis fan to the "SYS FAN 2" header on the server board and the front hard drive fan to "SYS FAN 5".
  Guidelines for Using the SCSI Y-Cable with Two Backplanes Connected
    Connect the I2C cables to the correct HSBP headers on the motherboard to corerctly assign SCSI IDs. You may also need to disable termination on the SCSI controller.
  Hot Swap Backplane Driver does not Install in Microsoft Windows Server 2003*
    If a yellow '!' persists in Device Manager, use the following method to install the driver:
    1. Download the Intel® SCA Backplane HSBP driver for Microsoft Windows* Server 2000
    2. Go to Device manager and delete ESG-SHV item from “Other Devices” tree
    3. Choose Actions > Scan for hardware changes
    4. Select Options > Don’t auto detect > Select from list
    5. From the list of Devices select "System"
    6. Choose "Have Disk"
    7. Browse to extracted Windows 2000* driver, and select "Intel® SCA Backplane"
    8. Override the driver signing warnings and choose "Install anyway"
  How to set up LAN Alerts

    On the managed server:
    Boot to the System Setup Utility (SSU) from either the Service Partition or the System Resource CD > Platform Event Manager > Configure LAN > Enable LAN Alerts

    On the client side:
    Install Intel® Server Management > Start > Programs > Intel Server Management > LAN Alerts Viewer > Configure

  IBM* U320 HDDs Not Recognized by Intel® RAID Controllers SRCMRU and SRCZCR
    The hard drives require firmware S25K, available from IBM.
  Korean EMC Certification
    E-G011-02-4579(A)
  Mean Time Between Failure (MTBF) Data
    94,385 hours at a maximum operating temperature of 35 C.
  One Boot/Flash Update Utility Appears To Hang
    The utility may take up to 45 seconds updating a system with a Hot Swap Controller (HSC).
  Platform Confidence Test - Installation and operating instructions

    | Intel® Server Board Platform Confidence Test (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  Power Budget Tool
    Power Budget Tool [EXE]
  Product Guide

    | Product Guide for the Intel® Server Board SE7501BR2 (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  Quick Start Guide (PDF)

    This guide is broken down into two documents.

    Quick Start Guide - Front (PDF)

    Quick Start Guide - Back (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  Server Installation and Integration Guide (PDF)

    | Server Installation and Integration Guide (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  Setting Up a Password for Intel® Server Management
    System Setup Utility > Platform Event Manager > Configure LAN > Password
  Spares/Parts List and Configuration Guide (PDF)

    | Spares/Parts List and Configuration Guide (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  System Event Log #83
    The BMC logs one or two system boot events in the SEL when the BIOS finishes POST. These messages are normal.
  Unknown Devices in Device Manager
    Ethernet Controller unknown devices refer to the on-board Network Card PRO/100 Adapter ESG-SHV SCA HSBP M15 SCSI Processor Device refers to the Hotswap Backplane of the SC5200 chassis. The unknown PCI Device and System Interrupt Controller refers to the E7501 Chipset.
  VRM is not needed when integrating processor(s)
    The baseboard has a single, integrated VRM (Voltage Regulator Module) to support up to two processors. It is compliant with the VRM 9.1 specification and provides a maximum of 130 AMPs.
  Which PCI Slot can the Zero Channel RAID Card be installed in?
    The ZCR cards are only supported in PCI-X Slot 4.
  Windows 2000 Advanced Server* recognizes only 4 GB of memory
    The /PAE option must be enabled in the ARC path in the boot.ini file in order for Windows* 2000 to recognize memory above 4.0GB (e.g. multi(0)disk(0)rdisk(0)partition(2)\WINNT="Windows 2000 Advanced Server" /PAE /basevideo /sos).
  Yellow Exclamation Mark (!) in Device Manager under Ports (Com & LPT)
    Check that the Chassis Intrusion Switch is connected to the correct header (J1C3) and not the Emergency Management Port in use jumper (J1C2). Clear the CMOS, then remove the AC cord and the CMOS battery completely for a few seconds.

Compatibility
  Tested Chassis
    Intel SR1350-E (SR1350E)
    Intel SR1350-E (SR1350ENA)
    Intel SC5200 (KHD3BASE450)
    Intel SC5200 (KHD3HSRP650)
    Intel SC5200 (KHD3HSRP650R)
    Intel SC5200 (KHD3RP450)
    Intel SC5250-E (KPTBASE450)
    AIC* RMC1H2-6I-DK8T
    AIC* RMC1Q2
    AIC* RMC3F2
    AIC* RMC2Q2
    Aopen* H800A
    Chenbro* SR101
    Chenbro* SR102
    Chenbro* RM212
    Chenbro* SR105
    Chenbro* SR107
    CiDesign* RS1400
    CiDesign* RS2100i
    CiDesign* RS4100i
    Evercase* ECS5000LX
    Evercase* R9112B-S35
    Guangshing Industrial* GHI-104DX
    MaCase* KA-036G
    MaCase* KA-066G
    Min Maw* MRC-1C
    Yeong Yang* YY-W201
  Tested Hardware and Operating Systems

    | Tested Hardware and Operating System List (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  Tested Memory

    The board supports up to 8 GB of memory. Memory must be installed in pairs; DIMM Bank1 must be populated before DIMM Bank2; Memory within a DIMM bank must be identical.

    | Tested Memory List Report (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  Tested Processors
    Intel® Xeon® Processor 3.20 GHz, 2M Cache, 533 MHz FSB
    Intel® Xeon® Processor 3.20 GHz, 1M Cache, 533 MHz FSB
    Intel® Xeon® Processor 3.06 GHz, 512K Cache, 533 MHz FSB
    Intel® Xeon® Processor 3.06 GHz, 1M Cache, 533 MHz FSB
    Intel® Xeon® Processor 3.00 GHz, 512K Cache, 400 MHz FSB
    Intel® Xeon® Processor 3.00 GHz, 4M Cache, 400 MHz FSB
    Intel® Xeon® Processor 2.80 GHz, 512K Cache, 533 MHz FSB
    Intel® Xeon® Processor 2.80 GHz, 512K Cache, 400 MHz FSB
    Intel® Xeon® Processor 2.80 GHz, 2M Cache, 400 MHz FSB
    Intel® Xeon® Processor 2.80 GHz, 1M Cache, 533 MHz FSB
    Intel® Xeon® Processor 2.66 GHz, 512K Cache, 533 MHz FSB
    Intel® Xeon® Processor 2.60 GHz, 512K Cache, 400 MHz FSB
    Intel® Xeon® Processor 2.50 GHz, 1M Cache, 400 MHz FSB
    Intel® Xeon® Processor 2.40 GHz, 512K Cache, 533 MHz FSB
    Intel® Xeon® Processor 2.40 GHz, 512K Cache, 400 MHz FSB
    Intel® Xeon® Processor 2.40 GHz, 1M Cache, 533 MHz FSB
    Intel® Xeon® Processor LV 2.40 GHz, 512K Cache, 400 MHz FSB
    Intel® Xeon® Processor 2.20 GHz, 512K Cache, 400 MHz FSB
    Intel® Xeon® Processor 2.20 GHz, 2M Cache, 400 MHz FSB
    Intel® Xeon® Processor 2.00 GHz, 512K Cache, 533 MHz FSB
    Intel® Xeon® Processor 2.00 GHz, 512K Cache, 400 MHz FSB
    Intel® Xeon® Processor 2.00 GHz, 2M Cache, 400 MHz FSB
    Intel® Xeon® Processor 2.00 GHz, 256K Cache, 400 MHz FSB
    Intel® Xeon® Processor 1.80 GHz, 512K Cache, 400 MHz FSB

Technical advisories
  AA679: Invalid firmware setting is present after using Intel® Server Setup Utilities

    | Action Alert 679-1 (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  TA629: BIOS Flash Chip Not Fully Write Protected

    | BIOS Flash Chip Not Fully Write Protected (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  TA645: FRUSDR Version 5.5.B does not support default shipping configuration

    | FRUSDR Version 5.5.B Does Not Support Default Shipping Configuration (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  TA667: Unexpected Reset Actions from Intel® Server Management

    | Unexpected Reset Actions (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  TA693: Updates Needed After Intel® Server Management Uninstall

    | TA69301.PDF (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  TA742: System Setup Utility Does Not launch When Invoked from Resource CD

    | Technical Advisory 742-1 (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*