This release note and the software that accompanies it are copyright (c) 2014, Intel Corporation or its suppliers, and may only be installed and used in accordance with the license that accompanies the software.

This Software is furnished under license and may only be used or copied in accordance with the terms of that license. No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. The Software is subject to change without notice, and should not be construed as a commitment by Intel Corporation or its suppliers to market, license, sell or support any product or technology. Unless otherwise provided for in the license under which this Software is provided, the Software is provided AS IS, with no warranties of any kind, express or implied. Except as expressly permitted by the Software license, neither Intel Corporation nor its suppliers assumes any responsibility or liability for any errors or inaccuracies that may appear herein. Except as expressly permitted by the Software license, no part of the Software may be reproduced, stored in a retrieval system, transmitted in any form, or distributed by any means without the express written consent of Intel Corporation.


==========================
Supported RAID Controllers
==========================
This download supports the following Intel(R) RAID controllers using the SAS software stack: RS3SC008, RS3MC044, RS3DC080, RS3DC040, RS3WC080, RCS25ZB040, RCS25ZB040LX, RS25AB080, RS25SB008, RMS2PB080, RMS25PB040, RMT3PB080, RMS25CB080, RMS25CB080N,MS25PB080N, RMS25CB040, RMT3CB080, RS25NB008, RS25DB080, RS2VB080, RS2VB040, RT3WB080, RS2WC040, RS2WC080, RS2SG240, RS2WG160, RMS2MH080, RMS2AF080, RMS2AF040, RS2MB044, RS2BL080, RS2BL080DE, RS2BL040, RS2PI008DE, RS2PI008.  Please verify that this utility has been tested with the RAID card you have chosen to use by checking the web page for your controller at http://support.intel.com.


===================
Package Information
===================
Version = 1.07.07
OS supported = EFI, FreeBSD, Linux, Solaris x86, Ubuntu, VMware, VMware MN, Windows


==================
Known Restrictions
==================
STORCLI PHASE 2.0 Specific Limitations:
1.	User can use both 'raid0' and 'r0' for mentioning the raid level. And user can find both the forms in the help command.
2.	When passing parameter,'set' for CC mode is mandatory. 
3.	The use of comma in between array no and row parameter in the syntax for making ‘pdreplacemissing’ should not be used.
4.	User would not be able to specify ROWs while creating ‘Dedicated Hot Spare’. Instead user needs to use ‘Drive Group ID’ as dgs=N
5.	In ‘Foreign Configuration show’, utility will display VD as ‘Foreign’ instead of showing the VD state.
6.	The success code and description is printed only after complete processing of the command. Success will not be printed unless the entire log is displayed to the output. Hence the success code and description is printed at the end of the log for this particular command.
7.	Any command syntax is still valid, if user uses “-” instead of “/”  for e.g. storcli.exe /c0-vall show.
8.	Show ‘Bus and PCI Slot type’ are not shown as part of the controller information.
9.	While creating a VD using non-Enc-ID Devices, user needs to provide inputs in the format ‘D:SlotID’ as syntax (for eg: Drives=D:1,2,3 where 1,2,3 are the slot ids of the non encID devices)
10.	Tape Drives will be listed only with /c0/sall show all command, /c0/sall show doesn’t list Tape drive but only display the direct attached drives if present or a blank table if none are connected.
11.	Importing Foreign Configuration while Rebuild is in progress then query for Show fall the output would display multiple R60 VDs.
12.	Date and Time of controller is not displayed in proper format in EFI Environment 
13.	JSON is not required in EFI
14.	The sector size of the drives are displayed in “KB” instead of bytes under the PD List table. This is just display error in tabular format but it is displayed correctly in drive details.
15.	The “Eid:slot” column while importing a foreign config is not populated. StorCLI: The VD name cannot contain spaces as allowed in MSM.
16.	Consistency Check cannot be scheduled beyond year-2037AD.
17.	Flashing 9260CV low-level controller firmware is supported only through DOS version of CLI (MegaCLI) and not through EFI version of StorCLI.  Flashing MegaRAID firmware does not have this issue.

Known Behavior:
1.	‘All VD initialization’ command when run through StorCLI utility, shows the error message as failed for cachecaded VD. This is a generic limitation.
2.	While reconstruction is in progress, start of CC/Init/BGI operations on same VD throws an inappropriate error message. This is a generic limitation.
3.	In controller show cc the field CC current state will change only when it meets the schedule CC parameters.
4.	All the unsupported commands for SWR controller if tried to execute may result in unknown behavior for example – system hang-up. For the list of unsupported commands refer to user guide Appendix C: Unsupported Commands in Embedded RAID.
5.	Output for controller information contains junk characters in VMware ESXi 4.1 update2.  
6.	FDE drives are displayed as secured drives on SWR- SCU controller.
7.	There is no check to see whether user has entered different properties or the same property multiple times in StorCLI command. Hence StorCLI  does not throw syntax error for the command “/c0/dall show all all all”. This issue is because of the implementation of accepting multiple properties in a single command line in some cases.


=======================
Contents on the package
=======================
The following files are included in this zip:

Name						Description
ir3_StorCli_v 1.09.08_rel-notes.txt		This file
License_v2.pdf					License Agreement
EFI\StorCli.efi					EFI Utility
FreeBSD\StorCli					FreeBSD 32bit Utility
FreeBSD\StorCli64 				FreeBSD 64bit Utility
Linux\storcli-1.09.08-1.noarch.rpm		Linux Installation package
Linux-ppc\StorCli64.tar 			Linux-ppc Utility
Solaris\StoCli.pkg				Solaris Installation package
Sparc\StoCli.pkg				Sparc Installation package
Ubuntu\storcli_1.09.08_all.deb			Ubuntu Installation package
VMware\StorCli					VMware Utility
VMware-MN\vmware-esx-storcli-1.09.08.vib 	VMware-MN utility
Windows\StorCli.exe				Windows 32bit utility
windows\StorCli64.exe				Windows 64bit utility


==========================
Installation instructions:
==========================

EFI
==========
This utility is an EFI Based command line utility that can be used to query the controller and attached devices for status, Update Firmware, and create/manage logical drive configuration.
Extract DOS folder contents to a user specified location such as = FS0:


FreeBSD
==========
This utility is a FreeBSD Based command line utility that can be used to query the controller and attached devices for status, Update Firmware, and create/manage logical drive configuration.
Extract the FreeBSD folder contents to a user specified location.
In FreeBSD OS, StorCli or StorCli64 application will not function if the user is trying to run it in CSH, the default shell in FreeBSD.
Please ensure that the user has entered the bash shell by executing the command "bash".


Linux
==========
This utility is a Linux Based command line utility that can be used to query the controller and attached devices for status, Update Firmware, and create/manage logical drive configuration.

To install StorCLI, perform the following steps:
1. Unzip the StorCLI package.
2. To install the StorCLI RPM, run the rpm -ivh <StorCLI-x.xx-x.noarch.rpm> command.
3. To upgrade the StorCLI RPM, run the rpm -Uvh <StorCLI-x.xx-x.noarch.rpm> command.


Solaris
==========
This utility is a Solaris Based command line utility that can be used to query the controller and attached devices for status, Update Firmware, and create/manage logical drive configuration.
Extract Solaris folder contents to a user specified location and install the utility pkg.

Requirement for Storcli Execution 

1) Download "libgcc-3.4.6-....-local.gz" from http://www.sunfreeware.com

2) Copy it to the setup and Extract.

3) Install the Package using bellow command.

	pkgadd -d libgcc-3.4.6-....-local.pkg

4) Prior to executing standalone Storcli binary, check the permissions of Storcli binary. 

	"ls -l storcli"

5) If executable permissions are not given, run the below command to change the permissions.

	"chmod +x storcli"

Ubuntu
==========
1. Copy the Package.sh and the Linux Binaries to the ubnutnu server.

2. Run the Package.sh with the version as argument as below. Version should not start with the alphabet.
	./Package.sh x.xx.xx

2. Installing debian Package
	sudo dpkg -i storcli_x.xx.xx_all.deb

3. verifying , if the package is installed successfully or not.
   dpkg -l | grep -i storcli

4. Run the commands    with super user as below.
	sudo /opt/MegaRAID/storcli/storcli adpcount


VMware & Vmware-MN
==========
This utility is a VMWare Based command line utility that can be used to query the controller and attached devices for status, Update Firmware, and create/manage logical drive configuration.
Extract Windows folder contents to a user specified location 



1. The installed VIB Package can be list using command 
	"esxcli software vib list "
 
2. The VIB Package can be installed using the command
	"esxcli software vib install -v=vmware-esx-storcli.vib"

3.The VIB Package can be removed using the command
	"esxcli software vib remove -n=vmware-esx-storcli.vib"


Windows
==========
This utility is a Windows Based command line utility that can be used to query the controller and attached devices for status, Update Firmware, and create/manage logical drive configuration.
Extract Windows folder contents to a user specified location.  The command prompt used to run storcli needs to have administrative privileges.


Supported commands and options
=============================
     Storage Command Line Tool  Ver 1.03.11 Jan 30, 2013

     (c)Copyright 2012, LSI Corporation, All Rights Reserved.


help - lists all the commands with their usage. E.g. storcli help
<command> help - gives details about a particular command. E.g. storcli add help

List of commands:

Commands   Description
-------------------------------------------------------------------
add        Adds/creates a new element to controller like VD,Spare..etc
delete     Deletes an element like VD,Spare
show       Displays information about an element
set        Set a particular value to a property 
start      Start background operation
stop       Stop background operation
pause      Pause background operation
resume     Resume background operation
download   Downloads file to given device
expand     expands size of given drive
insert     inserts new drive for missing
transform  downgrades the controller
/cx        Controller specific commands
/ex        Enclosure specific commands
/sx        Slot/PD specific commands
/vx        Virtual drive specific commands
/dx        Disk group specific commands
/fx        Foreign configuration specific commands
/px        Phy specific commands
/bbu       Battery Backup Unit related commands

Other aliases : cachecade, freespace, sysinfo

Use a combination of commands to filter the output of help further.
E.g. 'storcli cx show help' displays all the show operations on cx.
Use verbose for detailed description E.g. 'storcli add  verbose help'
Use 'page=[x]' as the last option in all the commands to set the page break.
X=lines per page. E.g. 'storcli help page=10'


Command options must be entered in the same order as displayed in the help of the respective commands.
     (c)Copyright 2012, LSI Corporation, All Rights Reserved.


storcli -v 
storcli -h| -help| ? 
storcli -h| -help| ? legacy
storcli show 
storcli show all
storcli show ctrlcount
storcli /cx add vd type=raid[0|1|5|6|00|10|50|60]
 [Size=<VD1_Sz>,<VD2_Sz>,..|all] [name=<VDNAME1>,..] 
 drives=e:s|e:s-x|e:s-x,y,e:s-x,y,z [PDperArray=x][SED]
 [pdcache=on|off|default][pi][DimmerSwitch(ds)=default|automatic(auto)|
 none|maximum(max)|MaximumWithoutCaching(maxnocache)][wt|wb][nora|ra]
 [direct|cached] [CachedBadBBU|NoCachedBadBBU] [cachevd]
 [Strip=<8|16|32|64|128|256|512|1024>] [AfterVd=X] 
 [Spares = [e:]s|[e:]s-x|[e:]s-x,y] [force]
storcli /cx add vd each type=raid0 [name=<VDNAME1>,..] [drives=e:s|e:s-x|e:s-x,y]
 [SED] [pdcache=on|off|default][pi] [DimmerSwitch(ds)=default|automatic(auto)|
 none|maximum(max)|MaximumWithoutCaching(maxnocache)] [wt|wb] [nora|ra]
 [direct|cached] [CachedBadBBU|NoCachedBadBBU]
 [Strip=<8|16|32|64|128|256|512|1024>] 
storcli /cx add vd cachecade Type = raid[0,1,10] drives = [e:]s|[e:]s-x|
 [e:]s-x,y [WT| WB] [assignvds = 0,1,2]
storcli /cx/ex show all 
storcli /cx/ex show status 
storcli /cx/vx del cachecade
storcli /cx delete events
storcli /cx show events [[type= <sincereboot| sinceshutdown| includedeleted|
latest=x| ccincon vd=<0,1,...>] filter=<info|warning|critical|fatal>]
file=<filepath>
storcli /cx show eventloginfo
storcli /cx delete securitykey
storcli /cx set securitykey=xxxxxxxx {passphrase=xxxx} {keyid=xxx}
storcli /cx set securitykey keyid=xxx
storcli /cx compare securitykey=xxxxxxxxxx
storcli /cx set termlog[=on|off|offthisboot]
storcli /cx show termlog [type=config|contents]
storcli /cx delete termlog
storcli /cx set securitykey=xxxxxxxx oldsecuritykey=xxxxxxxx
 {passphrase=xxxx} {keyid=xxx}
storcli /cx/dx show 
storcli /cx/dx show cachecade 
storcli /cx/dx show all 
storcli /cx show freespace
storcli /cx/fx show [all] [securityKey = xxx]
storcli /cx/fx del|delete [securityKey = xxx]
storcli /cx/fx import [preview] [securityKey = xxx]
storcli /cx/vx set ssdcaching=on|off
storcli /cx/vx set security=on
storcli /cx/vx show expansion
storcli /cx/vx expand Size=<xx> [expandarray]
storcli /cx[/ex]/sx show 
storcli /cx[/ex]/sx show all
storcli /cx[/ex]/sx start rebuild 
storcli /cx[/ex]/sx stop rebuild 
storcli /cx[/ex]/sx pause rebuild 
storcli /cx[/ex]/sx resume rebuild 
storcli /cx[/ex]/sx show rebuild 
storcli /cx[/ex]/sx start copyback target=eID:sID 
storcli /cx[/ex]/sx stop copyback 
storcli /cx[/ex]/sx pause copyback 
storcli /cx[/ex]/sx resume copyback 
storcli /cx[/ex]/sx show copyback 
storcli /cx[/ex]/sx start initialization  
storcli /cx[/ex]/sx stop initialization  
storcli /cx[/ex]/sx show initialization  
storcli /cx[/ex]/sx start locate  
storcli /cx[/ex]/sx stop locate  
storcli /cx[/ex]/sx show securitykey keyid 
storcli /cx[/ex]/sx add hotsparedrive [DGs=<N|0,1,2...>] [enclaffinity] [nonrevertible]
storcli /cx[/ex]/sx delete hotsparedrive
storcli /cx[/ex]/sx spinup
storcli /cx[/ex]/sx spindown
storcli /cx[/ex]/sx set online 
storcli /cx[/ex]/sx set offline 
storcli /cx[/ex]/sx set missing 
storcli /cx[/ex]/sx set jbod 
storcli /cx[/ex]/sx set good [force]  
storcli /cx[/ex]/sx insert dg=A array=B row=C 
storcli /cx/vx set emulationType=0|1
storcli /cx/vx set wrcache=WT|WB|AWB
storcli /cx/vx set rdcache=RA|NoRA
storcli /cx/vx set iopolicy=Cached|Direct
storcli /cx/vx set accesspolicy=RW|RO|Blocked|RmvBlkd
storcli /cx/vx set pdcache=On|Off|Default
storcli /cx/vx set name=<NameString>
storcli /cx/vx set ds=Default|Auto|None|Max|MaxNoCache
storcli /cx/vx set autobgi=On|Off
storcli /cx/vx set pi=Off
storcli /cx/vx show
storcli /cx/vx show all
storcli /cx/vx show init
storcli /cx/vx show cc
storcli /cx/vx show erase
storcli /cx/vx show migrate
storcli /cx/vx show bgi
storcli /cx/vx show autobgi
storcli /cx set consistencycheck|cc=[off|seq|conc] [delay=value]
 starttime=yyyy/mm/dd hh] [excludevd=x-y,z]
storcli /cx show cc|consistencycheck
storcli /cx show ocr 
storcli /cx set ocr=<on|off>
storcli /cx/vx start init[Full][Force]
storcli /cx/vx start erase [simple|normal|thorough][erasepatternA=<val>]
[erasepatternB=<val>]
storcli /cx/vx start cc[Force]
storcli /cx/vx start migrate type=raidx [option=add|remove drives=[e:]s|[e:]s-x|[e:]s-x,y] [Force]
storcli /cx/vx stop init
storcli /cx/vx stop erase
storcli /cx/vx stop cc
storcli /cx/vx stop bgi
storcli /cx/vx pause cc
storcli /cx/vx pause bgi
storcli /cx/vx resume cc
storcli /cx/vx resume bgi
storcli /cx show 
storcli /cx show all 
storcli /cx show preservedcache 
storcli /cx/vx delete preservedcache[force] 
storcli /cx[/ex]/sx download src=<filepath> [satabridge] 
storcli /cx/ex download src=<filepath> [forceActivate] 
storcli /cx[/ex]/sx secureerase [force]  
storcli /cx[/ex]/sx start erase [simple| normal| thorough][erasepatternA=<val>]
 [erasepatternB=<val>]
storcli /cx[/ex]/sx stop erase 
storcli /cx[/ex]/sx show erase 
storcli /cx[/ex]/sx set bootdrive=<on|off> 
storcli /cx/vx set bootdrive=<on|off>
storcli /cx show bootdrive
storcli /cx show bootwithpinnedcache
storcli /cx set bootwithpinnedcache=<on|off>
storcli /cx show activityforlocate
storcli /cx set activityforlocate=<on|off>
storcli /cx show exposeencldevice
storcli /cx set exposeencldevice=<on|off> 
storcli g/cx show copyback
storcli /cx set copyback=<on|off> type=smartssd|smarthdd|all 
storcli /cx show jbod
storcli /cx set jbod=<on|off> 
storcli /cx set autorebuild=<on|off> 
storcli /cx show autorebuild
storcli /cx show cachebypass
storcli /cx set cachebypass=<on|off> 
storcli /cx show usefdeonlyencrypt
storcli /cx set usefdeonlyencrypt=<on|off>
storcli /cx show prcorrectunconfiguredareas
storcli /cx set prcorrectunconfiguredareas=<on|off> 
storcli /cx show batterywarning
storcli /cx set batterywarning=<on|off> 
storcli /cx show abortcconerror
storcli /cx set abortcconerror=<on|off> 
storcli /cx show ncq
storcli /cx set ncq=<on|off> 
storcli /cx show maintainpdfailhistory
storcli /cx set maintainpdfailhistory=<on|off> 
storcli /cx show restorehotspare
storcli /cx set restorehotspare=<on|off> 
storcli /cx show bios
storcli /cx set bios=<on|off> 
storcli /cx set BIOSMode=<SOE|BE|HCOE|HSM> 
storcli /cx show alarm
storcli /cx set alarm=<on|off|silence> 
storcli /cx show foreignautoimport
storcli /cx set foreignautoimport=<on|off> 
storcli /cx show directpdmapping
storcli /cx set directpdmapping=<on|off> 
storcli /cx show rebuildrate
storcli /cx set rebuildrate=<value> 
storcli /cx show loadbalancemode
storcli /cx set loadbalancemode=<on|off> 
storcli /cx show enableesmarter
storcli /cx set enableesmarter=<on|off> 
storcli /cx show enableeghsp
storcli /cx set enableeghsp=<on|off> 
storcli /cx show enableeug
storcli /cx set enableeug=<on|off> 
storcli /cx show cacheflushint
storcli /cx set cacheflushint=<value> 
storcli /cx show prrate
storcli /cx set prrate=<value> 
storcli /cx show ccrate
storcli /cx set ccrate=<value> 
storcli /cx show bgirate
storcli /cx set bgirate=<value> 
storcli /cx show migraterate
storcli /cx set migraterate=<value> 
storcli /cx show spinupdrivecount
storcli /cx set spinupdrivecount=<value> 
storcli /cx show spinupdelay
storcli /cx set spinupdelay=<value> 
storcli /cx show coercion
storcli /cx set coercion=<value> 
storcli /cx show clusterenable
storcli /cx set clusterenable=<value> 
storcli /cx show smartpollinterval
storcli /cx set smartpollinterval=<value> 
storcli /cx show eccbucketsize
storcli /cx set eccbucketsize=<value> 
storcli /cx show eccbucketleakrate
storcli /cx set eccbucketleakrate=<value> 
storcli /cx show backplane
storcli /cx set backplane=<value> 
storcli /cx show perfmode
storcli /cx set perfmode=<value> 
storcli /cx set perfmode=<value> maxflushlines=<value> numiostoorder=<value>
storcli /cx show perfmodevalues
storcli /cx show pi
storcli /cx set pi=<on|off> 
storcli /cx show preventpiimport
storcli /cx set preventpiimport=<on|off> 
storcli /cx show time
storcli /cx set time=<yyyymmdd hh:mm:ss | systemtime> 
storcli /cx show ds
storcli /cx set ds=OFF type=1|2|3|4
storcli /cx set ds=ON type=1|2 [properties]
storcli /cx set ds=ON type=3|4 DefaultLdType=<val> [properties]
storcli /cx set ds [properties] 
storcli /cx show safeid
storcli /cx show rehostinfo
storcli /cx show ASO
storcli /cx set aso key=<key value> preview
storcli /cx set aso key=<key value>
storcli /cx set aso transfertovault
storcli /cx set aso rehostcomplete
storcli /cx set aso deactivatetrialkey
storcli /cx download file=<filepath> [fwtype=<val>] [ResetNow] [nosigchk] [noverchk]
storcli /cx flush|flushcache
storcli /cx/px show 
storcli /cx/px show all
storcli /cx/px set linkspeed=0|1.5|3|6|12 
storcli /cx/bbu show 
storcli /cx/bbu show all 
storcli /cx/bbu show status 
storcli /cx/bbu show properties 
storcli /cx/bbu show modes 
storcli /cx/bbu set [ learnDelayInterval=<val> | bbuMode=<val>  
 | autolearnmode=<val> | powermode=sleep | writeaccess=sealed ]
storcli /cx/bbu start learn 
storcli /cx show securitykey keyid 
storcli /cx start patrolread
storcli /cx stop patrolread
storcli /cx pause patrolread
storcli /cx resume patrolread
storcli /cx show patrolRead
storcli /cx set patrolread = {{on mode=<auto|manual> }|{off}}
storcli /cx set patrolread [starttime=< yyyy/mm/dd hh>]
 [maxconcurrentpd =<value>][includessds=<on|onlymixed|off>][uncfgareas=on|off]
storcli /cx set patrolread delay = <value>
storcli /cx set memscrubpattern = <value> [force]
storcli /cx show memscrubpatterns
storcli /cx show badblocks
storcli /cx flasherase 
storcli /cx transform iMR 

Legacy CMDTool2 commands are supported in this release of StorCLI.  The command is the same except that the name of the utility has changed.  To invoke the command, replace the tool name CMDTool2 with storcli.

StorCLI -v 
StorCLI -help|-h|-?
StorCLI -adpCount 
StorCLI -AdpSetProp {CacheFlushInterval -val}|{ RebuildRate -val} 
    |{PatrolReadRate -val}|{BgiRate -val}|{CCRate -val} 
    |{ReconRate -val}|{SpinupDriveCount -val}|{SpinupDelay -val} 
    |{CoercionMode -val}|{ClusterEnable -val}|{PredFailPollInterval -val} 
    |{BatWarnDsbl -val} |{EccBucketSize -val} | {EccBucketLeakRate -val} 
    |{AbortCCOnError -val} | AlarmEnbl | AlarmDsbl | AlarmSilence 
    |{SMARTCpyBkEnbl -val} | NCQEnbl | NCQDsbl -aN|-a0,1,2|-aALL 
    |{SSDSMARTCpyBkEnbl -val} -aN|-a0,1,2|-aALL 
    |{MaintainPdFailHistoryEnbl -val} -aN|-a0,1,2|-aALL 
    |{EnblSpinDownUnConfigDrvs -val} -aN|-a0,1,2|-aALL 
    |{EnblSSDPatrolRead -val} -aN|-a0,1,2|-aALL 
    | AutoEnhancedImportEnbl | AutoEnhancedImportDsbl -aN|-a0,1,2|-aALL 
StorCLI -AdpSetProp -AutoDetectBackPlaneDsbl -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Auto Detect of SGPIO and i2c SEP. 
             1=Disable Auto Detect of SGPIO. 
             2=Disable Auto Detect of i2c SEP. 
             3=Disable Auto Detect of SGPIO and i2c SEP. 
StorCLI -AdpSetProp -CopyBackDsbl -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Copyback. 
             1=Disable Copyback. 
StorCLI -AdpSetProp -LoadBalanceMode -val -aN|-a0,1,2|-aALL 
       val - 0=Auto Load balance mode. 
             1=Disable Load balance mode. 
StorCLI -AdpSetProp -UseFDEOnlyEncrypt -val -aN|-a0,1,2|-aALL 
       val - 0=FDE and controller encryption (if HW supports) is allowed. 
             1=Only support FDE encryption, disallow controller encryption. 
StorCLI -AdpSetProp -PrCorrectUncfgdAreas -val -aN|-a0,1,2|-aALL 
       val - 0= Correcting Media error during PR is disabled. 
             1=Correcting Media error during PR is allowed. 
StorCLI -AdpGetProp CacheFlushInterval | RebuildRate | PatrolReadRate | BgiRate 
    | CCRate | ReconRate | SpinupDriveCount | SpinupDelay | CoercionMode
    | PredFailPollInterval | EccBucketSize | EccBucketLeakRate | EccBucketCount
    | ClusterEnable | BatWarnDsbl | AbortCCOnError | AlarmDsply 
    | AutoDetectBackPlaneDsbl| CopyBackDsbl | LoadBalanceMode | SMARTCpyBkEnbl | SSDSMARTCpyBkEnbl | MaintainPdFailHistoryEnbl | EnblSpinDownUnConfigDrvs 
    | EnblSSDPatrolRead 
    | NCQDsply -aN|-a0,1,2|-aALL 
    | UseFDEOnlyEncrypt | WBSupport  -aN|-a0,1,2|-aALL 
    | AutoEnhancedImportDsply -aN|-a0,1,2|-aALL 
    | PrCorrectUncfgdAreas -aN|-a0,1,2|-aALL 
StorCLI -AdpAllInfo -aN|-a0,1,2|-aALL  
StorCLI -AdpGetTime -aN|-a0,1,2|-aALL  
StorCLI -AdpSetTime yyyymmdd hh:mm:ss -aN   
StorCLI -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
StorCLI -AdpBIOS -Enbl |-Dsbl | -SOE | -BE | -Dsply -aN|-a0,1,2|-aALL 
StorCLI -AdpBootDrive {-Set {-Lx | -physdrv[E0:S0]}}|-Get -aN|-a0,1,2|-aALL 
StorCLI -AdpAutoRbld -Enbl|-Dsbl|-Dsply -aN|-a0,1,2|-aALL
StorCLI -AdpCacheFlush -aN|-a0,1,2|-aALL
StorCLI -AdpPR -Dsbl|EnblAuto|EnblMan|Start|Stop|Info| SSDPatrolReadEnbl | SSDPatrolReadDsbl
         |{SetDelay Val}|{-SetStartTime yyyymmdd hh}|{maxConcurrentPD Val} -aN|-a0,1,2|-aALL
StorCLI -AdpCcSched -Dsbl|-Info|{-ModeConc | -ModeSeq [-ExcludeLD -LN|-L0,1,2]
   [-SetStartTime yyyymmdd hh ] [-SetDelay val ] } -aN|-a0,1,2|-aALL
StorCLI -AdpCcSched -SetStartTime yyyymmdd hh -aN|-a0,1,2|-aALL
StorCLI -AdpCcSched -SetDelay val  -aN|-a0,1,2|-aALL
StorCLI -FwTermLog -BBUoff|BBUoffTemp|BBUon|BBUGet|Dsply|Clear -aN|-a0,1,2|-aALL
StorCLI -AdpAlILog -aN|-a0,1,2|-aALL 
StorCLI -AdpDiag [val] -aN|-a0,1,2|-aALL
          val - Time in second.
StorCLI -AdpShutDown -aN|-a0,1,2|-aALL
StorCLI -PDList -aN|-a0,1,2|-aALL 
StorCLI -PDGetNum -aN|-a0,1,2|-aALL 
StorCLI -pdInfo -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
StorCLI -PDOnline  -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
StorCLI -PDOffline -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
StorCLI -PDMakeGood -PhysDrv[E0:S0,E1:S1,...] | [-Force] -aN|-a0,1,2|-aALL 
StorCLI -PDMakeSystem -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
StorCLI -PDHSP {-Set [-Dedicated [-ArrayN|-Array0,1,2...]] [-EnclAffinity] [-nonRevertible]} 
     |-Rmv -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
StorCLI -PDRbld -Start|-Stop|-ShowProg |-ProgDsply 
        -PhysDrv [E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
StorCLI -PDClear -Start|-Stop|-ShowProg |-ProgDsply 
        -PhysDrv [E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
StorCLI -PdLocate {[-start] | -stop} -physdrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
StorCLI -PdMarkMissing -physdrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
StorCLI -PdGetMissing -aN|-a0,1,2|-aALL 
StorCLI -PdReplaceMissing -physdrv[E0:S0] -arrayA, -rowB -aN 
StorCLI -PdPrpRmv [-UnDo] -physdrv[E0:S0] -aN|-a0,1,2|-aALL  
StorCLI -EncInfo -aN|-a0,1,2|-aALL 
StorCLI -PhyInfo -phyM -aN|-a0,1,2|-aALL  
StorCLI -PdFwDownload [-SataBridge] -PhysDrv[0:1,1:2,..]-f <filename> -aN|-a0,1,2|-aALL  
StorCLI -LDInfo -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
StorCLI -LDSetProp  {-Name LdNamestring} | -RW|RO|Blocked | WT|WB [-Immediate] |RA|NORA|ADRA 
        | Cached|Direct | -EnDskCache|DisDskCache | CachedBadBBU|NoCachedBadBBU
        -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
StorCLI -LDGetProp  -Cache | -Access | -Name | -DskCache -Lx|-L0,1,2|-LALL  
        -aN|-a0,1,2|-aALL 
StorCLI -LDInit {-Start [-full]}|-Abort|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL 
StorCLI -LDCC {-Start [-force]}|-Abort|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL 
StorCLI -LDBI -Enbl|-Dsbl|-getSetting|-Abort|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL  
StorCLI -LDRecon {-Start -rX [{-Add | -Rmv} -Physdrv[E0:S0,...]]}|-ShowProg|-ProgDsply 
        -Lx -aN 
StorCLI -LdPdInfo -aN|-a0,1,2|-aALL 
StorCLI -LDGetNum -aN|-a0,1,2|-aALL 
StorCLI -LDBBMClr -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
StorCLI -CfgLdAdd -rX[E0:S0,E1:S1,...] [WT|WB] [NORA|RA|ADRA] [Direct|Cached]
        [CachedBadBBU | NoCachedBadBBU][-szXXX [-szYYY ...]]
        [-strpszM] [-Hsp[E0:S0,...]] [-AfterLdX] [-Force]|[FDE|CtrlBased] -aN 
StorCLI -CfgEachDskRaid0 [WT|WB] [NORA|RA|ADRA] [Direct|Cached] 
        [CachedBadBBU|NoCachedBadBBU] [-strpszM]|[FDE|CtrlBased] -aN|-a0,1,2|-aALL
StorCLI -CfgClr -aN|-a0,1,2|-aALL 
StorCLI -CfgDsply -aN|-a0,1,2|-aALL 
StorCLI -CfgLdDel -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
StorCLI -CfgFreeSpaceinfo -aN|-a0,1,2|-aALL 
StorCLI -CfgSpanAdd -r10 -Array0[E0:S0,E1:S1] -Array1[E0:S0,E1:S1] [-ArrayX[E0:S0,E1:S1] ...] 
        [WT|WB] [NORA|RA|ADRA] [Direct|Cached] [CachedBadBBU|NoCachedBadBBU]
        [-szXXX[-szYYY ...]][-strpszM][-AfterLdX]|[FDE|CtrlBased] -aN
StorCLI -CfgSpanAdd -r50 -Array0[E0:S0,E1:S1,E2:S2,...] -Array1[E0:S0,E1:S1,E2:S2,...] 
        [-ArrayX[E0:S0,E1:S1,E2:S2,...] ...] [WT|WB] [NORA|RA|ADRA] [Direct|Cached] 
        [CachedBadBBU|NoCachedBadBBU][-szXXX[-szYYY ...]][-strpszM][-AfterLdX] | 
        [FDE|CtrlBased] -aN
StorCLI -CfgAllFreeDrv -rX [-SATAOnly] [-SpanCount XXX] [WT|WB] [NORA|RA|ADRA] 
        [Direct|Cached] [CachedBadBBU|NoCachedBadBBU] [-strpszM]
        [-HspCount XX [-HspType -Dedicated|-EnclAffinity|-nonRevertible]] 
        [FDE|CtrlBased] -aN 
StorCLI -CfgSave -f filename -aN   
StorCLI -CfgRestore -f filename -aN   
StorCLI -CfgForeign -Scan | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
StorCLI -CfgForeign -Dsply [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
StorCLI -CfgForeign -Preview [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
StorCLI -CfgForeign -Import [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
StorCLI -CfgForeign -Clear [x]|[-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
        x - index of foreign configurations. Optional. All by default. 
StorCLI -AdpEventLog -GetEventLogInfo -aN|-a0,1,2|-aALL 
StorCLI -AdpEventLog -GetEvents {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
StorCLI -AdpEventLog -GetSinceShutdown {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
StorCLI -AdpEventLog -GetSinceReboot {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
StorCLI -AdpEventLog -IncludeDeleted {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
StorCLI -AdpEventLog -GetLatest n {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
StorCLI -AdpEventLog -GetCCIncon -f <fileName> -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
StorCLI -AdpEventLog -Clear -aN|-a0,1,2|-aALL 
StorCLI -AdpBbuCmd -aN|-a0,1,2|-aALL  
StorCLI -AdpBbuCmd -GetBbuStatus -aN|-a0,1,2|-aALL  
StorCLI -AdpBbuCmd -GetBbuCapacityInfo -aN|-a0,1,2|-aALL  
StorCLI -AdpBbuCmd -GetBbuDesignInfo -aN|-a0,1,2|-aALL  
StorCLI -AdpBbuCmd -GetBbuProperties -aN|-a0,1,2|-aALL  
StorCLI -AdpBbuCmd -BbuLearn -aN|-a0,1,2|-aALL  
StorCLI -AdpBbuCmd -BbuMfgSleep -aN|-a0,1,2|-aALL  
StorCLI -AdpBbuCmd -BbuMfgSeal -aN|-a0,1,2|-aALL  
StorCLI -AdpBbuCmd -SetBbuProperties -f <fileName> -aN|-a0,1,2|-aALL 
StorCLI -AdpFacDefSet -aN 
StorCLI -AdpFwFlash -f filename [-NoSigChk] [-NoVerChk] -aN|-a0,1,2|-aALL  
StorCLI -AdpGetConnectorMode -ConnectorN|-Connector0,1|-ConnectorAll -aN|-a0,1,2|-aALL  
StorCLI -AdpSetConnectorMode -Internal|-External|-Auto -ConnectorN|-Connector0,1|-ConnectorAll -aN|-a0,1,2|-aALL  
StorCLI -PhyErrorCounters -aN|-a0,1,2|-aALL  
StorCLI -DirectPdMapping -Enbl|-Dsbl|-Dsply -aN|-a0,1,2|-aALL  
StorCLI -PDCpyBk -Start -PhysDrv[E0:S0,E1:S1] -aN|-a0,1,2|-aALL 
StorCLI -PDCpyBk -Stop|-ShowProg|-ProgDsply -PhysDrv[E0:S0] -aN|-a0,1,2|-aALL 
StorCLI -PDInstantSecureErase -PhysDrv[E0:S0,E1:S1,...] | [-Force] -aN|-a0,1,2|-aALL 
StorCLI -LDMakeSecure -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
StorCLI -DestroySecurityKey | [-Force] -aN 
StorCLI -CreateSecurityKey -SecurityKey sssssssssss | [-Passphrase sssssssssss] |[-KeyID kkkkkkkkkkk] -aN 
StorCLI -ChangeSecurityKey -OldSecurityKey sssssssssss | -SecurityKey sssssssssss| 
          [-Passphrase sssssssssss] | [-KeyID kkkkkkkkkkk] -aN
StorCLI -GetKeyID [-PhysDrv[E0:S0]] -aN 
StorCLI -SetKeyID -KeyID kkkkkkkkkkk -aN 
StorCLI -VerifySecurityKey -SecurityKey sssssssssss -aN 
StorCLI -GetPreservedCacheList -aN|-a0,1,2|-aALL 
StorCLI -DiscardPreservedCache -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 

       sssssssssss  - It must be between eight and thirty-two 
                      characters and contain at least one number, 
                      one lowercase letter, one uppercase 
                      letter and one non-alphanumeric character.
       kkkkkkkkkkk -  Must be less than 256 characters. 

    Note: The directly connected drives can be specified as [:S] 

    Wildcard '?' can be used to specify the enclosure ID for the drive in the 
      only enclosure without direct connected device or the direct connected 
      drives with no enclosure in the system.

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 


=============
Fixes/Updates
=============
v1.09.08
SCGCQ00567786 - not able get enclosure status
SCGCQ00571823 - Added a condition to check for no VDs in StrtDrCp
SCGCQ00573703 - Storcli shows wrong VD size for 4K VDs during foreign config import
SCGCQ00574165 - compare factorysettings is a factory command but works in storcli
SCGCQ00579423 - storcli - issung "storcli /c0/v256" command generating coredump segmentation fault
SCGCQ00600059 - Storcli creates configuration not using the OEM default value for Disk Cache Policy
SCGCQ00471826 - StorCli mbox value needs to be changed for the command "storcli /c0/bbu show gasgauge offset=1 numbytes=1"
SCGCQ00571832 - Added a condition to check for no VDs
SCGCQ00574325 - Storcli 'show ds' command fails with message "LD Power saving is unsupported"
SCGCQ00598687 - for bbu command In properties schedule time is showing twice
SCGCQ00599761 - storcli /c0/e1,2,3 show is showing enclouser properties multiple times.
SCGCQ00622402 - Changing the MR_MFC_DEFAULTS->biosContinueOnError behavior for StorCLI as per PDMs
SCGCQ00484361 - Removed the option all from tokenizer as it is not supported for enclosure firmware download.
SCGCQ00563031 - Even though there are no drive groups, the command storcli /c0/dxxx set security=on is getting success
SCGCQ00565409 - while Rebuild was going on Storcli was allows to create a partial VD on the same drive group
SCGCQ00576233 -  ./storcli64 /c0/bbu set learnstarttime command is failing with segmentation fault
SCGCQ00595061 - Storcli shows wrong estimated time for a rebuilding drive.
SCGCQ00602401 - ./storcli64 /c0/e252 show status displays success message
SCGCQ00581367 - MOn issuing command Adpalilog -a0 the Storcli throws an error 0x0c on PPC server
SCGCQ00601834 - The SCAPVPD commands are described as BBU instead of CV.
SCGCQ00559492 - Storcli displays the cc estimated time left out for the vd's where the operation is not in progress
SCGCQ00573720 - Need to display skipped images by storcil package flashing
SCGCQ00574205 - ./storcli64 /c252 show is displaying controller information of 1st controller
SCGCQ00601212 - Detailed help for storcli /c0/v0 set hostaccess is not showing
SCGCQ00581982 - Difference in behaviour across windows and linux platform after flashing FW from storclif
SCGCQ00598488 - storcli /c256 show is showing O/P as wrong synatx.
SCGCQ00600176 - command "/c0/p8 show" causing cli crash in windows OS
SCGCQ00602926 - when we query help for set perfmode the range is not mentioned for maxflush lines & numiostoorder.
SCGCQ00606117 - storlib library depended Make file flags check in
SCGCQ00577682 - MR Liberator :: ./storcli64 /c0 show dequeuelog file command failing with segmentation fault
SCGCQ00588916 - ./storcli64 /c0/sall show rebuild command shows success status
SCGCQ00598788 - "show termlog" command description is coming after displaying the logs.
SCGCQ00627716 - unable to create VD using Storcli
SCGCQ00553006 - Updated Help syntax for add vd w.r.t AWB
SCGCQ00572149 - Added the help changes for break and join mirror.
SCGCQ00601568 - nolog option is not working in MegaCLI
SCGCQ00526855 - Link libstdc++ statically to Linux versiosn of Strcli, storclio and storclif
SCGCQ00602432 - Linux-ppc 32-bit minimum driver version supported by storcli 06.603.04.00.
SCGCQ00554055 - Big endian architecture support for MR Linux driver and StorCli
SCGCQ00555468 - Added OEM based help and displaying it.
SCGCQ00568855 - Added new commands for join mirror
SCGCQ00550374 - Added new commands for break mirror
SCGCQ00569363 - Implemented the below CS syncro commands
SCGCQ00564470 - Request RAID CLI to display the Patrol Read Start Time
SCGCQ00523846 - Storcli to flash 16 and 32 MB images
SCGCQ00593583 - In Storcli, appropriate error description to be logged when FW flash is failed
SCGCQ00601765 - Storcli shows wrong estimated time for a rebuilding drive.
SCGCQ00576453 - Found storli will show incorrect Next starttime after changing CC from Automatic to OFF.
SCGCQ00592293 - Unable to replace failed drive
SCGCQ00598800 - StorCLI adpalilog command crashes in Windows 2012 R2 Build 9600 - version 1.06.03 and version 1.03.46
SCGCQ00558870 - Implemented the deviceExposure as a BIOS option to set /c0 set BIOS deviceExposure=n
SCGCQ00564130 - Added a condition to check for number of drives.
SCGCQ00604174 - BiosContinueOnError IssueWebBIOS for SAS9265-8i controller incorrectly reports "Pause on errors" instead of "Bypass Error"
SCGCQ00593384 - SCSI bus reset while collecting TFF smart logs
SCGCQ00593417 - 1.05.56 rpm installation failed saying "scriptlet failed, exit status 1"
SCGCQ00593572 - TFF firmware upgrade succeeded with mode 7 on Eagle board
SCGCQ00567735 - not showing DS3 enable properties.
SCGCQ00578982 - and storclif mention "nytrocache" in help message not an OEM feature
SCGCQ00593226 - When attempting to update DFF firmware, update fails with error "Failure 1001 failed to get ssd Controller type.
SCGCQ00593386 - 'start format' command form stocli on unconfigured drive deletes all the vds configured
SCGCQ00598815 - StorCLI adpalilog command crashes in Windows 2012 R2 Build 9600 - version 1.06.03 and version 1.03.46
SCGCQ00563046 - storcli64.exe /c0/cv start learn option is not present
SCGCQ00575400 - Getting segmentation fault when executed the command /c0 compare factorysettings file= file name
SCGCQ00555931 - storclif 1.07.06 does not have memory scrub test available
SCGCQ00567476 - getting segmentation fault when executed the command /c0 set factory file=filename
SCGCQ00578979 - space present in command compare factorysettings between words factorysettings
SCGCQ00593402 - Successful command execution depicted as a "failure" for the command: "add each vd type=r0"
SCGCQ00593571 - Storcli doesn't provide "Description" in output when extract paniclog is issued on all the TFFs.
SCGCQ00593568 - Storcli doesnot prompt the user to reboot the host after changing the link speed of a TFF.

v1.07.07
SCGCQ00493418 - FW breaks to MegaMon on executing "Cli /eall/sall show all" command.
SCGCQ00501866 - Time Left is not show correctly by sparc storcli
SCGCQ00521869 - /call/eall show not providing details of enclosure connected to the second controller
SCGCQ00526799 - Not able to flash PD firmware of 4TB Drive using storcli
SCGCQ00485777 - FW breaks to Megamon, after creating 16 R0 VD's and on executing command "cli /vall show all" from PCLI.
SCGCQ00501376 - "/c0 show dequeuelog file=_____" command is not working in OS OEL_5.9
SCGCQ00503993 - Command "./storcli /call/eall/sall show" fails for second controller with description drive not found.
SCGCQ00505348 - The help file for "/c0 start Diag duration=___" is missing
SCGCQ00503359 - Wrong PCLI version with junk charcters are displayed under GetControllerInfo.
SCGCQ00498965 - "/c0/bbu start learn" command starts battery learn cycle on supercap battery.
SCGCQ00518133 - LSI_MR Controllers fails to set "FACTORY SETTINGS"
SCGCQ00526503 - Flashing of FW in UEFI mode using storcli.efi is issuing File read error.
SCGCQ00501383 - "/c0 show dequeuelog file=_____" command is missing in main help file
SCGCQ00501414 - Online firmware update is not triggered on flashing FW
SCGCQ00524047 - Segmentation fault occures while converting binary to text file of DQlogs
SCGCQ00526385 - Unable to create cachecade VD with WT property .
SCGCQ00522666 - Command "cli /sall show all" 
SCGCQ00524755 - Storcli- Gives incomplete message while clearing config when CC VD is present on the controller
SCGCQ00493544 - "Error! App exec failed in FW PCLIError! Internal" is displayed on executing "Cli /eall/sall spindown" command with 25 drives.
SCGCQ00501437 - StorCLI - MR 6.2 StorCLI help syntax is wrong
SCGCQ00518372 - Displaying the Adapter health status in storcli show.
SCGCQ00501561 - Implemented the diag results to print on console
SCGCQ00484168 - Implemented the AWB for VD creations
SCGCQ00526393 - Implementation of "MegaCli adpbbucmd schedulelearn [options.....] an" equivalent command in storcli
SCGCQ00304999 - SWR- Retrieval of controller information fails .
SCGCQ00305001 - storcli command- show DS displays wrong information for type4 and DS off
SCGCQ00307493 - (RW LSIP200233165) Storcli: Reocurance should be spelled as reoccurrence in controller show all properties for PR and CC
SCGCQ00307495 - Displaying the correct operating system for Windows 2012 Server
SCGCQ00308671 - StorCLI is not showing correct driver version in Solaris 11
SCGCQ00309347 - StorCli-SATA Drives "PRODUCT ID" its not showing properly.
SCGCQ00312089 - Storcli- Not able to perform erase operation on a PD on VMWare 4.1 update 2
SCGCQ00312319 - Storcli- Status of /pall set linkspeed is showing success eventhough the operation is failure on ESX 4.1 update 2
SCGCQ00314106 - Remove all negative error codes
SCGCQ00314585 - StorCli - Cache cade VD information page doesn't have any details for associated VDs.
SCGCQ00322316 - Defect: Storcli-Controller show/set help page in that last line execute with Storcli Directory.
SCGCQ00328184 - StorCLI2.0: "endCtlrPropUpdate failed 4" when changing the properties of patrolread
SCGCQ00335239 - Virtual Drive properties(stripe size and size) got changed when VD is degraded
SCGCQ00338301 - StorCLI : Not able to set BBU modes using legacy syntax in EFI Environment
SCGCQ00341488 - stocli_EFI- In paged view the next line after "press enter to continue " should be displayed in next line
SCGCQ00342056 - StorCLI - in command "./storcli show " 2 fields are not getting displayed ( 1. Host Name , 2. Operating System )
SCGCQ00342074 - storcli should not depend on MFC_FEATURES instead check the other bits which indicates whether a particular feature is supported
SCGCQ00342549 - spelling mistake of initialization in (background initialization)
SCGCQ00343721 - (Cloned_EnhReq) - Drive /c0/ex/sx Hot Spare Information, displays array info under Dedicated Drive Group(s) = 0, 1
SCGCQ00343907 - StorCLI_EFI: System halts while performing import preview with securitykey in EFI Environment
SCGCQ00345525 - On performing an "add vd" with size provided in TB a decimal value is truncated to whole number as input.
SCGCQ00349419 - storcli /c0 show all -----> driver version and driver name field is missing
SCGCQ00350744 - ./storcli /c0/dall show -----> In the drive group info the alignment for global hot spare drive is improper.
SCGCQ00352569 - Buffer overflow
SCGCQ00360745 - StorCLI does not provide command to set HSM or HCOE SCGCQ00358662
SCGCQ00362717 - storcli /c0/d0 show " in that legend missing for "Dgrd/pdgd/Onln/ofLn/Rbld"
SCGCQ00363522 - storcli query for displaying controller properties is showing status , as failure.
SCGCQ00364248 - StorCLI failed to delete a VD that is just created under Windows 2008
SCGCQ00364622 - Reports wrong diskgroup size while querying controller level properties
SCGCQ00381100 - MR: not able to create PRL11 using 96 drives.
SCGCQ00462959 - Slow to create VD in HA Linux
SCGCQ00464708 - Storcli display total number of VDs in a individual drive group properties.
SCGCQ00466519 - StorCLI_6.1:The help file for "/c0 compare securitykey h" is missing
SCGCQ00467119 - SWR_SLES_11_SP3_GM Release validation : In storCli " serial number and FW package Build " fields are showing blank
SCGCQ00481532 - Msg comes for all /c0 show commands.
SCGCQ00305002 - Storcli:Unable to update PD Firmware using Storcli in Vmware 5.0
SCGCQ00310308 - Storcli -Format for Date/Time varies in show|show all controller properties .
SCGCQ00313759 - Storcli:Unable to create Cachecade VD in Windows 8
SCGCQ00314602 - StorCli - Cachecade VD information page should not display stripe size.
SCGCQ00316677 - Logical and Physical sector size must be hidden when 512E feature is not supported
SCGCQ00322262 - iMR_Inv:37 drives shown as unconfigured good in MegaCLI when "enable JBOD=0" in Ubuntu 12.04 32 bit OS
SCGCQ00324797 - Serial Number of controller is not displayed for some controllers.
SCGCQ00332212 - libsysfs custom implementation issue.
SCGCQ00341418 - In the command O/P of <./storcli /c0 show all>"Driver Name" and "Driver Version"are NOT matching with actual name and version
SCGCQ00342723 - It is displaying the driver version as driver name
SCGCQ00344992 - In the command O/P of <./storcli /c0 show all>, ErrMsg 255 Failed to get Bus Info is displayed
SCGCQ00348911 - Adapter 0: Failed to start SecureErase on Virtual Drive 0 in VMware_ESXi_5.1
SCGCQ00353679 - StorCli-"/c0/eall/sall show"in that need to be describe the GHS/Onln/Offln/F
SCGCQ00355536 - MegaCli and StorCli can not manage both Liberator (and prior) and TB controllers in the same system under FreeBSD with the mfi adn mrsas driver.
SCGCQ00357653 - Removing static memory allocation and allocating memory dynamically in function stricmp in file Cutils.cpp
SCGCQ00357913 - Update VD emulation feature in StorCLI Libmods module to sync with latest APIs.
SCGCQ00359998 - Code clean up in libmods and sysefi files are added
SCGCQ00360814 - StorCLI: Not able to set pr property includessds as onlymixed on Liberator cacheoffload controller
SCGCQ00362421 - StorCLI: Not able to detect Liberator Controller on FreeBSD 9.0(64-bit)
SCGCQ00364097 - iMR_Inv_6.1:StoreCLI- StoreCLI reports wrong Emulation type for VDs
SCGCQ00366000 - Storcli displays incomplete serial number for some SSDs
SCGCQ00374979 - Storcli ld info command displays R10 vd Span Depth to 1.
SCGCQ00469162 - In virtual drives information the Cac filed values are incorrect with regular VD's
SCGCQ00476030 - while running I/O ,It's taking time to load the controller information.
SCGCQ00312928 - Storcli- Abbreviation of UID should be mentioned in the output for /cx/fall show all
SCGCQ00314122 - Missing characters in PD model display
SCGCQ00317649 - Defect: StorCli-VD state "Dgrd'' is changed in the description-''dgrd''
SCGCQ00326862 - FreeBSD support for MegaWare Cli
SCGCQ00338688 - Storcli spelling mistakes and typos
SCGCQ00343593 - Description for different Drive "State" like DHS, Ugood, Online need to be provided under Show Drive Information
SCGCQ00363455 - The legend for the PD List table exceeds 80 char limit.
SCGCQ00364735 - UEFI, the O/P of <storcli /c0 show all>"Current Controller Date/Time" & "Current System Date/time" are not in proper format
SCGCQ00371445 - Vmware CLI fails to set the phy linkspeed
SCGCQ00377364 - StorCli shows Power Saving Option as enabled, despite controller having power saving option completely disabled.
SCGCQ00383043 - StorCLI-Invader : The "coercion" mode is not in sync with the legacy values.
SCGCQ00394883 - StorCli_MR: While Creating RAID1 with four drives command facing the "C0:BAIL_OUT at line 1354"
SCGCQ00396303 - Cfgclr command fails without force option in Sparc OS
SCGCQ00460861 - MR_Inv_6.1:StorCLI- Gives wrong message after battery retention test command is issued for Supercap FBU03
SCGCQ00462885 - Need to remove storcli /cx show clusterenable and storcli /cx set clusterenable=<value> since FW did not support this in HA
SCGCQ00466038 - MR_Inv_6.1:StoreCLI- StorCLI reports retention time as 0 for supercap FBU02 and FBU03
SCGCQ00466251 - HA : StorCLI crash when update drive firmware
SCGCQ00471042 - PCLI:Cant able to set securitykey for Controller and also VD name for VD(Takes as uppercharacter even if name given in lower)
SCGCQ00485270 - StorCLI- unsupported CV operations for SuperCap 'set' needs to be removed
SCGCQ00311990 - Removed unsupported property "Ra=Read Ahead Adaptive" from VD information.
SCGCQ00314114 - sector size of PDs are shown as 512 KB which is wrong.
SCGCQ00314128 - Add abbreviation description to all the PD states
SCGCQ00318435 - (Cloned_EnhReq) - Porting of 1.0 PRs to storcli phase 2.5 (Libmods)
SCGCQ00345372 - Storcli command "/cx show all" must display ROC temperature.
SCGCQ00359629 - In paged view the text " Press Enter to continue" should be changed to " Press any key to Continue"
SCGCQ00365950 - StorCLI cannot displays information for controller in Safe mode
SCGCQ00442610 - Onfi_patch_6.0:Firmware crashed @Line 244 in ../../raid/1078int.c for entering into CTRL-R with Pinned cache in R60 and R6.
SCGCQ00469179 - Aligning with FW for strip calculation for 4K drives
SCGCQ00337962 - StorCLI: not able to save events in txt file in EFI environment
SCGCQ00362216 - iMr_Fury_StorCli:4K Drive size shown wrong in Esxi4.1U3
SCGCQ00365632 - PCI Info for FreeBSD needs to be indicated as "N/A"
SCGCQ00379104 - Not able to get paged view of StorCLI output on VM-Ware Platform
SCGCQ00438350 - Megacli crashes after invoking any command in SGI system with one 9280-8e and 2 quad port qlogic FC cards.
SCGCQ00485561 - storclio set and get vpd gives a wrong output in failure case.
SCGCQ00493690 - /var/tmp//installobaWVe/checkinstallrbaWVe: line 11: syntax error at line 22
SCGCQ00481039 - option -v doesn't work with preboot storcli
SCGCQ00311436 - Storcli-SWR- Controller serial number display is different in show/showall controller properties .
SCGCQ00360040 - Storcli is returning error with show
SCGCQ00408070 - StorCLI does not show both "Current Write Policy" and "Default Write Policy" for VD
SCGCQ00423832 - EFI_ Storcli: Cannot set vpd file on controller, EFI hangs and cannot proceed for further operations until reboot
SCGCQ00470976 - Storcli shows irrelevant information about Nytro cache VD when user types "CfgCacheCadeDsply"
SCGCQ00484372 - Storcli:Help file modification required for command ''/cx set eghs''
SCGCQ00357263 - MegaCLI adpgetpciinfo returns a static Bus Number value "17d0"
SCGCQ00362070 - iMr_Fury_StorCLi:SectorSize show as "512KB" for 512Bytes drives
SCGCQ00396665 - StorcLi_5.7: Remove the description for "Ra=Read Ahead Adaptive" in VD show info.
SCGCQ00397663 - StorCli_MR: While creating VD using default values FW allows read policy as"Ra=Read Ahead Adaptive" as against PR-317400
SCGCQ00424978 - Is VD Emulated=Yes when emulationType=1
SCGCQ00436107 - The bootwithpinnedcache logic is backwards, both storcli and the FW are affected
SCGCQ00448094 - core dump while issuing storcli command ./storcli /c0/fall show all.
SCGCQ00454971 - storcli /c0 show is not listinf SWR controller
SCGCQ00471978 - Storcli does not show firmware version using Megacli syntax
SCGCQ00472000 - Storcli:"storcli /c0/v0 del help" does not show information on normal vd delete
SCGCQ00314119 - "Drive NCQ setting" field Removed
SCGCQ00357948 - StorCLI does not display drive information behind the Blackjack (Alta) interposer correctly
SCGCQ00384644 - iMR_Inv_6.1:StorCLI- StorCLI does not show 'Unsupported/Blocked' state for 4K drives even though FW is not supporting 4K
SCGCQ00413789 - storcli crashes on having a non PI drive and trying to create pi vd on all the drive
SCGCQ00442652 - SWR_1.34 - Serial number field is blank in controller information and the same could be updated with N/A in StorCli
SCGCQ00484230 - "Cli /ex/sx set offline" fails with errcd -1 and message enclosure ID not found.
SCGCQ00495121 - Unable to set pnpid using the ini file with captal letters mixed in the string
SCGCQ00330250 - StorCLI compliance with OSSRB recommendation
SCGCQ00342399 - CSET: (Tbolt PR 211180) Punctured Block Logging Improvements
SCGCQ00329470 - Implemented the StorCLI commands to erase contents from NVCache
SCGCQ00488282 - Add ability to change/program PCIDATA in StorClio (CLI for OEMs)
SCGCQ00501189 - MWCLI. Add command /cX/vX locate
SCGCQ00323426 - Porting of Vogel 1.0 PRs to storcli phase 2.5 [Libmods]
SCGCQ00349599 - Refer attached design doc
SCGCQ00352120 - MWCLI. Add HA support into storcli
SCGCQ00329469 - Implemented the StorCLI commands to scrub memory on controllers
SCGCQ00332606 - Display Drive Model number, Serial Number and Firmware Revision as in MSM
SCGCQ00349548 - Uneven span support is added in StorCLI.
SCGCQ00351234 - Provide a way to enable or disable 512E using Applications
SCGCQ00479543 - MWCLI: Need MegaOEM for Solaris x86 and Solaris SPARC
SCGCQ00333213 - Implemented 128 drive support by using the new ENCL_INFO structures
SCGCQ00322837 - Printing multiple json objects from different controllers as a single Array
SCGCQ00332600 - StorCLI compliance with OSSRB recommendation
SCGCQ00350668 - Create Spanned R0 array (00) in StorCLI
SCGCQ00381311 - dcmd path chagnes for supporting the new cachevault api
SCGCQ00369742 - MWCLI. R10, R50, R60, R00 VD creation
SCGCQ00381093 - PR SCGCQ00319011: Rebuild time reset
SCGCQ00433703 - Megacli/storcli support for lmrc driver
SCGCQ00413856 - remove the "Drive write cache" policy from Pd information.
SCGCQ00469192 - Aligning with FW for strip calculation for 4K drives
SCGCQ00471590 - Need to remove storcli /cx show clusterenable and storcli /cx set clusterenable=<value> since FW did not support this in HA
SCGCQ00504584 - Command "./storcli /call/eall/sall show" fails for second controller with description drive not found.
SCGCQ00413017 - Storcli reports "segmentation fault" when running command to downgrade controller to iMR
SCGCQ00376240 - System halts on issuing storcli commands in EFI Environment.
SCGCQ00437065 - Driver Version is not shown
SCGCQ00473065 - StorCli_6.1: The SATA drive is dropped while creating a R1 vd using mix of SAS and SATA drives
SCGCQ00478786 - (v 1.04.11) get a good return code (0) even when it failed
SCGCQ00471582 - Storclio:Spelling mistake during execution of command 'compare factorysettings'
SCGCQ00475598 - Storcli:4K -Wrong size updated after performing OCE on 4K Drives .
SCGCQ00475601 - storcli crash while using the command /cx/vx expand size=xx expandarray
SCGCQ00414383 - When a command fails, subsequent commands/actions are aborted in storcli (MegaCli)
SCGCQ00481849 - StorCLI- StorCLI reports wrong capacitance value for supercap FBU03
SCGCQ00412593 - Resolving compiler errors for Ctrl-R
SCGCQ00471048 - HA : StorCLI crash when update drive firmware
SCGCQ00469390 - MR_Inv_6.1:StoreCLI- StorCLI reports retention time as 0 for supercap FBU02 and FBU03

v1.05.07
SCGCQ00009501 - MPI2_FW_IMAGE_HEADER is 16 bits too long
SCGCQ00183867 - MPI2: IO Unit Page 10 structure incorrect
SCGCQ00364332 - iMR_Inv_6.1:StoreCLI-StoreCLI does not give proper message while trying to create 33rd VD on iMR FURY controller
SCGCQ00374336 - System halts on issuing storcli commands in EFI Environment.
SCGCQ00374732 - StorCLI cannot set "bypasserror" or "be"
SCGCQ00374733 - Storcli does not show 512 strip size in the online help
SCGCQ00378124 - Porting of AdpRestart Command
SCGCQ00379046 - MegaCLI help shows Storcli in generic help command
SCGCQ00379112 - storcli-legacy: The helpfile for "adpfwflash" needs to be updated for "NoVerChk"
SCGCQ00381383 - Storcli_Invader: "/c0 pause pr" Description message should be sync with command
SCGCQ00394588 - storcli only displays 1 vd when 7 present on DG view
SCGCQ00397280 - StorCli_MR:Need to modify the "DIMMER SWITCH" Help Description
SCGCQ00397877 - SWR: EFI:"Press any key to continue" displays twice.
SCGCQ00397893 - SWR: EFI: Operating system details shows nothing.
SCGCQ00399897 - BBU GasGauge Status information should not get printed for TMMC
SCGCQ00400429 - Storcli help lists unsupported /Fx option for foreign commands
SCGCQ00406358 - CLI does not provide appropriate error message and error code when secure erase is not supported
SCGCQ00414300 - StorCli_6.0-The help file for "storcli /cx/fx " is missing.
SCGCQ00415814 - storcli only associates 38 out of 48 VDs
SCGCQ00418295 - size=0 VD is getting created with remaining free space, when a VD is present in Drive Group.
SCGCQ00421114 - Storcli/Storclif/storclio:Help file for Legacy commands displays mrcli instead storcli.
SCGCQ00421282 - StorCLIO : not able to get or set hwdevice information with storCLIO
SCGCQ00423757 - EFI: Storcli : Not able to get and set vpd information on TMM module or Supercap
SCGCQ00435852 - misspelled word in storcli.efi message
SCGCQ00437754 - Help syntax is not aligned with 80 char per line limits.
SCGCQ00449926 - Power Shell support for megacli syntax for windows _ Porting
SCGCQ00450496 - StorcliF : output for the command /c0 compare factorysettings is not in sync with the legacy output.
SCGCQ00456135 - Unable to create Cachecade VD by referring the syntax in Help file for ''add vd'' .
SCGCQ00462959 - Slow to create VD in HA Linux
SCGCQ00466519 - StorCLI_6.1:The help file for "/c0 compare securitykey h" is missing
SCGCQ00372155 - Certain controller features displayed under "show all" exceeds 80-char limit.
SCGCQ00374118 - StorCli-"/c0/dall show all "in FreeSpaceDetails legend missing for "ID/VD/AfterVD"
SCGCQ00374979 - Storcli ld info command displays R10 vd Span Depth to 1.
SCGCQ00376643 - Fail to set/disable the Disk Cache Policy along with the vd creation.
SCGCQ00378135 - portings of AdpRestart command
SCGCQ00378828 - StorCLI-Legacy:'adpbootdrive get' fails to get bootdrive information.
SCGCQ00385101 - StorCli implementation of AdpRestart Command
SCGCQ00386429 - StorCLI help file shows /cx/dx show cachecade instead of /cx/dall show cachecade
SCGCQ00391731 - storcli displays message as firmware flash successfully completed even the flashing is failed.
SCGCQ00397014 - With one VD as foreign, StorCLI shows all VDs as foreign.
SCGCQ00397269 - StorCli_5.7: On SuperCap battery ''strat learn" operation is not allowed
SCGCQ00399002 - handleTokens(tokenListPtr);
SCGCQ00399387 - Not able to find range for Perf Mode value
SCGCQ00401663 - help text not working for the command set securitykey
SCGCQ00412827 - CV (CacheVault) does not support changing bbu mode but StorCLI show option to change bbu mode
SCGCQ00417435 - StorCLIF : the command /cx get hwdevice fails to get VPD information.
SCGCQ00417973 - Storclio/Storclif-Detailed help for the command start diag required .
SCGCQ00423781 - StorCLIF : getting wrong values for get gas gauge information.
SCGCQ00441696 - StoreCLI- Inconsistent behavior across different application when creating cachecade VD
SCGCQ00466251 - HA : StorCLI crash when update drive firmware
SCGCQ00467119 - SWR_SLES_11_SP3_GM Release validation : In storCli " serial number and FW package Build " fields are showing blank
SCGCQ00469179 - Aligning with FW for strip calculation for 4K drives
SCGCQ00372264 - StorCLI: The legend for "phy Error Counters" exceeds the 80-char limit.
SCGCQ00374377 - GetGGEEPData equivalent syntax is not present in storcli
SCGCQ00374418 - Storcli : controller information query is displaying the status as failure.
SCGCQ00375757 - "StorCLI /cx/bbu show modes" show the bbu modes description without the actual bbu mode number
SCGCQ00377364 - StorCli shows Power Saving Option as enabled, despite controller having power saving option completely disabled.
SCGCQ00380889 - Not able to set securitykey on controller
SCGCQ00381100 - MR: not able to create PRL11 using 96 drives.
SCGCQ00383043 - StorCLI-Invader : The "coercion" mode is not in sync with the legacy values.
SCGCQ00384644 - iMR_Inv_6.1:StorCLI- StorCLI does not show 'Unsupported/Blocked' state for 4K drives even though FW is not supporting 4K
SCGCQ00386586 - include support for SWR controllers in non LSI verison of storcli.
SCGCQ00394127 - Added the command to DOS SCU
SCGCQ00394883 - StorCli_MR: While Creating RAID1 with four drives command facing the "C0:BAIL_OUT at line 1354"
SCGCQ00396303 - Cfgclr command fails without force option in Sparc OS
SCGCQ00400019 - "storcli /c0/dall show" command not working
SCGCQ00411501 - StorCli_MR: Cache vault Strart learn command displaying twice in the hep file "/c0/cv h"
SCGCQ00414328 - Perf mode value not getting set when executed along with the other parameters
SCGCQ00414731 - Checking in StorcliF & storcli0 changes
SCGCQ00415454 - StorCLI help file does not display "add vd spanned array"
SCGCQ00420040 - StorCLIF : Not able to read or write factory settings with adpsettings command (legacy command )
SCGCQ00436928 - Illusive/Bad Data Extracted
SCGCQ00437762 - Exit code coming as 1 for adpbios (Megacli Syntax)
SCGCQ00443072 - SWR: In Store Cli if we start any background operation Estimated time left field showing Blank
SCGCQ00447686 - Storecli does not display complete information for the command ./storecli /c0/p0-x show.
SCGCQ00456501 - StorcliF: StorcliF and StorcliO crashes when given invalid file for the command /c0 set factorysettings file=filename
SCGCQ00460861 - MR_Inv_6.1:StorCLI- Gives wrong message after battery retention test command is issued for Supercap FBU03
SCGCQ00466038 - MR_Inv_6.1:StoreCLI- StorCLI reports retention time as 0 for supercap FBU02 and FBU03
SCGCQ00469162 - In virtual drives information the Cac filed values are incorrect with regular VD's
SCGCQ00379157 - StorCLI: the help file for "storcli /cx transform iMR" is missing
SCGCQ00380143 - The set phy linkspeed operation needs to have the unit(GB/s) mentioned and the Description" column is blank for set and Show.
SCGCQ00394952 - Segmentation fault hitting while executing the command "/c0 set bgi h "
SCGCQ00398246 - VD create syntax display improper output.
SCGCQ00398992 - Command displayed in the same line after "Press any key to continue".
SCGCQ00402499 - Storecli /c0 show eventloginfo 
SCGCQ00403335 - Mismatch of "Start Copyback " command in global help file and particular help file of copyback .
SCGCQ00436538 - pd version is not listing all if PDs are missing
SCGCQ00442610 - Onfi_patch_6.0:Firmware crashed @Line 244 in ../../raid/1078int.c for entering into CTRL-R with Pinned cache in R60 and R6.
SCGCQ00447972 - Storcli : adpgetprop command for enableeug/enableeghsp showing success and not getting reflected when we give wrong flag
SCGCQ00451393 - Megascu adpm0flash command hangs for Dell controllers.
SCGCQ00462885 - Need to remove storcli /cx show clusterenable and storcli /cx set clusterenable=<value> since FW did not support this in HA
SCGCQ00364097 - iMR_Inv_6.1:StoreCLI- StoreCLI reports wrong Emulation type for VDs
SCGCQ00375625 - StorCLI : Displaying failure in the output for querying Dimmer switch information
SCGCQ00379104 - Not able to get paged view of StorCLI output on VM-Ware Platform
SCGCQ00390777 - iMR_Inv_6.1:StorCLI- VD creation command does not give any message if we tried to create a PI VD using normal PDs
SCGCQ00392598 - Pause operation should be sync with in show status of the PR.
SCGCQ00392686 - For the perfmode command in the help file we are displaying the storcli.exe /cx set perfmode = <value> syntax
SCGCQ00393442 - Spelling mistake in keyword headlessSafeMode
SCGCQ00406580 - Adprestart command fails
SCGCQ00413803 - Factory Command /c0/bbu start retentiontest should not be supported in storcli
SCGCQ00438350 - Megacli crashes after invoking any command in system with one 9280-8e and 2 quad port qlogic FC cards.
SCGCQ00457906 - storcli_6.1:The help file for"./storcli /cx/mx set h " is missing
SCGCQ00374735 - StorCLI crashed when run on a Windows 2008 64-bit with 24GB of RAM and 66 drives attached
SCGCQ00380746 - Error handling for Drive FW download when the hardware is not supported.
SCGCQ00384729 - Storcli-Inv-multiple VD's in same DG, setting security using /cx/vall set security=on is Failing for every VD except 1st VD
SCGCQ00392501 - StorCli_5.7 : "/c0/bbu start learn h " is not showing.
SCGCQ00394005 - Enabling OCR from StorCLI actually disables the controller property.
SCGCQ00394375 - Adprestart command fails
SCGCQ00397920 - StorCli_MR: BBU Strart learn command displaying twice in the "/c0/bbu h"
SCGCQ00400025 - Storcli shows inaccurate Elapsed Time as recon progresses
SCGCQ00400640 - Copyright information is showing wrongly
SCGCQ00408070 - StorCLI does not show both "Current Write Policy" and "Default Write Policy" for VD
SCGCQ00423347 - Storclif :Segmentation Fault with execution of legacy command BBUMFGSET .
SCGCQ00423832 - EFI_ Storcli: Cannot set vpd file on controller, EFI hangs and cannot proceed for further operations until reboot
SCGCQ00433513 - StorcliF : Not able to get or set connector mode on cassiopeia controller
SCGCQ00436931 - CLI displays VPD data for TMM and Battery/Supercap = ONLY TMM Data Extracted but NOT Supercap Data
SCGCQ00449134 - Battery Over-temp is not showing correctly.
SCGCQ00454427 - Storcli_6.1:"press any key to continue" showing twice in the lagacy command
SCGCQ00464708 - Storcli display total number of VDs in a individual drive group properties.
SCGCQ00369258 - Description is shown as "None" when using verchk option while flashing fw.
SCGCQ00392053 - MegaCLI and StorCLI should display "Estimated Time Left" in hours, days and minutes format.
SCGCQ00396665 - StorcLi_5.7: Remove the description for "Ra=Read Ahead Adaptive" in VD show info.
SCGCQ00397663 - StorCli_MR: While creating VD using default values FW allows read policy as"Ra=Read Ahead Adaptive" as against PR-317400
SCGCQ00399443 - StorCLI App Crash while execution of event info for vd ccincon
SCGCQ00402910 - StorCli_6.0:Raid level can be created even wthout delimiter(i.e size=1gb1gb1gb1gb)
SCGCQ00424978 - Is VD Emulated=Yes when emulationType=1
SCGCQ00436107 - The bootwithpinnedcache logic is backwards, both storcli and the FW are affected
SCGCQ00448094 - core dump while issuing storcli command ./storcli /c0/fall show all.
SCGCQ00454971 - storcli /c0 show is not listinf SWR controller
SCGCQ00378448 - StorCLI reports incorrect message when download a firmware image to the controller with pinned cache
SCGCQ00395178 - storcli doesnt support legacy MegaCli elf commands
SCGCQ00400139 - StorCLI shows date of manufacture in non-convention format
SCGCQ00413789 - storcli crashes on having a non PI drive and trying to create pi vd on all the drive
SCGCQ00422006 - Storcli crashes when given wrong in put file to set VPD on controller
SCGCQ00442444 - MR_Inv_6.1:StoreCLI- StorCLI gives wrong info when preserved cache is generated on 4K VD (./storcli /c0 show preservedcache).
SCGCQ00442652 - SWR_1.34 - Serial number field is blank in controller information and the same could be updated with N/A in StorCli
SCGCQ00066241 - MPI 2.5: Power Management
SCGCQ00308453 - MPI2: IR reporting Elapsed Seconds
SCGCQ00299943 - MPI2: add IOCExceptions bit for Partial Memory Failure
SCGCQ00250721 - MPI2: Update Hard Reset Algorithm with new timings
SCGCQ00209048 - MPI2: Return Port info in the SAS Device Status Change Event
SCGCQ00201727 - MPI2: Add spin-up disable bit to SAS IO Unit Page 4
SCGCQ00201203 - MPI2: Remove/Obsolete MPI Power Management Control Feature PCIE_LINK
SCGCQ00194293 - MPI2: product specific range for extended image type
SCGCQ00116336 - Gen 3: method to enable/disable FastPath capability on a per-device basis
SCGCQ00125672 - Gen 3: add 12Gb/s option for link rate
SCGCQ00125683 - MPI2: add Link Rate of UNSUPPORTED_PHY_ATTACHED
SCGCQ00136677 - Gen3: add optional vendor-unique region to MPI25_SCSI_IO_REQUEST structure
SCGCQ00137514 - MPI2: add PCI Device ID for Warhawk
SCGCQ00138259 - MPI2: add alternative defines for SGE Direction bit
SCGCQ00140397 - MPI2: modify Host Based Discovery Action Request
SCGCQ00141834 - MPI2: ability to disable SATA NCQ on a per-device basis
SCGCQ00155192 - MPI 2.5: update PCI Device Ids for Invader / Fury
SCGCQ00157968 - MPI2: Add new Config Page Type - Extended Manufacturing
SCGCQ00159010 - MPI2: MFG 7 update: method to link ISTWI devices, GPIO, PHYs of a SAS connector
SCGCQ00160485 - MPI2: Change MPI Simple SGE Local bit description and IEEE Chain Flags to match HW
SCGCQ00161661 - MPI2: Add IOC Temperature Monitoring Capability
SCGCQ00162562 - MPI2: rework Pinout field of ConnectorInfo for MFG Page 7
SCGCQ00162597 - MPI2: reserve some FWDownload ImageType values for product-specific use
SCGCQ00163413 - MPI2: IOUnit page 7: Add new fields for Board temperature
SCGCQ00163641 - MPI 2.5: SCSI Initiator I/O path counters (SAS IO Unit Page 16)
SCGCQ00164407 - MPI 2.5: review SGE Flags for Local bit and Data Location Address Space changes
SCGCQ00166171 - MPI2: new event for NOTIFY(Enable Spinup)
SCGCQ00176893 - MPI 2.5: new Power Performance Change Event to report changes to global power management mode
SCGCQ00177635 - MPI 2.5: report offset of first EEDP error in SCSI IO Reply
SCGCQ00268818 - Allow for MPI 2.5 IEEE Chain Element in SATA Passthrough Request
SCGCQ00283196 - Toolbox Diagnostic CLI Request now uses IEEE SGL, including chain elements
SCGCQ00378774 - new storcli object is added to storcli to represent cachevault
SCGCQ00413314 - Implement storclif commands - get/set hwdevice and configpage
SCGCQ00413317 - Implementation of StorCLIF command for AdpSetSubOEMId XX -aN and AdpGetSubOEMId -aN
SCGCQ00421090 - Added the HA code to MR5.8 stream
SCGCQ00425077 - Set factory default command in StorCLI
SCGCQ00283198 - MPI2: Toolbox Diagnostic CLI Tool Request may now use chain elements in the SGL
SCGCQ00258327 - MPI2: Reserve Product Specific range for Event codes
SCGCQ00229719 - MPI2: BIOS Page 1 additions for UEFI HII
SCGCQ00228572 - MPI2: add 4K sectors supported bit to IOC Page 6 CapabilitiesFlags field
SCGCQ00203886 - MPI2: New RAID Action (COMPATIBILITY_CHECK)
SCGCQ00194461 - MPI2: Add auto reserve and 8-kbit seeprom support to ISTWII
SCGCQ00128142 - Gen 3: update MPI v2.5 header files
SCGCQ00132183 - MPI2: add optional vendor-unique region to MPI2_SCSI_IO_REQUEST structure
SCGCQ00136201 - MPI2 - additional IR status information
SCGCQ00142578 - MPI2: obsolete MPI2_IOUNITPAGE1_MULTI_PATHING
SCGCQ00169936 - MPI 2.5: remove Command Determines Data Direction bit from SCSI IO
SCGCQ00172984 - MPI2: for SRIOV, allow PF to access config pages for other VFs
SCGCQ00175997 - MPI2: Add IO Unit Page 10 - Host Credit Balancing
SCGCQ00218764 - MPI2: new name for SCSI IO Request Control bits
SCGCQ00227491 - MPI 2.5: IR - new Raid Action to enable the Fast Path
SCGCQ00209055 - MPI2: create product-specific range for RAID Action Request
SCGCQ00125496 - Gen 3: remove Release On Full option for diag trace buffer
SCGCQ00159395 - MPI 2.5: Obsolete MPI2_RAID_VOL_CREATION_BACKGROUND_INIT
SCGCQ00175743 - MPI2: method to communicate between hosts on virtual functions
SCGCQ00433477 - Mapping of MegaCLI(DPMenable(set/get) & ForceSGPIO(get/set) command to StorCLI( (show/set -> DPM) & (show/set SGPIOforce))
SCGCQ00438735 - Changed the storcli syntaxes as Suggested by PDM's and FAE's.
SCGCQ00157982 - MPI 2.5: Chain SGL Segment sizes
SCGCQ00399602 - storcli support for LSI and OEM, factory
SCGCQ00412981 - implementation of StorcliF commands for adpsetsasa,adpdiag,adpshutdown
SCGCQ00435665 - storcli mapping for the missing legacy commands
SCGCQ00125662 - MPI2: review Task Set Full handling
SCGCQ00353002 - Signed FW Update
SCGCQ00375811 - Need MegaSCU for changes in MFC
SCGCQ00380155 - Undo - blocking firmware update for drives behind ALTA
SCGCQ00413337 - MWCLI. storcli builds for LSI and OEM factory, please check description.
SCGCQ00137489 - MPI2: bring Diagnostic Data Upload Tool forward from MPI v1.5
SCGCQ00379169 - Remove support for flashing firmware on PDs behind ALTA
SCGCQ00413064 - Implementation of MegaSCU commands in storcli syntax
SCGCQ00413432 - Implementation of commands mentioned in the desc below
SCGCQ00441143 - Implementing Bad block management related comands in storcli.
SCGCQ00369601 - MWCLI. Add -adpbattest capability to EFI CLI
SCGCQ00369604 - Rebuild time reset
SCGCQ00381311 - dcmd path chagnes for supporting the new cachevault api
SCGCQ00419161 - Implementation of StorCLIO command for ADPMFGSET -f file a0 in storcli
SCGCQ00419336 - Implementation of setPcilinkspeed command in storCLIF
SCGCQ00423256 - RRB 45 - CLI Reporting of TMM VPD
SCGCQ00369742 - MWCLI. R10, R50, R60, R00 VD creation
SCGCQ00381093 - PR SCGCQ00319011: Rebuild time reset
SCGCQ00433703 - Megacli/storcli support for lmrc driver
SCGCQ00434744 - Equivalent storcli command implementation of MegaCLI -AdpGetPciInfo -aN|-a0,1,2|-aALL
SCGCQ00447069 - Implementation of StorCLIO command for Adpnvram clear a0 in storclio as well as support legacy command
SCGCQ00413330 - Storcli reports "segmentation fault" when running command to downgrade controller to iMR
SCGCQ00413856 - remove the "Drive write cache" policy from Pd information.
SCGCQ00417917 - UEFI StorCli doesn't show the correct UEFI Driver Version
SCGCQ00413017 - Storcli reports "segmentation fault" when running command to downgrade controller to iMR
SCGCQ00413888 - StorCli_6.0-The help file for "storcli /cx/dx set security " is missing
SCGCQ00376240 - System halts on issuing storcli commands in EFI Environment.
SCGCQ00411384 - Unable to start migration from R0 to R5
SCGCQ00411614 - hits segmentation fault while creating multiple Vd's on Raid 10.
SCGCQ00413311 - Cannot change or update controller date and time in MegaSCU
SCGCQ00437065 - Driver Version is not shown
SCGCQ00375839 - StorCLI: The legend for "phy Error Counters" exceeds the 80-char limit.
SCGCQ00411449 - Improper output when configure R10 VD.
SCGCQ00414863 - When a command fails, subsequent commands/actions are aborted in storcli (MegaCli)
SCGCQ00413041 - Getting error message while installing or upgrading on Linux platform
SCGCQ00458499 - Block configuration with unsupported strip element sizes
SCGCQ00414383 - When a command fails, subsequent commands/actions are aborted in storcli (MegaCli)
SCGCQ00391744 - StorCli-"show ctrlcount" help is not displaying.
SCGCQ00412593 - Resolving compiler errors for Ctrl-R
SCGCQ00425263 - storcli /c0 show all : did not have HA information+request to add additional info


v1.04.07
SCGCQ00364332 - StoreCLI does not give proper message while trying to create 33rd VD on iMR FURY controller
SCGCQ00374336 - System halts on issuing storcli commands in EFI Environment.
SCGCQ00374732 - StorCLI cannot set "bypasserror" or "be"
SCGCQ00374733 - Storcli does not show 512 strip size in the online help
SCGCQ00378124 - Porting of AdpRestart Command
SCGCQ00372155 - Certain controller features displayed under "show all" exceeds 80-char limit.
SCGCQ00374118 - StorCli-"/c0/dall show all "in FreeSpaceDetails legend missing for "ID/VD/AfterVD"
SCGCQ00378135 - portings of AdpRestart command
SCGCQ00378828 - StorCLI-Legacy:'adpbootdrive get' fails to get bootdrive information.
SCGCQ00372264 - StorCLI: The legend for "phy Error Counters" exceeds the 80-char limit.
SCGCQ00374418 - Storcli : controller information query for OEM controller is displaying the status as failure.
SCGCQ00375757 - "StorCLI /cx/bbu show modes" show the bbu modes description without the actual bbu mode number
SCGCQ00374735 - StorCLI crashed when run on a Windows 2008 64-bit with 24GB of RAM and 66 drives attached
SCGCQ00380746 - Error handling for Drive FW download when the hardware is not supported.
SCGCQ00369258 - Description is shown as "None" when using verchk option while flashing fw.
SCGCQ00378448 - StorCLI reports incorrect message when download a firmware image to the controller with pinned cache
SCGCQ00375811 - Need MegaSCU for changes in MFC
SCGCQ00380155 - Undo - blocking firmware update for drives behind interposer
SCGCQ00379169 - Remove support for flashing firmware on PDs behind interposer
SCGCQ00375839 - StorCLI: The legend for "phy Error Counters" exceeds the 80-char limit.

v1.03.11 - Initial release

*Third-party trademarks are the property of their respective owners.
