This release note and the software that accompanies it are copyright (c) 2014 Intel Corporation or its suppliers, and may only be installed and used in 
accordance with the license that accompanies the software.

This Software is furnished under license and may only be used or copied in accordance with the terms of that license. No license, express or implied, 
by estoppel or otherwise, to any intellectual property rights is granted by this document. The Software is subject to change without notice, and should not 
be construed as a commitment by Intel Corporation or its suppliers to market, license, sell or support any product or technology. Unless otherwise provided 
for in the license under which this Software is provided, the Software is provided AS IS, with no warranties of any kind, express or implied. Except as 
expressly permitted by the Software license, neither Intel Corporation nor its suppliers assumes any responsibility or liability for any errors or inaccuracies 
that may appear herein. Except as expressly permitted by the Software license, no part of the Software may be reproduced, stored in a retrieval system, 
transmitted in any form, or distributed by any means without the express written consent of Intel Corporation.

==========================
Supported RAID Controllers
==========================
Intel(R) Integrated RAID modules RMS2LL080 and RMS2LL040
Intel(R) RAID controller RS25GB008 and RS25FB044
Intel(R) Integrated RAID Module RMS25JB040, RMS25JB080, RMS25KB040, RMS25KB080, RMS25LB, and RMS25LB080

Please verify that this utility has been tested with the RAID card/module you have chosen to use by checking the drivers web page for your controller 
at http://WWW.intel.com/support/

===================
Package Information
===================
Driver Version = 19.0-2.00.72.02
OS supported = 
Windows* 2003 (x86, x64)
Windows* XP (x86, x64) 
Windows* 2008 & R2 (x86, x64) 
Windows* Vista (x86, x64) 
Windows* 7 (x86, x64)
Windows* 8 (x86, x64)
Windows* 8.1 (x86, x64)
Windows* 2012 (x64)
Windows* 2012 R2 (x64)

=========
Attention
=========
Please see the read me file in each release subdirectory for special instructions specific to that Windows version.

==================
Known Restrictions
==================
N/A

=======================
Contents on the package
=======================
The following files(or folders) are included in this package:

Name						Description
SAS2_ITIR_Windows_DRV_ph19_readme.txt		This file
License_v2.pdf					License file
/XP						x86 and x64 version drivers for Windows* XP
/Win2K3						x86 and x64 version drivers for Windows* 2003
/Win2K8						x86 and x64 version drivers for Windows* 2008
/Vista						x86 and x64 version drivers for Windows* Vista
/Win7_2K8R2					x86 and x64 version drivers for Windows* 7 and Server 2008R2	
/Win8_2K12					x86 and x64 version drivers for Windows* 8 and Server 2012
/Win8.1_2K12R2					x86 and x64 version drivers for Windows* 8.1 and Server 2012R2

=========================
Installation Instructions
=========================
This updated driver can be applied using the normal OS installation options.


The following procedure describes how to install Windows 2012/2008/Vista/7/8 system onto RAID logical disk:

1. Copy the driver files to a removable media, such as USB flash drive, CD-ROM, or floppy disk
2. Create RAID logical disk(s) using MPT OpROM Config Utility (during POST).
3. Boot Windows installation disk. Follow instructions on screen until below step is reached.
4. At "Which type of installation do you want?" screen, select "Custom (advanced)"
5. At "Where do you want to install Windows?" screen, select "Load Driver"
6. Install the removable media with the driver files (extracted in step 1)
7. Select "Browse" and locate the folder with the driver files and then select "OK"
8. Select "Next". There may be a 1-2 minute delay as drivers are loaded.
9. Select "Drive options (advanced)" to customize partitions - if necessary
10. Select "Next" to continue with the installation
11. There are several reboots during installation - ensure that the selected RAID array is the boot device during every reboot.

================

The following procedure describes how to provide the driver during installation of Windows* 2003/XP system:

NOTE: You will need a USB floppy drive in order to provide the driver during Windows installation. Some models of floppy drives have known limitations that result in driver installation failures. Intel recommends using USB floppy drives listed on the Tested Hardware and Operating Systems list for the serverboard you are using.

1. Extract package contents to a floppy diskette
2. Create RAID logical disk(s) using MPT OpROM Config Utility (during POST).
3. Start the Windows* 2003/XP installation by booting from the Windows installation CD-ROM.
4. Press <F6> when the screen displays: "Press F6 if you need..." 
Note: You must press <F6> for the system to recognize the new driver.
5. Choose <S> to specify an additional device when the screen displays:
"Setup could not determine the type of one or more mass storage devices..."
Note: If this screen is not displayed as the first user input, then pressing <F6> was not seen by the setup program. Reboot the system, and return to step 2.
6. The system prompts for the manufacturer-supplied hardware support disk. Insert the floppy diskette containing the Windows* 2003/XP device driver, and press <Enter>.
7. Scroll down the list until the appropriate selection for your system which contains the Intel Embedded Server RAID Technology II and for your operating system displays, then click <OK>.
8. Continue with the normal installation procedure.
   If installation fails after the first reboot, try another model of USB floppy drive from the tested list.

================

Installation of the driver after the operating system is installed:

1. Boot into applicable Windows OS. Click the Windows Start button and select Settings.
2. Click Control Panel.
3. Select Adapter.
4. Select the Drivers tab.
5. Scroll down the list until the appropriate selection for your system which contains the MPT SAS2 driver for your operating system displays, then click <OK>.
6. Select it, then remove it by clicking the Remove button.
7. Click the Add button.
8. Select the Have Disk button.
9. Insert the diskette or flash drive.
10. Select drive letter A: and click on <OK>.
11. Select MPT SAS2 and click OK.
12. After Windows* copies the driver, reset the system.

==================
Component Features
==================
N/A

============
Known Issues
============
N/A

=============
Fixes/Updates
=============
version 19.0-2.00.72.02
1. Resolves restart loop issue on Microsoft* Windows* 8.1 and Windows* Server 2012 R2 storage drivers 
   if the Microsoft Windows Update Rollup 2919355 (April 2014) has been installed.
2. Driver will send over temperature message to system event log when threshold exceeded
3. Implements Unit Attention Reset for multi-initiator environments
4. Peformance improvements for high CPU utilization workloads

version 17.0-2.00.66.02
1. Initial release for Windows* 8.1 and Server 2012R2
2. Adds support for Standby Immediate

version 15.0-2.00.60.00
1. Initial public release for for Intel(R) SAS Controller RS25LB040/80

version 14.0-2.00.58.00
1. Initial release for Win8 and Server 2012 only

version 13.5-2.00.55.01
1. Initial release for for Intel(R) SAS Controller RS25FB044

version 11.0-2.00.49.01
1. Initial release for Intel(R) Integrated RAID Modules RMS25JB040, RMS25JB080, RMS25KB040 and RMS25KB080

version 10.0-2.00.45.01
1. Package supports RS25GB008 and RMS2LL0x0

version 8.0-2.00.37.00
1. Initial release for for Intel(R) SAS Controller RS25GB008.

version 7.0-2.00.35.00
1. Posting IOCTL while not in Operational state
2. Add Intel RES2SV240 to windows lsinodrv.inf
3. Windows driver INF changes to support Intel unique identification in Device Manager when Intel Subsystem IDs are detected.

Version 5.0-2.00.20.00_upd_2010.07.06
1. Updated XP drivers to 5.0-2.00.21.00 and added 32 bit WHQL
2. Changed README file name

Version 5.0-2.00.20.00
1. Initial release for RMS2LL080 and RMS2LL040




*Third-party trademarks are the property of their respective owners.