================================================================================
Intel(R) Server Board S2600JF Family
Intel(R) Server System H2000JF Family Firmware Update Package
for embedded EFI Shell. 
================================================================================
Intel Product Collaboration and Systems Division
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================
DATE    : Jan 13, 2015
TO      : Intel(R) Server Board S2600JF Family
	  Intel(R) Server System H2000JF Family customers
SUBJECT : Release Notes for System Firmware Update Package 
================================================================================
                              ABOUT THIS RELEASE
================================================================================
BIOS   : 02.04.0003
ME     : 02.01.07.328
BMC    : 01.22.6890
FRUSDR : 1.13
================================================================================
                           Support Platforms and Dependency
================================================================================
Processors supported: 
Intel(R) Xeon processor E5-4600/2600/2400 series
Intel(R) Xeon processor E5-4600/2600/2400 v2 series

Microcode update versions:
Intel(R) Xeon processor E5-4600/2600/2400 series C0 stepping: 0x00000513 CPUID = 0x206D5
Intel(R) Xeon processor E5-4600/2600/2400 series C1 stepping: 0x00000619 CPUID = 0x206D6
Intel(R) Xeon processor E5-4600/2600/2400 series C2 stepping: 0x00000710 CPUID = 0x206D7
Intel(R) Xeon processor E5-4600/2600/2400 v2 series C0/C1 stepping: 0x00000428 CPUID = 0x306e4

On-Board Component Option ROM Versions:
Integrated Matrox VGA               : VBE BIOS V3.8 SQ
1G PXE Option ROM                   : Intel(R) Boot Agent GE v1.5.53.1
10G PXE Option ROM                  : Intel(R) Boot Agent XE v2.3.24.1
iSCSI Option ROM                    : Intel(R) iSCSI Remote Boot version v3.0.34
FCoE Option ROM                     : Intel(R) 10G FCoE OpROM v1.8.17
UEFI Pxe drvier:		    : v6.3.27
SAS RAID Option ROM - RSTe          : 4.1.0.1026
SATA RAID Option ROM - RSTe         : 4.1.0.1026
SATA RSTe EFI driver Version        : 4.1.0.1026
SAS RSTe EFI driver Version         : 4.1.0.1026
ESRT II FOR SATA                    : A.14.02121826
ESRT II FOR SCU                     : SCU.11.08131348I          
BIOSAC                              : V2.4  
SINIT                               : v2.2
Intel(R) QPI Reference Code Version : V2.00.00.03
Memory Reference Code Version       : V2.00.00.03

Management Engine Firmware Version  : 02.01.07.328

================================================================================
                  System Firmware Update Package Usage instructions                   
================================================================================
This package can be updated using one of the following methods:
 - The embedded UEFI shell
 - Intel(R) Deployment Assistant
 - Windows* or Linux* operating system using Intel(R) One-boot Flash Update (OFU)
   V11.0 Build 9 or later)
 - Windows* Preboot Execution Environment (WinPE)


*************************************************************************************
To Update from the embedded EFI Shell

update system firmware from Intel server EFI shell by the following steps:
- Download Intel server system firmware update package from support.intel.com
- Unzip package and copy all files to root folder in USB disk on key 
- Insert USB disk on key to server USB port
- Reboot server, system will start BIOS/BMC/FRUSDR update automatically

  If case for some reason or you didn't put unzipped package under root folder of USB key, 
  you can do it by:
- Reboot server to EFI shell manually
- Run command "map -r" in EFI shell to mount USB disk on key
- Run command "fs0:" to change folder to USB disk on key, USB key may also mount to
  fs1:. The number of "fs" is dependent on the result of command "map -r"
- Change folder to the folder storing the firmware package
- Run command "startup.nsh" to start firmware update process

Please refer to "EFI_Instructions.pdf" in this firmware package for a quick guide to 
use the EFI commands

To Update from Intel(R) Deployment Assistant (IDA)

The Intel(R) Deployment Assistant software is easy to use and is present on the 
"Intel(R) Server Deployment toolkit" CD shipped with the system.
User can download the latest version IDA CD ISO image from support.intel.com
To use the IDA CD to update the system firmware:
- Boot server with IDA CD
- Select "Get System Updates" 
- Choose one of the three options 

  . From support.intel.com
    Automatically downloads the latest Firmware Update Package from Intel 
    It requires Internet connection
    Enter your local IP address and proxy configuration
    Click "Next" to start the download and update process

  . From my network
    Download the latest Firmware Update Package from support.intel.com and copy 
    it to a Windows* shared folder
    Enter your local IP address, the Windows* file server name, and a
    Windows user name and password
    Select the firmware package in pop-up window
    Click "Next" to start the update process

  . From USB Disk on Key or Hard Disk
    Download the latest Firmware Update Package from support.intel.com and copy it 
    to a USB key, then insert the key into the server USB port
    Click "Browse"
    Select the firmware package in pop-up window
    Click "Next" to start the update process
    
  Note: The Firmware Update Package is in the ZIP file format. Do not unzip 
        before copying to a Windows* shared folder or USB disk.

To update from Windows* and Linux* or operating systems using the Intel(R) One Boot
Flash Update Utility (OFU)

Intel(R) One boot Flash Update utility can be downloaded from support.intel.com
and it is part of the "BIOS, Firmware Update & Configuration Utilities" for 
Windows* and Linux*. Please refer to Intel OFU user guide about the details of 
installation and usage of OFU.

Use OFU to update system firmware by the following steps:
- Install OFU on Windows* or Linux* system
- Download the latest firmware update package from support.intel.com
- Unzip package to a folder
- Run the following command in Windows* command line/Linux* terminal window:
  <OFU install folder name>:\flashupdt -u  <package folder name>\flashupdt.cfg
                       
To update from Windows* Preboot Execution Environment (WinPE)

The System Firmware Update Package can be inserted to Windows* PE customized image 
for creating a bootable Windows* PE CD. User is able to update system firmware from 
customized WinPE CD by the following steps:
- Boot server with customized WinPE CD
- Run script "WinPE21_x64_Update.bat" or "WinPE20_x86_Update.bat" 
  (name may be varied depends on your own customization)
  
Note:
1. The Intel(R) OFU utility is case sensitive. Therefore, when you transfer the 
Firmware Update Package using USB key from a Microsoft Windows* system to a Linux
environment, you must first extract under the Linux* environment. Otherwise, you 
will need to mount the USB key manually with 'vfat' option under Linux to avoid 
conversion from upper case to lower case and vice versa.

2. To make Intel(R) OFU utility run properly under x86 or x64 OS, you have to read
OFU releaenotes on known issues for OFU installation.

3. In this SFUP package, Intel only provide batch file "WinPE_x86_Update.bat"
for WinPE2.0 32 bit solution "WinPE_x64_Update.bat" for WinPE2.1/3.0 64 bit 
solution as an example. Please refer to white paper "White Paper-Intel Server 
Utilities Procedure for WinPE.pdf" for details on building your own customized 
WinPE CD.

4. Windows PE 2.0 - built from Windows Vista SP1 32bit or EM64T
5. Windows PE 2.1 - built from Windows Vista SP1 or Windows Server 2008, EM64T
6. Windows PE 3.1 - built from Windows Server 2008R2, EM64T
7. Microsoft IPMI driver is loaded by default from WinPE CD, if you want to use 
Intel IPMI driver instead of MS IPMI driver for firmware update, you can un-install
Microsoft IPMI driver by:
                Devicesetup.exe ¨Cv remove *IPI0001
                Note: IPI0001 is the device ID for Microsoft IPMI driver.



================================================================================
				KNOWN ISSUES/WORKAROUND
================================================================================
- BIOS R02.01.0002 and later is compliant to UEFI specification 2.3.1.
  If the system is running these versions then the user needs to update their
  utilities and System Management Software to the versions shown below. 
  Failure to do so may cause the lower versions of the utilities and System
  Management Software to malfunction.
    Utilities
      OFU       v11 Build 15 or higher
      selview   v11 Build 10 or higher
      syscfg    v12 Build 8 or higher
      sysinfo   v12 Build 10 or higher
    
    System Management Software
      Intel(R) Active System Console (IASC)  6.1.10 or higher
      Intel(R) SNMP Subagent (SNMP-SA)       6.0.10 or higher
      Intel(R) Deployment Assistant (IDA)    5.1.3 or higher


=================================================================================   
 				BIOS R02.04.0003
=================================================================================
 - Update: Integrate the new SSID(0x355B) of Intel Ethernet Controller X540 module in BIOS for supporting the new EEPROM of this IOM.


=================================================================================   
 				BIOS R02.04.0002
=================================================================================
 - Updated: LAN Oprom (1G PXE_v1.5.53.1;10G PXE_v2.3.24.1; 10G Fcoe_v1.8.17; iSCSI_v3.0.34) 
 
 
 =================================================================================   
 				BIOS R02.04.0001
=================================================================================
 - Fixed: SUT won't occur SPD failure
 - Fixed: AMIBCP not able change BIOS setting "C6".
 - Fixed: No video output from K5000 DVI port on LHP platform
 - Updated: RSTe 4.1.0.1026 OPROM 
 - Updated: LAN Oprom (1G PXE_v1.5.56;10G PXE_v2.3.27; 10G Fcoe_v1.8.17; iSCSI_v3.0.34)
 - Updated: Disable A7 setting

 
=================================================================================   
 				BIOS R02.03.0004
=================================================================================
 - Fixed: SMBIOS utility reports error:Internal Reference Designator
 - Fixed: Some Options show up in BIOS setup but do not exist in BIOS EPS1.0
 - Fixed: Removable RAID Controller in GZP
 - Fixed: Boot device discover problem after BMC reset with EFI Optimize
 - Fixed: Boot stop on an abnormal screen after excute cmd iflash32 /rd 
 - Fixed: Zepher related issue on BlackBearPass
 - Fixed: No password was required in order be able to using the key for Network
 - Fixed: The ACPI test log have an error after run Pets10.0.
 - Fixed: Error messeage will not be logged after CMOS battery removal
 - Fixed: WHEAHCT Logo failed in Win2012R2 WHQL test on S4600LH.
 - Fixed: Utilities cannot get SMBIOS in UEFI aware Linux.
 - Fixed:Utilities need BIOS help to allocate 8KB reserved memory below 640
 - Updated: New ESRT2 OpROMs for Romley Production BIOSes.- 
 - Updated: RH7 support
 - Updated: Support NTB on Freemontpass
 - Updated: Processor Microcode 0x00000428 CPUID = 0x306e4
 
 
=================================================================================  
 				BIOS R02.03.0003
=================================================================================
 - This version enhances the protection of certain UEFI variables as described in 
	Intel Security Advisory INTEL-SA-00038

=================================================================================   
 				BIOS R02.03.0002
=================================================================================
 - Add "Memory Performance" option in BIOS Setup

=================================================================================   
 				BIOS R02.03.0001
=================================================================================
 - Fixed: IRQ of 10GigE (on board) is not described by BIOS on S4600LH
 - Fixed: System does not reset when memory address parity error
 - Fixed: Blank console issue fix 
 - Fixed: CTLE Settings for S4600LH platforms
 - Fixed: System halt after creating RAID with 9750 card
 - Fixed: User selected power policy not programmed into MSR 0xB01
 - Fixed: ME not reporting SmaRT/CLST events to the SEL.
 - Fixed: blank lines in server management screen
 - Fixed: Change SMBIOS Type 1 - "SKUNum and Family fields" default from 
   "To be filled by O.E.M" to "00"
 - Fixed: Show error "BIOS handoff failed"after installLinux OS under UE
 - Fixed: The SMBIOS log has wrong description about Port Type in Type8
 - Fixed: Qlogic 4-Port Fiber Channel Cards Configuration does not work
 - Fixed: SYSCFG "/bbo" and "/bbosys" not working as expected when "Static Boot Order" Enabled
 - Fixed: After setting Admin password to enabled, no password is requested
 - Fixed: BIOS needs to support more than 8 NIC boot from PXE
 - Fixed: RMS25CB080 -610 board may not be detected on some platforms

 
Others:
 - Update processor microcode
 - Update support for additional devices on PCIe Gen 3 qualified list on the 
   Intel(R) Server Platforms for E5-4600/2600/2400 CPUs.
 - Restore customized defaults when auto recovering from NVRAM corruption 
 - Update reference code (V02.00.00.03)


=================================================================================   
 				BIOS R02.02.0003
=================================================================================
 - Fixed: IRQ of 10GigE (on board) is not described by BIOS on S4600LH
 - Fixed:System does not reset when memory address parity error
 - Fixed: CTLE Settings for S4600LH platforms
Others:
- Update processor microcode.

=================================================================================   
 				BIOS R02.02.0002
=================================================================================
- Fixed: The system can't power up after restoring the BIOS default value via removing the
         CMOS battery

=================================================================================   
 				BIOS R02.01.0001
=================================================================================
- Fixed: Network Stack is hidden and the default value of IPV4 PXE option is set 
         to disabled.
- Fixed: The Onboard infiniband controller name is shown incorrectly in BIOS setup
         on some half-width board.
- Fixed: Adaptec* 6405E installation causes system unstable in earlier BIOS POST.
- Fixed: System boot takes longer time when Throttling mode is set to "Auto" with 
         particular memory DIMM populated. 
- Fixed: 2 ports of Qlogic* QLE2562 card can not be configured in Option rom. 
- Fixed: Device manager of Windows Server 2008R2/2012 shows some unknown devices 
         when Intel(R) Xeon processor E5-4600/2600/2400 v2 series installed.
- Fixed: The fourth NIC information is missing in SMBIOS table Type 41 on Intel(R)
         Server Boards S2600GZ and S1400SP.
- Fixed: Unexpected "." is shown after the product name in SMBIOS Type 1.
- Fixed: Some BIOS options have different values after loading Default (press F9 in
         setup) and CMOS clear.
- Fixed: Wake-on-LAN (WOL) feature does not work on Windows Server 2008R2/2012 OS.
- Fixed: Unable to enter the LSI* MegaRAID Configuration Utility by pressing "Ctrl+C" 
         on LSI* SAS 9200 controllers in some specific scenario.

Others:
 - Add UEFI 2.3.1 support.
 - Add UEFI PXE support.
 - Add UEFI Driver Control option in BIOS setup menu.
 - Add Intel(R) Virtualization technology support for Intel(R) Xeon processor E5-4600/2600/2400 v2 series.
 - Add QLogic* QLE2762 Gen3 support for Intel(R) Server Board S2600GZ/GL.
 - Add an option in setup layout for enable/disable Intel(R) RAID modules RMT3CB080/RMS25CB080/RMS25CB040.
 - Add C600 unsupported Upgrade Keys warning message implemented.
 - Add Intel(R) SAS module RMS25LB Gen3 support for S2600JF, S2600WP, S1600JP. 
 - Update Intel(R) Boot Agent (1G PXE Option ROM, 10G PXE Option ROM, iSCSI Option ROM, FCoE Option ROM).
 - Update ESRT2 Option ROM for SCU and AHCI.
 - Update RSTe 3.7 Option ROM.
 - Update micro code for Intel(R) Xeon processor E5-4600/2600/2400 processors.
 - Update micro code for Intel(R) Xeon processor E5-4600/2600/2400 v2 processors.
 - Update ACM 2.2.
 - Update "Extended ATR" default setting to 0x01 from 0x03.
 - Update ATA secure erase to non-frozen state.


================================================================================   
 				BIOS 01.08.0003
=================================================================================
- Added C0 microcode version 0x405 for Intel(R) Xeon processor E5-4600/2600/2400 v2.

NOTE:This BIOS does *not* support Intel(R) Xeon processor E5-4600/2600/2400 v2 steppings earlier than C0.

================================================================================   
 				BIOS 01.08.0002
=================================================================================
- Fixed: Quiet Boot option doesn't work sometime. 

Others:
 - Do not display add-in card option rom in Quite Boot Mode.

================================================================================   
 				BIOS 01.08.0001
=================================================================================
- Fixed: BIOS can't automatically detect the boot files on the local HDD in EFI optimized boot mode.
- Fixed: Utility such as DMIDECODE and SYSCFG utility can't get SMBIOS information 
         under UEFI RHEL 6.2.   
- Fixed: Device on PCIe slot 4 cannot be recognized on Intel(R) Server Board S2400SC.
- Fixed: NIC1 Port2 PXE still shows as a boot option even when disabled in setup on 
	 on Intel(R) Server Board S1400SP.
- Fixed: Some add-on graphics card have compatibility issues with Microsoft* Windows* 7.
- Fixed: The length of BMC user password doesn't meet the specification.
- Fixed: S3 resume will hang sometimes.
- Fixed: NM Power reading is incorrect on Intel(R) Server Boards S2400SC and S2400EP.
- Fixed: Issue on Intel(R) Workstation Board W2600CR2 w/ Nvidia* Quadro* K5000 video adapter.

Others:
 - Add Fast Video feature on multiple platforms.
 - Update Onboard LAN Oprom incl. 1G/10G PXE, 10G FCoE, iSCSI.
 - Update ACM version.
 - Add support for the Intel(R) Xeon processor E5-2600 v2 series - bootable only. 
 - Add a warning message for the first boot if an Intel(R) Xeon processor E5-2600 v2
   production processor is inserted.
 - Add NTB support for Intel(R) Server Board S2600CO.
 - Serial Over Lan function works if Console Redirection is either disabled or enabled.
 - Update ME version.
  
================================================================================   
 				BIOS 01.07.0001
================================================================================= 
- Fixed: Update USB Stack to fix several USB issues.
- Fixed: HDD Driver Fault LED can't be set on Intel(R) Server Board S2400LP.
- Fixed: Update BIOS to higher UEFI version causes some failures with the flash utility.
- Fixed: System will hang after setting NIC1 Port1 to Disabled and then performing a reboot on Intel(R)
         Server Board S4600LH.
- Fixed: Correct SMBIOS Type 8 E-USB Connector Port Type on Intel(R) Server Board S4600LH.

Others:
 - Update help strings for setup item "Memory SPD Override".
 - Add Intel(R) Server Board S4600LH support for production.
 - Update Board Pre-link Initial Values, VGA selection routine to cover up to four sockets
   on Intel(R) Server Board S4600LH.
 

================================================================================   
 				BIOS 01.06.0002
=================================================================================   
Others:
- Add fix to avoid the potential issues by limiting the PCIe slot speed to Gen2 unless
  the add-in adapters are PCIe Gen 3 qualified on the Intel?Server Platforms.


================================================================================   
 				BIOS 01.06.0001
=================================================================================  
- Fixed: Remove NUMA setup option in Intel(R) Server Board S1400SP.                                     
- Fixed: IO_MOD/SAS_MOD slot number is displayed incorrectly in Microsoft* Windows* 2008.      
- Fixed: When the PCIe slot option ROM is set to disabled in BIOS setup, the option RoM is still enabled. 
- Fixed: WHEAHCT Logo Test fails in some Microsoft* Windows* certification.                
- Fixed: BIOS Setup screen may hang when loading efi image.
- Fixed: Some USB devices can not be recognized in Bios USB configuration page.

Others:
 - Update onboard SATA and SAS RAID option rom versions 
 - Update MRC rev. to 01.00.00.18
 - Display RAID configuration page in Quite Boot Mode when option rom is dispatched
 - Add PCIe Performance Tuning Knobs setup items
 - Add warnings in post screen when showing the capacity of the onboard RAID controller
 - Add memory 1866Mhz support for some platforms
 - Add fix in SMM hook in the runtime service
 
================================================================================   
 				BIOS 01.05.0001
=================================================================================  
- Fixed: User privilege of RMM4's channel3 mismatch with BIOS setup.
- Fixed: Abnormal items will be displayed in PCIe slot OPROM control page after 
         pressing F9 and then discard changes.
- Fixed: Onboard NIC can not be disabled through BIOS setup on Intel(R) Server board S2600IP.
- Fixed: There is "unknown device" in boot order when USB floppy plugs.

Others:
- Add Intel(R) Server Board S1400SP support.
- Fix some compatbile issue on memory Dimms with Atmel sensor.
- Update processor microcode.

================================================================================   
 				BIOS 01.04.0001
=================================================================================  
- Fixed: There are some error information in smbios type 178 on some platform.
- Fixed: BIOS Server Management Screen is not compliant with specification.
- Fixed: No Type 10 information within the SMBIOS table.
- Fixed: Only Serial port B could be found under Serial Port Config on some product.
- Fixed: Fix a bug in redirecting a Microsoft* Windows* OS ISO image file to another 
         system from a remote client. 
- Fixed: Can not disable NIC1 port1 in BIOS setup on Intel Server Board(R) S1400SP.
- Fixed: Some failures in SMBIOS Type 8 and Type 10 structure.
- Fixed: No ACPI S1 peripheral wake support under Red Hat* Linux 6.2 on Intel Server 
         Board(R) S4600LH.
- Fixed: Workaround for SDR Version incorrect in some cases.

Others:
- Add enable/Disable Option for PCIe option Rom.
- Add support socket 3 and 4 in Legacy VGA socket on Intel Server Board(R) S4600LH.
- Add PCIE CTLE setting on Intel Server Board(R) S1400SP.


================================================================================   
 				BIOS 01.03.0002
=================================================================================  
- Fixed: NIC Information can not be saved in the Sysinfo log file and it cannot be 
	 retrieved or set using the syscfg utility. 
- Fixed: If Remotely redirecting an ISO image from a client and the target system is restarted, 
	 the target system will automatically boot to the redirected ISO image and start an OS installation.

================================================================================   
 				BIOS 01.03.0001
================================================================================= 
- Fixed: On GUID based partitions any SMI call freezes system.
- Fixed: When the baseboard LAN IPV6 is enabled in BIOS setup, the RMM4 configuration is greyed out.
- Fixed: Unable to disable onboard NIC ports in BIOS setup.
- Fixed: C1E is disabled when both C3 and C6 processor Cstates are disabled in BIOS setup.
- Fixed: In BIOS setup, Serial B is incorrectly set to disabled by default and cannot be enabled.
- Fixed: TPM Admin Control option should be disabled (grayed out) when the BIOS admin password is not set.

================================================================================   
 				BIOS 01.02.0010
=================================================================================  
- Fixed: Onboard NIC2 MAC address can not be shown correctly and it can't boot to PXE from NIC2 on
         Intel(R) Server Board S2400EP. 

================================================================================   
 				BIOS 01.02.0009
=================================================================================  
- Fixed: Update add-in video output policy

================================================================================   
 				BIOS 01.02.0008
=================================================================================  
- Fixed: PCIe slot 5 max link width can only be detectes as x4 on Intel(R) Server Board S1400FP.
- Fixed: EFI network stack incorrectly uses Mezzenine NIC port.
- Fixed: FRB2 timer will reset the system after 6 minutes when entering BIOS Setup via the <F6> boot menu.
- Fixed: System cannot enter EUP Lot6 deep sleep mode.
- Fixed: PCIe link speed changes occur without logging a SEL event.
- Fixed: During POST, populeated PCIe slots numbers are incorrectly identified.
- Fixed: Cannot change Serial Port A to IRQ3 on Intel(R) Server Board S2600JF.
- Fixed: NIC1 and NIC2 cannot be disabled on Intel(R) Server Board S2400SC.
- Fixed: ACPI errors are reported in dmesg.log in SUSE* Linux* 11 SP2 RC x64.

================================================================================ 
 				BIOS 01.02.0007
=================================================================================
- Fixed: W2600CR Windows* 7 WHQL cert Failure - Single computer Display object Test Failure

================================================================================ 
 				BIOS 01.02.0006
=================================================================================
Others:
- Update ME version to 02.01.05.091
=================================================================================     
 				BIOS 01.02.0004                                     
=================================================================================
- Fixed:  S4 resume function is not stable on S2400BB.
- Fixed:  Correct some products' onboard slot numbers shown in Windows device manage
- Fixed:  Some NIC IO Modules cann't be displayed in the NIC Configuration page of BIOS Setup.
- Fixed:  Added specific blades items for S2600KI
- Fixed:  Workstation System cannot enter S3 state in UEFI Windows* 7.
- Fixed:  Onboard NIC device still can be detected in OS after disabled in BIOS
- Fixed:  MAC addresses are not shown in BIOS setup on S2400EP Dual port SKU.
- Fixed:  Some BIOS setup pages have incorrect strings and use incorrect format
- Fixed:  ME interface fails sometime after S3 resume back on S2600CP
- Fixed:  SMBIOS Type 8 of some product has some incorrect information
- Fixed:  Intel(R) X520-T2 10G NIC did not work at expected PCI-E link speed
- Fixed:  The HDD Fault LED on HSBP might behave incorrectly under some specific configurations.
- Fixed:  System sometimes can’t detect PCI-x storage card.

Others:
- Update new processor microcode and onboard device option roms

=================================================================================     
 				BIOS 01.02.0003                                      
=================================================================================
- Fixed:  NIC1 and NIC2 cannot be disabled in BIOS setup.
- Fixed:  Legacy VGA on CPU socket one is greyed out when add-in VGA card is associated
          with CPU socket 2.
- Fixed:  Serial over LAN cannot be activated via IPMI with Console Redirection enabled
          in BIOS setup. 
- Fixed:  PXE OPRom inoperative.
- Fixed:  ISCSI option missing on some platforms. 
- Fixed:  Implementation of "Iflash32 -rd" to load defaults on next system reset.
- Fixed:  The DIMM fault LED behaves incorrectly on DIMM_D3 under memory Sparing mode.
- Fixed:  Some Intel(R) NIC IO modules can't be detected under Microsoft* Windows* 2008 SP2.
- Fixed:  The information for Onboard NICs is shown incorrectly in BIOS setup.
- Fixed:  RAID RSTe OpROM fails to launch on AHCI SATA ports in RAID configuration.
- Fixed:  There is no "RMM4 IPv6 Enable/Disable" option in BIOS setup.
- Fixed:  The default value of Lan port PXE will show disabled for Intel(R) NIC I/O module.
- Fixed:  CPU information is shown incorrectly in SMBIOS table if the user populates
          different frequency processors.
- Fixed:  Active Processor Cores cannot be changed in BIOS setup.
- Fixed:  Turbo boost will be disabled when choosing the balanced performance policy in
          BIOS setup.
- Fixed:  Unexpected SEL entries logged after BIOS update.

=================================================================================     
 				BIOS 01.01.1002                                      
================================================================================= 
- First production release BIOS.


================================================================================
                     KNOWN ISSUES in 02.01.07.328 release
================================================================================
- On simulated memory throttling PECI register it was observed that Memory
  Throttling Statistics sensor reading value is update too late. Based on 250 ms
  sensor scanning interval sensor value should be updated after 6 seconds,
  actually it was updated later, up to 15 seconds.
- Too few steps in the ramp generated by SMART & CLST.
- No monitoring capability is reported in NM Capabilities sensor if temperature
  reading source is set to OEM command.
- PEC error is not reported for Send Raw PMBus commands of write/read word and
  block write/read type.
- Unstable limiting and Correction Time Exceeded event was sometimes observed
  for memory domain (id 2).
- In a system with more than 2 PSU the PSU discovery procedure is done every 1
  seconds while it should be done every 10 seconds. Too much traffic is observed
  on PMBus.
- Few percent power limit oscillations were observed when limiting in memory
  domain.
- P-state limit lock was observed two times in longevity tests of power
  limiting enable (policy create) and disable (policy destroy) cycles.
- If power threshold is defined in several NM polices and the power consumption
  exceeds the threshold the NM Alert Threshold Exceeded message is sent only
  for the first policy, not for all polices.
- There is no ME FW Health Event (Event Data 2 = 5: BMC did not respond to cold
  reset request and ME rebooted the platform) generated after shutdown caused
  by policy with shutdown action.
- Operational S0/S1 Only unblocks "Set Reset Mode" HECI command after ME reset.
- There is an additional global reset after the global reset caused by
  CPU_PWROK (or PCH_PWROK) dropdown.
- BIOS does not boot when ME is in Recovery mode. This affects boot from G3
  (Always On configuration) and any Sx exit (S0/S1 configuration).
- Get Self Test Results command does not return error for missing PSUs if their
  "PSU Status Sensor" is disabled.
- Global platform power NM Policy correction time is exceeded when power
  readings scanning period is set to 1000ms.

================================================================================
                     Issues fixed in 02.01.07.328 release
================================================================================
- Fixed: Platform is not able to power on properly after being shut down by NM
         Policy
- Fixed: Global platform power consumption reported by NM Statistics in S5 is
         incorrect
- Fixed: OOB (out-of-band) stress test by issuing the wrong username may cause
         connection to be unavailable
- Fixed: Shutdown action can be interrupted by cold reset when volatile NM
         policy is in use

================================================================================
			Issues fixed in 02.01.07.231 release
================================================================================
- Fixed: Improper ME FW Health Event is sent when ME is reset to factory
         defaults with IPMI command Force ME Recovery
- Fixed: Throttling statistics in domain 0 and 1 are equal to 0, when power
         policy is active in domain 0
- Fixed: Power limit oscillations were observed after adding 7 NM power
         limiting policies
- Fixed: NM Capabilities event is not sent after disabling then re-enabling
         scanning on its sensor
- Fixed: ME Power State Change notification is not sent after Set ME Power
         State command (M3 -> MOff)

===============================================================================
			ME Issues fixed in 02.01.07.112 release
================================================================================
- Fixed: ME may fail to perform reset initiated with IPMI command (02h Cold Reset
         or DFh Force ME Recovery) - observed after few hundreds of successful 
         resets. Following sequence happens when repeating 02h Cold Reset: 
           - CC 00h - command is accepted, but ME reset is not performed, 
           - CC CFh - command rejected, 
           - CC C0h - command rejected, repeated for all subsequent retries.
- Fixed: CPU Memory Throttling Status Sensor gets latched in "upper non recoverable"
         state following Memory Throttling event after G3. 

================================================================================
			 ME Issues fixed in 02.01.05.107 release
================================================================================
- Fixed: FW may hang in initialization state after the update of entire ME
         region is interrupted by AC loss. 
         - None of the available ME resets (AC cycle or Global Reset or Power
           Button Override) can get ME out of the error condition, only
           reflashing ME image. 
- Fixed: FW may become unresponsive after switching from Recovery to
         Operational (e.g. during Direct Update).
         - Global Reset or Power Button Override can’t get ME out of the error
           condition. 

================================================================================
			ME changes 02.01.05.091
================================================================================
- Fixed: Fix for Double AC cycle for recognizing OPROM changes

================================================================================
                   ME Changes in release 02.01.05.069
================================================================================

- Fixed: ME FW Health Event with Event Data 2 = 0 (Recovery GPIO forced) will
         be generated after IPMI command "Force ME Recovery" issuing.
- Fixed: ME FW unexpectedly resets when SMLink clock held low for a long period
         of time
- Fixed: Sometimes system stops responding after Power Cycle.

===============================================================================
			02.01.05.064
===============================================================================
- First production release of ME

===============================================================================
                               BMC changes
===============================================================================

===============================================================================
                          01.22.6890
===============================================================================

- Fixed: IPMB Bridging commands to a Satellite controller doesn't work
- Fixed: The result of IPMI raw command 20 c0 71 00 02 00 00 shows telnet can be supported.
- Fixed: The satellite FW updating status is 00 while updating HSBP FW.
- Fixed: i2c-adapter i2c-7: Arbitration lost on data transmission
- Fixed: Remote KVM video have some dirty mouse cursor under linux system
- Fixed: The System Fan 5 spining in 100% speed on S2400BB Platform after updated the BMC to 1.21.6038.
- Fixed: FW update will fail with OS based utility (OFU), failure rate is 20% with USB mode and 40% with KCS mode.
- Fixed: BMC code issue for fan detection on S2600CO.
- Fixed: EWS can't interpret SmaRT/CLST event
- Fixed: S2600GZ/GL EWS_update tool fail with SUP S2600GZ_GL_EFI_BIOS02030003_ME20107328_BMC1216038_FRUSDR113 
- Fixed: Openssl update (see TA-1065)
- Fixed: IPv6 can't get IP address via DHCP server.
- Fixed: S4600LH P3 LVDIMM voltate reading is 1.5V sometimes during system booting up
- Fixed: HSC firmware not updating with BMC 1.21.6038;
- Fixed: BMC Hangs upon the first A/C Power On of the board. Subsequent A/C power cycles, the BMC boots. 
-Bundled the new PSU fw for PSSF162202A.
-Bundled the new PSU fw for "DPS 750AB 32A".
-Set RMM4 DMN speed to 100Mbps on half width products

=================
                         01.21.6680
===============================================================================

- Fixed:  Downgrade RMM4 NIC Link speed from 1G to 100M 
===============================================================================
                         01.21.6593
===============================================================================

- Fixed: EPSD100243260-HSC firmware not updating with BMC
- Fixed: The satellite FW updating status is 00 while updating HSBP FW.
- Fixed: IPv6 can't get IP address via DHCP server.

===============================================================================
                         01.21.6467
===============================================================================

- Fixed: "Restore to default config" issue.

===============================================================================
                         01.21.6414
===============================================================================

- Fixed: Fan redundancy lost issue on 3th party chassis
- Fixed: 3th party chassis missing FAN presence events in SEL
- Fixed: OpenSSL update (see TA-1065)

===============================================================================
                         01.21.6038
===============================================================================
- Fixed: BMC User configuration is corrupted and users cannot be re-created.
- Fixed: The response of getting satellite fw update status is always 01
- Fixed: HSC slots status present sensor showed NA in EWS.
- Fixed: (X) Disk Drive LED - Locating drive is inconsistent in time to illuminate and stop
- Fixed: Hot Plug Fan not changing system status on Fan failure.
- Fixed: EWC Fan sensor readings disappear when filtered and there is a fan failure.
- Fixed: (X) BMC hung after network Scan.
- Fixed: Current power is incorrect on EWS while power down SUT by pressing power button.
- Fixed: Special characters '<>' of FRU info can't be shown in the EWS page.
- Fixed: Recurring temperature alarms on sensor #0x22(SSB).
- Fixed: (X) S600GL/S2600GR - Fail EMC Brownout testing.
- Fixed: DIMM Thrm Mrgn sensor shows "unknown" when just plug DIMM in Channel3 
- Fixed: [X] Updated Java signitures to support new JAVA requirements.
- Fixed: Get SOL Configuration parameters 5 & 6 should not return invalid response.
- Fixed: EWS is incorrectly decoding ME firmware update SEL events.
- Fixed: BMC channle 1 can not ping succesfully and EWS login fail while using static IPV6 address.
- Fixed: Baseboard IP address can't be assigned when IPv6 address set as auto-configuration.
- Fixed: IP address can't be assigned when IPv6 address set as dynamic.
- Fixed: BMC Hangs during first A/C power up.
- Fixed: Reading the PCI Riser temperature sensors for S2600CP was not operating correctly.
- Fixed: CFM calculation failed on PSU removal/insertion.
- Fixed: Enable FPGA logic to preserve PWM registers.
- Fixed: Check in 750AB V8 PSU image per PSU verification team's request
- Fixed: Porting FRU discovery APIs from Grantley where the Auto-Configuration feature requires the operational 
         status of the managed FRUs.
- Fixed: Add the displaying of the PS HW Revison for the PS if update is required or not.
===============================================================================
                                01.20.5793
===============================================================================
- Fixed: Cold Redundant Power Supply Configuration Issue, fix it by a DPS 750XB 
         A PSU v100 image.
===============================================================================
                                01.20.5446
===============================================================================
- Fixed: The Embedded Web Console was showing the incorrect version of ME
         Firmware when the ME was in firmware update mode.
- Fixed: Nothing displayed on the Embedded Web Console while logging in with an
         IPv6 address (stateless ICMPv6 discovery).
- Fixed: BMC Embedded Web Console session not maintained with a power cycle
- Fixed: E1208GL4GCN - does not maintain BMC web console session during power
         state change or system reset.
- Fixed: The Intel(R) Xeon(R) Phi(TM) Coprocessor adapters numbering is not
         consistent with riser slot numbering on server board.
- Fixed: Embedded Web Console SEL text log not decoding BIOS update versions
         correctly.
- Fixed: No video display in BMC KVM when SUT wakes up from S1 or S3 in 
         Windows* 2012.
- Fixed: S2600IP - Intel(R) Xeon(R) Phi(TM) Coprocessor adapter MIC Status 7
         shows as Unknown in some configurations.
- Fixed: S2600GZ - Intel(R) Xeon(R) Phi(TM) Coprocessor adapter MIC Status
         Sensor shows "Unknown" when only 1 MIC card exists in system.
- Fixed: Cannot set link-local gateway for BMC Network Management Interface
         using IPv6.
- Fixed: [X] Web Console not defaulting to English when another non-English
         browser is detected.
- Fixed: Add Cross Frame Options to prevent cross-frame scripting of Embedded
         Web Console
- Fixed: Browser autocomplete enabled before authentication.
- Fixed: SMI Timeout errors not logging IIO Global error registers in Debug Log
- Fixed: BMC LAN connection not working after IP address change.
- Fixed: Multi-node boards with node ID 1111 are not regarded as a single node.
- Fixed: BMC email alerts refused by some servers.
- Fixed: IP address of baseboard management NIC can't be configured
         successfully when dynamic and static IP changed.
- Fixed: The baseboard management NIC can't get a dynamic IP address when the
         VLAN set as enable.
- Fixed: Change to 1600W PSU firmware for an acoustic issue.
- Fixed: POST Error code 0xA6A0 was causing the SEL page to fail to render.
         - Also fixes decode of POST Error code 0x0012 and invalid POST Errors
           causing the SEL page to fail to render.
- Fixed: The ME firmware has 2 minor versions in the update related SEL.
         Updated the OEM command format to support this.
- Added: Support Intel(R) Xeon(R) Phi(TM) Coprocessor adapters in Intel(R)
         Server Boards and Systems.
- Added: Added a button on Web to enable/disable IPMI over LAN.

===============================================================================
                               BMC 01.19.5018
===============================================================================
- Fixed: The Intel(R) Xeon(R) Phi(TM) Coprocessor adapters Status Sensor shows
         "Unknown" when only 1 adapter is in the system
- Fixed: System Events for DIMM thermal margin sensors are not decoded properly
         in the Embedded Web Server and Embedded Web Server log files.
- Fixed: Embedded Web console not displaying sensor values for sensors from
         another controller
- Fixed: Chassis identify not working as expected.
- Fixed: The IHC (Intel(R) Hybrid Cloud) interface exposes a self-signed
         certificate containing a developer name and email address.
- Fixed: Integrated BMC Web Console Keyboard Macro Cltrl+Alt+F1 not working as
         expected.
- Fixed: BMC does not ignore momentary PWM interruptions after SMBALERT is
         asserted (SmaRT event).
- Fixed: Embedded Web Console Power Statistic page time value not getting
         updated.
- Fixed: IBMC used in Web Console Server Health > Event Log Page.
- Fixed: Embedded Web Console SEL decoding BMC FW Update Minor version
         incorrectly.
- Fixed: IO module Temperature sensor reading is always 0 on S2600JF.
- Fixed: Get User Access Command - Number of enabled users not correct.
- Fixed: Get/Set Processor Error Configuration and Status command not working
          as expected.
- Fixed: BMC update failing after 4 consecutive firmware updates.
         BMC will no longer stay in recovery mode (uboot) after four
         consecutive firmware updates.
- Fixed: JViewer always shows "Error reading video data" popup and a black
         screen when mouse mode is set to relative and JViewer tries to hide
         the cursor.
- Fixed: Multicast traffic was being passed through to the BMC causing slow
         downs and resets. This change enables multicast filtering, but still
         allows IPv6 multicasts for Neighbor Advertisement, Router
         Advertisement, and DHCPv6 relay and server multicast.
- Fixed: The UBoot code detects a bad CRC of the Ram Image when attempting to
         boot after getting a cold reset.
- Fixed: The recommendations in the Web Console Mouse Mode tab are out of date.
- Fixed: S1600JP 5V STBY sensor intermittently reporting low voltage error
         during AC cycle testing.
- Fixed: Disable POST codes LED output after system has completed POST
- Fixed: Correct the 750w PSU FW version. 
- Fixed: S2600JP: Update SDR to version 1.04.
- Fixed: S2600CO: Update SDR to version 1.10.
- Fixed: W2600CR/S2600IP: Update SDR to version 1.10.
- Fixed: S2600JF: Update SDR to version 1.11.
- Fixed: Update EPSD Platforms Based on Intel(R) Xeon(R) Processor
         E5-4600/2600/2400/1600/1400 Product Families HSBP to 1p3 .
- Fixed: Update for 1600W DC PSU FW.
- Fixed: Updated version number information for S2400BB and S2600GL/S2600GL
         platforms.
- Fixed: Changed Fan Speed sensing and control when SMB Alert assertion is
         detected (SmaRT event)
- Fixed: Seeing false watchdog events after a BMC update or reset.
- Fixed: BMC watchdog resets seen during network flooding.
- Fixed: Some logged POST Errors codes causing Embedded Web Server SEL viewer
         to stop displaying.
- Added: DCMI 1.5 spec compliance on EPSD Platforms Based on Intel(R) Xeon(R) 
         Processor E5-4600/2600/2400/1600/1400 Product Families
- Added: Enable Intel(R) Xeon(R) Phi(TM) Coprocessor adapters for
         W2600CR/S2600IP.
- Added: Added remote KVM watchdog.
         If there is an error on the remote KVM then wait one minute and then
         open a new KVM session.

===============================================================================
                                BMC 01.17.4151
===============================================================================
- Fixed: S4600LH: Updated to FRUSDR 19 package
- Fixed: S2600JF: Updated to FRUSDR 1.10 package
- Fixed: S2400SC: Updated to FRUSDR 1.08 package
- Fixed: S2400EP: Updated to FRUSDR 1.01 package
- Fixed: S1400FP: Updated to FRUSDR 1.01 package
- Fixed: S2600WP: Updated to FRUSDR 1.07 package
- Fixed: S2400BB: Updated to FRUSDR 1.02 package
- Fixed: S1600JP: Updated to FRUSDR 1.00 package
- Fixed: Fixed typo in uboot code for S1400FP
- Fixed: VFP power led always solid green while system into S1 state.
- Fixed: FW versions retrieved by IHC are incorrect.
- Fixed: PSU Config Error deassert event not in SEL after removal of incorrect
         power supply.
- Fixed: Fix a DIMM Thrm Mgn error in SEL while load BIOS EPSD default
- Fixed: Embedded Web Server SEL logs, added "OS Event" as the sensor name for
         events generated by 0x0041, to resolve incorrect sensor name & 
         type of SEL after Windows 2008 R2* 64bit graceful shutdown
- Fixed: Remove the option of selecting IPv6 address from LCP.
- Fixed: Some special characters show incorrectly on the LCP
         - Special characters will be shown as the nearest look alike
           available.
- Fixed: The last BIOS POST code on the LCD panel doesn't match with the
         boards POST CODE LED.
- Fixed: Failed to test PEF Bit for Get PEF Capabilities.
         - Was incorrectly identifying that Diagnostic Interrupt was available
           and OEM Action was not available.
- Fixed: LCP displays "No BIOS POST C" when enter into LPC under VIEW menu.
- Fixed: Connecting LCP to faulty system (system which keeps logging events)
         then LCP is unusable.
         - A small delay (half a sec) was added between the screen transitions
- Fixed: Multiple KVM socket error and media redirection errors
- Fixed: Embedded Web Server - JViewer "Error opening video socket" (Console
         Redirection Fails)
         - Various fixes for KVM and media redirection.
- Fixed: Web Console Remote Session check.
         - Do not allow web console to change remote session parameters while
           JViewer is running. Suspected of causing blank screens/Video Socket
           errors in JViewer.
- Fixed: BMC FW versions displayed by LCP are incorrect
- Fixed: SOL session started in SMASH session times out after 5 minutes
- Fixed: SSH SMASH session does not allow settings1/timeout value greater than
         600 seconds.
- Fixed: LCP Configuration LAN Subnet Mask shortened name incorrect.
- Fixed: VBAT voltage is low from BMC sensor reporting.
         - Vbat voltage was reporting low critical on some platforms.
- Fixed: PEF Postpone timer test failing
- Fixed: S4600LH: LCP displays incorrect Server Name
- Fixed: LCP: Active event is displayed incorrectly
         - Some event descriptions were confusing as they did not provide
           enough information.
- Fixed: LCP custom string not replacing the banner
         - Setting of a custom string should automatically become the LCP
           banner.
- Fixed: Embedded Web console not displaying sensor values for sensors from
         another controller
- Fixed: IPv6 is not supported on LCP, but the "Conf" screen showed an option
         to configure IPv6 address.
- Fixed: Update PSSF162202A firmware
         - bootloader changes
         - CRC 16 changes to fix firmware update failure issue.
         - Fix for READ_EIN and READ_PIN calculation
         - Fix includes Embedded Web Server reporting 0 W, double Power value
           workaround for ME issue.
- Fixed: Add auto detection, sensor, and Fan Speed Control support for Intel(R)
         Xeon(R) Phi(TM) Coprocessor adapters
- Fixed: Added additional product ID for Intel(R) Xeon(R) Phi(TM) Coprocessor
- Fixed: S4600LH: Change maximum link speed of RMM4 Dedicated NIC to 100Mbps
- Fixed: The current scrolling functionality of the LCP forcing the user to
-        wait till the scrolling of the existing text completes though the
-        user is not interested in reading the entire text.
- Fixed:Fix wrong slot number mapping for S2600GZ/S2600GL. Slot numbers were
        reversed.
- Fixed: 1200 W 02 F PSU FW file name was specified in hex instead of decimal.
         - Correcting the same to maintain consistency and for correct release
           notes generation.
- Fixed: S4600LH: LAN sku, doesn't have Power button.
         - BMC shouldn't support "stayoff" option in power restore policy.
         - Restore policy should be POWERON by default.
- Fixed: S2600JF and S2600WP: IO Mod Presence shows not present when SAS Module
         is present.
- Fixed: Power Unit Redundancy sensor did not behave as expected.
         - The Power Unit Redundancy sensor was not getting rearmed when AC/DC
           Input power was removed and then restored.
         - When interrupting input power from one of the redundant power
           supplies, the Status LED will blink green.
         - Restoring power to the power supply causes the Status LED to return
           to solid green and there is a SEL entry for Redundancy regained.
- Fixed: Scale CFM sensor reading by B value in SDR.
         - Platforms are using different scaling factors in the SDR for the
           system CFM sensor. This change reads the scaling factor from the SDR
           and adjusts the raw sensor reading accordingly.
- Fixed: When a Power Supply was inserted, the PS Redundancy sensor was not
         getting rearmed.
         - The PS Redundancy sensor is rearmed when a PS is inserted and full
           redundancy is regained.
         - When redundancy is regained, the LED should stop blinking and turn
           solid green.
         - There should also be a Redundancy Regained SEL event logged.
- Added: Disable POST codes LED output after system has completed POST


===============================================================================
                             BMC changes in    01.16.4010
===============================================================================
- Fixed: System power statistics shows N/A on EWS.
         - Power statistics were not available via Web interface when the PMBUS
           cable was connected.
- Fixed: Update power supply firmware for selected supplies to handle a PSON
         strobing issue which was causing problems on some systems.


===============================================================================
                               BMC changes in 01.16.3908
===============================================================================
- Fixed: S2600CO: Update SDR to version 1.09. 
- Fixed: W2600CR and S2600IP: Update SDR oto version 1.09. 
- Fixed: S2400GP: Update SDR to version 1.06. 
- Fixed: S2600GL/S2600GZ: Update SDR to version 1.05
- Fixed: S2400BB and S1400FP: Update SDR to current distro.
- Fixed: Corrects an issue where the BMC was generating incorrect SEL events.
         - The BMC will not generate SEL events for CPU presence when it starts
           up or after an SDR update, per requirement to exclude such events.
- Fixed: After enable lan failover, lan1 IPv6 address getting re-assigned by
         DHCPv6
- Fixed: RMM4 remote console port forwarding issue
         - Add support for handling network configurations with NAT/Port
           Forwarding between the browser and the BMC.
- Fixed: Embedded Web Server Sensor Readings are not correctly displayed after
         a SDR update and reset or a DC cycle.
         - Was requiring an AC power cycle or a BMC Cold Reset before the
           sensor were displayed correctly.

===============================================================================
                              BMC changes in  01.15.3885
===============================================================================
- Fixed: S4600LH: Added another Platform ID (S4600LH DP).
- Fixed: S2400LP: Added SAS module Temp to this platform.
- Fixed: S4600LH: Update to FRUSDR17.
- Fixed: S1600JP: Update FRUSDR from version 0.05 to version 0.07.
- Fixed: Added power-state fixes for the following conditions:
         - Chassis power-off when i2c connection to PCH fails, now supports
           4-second power button shutdown
         - Allows user to configure OEM PEF to perform graceful shutdown if
           they wish. Default remains immediate hard-shutdown.
- Fixed: Power Statistics displays 0w instead of Not Applicable on Embedded
         Web Server page with a Non PMBus power supply
- Fixed: Issue command of "Enter Firmware Transfer Mode" through RMCP(IOL)
         interface, the completion code is successful.
         - Firmware transfer mode commands are now disabled over
           IOL/RMCP/RMCPP and will fail with 0xD4.
- Fixed: When Onboard NIC 1 is disabled, it also disables the RMM NIC and
         should not

===============================================================================
                              BMC changes in  01.14.3855
===============================================================================
- Fixed: For S2600JF and S2600JF:
         1. Add sensor # 2D to monitor address 0x90 on i2c bus 2.
         2. Add sensor # 28 to monitor address 0x94 on i2c bus 2.
         3. Alter sensor monitor code for 240VA Fault.
- Fixed: Re-enable 1600W PSU and update FW to version 0.9.53 for S3F and 00A
         PSU Models
- Fixed: S4600LH: Updated from FRUSDR15 to FRUSDR16 package
- Fixed: Remove Intel branding from virtual front panel background image.
         - Since this image is outside of the scope of Embedded Web Server OEM
           updates, we have removed the Intel branding so that OEMs can rebrand
           everything with only the EWS OEM updates.
- Fixed: S2400EP: RGMII_IBMC_RMM4_TXD_0 and RGMII_IBMC_RMM4_TXD_1 failing
         ringback specification and is non-monotonic
- Fixed: The last 8 bytes of OEM data of SEL record retrieved by IHC are
         different from SELVIEWER or Embedded Web Server SEL.
- Fixed: SMI timeout will not be triggered when low for 2 minutes.
- Fixed: Local Control Panel: Reboot system twice, the boot option still boot
         to NetBoot.
         - Boot option configured by LCP config menu will no longer permanently
           change the selection. It will now be applicable only for the next
           boot.
- Fixed: After BMC or FRUSDR update, power unit redundancy lost asserted and
         deasserted event generated in SEL
- Fixed: Power unit redundancy has been lost -Asserted/Deasserted" events
         occurred after BMC reset via Cold Reset/Enter-Exit Firmware Transfer
         Mode commands.
- Fixed: S1600JP: Execute "Get CR Configuration" command with 450W mini-ERP PS
         gets unexpected response.
         - The 450W mini-ERP power supply used with S1600JP does not support
           Cold Redundancy. The Get/Set CR Configuration commands have been
           changed to return 0x81 for S1600JP.
- Fixed: Remove power supply will trigger a unexpected 03-A/C lost deasserted
         log in SEL.
- Fixed: Status LED is blinking green and 01-redund lost can not be recovered
         after removing any one 460W power supply and insert 750W power supply.
- Fixed: BMC Automatic Update of HSBP FW Unstable and Impacting BIK Factory
- Fixed: MTT sensor scaling is incorrect in all SDR files.
         - Corrected for S4600LH
- Fixed: Random Temp and Voltage events logged in SEL during factory SEL Check
- Fixed: IPMITOOL cannot get chassis ID LED status if we use web console to
         turn chassis ID LED on or off.
- Fixed: IPMItool identify LED with wrong status
- Fixed: IPMI to get chassis ID LED results is not same as "Manually press to
         light on Chassis identify LED"
         - The Chassis Identification fields of the Get Chassis Status response
           were not set properly for all methods of turning on the ID LED. This
           change adds the status to all methods of turning the ID LED On/Off.
- Fixed: IPMI Chassis Control Power Down incorrectly initiates a clean shutdown
         of OS
         - The Chassis Control command to power off the chassis was implemented
           with the Power Button press. This started a Graceful shutdown
           instead of an immediate one. This change causes the Chassis Control
           command for power down to immediately power down.

===============================================================================
                               BMC changes in 01.13.3724
===============================================================================
- Fixed: Updated S1400SP SDR to FRUSDR0.05 package
         - Changed SAS module address to 0x98
- Fixed: Updated S1400FP SDR to FRUSDR0.04 package
- Fixed: Updated S1600JP SDR to 0.07 package
         - Corrected the slave address for Full Height Full Length riser
           temperature device
         - Added new temperature sensors for new SAS module
- Fixed: Updated S2400BB SDR to FRUSDR1.00 package
- Fixed: Updated S2400GP SDR to FRUSDR1.05 package
- Fixed: Updated S2400LP SDR to FRUSDR1.08 package
- Fixed: Updated S2400SC SDR to FRUSDR1.05 package
- Fixed: Updated S2600IP SDR to FRUSDR1.08 package
- Fixed: Updated W2600CR SDR to FRUSDR1.08 package
- Fixed: Updated S4600LH SDR to FRUSDR0.15 package
         - Updated BB DDR Voltage SDR records
         - Added filtering logic
- Fixed: Added S4600LH baseboard FRU files for all the supported SKUs
         - S4600LH ROW with Intel(R) Ethernet Controller 10 Gigabit X540
         - S4600LH ROW with Intel(R) Ethernet Controller I350-AM4
         - S4600LH LAN with Intel(R) Ethernet Controller 10 Gigabit X540
- Fixed: S1600JP: Changed Mac0 Drive strength to conform to SI/EAs requirement

- Fixed: Green status LED keeps blinking after rearming the Power Unit
         Redundancy sensor.
         - When using manual rearmed sensor with deassertions disabled, status
           LED would not go back to green.
- Fixed: After issuing a turn off KVM services command, Launch Console button
         allows KVM to be launched, but KVM is not available, it will pop-up
         "Socket Error" message
- Fixed: In LCP, all the SEL entries are displaying in EVT MENU but it should
         not display informational events.
         - Only current active events in the system need to be displayed when
           the EVT menu item is selected for LCD.
- Fixed: Incorrect event "Redundancy regained " when PSU plugged in but no AC
         power applied.
- Fixed: BMC does not use a consistent IPv6 DUID

===============================================================================
                               BMC changes in 01.12.3663
===============================================================================
- Fixed: Updated S2400BB FRUSDR
- Fixed: Updated S4600LH to FRUSDR14 release
- Fixed: ADM1276 fails to respond after NACK.
         - Workaround developed and applied.
- Fixed: S2600CO customer SKU showing System Fan RPM 0.
- Fixed: S4600LH After CATERR the system halts instead of rebooting
- Fixed: S4600LH SMI timeout not triggered after 2 minutes
- Fixed: S4600LH Fan fault LEDs not working for system fan 7 to 11
- Fixed: Vlan help page of Embedded Web Server shows incorrect info.
         - Changed help page to align with functionality.
- Fixed: Typo errors found in Embedded Web Server
         -Virtual Front Panel help, IPv6 Network Setting Page, Alerts help
- Fixed: Onboard VGA cannot setup to highest resolution (1920x1080 up)
- Fixed: BMC FAN PWM freq reduced to 11KHz from 22KHz
         - Did not affect fan speed control functionality
- Fixed: S4600LH DIMM thermal trips on P3 and P4 being incorrectly reported
- Fixed: S4600LH Processor DIMM Thermal Margin sensor reading unavailable when
         in a 2 processor configuration
- Fixed: The description of NM Exception event is incorrect on Embedded Web
         Server.
- Fixed: With Intel(R) RAID Expander RES2SV240 connected, Drive "locate" action
         needs 10 to 30 seconds before the drive is blinking
- Added: Detect the node presence in chassis. Provide an OEM command to respond
         with data that indicates which nodes are populated in a multiple node
         system.

===============================================================================
                               BMC changes in release  01.10.3656
===============================================================================
-Fixed: NPD board I2C fails to respond after NACK no hold time case.


===============================================================================
                              BMC changes in  01.10.3560
===============================================================================
- Fixed: Updated FRUSDR files.
         - S2400BB to version 0.09
         - S2600CP to version 1.06
         - S2600CO to version 1.07
         - W2600CR to version 1.07
         - S2400EP to version 1.00
         - S2600IP to version 1.07
         - S2600JF to version 1.07
         - S2400LP to version 1.06
         - S2600CP to version 1.07
         - S2600CO to version 1.08
         - W2600CR/S2600IP to version 1.08
         - S2400GP to version 1.05
         - S1600JP to version 0.05
         - S2600JF to version 1.09 
         - S4600LH to version 0.12
         - S2600JP to version 1.05
         - S2600GZ/S2600GL to version 1.03
- Fixed: Adjust RGMII Tx clock delay to -250ps for S1400SP according to SI
         requirement
- Fixed: Command OEM Get Reading. will now return units-based value converted
         by using .y=Mx+B
- Fixed: Fixes to LCD Code defects identified in code review were incorporated
- Fixed: Some strings on LCD were formerly displayed improperly on LCD
- Fixed: Increased total SDR record length to 0x48h from 0x40h to accommodate
         the S4600LH SDR requirements
- Fixed: S1600JP: Corrects the baseboard temperature sensor mapping so that it
         works
- Fixed: After forcing a CATERR on S4600LH, the debug information from Embedded
         Web Server lacks some information
- Fixed: LAN channel cannot get DHCP IPv4 address after disabling VLAN on it
- Fixed: NMI sensor event isn't logged after issuing "chassis control" command
         to trigger NMI
- Fixed: SUT hang at POSTCODE: 0x63 while BMC LAN connected to a switch loop
         environment
         - BMC would freeze under heavy network traffic loads (e.g. broadcast
           storm)
- Fixed: S4600LH: Fan speed reading not correct
         - Added other chassis support in S4600LH and corrected RPM calc
         - Also updated S1400FP/S1400SP SDR to reflect change.
- Fixed: Network Interface hold time was out of spec for S2600GZ/S2600GL and
         S2400BB
- Fixed: Issuing incorrect "Set CR Configuration" command returns wrong error
         code
- Fixed: LCP error messages are not scrolling automatically without pressing
         LEFT and RIGHT keys
- Fixed: LCP default banner text when server with normal health is displaying
         some junk characters at the end
- Fixed: Number of characters displaying in LCP display is only 16 but it
         should be 18 characters
- Fixed: LCP displays "No BIOS POST C" when enter into LPC under VIEW menu
- Fixed: Unable to view the entire IP or Gateway or Subnet addresses using LCP
         display, last digit is missing during display.
- Fixed: Firmware information contents in LCP displaying does not match the
         actual version
- Fixed: Banner text is not reflecting correct information after selecting SM,
         LPC, or POW as a banner
- Fixed: LCP default screen after power on is not the correct banner text
- Fixed: S2400SC shows no socket present in CPU information page of Embedded
         Web Server
         - SMBIOS rev 2.7.1 added additional socket types. This change adds
           those types to the SMBIOS translation tables.
- Fixed: Updated S4600LH SDR to resolve issues where fans specified in FCT
         SDRs couldn't be controlled with fan domains.
- Fixed: BMC 1.08 S4600LH SDR was missing Sensor 0x2C (Riser 2 Left Forward
         Temperature)
- Fixed: Exit Air Temp reading mismatch when using IPMI command under Linux
         - The sensor initialization code was checking both assertion and 
           deassertion enables and settable/readable thresholds before actually
           setting the thresholds. This was causing the Exit Air Temp sensor to
           fail to set thresholds (all thresholds became 0)
- Fixed: Host name is not included in Email Alert subject line
         - Subject line could potentially be set before host name was set. This
           change sets the subject line again after the host name is changed
- Fixed: BMC FW must satisfy open source advertising clause for OpenSSL
         - Added "About" button to top bar to satisfy item 6 in the OpenSSL
           license.
- Added: Changed SDR of S2600CP, S2600CO, W2600CR/S2600IP, and S2400GP to add
         Dynamic Power Unit Redundancy Sensors
- Added: Add S1600JP and S2600JF PCIeSlotMap Table
- Added: Adds option (0xfe) for SlotIPMB command to ignore mux completely

===============================================================================
                              BMC changes in  01.09.3404
===============================================================================
- Fixed: Update FRUSDR packages to following versions:
         - S1600JP: S1600JP_FRUSDR_0.03
         - S1400SP: S1400SP_FRUSDR_01
         - S2400LP: S2400LP_FRUSDR_0105
         - S2400SC: S2400SC_FRUSDR_0104
         - S2400BB: S2400BB_FRUSDR_08
         - S2400EP: S2400EP_FRUSDR_03
         - S2600JP: S2600JP_FRUSDR_1.03
         - S1600JP: S1600JP_FRUSDR_0.04
         - S4600LH: S4600LH_FRUSDR_11
- Note: Testing with BIOS/2050_Package.zip (2.05 BIOS) with ME 02.01.05.091
        UBoot increments to 1.11 in this release due to changes in LCD
        handling
- Fixed: S2400EP: Add one additional 250ps delay for Tx clock and MAC0 drive
         strength to improve Signal Integrity on S2400EP
- Fixed: Fixed a case that had been missed for LDAP login to EWS.
- Fixed: uboot not updated after BMC FW updated when BMC executing from uboot
- Fixed: Wrong DIMM location is displayed in Embedded Web Server when a
         non-working DIMM is populated
- Fixed: Fixes to LCD module to address occcasional failures in Fan Speed
         Control tests.
- Fixed: LED control and status changes for S1400FP and S1400SP.
- Fixed: Updated the text output of ews-oem-tools to match documentation
- Fixed: Channel 1 or channel 2 LAN cannot ping through with IPV6 address when
         the LAN cables are both installed.
- Fixed: Corrected typoes in Embedded Web Server online help page.
- Fixed: S2400LP: After successful issue command to load BMC configuration
         default, "shutdown policy" option is not set to "disabled" which is
         the default
- Fixed: LCD SN [Server Name] displays different values at VIEW menu and SN as
         a banner
- Fixed: S2400BB: System Fans are constantly boosting and all sensors = OK

===============================================================================
                              BMC changes in  01.08.3329
===============================================================================
- Fixed: Updated S1600JP SDR to 0.03
- Fixed: Updated S1400SP GPIO table to improve Fan Tach reading.
- Fixed: BMC was sending PMBus command to non-supported CR feature PSU.
- Fixed: Update S4600LH SDR and associated zip to sync with latest FSC sheet
         Rev0.5,Version (v6)
- Fixed: Removing 1600 W S2 PSU FW image from the BMC.
- Fixed: S4600LH: Added debug to identify cause of system resets after CATERR.
- Fixed: IPv6 not working when 2 NCSI channels enabled or Failover is enabled:
- Fixed: There is an error message on Virtual Front Panel page when logging
         into the Embedded Web Server with user privilege.
- Fixed: Virtual Front Panel power LED always solid green when system is in s1
         state.
- Fixed: Event description different when viewed in Embedded Web Console vs.
         when saved via EWC.
         - Added decode of OEM event type 0x70, sensor type 0x2B events.
- Fixed: Embedded Web Server user disappears when  privilege is set to 5 using
         ipmitool.
- Fixed: BMC unresponsive when added all the users and then deleted all the
         users from Embedded Web Server
- Added: Added S1600JP to initial platform list
- Added: Add zlib license info to OEM Embedded Web Services documentation.
- Added: OEM Command to enable/disable BMC Services. This implements a command
         to enable/disable BMC Services and another to get current state.
         Currently controls sshd (SMASH), Web Console, and rKVM.

===============================================================================
                            BMC changes in    01.07.3244
===============================================================================
** NOTE: THERE IS A CHANGE TO THE PASSWORD SYSTEM USED BY SSH AND SMASH.
         - As a result SMASH users may be informed of a possible security
           attack, by the utility, when they first log in after updating.
           This is not an attack, it is an update which will take place once.

- Fixed: Updated S1400SP SDR, update SAS module presence sensor number to 0x2d
- Fixed: S2400BB - Default and FCT version 0.07 SDR files provided.
- Fixed: Update FRUSDR package (and defaults) for S4600LH to revision 08
- Fixed: Updated SDRs for S4600LH platform:
         - Modified and added SDR
         - Modified HSBP temp SDR threshold values
         - Corrected problem with S4600LH FRUSDR with Other chassis options
           that was causing system fan issues.
         - Some of the sensor numbers used were the same as other platforms,
           resulting in some erroneous displays of processor fan info. The
           Sensor numbers have been changed to avoid conflict
- Fixed: Adding S1400FP SDR. Updates S1400FP and S1400SP DIMM offsets in the
         web display, and also adds information on S1400FP Fan Fault LED.
- Fixed: BMC sshd password set to invalid by default
- Fixed: Additional support for SSL - spec requires that user can upload both
         certificate and private key, now supported
- Fixed: Update U-boot version to 1.8
- Fixed: BMC boot up had a window where BMC HW watchdog was not enabled.
         - Changed to 4 minutes so that if BMC fails to start, the hardware
           watchdog will trigger.
- Fixed: When the BMC reboots with an active SOL session, the SOL mux was not
         automatically reset to redirect serial data out the system serial
         port. This prevented both SOL and system serial from working. Now
         resets SOL mux at BMC boot to prevent this situation.
- Fixed: The PET Acknowledge command was requiring an open IPMI session. As per
         IPMI spec, this command will be sessionless and belongs to same class
         as Get Channel Authentication capabilities.
- Fixed: Enter Firmware Transfer Mode will generated a unexpected log about FW
         update status
- Fixed: When Exit FW transfer happens after the download of the image (i.e
         aborted before programming), the update failure sel event was not
         logged
- Fixed: HSBP unresponsive after FW update.
- Fixed: HSBP FRU information was sometimes unreadable via IPMITOOL.
- Fixed: Combined both debug files into a single zip. Passwords on individual
         files are unchanged. Container zip has no password. Modified system
         debug commands to only accept log type 0x00 as a parameter, since
         there is now only one file generated.
- Fixed: BMC disk drive numbering scheme does not match LSI tools (RWC2 and
         webBIOS) numbering scheme and marketing’s documentation
         - The BMC was using 1 based drive numbers, while documentation
           specified 0 based numbers. This change implements the changes for
           S2600GZ/S2600GL SDR as well as internaming conventions for the
           sensor numbers.
- Fixed: HSBP Drive Slot Sensors report drive removal and insertion on every
         warm reboot
- Fixed: GRUB serial terminal causes BMC distress
- Fixed: Get DIMM Offset command was rejecting any DIMM number greater than 48
         with completion code 0xCC.
- Added: "Get drive fault LED status" and "Set drive fault LED status" IPMI
         commands
- Added: All files required to support the add-in LCD hardware on S2600CP,
         S2600GL, and S2600GZ have been added.  User can now plug in module and
         traverse the LCD menus by pressing the buttons provided on the LCD
         hardware module.

===============================================================================
                           BMC changes in  01.06.3156 & 00.36.3156
===============================================================================
Note: The update package provided for this release was validated with BIOS
release x045.
- Fixed: Patch fixes a problem with excessive Power Supply SEL events for 1200W
         power supplies.
- Fixed: Update cipher suite LAN parameters to be consistent with IPMI spec
- Fixed: Update S2400LP SDR for factory build, FAN4a~6b was added
- Fixed: Changed Node Manager SEL entry descriptions.
- Fixed: Update for S2400LP to solve the FAN5a~6b reading zero issue reported
         by the factory.
- Fixed: Update S2400EP Default SDR
- Fixed: Add more thorough checking to Embedded Web Server action image
         validation
- Fixed: Update SDR on slave node, PSU temp sensors will be in Disabled status,
         while other PSU sensors are correct
- Fixed: A failed node can't be power-offed gracefully by BMC when there is a
         simulated critical event of a temp sensor and stopped ystem fan.
- Fixed: "Shutdown Policy" available after BIOS update
         - BMC returned the wrong completion code of 'get shutdown policy'
           command on non-halfwidth platform.
- Fixed: Allow OEM Embedded Web Server image to be completely removed to
         factory settings
- Fixed: SNMP alert and Email alert can't be received when node manager power
         policy defined threshold is exceededon S2400EP
- Fixed: The status LED will be solid amber for a while after an AC cycle on
         S2400EP, S1400FP, and S1400SP.
- Fixed: S2400LP DIMM event SEL does not match with the location in the board.
- Fixed: Sometimes the minimum power reading is 0W on the power statistics page
         - Fixed for all platforms.
- Fixed: Unexpected results with PS fault condition(FP Status LED, BMC Sensors)
- Fixed: Slow Fan Limit event verification failed on 1200W PSU
         - Failed Power Supply status was not being maintained. Will not clear
           the PS Fault status until the Power Good is negated.
- Fixed: Read platform debug command after exitng the debug log file transfer
         mode, the response is failed
- Fixed: BMC may hold IPMB CLK low after BMC reset if the BMC is addressed over
         IPMB and the BMC resets before that I2C transaction completes.
- Fixed: BB +1.1V STBY low critical log during DC off
         - The 1.1V Stby voltage sensor was generating events when the power
           button was held in over 4 sec.
- Fixed: Emulex* Pilot III P02 Chip - Prefetchable bit (BAR10-BIT3) is not set
         for memory range.
- Fixed: S4600LH: Add Memory Trip support for CPU 3 and CPU 4
- Fixed: S4600LH: Updated SDR version to 08.
- Fixed: S4600LH: Fixed the System Fans reading.
- Fixed: Incorporated generally released Linux driver fixes for bonding-related
         bugs, glitches, etc.
- Fixed: The cramfs tools used in Embedded Web Server image were licensed as
         GPL, these have been rewritten. In more paranoia was added in image
         creation, throwing errors if anything but regular files are in the
         source directory.  This prevents symlink and device node attacks.
         Also added is code to allow for building .deb, .rpm and .msi install
         packages. Currently the windows installer only does 32-bit, but the
         linux packages are available in both 32- and 64-bit varieties.
         Some of these changes are outlined in the updated user document that
         gets distributed with the binary.
- Fixed: Corrects a reaction to bad OEM records in SDR. Previously, this would
         report an error and reset the entire SDR with default values. This is
         not required, and the delete step will no longer happen.
- Fixed: Modified uboot handling of Enter FW Transfer Mode command to return
         completion code 0x80 (already in FW transfer mode) if the Enter FW
         Transfer Mode command has been sent previously.
- Fixed: 1200W power supplies were generating spurious Fan Failure events.
- Fixed: HSBP FW crash during firmware image updates.
- Fixed: PS temperature cannot be read after power cycling over night.
- Fixed: BMC boot up has a window where BMC HW watchdog is not enabled
         -BMC HW WDT was defaulted to trigger after 18 hours. This default
          timeout has been changed to 4 minutes.
- Added: Add a software-only method to replace public key and API to query key
         info

===============================================================================
                          BMC changes in      01.05.2974
===============================================================================
Note: The update package provided for this release was validated with BIOS
      release x045.
- Fixed: Update default SDR of S2600CO to version 1.04.
         Update default SDR of W2600CR/S2600IP to version 1.03.
         Update default SDR of S2400BB to version 0.06.
- Fixed: Updates PSU FW for 460W CRPS PSU to DPS-460KB A S3 3.09.29
         - This version contains a fix to set the SMBALERT interval to 30
           seconds.
- Fixed: Insert two DIMMs on channel A1 and A2, and inject an ECC error at A1,
         the event log will record correctable ECC at B1.
         - S2400GP: The channel number for DIMMS on channel A1 and A2 were
           being recorded incorrectly as being channel B1 when correctable ECC
           errors were injected.
- Fixed: Sometimes the minimum power reading is 0W on the Embedded Web Server
         power statistics page.
         - For S2400SC ME must receive a Reset NM Statistics command upon
           entering ACPI state S0 to get an accurate minimum power reading.
- Fixed: The Hex data of the sel event retrieved by Intel(R) Hybrid Cloud (IHC)
         is different from those in selviewer.
- Fixed: Execute Get DIMM info command to check Empty slot response "0x03"
         - Per EPS an empty DIMM slot should return 0x83 but was returning 0x03
- Fixed: Perform Action Button is disabled when Graceful OS shutdown option is
         used in Embedded Web Server
         - The Graceful OS Shutdown action caused the "Perform Action" button
           in the Embedded Web Server to be disabled during the process,
           however it wasn't re-enabled until the user reloaded the page.
           This change disables the button after any action, and re-enables the
           button after any power-control action completes.
- Fixed: Embedded Web Server Remote Control Page - Message is not consistent
         across all pages for a User with USER privilege.
         - Embedded Web Server Remote Control Page: Remote KVM is not available
           except to users with ADMIN or better privileges. The informational
           message was not consistent across all pages for a User connected
           with USER privilege. Logging into the EWS with a non-admin user, and
           attempting to open an Remote KVM window, will now redirect to a page
           explaining this. The help page has also been updated with this
           information.
- Fixed: KVM - Help Button - About "Jviewer" copyright statement is wrong.
           - The copyright date presented by JViewer in the Help->About
           interaction should now show copyright 2011 rather than 2005.
- Fixed: Embedded Web Console: Node Manager page hard shutdown does not seem to
         be a hard shutdown.
         - According to the Node Manager documentation, a hard shutdown is used
           but NM actually attempts a graceful shutdown first, only performing
           the hard shutdown if the graceful shutdown stalls for 30 seconds.
           The Embedded Web Server description and help page should correctly
           indicate that this is the expected behavior.
- Fixed: Get Chassis Status command identify LED with wrong status
         - The Get Chassis Status command was not returning the correct
           "Identification LED" status.
- Fixed: Fans stay boosted after BMC force update followed by SDR update
         - Fans should no longer boost after updating the SDR after a forced FW
           update.
- Fixed: Empty or Unconfigured HDD will continuously report faulty or
         assert/deassert
         - Fixes an issue where a system with ESRTII RAID 5, configured with
           three HDDs and a fourth installed but set either unconfigured or
           global-hot-spare, would generate numerous spurious drive fault
           errors to the System Event Log.
- Fixed: Firmware hang if BMC is crashed one time and BMC cold reset is
         executed 3 times after a crash within 30 minutes.
- Fixed: There is a typo error in BMC WebUI help document for "Alert Email"
         sub-menu
- Added: Adds new de-pop PBA (G49054-XXX) for S2600JF. Halfwidth projects will
         auto load de-pop SKU SDR when PBA# of FRU is G49054-XXX.

===============================================================================
                           BMC changes in     01.04.2963
===============================================================================
Note that this release is intended to fix a single issue for the S2400SC
platform. It was provided only for that platform.
- Fixed: On S2400SC, sometimes the minimum power reading is 0W on the Embedded
         Web Console power statistics page.

================================================================================
                   BMC Changes in release 1.04.2896
================================================================================

- Fixed: Update to PSU FW for 460W CRPS PSU - contains fix to set the SMBALERT
         interval to 30 seconds.
- Fixed: Empty or Unconfigured HDD will continuously report drive faults
         - There were many spurious drive fault SELs when ESRTII RAID5 was
           configured with 3 disks and 1 hotspare or an unconfigured disk.
           This change, with HSBP FRUSDR package 02, will correct the spurious
           SEL errors.
- Fixed: Firmware stuck if BMC is crashed and then a BMC cold reset is executed
         3 times within the next 30 minutes

===============================================================================
                         BMC changes in       01.04.2774
===============================================================================
- Fixed: Fixed issue where during reboot the BMC was not disabling the i2c-4
         channel, resulting in spurious SEL entries from the Management Engine.
- Fixed: New FW drop for the PMAX issue in PSU FW for 750W, 1200W S3/00
         revisions.
- Fixed: Additional FW drop for i2c timeout issue - 2nd timeout happening after
         a i2c reset for 750W, 1200W S3/00F
- Fixed: Fixed issue with bridging commands to ME via BMC IPMI.
- Fixed: Updates SDR for some boards to newest versions:
         - S2600JP IB/De-pop SKU to version 00.08
         - S2600JF IB/De-pop SKU to version 1.03
         - S2600CP to version 1.03
         - S2400GP to version 1.00
- Fixed: VCCQ VR temperature sensors were not working in S2400BB
- Fixed: Duplicated warning event logged about senor unavailable generated
         during ME update
         - Changed the BMC to not count update mode codes against the
           management subsystem health sensor.
- Fixed: Login through SMASH with LDAP authorized user and password failed
         - Enabled the use of LDAP authorization for SMASH logins to BMC. To
           use this there must be an LDAP server (not the BMC) which can
           authorize a user with a given password, and the BMC must be
           configured to allow LDAP with that server, and to map to an allowed
           set of functions.
- Fixed: IPv6 auto-configure mode not working 
- Fixed: Initialized Node Presence pins as Output-High for S2400LP, S2600JF,
         and S2600JP.
- Fixed: IPv6 ping failed after LAN failover enabled
- Fixed: When the Onboard NIC 1 is disabled in BIOS the system fans boost
- Fixed: RMS25CB080 SAS Mod Temp sensor has Unknown Health/Reading
- Fixed: ME events are not interpreted in Embedded Web Server SEL log
- Fixed: S2600JF PSOC HSBP temperature sensor intermittently unavailable during
         node hotplug
- Added: The BMC will now check the most significant bit (bit 7) of the PSU FW
         major revision number. If it is set to 1 then the BMC will refuse to
         downgrade the supply to any earlier revision.
         - Added since power supply stability issues can arise if power
           supplies are updated to an earlier revision of the power supply FW.
           This ONLY applies for this revision of BMC and later.

===============================================================================
                          BMC changes in      01.03.2674
===============================================================================
- Fixed: Update SDR of S2600CP to version 1.02.
- Fixed: Update SDR of W2600CR and S2600IP to version to 1.02.
- Fixed: Updated PSU FW for 1200W CRPS (S3 and 00 model) to correct the issue
         in S2600JF system, where system shuts down under certain conditions.
- Fixed: The description of a memory thermal trip event is incorrect.
         - For S2400SC and S2400LP, CPU1/2 DIMM channel 0 is not used. When
           DIMM thermal trip events are found on CPU1 they should show in the
           SEL as "CPU1, DIMMA", and when found on CPU2, as "CPU2, DIMMD"
- Fixed: It is hard to enter BIOS Setup via press F2 in KVM console when using
         LAN2.
- Fixed: An error dialog box pop-up was appearing when accessing the Alerts
         page on platforms that only support a single onboard shared NIC.
- Fixed: The fault reason is "Temperature has crossed critical value" on 
         Virtual Front Panel when SUT was powered off due to processor thermal
         trip.
         - Sensor severity for thermal trip was incorrect. It should now read
           "Thermal fault" on VFP when the system under test powers off due to
           processor thermal trip.
- Fixed: Dump debug file with non-redundant PSU, no information in PEC feature
         support status.
         - When installing a non-redundant PSU, an advisory is now added to the
           system debug log.
- Fixed: Alerts taking 10 seconds after an AC cycle.
- Fixed: On Half Width Form Factor platforms one Node reports raid rebuild that
         happened on another Node, these two Nodes share a HSBP.
- Fixed: Seeing excessive Frame Errors on RMM4 PHY when EEE (energy efficient
         ethernet) function was enabled.
         - When RMM4 PHY EEE (energy efficient ethernet) is enabled, receive
           frame errors increased to an unacceptable level. EEE has been 
           disabled.
- Fixed: Voltage 1.1V Standby monitoring for W2600CR, S2600IP, and S400GP not
         supported while in standby mode.
- Added: Node Auto-Shutdown behavior has been defined for multi-node systems
         (S2600JF, S2400LP, S2600JP). "BMC will turn off designated nodes in
         event of PS failure resulting in PSU not able to supply enough power
         and throttling the node. Based on BIOS setup and slot position of the
         board, BMC will forcefully shut down the node throttling due to PSU
         not supplying enough power."
         - With a properly configured system where nodes have a shutdown
           policy configured in BIOS to permit it, the last two nodes in the
           chassis can be shut down rather than running in a degraded state,
           allowing the remaining node(s) to work at full efficiency to
           complete tasks.

===============================================================================
                           BMC changes in     01.02.2608
===============================================================================
- Fixed: This build will be tested with the 041 BIOS release.
- Fixed: Updates to the zip-bundled FRUSDR packages are provided as follows:
         - S2600CP_FRUSDR_100.zip updated to S2600CP_FRUSDR_101.zip
         - S2600CO_FRUSDR_1.00.zip updated to S2600CO_FRUSDR_1.01.zip
         - S2600GZ_FRUSDR_08.zip updated to S2600GZ_FRUSDR_100.zip
         - S2600JF_FRUSDR_1.00.zip updated to S2600JF_FRUSDR_1.01.zip
         - S2400LP_FRUSDR_11.zip updated to S2400LP_FRUSDR_13.zip
         - S2400SC_FRUSDR_23.zip updated to S2400SC_FRUSDR_24.zip
         - S2600JP_FRUSDR_06.zip updated to S2600JP_FRUSDR_07.zip
         - Updated W2600CR and S2600IP SDR version to 1.01
- Fixed: The Chassis Intrusion flag is cleared when a Get Chassis Status
         command is processed.
         - The Get Chassis Status command now reads the state of the sensor
           rather than the value of the flag, when reporting chassis intrusion
           state.
- Fixed: Restores the Cipher Suites and features for RMCP+ which had been
         added then removed.
- Fixed: BMC NVRAM incorrect after DHCP configuration
- Fixed: Reduce RMM4 link speed on some platforms for EMI reductions.
         - On platforms S2600CP, S2600IP, W2600CR, S2600CO, S2400GP, S2400SC,
           and S1400FP, RMM4 Dedicated Management NIC should only connect at
           100MBps.
- Fixed: For S2600JF and S2600JP changed RGMII drive strength to correct EMI
         issues.
- Fixed: There is an error message on Virtual Front Panel page when logging
         into Embedded Web Server with user privilege.
          - When logging in with an account which only has the "user" privilege
            set, the "wait" status should not be displayed for the Virtual
            Front Panel.
- Fixed: The format of memory location error message in Embedded Web Server is
         different from SELviewer.
- Fixed: Update FW under EFI Shell using wrong package will cause a hang at
         "BMC Firmware Update Status".
         - If update fails it should now provide an advisory as expected.
- Fixed: S2400LP systems could experience an "NMI activated-system halted"
         error during system reset.
- Fixed: Embedded Web Server - "LOADING...PLEASE WAIT" is not displayed when
         clicking the refresh link.
         - There was text that was white on a white background. This is
         redundant, as the moving gif is visible, and an accepted form of
         loading indicator. This removes the invisible text.
- Fixed: When BMC is booting the on board Status LED is solid Green, the FP
         Status LED is off.
         - For S2600CO, when BMC is booting, the on board Status LED and FP
           status LED now follow the same blink and color status values as
           other platforms.
- Fixed: Static IPs are still retained when all the LAN 1 & LAN 3 IP set to
         DHCP
- Fixed: Reading more than 106 bytes from ID ROM caused an error if the IPMI
         requests was sent via RMCP
- Fixed: Alerts taking 10s after an AC cycle.
- Fixed: The last two SEL record datas retrieved by iHC are incorrect when the
         SEL is full.
- Fixed: Clear the SEL and issue Get all SEL Entries using wget in Linux, the
         response is incorrect.
- Fixed: Clear the events, there is no Hex version of "the log area has been
         cleared" when reading events using wget.
- Fixed: The last SEL record data retrieved by iHC was missing compared with
         the selviewer tool.
- Fixed: SEL/Power/FWver handlers are not giving error response for iHC
         negative testing.
- Fixed: Channel Access Disabling command not working correctly.
         - Channel Access flag was not checked before sending the PEF entry.
           This was causing some alerts to be lost.
- Fixed: Power Supply Sensors can get disabled on non-master half-width boards
         - Power Supply Sensors on Half Width boards could be disabled and not
           re-enabled.

===============================================================================
                          BMC changes in      01.01.2484
===============================================================================
- Fixed: S1600JP Porting code checked in
- Fixed: Added FRU id for external fan controller board detection.
- Fixed: Updated S2400EP Default.sdr and FCT.sdr according to 1.0 sys config
         table
- Fixed: Fixed ID LED issue broken by fix for chassis issue 
- Fixed: HSBP changes: for half-width backplanes, a complex formula decides
         which BMC will act as CMM for the chassis. Added new logic in CMC to
         monitor and grant the PSoC* ownership every 10 seconds. This should
         prevent deadlock issues.
- Fixed: Implemented FWupdate status sensor to log BMC build id (binary) and ME
         build id (bcd) plus decoding logic has been added in Embedded Web
         Server
- Fixed: Modified as per the latest S4600LH SGPIO table 
- Fixed: Updated FCT and Default SDRs as per the S4600LH latest FSC sheet
- Fixed: Updated S4600LH Default.sdr and FCT.sdr according to config table 1.0 
- Fixed: Modified the Bus number for external fan board FRU
- Fixed: Updated S2400SC Default.sdr and FCT.sdr
- Fixed: SDR S2600JF IB/Depop Factory SDRs are updated to V1.01
- Fixed: SDR Update Default/FCT.sdr of S2600CP to version 1.01.
- Fixed: SDR Update Default/FCT.sdr of S2600CO to version 1.01. 
- Fixed: SDR Update Default/FCT.sdr of W2600CR/S2600IP to version 1.01.
- Fixed: SDR Update S2600JP IB/Depop factory SDRs to V0.07
- Fixed: S2600KI BMC specific: SOL - last couple characters not echo'ed back,
         fixed
- Fixed: In Embedded Web Server cannot see the RMM4 LAN alerts setting when
         using IDA to set it.
         - Corrected the alert entry and destination selector configuration
           similar to IDA, so configuration by Embedded Web Server will be
           visible to IDA and vice versa.
- Fixed: W2600CR: IPMITOOL cannot activate SOL session, with console
         redirection enabled via serial port B
- Fixed: W2600CR: DPCCLI cannot be redirected to the serial B output with the
         console redirection enable on serial port B
         - W2600CR board doesn't have COM port COMA, SOL was failing because
           default port was COMA. Now checks for COMB as well.
- Fixed: Debug dump now contains BMC revision number.
- Fixed: Removed almost all BMC centric debug dump from the regular file. Also,
         removed memory info and processes info in the regular debug dump file.
- Fixed: No information about support PEC in debug file.
         - Add information about support PEC in debug file
- Fixed: Send IPMI command to Read Platform Debug Log file has response "C1"
         - Command to Read Platform Debug Log file was returning Normal
           Completion in a circumstance where it should have returned invalid
           command (C1)
- Fixed: Stop the PSU fan, system status LED blink green. after a while, it
         return to solid green, but the PSU FAN still remain stopped
         - Updates to PSU Firmware for 460W and 1200W 00 & S3F power supplies
- Fixed: The VR Watchdog Timeout sensor will auto re-arm within 1 second when
         system power good is deasserted and held deasserted
         - When the VR timeout event was asserted, the VR timeout flag was
           cleared. It resulted in a deassertion in the next sensor scan. Will
           not clear the flag until the VR power good# is asserted
- Fixed: S2400SC: When causing a CPU 2 fan failure ,the rear fan fault LED will
         turn to solid amber
         - CPU2 FAN fault LED and Rear FAN fault LED SGPIO number was swapped,
           resulting in incorrect LED lighting amber when one or the other
           failed
- Fixed: There are some failures in the VLAN ID  stress test .
         - VLAN config fixes:
           - VLAN ID was not always being read back correctly.
           - Fixed to return IPMI value for VLAN ID, not stale value 
           - Fixed VLAN Priority to work like all the other network parameters
           - Fixed IPv6 support
           - Fixed setting IPv6 to DHCP on web, which was erroneously returning
             IPMI Error 213
- Fixed: The Virtual Front Panel chassis ID LED blinking frequency is not
         synchronized with the front panel chassis ID LED
         - Virtual Front Panel was not reflecting chassis ID LED blink. It now
           detects and replicates this
- Fixed: There is a "BB +1.1V STBY low critical" event in SEL after AC cycling
         the SUT
         - 1.1V Standby voltage senor generating unwanted events when AC was
           removed with DC power on. Root caused to the 1.1V Stby voltage rail
           dropping very rapidly when AC is removed from a system that has DC
           power on. The BMC runs for a longer period so it saw the voltage
           drop out and generated events for it. Fix is to ignore voltage lower
           threshold crossings on this sensor if AC power is removed with DC
           power on.
- Fixed: Issue "Set CR Configuration" command with invalid value, the response
         isn't the correct error code
         - Was setting the user specific ranking. Ranking should be unique and
           less than number of working PS, should reject invalid numbers now.
- Fixed: S2600JP: MBE/DBE memory error did not sent SNMP and Email Alerts
- Fixed: Continuous Add SEL requests via KCS or IPMB leads to BMC auto-reset
- Fixed: Fwpiaupdt 11 Build 2: BMC update takes too long in all OS and EFI
- Fixed: Webserver sometimes shows socket error and does not respond till
         timeout when buttons pressed in quick succession
         - The refresh button at the bottom of the sensor reading page wasn't
           set to disable after a request, allowing for multiple rapid-fire
           requests with a very large overhead. The refresh button is now
           locked until the request completes, to prevent ASP floods on the
           sensor reading page.
- Fixed: RMM4 Ping Pong test failing with latest BMC 1.00
         - RMCP PING packets with non-0xff sequence were being dropped, but
           non-0xFF sequence numbers are allowed when the sender wants an ACK
           reply.
- Fixed: Update to BMC 1.0 with boot flag alone, doesn't reflect the boot area
         version
- Fixed: BMC Debug console constantly reporting "Invalid Logical GPIO: 197. Max
         is 161!" errors
- Fixed: S2600KI: DIMM Thermal Margin sensor readings should not be available
         in OLTT mode
- Fixed: Extended SEL severity code for Deassertions has non-informational
         severity
- Added: FRU IDs for PCI Risers 3 and 4 for S4600LH 
- Added: Initial FRUSDR release package for S4600LH
- Added: IO Module 2 support for S4600LH
- Added: IO Module 2 temp sensor support for S4600LH 
- Added: P3 and P4 related voltage sensors support for S4600LH
- Added: System fan1 and fan2 sensor numbers for S4600LH baseboard only support
- Added: BMC command implemented to read the ID and system fault LED

===============================================================================
                            BMC changes in    01.00.2612
===============================================================================
- First production release of BMC


=============================================================================
                           FRUSDR FEATURES ADDED
=============================================================================
S2600JF_FRUSDR_1.13:
- Add SDR 'PSU0 Status' and 'PSU1 Status'.

S2600JF_FRUSDR_1.12:
- Upgrade FRUSDR utility to Version11 Build20 

S2600JF_FRUSDR_1.11:
- Modify SDR 'IB QDR Temp' (Sensor#: 25h) to 'IB Temp'.
- Add 1600WDC PSU support.

S2600JF_FRUSDR_1.10:
- Install both 'IO Mod Presence' and  'SAS Mod Presence' in any case.
- DISPLAY "CPU1 is detected." in any case when Auto-detecting.

S2600JF_FRUSDR_1.09:
- Modify to probe IO Module FRU device instead of temperature device in master.cfg.
- Modify to set Other Chassis if GPU node power board is detected.
- Modify Sensor-reading-unavailable Control Value of 'LAN NIC Temp' (Sensor#: 2Fh) to 00h.
- Modify temperature points for "Curve Record".
- Add 'SAS Mod Temp 1' (Sensor#: 2Dh) and 'SAS Mod Temp 2' (Sensor#: 28h) 
  SDRs, Clamp records and Clamp sub-records.
- Modify SDR 'P1 MTT' and 'P2 MTT' M value to 05h, R exp value to Fh.
- Add 'SAS_MODULE' detection in master.cfg.
- Add SDR 'SAS Mod Presence' (Sensor#: 0Fh).
- Update FRUSDR UTILITY to Version 11.0 Build 14

S2600JF_FRUSDR_1.08:
- Modify HSBP FRU address in master.cfg to "AC" from "AE".
- Modify SDR 'Exit Air Temp' (Sensor#: 2Eh) Settable / Readable Threshold Masks
  to 0000h from 1B1Bh.
- Modify SDR 'Pwr Unit Redund' (Sensor#: 02h) Sensor Capabilities to 00h from 40h

S2600JF_FRUSDR_1.07:
- Update FRUSDR.efi to Build 11.
- Add FRUSDR loader version into ReleaseNote.txt
- Modify B value and threshold of SDR 'HSBP Temp'.
- Modify Global Stepwise Records.
- Modify SDR 'Powerville Temp' (Sensor#: 2Fh) to 'LAN NIC Temp'.

S2600JF_FRUSDR_1.06:
- Modify Global Stepwise Records for 3.5" and 2.5" HDD SKU.
- Modify SDR 'HDD 1 Status' (Sensor#: F0h) to 'HDD 0 Status'.
- Modify SDR 'HDD 2 Status' (Sensor#: F1h) to 'HDD 1 Status'.
- Modify SDR 'HDD 3 Status' (Sensor#: F2h) to 'HDD 2 Status'.
- Modify SDR 'HDD 4 Status' (Sensor#: F3h) to 'HDD 3 Status'.
- Update frusdr.efi to Version 11.0 Build 9.

S2600JF_FRUSDR_1.05:
- Modify the chassis name form to "Intel(R) Server Chassis - H2216/H2312"

S2600JF_FRUSDR_1.04:
- Modify the Entity ID of ¡¥HSBP Temp¡¦ (sensor# 0x21) to 0x40.
- Modify OEM System Airflow record for H2300JF/H2200JF.

S2600JF_FRUSDR_1.03:
- Modify Global Clamp Records for 74h and 2Eh.
- Modify OEM System Airflow record for H2200JF.
- Add SDRs for 1600W PSU.
- Add SDR, 'Auto Shutdown' (Sensor#: B8h).

S2600JF_FRUSDR_1.02:
- Add PBA Number G49052 for IB-QDR SKU.
- Add PBA Number G49053 for IB-FDR SKU.

S2600JF_FRUSDR_1.01:
- Modify 'System Airflow' (Sensor#: 11h) M value to 02h.
- Modify 'Exit Air Temp' (Sensor#: 2Eh) Normal Maximum to 4Bh.
- Modify DIMM Air Velocity Records for H2200JF.
- Modify Global Clamp/Stepwise Records.
- Modify OEM System Airflow record for H2300JF/H2200JF.
- Delete OEM DTS Look-up Table Records.
- Delete OEM DTS Parameter Records for H2300JF/H2200JF.
- Modify the "Stepwise sub-record" for H2300JF/H2200JF/Test Plate.
- Modify OEM Aggregate Sensor Configuration Record for H2300JF/H2200JF.
- Modify "Normal Control Value" for H2200JF.
- Change Fans-off PWM to 20% for H2200JF.

S2600JF_FRUSDR_1.00:
- Modify 'PS1 Temperature' (Sensor#: 5Ch) UC to 3Ch, UNC to 37h, Normal Reading to 19h, Normal Maximum to 32h.
- Modify 'PS2 Temperature' (Sensor#: 5Dh) UC to 3Ch, UNC to 37h, Normal Reading to 19h, Normal Maximum to 32h.
- Modify 'Exit Air Temp' (Sensor#: 2Eh) Assertion/Deassertion Event Mask to 0000h.
- Modify Temperature of Global Clamp Record for Clamp ID 74h, 75h, 24h, 23h, 5Ch, 5Dh.
- Modify Global Clamp/Stepwise Records.
- Change Fans-off PWM to 25% for H2300JF/H2200JF.
- Modify DIMM Air Velocity Records for H2300JF.
- Modify OEM System Airflow record for H2300JF/H2200JF.
- Modify "Domain configuration sub-record" to add 'Exit Air Temp' (Sensor#: 2Eh) in Sensor Exclusion for H2300JF/H2200JF.
- Modify "Clamp sub-record 1&2" for H2300JF/H2200JF/Test Plate/Other Chassis.
- Modify the "Stepwise sub-record" for H2300JF/H2200JF/Other Chassis.
- Modify Entity instance of SDRs.



=============================================================================
                           ISSUES FIXED
=============================================================================
S2600JF_FRUSDR_1.13:
- Add SDR 'PSU0 Status' and 'PSU1 Status'.

S2600JF_FRUSDR_1.12:
- Upgrade FRUSDR utility to Version11 Build20 

S2600JF_FRUSDR_1.11:
- Modify SDR 'IB QDR Temp' (Sensor#: 25h) to 'IB Temp'.
- Add 1600WDC PSU support.

S2600JF_FRUSDR_1.10:
- There is now "CPU 1 detected" indication string during the FRUSDR update processing

S2600JF_FRUSDR_1.06:
- None.

S2600JF_FRUSDR_1.03:
- : Can't get FRU data from 1600W PSU.

S2600JF_FRUSDR_1.02:
- : "No IB SKU is detected" will appear when flash frusdr.

S2600JF_FRUSDR_1.01:
- : Exit Air Temp (#0x2E) senser reading is abnormal.

S2600JF_FRUSDR_1.00:
- : Detect Temperture Exit Air Temp (#0x2E) Upper Non-Critical,Upper Critical event when plugged all nodes in chassis.
- : Status LED will amber blinking when system power on before BIOS post screen.

S2600JF_FRUSDR_19:
- : Some BIOS Memory Sensors are missing either in SDR repository or in BIOS EPS

S2600JF_FRUSDR_17:
- : No memory throttling sensor to indicate memory throttling status

S2600JF_FRUSDR_16:
- : Very hard to enter to other chassis based on current auto detection process
- : DIMM sensor FSC clamp configuration causing unexpected 100% fan boost
- : SDR record rejected by BMC
- : Incorrect Advanced Fan Failure sub-record in SDR

FJP_15:
- : BB 1_2V IB OTHER' reading value is incorrect.

FJP_13:
- : "BB P1 Vcc" and "BB P2 Vcc" Sensor generated in SEL log
  during OS installation and boot in OS.(W2K8R2SP1, RHEL6.1)
- : No log for "LAN Leash Lost" event

FJP_12:
- [EWS] "PWr Unti Redund" sensor is always show "Warning".

FJP_11:
- None.

FJP_10:

-modified "IBMC WATCHDOG" to "IntegratedBMCWDT"

FJP_09:
- FRUSDR 06 fan low critical & lower non-critical threshhold setting mismatch.
- no logs related to DIMM Thermal Trip in the SEL when generated DIMM Thermal Trip.
FJP_08:
- FSC not work in S2600JF, all fan full run
- Physical Security (Chassis Intrusion),Physical Scrty (#0x04) report in S2600JF system.



FJP_07:
- None.


FJP_06:
- None.

FJP_05:
- : Has not¡§Expected Detected Chassis¡¨ can choose  when update FRUSDR.
- : Has not¡§Other Chassis¡¨ can choose  when update FRUSDR.

FJP_04:
- : PSU redundant is not supported but we still have Pwr Unit Redund sensor.
- : FP NMI is not supported but we still have FP NMI Diag Int sensor.
- : Cannot read sensor value of HSBP temp.

FJP_02:
- : Detect MEM voltage sensor 0xE4 to 0xE7 SEL log when system execute Power on, reset and power off.
- : Detect MEM voltage sensor "IB other 0xEF" SEL log when system execute Power on, reset and power  off.

FJP_01:
- None.



=============================================================================
                            LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products. 
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation may 
have patents or pending patent applications, trademarks, copyrights, or other 
intellectual property rights that relate to the presented subject matter.  
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any 
such patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product 
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 
*Other names and brands are the property of their respective owners.
Copyright (c) 2012 Intel Corporation.

A portion of this firmware is open source code, which falls under the
GPL 2.0 license.  

[END OF RELEASE NOTES]
