=============================================================================
    Intel(R) Server Platform S2600JF FRU/SDR Update Release Notes
=============================================================================

INTEL Product Collaboration and Systems Division
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA

=============================================================================

DATE:  February 18, 2014

TO:     Intel(R) Server Platform S2600JF customers

SUBJECT:    IBMC(R) FRU/SDR update package S2600JF_FRUSDR_1.13 release notes

=============================================================================
                               LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products.
No license, express or implied, by estoppel or otherwise, to any intellectual
property rights is granted by this document. Except as provided in Intel's
Terms and Conditions of Sale for such products, Intel assumes no liability
whatsoever, and Intel disclaims any express or implied warranty, relating to
sale and/or use of Intel products including liability or warranties relating
to fitness for a particular purpose, merchantability, or infringement of any
patent, copyright or other intellectual property right. Intel Corporation may
have patents or pending patent applications, trademarks, copyrights, or other
intellectual property rights that relate to the presented subject matter.
The furnishing of documents and other materials and information does not
provide any license, express or implied, by estoppel or otherwise, to any
such patents, trademarks, copyrights, or other intellectual property rights.
Intel products are not intended for use in medical, life saving, or life
sustaining applications. Intel may make changes to specifications and product
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation.

*Other names and brands are the property of their respective owners.

Copyright (c) 2010 - 2013 Intel Corporation.

=============================================================================
                              ABOUT THIS RELEASE
=============================================================================

SDR file version: 1.13
Baseboard FRU file version: 0.01
Master configuration file version: 1.13
FRUSDR loader version: 11.0 Build 20

=============================================================================
        SYSTEM HARDWARE & SOFTWARE REQUIREMENTS/REVISIONS
=============================================================================

- This FRU/SDR package has only been tested on S2600JF FAB1 baseboards.

- BMC firmware rev 00.01 (or later) MUST be preinstalled prior to installing
  this FRU/SDR package.

- BIOS R0025 or later

=============================================================================
                      IMPORTANT INSTALLATION NOTES
=============================================================================

- None

=============================================================================
            INSTALLATION PROCEDURE
=============================================================================

1. Ensure BMC release 00.01 or later is pre-installed before attempting this
   FRU/SDR update.

2. Copy all of the files in the S2600JF_FRUSDR_1.13.zip archive to a USB key,
   hard disk drive or floppy drive.
   All of the files in this zip archive must reside in the same directory.

3. Boot to EFI and then run the following command to display the
   contents of the baseboard FRU device:

    FRUSDR /d FRU

   If device is empty(which is the case for all new FAB1 baseboards) or corrupted, then
   execute the following command to program the empty FRU device:

   For S2600JF:
        FRUSDR /fru S2600JF.fru

4. Now execute the following command to bring up the main FRU/SDR load menu:

    FRUSDR /cfg master.cfg


5. Select the option which is applicable to what you want to do. On a brand
   new baseboard I would highly recommend to run option 3 to program both
   the FRU and SDR. By reprogramming the FRU you will be given the option
   to input data from the keyboard into various chassis, board and product
   areas. Ensure that you select the correct chassis from the chassis
   selection menu otherwise your fan sensors will not be configured
   properly.

6. Once the package has finished its installation, I would highly recommend
   to DC power off the system and cycle AC power.

=============================================================================
                           KNOWN ISSUES/WORKAROUNDS
=============================================================================
S2600JF_FRUSDR_1.00:
- Known issue: The first time to update FRU will fail. Please use another method 
  to update FRU the first time you update FRU. Frusdr.efi /fru S2600JF.fru.
 
=============================================================================
                           FEATURES ADDED
=============================================================================
S2600JF_FRUSDR_1.13:
- Add SDR 'PSU0 Status' and 'PSU1 Status'.

S2600JF_FRUSDR_1.12:
- Upgrade FRUSDR utility to Version11 Build20 

S2600JF_FRUSDR_1.11:
- Modify SDR 'IB QDR Temp' (Sensor#: 25h) to 'IB Temp'.
- Add 1600WDC PSU support.

S2600JF_FRUSDR_1.10:
- Install both 'IO Mod Presence' and  'SAS Mod Presence' in any case.
- DISPLAY "CPU1 is detected." in any case when Auto-detecting.

S2600JF_FRUSDR_1.09:
- Modify to probe IO Module FRU device instead of temperature device in master.cfg.
- Modify to set Other Chassis if GPU node power board is detected.
- Modify Sensor-reading-unavailable Control Value of 'LAN NIC Temp' (Sensor#: 2Fh) to 00h.
- Modify temperature points for "Curve Record".
- Add 'SAS Mod Temp 1' (Sensor#: 2Dh) and 'SAS Mod Temp 2' (Sensor#: 28h) 
  SDRs, Clamp records and Clamp sub-records.
- Modify SDR 'P1 MTT' and 'P2 MTT' M value to 05h, R exp value to Fh.
- Add 'SAS_MODULE' detection in master.cfg.
- Add SDR 'SAS Mod Presence' (Sensor#: 0Fh).
- Update FRUSDR UTILITY to Version 11.0 Build 14

S2600JF_FRUSDR_1.08:
- Modify HSBP FRU address in master.cfg to "AC" from "AE".
- Modify SDR 'Exit Air Temp' (Sensor#: 2Eh) Settable / Readable Threshold Masks
  to 0000h from 1B1Bh.
- Modify SDR 'Pwr Unit Redund' (Sensor#: 02h) Sensor Capabilities to 00h from 40h

S2600JF_FRUSDR_1.07:
- Update FRUSDR.efi to Build 11.
- Add FRUSDR loader version into ReleaseNote.txt
- Modify B value and threshold of SDR 'HSBP Temp'.
- Modify Global Stepwise Records.
- Modify SDR 'Powerville Temp' (Sensor#: 2Fh) to 'LAN NIC Temp'.

S2600JF_FRUSDR_1.06:
- Modify Global Stepwise Records for 3.5" and 2.5" HDD SKU.
- Modify SDR 'HDD 1 Status' (Sensor#: F0h) to 'HDD 0 Status'.
- Modify SDR 'HDD 2 Status' (Sensor#: F1h) to 'HDD 1 Status'.
- Modify SDR 'HDD 3 Status' (Sensor#: F2h) to 'HDD 2 Status'.
- Modify SDR 'HDD 4 Status' (Sensor#: F3h) to 'HDD 3 Status'.
- Update frusdr.efi to Version 11.0 Build 9.

S2600JF_FRUSDR_1.05:
- Modify the chassis name form to "Intel(R) Server Chassis - H2216/H2312"

S2600JF_FRUSDR_1.04:
- Modify the Entity ID of ¡¥HSBP Temp¡¦ (sensor# 0x21) to 0x40.
- Modify OEM System Airflow record for H2300JF/H2200JF.

S2600JF_FRUSDR_1.03:
- Modify Global Clamp Records for 74h and 2Eh.
- Modify OEM System Airflow record for H2200JF.
- Add SDRs for 1600W PSU.
- Add SDR, 'Auto Shutdown' (Sensor#: B8h).

S2600JF_FRUSDR_1.02:
- Add PBA Number G49052 for IB-QDR SKU.
- Add PBA Number G49053 for IB-FDR SKU.

S2600JF_FRUSDR_1.01:
- Modify 'System Airflow' (Sensor#: 11h) M value to 02h.
- Modify 'Exit Air Temp' (Sensor#: 2Eh) Normal Maximum to 4Bh.
- Modify DIMM Air Velocity Records for H2200JF.
- Modify Global Clamp/Stepwise Records.
- Modify OEM System Airflow record for H2300JF/H2200JF.
- Delete OEM DTS Look-up Table Records.
- Delete OEM DTS Parameter Records for H2300JF/H2200JF.
- Modify the "Stepwise sub-record" for H2300JF/H2200JF/Test Plate.
- Modify OEM Aggregate Sensor Configuration Record for H2300JF/H2200JF.
- Modify "Normal Control Value" for H2200JF.
- Change Fans-off PWM to 20% for H2200JF.

S2600JF_FRUSDR_1.00:
- Modify 'PS1 Temperature' (Sensor#: 5Ch) UC to 3Ch, UNC to 37h, Normal Reading to 19h, Normal Maximum to 32h.
- Modify 'PS2 Temperature' (Sensor#: 5Dh) UC to 3Ch, UNC to 37h, Normal Reading to 19h, Normal Maximum to 32h.
- Modify 'Exit Air Temp' (Sensor#: 2Eh) Assertion/Deassertion Event Mask to 0000h.
- Modify Temperature of Global Clamp Record for Clamp ID 74h, 75h, 24h, 23h, 5Ch, 5Dh.
- Modify Global Clamp/Stepwise Records.
- Change Fans-off PWM to 25% for H2300JF/H2200JF.
- Modify DIMM Air Velocity Records for H2300JF.
- Modify OEM System Airflow record for H2300JF/H2200JF.
- Modify "Domain configuration sub-record" to add 'Exit Air Temp' (Sensor#: 2Eh) in Sensor Exclusion for H2300JF/H2200JF.
- Modify "Clamp sub-record 1&2" for H2300JF/H2200JF/Test Plate/Other Chassis.
- Modify the "Stepwise sub-record" for H2300JF/H2200JF/Other Chassis.
- Modify Entity instance of SDRs.

=============================================================================
                             REFERENCE MATERIAL
=============================================================================
S2600JF FSC Config Sheet Rev 2.6.xlsm datasheet
HWFF EP chassis Auto-detection V02.vsd
CONFIG-BIOS SDRs Rev 0_53_Bromley.xlsx
[END OF RELEASE NOTES]