This release note and the software that accompanies it are copyright (c) 2015, Intel Corporation or its suppliers, and may only be installed and used in accordance with the license that accompanies the software.

This Software is furnished under license and may only be used or copied in accordance with the terms of that license. No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. The Software is subject to change without notice, and should not be construed as a commitment by Intel Corporation or its suppliers to market, license, sell or support any product or technology. Unless otherwise provided for in the license under which this Software is provided, the Software is provided AS IS, with no warranties of any kind, express or implied. Except as expressly permitted by the Software license, neither Intel Corporation nor its suppliers assumes any responsibility or liability for any errors or inaccuracies that may appear herein. Except as expressly permitted by the Software license, no part of the Software may be reproduced, stored in a retrieval system, transmitted in any form, or distributed by any means without the express written consent of Intel Corporation.

==========================
Supported RAID Controllers
==========================
This download supports Intel(R) RAID controllers using MegaRAID SAS software stack (RS3SC008, RS3DC080), please verify that this utility has been tested with the RAID card you have chosen to use by checking the drivers web page for your controller at http://www.intel.com/support/.

===================
Package Information
===================
Flash package = v26.2.0-0025

==========
Attention!
==========
Intel recommends to loading Factory Default setting after the firmware upgrade which will not affect data on any existing array. 
To do so:
1. Reboot the system and login to the RAID BIOS Console. 
2. Select the controller and select 'Adapter Properties'->'Next'
3. Set the 'Set Factory Defaults' setting to 'Yes' and submit the change.
4. Reboot the system (the default settings are applied).
5. Re-configure to the desired settings in RAID Web Console2.

==================
Known Restrictions
==================
This download does NOT support EFI v1.1 environment. Please use the EFI shell commander which will display the EFI version, to identify the EFI version.

1. Firmware update needs to be performed on one node at a time. When a node is performing firmware update, the firmware updates on the other node is blocked until the firmware update process on the first node is completed. 
2. While not in cluster (Single node), shutdown of the node is treated as a planned failover. Hence resuming of background operations behaviour would be same after the reboot in the same way as a failover.
3. When a node is not part of the cluster (Single node) is rebooted, if it had a hotspare as part of the configuration, then on reboot all the drives that are part of any LD before the reboot are marked foreign and the configuration would be imported through enhanced foreign import. (No user impact, but only a behavioural difference compared to MR 6.x in single node)
4. User needs to select OFU while updating the firmware so that after the firmware flash.
(In Syncro if IOs are allowed after FW update (that has cache layout change) then on reboot when the new FW takes over the controller does not come up. This is because with new local IOs (though they are in WT) and mirror IOs we still mark cache dirty. This dirty cache cannot be recovered after reboot when the new FW takes over.)
5. User cannot create Blocked VDs. If user tries to create blocked VD, operation will be rejected with generic message of operation not supported. 
6. SCGCQ00722176: When the dirty lines are present, the auto foreign import will fail. The pinned cache needs to be cleared or the user has to import the foreign configuration. This is the limitation from base MR and needs an ER to handle this. 
7. If more than 32 FDE drives are used for creating secure VDs, failover may fail for few VDs. Hence a maximum of 32 FDE drives are recommended for creating secure configurations. 
8. Auto Enhanced Import feature is enabled by default and cannot be disable by user.
9. SCGCQ00665571   : Suspend Copy back/Rebuild is resumed automatically on FO
10. SCGCQ00413571 (PR) Cannot update physical drive (PD) or enclosure/ESM firmware with an active HA cluster.
Workaround: Shutdown one node for the duration of the PD/ESM firmware update process. Once the update has been completed, the previously shutdown node may be returned to an operational state.
11.SCGCQ00497037  Both SAS cables pulled from one node while IOs running in Linux caused all IOs to stop after LDs failed over to peer node
Workaround: Restart IO from client (surviving peer node will service IO)
12.SCGCQ00496951  Hit IO stop on SQLStress test when pulling out power cord on each node 
Workaround: See IO stop solution steps in Table 4 of Section 5.4 of the Syncro CS Solution User Guide 
13. SCGCQ00555272: Clear config from one node does not clear GHSP in Peer node where GHSP is the only config that the peer has.
14. SCGCQ00529668: Multi bit ECC error injection from megaon is not supported and would result in drives becoming foreign.
15. Recommendation is to perform configuration changes like Create/Delete of VDs on one node at a time.


=======================
Contents on the package 
=======================
The following files are included in this zip:

Name:						Description:
COPYING.NEWLIB.txt				License Agreement
3108-HADAS_FWPKG-v26.2.0-0025_readme.txt	This file
3108s22.rom					Firmware binary
License_v2.pdf					License Agreement
update.nsh					UEFI firmware update batch file
StorCLI\*					StorCLI command line utilities (See the StorCLI release notes file for details regarding StorCLI)



==========================
Installation instructions:
==========================
Note: Flashing non-Syncro firmware images on Syncro controllers can impact HA functionality.

UEFI shell instructions for updating RAID Firmware:
-----------------
   1. Download and extract all files to a USB flash drive.
   2. Boot the target system to EFI shell. 
   3. Change directory to the local drive and directory containing the flash update files and the firmware image file.
   4. Type "update.nsh" and press <Enter> to execute the command
   5. Wait for the flash to complete. Do NOT reboot the system during the update.

You can also use RAID Web Console 2 or OS version of StorCLI to update the RAID firmware.  For more detail, please refer to the Intel(R) RAID Software User's Guide.


====================
Product Limitations: 
====================
1.SATA drives are not supported 
2.SAS drives which do not support SCSI-3 persistent reservation are not supported
3.Dimmer Switch functionality is not supported 
4.SGPIO sideband signal for enclosure management is not supported 
5.Cachecade functionality is not supported
6.System/JBOD mode PDs are not supported
7.Drives that are direct-attached to the controller (not via expander device) is not supported
8.Cluster-Active Reconstruction operations (RAID Level Migration or Online Capacity Expansion) is not supported (SCGCQ00320755)
9.Patrol Read operations that are in progress do not resume after failover (SCGCQ00468449)
10.BBU is not supported
11.Firmware-level node incompatibility details are not reported for non-premium features (SCGCQ00504637)
12. Maintain PD Fail History feature is not supported.
13. CME recovery is not supported for IO shipped commands. IO shipped commands will be failed on hitting CME (SCGCQ00697526).
14. Rebooting both nodes with only GHS configured (SCGCQ00712021).

===================
Third Party Issues:
===================
1. SCGCQ00423092: (#41756) HAMR: I/O's fail during failover when cables are pulled on enclosure.
   Microsoft case:113122611052586
2. SCGCQ00465589: TC 45049:  I/O stop after trigger OCR( debugOcr reset 0 0 )  while rebuild are in progress . 
   Microsoft case: 113122611052604
3. SCGCQ00503608: Creating cluster with non-shared and shared LDs, some shared LDs in failed state in the Cluster Manager.
4. SCGCQ00595355: Non-shared VD is pulled into OS (Windows) cluster during cluster creation
   (Please refer to Microsoft KB article: http://support.microsoft.com/kb/2813005)
5. Install Microsoft hot fix in case of delayed Write Failed" error when an I/O stress test runs against a Windows Server 2012 failover cluster from a Windows 8-based or Windows Server 2012-based client .
http://support.microsoft.com/kb/2842111
6. SCGCQ00619231: Seagate ST200FM0053 12G SSD will be shown as direct attached drive even its connected to enclosure.
7. SCGCQ00676113: Remote IO Failure observed in SLES11SP2 while removing the sas cables of the owner node.
 Workaround:  Restart IO from client



Bug Fixes and Enhancements:
===========================
Firmware Package: 26.2.0-0025 (Syncro 2.2)

Firmware 4.320.00-4272
  Bug Fixes:
	SCGCQ00564435 - (Closed) - Unable to install OS after putting the peer into Maintenance Mode
	SCGCQ00568555 - (Closed) - Firmware faulted when the controller got reset during Enclosure firmware update
	SCGCQ00660280 - (Closed) - MonTask when importing many LDs
	SCGCQ00682854 - (Closed) - All drives became foreign on peer when failover happened
	SCGCQ00688743 - (Closed) - During expander firmware download, the peer controller resets when the expander goes missing
	SCGCQ00701909 - (Closed) - Assertion failure in mptrec.c at line 2606 while running DevBST
	SCGCQ00702899 - (Closed) - Enable more target pause debug
	SCGCQ00703741 - (Closed) - Intermitent DC with rebuild when running heavy stress and resets
	SCGCQ00741765 - (Closed) - IntBST test case hits MonTask: line 2033 in file ../../cluster/rmangler.c
	SCGCQ00749724 - (Closed) - If one of the controller goes into maintenance mode while IOs running, LDs that are failed over to the peer become access blocked.
	SCGCQ00751527 - (Closed) - Configuration is cleared after rebooting system with multiple sliced arrays configured
	SCGCQ00765344 - (Closed) - System will not boot to OS when second attempt to put the controller into maintenance mode
	SCGCQ00765375 - (Closed) - Add boot message prints to improve debug
	SCGCQ00767677 - (Closed) - Global hot spare becomes foreign unconfigured good drive after a controller reset
	SCGCQ00771184 - (Closed) - Firmware fault during reboot after entering maintenance mode
	SCGCQ00776301 - (Closed) - Global hot spare disappears during reboot
	SCGCQ00776782 - (Closed) - For cache mirror commands transport the initiator cmdId to the target side for additional debug information
	SCGCQ00776796 - (Closed) - Target ID 63 can be incorrectly included in a pinned cache discard
	SCGCQ00781055 - (Closed) - Kill Adapter may occur with Debug Queue logging enabled
	SCGCQ00783057 - (Closed) - Data integrity test failed to verify the data after a reboot with pinned cache and an imported config
	SCGCQ00783141 - (Closed) - Task Mangement Timer is deleted in completion path(not in Task time)
	SCGCQ00787473 - (Closed) - OS crashed while running IOs and Rebuilding
	SCGCQ00800437 - (Closed) - Data Corruption encountered due to a kill adapter with repeated shutdown commands from storcli
	SCGCQ00804009 - (Closed) - Make sure PL timer is called every 250 milliseconds while processing Task List
	SCGCQ00805663 - (Closed) - MonTask @ line 2386 in file ../../cluster/peertarget.c while initiating the OCR through App.
	SCGCQ00807138 - (Closed) - IO stopped with "C0:DM_PL_MsgGetNum(00001000) : Invalid Ptr" in node-1 for multipath break/connect with shipped FP IOs
	SCGCQ00809634 - (Closed) - Enabling Cache Bypass Debug
	SCGCQ00810175 - (Closed) - Peer controller degraded VD's PDs(online) are rebuilding with degraded VDs on peer controller UPFO(power-off node2)
	SCGCQ00816112 - (Closed) - line 3183 in file ../../dm/mpt2/mptrec.c for enclosure reboots with PRL11 with sequential Large IOs.
	SCGCQ00837871 - (Closed) - *** DATA TLB ERROR(SRR0/1,ESR) exception: sf=c03fff50 for IO shipping by toggling paths in multipath environment
	SCGCQ00574067 - (Closed) - Fix compilation errors
	SCGCQ00597735 - (Closed) - Fix double spacing in ld.h
	SCGCQ00612686 - (Closed) - StorCLI return failure to enter maintenance mode even thought firmware enter into maintenance mode
	SCGCQ00660431 - (Closed) - Firmware incorrectly reports preserved cache during boot time
	SCGCQ00677738 - (Closed) - IO stop with when controller gets reset.
	SCGCQ00688725 - (Closed) - Problem transitioning between SSHA subtopologies
	SCGCQ00705393 - (Closed) - Kill adapter after enclosure firmware download completes with IO
	SCGCQ00715674 - (Reworked) - IOs will stop when user enters maintenance mode on one controller
	SCGCQ00726636 - (Closed) - Enable checked asserts
	SCGCQ00729590 - (Closed) - All VDs show up on only one of the controllers when SSHA setup is moved from one to another
	SCGCQ00741967 - (Closed) - Firmware never completes DISM when attempting peer arbitration white peer is not present
	SCGCQ00767253 - (Closed) - A peer target reset can cause an Unplanned Failover
	SCGCQ00767330 - (Closed) - Rebuild progress starts at 0% after a system reboot
	SCGCQ00768726 - (Closed) - Timeout in waiting for peer signal to boot due to delayed DDF update completion on the peer
	SCGCQ00769483 - (Closed) - IO drops on an LD while migrating from R1 to R6
	SCGCQ00771888 - (Closed) - Preserved Cache boot message when the controller does not have preserved cache
	SCGCQ00772352 - (Closed) - Physical Drives do not get discovered in one of the node after first powercycle of the enclosure.
	SCGCQ00775129 - (Closed) - Allow preempt and reserve without arbitration for special cases.
	SCGCQ00776777 - (Closed) - False missing VDs message can be generated
	SCGCQ00776779 - (Closed) - Improve pinned cache debug
	SCGCQ00783564 - (Closed) - Kill adapter seen while doing a RAID Level Migration
	SCGCQ00787179 - (Closed) - Data corruption found while running a script to enter and exit maintenance mode repeatedly.
	SCGCQ00791491 - (Closed) - A controller reset with a high VD count can cause the peer controller to crash
	SCGCQ00795413 - (Closed) - line 670 in file ../../ddf/ddfPd.c for trying to configure more GHS hotspares using available disks.
	SCGCQ00797728 - (Closed) - Before we do task list processing every time, we make sure PL is given a context to run.
	SCGCQ00797788 - (Closed) - enabling DQ
	SCGCQ00800749 - (Closed) - Assertion failure in ../../ddf/ddfPd.c at line 670 for running multipath cable break script with 64 Logical disks & IO.
	SCGCQ00802390 - (Closed) - Montask occurs when deleting a rebuilding LD with an emergency hot spare
	SCGCQ00803575 - (Closed) - line 1127 in file ../../dm/mpt2/mptDirect.c for offlining 64 R0 LDs with shipped 100%seq,writes.
	SCGCQ00804525 - (Closed) - LD creation may cause MSM to hang
	SCGCQ00804820 - (Closed) - Multiple Disks observing in the Disk management of the non-owning node, instead of 2 disks it is showing 190 disk
	SCGCQ00818599 - (Closed) - FW hits to montask at line 4440 in file ../../raid/pd.c on rebooting the setup during rebuild
	SCGCQ00564197 - (Closed) - Pinned cache occurs when entering maintenance mode while IO's are running to write back cache enabled VD's
	SCGCQ00573513 - (Closed) - When SAS cables are moved from first setup to second, then volumes are not seen on second setup.
	SCGCQ00594259 - (Closed) - Remove topology debug prints
	SCGCQ00644477 - (Closed) - Fix FindDev.c merge errors
	SCGCQ00686617 - (Closed) - MonTask: line 260 in file ../../raid/1078int.c during firmware initialization
	SCGCQ00715577 - (Closed) - Peer arbitration is not getting granted during device initialization when peer is not found.
	SCGCQ00731664 - (Closed) - Patrol Read structure that is completely zero'd incorrectly loaded instead of reinitialized
	SCGCQ00752190 - (Closed) - Enable cache mirroring debug until Beta
	SCGCQ00766085 - (Closed) - With IO and a RAID level migration the adapter faults
	SCGCQ00768574 - (Closed) - Fixed Stack Corruption caused by storing more data in a buffer than it had allocated space as a local variable
	SCGCQ00770856 - (Closed) - Perform an unplanned failover when the node doing ESM update crashes
	SCGCQ00781588 - (Closed) - Target reset are retried even if there is no outstanding IOS on target device
	SCGCQ00781752 - (Closed) - Controller was not discovered the Unconfigured Good drives on setting back to normal maintenance mode
	SCGCQ00783718 - (Closed) - Disable crashing the peer when a node is crashed for test/debug
	SCGCQ00784327 - (Resolved) - ASSERT - line908 in file././dm/devMgr.c in Node1
	SCGCQ00786032 - (Closed) - Data integrity test fails after pinned cache is recovered.
	SCGCQ00786042 - (Closed) - Firmware faults while doing foreign import
	SCGCQ00787452 - (Closed) - Controller lost volumes during reboot
	SCGCQ00795341 - (Closed) - FW hits to montask at line 7088 in file ../../raid/cache.c on powering-off the redundant enclosure while running IOs
	SCGCQ00797766 - (Closed) - fixing compilation errors after merging phase6 PL
	SCGCQ00803772 - (Closed) - Increased the number of error interrupt processing from 1 to 10
	SCGCQ00806270 - (Closed) - PDs failed to discover at node1 and HA domain lost while running enclosures powercycle with import in loop
	SCGCQ00807491 - (Closed) - System hangs at BIOS with offline VDs
	SCGCQ00809839 - (Closed) - MonTask @line 3362 in file ../../dm/mpt2/mptrec while removing a cable from controller to enclsoure
	SCGCQ00813036 - (Closed) - line 7898 in file ../../raid/cache.c for rebooting with pinned cache and offline Logical disks.
	SCGCQ00817070 - (Closed) - MonTask: line 203 in file ../../cluster/peerIo.c while running IOs update enclosure Firmware
	SCGCQ00824946 - (Closed) - MonTask: line 2283 in file ../../raid/cacheMirror.c
	SCGCQ00574011 - (Closed) - Fix continuation characters in makefile
	SCGCQ00574063 - (Closed) - Fix compiler errors and warnings
	SCGCQ00598883 - (Closed) - Update files with new Peer Arbitration parameters
	SCGCQ00622835 - (Closed) - "FW could not sync up config/prop changes for some of the VDs" message intermittently after a failover
	SCGCQ00658879 - (Closed) - Drives become foreign unconfigured bad on one controller when rebooting both controllers at the same time.
	SCGCQ00679197 - (Closed) - When importing a configuration, the firmware faulted
	SCGCQ00695557 - (Closed) - Not able to boot back to OS after finish OS installation
	SCGCQ00706113 - (Closed) - MonTask: line 1266 in file ../../raid/1078dma.c when powering on/off enclosure.
	SCGCQ00766279 - (Closed) - Assert immediately on other core when one core asserts
	SCGCQ00768320 - (Resolved) - Foreign config auto import did not import any drives error message in POST during reboot
	SCGCQ00769258 - (Closed) - Rename function for coding clarity
	SCGCQ00772690 - (Reworked) - Junk character at POST when reboot with missing VD "The following VDs are missing: ä©-Àà©-ÀÀ©-ÀÐ15À"
	SCGCQ00775677 - (Closed) - intBST-MonTask: line 548 in file ../../raid/cmd.c.
	SCGCQ00776175 - (Closed) - intBST-line 1439 in file ../../raid/cache.c. for running cluster Validation.
	SCGCQ00777869 - (Closed) - Data integrity test failed to verify the data after a reboot with pinned cache and an imported config
	SCGCQ00779496 - (Closed) - Load balancing does not occur correctly after foreign import when pinned cache is present
	SCGCQ00781553 - (Closed) - While rebuild is in progress, a kill adapter occurs after resetting the controller
	SCGCQ00796402 - (Closed) - line 627 in file ../../dm/mpt2/mptIniTM.cl for single path removal of the controller with 100% heavy sequential IOs.
	SCGCQ00804675 - (Closed) - Handling the error cases(DISM error case and a rmgr request fire) of a FAILED drives!
	SCGCQ00816223 - (Closed) - INSTRUCTION TLB ERROR(SRR0/1) exception: sf=c03fff50 for Toggling WT<--->AWB with Shipped sequential IOs.
	SCGCQ00817051 - (Closed) - "DM_IsAnyRemovalPending: flags 1a0008a devId 0 devH fff"continueous event for multiple split brains.
	SCGCQ00818679 - (Closed) - One node entering safe mode everytime we reboot our setup
	SCGCQ00818979 - (Closed) - line 1543 in file ../../dm/pl2/pliopi.c for rebuild,copyback by enclosure reboots with R0,R1,R5,R6.R00,R10,R50,R60.
	SCGCQ00823679 - (Closed) - intBST-Montask @ line 1543 in file ../../dm/pl2/pliopi.c.
	SCGCQ00827636 - (Closed) - Montask at line 202 in file ../../cluster/peerIo.c while running enclosures powercycle import and IO on VDs
	SCGCQ00503016 - (Closed) - Fix the way the function "if all drives inserted to RAID layer or not present" is implemented.
	SCGCQ00569118 - (Closed) - Lock Peer node devices when an enclosure firmware update is underway
	SCGCQ00571721 - (Closed) - FW does not auto change topology from MEC to SSC after moving controller from SSHA to SSC
	SCGCQ00658893 - (Closed) - When direct connect cable is removed the controller will reset
	SCGCQ00675278 - (Closed) - Applications do not correctly report EnableConfigAutoBalance values
	SCGCQ00734443 - (Closed) - Cable pull caused fatal FW error in dmDrvPrep.c
	SCGCQ00738585 - (Closed) - Server hang at POST and not able to boot to OS unless Cn on both node
	SCGCQ00741982 - (Reworked) - Applications see auto load balancing as disabled even though it is enabled in the firmware
	SCGCQ00747285 - (Closed) - Add preferred owner debug prints
	SCGCQ00749597 - (Closed) - Use topology setter functions when appropriate
	SCGCQ00749690 - (Closed) - When one of the controller enters maintenance mode, firmware hits a montask in config.c
	SCGCQ00759161 - (Closed) - LSA displays 'Invalid Sequence number' while creating a Volume in Syncro setup.
	SCGCQ00771277 - (Closed) - Occasionally VDs on one controller are lost during reboot. All PD members become UNCONFIGURED_GOOD.
	SCGCQ00777107 - (Closed) - MonTask: line 208 in file ../../raid/sentinellock.c in Node1 instead of booting into safe mode with FW mismatch of HSM
	SCGCQ00779201 - (Closed) - External defect to work on D30806
	SCGCQ00780766 - (Closed) - Discovery is not completed,config lost,Pinned cache got generated for cable removals to make HA to Inactive <->Active
	SCGCQ00805177 - (Closed) - Enable Ring Buffer by default until Beta
	SCGCQ00821340 - (Closed) - Optimized CM command using stale dmIoCtx for mirror line validation
	SCGCQ00822386 - (Closed) - Montask at line 2274 in file ../../raid/cacheMirror.c while running redundant enclosure powercycle with IOs
	SCGCQ00842937 - (Closed) - DC hits on one of the R1 VD while running weekend IO after rebuild operation
	SCGCQ00574065 - (Closed) - Fix compile errors
	SCGCQ00680508 - (Closed) - An error is signaled if the peer is not connected to the storage while executing expander firmware download.
	SCGCQ00698176 - (Closed) - Firmware hit a kill adapter when one controller is reset
	SCGCQ00700810 - (Closed) - Compiler warning
	SCGCQ00713912 - (Closed) - Kill adapter when flashing enclosure firmware while the peer controller is in Maintenance mode
	SCGCQ00721363 - (Closed) - Rebooting after OS installation causes OS to fail to boot
	SCGCQ00726702 - (Closed) - FW still stay in maintenance mode instead of safe mode after reconstruction and reboot server
	SCGCQ00776618 - (Closed) - intBST-Montask @ 5520 in file ../../ddf/ddfConfig.c
	SCGCQ00778821 - (Closed) - Junk character at POST when reboot with missing VD.
	SCGCQ00786094 - (Closed) - Firmware faults while entering maintenance mode after an enclosure firmware update
	SCGCQ00795042 - (Closed) - FW hits to montask at line 1517 in file ../../dm/pl2/pliopi.c on removing and inserting back the drives while FPIOs
	SCGCQ00795057 - (Closed) - To fix the compilation issues after rebasing to the latest fw_sas_mega_api files
	SCGCQ00799375 - (Closed) - FW hits to montask at line 1809 in file ../../cluster/peertarget.c on powering-off the enclosures while LargeSeqWrites
	SCGCQ00800241 - (Closed) - line 129 in file ../../raid/reglockhw.c for reboots for OS install on both the nodes with LDs present.
	SCGCQ00804561 - (Closed) - Command loss while processing completions
	SCGCQ00806558 - (Closed) - Data corruption reported when calling the shutdown code repeatedly
	SCGCQ00813121 - (Closed) - Firmware crash@line 1002 in file ../../dm/src/dm.c while injecting media error on DIF drives
	SCGCQ00816520 - (Closed) - halted Peer Discovery on peer and cache sync aborted reason 8a for <4 s pull/push
	SCGCQ00833317 - (Closed) - Disable PL debug and tty during discovery
	SCGCQ00529668 - (Closed) - VDs lost and PDs become foreign after triggering Multibit ECC error
	SCGCQ00555271 - (Closed) - Controller with out Syncro license is not entering safe mode
	SCGCQ00574061 - (Closed) - Merge cleanup
	SCGCQ00671381 - (Closed) - Found Fatal firmware error: Line 5675 in ../../bbu/onfi.c after flash new release FW
	SCGCQ00673403 - (Closed) - Firmware crashed after rebooting machine from another crash
	SCGCQ00674284 - (Closed) - Invalid memory reference when pull cable between 2 controllers with IO running
	SCGCQ00680762 - (Closed) - Firmware on the peer node faults during enclosure firmware is updated
	SCGCQ00688305 - (Closed) - Code review changes
	SCGCQ00767248 - (Closed) - Clarify boot message termination
	SCGCQ00769734 - (Closed) - Firmware Crash @line 260 in file ../../raid/1078int.c after flashing the Firmware
	SCGCQ00790681 - (Closed) - MonTask@ line 284 in file ../../inc/cacheVersion.h while making multiple PD offline
	SCGCQ00791231 - (Closed) - KillAdapter is seen in both Nodes during reboot after setting enableLDDBM 1 via firmware trace with 4K PD's inserted.
	SCGCQ00795055 - (Closed) - MonTask: line 1990 in file ../../raid/cache.c Reboot config owning node when shipped IOs running
	SCGCQ00795140 - (Closed) - line 910 in file ../../raid/raidscsi.c for creating pinned cache on 64 R0 Logical disks by enclosure off.
	SCGCQ00803388 - (Closed) - Disable CM DQ by default
	SCGCQ00813600 - (Closed) - Assertion failure in ../../cluster/peertarget.c at line 2394 for rebooting with offline,Degraded LDs.
	SCGCQ00817988 - (Closed) - fixing compilation error
	SCGCQ00819043 - (Closed) - Assertion failure in ../../dm/src/devmgr.c at line 5107 while flashing corrupted binary to enclosure
	SCGCQ00823161 - (Closed) - FW hits montask at line 967 in file dm/src/devmgr.c while running enclosures powercycle with import and shippedIOs
	SCGCQ00824760 - (Closed) - Firmware breaks @ line 260 in file ../../raid/1078int.c for flashing the firmware with IO running from peer node
	SCGCQ00574062 - (Closed) - SSHA Merge Compiler Warnings/Errors Fix
	SCGCQ00574066 - (Closed) - SSHA Merge Compiler Warnings/Errors Fix
	SCGCQ00660415 - (Closed) - Device initialization state machine does not complete when VDs are configured across two enclosures and enclosure is power cycled
	SCGCQ00713617 - (Closed) - VDs are lost and preserved cache is present when peer is reset
	SCGCQ00729581 - (Closed) - Enable PLDEBUG
	SCGCQ00736854 - (Closed) - Certain systems are not able to boot with firmware 3647
	SCGCQ00759477 - (Closed) - Enable Discovery prints until Beta
	SCGCQ00780770 - (Closed) - Killadapter- line1266 in file././raid/1078dma.c in Node1 after flashing firmware & rebooting nodes with 64VD's present.
	SCGCQ00791260 - (Closed) - MonTask: line 2643 in file ../../cluster/rmangler.c reboot the node when copyback and rebuid is running on same DG
	SCGCQ00793760 - (Closed) - FW hits to montask at line 939 in file ../../dm/src/devmgr.c in node2 & node1 line 3044 in file ../../dm/mpt2/mptrec.c
	SCGCQ00794114 - (Closed) - Kill adapter due to a SES command when pull/push pds for rebuild.
	SCGCQ00796456 - (Closed) - observing continues prints while doing cable pull "iopiSCSIIOCompleteError: FPESTATUS_DEVHANDLE_OUT_OF_RANGE mid x017b
	SCGCQ00803390 - (Closed) - line 1002 in file ../../dm/src/dm.c for for single path removal of the controller with 100% heavy sequential IOs.
	SCGCQ00803480 - (Closed) - FW hits to montask at 7859 in file ../../raid/cache.c on importing VDs with pinned cache where Shipped IOs running
	SCGCQ00818682 - (Closed) - One of the node gets hung if both the nodes are rebooted with one node with OFFLINE LDs.
	SCGCQ00827835 - (Closed) - Configured PDs dropped from the R6 & R60 VDs from the enclosure while power-cycling the other redundant enclosure
  EnhancementRequests 
	SCGCQ00570284 - (Closed) - Copy new files
	SCGCQ00571425 - (Closed) - Merge SSHA raid related files into 2.0
	SCGCQ00571710 - (Closed) - 1078main.c
	SCGCQ00668708 - (Closed) - Add UNIT ATTENTION support
	SCGCQ00802712 - (Closed) - VD goes to Blocked stated on importing the VDs after enclosure powercycle
	SCGCQ00571371 - (Closed) - log.c and raidpci.c
	SCGCQ00571405 - (Closed) - SSHA to 2.0 port
	SCGCQ00571717 - (Closed) - dm.c and Balance.c
	SCGCQ00651360 - (Implemented) - 4K, DIF and SED indicators in logging
	SCGCQ00767267 - (Closed) - Disable debug functionality
	SCGCQ00773718 - (Closed) - Enable cache bypass for better performance with large writes on WB volumes
	SCGCQ00774031 - (Implemented) - GHS enhancements
	SCGCQ00571421 - (Closed) - Merge SSHA inc related files into 2.0
	SCGCQ00571666 - (Closed) - Expander DM and MISM
	SCGCQ00577416 - (Closed) - Remove topology debug injection functions
	SCGCQ00756633 - (Implemented) - Handling of erroneous drives during DISM/failover and slow failover
	SCGCQ00768433 - (Implemented) - Recommendation is to perform configuration changes like Create/Delete of VDs on one node at a time
	SCGCQ00571555 - (Closed) - Misc files
	SCGCQ00572475 - (Closed) - ddf.c and ddfForeign.c
	SCGCQ00603079 - (Closed) - Misc code review enhancements
	SCGCQ00710134 - (Implemented) - VD Failover not happening while doing a node reboot with the pinned cache present
	SCGCQ00571414 - (Closed) - Merge SSHA changes for firmware download into SSHA 2.0
	SCGCQ00572465 - (Closed) - devMgr.c and FindDev.c
	SCGCQ00690196 - (Closed) - Preventive action when premium feature is not enabled for the topology that the controllers are connected in.
	SCGCQ00692435 - (Closed) - Do not post LD deleted events during Mini Failover
	SCGCQ00797147 - (Implemented) - Improve performance for I/O shipped large sequential writes on WB volumes
	SCGCQ00571638 - (Closed) - SSHA to 2.0 port
	SCGCQ00573421 - (Closed) - Add Premium Feature support via electronic licensing for Syncro solutions
	SCGCQ00764625 - (Implemented) - allocate dedicated RDMs for each PD to avoid waiting for RDMs.
	SCGCQ00793398 - (Closed) - Enhancement request to utilize the full cache when the peer is not present or the cache mirror is not enabled
	SCGCQ00571373 - (Closed) - DDF Related Files
	SCGCQ00695239 - (Closed) - While recovering from a split brain scenario, Peer Discovery fails if a conflicting target ID is detected.
BIOS 6.24.05.0
	SCGCQ00769239 - (Closed) - Don't issue REAID I/O on the 4K JBOD
	SCGCQ00720411 - (Closed) - Not able to boot to OS from the VD whose target ID is greater than 128
	SCGCQ00659974 - (Closed) - OpROM - If there is boot message, BIOS won't detect > 64 VDs
	SCGCQ00629987 - (Closed) - With more than 64 VD's in the configuration, number of Virtual Drives handled by BIOS message is not shown in the POST.
	SCGCQ00626821 - (Closed) - In Post Restrict to 64 VD only
	SCGCQ00808137 - (Closed) - Line between "VDs handling" prints to be removed to match with "JBODs handling" prints
	SCGCQ00808086 - (Closed) - Exposes "SecureJBOD" to system BIOS when 'Ask password at boot' entered wrongly
	SCGCQ00783579 - (Closed) - INT13 drive type is not set correctly for physical disk
	SCGCQ00653048 - (Closed) - AutoSelectBootLd is not working if user has OS in VD > 64
	SCGCQ00826174 - (Closed) - 64VDs found on Host adapter eventhough more than 64 VDs are present
	SCGCQ00799339 - (Closed) - Legacy OpROM doesn't show proper PCI slot number on Intel WCP system.
	SCGCQ00798656 - (Closed) - Handle new changes of BBU doc related to Battery Status
	SCGCQ00769269 - (Closed) - Before calling Translate_LdTargetIdList_To_LdList set int13 drive type
	SCGCQ00455591 - (Closed) - Memory access issue for Mercury when loading Ctrl R
	SCGCQ00682646 - (Closed) - Display the first 64 VDs in the POST (in the same sequence we get it from FW)
	SCGCQ00632011 - (Closed) - Firmware enters faults state after a reboot on flashing firmware with IO in progress.
	SCGCQ00579962 - (Closed) - Initialize deviceExposure with MAX_INT13DISKS instead of 0xFF
	SCGCQ00693494 - (Closed) - setting deviceExposure greater than or eaual to 128 will show wrong VD handled by bios
	SCGCQ00809682 - (Closed) - Shows expander as JBOD in POST
	SCGCQ00787941 - (Closed) - Update Attribution Language - Copyright, Trademark, Confidentiality to Avago
	SCGCQ00626602 - (Implemented) - VT-d/IOMMU support for iMR - Implement mechanism to allow system BIOS to put entries for iMR mem allocation into proper table
	SCGCQ00621895 - (Closed) - WebBIOS of MR card hangs due to bios control mis-direct in Wildcat EVT boards
	SCGCQ00572939 - (Closed) - Make sure all the make file adheres to the latest binary names.
	SCGCQ00613355 - (Implemented) - Add the logic to handle the Boot message till the controller state remains boot message pending
	SCGCQ00550426 - (Closed) - Increase OpROM code size from 40k to 48k
	SCGCQ00593245 - (Closed) - SSHA boot support
	SCGCQ00559095 - (Closed) - Provide an option to limit the max number of INT 13h devices presented to system BIOS
	SCGCQ00455597 - (Closed) - Memory allocation: Allocate only two 64k
	SCGCQ00795550 - (Closed) - Address BBU/Supercap inconsistent Behavior across HSW apps.
	SCGCQ00550388 - (Closed) - Write Caching HBA, JBOD/R0 supported TB controller with 240 SystemPD/LD support
CTRL-R/CTRL-H 5.09-0700
	SCGCQ00806497 - (Closed) - CtrlR shows different size against same CCVD
	SCGCQ00759987 - (Closed) - AWB option support with CCVD should not be there.
	SCGCQ00720815 - (Closed) - <prev> and <next> links in Properties Page both redirects to next page and vice versa.
	SCGCQ00693498 - (Closed) - Shared VDs are shown in setting boot VD options
	SCGCQ00625148 - (Closed) - in-appropriate drive state is seen on connecting back the drives in ctrl-r .
	SCGCQ00568586 - (Closed) - help file for emergency spare displays wrong
	SCGCQ00485184 - (Closed) - Change Emergency Spare to NONE with enable enmergency on Smarter checked will fail with error=03
	SCGCQ00811247 - (Closed) - Exception in Core0 DATA TLB ERROR(SRR0/1,ESR) during VD creation with mix of 512n and SSD 512e PD's in Ctrl-R.
	SCGCQ00798966 - (Closed) - Ther term "Security Key" is not consistently used across the tool.
	SCGCQ00798807 - (Closed) - Battery Management - Learn Mode improvements
	SCGCQ00764750 - (Closed) - Not able to see Advanced Software Option (ASO) in Virtual Drive Management
	SCGCQ00764187 - (Closed) - Ctrl-R: Not able to set the Boot Device and other controller propertie
	SCGCQ00738006 - (Closed) - Incorrectness in the popup for Virtual drive Expansion
	SCGCQ00704259 - (Closed) - Firmware Hangs/breaks while creation of RAID1 with GHS
	SCGCQ00690731 - (Closed) - Showing incorrect reason for change in Write Policy in presence of Pinned Cache
	SCGCQ00673165 - (Closed) - Spelling mistake and unexpected comma in Ctr-R properties page
	SCGCQ00635638 - (Closed) - spelling issue in help file of VD Size.
	SCGCQ00560490 - (Closed) - Ctrl-R is not showing the Syncro option in ASO
	SCGCQ00484509 - (Closed) - VD properties dialog the VD operation box is coming out of the dialog space
	SCGCQ00809681 - (Closed) - CtrlR masking/does not show foreign secure JBOD in case if user enter 'Ask password at boot' 3 times wrongly
	SCGCQ00785679 - (Closed) - Controllers are not sorted according to BDF(bus device funtion) in CTRL-R.
	SCGCQ00777828 - (Closed) - CTRL-R reports CCVD deleted even though its still under deletion process by FW
	SCGCQ00760989 - (Closed) - FW hits monTask, When CTRL-R is launched immediately after the MR Controller initialization is complete and before the iMR card initialization starts in the BIOS POST.
	SCGCQ00710520 - (Closed) - Incorrectness in Help file generated by pressing F1
	SCGCQ00707450 - (Closed) - While creating cachecade vd with one SAS-SSD;Raid 1 option is also enabled
	SCGCQ00677460 - (Closed) - Montask on joining the mirror arm as new virtual drive when doing with the second array.
	SCGCQ00648182 - (Closed) - Port informations are not displayed in Connector field for the drives attached to antares card.
	SCGCQ00644056 - (Closed) - Join mirror is not enabled in CTRL-R for OEM PNP ID's.
	SCGCQ00642546 - (Closed) - Help is missing for break and join mirror feature in Control-H
	SCGCQ00628684 - (Closed) - enclosure connected in multi-path is not showing all ports
	SCGCQ00593822 - (Closed) - Both the Connector information(0-3 & 4-7) is not shown in PD properties while connected in Multipath
	SCGCQ00584993 - (Closed) - unable to diplay the reason for difference in write policy
	SCGCQ00568182 - (Closed) - showing wrong page number in properties page
	SCGCQ00765643 - (Closed) - Ctrl+R not handling VD policy change error case for Autoconfigured Virtual Drives
	SCGCQ00756487 - (Closed) - Incorrectness in the popupmenu generated for the controller info when controller is in Safe Mode
	SCGCQ00730497 - (Closed) - ctrl-r gives the option to set -head of queue for raid 0
	SCGCQ00678600 - (Closed) - Gramatical Error in Ctrl-R while modifying SuperCap properties
	SCGCQ00615350 - (Closed) - In multicontroller environment unable to enter into ctrl-R after 1st controller initililization.
	SCGCQ00584991 - (Closed) - current write policy is not getting updated until we press f5 .
	SCGCQ00808151 - (Closed) - CtrlR allows to set 4Kn VD or 4Kn JBOD as bootable device even though legacyBIOS does not handle it
	SCGCQ00798972 - (Closed) - Add "RAID" information for the "Cachecade VDs" in the VD menu.
	SCGCQ00727409 - (Closed) - Incorrectness in CTRL Management while launching Manage Link Speed
	SCGCQ00715452 - (Closed) - Ctrl R version 5.02-0002 has no option to create exlusive VDs
	SCGCQ00706013 - (Closed) - VD I/O policy changes from cached to direct when VDs are created from Ctrl-R
	SCGCQ00647392 - (Closed) - MR-6.4-join mirror-mirror drive is not seen in join mirror-choose option in CTRL-R
	SCGCQ00646220 - (Closed) - Getting an option in join mirror to select both "add new vd" and "existing VD" in ctrl-r
	SCGCQ00625175 - (Closed) - on having more than 64 VD's and initiating a copyback from ctrl-r will result in montask
	SCGCQ00606059 - (Closed) - In iMR controller we are able to set VD properties to write back and cached .
	SCGCQ00568220 - (Closed) - observing wrong help for "cache flush interval"
	SCGCQ00798810 - (Closed) - Prepare for removal appears even when Drives is in progress
	SCGCQ00786830 - (Closed) - In 2 iMR controller environment switching between iMR cards hits MonTask
	SCGCQ00758768 - (Closed) - Incorrectness in the confirmation popupmenu while creation of VD from available size.
	SCGCQ00725545 - (Closed) - In foreign Config Preview VD Size is coming as NA instead of actual size,when VD state is foreign.
	SCGCQ00667550 - (Closed) - Not able to Manually stop or suspend the copyback operation once started
	SCGCQ00490789 - (Closed) - Selecting "Manage Link Speed" in CTL+R causes Fatal Error with SAS 9343-4i
	SCGCQ00487220 - (Closed) - ctrl-r dosent lists all the drives to do replace drive.
	SCGCQ00816672 - (Closed) - Handle CCVD Changes Based on new API changes
	SCGCQ00795128 - (Closed) - Create VD screen basic settings options are overlapped on border of Create VD box
	SCGCQ00760689 - (Closed) - not able to set cacheflushint value to 255 for MR card.
	SCGCQ00735369 - (Closed) - not able to navigate through "join mirror -choose option" window
	SCGCQ00730412 - (Closed) - Incorrectness in the popup generated during deletion of Cachecade associated Virtual Drive
	SCGCQ00666807 - (Closed) - "enable jbod" help file is not opening with f1 option on it.
	SCGCQ00663996 - (Closed) - Not able to change emulation properties in CTRL-R for iMR
	SCGCQ00565979 - (Closed) - /c0/pall show and Linkspeed information is not in same in Ctrl-R.
	SCGCQ00484556 - (Closed) - Controller peer status and others in Property-page is coming wrong
	SCGCQ00811322 - (Closed) - Not able add new VD in Drive Group
	SCGCQ00803755 - (Closed) - FW hangs during SVD and CCVD migration based on DDR Size
	SCGCQ00798968 - (Closed) - User entering with 3 times wrong password, should not be able to attempt to create the Secure VD.
	SCGCQ00760972 - (Closed) - Error code coming as "Unknown" while importing Foreign Configuration, when controller is in Safe Mode
	SCGCQ00742106 - (Closed) - Remove Head Of Queue rebuild feature
	SCGCQ00731292 - (Closed) - Unable to see PD(s) Count in Cachecade RAID1 w.r.t to Cachecade RAID0
	SCGCQ00709969 - (Closed) - Showing incorrectness in Memory Size in Properties Page2
	SCGCQ00685370 - (Closed) - Showing extra : in the CacheCade(Write) while seeing property of VD
	SCGCQ00666806 - (Closed) - Set factory defaults option is blocking the "prev" button in controller properties page
	SCGCQ00647015 - (Closed) - LD emulation properties not getting set on updating VD properties
	SCGCQ00568725 - (Closed) - Not showing PD to assign as DHS to R50/ R60 VD if PD is of lesser size than largest PD in VD
	SCGCQ00490688 - (Closed) - ctrl-H doesn't lists the drives to do replace drive while doing copyback in PD MGmt Screen
	SCGCQ00488424 - (Closed) - Ctrl-R VD properties are not showing host access in the main VD management page
	SCGCQ00488372 - (Closed) - Ctrl-R VD properties are not reflecting after changing the host acess policy
	SCGCQ00487602 - (Closed) - Power savings button not enabled on Ctrl-R
	SCGCQ00483586 - (Closed) - Added HA changes (shared access option during VD creation, PFK related changes and property display)
	SCGCQ00642229 - (Closed) - Added a new property HOQ rebuild in VD advanced properties dialog.
	SCGCQ00493479 - (Closed) - Implemented the safe mode in Ctrl-R
	SCGCQ00711564 - (Implemented) - enable SED support for iMR JBOD
	SCGCQ00671938 - (Closed) - SSHA implementation for Control-H Synchro
	SCGCQ00656615 - (Closed) - DG/VD Hide&Unhide operations are added.
	SCGCQ00787944 - (Implemented) - Update Attribution Language - Copyright, Trademark, Confidentiality to Avago
	SCGCQ00707608 - (Closed) - Maintenence Mode implementation.
	SCGCQ00707519 - (Closed) - SSHA Licensing (PFK)
	SCGCQ00688692 - (Implemented) - Complete 240VD support for utilities
	SCGCQ00630099 - (Closed) - Requirement for 512e implementation changes
	SCGCQ00585013 - (Closed) - Added the code to unset the boot-device to NONE
	SCGCQ00787970 - (Closed) - system hang when entering 9341 or 9361 CTRL-R BIOS with headless systems without VGA.
	SCGCQ00625862 - (Closed) - Add Mirror Join functionality: PR SCGCQ00521537
	SCGCQ00787965 - (Implemented) - Address BBU/Supercap inconsistent Behavior across apps.
	SCGCQ00630308 - (Closed) - SED/FDE changes for Control-R Synchro
HII 03.13.09.00
	SCGCQ00594011 - (Closed) - With out selecting any drives I am seeing the previous config VD size.
	SCGCQ00811359 - (Closed) - Change the Media type before the protocol.
	SCGCQ00798962 - (Closed) - When Bootable JBOD is present under controller management ''Question value mismatch with option value'' window is displayed.
	SCGCQ00798657 - (Closed) - Handle new changes of BBU doc related to Battery Status
	SCGCQ00740787 - (Closed) - HII issues Add Config when there is no config
	SCGCQ00738687 - (Closed) - Incompatibility details are not displayed under HII properties
	SCGCQ00696506 - (Closed) - Grammaical errors in HII warning message during FW Flash.
	SCGCQ00692849 - (Closed) - When Controller is in Safe Mode don't remove UCM formset
	SCGCQ00689437 - (Closed) - Schedule consistency check gives an error message on Apply changes
	SCGCQ00633320 - (Closed) - Handling code collaborator Defects:SCGCQ00573222 andSCGCQ00568814
	SCGCQ00625438 - (Closed) - Minor Typos and consistency issues in HEFU HII help text
	SCGCQ00618674 - (Closed) - StartHiiImpl() WriteToLogger uses %g and EFIHiiDriverEntryPoint() Print statement uses %g for displaying EFI status
	SCGCQ00609737 - (Closed) - Confiuration Restore is not working
	SCGCQ00595344 - (Closed) - Support for SSC & SSHA configuration.
	SCGCQ00557402 - (Closed) - System hang observed when the "PdInfo.userDataBlockSize" is set to 0.
	SCGCQ00579816 - (Closed) - HII\EKM-LKM without reboot should show proper message
	SCGCQ00764936 - (Closed) - Schd CC page/Consistency Check mode does not explain the difference between sequential & concurrent
	SCGCQ00768459 - (Closed) - HII 5.13 PKG 01/Enclosure Management screen and Drive managment screen do not match
	SCGCQ00452128 - (Closed) - HII cannot assign partial space less than 1 GB
	SCGCQ00810866 - (Closed) - Advanced Properties of VD are not displayed when it is Selected under Virtual Drive Management.
	SCGCQ00804281 - (Closed) - FW hangs during SVD and CCVD migration based on DDR Size
	SCGCQ00771730 - (Closed) - Locked PD is shown in Preview Foreign Configuration form.
	SCGCQ00758589 - (Closed) - Dashboard View Help Content: Reuse the string where possible and incoporate following changes suggested by tech pub
	SCGCQ00716628 - (Closed) - To Handle Code collab review Defect forSCGCQ00700199
	SCGCQ00700304 - (Closed) - MSystem fails to boot into SETUP[F2] and displays blank screen with 160 and 240 VDs
	SCGCQ00691938 - (Closed) - Return device error when MR_DCMD_CTRL_PROPERTIES_SET fails.
	SCGCQ00658674 - (Closed) - Hii - Restrict the user from creating the 65th VD.
	SCGCQ00615221 - (Closed) - Form UF003 prints error messages (use WriteToLogger to log these debug messages)
	SCGCQ00614110 - (Closed) - Support the API change ExclusiveLDSupported to ExclusiveLDNotSupported for compatibility reasons
	SCGCQ00614027 - (Closed) - Firmware updation fails in OEM machine
	SCGCQ00602492 - (Closed) - HII fails to list the foreign configuration
	SCGCQ00595445 - (Closed) - Remove the option to create non-shared VD in the SSHA configuration
	SCGCQ00573871 - (Closed) - fixing code review defects (AIM version + UCM GUID + deallocation)
	SCGCQ00565876 - (Closed) - Remove duplicated strings from the UNI FIle
	SCGCQ00521488 - (Closed) - Getting error message when we suspend Patrol read operation through HII browser
	SCGCQ00472196 - (Closed) - Profile based VD creation path incorrectly showing protect VD/secure VD checkbox when user clicks on drive selection criteria
	SCGCQ00402740 - (Closed) - Create VD change VD Size causes HII to freeze
	SCGCQ00413924 - (Closed) - Schedule CC in concurrent mode behaves unexpectedly.
	SCGCQ00571353 - (Closed) - Allow user to select RAID level when controller has other VD + error handling
	SCGCQ00617617 - (Closed) - FWMgmt Prtocol:<config ID="LSIMegaRAIDConfigurationTool"> has no "versionid" info.
	SCGCQ00762860 - (Closed) - HII Dashboard/3.11.02.00/View server profile is showing two periods after the word "them" under Hardware Components
	SCGCQ00767605 - (Closed) - When you have a locked PD/FDE in a foreign state, it is not showing up on the dashboard only under configure
	SCGCQ00598822 - (Closed) - VD details display is improper in Expand Virtual Drive
	SCGCQ00810827 - (Closed) - 3 times wrong password at boot time – Handle the 'Manage Foreign Configuration' page options properly with Secure JBOD present
	SCGCQ00803946 - (Closed) - HII does not show HDD /SSD information for the PDs in HII Drive management and Advanced drive properties page
	SCGCQ00783556 - (Closed) - Question value mismatch when Fan3 and 4 is selected
	SCGCQ00756533 - (Closed) - Remove FRU from Enclosure Management
	SCGCQ00709543 - (Closed) - gHiiDriver.ExtLDSupport should be Filled with appropriate value before it's used
	SCGCQ00702200 - (Closed) - Firmware Update feature fails to update firmware in HII
	SCGCQ00700199 - (Closed) - After selcting Discard pinned Cache from Controller Management, Form will be taken to Cache and Memory after success.
	SCGCQ00630532 - (Closed) - Consistency Check Start - remove mm/dd/yyyy from the string as the format is out of control of LSI
	SCGCQ00613822 - (Closed) - Advanced Controller Properties- Power Saving Settings has broken form
	SCGCQ00565088 - (Closed) - Help content for Firmware Update in Controller Management is inappropriate
	SCGCQ00555333 - (Closed) - To be in sync with other subtitles make all letters capital for "High Availability Properties" and add colon at the end
	SCGCQ00413061 - (Closed) - BBU information and propererties are not displayed in HII browser for Perc9-H730P controller.
	SCGCQ00569098 - (Closed) - Enter security key for locked drives screen, press down to get to OK, OK will show up again on right
	SCGCQ00762856 - (Closed) - HII Dashboard/3.11.02.00/When preview foreign config from Dashboard, it is coming up as HF034 at the top
	SCGCQ00598431 - (Closed) - Drop Down option in VD properties for Cached is present
	SCGCQ00820006 - (Closed) - Address review comments
	SCGCQ00806514 - (Closed) - After entering security key it goes back to Manage Foreign config page
	SCGCQ00798824 - (Closed) - HII - NVRAM size shown as 32MB instead of 32KB
	SCGCQ00798820 - (Closed) - Does not show RAID level for CCVD in 'VD management' and 'View DG properties' pages
	SCGCQ00784597 - (Closed) - HII Configuration Management Enable Security On JBOD OK button is grayed out
	SCGCQ00783374 - (Closed) - HII reports CCVD deleted even though its still under deletion process by FW
	SCGCQ00755277 - (Closed) - Change "Consistency Check" to "Make Data Consistent" for CC Rate and Stop CC on error is not changed
	SCGCQ00731567 - (Closed) - use hwPresent.memory to determine iMR
	SCGCQ00714530 - (Closed) - Firmware Update - On selecting empty folder, hang is seen.
	SCGCQ00704309 - (Closed) - Question value mismatch message seen in Enclosure Management screen.
	SCGCQ00702196 - (Closed) - Asserts seen before loading HII
	SCGCQ00678695 - (Closed) - Change the Step Value to 0 for all numeric to make sure for free edit instead of Incrementing and decrementing using +/-
	SCGCQ00624890 - (Closed) - Handling Code Collaborator Defect:SCGCQ00573222
	SCGCQ00615190 - (Closed) - Cloning Changes: Fill Controller Index in RouteConfig + for UF003 calculate checksume only for the actual config size
	SCGCQ00610889 - (Closed) - Customize help string for Select Interface Type
	SCGCQ00595864 - (Closed) - On Success of creating Drive Security Form loads into Advacned controller properties
	SCGCQ00589301 - (Closed) - System/HII hang when clicks on Hardware Components menu option in HII.
	SCGCQ00402839 - (Closed) - HII warning message is not displayed before reconfigure/reconstruction.
	SCGCQ00407234 - (Closed) - HII hangs when trying to access an Unconfigured Bad PD while in Safe Mode
	SCGCQ00412758 - (Closed) - HII Manage Foreign Configuration menu is not available when a foreign locked drive is present in the configuration.
	SCGCQ00556839 - (Closed) - Able to select EKM even when the EKM FOD key is removed from the system.
	SCGCQ00770227 - (Closed) - HII displays supercap module version as "Firmware Version"
	SCGCQ00771193 - (Closed) - Entering security key in HII to unlock PD fails to import afterwards
	SCGCQ00593558 - (Closed) - Auto Learn Mode is showing wrong data
	SCGCQ00808162 - (Closed) - HII allows to set 4Kn VD or 4Kn JBOD as bootable device even though legacyBIOS does not handle it
	SCGCQ00798579 - (Closed) - Schedule consitecny check gives invalid time when change from diable to hour, daily, weekly and monthly.
	SCGCQ00797318 - (Closed) - Change UCM form set title from AVAGO to LSI
	SCGCQ00765519 - (Closed) - R5/R6 creation fails in HII from Profilebased creation
	SCGCQ00755021 - (Closed) - Operation's are not refreshed in Dashboard
	SCGCQ00719117 - (Closed) - Domain ID should be displayed under High Availability properties
	SCGCQ00706817 - (Closed) - Virtual Drive properties[Read/Write/IO Policy] gets changed after VD creation from HII
	SCGCQ00679861 - (Closed) - Not able to create VD with 4k drives on intel wildcat server.
	SCGCQ00645532 - (Closed) - Update the help string
	SCGCQ00640534 - (Closed) - HII is showing RAID6 and RAID5 levels while creating VD when we have 2 512n drives and 1 4k Drives
	SCGCQ00634621 - (Closed) - VD Proprties-Advanced-GUID Value left blank and add customiztion for the string STR_FORM_HF115_PHNA_HELP
	SCGCQ00622464 - (Closed) - Toggling bewtween Legacy to Uefi mode vice versa junk values seen .
	SCGCQ00613820 - (Closed) - Typo in HII form Controller Status
	SCGCQ00612574 - (Closed) - Addressed review comments
	SCGCQ00557977 - (Closed) - Handling code review defects
	SCGCQ00412098 - (Closed) - Unable to create UnevenSpan R10 Vd in HII.
	SCGCQ00760501 - (Closed) - DashBoard HII showing 1 enclosure connected even though there are 0 connected.
	SCGCQ00799642 - (Closed) - In copyback window the Associated Virtual Drive shows free space only for replacing drive
	SCGCQ00798806 - (Closed) - HII - Schedule CC right side info pane to be corrected (Add Monthly and Change Disabled to Disable as per drop down box)
	SCGCQ00766787 - (Closed) - HII- DHS assgining fails in presence of 240 Vds
	SCGCQ00765523 - (Closed) - BGops fails to start when VD erase is already runnign on the other VD
	SCGCQ00716636 - (Closed) - Incomplete SAS Address
	SCGCQ00710064 - (Closed) - Handline code collaborator Defect forSCGCQ00709543
	SCGCQ00707614 - (Closed) - Addressed review comments
	SCGCQ00678603 - (Closed) - HII does not display power state of a PD
	SCGCQ00590465 - (Closed) - On selecting a wrong parameter for size while creating VDs, Options greyed, Create VD page exits to parent page.
	SCGCQ00524969 - (Closed) - HII PKG 0006/Going from LKM to EKM asks for a Current Security key Identifier and Security key.
	SCGCQ00595463 - (Closed) - Security feature is enabled but HII sees "Drive Security" as disabled
	SCGCQ00637539 - (Closed) - Remove FMP installed on the controller handle in HII
	SCGCQ00760435 - (Closed) - Date getting corrupted when selecting different Check Consistency Frequencie
	SCGCQ00768437 - (Closed) - Entering the wrong security key in HII & go back to enter the correct one the security key form should be cleared
	SCGCQ00816666 - (Closed) - Handle CCVD Changes Based on new MR.h bit supportExtendedSSCSize
	SCGCQ00795338 - (Closed) - SSD caching enabled on a Recon VD .
	SCGCQ00791138 - (Closed) - Handle the maximum cache size value based on the max supported by FW, in the warning message shown during CCVD creation.
	SCGCQ00779364 - (Closed) - Wrong drivegroup count shown with foreign config in safe mode
	SCGCQ00767138 - (Closed) - Controller in Safe Mode - ASSERTs seen on console during the Preview of Foreign Configuration
	SCGCQ00765244 - (Closed) - Dashboard: comment out the referesh interval for all other fields except conroller status.
	SCGCQ00756640 - (Closed) - In configuration Management creation of JBOD not possible as option to set JBOD is grey out.
	SCGCQ00730496 - (Closed) - HII gives the option to set -head of queue for raid 0
	SCGCQ00723184 - (Closed) - Capacity Allocation in drive group properties is inappropriate
	SCGCQ00715566 - (Closed) - Addressing review comments
	SCGCQ00705577 - (Closed) - Unable to select the second enlcosure when multiple enclosures are connected to a controller .
	SCGCQ00684992 - (Closed) - Question about "Connected Port" in PD advance menue
	SCGCQ00627778 - (Closed) - Address review comments
	SCGCQ00597641 - (Closed) - MR6.3 HII aesthetic change
	SCGCQ00578190 - (Closed) - HII should calculate checksum before setting bios data (MR_BIOS_DATA)
	SCGCQ00573222 - (Closed) - Handling Code Collaborator Review Defects forSCGCQ00568814 andSCGCQ00569197
	SCGCQ00571359 - (Closed) - Typo "Clear Configuaration" -> "Clear Configuration"
	SCGCQ00401410 - (Closed) - no help information for "Default Initialization"
	SCGCQ00406502 - (Closed) - VD creation with Access Policy Read Only fails with PopUp message
	SCGCQ00575062 - (Closed) - added a while loop and take care of the multiple PD Groups scenario.
	SCGCQ00761105 - (Closed) - controller yields spaces in HII Dash
	SCGCQ00764215 - (Closed) - HII 5.13 PKG 01/3.11.02.00/Preview foreign configuration screen missing words
	SCGCQ00776052 - (Closed) - 5.13 HII PKG 02/When creating a VD that is more than 1TB in size in HII, you will loose the extra space after saving the VD
	SCGCQ00811295 - (Reworked) - Generic RAID1 Profile based VD creation option is not grayed out after creating 64VD's.
	SCGCQ00798739 - (Closed) - HII Server profile shows "SILENCE ALARM" instead of "SERVER" subtitle as per design
	SCGCQ00798684 - (Closed) - HII -> Drive management does not show "Secure" when JBOD created from a SED drive
	SCGCQ00778462 - (Closed) - HII Boot time Asserts
	SCGCQ00760450 - (Closed) - Need to remove Force Write Back option with CCVD creation
	SCGCQ00756784 - (Closed) - Chk the err status for HL_Get_PD_List() and HL_Get_PD_Info in UF002_PrepareData() + check Driver handle if index is valid
	SCGCQ00750118 - (Closed) - Remove Head Of Queue rebuild feature
	SCGCQ00704216 - (Closed) - HII hangs on selecting "View Drive Group Properties"
	SCGCQ00672925 - (Closed) - Unable to set spinup drive count in HII
	SCGCQ00619028 - (Closed) - Not able to schedule CC in concurrent mode from HII(03.07.09.00).
	SCGCQ00614675 - (Closed) - To address FW Update help Strings
	SCGCQ00574989 - (Closed) - Creation+ FW updation+ Scan foreign Configuration is disabled/grayed out in HII page
	SCGCQ00574041 - (Closed) - AIM (Agentless Inventory Manager) Issues
	SCGCQ00503036 - (Closed) - Changing Percentage of Space to Expand Does not Update Final VD Size
	SCGCQ00614466 - (Closed) - HII 03.07.05.00/Under advanced controller properties and selecting Cache and Memory, it says's "scontroller cache"
	SCGCQ00734447 - (Closed) - Patrol read prop page gives an error message on Apply changes
	SCGCQ00760432 - (Closed) - Getting question value mismatch when changing the Consistency check Frequency settings
	SCGCQ00768009 - (Closed) - Locked PD on controller with security disabled does not show properly when viewing under Foreign config
	SCGCQ00526978 - (Closed) - Provide controller FW update function
	SCGCQ00765822 - (Implemented) - Display the expander firmware version under Controller properties in HII when there is an expander on the controller
	SCGCQ00626605 - (Closed) - (Phase1) HII-based PCI Inventory - MR) into the mainline
	SCGCQ00550390 - (Closed) -  Write Caching HBA, JBOD/R0 supported TB controller with 240 SystemPD/LD support
	SCGCQ00620259 - (Closed) - Port 240VD change to TboltSCGCQ00441334
	SCGCQ00730596 - (Closed) - Refreshing individual field (in this case progress field)
	SCGCQ00568814 - (Closed) - Simplify controller propety page
	SCGCQ00789495 - (Closed) - Suppress UEFI HII Clear Configuration setting
	SCGCQ00689070 - (Closed) - Negative test HII browser- Mixing unsupported drives message needs update
	SCGCQ00650085 - (Implemented) - HEFU HII UDK2010 complaince
	SCGCQ00642228 - (Implemented) - Implement Head of Queue drive rebuild for MegaRAID controllers
	SCGCQ00633875 - (Closed) - Support for SED.
	SCGCQ00568706 - (Closed) - Remove limitation for creating R6 in HII for Perc9.0/9.1
	SCGCQ00787943 - (Closed) - Update Attribution Language - Copyright, Trademark, Confidentiality to Avago
	SCGCQ00664753 - (Closed) - Ability to enable/disable JBOD mode in HII & CTRL-R
	SCGCQ00634019 - (Closed) - Change the default Setting of Disk Cahce Policy from Unchanged to Disable.
	SCGCQ00612466 - (Closed) - Provide pop-up to display current version and update fw version as part of HEFU HII Firmware Update functionality
	SCGCQ00804082 - (Closed) - HII reports 'Security key entered is incorrect' even though it sent this request to FW and FW report as success.
	SCGCQ00797917 - (Implemented) - MegaRAID CPLD update improvements
	SCGCQ00789505 - (Closed) - Replace the word enclosure with expander for 720ix
	SCGCQ00711563 - (Closed) - enable SED support for iMR JBOD
	SCGCQ00789504 - (Closed) - Consistency check date entry fix issue and Start Immediatley option required in SCC form
	SCGCQ00787942 - (Implemented) - Update Attribution Language - Copyright, Trademark, Confidentiality to Avago
	SCGCQ00721161 - (Closed) - HII Create Virtual Drive advanced option defaults Protect Virtual Drive to enabled
	SCGCQ00656614 - (Closed) - Add ability to take a VD offline, bring back VD online
	SCGCQ00626591 - (Closed) - Add Mirror Join functionality 
	SCGCQ00626585 - (Closed) - Requirement for 512e implementation changes - PRSCGCQ00425778
	SCGCQ00571579 - (Implemented) - Create a formset with classGUID that customer has provided. This formset will have two forms. The majority of the time will be spend on collecting and finalizing requirement from Customer and validating the code using test tool from customer. Only HI
	SCGCQ00593247 - (Closed) - SSHA boot support
	SCGCQ00787964 - (Closed) - Address BBU/Supercap inconsistent Behavior across HSW apps.
	SCGCQ00688454 - (Implemented) - HEFU HII UDK2010 complaince
	SCGCQ00569197 - (Closed) - Move Disable Protection option from Controller Management to VD management
	SCGCQ00712484 - (Closed) - Create dashboard view as a landing form in HII
	SCGCQ00621285 - (Closed) - Change the wording in HII from Check Consistency to Make data consistent
	SCGCQ00557104 - (Closed) - Provide support for toggling the controller to and from MAINTENANCE mode.	
UEFI_Driver 0x060D0200
	SCGCQ00335617 - (Closed) - Drives are reporting timeout on Write Buffer cmd
	SCGCQ00378953 - (Closed) - HII not showing up + other enhancement for driver health formset
	SCGCQ00413986 - (Closed) - HII app doesnt appear when there is critical message and when platform uses SetOptions
	SCGCQ00479003 - (Closed) - Disable Debug print in UEFI Driver
	SCGCQ00320619 - (Closed) - Build Device Path and Get Next Target function of SCSI Pass Thru is not returning correct EFI status for certain cases
	SCGCQ00339371 - (Closed) - Driver fails SCT Test
	SCGCQ00408333 - (Closed) - Critical boot message formatting issue
	SCGCQ00347171 - (Closed) - having pinned cache on controller, the option to invoke storage dosent come.
	SCGCQ00384884 - (Closed) - Customize health formset + few other issues
	SCGCQ00395190 - (Closed) - When trying to create an R6/R5, I am unable to create though there are 3 SAS unconfigured good avail
	SCGCQ00396051 - (Closed) - UEFI Driver (MR 5.7) should not display finite boot messages
	SCGCQ00435384 - (Closed) - UEFI System hang if controller FW is in fault state
	SCGCQ00343869 - (Closed) - Enhance critical boot message handling
	SCGCQ00369636 - (Closed) - Settime only when FW time is not set; Return appropriate health status when there is no critical boot message
	SCGCQ00408094 - (Closed) - system with a critical message does not enter EFI preboot config utility
	SCGCQ00498925 - (Closed) - Not able to boot into BIOS boot menu in server
	SCGCQ00312683 - (Closed) - UEFI Driver not timing out in 3 mins when FW is in undefined state
	SCGCQ00518791 - (Closed) - In IsValidHandle() - Free the buffer if status is not EFI success for LocateHandle
	SCGCQ00493654 - (Closed) - Memory Leak issue in UEFI driver when reconnect happens
	SCGCQ00308870 - (Closed) - When disconnecting the driver in EFI, I am still able to exectue the EFI utility menu.
	SCGCQ00614111 - (Closed) - Support the API change ExclusiveLDSupported to ExclusiveLDNotSupported for compatibility reasons
	SCGCQ00262858 - (Closed) - Debug message is shown from EFI app choice prompt on a system
	SCGCQ00624894 - (Closed) - Handling Code Collaborator Defect: SCGCQ00593243
	SCGCQ00483847 - (Closed) - Remove private GUID and use EFI_KMS_PROTOCOL_GUID defined in UEFI 2.3.1 spec
	SCGCQ00340581 - (Implemented) - UEFI Driver should check pMRCtrlInfo ->maxHANodes with > 1 to determine HAMR
	SCGCQ00365374 - (Implemented) - Add 3108 device ID
	SCGCQ00385365 - (Closed) - PCIDATA
	SCGCQ00593243 - (Closed) - SSHA boot support
	SCGCQ00285974 - (Implemented) - Add 4k secotor boot support in UEFI Driver
	SCGCQ00404216 - (Closed) - Add 3008 device ID for iMR product.
	SCGCQ00318101 - (Closed) - Timed critical boot message under UEFI mode
	SCGCQ00347492 - (Closed) - Retry read capacity if scsi status is not success
	SCGCQ00395996 - (Closed) - Parse Boot message and remove \r\n at the beginning and replace \n with \r in other parts
	SCGCQ00292963 - (Implemented) - Disables all requirement for human input at boot time
	SCGCQ00331573 - (Closed) - Remove dependency on deprecated Driver Configuration2 protocol from UEFI Driver
	SCGCQ00392836 - (Closed) - LSI to Support Remote Key Management
	SCGCQ00278257 - (Implemented) - Add FoD support for 3108
	SCGCQ00436609 - (Closed) - add PnPID's for 3004 and 3108
	SCGCQ00338782 - (Implemented) - If SetOptions is called for Invader dont show EFI WebBIOS and EFI CLI option
	SCGCQ00338066 - (Implemented) - Fire LD list query based on maxHANodes
	SCGCQ00310476 - (Implemented) - Load HII when user responds to critical boot message by pressing C
PCLI 05.06.03
NVDATA 3.1505.00-0004
BootBlockCommon 07.26.26.219
BootBlock 3.02.00.00-0001
ROMENV 1.09


Package 26.0.0-0056 - Initial release (HA-DAS 2.0)
	Firmware - 4.300.00-3867
	FCODE - 4.15.06.00
	UEFI_Driver - 0x06040900 (SIGNED)
	Hii - 04.01.10.00 (SIGNED w/correct Size)
	BIOS - 6.15.08.0
	Ctrl-H - 5.02-0004
	NVDATA - 3.1409.00-0008 
	BootBlock - 3.02.00.00-0001
	ROMENV - 1.09

*Third-party trademarks are the property of their respective owners.

