================================================================================
Intel(R) Server Platform S1200V3RP System Firmware Update Package for 
The embedded EFI Shell
================================================================================
Intel Enterprise Platform & Services Division - Marketing
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================
DATE    : July 6, 2015
TO      : Intel(R) Server Board S1200V3RP
SUBJECT : Release Notes for System Firmware Update Package 
================================================================================
                              ABOUT THIS RELEASE
================================================================================
BIOS   : R03.02.0003
ME     : R03.00.07.024
BMC    : 1.13.8619
FRUSDR : 1.08
================================================================================
                           Support Platforms and Dependency
================================================================================
This update package is for Intel(R) Server Board S1200V3RPM_RPL_RPO

Intel(R) Server Platform S1200V3RP family Processors supported: 
  Intel(R) Xeon(R) Processor E3-1200 V3 series
  Intel(R) Xeon(R) processor E3-1200 V4 series
  
Microcode update versions:
Intel(R) Xeon processor E3-1200 V3 series A0 version: 0xffff0014 CPUID = 0x306C1
Intel(R) Xeon processor E3-1200 V3 series B0 version: 0xffff0006 CPUID = 0x306C2
Intel(R) Xeon processor E3-1200 V3 series C0 version: 0xffff0017 CPUID = 0x306C3
Intel(R) Xeon processor E3-1200 V3 series C0 version: 0x0000001D CPUID = 0x306C3 
Intel(R) Xeon processor E3-1200 V4 series G0 version: 0x0000000B CPUID = 0x40671 

On-Board Component Option ROM Versions:
Integrated Matrox VGA               : VBE BIOS V3.8 SQ
1G PXE Option ROM                   : Intel(R) Boot Agent XE v1.5.53.1
10G PXE Option ROM                  : Intel(R) Boot Agent XE v2.3.24.1
82599 10G PXE Option ROM            : Intel(R) FCoE Boot v1.8.17
iSCSI Option ROM                    : Intel(R) iSCSI Remote Boot version 3.0.43
NIC UEFI Driver                     : E6327X3.EFI
SATA RAID Option ROM - RSTe         : 4.1.0.1026
UEFI SATA RAID Option ROM - RSTe    : 4.1.0.1026
ESRT II FOR SATA                    : A.14.02121826
Legacy Processor Video              : 5.5.1038
UEFI Processor Video driver         : 5.5.1032 

Reference Code Version              : 2.7.1
Memory Reference Code Version       : 1.8.0.3
v4 Memory Reference Code Version    : 2.7.1.0
Management Engine Firmware Version  : 03.00.07.024
ACM                                 : BDW v1.2

      
================================================================================
                           INSTALLATION NOTES
================================================================================


WARNING:  It is very important to follow these instructions as they are written.
Failure to update using the proper procedure may cause damage to your system.

A:UEFI iFlash32 
   1.  Boot the system to EFI Shell
   2.  Copy IFlash32.efi and BIOS.CAP file to a USB Flash Drive
       ( Do not use the *Rec.CAP file as it will clear the NVRAM)
   3.  Map the respective storage device in the system with the command
	   Shell> map -r
   4.  Change the Shell to mapped device file system
	   Example: Shell> fs0: (or fs1:)
   5.  Run the IFlash32 utility at the prompt
	   fs0:\> IFlash32 [File Name] /u /ni
   6.  Either reboot the system and Go into BIOS setup <F2>, reset defaults <F9>
       and save <F10> or After the BIOS update and before rebooting, 
       run: fS0:> Iflash32 -rd
   7.  Reboot the system

B:Backup BIOS update instructions
   1.  Boot the system to EFI Shell
   2.  Copy IFlash32.efi and BIOS .CAP file to a USB Flash Drive
       ( Do not use the *Rec.CAP file as it will clear NVRAM)
   3.  Map the respective storage device in system with the command
	   Shell> map -r
   4.  Change the Shell to mapped device file system
	   Example: Shell> fs0: (or fs1:)
   5.  Run the IFlash32 utility on the prompt
	   fs0:\> IFlash32 [File Name] /u /ni UpdateBackupBios
   6.  It will update primary BIOS with processed capsule, and the backup BIOS 
       update will be completed in next normal boot.
   7.  Reboot the system.
================================================================================
                        BIOS RECOVERY INSTRUCTIONS
================================================================================

The Recovery process can be initiated by setting the recovery jumper. (called 
BIOS Recovery Boot Jumper)
 
A BIOS recovery can be accomplished from the backup BIOS region or USB Mass Storage device. 
Please note that recovery from USB floppy is not supported on this platform. 
 
The recovery media must contain the following files under the root directory:
   2.  UEFI iFlash32 (including IFlash32.efi and ipmi.efi )
   3.  *Rec.CAP
   4.  Startup.nsh (update accordingly to use proper *Rec.CAP file)
 
BIOS starts the recovery process by first loading and booting to the recovery image from the 
backup BIOS region.

This process takes place before any video or console is available. Once the system boots 
to recovery image, it will boot automatically into EFI Shell to invoke the Startup.nsh 
script and start the flash update application (IFlash32.efi). IFlash32.efi requires the 
supporting BIOS Capsule image file (*Rec.CAP). After the update is complete, there will 
be a message displayed stating that the "BIOS has been updated successfully" indicating 
the recovery process is finished. The User should then switch the recovery jumper back to
normal operation and restart the system by performing a power cycle.
 
The following steps demonstrate this recovery process:
   1.  Power OFF the system.
   2.  Insert recovery media.(Optional if the backup BIOS region works)
   3.  Switch the recovery jumper. Details regarding the jumper ID and location
       can be obtained from the Product Board TPS.
   4.  Power ON the system.
   5.  The BIOS POST screen will appear displaying the progress and system automatically 
       boots to the EFI SHELL.
   6.  Startup.nsh file executes, and initiates the flash update (IFlash32.efi)
       with new capsule file (*Rec.CAP). The regular IFlash message will be displayed at
       the end of the process, once the flash update succeeds.
   7.  Power OFF the system, and revert the recovery jumper position to "normal".
   8.  Power ON the system. 
   9.  Do *NOT* interrupt the BIOS POST during the first boot.

================================================================================
                            KNOWN ISSUES/WORKAROUNDS
================================================================================
- If you want to install Linux* SUSE* 11 SP2 or boot to a pre-installed Linux* SUSE* 11 SP2 OS, 
- R02.01.0002 and later version need use command "iflash32 -u RB_R02.0x.xxxxRec.cap UpdateBackupBios -ni" 
to upgrade from R01.04.0002 and early version. Similarly, R01.04.0002 and early version need use command "iflash32 -u RB_R01.0x.xxxxRec.cap UpdateBackupBios -ni" to downgrade from R02.01.0002 and later version.
- As security requirement, R03.01.0001 reversion doesn't support capsule downgrade in normal mode.
- R03.01.0002 is the first BIOS that adds support for Intel(R) Xeon processor E3-1200 V4 series. If you
   are upgrading from R02.02.0004 or earlier BIOS versions,  you will need to use  
   a Intel(R) Xeon processor E3-1200 V3 series processor first to boot to EFI shell and use capsule files to update BIOS to R03.01.0002.
   After flashing with the Intel(R) Xeon processor E3-1200 V3 series processor, you can install
   the Intel(R) Xeon processor E3-1200 V4 series processor and boot.  
==============================================================================
==
                                R03.02.0003
================================================================================
NOTICE:  R03.02.0003 supports the Intel(R) Xeon processor E3-1200 V4 series. If you
   are upgrading from R02.02.0004 or earlier BIOS versions,  you will need to use  
   a Intel(R) Xeon processor E3-1200 V3 series processor first to boot to EFI shell and use capsule files to update BIOS to R03.01.0002.
   After flashing with the Intel(R) Xeon processor E3-1200 V3 series processor, you can install
   the Intel(R) Xeon processor E3-1200 V4 series processor and boot.
  - Added: Microcode update 0x0000000D for CPUID = 0x40671
  - Fixed:  Variable can't be set or deleted in EFI Shell via EFI shell commands-----intermittent issue
  - Fixed:  [BMC_BDW]There're some SMI timeout event logs when run DC cycle
  - Fixed:  Nvidia 06G-P4-2790-KR X16 card hang at 0x15 during POST with BIOS PV RC1

  - Fixed:  The PCIE Oprom Control options are expected to be invisible in UEF
  - Fixed:  L3 cache Associativity of SMBIOS type 7
  - Fixed:  sysinfo_log.txt file does not match with Bios information
  - Fixed:  The SUT hang at 0x0E with CPU QJ6G when 3 wrong password attempt
  - Fixed:  Gen3 card working on Gen2 on LC/RO/RM slot 6 when no other device populated.
  - Fixed:  Hyper -V installation on S1200V3RP system fail on R03.02.0002 while no this issue on R03.02.0001. the issue also happened on Vmware ESXi5.5

==============================================================================
==
                                R03.01.0002
================================================================================
NOTICE: As security requirement, R03.01.0002 and later revision doesn't support capsule downgrade to R02.02.0005 and previous revision in normal mode. It only supports capsule downgrade in Recovery mode.

NOTICE:  R03.01.0002 is the first BIOS that adds support for Intel(R) Xeon processor E3-1200 V4 series. If you are upgrading from R02.02.0005 or earlier BIOS versions,  you will need to use a Intel(R) Xeon processor E3-1200 V3 series processor first to boot to EFI shell and use capsule files to update BIOS to R03.01.0002.
   After flashing with the Intel(R) Xeon processor E3-1200 V3 series processor, you can install
   the Intel(R) Xeon processor E3-1200 V4 series processor and boot.


 -Added: Microcode update 0x0000001D for CPUID = 0x306C3
 -Added: Microcode update 0x0000000B for CPUID = 0x40671

 -Fixed: The SUT halt at 0x0D when the backup bios was updated at POST stage
 -Fixed: The type 4 Processor Upgrade Field vaule is incorrect for LGA1150 
 -Fixed: Cannot log in to BMC Webconsole after set user and password
 -Fixed: Sleep S3 wake up failed with BDW CPU. 
 -Fixed: System hangs at 0x9A with BDW CPU when VT-d is enabled   
 -Fixed: The value of Creator ID/OEM Revision/Creator Revision in FPDT tabl
 -Fixed: System will automatic resume from S1/S3/S5 after S3 wake on LAN.
 -Fixed: The maximum length of password don't match with the length of EPS
 -Fixed: The value at Bit 3 to Bit 7 of Processor Characteristics field
 -Fixed: The value of current usage field when it is populated for each in
 -Fixed: Sometimes the system hang at 0x96 with add-on graphic card.
 -Fixed: SUT will reboot unexpectedly  when run IWVSS  in Win2012R2.
 -Fixed: TBoot test failed 
 -Fixed: There are 16 N/A devices in BIOS USB configuratoin tab after usb controller disable
================================================================================ 
                              R02.02.0005
================================================================================
NOTICE: If BIOS Rev 02.01.0002 is not pre-installed then please upgrade/downgrade that release first.
  - Fixed: RS25GB008/RS2PI008 RAID cards lost after S3 resume when it plugged into slot4/7.
  - Fixed: The primary display option doesn't show in the MFG mode.
  - Fixed: The "Internal Graphics" option displayed on BIOS Setup in MFG mode with no-graphic CPU.
  - Fixed: NMI activated-system halted when three specific cards plugged into slot 4/6 and SAS_mod slot.
  - Fixed: [x]incorrect message showed on POST that S1200RPL with two SATA ports @ 3Gbps and 4 SATA ports @6Gbps.
  - Fixed: The onboard VGA would display after S3 when on board video was set to disabled in BIOS Setup.
  - Disable ACPI S4 support
================================================================================
                               R02.01.0004
================================================================================
NOTICE:  If BIOS Rev 02.01.0002 is not pre-installed then please install that release first prior to installing this release.
         The BIOS Rev 02.01.0002 contains a critical update which must be present before installing this release.

- This version enhances the protection of certain UEFI variables as described in 
	Intel Security Advisory INTEL-SA-00038
================================================================================
                                R02.01.0002
================================================================================
NOTICE: Need to use recovery capsule file to downgrade/upgrade between R02.01.0002 
        and any earlier BIOS versions (incluing R01.04.0002).  
  - Fixed: After loading default, the internal Graphics will change from enable to disable
  - Fixed: After Loading default and boot into Windows server 2012, SUT has yellow 
           mark in device manager
  - Fixed: After setting Primary Display as PCI Add-on Card or Onboard Video in BIOS Setup, 
           there is no display when SUT boots into Windows Server 2012
  - Fixed: System cannot save Password after clearing Password.
  - Fixed: Failed flash Me after AC/DC.
================================================================================
                                R01.04.0002
================================================================================
Note: This BIOS version is able to support more CPUs which are listed in Processor
      support list on support.intel.com

- Fixed: Unexpected event logged when heating the PCH with heat gun.
- Fixed: The system will hang at POST Code 0xB2 with add-on video card after "Primary Display" 
         BIOS setting is changed to "Onboard Video".
- Fixed: If process cannot support VT-d, Intel(R) VT for directed I/O Option is visible.
- Fixed: The NIC1/NIC2 controller option cannot be saved to "Disabled" in BIOS setup menu.
- Fixed: Internal Graphic of the Intel(R) Processor G1820T doesn't work on the Intel(R) Server Board S1200V3RPM.
- Fixed: The read/write speed of USB3.0 device cannot reache the right speed when connected to USB3.0 port.
- Fixed: If AC lost occurs during BIOS update, the system may not be recovered via BIOS recovery method.
- Fixed: When windows running in S3+S5 mode and shutting down the system, the system will reboot.
- Fixed: Sometimes the system will reboot after shutting down the system in windows.
================================================================================
                                R01.04.0001
================================================================================
- Added: Microcode 0x00000017 update
- Added: ESRT2 legacy oprom update
- Added: iSCSI v2.8.25 legacy oprom update
- Added: RSTe legacy oprom and efi driver update
- Added: Code enhancement for SRIOV support
- Added: iGFX GOP UEFI driver update
- Added: PCI Enumeration Complete Protocol support
- Fixed: Slot4 PCIe device lost issue
- Fixed: Windows 2008 R2 blue screen issue when Adaptec* 6805 controller installed in slot 7
- Fixed: Processor1 P1 MTT - Upper Fatal error on VMWare ESXi 5.1 U1
- Fixed: Wrong SMBIOS type 41 records for Ethernet
- Fixed: "Turbo Boost" and "SpeedStep" don't work under Windows 2012

================================================================================
                                R01.03.0005
================================================================================
  - Add link retrain on slot 4 before RC code executed(For PCIe device lost issue on slot4).


================================================================================
                                R01.03.0004
================================================================================
- Fixed: System can't boot into an OS or UEFI using Intel(R) Pentium(R) processors.
- Fixed: Red Hat* Linux* RHEL 6.4 32bit cannot be installed with 1GB DIMMs installed.
- Fixed: Corrected help text for "USB 3.0 support".
- Fixed: RAID mode incorrectly listed as "RST" - changed to "RSTe".
- Fixed: "9266" error is reported with certain add-in video adapters.

Other:
Added:	 TXT ACM V1.3 integration.
Updated: Video BIOS updated to version 2170

================================================================================
                                R01.02.0004
================================================================================
- Fixed: Signed driver check test fails due to an unknown device found in Windows 2012 WHQL
         (Windows Hardware Quality Labs) certification.

================================================================================
                                R01.02.0002
================================================================================
- Fixed: Memory DIMM will sometimes starts throttling, even in good thermal conditions.
- Fixed: System can't wake up from S3 via power button/USB device/Lan.
- Fixed: System power consumption cannot be limited by Node Manager.
- Fixed: BIOS version is not be updated accordingly in server management remote console.

Others:
 - Updated RSTe UEFI/Legacy OPROM to 3.7
 
================================================================================
                                R01.01.0006
================================================================================
- First production BIOS release.

================================================================================
                          ME Changes in 03.00.07.024
================================================================================
- Fixed: Platform does not go to S3/S4 state in recovery mode
- Fixed: Wrong value returned from Get Max Allowed Logical Processors command after
         S0->(S4,S3)->S0 transition
			  ME Changes in 03.00.07.018
================================================================================
- Fixed: Wrong value returned from Get Max Allowed CPU P-states/T-states while limiting
		using Total Power Budget

================================================================================
			  ME Changes in 03.00.05.128
================================================================================
- Fixed: Bit Reserved16 in PCH Strap 15 is set incorrectly. This change in Flash 
       Descriptor was introduced in previous release and reverted in this one.

================================================================================
			  ME Changes in 03.00.05.068
================================================================================   
- Fixed: "Firmware Update In Progress¡± bit does not set in FW Status register
         during online update.
- Fixed: ME-BIOS Interface major and minor version swapped on EFI and DOS.
- Fixed: The Mode Manager does not support reading power from HSC, when the 
         LM25066i chip is used.
- Fixed: After ME reset (Cold Reset command, or any host reset in S0/S1 Only power
         mode except host warm reset) ME returns incorrect version and CRC of mPhy
         settings (0). This causes the BIOS to perform (unnecessary) mPhy settings 
         update in ME, which gets rejected with 0x101E error code while it should
         be accepted.
- Fixed: Sporadically on some platforms ME may be reset during host booting due
         to internal exception.
- Fixed: ¡°Read mPhy settings¡± HECI message returns ICC_STATUS_FAILURE (0x0001)
         in ¡°ICC Status¡± field.
- Fixed: PCH register SECRT98 (SATA Electrical Control Register T98) has improper
         value due to incorrect mPhy settings value in ME. As a workaround the BIOS 
         may force update of these settings during boot.
================================================================================
			  ME Changes in 03.00.04.209
================================================================================   
- Fixed: Disabling spectrum spread with ICC_SET_SPREAD_SPECTRUM message over HECI
         causes the BIOS to hang.
- Fixed: When PSU Status sensors are disabled and one of the PSUs gets disconnected
         from AC, ME resets due to exception, causing SPS FW Health sensor 0x17 event
         to be stored in the BMC SEL.
- Fixed: When Factory Defaults are restored using IPMI command, there is incorrect
         SPS FW Health sensor 0x17 event sent to the BMC SEL.
- Fixed: Sometimes Dynamic Core Allocation temporarily parks cores in unexpected
- Fixed: Sometimes aggressive power policy in Domain Total is not able to limit 
         power in specified correction time.


===============================================================================
                               BMC Changes in 01.13.8619:
===============================================================================
- Fixed: CPU CATERR occurs after sending peci command IA32_MC10_CTL and 
       IA32_MC10_CTL2. 
                               BMC Changes in 01.13.7782:
===============================================================================
- Fixed:  [x]Axacore report Rainbow Pass board takes 5+ minutes to boot.  Seems
          to have something to do with initialization of the BMC at startup.
- Fixed:  The content of "About" button is still in English when using the 
          Chinese Browser.
- Fixed:  FWPIAUPD_v13.1.3:Can’t upgrade BMC to the same version with “No down rev?
          parameter on Denlow
- Fixed:  RMM4 dedicated NIC on the S2600WP may no responding after disabled 
          onboard NIC around 2 hours
- Fixed:  After insert the IHC certificate file,get session id always failed.
- Fixed:  EWS login failed during run DC cycle with ITAS.
- Fixed:  The response of "Get DIMM Information" is wrong.
- Fixed:  "syscfg /cr rank "2 1" " does not take effect on S1200RP.
- Fixed:  the copyright's timestamp and sign shown in KVM window's help menu is 
          incorrect.
- Fixed:  The copyright duration shown in EWS's "About" information is incorrect.
- Upgrade OpenSSL to 0.9.8zf.

===============================================================================
                                BMC Changes in 01.12.6784:
===============================================================================
- Fixed:  Can't get the last entry when bmc event log is 100%
- Fixed:  FW update will fail with OS based utility (OFU), failure rate is 20% 
          with USB mode and 40% with KCS mode.
- Fixed:  Sometimes FRB2 will be triggered after resuming from S3.
- Fixed:  IPv6 can't get IP address via DHCP server.
- Fixed:  After turning off then turning on the KVM/SSH/EWS/IPMI over lan 
          services using Control BMC Services command, IPMI over lan service
	  was still available.
- Fixed:  In the EWS page "Security Settings", when click the "Enable" label of 
          "SSH", "HTTP/HTTPS" and "IPMI over LAN", it will disable or enable the 
	  "Force HTTPS" option.
- Fixed:  There are assert and de-assert events logged for sensor HDD Status -
          Device Faulty during DC cycle stress test.
- Fixed:  There'll be a warning message for SEL is full after force update BMC
- Fixed:  There's no SEL indicate the FW has been updated successfully when update BMC.
- Fixed:  The SEL log event ID began at 512 the rather than starting from 1.
- Fixed:  SEL log Timestamp message incorrect after AC cycle or BMC reset.
- Fixed:  Updated to newer Openssl code version 0.9.8za .
===============================================================================
                                BMC Changes in 01.11.5801:
===============================================================================
- Fixed: Updated Java Signatures files in BMC to support requirement changes of JAVA

===============================================================================
                                BMC Changes in 01.10.5637
===============================================================================
- Fixed: The BMC may corrupt within 10 DC cycles on the Intel(R) Server board S1200V3RPM.

===============================================================================
                                BMC Changes in 01.08.5091
===============================================================================
- Fixed: No video display in BMC KVM console when SUT wakes up from S1 or S3
         in Win2012.
	
===============================================================================
                                BMC Changes in 01.07.5021
===============================================================================
- Fixed: After a BMC reset or BMC update a BMC watchdog SEL event is logged and
         system will be in degraded state. Status LED will be green blinking.

===============================================================================
                                BMC Changes in 01.06.4994
===============================================================================
- Fixed: Update SDR of S1200RP to version 1.05.
- Fixed: BMC update failing after 4 consecutive firmware updates.
         BMC will no longer stay in recovery mode (uboot) after four
         consecutive firmware updates.
- Fixed: Repeated Pwr Unit Redund warning SEL entries when AC power removed
         from either PS1 or PS2.
- Fixed: Corrected Embedded Web Server help text for Serial Over LAN
- Fixed: Updated Embedded Web Console Mouse Mode text
- Fixed: JViewer always shows "Error reading video data" popup and a black
         screen when mouse mode is set to relative and JViewer tries to hide
         the cursor.
- Fixed: The UBoot code detects a bad CRC of the Ram Image when attempting to
         boot after getting a cold reset.

===============================================================================
                               BMC Changes in 01.05.4775
===============================================================================
-Fixed: Change Intel(R)RMM in EWS into RMM Dedicated Mgmt.
-Fixed: The LCD Screen display is not clear while scrolling error events.
-Fixed: LAN leash lost event is shown during DC cycle testing.
-Fixed: Px DIMM Thrm Mrgn and Px DIMM Thrm Trip not decoding DIMM number
        correctly in the Embedded Web Server SEL text log.
-Fixed: Embedded Web Server SEL text log not decoding BIOS update versions
        correctly.
-Fixed: There are assert events for Mem Err Sensor 0x28 - 'DIMM Thrm Mrgn 1'
        sensor and 'SPS FW Health' sensor after updating ME firmware.


===============================================================================
                                BMC Changes in 01.04.4674
===============================================================================
-Fixed: Update SDR to version 1.04.
-Fixed: The BMC version information not displaying as expected in Embedded Web
        Server after entering firmware transfer mode..
-Fixed: The host power status show inconsistently betweeen system information
        page and server power control page in Embedded Web Server when system
        is in S1 or S3.
-Fixed: There are assert and deassert events logged for PCH temp sensor 0x22 -
        low critical and low non-critical during DC cycle stress test.
-Fixed: System status LED is incorrect and there is no assert event logged for
        DIMM thermal trip after DIMM thermal trip is triggered.
-Fixed: Multiple KVM socket error and media redirection errors.
-Fixed: Integrated BMC Web Console Keyboard Macro Cltrl+Alt+F1 not working as expected.

===============================================================================
                                BMC Changes in 01.03.4595
===============================================================================
-Fixed: Update SDR to version 1.03.
-Fixed: RGMII signal integrity test failed on S1200RP.
-Fixed: BMC shared NIC cannot be pinged successfully after BMC shared NIC IP
        address is set in BIOS setup.
-Fixed: The Web Console Event Log page uses IBMC.

===============================================================================
                                BMC Changes in 01.02.4452
===============================================================================
-Fixed: Update SDR to version 1.02.
-Fixed: DIMM margin resolution isn't right when saving DIMM inventory into
        extend SEL.
-Fixed: There are four BIOS recovery boot entries in the SEL for a recovery
        boot,only two are expected.
-Fixed: When recovery jumper is connected to 1-2 pin(normal mode), system
        always boots from recovery mode after programming a new BIOS offline.
-Fixed: BMC shared NIC cannot be pinged successfully after run VLAN id set/get
        stress test from VLAN id 0 to 4094.
-Fixed: Source of DIMM event does not show in the SEL extended data.

===============================================================================
                                BMC Changes in 01.01.4412
===============================================================================
-Fixed: Update SDR to version 1.01.

-Fixed: Change resolution of DIMM temp sensor reading.
-Fixed: SUT is reset even when the timer action is "none" after getting a
        Watchdog timeout.
-Fixed: Sensor reading/state for DIMM Thermal Margin 1 is unavailable.
-Fixed: Fail to generate system debug log in Embedded Web Server.
        - Refreshing the page shows the debug log is available
-Fixed: Embedded Web Server Power Policy numbers cannot be set to 255. Per the
        help information 255 should be valid.
-Fixed: There are unnecessary event logged for sensor Voltage BB +5.0V STBY
        (#0xD3) lower non-critical during AC cycle test.
-Fixed: Message shows as "undefined" with ff in Embedded Web Server SEL page
        when SEL is full.
-Fixed: Intel(R) Hybrid Cloud cannot get session ID when use BMC
        username/password with special characters.

================================================================================
				BMC Changes in Release 00.14.4348
================================================================================
01.00.4348:
- Count of currently enabled users still is changed even failed to enable users without 
 name setting with command "set user access".
- Wrong completion code returned by issuing "Get DIMM information" IPMI OEM command.
- Failed to check the timer Interrupt-Action Interaction when settting pre-interrupt as NMI.
- Lan configuration information and User configuration information change to default value

 after updating BMC FW ver:00.19.4290.
===============================================================================
                          BMC Changes in Release R0014
===============================================================================
- Initial Version
===============================================================================
                           FRUSDR Changes in release 1.08
===============================================================================
 - Fixed-The sensor reading of P1 MTT is always 0 in EWS(Intel(R) Integrated BMC Web Console)

=============================================================================
                           FRUSDR Changes in release 1.07
=============================================================================
 - Update system Fan1 to FSC domain2, system Fan2 to domain0 in other chassis to align with schematic.

=============================================================================
                           FRUSDR Changes in release 1.06
=============================================================================
 - update FRUSDR utility to 12.0 build5
=============================================================================
                           FRUSDR Changes in release 1.05
=============================================================================
 - Sensor 0xc0 name is inconsistent between EWS and EPS.

=============================================================================
                           FRUSDR Changes in release 1.04
=============================================================================
 - Fixed the issue of System status LED show green blinking when unplug the front panel

===============================================================================
			   FRUSDR Changes in release 1.03
===============================================================================
- Initial version

=============================================================================
                            LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products. 
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation may 
have patents or pending patent applications, trademarks, copyrights, or other 
intellectual property rights that relate to the presented subject matter.  
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any 
such patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product 
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 
*Other names and brands are the property of their respective owners.
Copyright (c) 2013 Intel Corporation.

A portion of this firmware is open source code, which falls under the
GPL 2.0 license.  

[END OF RELEASE NOTES]
