================================================================================
Intel(R) Server Board S2600TP Product Family and Intel(R) Compute Module HNS2600TP Product Family Firmware Update Package 
for Intel(R) Deployment Assistant, Intel(R) One Boot Flash Update Utility,
Windows* Preboot Execution Environment 
================================================================================
Intel Enterprise Platform & Services Division - Marketing
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================
DATE    : 	Sept. 17, 2015
TO      : 	Intel(R) Server Board S2600KP Product Family and Intel(R) Compute Module HNS2600KP 
                   Product Family customers
SUBJECT : Release Notes for System Firmware Update Package 
================================================================================
                              ABOUT THIS RELEASE
================================================================================
BIOS:     	01.01.0009
ME:        	03.00.07.168
BMC:     	01.35.9065
FRUSDR:	    1.09
================================================================================
                           Support Platforms and Dependency
================================================================================
Processors supported: 
Intel(R) Xeon processor E5-2600 v3 series

Microcode update versions:
Intel(R) Xeon(R) processor E5-2600 V3 series C0/C1 stepping: 0x0000002E CPUID = 0x306f2

Production boards:
  Product		Fab Version	      
  S2600TP		Fab3 (PBA# -350) or above    
  S2600TPF	    Fab3 (PBA# -350) or above 

The following update process must be followed to ensure a trouble free update.
1.	BMC firmware
2.	BIOS
3.	Manageability Engine (ME) firmware
4.	FRUSDR

================================================================================
                  System Firmware Update Package Usage instructions                   
================================================================================
This package can be updated using one of the following methods:
 - Intel(R) Deployment Assistant
 - Windows* or Linux* operating system using Intel(R) One-boot Flash Update (OFU)
   V11.0 Build 14 or later)
 - Windows* Preboot Execution Environment (WinPE)

To Update from Intel(R) Deployment Assistant (IDA)

The Intel(R) Deployment Assistant software is easy to use and is present on the 
"Intel(R) Server Deployment & Management" DVD shipped with the system.
User can download the latest version IDA CD ISO image from http://downloadcenter.intel.com/
To use the IDA CD to update the system firmware:
- Boot server with IDA CD
- Select "Get System Updates" 
- Choose one of the three options 

  . From http://www.intel.com/support/
    Automatically downloads the latest Firmware Update Package from Intel 
    Requires Internet connection
    Enter your local IP address and proxy configuration
    Click "Next" to start the download and update process

  . From my network
    Download the latest Firmware Update Package from http://downloadcenter.intel.com/ and copy 
    it to a Windows* shared folder
    Enter your local IP address, the Windows* file server name, and a
    Windows user name and password
    Select the firmware package in pop-up window
    Click "Next" to start the update process

  . From USB flash drive or Hard Disk
    Download the latest Firmware Update Package from http://downloadcenter.intel.com/ and copy it 
    to a USB flash drive, then insert the USB flash drive into the server USB port
    Click "Browse"
    Select the firmware package in pop-up window
    Click "Next" to start the update process
    
  Note: 1) The Firmware Update Package is in the ZIP file format. Do not unzip 
        before copying to a Windows* shared folder or USB flash drive.
	2) The IDA will always update backup bios with this FSUP package even if the IDA backup bios check box is not selected.

To update from Windows* and Linux* or operating systems using the Intel(R) One Boot
Flash Update Utility (OFU)

Intel(R) One boot Flash Update utility can be downloaded from http://downloadcenter.intel.com/
and it is part of the "BIOS, Firmware Update & Configuration Utilities" for 
Windows* and Linux*. Please refer to Intel OFU user guide about the details of 
installation and usage of OFU.

Use OFU to update system firmware by the following steps:
- Install OFU on Windows* or Linux* system
- Download the latest firmware update package from http://downloadcenter.intel.com/
- Unzip package to a folder
- Run the following command in Windows* command line/Linux* terminal window:
  <OFU install folder name>:\flashupdt -u  <package folder name>\flashupdt.cfg
                       
To update from Windows* Preboot Execution Environment (WinPE)

The System Firmware Update Package can be inserted to Windows* PE customized image 
for creating a bootable Windows* PE CD. User is able to update system firmware from 
customized WinPE CD by the following steps:
- Boot server with customized WinPE CD
- Run script "WinPE21_x64_Update.bat" or "WinPE20_x86_Update.bat" 
  (name may be varied depends on your own customization)
  
Note:
1. The Intel(R) OFU utility is case sensitive. Therefore, when you transfer the 
Firmware Update Package using USB flash drive from a Microsoft Windows* system to a Linux
environment, you must first extract under the Linux* environment. Otherwise, you 
will need to mount the USB flash drive manually with 'vfat' option under Linux to avoid 
conversion from upper case to lower case and vice versa.

2. To make Intel(R) OFU utility run properly under x86 or x64 OS, you have to read
OFU release notes on known issues for OFU installation.

3. In this SFUP package, Intel only provide batch file "WinPE_x86_Update.bat"
for WinPE2.0 32 bit solution "WinPE_x64_Update.bat" for WinPE2.1/3.0 64 bit 
solution as an example. Please refer to white paper "White Paper-Intel Server 
Utilities Procedure for WinPE.pdf" for details on building your own customized 
WinPE CD.

4. Windows PE 2.0 - built from Windows Vista SP1 32bit or EM64T
5. Windows PE 2.1 - built from Windows Vista SP1 or Windows Server 2008, EM64T
6. Windows PE 3.1 - built from Windows Server 2008R2, EM64T
7. Microsoft IPMI driver is loaded by default from WinPE CD, if you want to use 
Intel IPMI driver instead of MS IPMI driver for firmware update, you can un-install
Microsoft IPMI driver by:
                Devicesetup.exe ¨Cv remove *IPI0001
                Note: IPI0001 is the device ID for Microsoft IPMI driver.
8. If to update backup BIOS region or NVRAM, you need to customize the OFU update 
       scripts (eg.flashupdt.cfg) and add "UpdateBackupBios" or "UpdateNvram" parameter.
 
================================================================================
				BIOS 01.01.0009
================================================================================
- Fixed   ME status show "Not Ready" in SETUP(MFG mode).
- Fixed   HII - Day information hard coded to always 'Thu' irrespective
                of date we save in Schedule CC page
- Fixed   System intermittently reboots due to watchdog timer failure.
- Fixed   The description for "boot mode" under advanced controller
                property gets truncated
- Fixed   Set Boot Mode=UEFI via ITK,"Launch EFI Shell" will disappear.
- Fixed   No video signal when enable ESRT2 UEFI BIOS and Emulex 16002B.
- Fixed   Sysinfo_v13.1.6:some BIOS options should not displayed
                "Possible Values" in sysinfo_log.txt.
- Fixed   Cannot enter BIOS setup after enabling serial console redirection
                for serial port B
- Fixed   [E5-16xx] Wrong "Memory Array Handle" mapping cause SMBIOS Type
                16/17/19/20 has wrong structure.
- Fixed   "Intel Embedded Server RAID Technology 2" OpROM not show in BIOS
- Fixed   [E5-16xx] Trigger MBE at channel A1 will get wrong sel log.
- Fixed   BSOD under Windows* 2012 R2 when hot plugging NVMe SSD drives
- Fixed   Pressing multiple F6 from SOL skips through boot manager.
- Fixed   BMC DHCP HOST NAME can not be changed if DMN is DYNAMIC and BMC
- Fixed  HW RAID HII: Arrow listing is not displayed correctly when lines
- Fixed  Help to integrate the LAN OPROM20 oprom.
- Fixed  System sporadically hangs at post code 0x89
- Fixed  [24HDD] The value of OEMID at ACPI table is not expected value.
- Fixed   No Error Message display when boot into unsigned OS with secure
                boot enable
- Fixed   ME status error with ME force update jumper
- Fixed   SUT will get IERR event when enable secure boot via ITK or Syscfg.
- Fixed   Windows2012R2 reboot cycle failed.
- Fixed   [S2600WT] System locks up during OS DC cycling test
- Fixed   Conflict message in Linux when serial port A is set as 0x2f8 and IRQ3
- Fixed   After change "Active Processor Cores" , then press F10 to save Setup
                menu, it will pop up a fail screen as picture.
- Fixed   Memory speed changes when POR setting is disabled and with a specific
                CPU - 3 DIMMS per channel

================================================================================
                            ME 03.00.07.168
================================================================================
- If host main power delayed relatively to the standby power for 720-770ms ME stop responding.
- Unable to set Alert Threshold Limit to 0 degrees (minimum from capabilities) for Inlet Temperature Trigger Type Policy. 
- During Host Warm Reset flow, unexpected Intel® SPS 3.0 E5 Firmware exception may be promoted to Platform Global Reset. 
- When auto configuration is performed and efficiency readings are provided from BMC, ME keeps requesting PSUs for readings.
- NMPTU Get NM Capabilities updated to invalid values.

===============================================================================
                             BMC 01.35.9065
===============================================================================
-Fixed the issue of BMC may record HDD1 and HDD2 Presence event even no HDDs are installed
-Fixed the issue of the 12GB bridge board temperature sensor no longer seen after using
FW 01.28.8586

================================================================================
                             FRUSDR 1.09
================================================================================    
- Fixed the issue of fan speed cannot be changed with the PWM offset value in BIOS 
configuration interface if chassis type is set as "Other" when loading FRUSDR


=============================================================================
                            LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products. 
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation may 
have patents or pending patent applications, trademarks, copyrights, or other 
intellectual property rights that relate to the presented subject matter.  
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any 
such patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product 
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 
*Other names and brands are the property of their respective owners.
Copyright (c) 2014 Intel Corporation.

A portion of this firmware is open source code, which falls under the
GPL 2.0 license.  

[END OF RELEASE NOTES]
