This release note and the software that accompanies it are copyright (c) 2015, Intel Corporation or its suppliers, and may only be installed and used in accordance with the license that accompanies the software.

This Software is furnished under license and may only be used or copied in accordance with the terms of that license. No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. The Software is subject to change without notice, and should not be construed as a commitment by Intel Corporation or its suppliers to market, license, sell or support any product or technology. Unless otherwise provided for in the license under which this Software is provided, the Software is provided AS IS, with no warranties of any kind, express or implied. Except as expressly permitted by the Software license, neither Intel Corporation nor its suppliers assumes any responsibility or liability for any errors or inaccuracies that may appear herein. Except as expressly permitted by the Software license, no part of the Software may be reproduced, stored in a retrieval system, transmitted in any form, or distributed by any means without the express written consent of Intel Corporation.

==========================
Supported RAID Controllers
==========================
This download supports Intel(R) RAID controllers using MR software stack (RMS3CC080, RMS3CC040, RS3MC044, RS3SC008, RS3DC080, RS3DC040), please verify that this utility has been tested with the RAID card you have chosen to use by checking the drivers web page for your controller at http://support.intel.com.


===================
Package Information
===================
Flash package = v24.10.0-0020


==========
Attention!
==========
Intel recommends to loading Factory Default setting after the firmware upgrade which will not affect data on any existing array. To do so:
1. Reboot the system and login to the RAID BIOS Console. 
2. Select the controller and select 'Adapter Properties'->'Next'
3. Set the 'Set Factory Defaults' setting to 'Yes' and submit the change.
4. Reboot the system (the default settings are applied).
5. Re-configure to the desired settings in RAID Web Console2.

---------------------------------------
Firmware downgrade notice
---------------------------------------
Intel does not recommend to downgrade the factory installed firmware on your RAID module or controller, it has important enhancements and bug fixes you may lose when going to a previous version.
If you need to install an older firmware version, please contact Intel for instructions on how to perform this action.


==================
Known Restrictions
==================
1) This download does NOT support EFI v1.1 environment. Please use the EFI shell command “ver" which will display the EFI version, to identify the EFI version.
2) When 2 or more VDs are created, VD cache settings must be the same.

**************************************************************************************************************************
***********PLEASE READ BEFORE DOWNGRADING FROM THIS FIRMWARE VERSION TO ANY PRIOR FIRMWARE VERSION************************
**************************************************************************************************************************
Online Firmware Update should not be performed when downgrading from this release to a prior release.  Please refer to the 240_VD_Feature_Limitations_Known_Issues_Addendum_v1.0.pdf document included with this package for additional details.
**************************************************************************************************************************
**************************************************************************************************************************


=======================
Contents on the package 
=======================
The following files are included in this zip:

Name:						Description:
COPYING.NEWLIB.txt				License Agreement
3108-MR_FWPKG_v24.10.0-0020_Readme.txt		This file
MR69p.rom					Firmware binary
License_v2.pdf					License Agreement
update.nsh					UEFI firmware update batch file
StorCLI\*					StorCLI CLI tool for various Operating Systems


==========================
Installation instructions:
==========================

UEFI shell instructions for updating RAID Firmware:
-----------------
   1. Download and extract all files to a USB flash drive.
   2. Boot the target system to EFI shell. 
   3. Change directory to the local drive and directory containing the flash update files and the firmware image file.
   4. Type "update.nsh" and press <Enter> to execute the command
   5. Wait for the flash to complete. Do NOT reboot the system during the update.

You can also use RAID Web Console 2 or OS version of StorCLI to update the RAID firmware.  For more detail, please refer to the Intel(R) RAID Software User's Guide.

=============================
Package Details/Fixes/Updates 
=============================
Version Numbers:	
===============
Firmware Package:24.10.0-0020 (MR 6.9 P1)
	Firmware 4.600.00-4907
		SCGCQ00864348 - (Closed) - Unexpected AEN of aborting Init During Firmware Down/upgrade
		SCGCQ00894719 - (Closed) - Reconstruction error message "invalid arguments"
		SCGCQ00898140 - (Closed) - Code changes to be made under specific macro for a feature
		SCGCQ00898564 - (Closed) - MSM shows "null x0" to describe port connection to enclosure when multipath is broken
		SCGCQ00900237 - (Closed) - Created VD configuration with PDs released from previous VD erased will lost after next reboot
		SCGCQ00901889 - (Closed) - A hidden VD can be configured as bootdrive
		SCGCQ00901919 - (Closed) - hot remove then hot add of drive in array causes BSOD
		SCGCQ00906997 - (Closed) - forceCacheFlush check was added inappropriately in flush_cache() function
		SCGCQ00907673 - (Closed) - Handling the DIF errors identified by BLADE DMA.
		SCGCQ00908165 - (Closed) - Firmware logs event MR_EVT_CTRL_PR_PROP_CHANGED twice.
		SCGCQ00908885 - (Closed) - Random Write perf drop up to %30 in 2R1 WB RA DCD 
		SCGCQ00910433 - (Closed) - HDD LED state indicating Ready-To-Remove is affected by Locate LED on/off
		SCGCQ00913426 - (Closed) - Controller hits MonTask: line 1278 in file ../../raid/1078dma.c after importing PD's with pinned cache
		SCGCQ00914515 - (Closed) - Make sure boot target ID is in valid range
		SCGCQ00916037 - (Closed) - Controller encountered fatal error and was reset during IO and Drive Pull
		SCGCQ00919487 - (Closed) - Handle recon allowed Operation in Firmware
		SCGCQ00925394 - (Closed) - Native config come up as foreign during FW upgrade from non-240 VD FW to 240VD FW.
		SCGCQ00925640 - (Closed) - Set factory default does not reset the modified phy link speed
		SCGCQ00927792 - (Closed) - Particular Drive not discovered in MR6.8, but MR6.7 works fine.
		SCGCQ00928506 - (Closed) - StorCLI show all command triggers datastore disconnect on 3 R5 VD VMware ESXi
		SCGCQ00928699 - (Closed) - Unexpected AEN "Warning Error during boot - Configuration command was not committed, please retry"
		SCGCQ00930593 - Wrong MFI_STAT was returned in PdDcmdSysPdMapAbort()
		SCGCQ00945033 - (Closed) - Add Flush in LdInitPdDone
		SCGCQ00880907 - (Closed) - MR Controller reported fatal error and reset while creating 240 VD
		SCGCQ00883996 - (Closed) - StorCLI/StorCLIO allows to Hide boot drive which is already in Hidden State.
		SCGCQ00890968 - (Closed) - R6 Stays Enabled on TFM
		SCGCQ00904616 - (Closed) - Fails to downgrade hba fw
		SCGCQ00904833 - (Closed) - OOB SLT not displaying Show Configuration Summary for 240 VDs created
		SCGCQ00907123 - (Closed) - CtrlH will halt(no responding) at the end of erase When perform VD erase and delete VD on the 2 VDs simultaneous
		SCGCQ00923103 - (Closed) - Remove environment string for large IO support
		SCGCQ00889734 - (Closed) - StorCLI/StorCLIO allows to Hide drive which is already in Hidden State
		SCGCQ00893368 - (Closed) - Cachecade related 240VD checks needs to account for controller property settings.
		SCGCQ00904466 - (Closed) - MSM shows messages with Error code 240 and no description
		SCGCQ00883612 - (Closed) - Enable sgpioSmpPresenceDetect for all Invader based OEM controllers.
		SCGCQ00935706 - (Closed) - Support Single Write for 4GB 3108 ROMB Design using 8GB Ptolemy for an OEM (MR FW)
		SCGCQ00917409 - (Closed) - MR 6.8: Integrating PL 08.00.09.00 to MR 6.8
		SCGCQ00916738 - (Closed) - MR 6.7: Integrating PL 07.00.10.00 to MR 6.7
		SCGCQ00915869 - (Closed) - Block upgrade and downgrade Firmware when reconstruction is in progress
		SCGCQ00903649 - (Closed) - Support locate bit for locate LED on/off on JBOD PD
		SCGCQ00886938 - (Closed) - when multiple VDs are present VD reconstruction fails, but throws the error message "invalid arguments" in storCLI
		SCGCQ00833849 - (Port_Complete) - FW hung at LogInit: Flushing events from previous boot while running policy change script of Vd and learn cycles.
		SCGCQ00833850 - (Port_Complete) - FW hung at LogInit: Flushing events from previous boot while running policy change script of Vd and learn cycles.
		SCGCQ00833852 - (Port_Complete) - FW hung at LogInit: Flushing events from previous boot while running policy change script of Vd and learn cycles.
		SCGCQ00849554 - (Port_Complete) - Unexpected controller reset during test run
		SCGCQ00876061 - (Port_Complete) - FW hits to MonTask: line 4946 in file ../../raid/ld.c while multipath push pull with patrol read
		SCGCQ00876102 - (Active) - 'Watchdog Timer Exception' followed by FW crash after initiating PD Erase on UG PD, with BG operation & IO's on 64 VD's
		SCGCQ00877435 - (Port_Complete) - Recon VD made "degraded" when the recon pd is pulled out allowing for rebuild once the drive is plugged back in.
		SCGCQ00880776 - (Port_Complete) - Foreign config is not allowed to be cleared if there is preserved cache
		SCGCQ00880870 - (Port_Complete) - MR 6.6.3 "storcli /c0 show all" shows lot of bad block messages in the log
		SCGCQ00880875 - (Port_Complete) - Do not automatically assign boot VD by default
		SCGCQ00880877 - (Port_Complete) - Support Zone Out functionality for OEM expanders
		SCGCQ00880878 - (Port_Complete) - Megaraid Thunderbolt controller reports cache memory size as 0 when no logical drives are present.
		SCGCQ00880880 - (Port_Complete) - StorCli to Message Hide Boot VD User Operation Status correctly
		SCGCQ00882931 - (Port_Complete) - Fault LED behavior in OEM Blades
		SCGCQ00883500 - (Port_Complete) - MonTask after Initiating a Raid Level migration
		SCGCQ00885571 - (Port_Complete) - Windows BSOD when upgrade FW 24.6.0-0040 to 24.8.0-0026 with driver 6.707.08.00
		SCGCQ00885733 - (Port_Complete) - StorCLI/StorCLIO allows to Hide boot drive which is already in Hidden State.
		SCGCQ00885734 - (Port_Complete) - StorCLI/StorCLIO allows to Hide boot drive which is already in Hidden State.
		SCGCQ00886910 - (Port_Complete) - Data TLB error found while running the target reset script with multipath cable pull-push operation
		SCGCQ00889826 - (Port_Complete) - Add support for show SBR command
		SCGCQ00889922 - (Port_Complete) - FW hung at LogInit: Flushing events from previous boot while running policy change script of Vd and learn cycles.
		SCGCQ00893924 - (Port_Complete) - IO halts on JBODs with read/write error when the target drives are reset via MFI or MPT path on Linux distro
		SCGCQ00895476 - (Port_Complete) - FW breaks MonTask: line 245 in file ../../raid/1078int.c with IOs on max VD configured and BGOps
		SCGCQ00898359 - (Port_Complete) - 'Watchdog Timer Exception' followed by FW crash after initiating PD Erase on UG PD, with BG operation & IO's on 64 VD's
		SCGCQ00898397 - (Port_Complete) - Firmware does not log controller property change event for enabling/disabling 240VD feature
		SCGCQ00898473 - (Port_Complete) - Firmware breaks to montask while importing the Foreign Config.
		SCGCQ00898730 - (Port_Complete) - Core 0 exception seen while trying to import foreign configuration with pinned cache present.
		SCGCQ00898752 - (Port_Complete) - FW downgrade fails with IOs and BGops .
		SCGCQ00898758 - (Port_Complete) - Controller killed on issuing OCR from StorCLI after disabling it from OS.
		SCGCQ00898762 - (Port_Complete) - TTY log dump is not persistent for multiple boots.
		SCGCQ00898773 - (Port_Complete) - Add sanity check for iPtr and rPtr after restore is completed.
		SCGCQ00898780 - (Port_Complete) - One deletion of CCVD FW displays incorrect CCVD target id and remaining CacheCade size on the system
		SCGCQ00898790 - (Port_Complete) - sasPortNumberValid bit does not get updated in CtrlR
		SCGCQ00898808 - (Port_Not_Required) - Remove checkSysPwrStatus() and processSysPwrReturn() functions.
		SCGCQ00898880 - (Port_Complete) - Kill adapter during test run
		SCGCQ00899333 - (Port_Complete) - Controller discovery failed due to pending Boot messages, adapter at baseport not responding.
		SCGCQ00899474 - (Port_Complete) - On receiving CACHE_FLUSH_DCMD, set forceCacheflush flag to 1 to flush the cache
		SCGCQ00904475 - (Port_Complete) - Unexpcted AEN of aborting Init During Firmware Down/upgrade
		SCGCQ00905418 - (Port_Complete) - Controller encountered fatal error and was reset under heavy IOs and background operations.
		SCGCQ00905782 - (Port_Complete) - FW breaks MonTask: line 245 in file ../../raid/1078int.c with IOs on max VD configured and BGOps
		SCGCQ00907679 - (Port_Complete) - on creating 240VD and rebooting the server, FW breaks into montask.
		SCGCQ00907680 - (Port_Complete) - on creating 240VD and rebooting the server, FW breaks into montask.
		SCGCQ00907682 - (Port_Complete) - LUID gets changed during foreign import from non-240VD FW to 240VD FW
		SCGCQ00908903 - (Port_Complete) - LUID gets changed during foreign import from non-240VD FW to 240VD FW
		SCGCQ00909037 - (Port_Complete) - fails to downgrade hba fw
		SCGCQ00910375 - (Port_Complete) - OOB SLT not displaying Show Configuration Summary for 240 VDs created
		SCGCQ00910389 - (Port_Complete) - Firmware logs event MR_EVT_CTRL_PR_PROP_CHANGED twice.
		SCGCQ00910569 - (Port_Complete) - After reboot imported 4K drive R0 is not visible
		SCGCQ00911211 - (Port_Complete) - Created VD configuration with PDs released from previous VD erased will lost after next reboot
		SCGCQ00911213 - (Port_Complete) - Created VD configuration with PDs released from previous VD erased will lost after next reboot
		SCGCQ00911215 - (Port_Complete) - Created VD configuration with PDs released from previous VD erased will lost after next reboot
		SCGCQ00911773 - (Port_Complete) - Handling Functional Level Reset (FLR) .
		SCGCQ00911790 - (Active) - Reduce Command Block Latency during Background Operations
		SCGCQ00922541 - (Port_Complete) - Importing 240 VD foreign configuration leads to FW Crash
		SCGCQ00922542 - (Port_Complete) - as been observed that the firmware retires the FPIO timed out IOs for 3 times instead of the reduced count to
		SCGCQ00922716 - (Port_Complete) - Controller encountered fatal error and was reset under heavy IOs and background operations.
		SCGCQ00923113 - (Port_Complete) - hot remove then hot add of drive in array causes BSOD
		SCGCQ00923405 - (Port_Complete) - Configuration creation on Controller fails after creation of a CC VD followed by JBOD creation.
		SCGCQ00929473 - (Port_Complete) - Handling the DIF errors identified by BLADE DMA.
		SCGCQ00934617 - (Port_Complete) - RAID 10 PI error message "SAS core detected EEDP error in application tag".
		SCGCQ00934619 - (Port_Complete) - CRC mismatch and invalid log event found while querying for Controller properties and learn cycle in parallel.
		SCGCQ00934711 - (Port_Complete) - CtrlH will halt(no responding) at the end of erase When perform VD erase and delete VD on the 2 VDs simultaneous
		SCGCQ00873095 - (Port_Complete) - FW allows CCVD deletion with pinned windows
		SCGCQ00873096 - (Port_Complete) - FW allows CCVD deletion with pinned windows
		SCGCQ00880876 - (Port_Complete) - Support Zone In functionality for OEM expanders
		SCGCQ00883175 - (Port_Complete) - Consistency Check running under high I/O load causing VMWare DataStore disconnect on RAID 5 VDs
		SCGCQ00898761 - (Port_Complete) - FW breaks MonTask: line 245 in file ../../raid/1078int.c with IOs on max VD configured and BGOps
		SCGCQ00899818 - (Port_Complete) - MonTask: line 1280 in file ../../raid/1078dma.c. DCDB cmd timed out
		SCGCQ00905494 - (Port_Complete) - fails to downgrade hba fw
		SCGCQ00906991 - (Port_Complete) - On receiving CACHE_FLUSH_DCMD, set forceCacheflush flag to 1 to flush the cache
		SCGCQ00908347 - (Port_Complete) - Copyback fails to start and causes a FW fault
		SCGCQ00908894 - (Port_Complete) - LUID gets changed during foreign import from non-240VD FW to 240VD FW
		SCGCQ00908904 - (Port_Complete) - on creating 240VD and rebooting the server, FW breaks into montask.
		SCGCQ00914742 - (Port_Complete) - Medium error correction events were not reported
		SCGCQ00917202 - (Active) - During long run reboot test, FW eventually reports "Disabling writes to flash due to a critical error"
		SCGCQ00922595 - (Port_Complete) - Cachecade related 240VD checks needs to account for controller property settings.
		SCGCQ00923292 - (Port_Complete) - Remove environment string for large IO support
		SCGCQ00929474 - (Port_Complete) - Controller encountered fatal error and was reset during IO and Drive Pull
		SCGCQ00880864 - (Port_Complete) - StorCLI reports success on 4MB MR flash on iMR which fails after reset - (SCGCQ00870439)
		SCGCQ00880872 - (Port_Complete) - Disable FLR support in MR FW to address VMware guest VM abrupt shutdown issue
		SCGCQ00881276 - (Port_Complete) - Megaraid_sas driver fails to communicate with the FW and fails to discover any disks attached
		SCGCQ00885732 - (Port_Complete) - StorCLI/StorCLIO allows to Hide boot drive which is already in Hidden State.
		SCGCQ00911685 - (Active) - wave4scrum pdisk state remains as ready even after creating a vdisk on that
		SCGCQ00942794 - (Port_Complete) - Chaos report DC after rebuild complete on R6 with SAS SSD
		SCGCQ00880866 - (Port_Complete) - Handling NVRAM migration for Patrol Read
		SCGCQ00833851 - (Port_Complete) - FW hung at LogInit: Flushing events from previous boot while running policy change script of Vd and learn cycles.
		SCGCQ00922681 - (Port_Complete) - Sanity check for handling the cases where event length comes up as zero/ rPtr goes beyond iptr
	NVDATA  3.1508.00-0009
		Numerous changes for specific customers
	Hii 03.17.14.01(signed)
		SCGCQ00932071 - (Port_Complete) - Inconsistency across apps for retention time in HII.
		SCGCQ00914259 - (Port_Complete) - HII Dashboard doesn't refresh enclosure and drive counter when an enclosure with foreign config is disconnected
		SCGCQ00897835 - (Port_Complete) - HII Missing WB Option
		SCGCQ00905879 - (Port_Complete) - MegaRAID Firmware Information not Displayed Under IMM
		SCGCQ00932045 - (Port_Complete) - With pinned cache HII hangs while trying to enter "cache and memory" tab under advanced controller properties
		SCGCQ00932117 - (Port_Complete) - DATA TLB Error(MonTask: line 245 in file) on enabling JBOD from HII while running patrol read.
		SCGCQ00931887 - (Port_Complete) - In-correct associated drive group number showing for DHS drive
		SCGCQ00931890 - (Port_Complete) - 'Next Learn Cycle Time' & 'Learn Period' not displayed when battery supports transparent learn.
		SCGCQ00911105 - (Port_Complete) - HII Firmware Update Option
		SCGCQ00931921 - (Port_Complete) - Display NVRAM Size only if hwpresent.nvram is present
	Ctrl-R 5.13-1101
		SCGCQ00907053 - (Port_Complete) - Apply button is active in Ctrl Mgnt when traversed from Rebuild rate to BGI rate
		SCGCQ00916359 - (Port_Complete) - Manage dedicated hotspare is available for Cachecade DG and assign hotspare fails at the end
		SCGCQ00916352 - (Port_Complete) - Expand size link is enabled even though available size is 0 in Cachecade diskgroup
		SCGCQ00914214 - (Port_Complete) - Error code "Unknown" for setting hidden VD as boot VD in Ctrl-R
		SCGCQ00933861 - (Port_Complete) - CTRL-H Missing WB Option
		SCGCQ00897838 - (Port_Complete) - CTRL-H Missing WB Option
		SCGCQ00914218 - (Port_Complete) - No error message for failure of Disable SSD Caching of an offline VD
		SCGCQ00931889 - (Port_Complete) - CTRL_H showing on-board memory size when memory is not present
		SCGCQ00932144 - (Port_Complete) - storcli command shows Failure on SWR for command "storcli /c0 show all"
		SCGCQ00932043 - (Port_Complete) - 'Next Learn Cycle Time' & 'Learn Period' not displayed when battery supports transparent learn.
	ROMENV 1.09
	BootBlock 3.07.00.00-0003
	UEFI_Driver 0x06110200(signed)
	FCODE 4.17.08.00
	BIOS 6.28.04.0
	PCLI 1.07.05
Firmware Package:24.10.0-0017 (MR 6.9)
	Firmware 4.290.00-4536
		SCGCQ00718801 - (Closed) - FW breaks to MonTask: line 1168 in file ../../raid/raid.c during RAID Operations
		SCGCQ00724451 - (Closed) - FW breaks to MonTask: line 889 in file ../../raid/bladeDMA.c while creating a filesystem on R5 VD.
		SCGCQ00725844 - (Closed) - Intruder pre alpha 2 : On a R1 to R5 reconstructing Virtual Drive, IO failed with data miscompare
		SCGCQ00729599 - (Closed) - Intruder pre alpha 2 : "MonTask: line 396 in file ../../ssd/ssd_cache_fw.c" with IO on R5 VD with a CacheCade VD in WB
		SCGCQ00747258 - (Closed) - .10 PL cause DataTLB error with MR FW.
		SCGCQ00751361 - (Closed) - 512e support needs to be enabled in MR FW
		SCGCQ00788071 - (Closed) - Code review items were fixed
		SCGCQ00788072 - (Closed) - Code Review fixes for review Review #38871 -Integrate 6.5 Changes with Intruder Code stream
		SCGCQ00791766 - (Closed) - Rebase Dev stream with Integration 6.5 manual changes
		SCGCQ00794871 - (Closed) - FW breaks to MonTask: line 257 in file ../../dm/src/dmDrvPrep.c when booting FPGA
		SCGCQ00807498 - (Closed) - Data corruption detected with offload and restore operation
		SCGCQ00812867 - (Closed) - Data corruption reported with Intruder ONFI2 offload and restore operation
		SCGCQ00819772 - (Closed) - Flash wrongly discovered as transported across back to back offload and restore cycles
		SCGCQ00822311 - (Closed) - ONFI unable to offload to controllers with multiple chipselects
		SCGCQ00823817 - (Closed) - FPGA stream missing .4 release stream content
		SCGCQ00831595 - (Closed) - FW hanging with 0.6 release while bootup.
		SCGCQ00832908 - (Closed) - MSM displays error message if 'Schedule Consistency Check' is selected.
		SCGCQ00843098 - (Closed) - Un-correctable ECC error on Armstong board during cold boot
		SCGCQ00844777 - (Closed) - Modifying SBR PnP IDs offset
		SCGCQ00845435 - (Closed) - Data Corruption on WB VDs
		SCGCQ00846621 - (Closed) - Medium error correction events were not reported
		SCGCQ00848339 - (Closed) - FW hangs during cache flush after restore cache from flash.
		SCGCQ00850401 - (Closed) - ONFI: FC0 CS0 offload meta length not valid:0, expected:7c00 causing restore to not start after offload.
		SCGCQ00850839 - (Closed) - FW hangs after re-inserting SATA drive in direct connect topology during I/O.
		SCGCQ00856977 - (Closed) - Unable to update drive firmware on customer specific FDE SATA SSDs
		SCGCQ00858697 - (Closed) - For Sugon Romb dont Initialize the port activity LED's GPIO.
		SCGCQ00863880 - (Closed) - MR_6.9_FW : Core 0 exception seen while trying to import foreign configuration with pinned cache present.
		SCGCQ00864054 - (Closed) - Perform the PCI release retry while performing BISR on the second CPU.
		SCGCQ00865116 - (Closed) - ROC Temp GPIO action item
		SCGCQ00866261 - (Closed) - Invader firmware (4.280.00-4331 in MR 6.7) with write-verify has abnormal behavior/performance.
		SCGCQ00867065 - (Closed) - Increase CACHE HEADER version, since new member was added to PinnedCacheDataStructure(Persistent DRAM)
		SCGCQ00872875 - (Closed) - MR_6.9: MonTask: line 1280 in file ../../raid/1078dma.c. DCDB cmd timed out
		SCGCQ00872889 - (Closed) - MR6.9_FW : Kill adapter seen while issuing Task Management in loop on 240 JBODs with IOs.
		SCGCQ00873991 - (Closed) - Data TLB error occured after issuing task abort from host
		SCGCQ00878414 - (Closed) - 6.9 : Write perf drops in 16R5 WT NoRA DCD SS64 1MB IO at QD128/256
		SCGCQ00878432 - (Closed) - Blade DMA errors observed while running IOs
		SCGCQ00878587 - (Closed) - MonTask: line 245 in file ../../raid/1078int.c while running I/Os with 64VDs and pull out drives belonging to CacheCade VD
		SCGCQ00879193 - (Closed) - Restricting the VD deletion optimization to reduce IO freeze to least latency mode.
		SCGCQ00881001 - (Closed) - StorCLI Reports Incorrect TFM Manufacturing Date
		SCGCQ00881901 - (Closed) - FW hang, even-after Task Abort is successful on a drive in Linux OS
		SCGCQ00882125 - (Closed) - On receiving CACHE_FLUSH_DCMD, set forceCacheflush flag to 1 to flush the cache
		SCGCQ00882897 - (Closed) - Need to set perfTunerMode appropriately on controller reset.
		SCGCQ00884589 - (Closed) - Windows BSOD when upgrade FW 24.6.0-0040 to 24.8.0-0026 with driver 6.707.08.00
		SCGCQ00890133 - (Closed) - Invader 6.9: FW breaks MonTask: line 245 in file ../../raid/1078int.c with IOs on max VD configured and BGOps
		SCGCQ00891924 - (Closed) -  Buffer Size is set to 1M and number of BSB per BB is set to 1.
		SCGCQ00893588 - (Closed) - MR6.9_FW : IO halts on JBODs with read/write error when the target drives are reset via MFI or MPT path on Linux distro
		SCGCQ00895554 - (Closed) - MR_6.9_FW: Kill adapter during test run
		SCGCQ00904905 - (Resolved) - Copyback fails to start and causes a FW fault
		SCGCQ00717238 - (Closed) - MR Intruder Fault x6101 - FW breaks to Montask: line 1557 in file ../../dm/pl2/pliopi.c
		SCGCQ00738085 - (Closed) - Change flags for each sge in the sglist.
		SCGCQ00750804 - (Closed) - FW breaks to MonTask: line 299 in file ../../raid/1078int.c when try to run IO on 32 drive R0 16 VD configuration.
		SCGCQ00771238 - (Closed) - remove Cache split related changes from Int stream
		SCGCQ00788087 - (Closed) - Multi- SAS Core - Code reivew defect fixes.
		SCGCQ00788526 - (Closed) - Defect to check in code changes reported by static analysis tool for intruder
		SCGCQ00803219 - (Closed) - Data corruption when destaging pinned cache after foreign config import.
		SCGCQ00812295 - (Closed) - Back to back restore happen because flash region not toggled after a restore operation
		SCGCQ00819786 - (Closed) - FW should prepare and arm HW for second offload before starting cache flush
		SCGCQ00836031 - (Closed) - NVDATA and Controller Properties all zero
		SCGCQ00845921 - (Closed) - Development defect for Cache Offload work around.
		SCGCQ00846655 - (Closed) - Battery relearn timed out on Supercap on Armstrong board
		SCGCQ00847001 - (Closed) - MR6.6 Controller is not accessible through OOB before OS is up and running
		SCGCQ00848264 - (Closed) - Development defect for flash chip M83C workaround in Intruder
		SCGCQ00850368 - (Closed) - Firmware Faults with error code 0x22 after an OCR
		SCGCQ00855837 - (Closed) - A race condition exists while creating the flash filesystem and making the corresponding entries in NVRAM
		SCGCQ00855845 - (Closed) - Disable pause for memory offload control 1.
		SCGCQ00857181 - (Closed) - On performing back to back target reset on the same JBOD results into online controller reset(OCR)
		SCGCQ00857680 - (Closed) - MR 6.7 Point : Few test cases fail when PCIeCV tool is executed
		SCGCQ00857692 - (Closed) - MR 6.9 : Firmware allows to perform Reconstruction when Pinned Cache is present.
		SCGCQ00859850 - (Closed) - Pinned Cache lost after trigger few OCR and reboot server as result data got corrupt
		SCGCQ00860066 - (Closed) - Firmware breaks to montask while importing the Foreign Config.
		SCGCQ00860503 - (Closed) - MR 6.9 : Controller boots to OS Even when Pinned Cache is present and Boot Error handling is set to Stop on Error.
		SCGCQ00860635 - (Closed) - Firmware hang is observed when Cache Offload is interrupted by power restore.
		SCGCQ00860716 - (Closed) - Firmware allows to create more than 64 logical drives in legacy mode.
		SCGCQ00861819 - (Closed) - Address code review defects for ER SCGCQ008554
		SCGCQ00871973 - (Closed) - FW allows CCVD deletion with pinned windows
		SCGCQ00873239 - (Closed) - FW downgrade fails with IOs and BGops .
		SCGCQ00874200 - (Closed) - Re-eanbling 1MB IO support.
		SCGCQ00878554 - (Closed) - Core 0 exception in line 245 in ../../raid/1078int.c while Target reset on PDs and BG Operations in parallel
		SCGCQ00879198 - (Closed) - MR6.9_FW : Assertion failure in ../../dm/src/dmDrvPrep.c at line 836: while Cable pull push on secondary enclosure.
		SCGCQ00882742 - (Closed) - Fix coverity defects
		SCGCQ00886685 - (Closed) - Add sanity check for iPtr and rPtr after restore is completed.
		SCGCQ00894472 - (Closed) - Adjust cache thresholds appropriately after the pinned cache is generated and volumes are retained in WB mode.
		SCGCQ00894608 - (Closed) - OS become unresponsive after creating multiple sliced VD's
		SCGCQ00899762 - (Closed) - SKINNY compilation was broken after fixing SCGCQ00882125
		SCGCQ00906129 - (Closed) - Intruder : Data Corruption issue seen while running cable breaker with CCVD associated
		SCGCQ00908325 - (Closed) - Undoing the changes of CSET activity SCGCQ00803718
		SCGCQ00914740 - (Closed) - 6.9: Default values does not get picked up for un-changed controller property sharing same byte.
		SCGCQ00764924 - (Closed) - FW breaks to Montask: line 891 in file ../../raid/bladeDMA.c while creating file system on VDs.
		SCGCQ00788106 - (Closed) - Code review fixes for 33080
		SCGCQ00819441 - (Closed) - Port ONFI changes to Intruder .5 stream.
		SCGCQ00823465 - (Closed) - Reconstruction from R1 to R5 causing FW hang.
		SCGCQ00844839 - (Closed) - Armstrong board causing HP server to hang during bootup.
		SCGCQ00845436 - (Closed) - Limit the Memory size to 1GB as temp workaround to DC issue.
		SCGCQ00850220 - (Closed) - Check in OCR work around
		SCGCQ00850441 - (Closed) - iMR 6.1.1 : Exception seen during OS Reboot heat run test
		SCGCQ00850818 - (Closed) - Controller hangs during post if you have dirty cache that needs to be flushed to the VD.
		SCGCQ00851267 - (Closed) - Firmware halted after trigger OCR with I/O
		SCGCQ00852327 - (Closed) - When no drives connected tlb error is seen
		SCGCQ00853020 - (Closed) - Firmware Test API returns incorrectly that hardware is armed for offload, when supercap is bad.
		SCGCQ00855322 - (Closed) - !!! Firmware initialization failed. Fault code = 0x4 !!!
		SCGCQ00857528 - (Closed) - MR_6.8:FW hits to MonTask: line 4946 in file ../../raid/ld.c while multipath push pull with patrol read
		SCGCQ00859961 - (Closed) - Cannot disable patrol read on an Armstrong controller.
		SCGCQ00865963 - (Closed) - Too many event in firmware log : onfiHwIsOffloadSustainableStateSet onfi_status 0
		SCGCQ00872140 - (Closed) - MR6.9:'Watchdog Timer Exception' followed by FW crash after initiating PD Erase on UG PD, with BG operation & IO's on 64 VD's
		SCGCQ00873201 - (Closed) - Avoid cache FLUSH during VD Deletion to reduce IO Freeze time on other VDs
		SCGCQ00874332 - (Closed) - MR6.9_FW : FW hits montask due to a non-spinning up FDE drive, issue seen on repeated reboots.
		SCGCQ00880919 - (Closed) - MR6.9_FW : Controller discovery failed due to pending Boot messages, adapter at baseport not responding.
		SCGCQ00886351 - (Closed) - MR 6.8 : Few test cases fail when PCIeCV tool is executed
		SCGCQ00900250 - (Closed) - Send appropritate MFI status for the command which needs to be aborted
		SCGCQ00827430 - (Closed) - Loss of smart recovery blocks in a small window when switching regions
		SCGCQ00832205 - (Closed) - Development defect to fix Code Coverity issues found in Intruder 0.6 Stream.
		SCGCQ00845707 - (Closed) - MSM reports 4MB and 8MB FW image is corrupt and does not allow flashing Armstrong board.
		SCGCQ00846582 - (Closed) - SATA drives not detected in direct connect topology -MR
		SCGCQ00846657 - (Closed) - ONFI offload descriptors are not set to offload all valid DATA cache
		SCGCQ00859720 - (Closed) - On OCR or reboot, retain volumes in WB if the number of pinned buffers is less than 50% of available buffers.
		SCGCQ00859975 - (Closed) - Code review defect with 6.9 merge with Inv team
		SCGCQ00860140 - (Closed) - Coverity: fix Coverity defect 16729
		SCGCQ00874357 - (Closed) - Data TLB error occured while tring dereference invalid command ID
		SCGCQ00877673 - (Closed) - Kill adapter while running IO with Task Reset on JBODs
		SCGCQ00878923 - (Closed) - Remove PinnedCacheDataStructure totalPinnedBbs and totalPinnedBsbs update in PinCacheForLd()
		SCGCQ00881919 - (Closed) - Data TLB error found while running the target reset script with multipath cable pull-push operation
		SCGCQ00848368 - (Closed) - Armstrong Controller hangs when make JBOD from powersave PD.
		SCGCQ00848372 - (Closed) - API calls to corrupt and verify DIS on ONFI NAND flash are not available in Intruder code release
		SCGCQ00856566 - (Closed) - Code review defect with 6.9 merge with Inv team
		SCGCQ00866487 - (Closed) - MR6.9_FW : sasPortNumberValid bit does not get updated in CtrlR
		SCGCQ00867120 - (Closed) - MR6.8_FW : DISM stuck at device discovery on enclosure power cycle, Devices present with DM but not reflected in upper layers
		SCGCQ00869626 - (Closed) - Compilation Error in Invader with Intruder merged code
		SCGCQ00878097 - (Closed) - MR6.9:Assertion failure in ../../raid/cache.c at line 774, after pulling out the enclosure cable
		SCGCQ00864019 - (Closed) - One deletion of CCVD FW displays incorrect CCVD target id and remaining CacheCade size on the system
		SCGCQ00878150 - (Closed) - Controller killed on issuing OCR from StorCLI after disabling it from OS.
		SCGCQ00881005 - (Closed) - Code cleanup issues.
		SCGCQ00848321 - (Closed) - Offload starting with residual power, which corrupts metadata
		SCGCQ00849733 - (Closed) - Development defect to remove the hardcoded TFM VPD values in firmware for Intruder.
		SCGCQ00863348 - (Closed) - Remove checkSysPwrStatus() and processSysPwrReturn() functions.
		SCGCQ00866206 - (Closed) - Modify app.ld to address iopath and dramCode region overflow - MR 6.9Intruder
		SCGCQ00869060 - (Closed) - Intruder6.9 code review changes
		SCGCQ00877100 - (Closed) - TTY log dump is not persistent for multiple boots.
		SCGCQ00848328 - (Closed) - L2 Cache Error was NOT detected at POST after inject ECC error
		SCGCQ00859968 - (Resolved) - Deleting duplicate/unwanted files from source contr
		SCGCQ00679021 - (Closed) - Bringup MR Intruder fpga with Init bit stream.
		SCGCQ00681940 - (Closed) - Following FW interfaces are implemented
		SCGCQ00696857 - (Closed) - Invader 6.3 GCA code ported to Invader stream
		SCGCQ00713577 - (Closed) - 2.1b Bitstream related MR Fw changes for Dallas FPGA Validation.
		SCGCQ00760455 - (Closed) - Integrate .12 PL into MR code
		SCGCQ00772420 - (Closed) - Merge 6.5 Changes with Intruder Code stream
		SCGCQ00791733 - (Closed) - New PL integrated.
		SCGCQ00804452 - (Closed) - Integrate Latest PL .19 with MR stack
		SCGCQ00813852 - (Closed) - PL 0.85 release check-in
		SCGCQ00813853 - (Closed) - Flash header changes for Intruder
		SCGCQ00814430 - (Closed) - Code bring up on 3108 controller
		SCGCQ00817806 - (Closed) - Updating release script for Intruder code base
		SCGCQ00827051 - (Closed) - Integrate .22 PL and Invader 6.7 code.
		SCGCQ00827085 - (Closed) - Adding Support in Firmware for a new Flash Controller for Intruder.
		SCGCQ00834328 - (Closed) - Enable Synchronous mode of communication between Intruder and Flash Chip.
		SCGCQ00840256 - (Closed) - Code changes for A0 silicon & Eval board.
		SCGCQ00842347 - (Closed) - Creation and productization of new product SKU for 9361-8i board with 2GB of memory
		SCGCQ00844787 - (Closed) - support for dual rank ddr memory in Intruder, new pl library, and DMA workaround
		SCGCQ00846939 - (Closed) - Re-branding effort for customer.
		SCGCQ00850707 - (Closed) - Fault LED support for predictive failure drives for SGPIO
		SCGCQ00855889 - (Closed) - OEM wants controller VPD reporting should be disable
		SCGCQ00856088 - (Closed) - GPIO Settings for a customer
		SCGCQ00861994 - (Closed) - Check-in 6.9 Intruder code changes to use same MEM_FIXED for Inruder and Invader
		SCGCQ00864357 - (Closed) - Check-in PL 250.34 to Inruder A0.
		SCGCQ00865372 - (Implemented) - Reduce Command Block Latency during Background Operations
		SCGCQ00882016 - (Closed) - Integrating PL 06.00.05.00 with 6.6 FW stream.
		SCGCQ00884951 - (Closed) - Integrate 08.00.05.00 MR PL with MR 6.8
		SCGCQ00893029 - (Closed) - Add support to enable/Disable of Large IO Support - 1 MB IO
		SCGCQ00908329 - (Closed) - SCSI Inquiry string should not change in current generation HBA
		SCGCQ00681943 - (Closed) - ONFI debug functionality implemented to test software based offload and restore operations
		SCGCQ00687251 - (Closed) - Implement Cache-split feature
		SCGCQ00710266 - (Closed) - Intruder Dual SAS core changes.
		SCGCQ00721312 - (Closed) - Add support for TM and Error handling with dual sas core to MR.
		SCGCQ00772441 - (Closed) - Intergrate PL 0.13 to Intruder fpga
		SCGCQ00772443 - (Closed) - Put Infrastructure to compile Intruder and Invader on same code base.
		SCGCQ00792619 - (Closed) - Implemented as part of Intruder FPGA bringup.
		SCGCQ00837210 - (Closed) - For the new flash chip in Intruder, additional DDR Regions is memset to 0 after cache restore is complete.
		SCGCQ00841116 - (Closed) - Add Manual BISR to bring up secondary core for Intruder
		SCGCQ00862035 - (Closed) - New LED to indicate Over Temperature in Intruder.
		SCGCQ00809693 - (Closed) - Invader 6.6 Code stream merge to Intuder.
		SCGCQ00852052 - (Closed) - Add pl 0.250.27 to Intruder code.
		SCGCQ00853299 - (Closed) - Incorporate Memory Port difference for xor base address for Intruder
		SCGCQ00853423 - (Closed) - Implement the HW workaround in Intruder to recover from warm reset
		SCGCQ00855457 - (Implemented) - Task management support for JBOD/sysPD to Windows and Linux drivers (follow-on to PR SCGCQ00687438)
		SCGCQ00860586 - (Closed) - Add 5/15 6.9 action item changes
		SCGCQ00861695 - (Closed) - Add support for Micron M83C flash part for Intruder generation products.
		SCGCQ00880731 - (Closed) - Integrate Phase 9 PL 9.0.0.0 with MR 6.9
		SCGCQ00781019 - (Closed) - Retain Configuration btw boots on FPGA environment
		SCGCQ00846602 - (Closed) - New GPIO definitions for Intruder
		SCGCQ00868957 - (Closed) - Integrate Phase 9 PL (version 9.0.0.0) with MR 6.9
		SCGCQ00841181 - (Closed) - A0 Intruder bring activities Part 2
		SCGCQ00856859 - (Closed) - Check in new pl 250.32
		SCGCQ00860624 - (Closed) - Update ManPage12 and ManPage13 as per new structures defined for Intruder
		SCGCQ00852061 - (Closed) - MPIC configuration table changes
		SCGCQ00852502 - (Implemented) - Avoid Moving WB volumes to WT on pinned cache genera
		SCGCQ00805369 - (Port_Complete) - Bad physical drive caused controller error recovery go in loop
		SCGCQ00833943 - (Port_Complete) - MR6.7-Beta:FW hits to MonTask: line 1272 in file ../../raid/1078dma.c after Injecting media error in loop on CCVD metadata
		SCGCQ00833944 - (Port_Complete) - MR6.7-Beta:FW hits to MonTask: line 1272 in file ../../raid/1078dma.c after Injecting media error in loop on CCVD metadata
		SCGCQ00833945 - (Port_Complete) - MR6.7-Beta:FW hits to MonTask: line 1272 in file ../../raid/1078dma.c after Injecting media error in loop on CCVD metadata
		SCGCQ00833946 - (Port_Complete) - MR6.7-Beta:FW hits to MonTask: line 1272 in file ../../raid/1078dma.c after Injecting media error in loop on CCVD metadata
		SCGCQ00837206 - (Port_Complete) - Setting the Learn Cycle property of iBBU09 gives an I2C error
		SCGCQ00838545 - (Port_Complete) - MR_6.8_FW: Fw hits to MonTask: line 1272 in file ../../raid/1078dma.c while running IO in VM
		SCGCQ00841545 - (Port_Complete) - Performing a cable pull/push with array property change resulting into FW hang.
		SCGCQ00844445 - (Port_Complete) - Commands to the fde drives are not responding within 500ms.
		SCGCQ00845203 - (Port_Complete) - MR_6.8_FW:Firmware halted and restarted while doing flash erase on the onfi flash
		SCGCQ00848415 - (Port_Not_Required) - flush cache with write_verify on R0 volume and sata drive
		SCGCQ00849553 - (Port_Complete) - Unexpected controller reset during test run
		SCGCQ00849614 - (Port_Complete) - chain element for non RW commands were not pulled in the FW
		SCGCQ00849620 - (Port_Complete) - Deleting a Cachecade VD (CC VD) results in a firmware hang situation.
		SCGCQ00850990 - (Port_Complete) - Rebuild Performance for RAID 1 arrays is slower.
		SCGCQ00851993 - (Port_Complete) - Patrol Read Properties window does not pop up on MSM
		SCGCQ00853534 - (Port_Complete) - L2 unrecoverable cache error was seen during Patrol read properties modification in certain conditions.
		SCGCQ00854160 - (Port_Complete) - Controller Reboots after doing an OCR with IOs running in the background
		SCGCQ00854164 - (Port_Complete) - Controller cache fails to destage when multiple SVDs are present
		SCGCQ00854165 - (Port_Complete) - Controller cache fails to destage when multiple SVDs are present
		SCGCQ00854168 - (Port_Complete) - Controller cache fails to destage when multiple SVDs are present
		SCGCQ00854169 - (Port_Complete) - Controller cache fails to destage when multiple SVDs are present
		SCGCQ00854170 - (Port_Complete) - Controller cache fails to destage when multiple SVDs are present
		SCGCQ00869785 - (Port_Complete) - Fault LED support for predictive failure drives for SGPIO
		SCGCQ00873092 - (Port_Complete) - FW allows CCVD deletion with pinned windows
		SCGCQ00873093 - (Port_Complete) - FW allows CCVD deletion with pinned windows
		SCGCQ00873094 - (Port_Complete) - FW allows CCVD deletion with pinned windows
		SCGCQ00878362 - (Port_Complete) - Code collab fixes delivered
		SCGCQ00878401 - (Port_Complete) - Cleanup device wait queue if drive is no longer online
		SCGCQ00882474 - (Port_Complete) - Disable FLR support in MR FW to address VMware guest VM abrupt shutdown issue
		SCGCQ00886272 - (Port_Complete) - Windows BSOD when upgrade FW 24.6.0-0040 to 24.8.0-0026 with driver 6.707.08.00
		SCGCQ00886665 - (Port_Complete) - disableImmediateIO is not reflected in FW
		SCGCQ00886666 - (Port_Complete) - disableImmediateIO is not reflected in FW
		SCGCQ00886826 - (Port_Complete) - Need to set perfTunerMode appropriately on controller reset.
		SCGCQ00889407 - (Port_Complete) - MonTask: line 245 in file ../../raid/1078int.c while running I/Os with 64VDs and pull out drives belonging to CacheCade VD
		SCGCQ00889884 - (Port_Complete) - MonTask: line 245 in file ../../raid/1078int.c while running I/Os with 64VDs and pull out drives belonging to CacheCade VD
		SCGCQ00891282 - (Port_Complete) - Recon VD made "degraded" when the recon pd is pulled out allowing for rebuild once the drive is plugged back in.
		SCGCQ00891288 - (Port_Complete) - Cisco - Colusa1 MonTask after Initiating a Raid Level migration
		SCGCQ00908121 - (Port_Complete) - on creating 240VD and rebooting the server, FW breaks into montask.
		SCGCQ00908153 - (Port_Complete) - LUID gets changed during foreing import from non-240VD FW to 240VD FW
		SCGCQ00914823 - (Port_Complete) - Created VD configuration with PDs released from previous VD erased will lost after next reboot
		SCGCQ00803718 - (Port_Complete) - Ctrl-r and HII does not show proper message when you try to import the 65th VD.
		SCGCQ00838560 - (Port_Complete) - MR6.8_FW : Unable to Convert a JBOD PD to UG in Solaris
		SCGCQ00843936 - (Port_Complete) - Handling Functional Level Reset (FLR) .
		SCGCQ00844446 - (Port_Complete) - Enable I2C clock frequency of 100kHz for specific OEM is not working accurately
		SCGCQ00844447 - (Port_Complete) - Handle enabling disk "write" cache setting from OS for OEM
		SCGCQ00846479 - (Port_Complete) - Secure Erase on SATA SSD via CtrR or HII leads to unresponsive application, Secure erase failing intermittently
		SCGCQ00849580 - (Port_Complete) - Failed to import iMR RAID configuration to 12G MR
		SCGCQ00850924 - (Port_Complete) - MR & iMR FW Work-around is required for 3x08 chip Errata ID - 2012-RC714 for PCIE 3.0 compliance
		SCGCQ00853537 - (Port_Not_Required) - L2 unrecoverable cache error was seen during Patrol read properties modification in certain conditions.
		SCGCQ00854177 - (Port_Complete) - Vd erase does not resume after reboot in the presence of CCVD
		SCGCQ00871400 - (Port_Complete) - Fault LED support for predictive failure drives for SGPIO
		SCGCQ00886271 - (Port_Complete) - Windows BSOD when upgrade FW 24.6.0-0040 to 24.8.0-0026 with driver 6.707.0
		SCGCQ00887602 - (Port_Complete) - MR 6.8 : Few test cases fail when Intel PCIeCV tool is executed
		SCGCQ00895459 - (Port_Complete) - Removal of "LdDcmd ***** return pinned list 0" spam in FW logs.
		SCGCQ00844068 - (Port_Complete) - iMR:6.5-Exception in core 0 is seen when drives are spun down and an ocr is triggered
		SCGCQ00844152 - (Port_Complete) - FW doesn't poll all temp sensor channels every 5 seconds
		SCGCQ00853147 - (Port_Complete) - Continuous "TASK_ABORT_INTERNAL" prints observed in FW, after running heavy IO's on JBOD configured using 12Gig SAS SSD
		SCGCQ00868527 - (Port_Complete) - MR 6.9 : Controller boots to OS Even when Pinned Cache is present and Boot Error handling is set to Stop on Error.
		SCGCQ00870846 - (Port_Complete) - FW unable to detect the inserted drives
		SCGCQ00876154 - (Port_Complete) - SAS and SATA HDD R0 and R10 1M performance regressions (-15% to -35%) at QD16 to QD256
		SCGCQ00882149 - (Port_Complete) - StorCLI reports success on 4MB MR FW package flashing on iMR only controller.
		SCGCQ00884719 - (Port_Complete) - 'Fw initializing devices' hangs on controller with specific failed drives on backplane
		SCGCQ00891273 - (Port_Complete) - Megaraid Thunderbolt controller reports cache memory size as 0 when no logical drives are present.
		SCGCQ00841533 - (Port_Complete) - Instruction TLB error seen when auto configuration command exectued from CLI application
		SCGCQ00843390 - (Port_Complete) - Megaraid-sas driver hang with Falcon card
		SCGCQ00851886 - (Port_Complete) - MSM displays error message if 'Schedule Consistency Check' is selected.
		SCGCQ00892136 - (Port_Complete) - MR 6.6.3 "storcli /c0 show all" shows lot of bad block messages in the log
		SCGCQ00835227 - (Port_Complete) - STASH firmware entered fault state with SSD drive
		SCGCQ00872263 - (Port_Complete) - Fw crash and BIOS RSODs when VD1 deleted with recon on a PI VD(VD2) and Slow init on VD3.
		SCGCQ00841772 - (Port_Complete) - MR firmware reports no smart error when attaching a PFA drive
		SCGCQ00876142 - (Port_Complete) - FW unable to detect the inserted dr
	BIOS 6.28.04.0
		SCGCQ00879731 - (Closed) - Legacy OpROM: Handle the conditions for battery failed state as per the Battery design do
		SCGCQ00882729 - (Closed) - Legacy OpROM: Controller POST shows JBOD found on host adapter, when number of INT13 device is > deviceExposure
		SCGCQ00866982 - (Closed) - Legacy OpROM: Overlapping seen in POST in presence of two controllers and foreign config during CTRL-H laun
		SCGCQ00834718 - (Closed) - PNPs and support for 16 port 12G designs
	NVDATA  3.1507.00-0006
		Numerous changes for specific customers
	UEFI_Driver 0x06110200(signed)
		SCGCQ00898506 - (Closed) - OS doesn't boot after installing OS on the 100th VD , while having 240 VDs created in EFI mod
		SCGCQ00834720 - (Closed) - PNPs and support for 16 port 12G designs
	Hii 03.17.14.00(signed)
		SCGCQ00844774 - (Closed) - Handle coverity defects
		SCGCQ00880737 - (Closed) - Handled the coverity defects.
		SCGCQ00892931 - (Closed) - Not able to set Controller properties
		SCGCQ00896827 - (Closed) - Cannot convert the state of drive from JBOD to UG if the drive is not 16byte CDB
		SCGCQ00825741 - (Closed) - UEFI Driver: Compilation error when debug Flags are enabled
		SCGCQ00852480 - (Closed) - "Question value mismatch type!Press Enter" message is displayed while entering create virtual drive page
		SCGCQ00878350 - (Closed) - HII Enclosure Management form multiple time navigation results in hang/multiple entries of enclosure seen
		SCGCQ00879673 - (Closed) - HII: Add GUID check for bootable drive
		SCGCQ00894460 - (Closed) - Controller status inconsistency between Dashboard and Controller management in HII
		SCGCQ00915093 - (Closed) - HII: Updating LargeIOSupport as per the new API changes
		SCGCQ00870398 - (Closed) - Incomplete Port enumeration i.e connector information is displayed for ESM and PD's in HII
		SCGCQ00873973 - (Closed) - Profile Based DHS creation grayed out
		SCGCQ00879726 - (Closed) - HII: Handle the conditions for battery failed state as per the Battery design doc
		SCGCQ00889780 - (Closed) - HII: Address review comments
		SCGCQ00903490 - (Closed) - HII RLM for only R0 available when 18 or more drives are present
		SCGCQ00860564 - (Closed) - In Make UG warning message OS JBOD drives are not listed
		SCGCQ00898506 - (Closed) - OS doesn't boot after installing OS on the 100th VD , while having 240 VDs created in EFI mode
		SCGCQ00881426 - (Closed) - VD properties does not display Emulation type.
		SCGCQ00893928 - (Closed) - HII: Address review comment
		SCGCQ00834719 - (Implemented) - PNPs and support for 16 port 12G designs
		SCGCQ00834720 - (Closed) - PNPs and support for 16 port 12G designs
		SCGCQ00844917 - (Implemented) - OEM requesting to do a WRITE VERIFY prior to flushing cache. This needs to be managed via CLI
		SCGCQ00893152 - (Closed) - HII: Add support to enable/Disable of Large IO Support
		SCGCQ00828031 - (Implemented) - Add support to detect that an OS is installed on a JBOD
		SCGCQ00854621 - (Closed) - Provide a more descriptive port enumerati
		SCGCQ00888846 - (Port_Complete) - HII: Spelling mistakes in strings
		SCGCQ00893220 - (Port_Complete) - Inconsistency in showing controller status between MSM and HII for Fake Flash errors
		SCGCQ00865978 - (Port_Complete) - Pause for Password at boot time Enable/Disbale based on Boot Mode
		SCGCQ00878512 - (Port_Complete) - HII-VD renaming truncates 15th character & allows for 16 characters,though only 15 supported
		SCGCQ00882762 - (Port_Complete) - "Question value mismatch type!Press Enter" message is displayed while entering create virtual drive page
		SCGCQ00884560 - (Port_Complete) - 13G Exception Screen thrown in uEFI environm
	Ctrl-R 5.13-1100
		SCGCQ00873155 - (Closed) - Ctrl-R:Not able to lauch ctrl-R if 2 controllers, one with huawei and another with generic PnP ID is present.
		SCGCQ00871350 - (Closed) - Handled the coverity defects.
		SCGCQ00837424 - (Closed) - Storcli reports cache type as 'RW' instead of 'R' after R1 CC VD is degraded
		SCGCQ00855701 - (Closed) - StorCLI does not find enclosures in multipath environment
		SCGCQ00869436 - (Closed) - Include Partition table and GPT GUID check to detect OS/FS
		SCGCQ00892967 - (Resolved) - Intruder: The size of the foreign config shown does not match with that after an import.
		SCGCQ00893032 - (Closed) - With Liberator the Physical sector size of 512E drive is shown wrong
		SCGCQ00853268 - (Resolved) - In EFI, Storcli displaying Bus Number ,Device Number and Function Number = 0 for all the controllers.
		SCGCQ00868215 - (Closed) - Connector name field is displayed as & port 4-7 when a single ESM is connected in Multipath
		SCGCQ00864200 - (Closed) - Checking in fix for resource leak
		SCGCQ00867569 - (Closed) - storcli /c0 vall show is not listing CaC column when CC is not supported and displaying sCC with wrong value.
		SCGCQ00870485 - (Closed) - EFI storcli is not working with intruder
		SCGCQ00880534 - (Closed) - Invader 6.9 : Efi cli - Command fails with a hang when multiple controllers connected .
		SCGCQ00860461 - (Closed) - In JBOD warning message all the drives are getting listed
		SCGCQ00881720 - (Closed) - Foreign Config pop up scrollup/down does not respond
		SCGCQ00860056 - (Closed) - "storcli show" shows wrong count for aso.
		SCGCQ00868198 - (Closed) - Removing Phy information from Enclosure PD details.
		SCGCQ00874381 - (Closed) - StorCLI: Memory Leak in function _available_memory_calc1.
		SCGCQ00876796 - (Closed) - null pointer dereference
		SCGCQ00892129 - (Resolved) - Most of the commands fail with "Invalid argument" error.
		SCGCQ00884910 - (Closed) - StorCli Libmods 6.9 coverity fixes
		SCGCQ00865108 - (Closed) - Ventura: storcli add vd fails with NVMe
		SCGCQ00883409 - (Closed) - Storcli shows the wrong position of enclosures when they are connected in daisy chain with controller
		SCGCQ00899384 - (Closed) - Buffer is not incremented when reading sector of the drive
		SCGCQ00915164 - (Closed) - CTRL-H: Updating LargeIOSupport as per the new API changes
		SCGCQ00889924 - (Closed) - Intruder Port2 and Port3 display are not handled in PD Mngt
		SCGCQ00889771 - (Closed) - CTRL-H:Address Review comments
		SCGCQ00881936 - (Closed) - Ctrl-R doesnot show the controller name above the menu 
		SCGCQ00850607 - (Closed) - added new command /c0 show swalilog equivalent to adpalilog
		SCGCQ00834721 - (Implemented) - PNPs and support for 16 port 12G designs
		SCGCQ00854633 - (Implemented) - Add details of pending FW images to StorCLI/sho adpinfo
		SCGCQ00859740 - (Implemented) - RRB 88: Provide a more descriptive port enumeration (Libmods changes)
		SCGCQ00893498 - (Closed) - LibMods: Add support to enable/Disable of Large IO Support - 1 MB IO
		SCGCQ00893153 - (Closed) - CTRL-H: Add support to enable/Disable of Large IO Support
		SCGCQ00854622 - (Closed) - Provide a more descriptive port enumeration
		SCGCQ00850636 - (Closed) - Added support for flashing the FW on intruder and new Dev-ID's of Invader are added for EFI.
		SCGCQ00828032 - (Implemented) - Add support to detect that an OS is installed on a JBOD
		SCGCQ00853218 - (Implemented) - Add support to detect that an OS is installed on a JBOD
		SCGCQ00844918 - (Implemented) - OEM requesting to do a WRITE VERIFY prior to flushing cache. This needs to be managed via CLI
		SCGCQ00854626 - (Closed) - Provide a more descriptive port enumera
		SCGCQ00904852 - (Port_Complete) - Checking-in changes for defect-SCGCQ00904794
		SCGCQ00857695 - (Port_Complete) - Consistent Sorting of Controllers for End Users in Customer Facing Tools (EFI storcli)
		SCGCQ00873795 - (Port_Complete) - CTRL-H: MonTask - line 243 in file ../../raid/1078int.c during rebuild
		SCGCQ00854296 - (Port_Complete) - Add Pause For Password feature in CTRLH
		SCGCQ00853654 - (Port_Complete) - Libmods implementation for WRITE VERIFY prior to flushing cache.
		SCGCQ00878517 - (Port_Complete) - CTLR_R: PI-DG : After break mirror, data protection shown as "NA"
		SCGCQ00900172 - (Port_Complete) - Added the iMR cutlass PNP id's(0x1000/0052h, 0x1000/0x0053h) to EFI controller explorer class.
		SCGCQ00901264 - (Port_Complete) - MR 6.8: storcli reports legacy driver version when native driver is loaded for a Fury controller in ESXi 6.0
		SCGCQ00853586 - (Port_Complete) - Get and Set Factory settings Failure
		SCGCQ00850019 - (Port_Complete) - storcli /c0/eall/sall show smart command gives all zeros in the output
		SCGCQ00849728 - (Port_Complete) - LibMOD:OEM requesting to do a WRITE VERIFY prior to flushing cache.
		SCGCQ00878555 - (Port_Complete) - Ctrl-R is creating a smaller VD than specified when selecting a VD size in TB
		SCGCQ00867486 - (Port_Complete) - Changed the Message for Hiding Boot VD Operation Status as per FW return error status.
		SCGCQ00854279 - (Port_Complete) - Add Pause For Password feature in CTRLH
		SCGCQ00893015 - (Port_Complete) - Inconsistency in showing controller status between MSM and Ctrl-R for Fake Flash errors
		SCGCQ00874679 - (Port_Complete) - storcli doesnt display E252/E253 enclosure info on an 84016
		SCGCQ00894487 - (Port_Complete) - Inconsistency in showing controller status between MSM and StorCLI for Fake Flash errors
		SCGCQ00841286 - (Port_Complete) - Storcli : The bus error message is displaying for storcli /c0/eall/sall show smart comm
	ROMENV 1.09
	BootBlock 3.07.00.00-0002
	FCODE 4.17.08.00
	PCLI 1.07.05

Firmware Package:24.9.0-0022 (MR 6.8)
 Firmware - 4.290.00-4536
	SCGCQ00781736 - (Closed) - Customer ROMB design GPIO/SGPIO drive LED question
	SCGCQ00808221 - (Closed) - Correctable ECC errors are not getting detected.
	SCGCQ00819314 - (Closed) - SSDs getting data with bad PI CRC.
	SCGCQ00819811 - (Closed) - When consistency check is aborted/suspended, HBA resets
	SCGCQ00825126 - (Closed) - Unexpected controller reset during test run
	SCGCQ00825568 - (Closed) - Montask at Line 108 in ../../raid/span.c while configuring PR11/R0 CCVD using 1.4 TB SSD's
	SCGCQ00825602 - (Closed) - Function isCcvdOkToImport was failing the import
	SCGCQ00826884 - (Closed) - During one MB IO’s along with background flush causing the chainframe(MID) getting leaked leads to Montask.
	SCGCQ00828327 - (Closed) - OEM check for SCGCQ00762968 fix as it is only for OEM.
	SCGCQ00829214 - (Closed) - MR firmware exposes more than 240 VD's to the host, even when the host driver doesn't support more than 64VD's.
	SCGCQ00829218 - (Closed) - With 6.7MR driver and 6.8MR fw a kill adapter is observed while IO in progress and importing of degraded VD.
	SCGCQ00830847 - (Closed) - Block CCVD creation if the number of CCVd’s > 1 and CCVD’s are associated with SVD
	SCGCQ00835586 - (Closed) - Instruction TLB error seen when auto configuration command exectued from CLI application
	SCGCQ00835725 - (Closed) - Source VD of Config2 [2G-CTRL] fails to imports in Config1 [1G-CTRL]
	SCGCQ00837878 - (Closed) - Firmware halted and restarted while doing flash erase on the onfi flash
	SCGCQ00837937 - (Closed) - Fail to set read and write command timer for multiple SATA drives.
	SCGCQ00839323 - (Resolved) - Authentication Raid key Failed! err:1 error while issuing OCR with IOs on multiple VDs
	SCGCQ00841359 - (Closed) - Rebuild Performance for RAID 1 arrays is slower.
	SCGCQ00841512 - (Closed) - Multi CCVD import fails after FW downgrade from MR 6.8 to 6.7
	SCGCQ00842625 - (Closed) - Controller cache fails to destage when multiple SVDs are present
	SCGCQ00842804 - (Closed) - CacheCade allows the user to create a as small as 32-MB
	SCGCQ00844101 - (Closed) - Reverting Simplified Buffer Manager Code Changes
	SCGCQ00844102 - (Closed) - Mismatch in the CCVD size after importing the CCVD configuration from MR 6.7 to MR 6.8
	SCGCQ00844698 - (Closed) - Deleting a Cachecade VD (CC VD) results in a firmware hang situation.
	SCGCQ00844838 - (Closed) - Pd counters are reset to zero on every iteration.
	SCGCQ00845569 - (Closed) - Observed drops around 15-25 % across all RAID levels in many areas for 1MB stripe size
	SCGCQ00845695 - (Closed) - FW gives wrong warning message"Warning!!! no free slot in nvram" in the logs
	SCGCQ00851230 - (Closed) - MR6.8 Alpha SSD Random Read/Write performance regressions (15-45%) vs MR6.7GCA
	SCGCQ00852739 - (Closed) - MR6.8 Alpha SAS HDD Random Write performance regressions (15-35%) vs MR6.7GCA
	SCGCQ00855258 - (Closed) - Compilation warning occurring due to usage of inline boolean macro
	SCGCQ00856313 - (Closed) - Undo the changes made for defect SCGCQ00837917 [DISM stuck at device discovery on enclosure power cycle]
	SCGCQ00860270 - (Closed) - FW unable to detect the inserted drives
	SCGCQ00867117 - (Closed) - OFU fails when FW downgraded from 6.8 to 6.7(GCA)
	SCGCQ00869551 - (Closed) - SAS and SATA HDD R0 and R10 1M performance regressions (-15% to -35%) at QD16 to QD256
	SCGCQ00879124 - (Closed) - Cache bypass algorithm bypasses sequential writes even when there are no sufficient writes to bypass cache
	SCGCQ00820519 - (Closed) - Performance drop seen with 1MB + SBM compared against SBM as base code.
	SCGCQ00821359 - (Closed) - With IO in progress a Data TLB error is seen on performing background operations.
	SCGCQ00824415 - (Closed) - Missed to memset the datastructure used to populate the devhandle
	SCGCQ00825797 - (Closed) - Performing a cable pull/push result to Data TLB Error at "RaidIoWriteOver+684".
	SCGCQ00827713 - (Closed) - Certian CCVDs created using older FW cannot be properly import on to MR6.8
	SCGCQ00831369 - (Closed) - FW doesn't allow auto/foreign import of CCVDs created on MR6.7 or earlier systems
	SCGCQ00831398 - (Closed) - Deleting a Cachecade VD (CC VD) results in a firmware hang situation.
	SCGCQ00834552 - (Closed) - Unable to Convert a JBOD PD to UG in Solaris
	SCGCQ00836496 - (Closed) - Performing a cable pull/push with array property change resulting into FW hang.
	SCGCQ00837917 - (Resolved) - DISM stuck at device discovery on enclosure power cycle, Devices present with DM but not reflected in upper layers
	SCGCQ00838222 - (Closed) - DATA TLB seen when trying to offline a drive from R1 virtual drive
	SCGCQ00838953 - (Closed) - Deleting a Cachecade VD (CC VD) results in a firmware hang situation.
	SCGCQ00839635 - (Closed) - chain element for non RW commands were not pulled in the FW
	SCGCQ00839936 - (Closed) - FW crash observed, when trying to destage the Pinned Cache
	SCGCQ00841317 - (Closed) - Secure Erase on SATA SSD via CtrR or HII leads to unresponsive application, Secure erase failing intermittently
	SCGCQ00845245 - (Closed) - Reverting code changes done in SSD Metadata
	SCGCQ00853558 - (Closed) - On performing a SATA drive pull/push operation less than 4sec, result to Read/write command timer set to drive default value.
	SCGCQ00854856 - (Closed) - Assertion failure while restoring Pinned data with least latency mode switch
	SCGCQ00857115 - (Closed) - Pd counter "last 8hour ago" is not propagating/copying to "16hour ago" after reboot.
	SCGCQ00862519 - (Closed) - Disabling 1MB IO support
	SCGCQ00864181 - (Closed) - CID 16728, Uninitialized pointer read results in DATA TLB error
	SCGCQ00763934 - (Closed) - Storcli show device link speed is confused for SATA/SAS drive when connected expander have buffer feature enable
	SCGCQ00797643 - (Closed) - FW hung at LogInit: Flushing events from previous boot while running policy change script of Vd and learn cycles.
	SCGCQ00800589 - (Closed) - Unexpected all device insert event causes logical state change and VD deletion
	SCGCQ00812842 - (Closed) - Firmware will POST bios message when there is a romId mismatch and no features present on the controller
	SCGCQ00832774 - (Closed) - Sgl frames crunch observed with Random larger IO's
	SCGCQ00833765 - (Closed) - Failed to import iMR RAID configuration to 12G MR
	SCGCQ00835377 - (Closed) - With MR6.8 firmware, A phantom LD is being created when LD 0 is created.
	SCGCQ00836103 - (Closed) - Incorrect error returned by FW when when PDs with different block size are mixed.
	SCGCQ00840587 - (Closed) - Introduce macro and inline function to distinguish between OEM Rack Server and OEM Blade Server
	SCGCQ00845703 - (Closed) - FW is setting wrong recovery time Limit in SAS/SATA drives, when detection type is 3 and recoveryTimeLimit is 0 in Nvdata
	SCGCQ00863066 - (Closed) - CCVD size inconsistency across FW upgrade to 6.8 and downgrade to lower FW version
	SCGCQ00798701 - (Closed) - 4K virtual drive missing across power cyle on iMR controller
	SCGCQ00818560 - (Closed) - FW should not block manual check consisteny operation on excluded VDs
	SCGCQ00820037 - (Closed) - PL Fault hit while performing Reconstruction.
	SCGCQ00828174 - (Closed) - firmware will get Kill Adapter at reboot or power on.
	SCGCQ00828305 - (Closed) - Missing/offline PDs in a R0 CCVD to be marked as offline
	SCGCQ00830541 - (Closed) - DATA TLB error while unblocking SVD
	SCGCQ00830918 - (Closed) - EFI driver health fails when more than 64VDs configured
	SCGCQ00836500 - (Closed) - Release buffers appropriately on volume deletion
	SCGCQ00850961 - (Closed) - Tuning the Debug Infrastructure for testing Predictive Failure PR
	SCGCQ00853249 - (Closed) - FW hangs on changing the Write policy of CCVD
	SCGCQ00856310 - (Closed) - Fw hits to MonTask: line 325 in file ../../raid/mem.c while spin up drive.
	SCGCQ00822403 - (Closed) - Fw hits to MonTask: line 1272 in file ../../raid/1078dma.c while running IO in VM
	SCGCQ00823876 - (Closed) - Fix group code review issues.
	SCGCQ00825725 - (Closed) - FW upgrade from non 240VD FW to 240VD FW when OS is behind the controller results in BSOD
	SCGCQ00832596 - (Closed) - R10 performance with large block IOs has a large drop while scaling QD with 12Gb/s SAS HDDs
	SCGCQ00851810 - (Closed) - Vd erase does not resume after reboot in the presence of CCVD
	SCGCQ00852019 - (Closed) - Handling of ONFI Transport case with different Performance Tuner Modes.
	SCGCQ00822356 - (Closed) - Fixed build issues from merge.
	SCGCQ00828781 - (Closed) - Controller goes into a deadlock when a Logical Drive (LD) is deleted during foreground initialization
	SCGCQ00835359 - (Closed) - Controller Reboots after doing an OCR with IOs running in the background
	SCGCQ00836381 - (Closed) - ssdDebug to be disbled by default
	SCGCQ00843579 - (Closed) - Unexpected behaviour in VD erase after FW upgrade
	SCGCQ00845506 - (Closed) - FW is setting Recovery time limit, read and write command timer for SSD drives.
	SCGCQ00829098 - (Closed) - added condition check avoid calling the ssdModifyMagicBlock() in case of missing VD’s across reboot/ocr
	SCGCQ00837454 - (Closed) - User can create CCVDs whose size can exceed maximum configurable CacheCade size
	SCGCQ00846735 - (Closed) - Host TM active flag is not cleared once the target reset completes on JBOD
	SCGCQ00850943 - (Closed) - Unable to delete CCVD after foreign import
	SCGCQ00827732 - (Closed) - FW hits to MonTask: line 4538 in file ../../raid/cache.c on discarding Preserved Cache
	SCGCQ00831819 - (Closed) - Add the forward compatibility bit in DDF to avoid importing CCVD on legacy firmware.
	SCGCQ00728066 - (Closed) - update copyright info
	SCGCQ00846677 - (Closed) - port latency improvements from development stream
	SCGCQ00842239 - (Closed) - Modified SSD Metadata to store number of cache windows generated
	SCGCQ00823759 - (Closed) - Increase maximum cache size for Cachecade to 2048GB.
	SCGCQ00820593 - (Closed) - Program CVFM(Cache Vault Flash Module) VPD without Supercap connected.
	SCGCQ00816361 - (Closed) - Task management support for JBOD/sysPD
	SCGCQ00812722 - (Closed) - Single write COL with FBU03 for OEM
	SCGCQ00806537 - (Implemented) - Use config sequence number to SYSTEM PD fastpath IOs
	SCGCQ00770194 - (Closed) - Include learn cycle failure debug command in FW.
	SCGCQ00823470 - (Closed) - Monitoring Drive Performance
	SCGCQ00820067 - (Closed) - Request to remove the repeated ROC temperature warnings in ttylog when above 104 deg C.
	SCGCQ00817914 - (Implemented) - Refactor Buffer Manager to avoid overheads with various lists
	SCGCQ00812724 - (Closed) - FW change for single write to be fully supported for 2:4.
	SCGCQ00792582 - (Closed) - Event for LED locate start and stop
	SCGCQ00758184 - (Closed) - GG update to include concatenated GG/VPD data for Invader product generation.
	SCGCQ00758178 - (Closed) - MegaRAID CPLD update improvements
	SCGCQ00824803 - (Closed) - CCVD size parameters have to be handled properly and stored in the DDF
	SCGCQ00820055 - (Closed) - CacheCade changes for SBM
	SCGCQ00816316 - (Implemented) - Large I/O Suport - suport 1MB transfer size
	SCGCQ00839643 - (Closed) - Add strict sequentiality check in cache bypass algorithm
	SCGCQ00825197 - (Implemented) - Add Log Latency Framework
	SCGCQ00823063 - (Implemented) - Create build environment for MR 6.8 stream
	SCGCQ00820329 - (Implemented) - Decouple MR_FW_RAID_MAP update from Command block
	SCGCQ00816307 - (Implemented) - Reduce retries for timed-out FastPath I/O’s ( enable CTIO and FP)
	SCGCQ00806517 - (Closed) - Add set "Fail PD on SMARTer" property feature to StorCLI
	SCGCQ00784955 - (Port_Complete) - Virtual Disk GUID field changes when a VD is moved. The LUID is supposed to be unique and invariant.
	SCGCQ00790037 - (Port_Complete) - Firmware logs are not dumped to flash during device discovery phase
	SCGCQ00791671 - (Port_Complete) - Command timeout happens though the response returns in 130ms.
	SCGCQ00791672 - (Port_Complete) - Command timeout happens though the response returns in 130ms.
	SCGCQ00804284 - (Port_Complete) - Calculation for minimum blocks required to offload is wrong for single image configuration.
	SCGCQ00806806 - (Port_Complete) - HII hangs for several minutes when entering the security key in for a locked PD
	SCGCQ00813167 - (Port_Complete) - Offload timed out for single image configuration
	SCGCQ00813744 - (Port_Complete) - Offload timed out for single image configuration
	SCGCQ00814987 - (Port_Complete) - GG update to include concatenated GG/VPD data for Invader product generation.
	SCGCQ00814997 - (Port_Complete) - Correctable ECC errors are not getting detected.
	SCGCQ00821670 - (Port_Complete) - Reduce the clean up time of all the IOs from a host that is powered off.
	SCGCQ00822131 - (Port_Complete) - Immediate IO failed in write back cache recovery code 
	SCGCQ00822235 - (Port_Complete) - Reduce PD time out value from 12 seconds to 8 Seconds
	SCGCQ00822481 - (Port_Complete) - Feature to retrieve the TTY logs compressed
	SCGCQ00822642 - (Port_Complete) - Virtual Disk GUID field changes when a VD is moved. The LUID is supposed to be unique and invariant.
	SCGCQ00823448 - (Port_Complete) - Fix for crash with Raid 5 write through
	SCGCQ00824818 - (Port_Complete) - Megaraid_sas driver fails to communicate with the FW and fails to discover any disks attached
	SCGCQ00825773 - (Port_Complete) - OS (CentOS 7.0) crash observed while doing online FW update on IMR Fury controller
	SCGCQ00825774 - (Port_Complete) - Background IO's on 235 R0 VD's and abrupt enclosure power cable pull resulting into Fatal FW error
	SCGCQ00839018 - (Port_Complete) - After successful reconstruction of VDs, they are not getting reflected in MSM unless the user reboots the system
	SCGCQ00839974 - (Port_Complete) - To support secondary key on baseboard to enable fearures for iMR cards
	SCGCQ00840631 - (Port_Complete) - MegaRAID CPLD update improvements
	SCGCQ00787362 - (Port_Complete) - Firmware logs are not dumped to flash during device discovery phase
	SCGCQ00789739 - (Port_Complete) - Virtual Disk GUID field changes when a VD is moved. The LUID is supposed to be unique and invariant.
	SCGCQ00791673 - (Port_Complete) - Command timeout happens though the response returns in 130ms.
	SCGCQ00813062 - (Port_Complete) - Offload timed out for single image configuration
	SCGCQ00820086 - (Port_Not_Required) - SVD's are getting 'Access Blocked' after OCR followed by System Reboot
	SCGCQ00820917 - (Port_Complete) - 95% longer boot time compared to shipping stream
	SCGCQ00821672 - (Port_Complete) - Host IO may get an error - code review defect
	SCGCQ00821693 - (Port_Complete) - Controller commands are getting failed resulting in application hang when Logical Drive (LD) is deleted during reconstruction
	SCGCQ00822182 - (Port_Complete) - IO completion may not happen because of earlier aborts
	SCGCQ00822184 - (Port_Complete) - Crash when completing Abort.
	SCGCQ00822315 - (Port_Complete) - Remove unnecessary debug prints to console (during dma failure)
	SCGCQ00822739 - (Port_Complete) - Incorrect SGL from driver crashes FW (expected) but does not let driver do OCR
	SCGCQ00825765 - (Port_Complete) - Command timeouts with cdb=ff ff ff ff
	SCGCQ00826083 - (Port_Complete) - Invader MR does not update Expander Information dynamically
	SCGCQ00839970 - (Port_Complete) - New event when patrol read is aborted due to conflict with other background operation
	SCGCQ00844697 - (Port_Complete) - Deleting a Cachecade VD (CC VD) results in a firmware hang situation.
	SCGCQ00844801 - (Port_Complete) - Behavior change when FW hit fault code 0x81 (uncorrectable ECC error)
	SCGCQ00797554 - (Port_Complete) - Flash of incorrect GG on controller, does not restore VDs back to WB
	SCGCQ00814991 - (Port_Complete) - Include learn cycle failure debug command in FW.
	SCGCQ00815618 - (Port_Complete) - FW pkg 23.22.0-0017 and later initialize drives ~50% slower
	SCGCQ00820922 - (Port_Complete) - Auto Configure RAID0 DG set to READ AHEAD policy instead of NO READ AHEAD
	SCGCQ00821671 - (Port_Complete) - IO may not do error recovery (code review fix)
	SCGCQ00821674 - (Port_Complete) - Bad physical drive caused controller error recovery go in loop
	SCGCQ00825775 - (Port_Complete) - FW breaks into montask while making VDs offline when rebuild is going on with IOs
	SCGCQ00826980 - (Port_Complete) - Single OEM card reporting SDRAM Unrecoverable Error
	SCGCQ00829706 - (Port_Complete) - SSDs fall offline after reset under heavy IO.
	SCGCQ00829929 - (Port_Complete) - Storcli show device link speed is confused for SATA/SAS drive when connected expander have buffer feature enable
	SCGCQ00832121 - (Port_Not_Required) - Controller goes into a deadlock when a Logical Drive (LD) is deleted during foreground initialization
	SCGCQ00838186 - (Port_Complete) - Makefile Changes to include the macro by default
	SCGCQ00840009 - (Port_Complete) - IO freeze on R5 while running host IO with BGI
	SCGCQ00853535 - (Port_Complete) - L2 unrecoverable cache error was seen during Patrol read properties modification in certain conditions.
	SCGCQ00818815 - (Port_Complete) - Battery Failure observed when upgrading FW from previous versions to latest one.
	SCGCQ00821002 - (Port_Complete) - Handling DMA Errors and Write Back Cache Recovery for new program
	SCGCQ00821667 - (Port_Complete) - Support in Device module to handle DMA errors
	SCGCQ00822081 - (Port_Complete) - This ER is to support DMA failure from SysDma
	SCGCQ00822227 - (Port_Complete) - Crash in FW because of two commands having same SMID.
	SCGCQ00822321 - (Port_Complete) - Host IO did not complete
	SCGCQ00839973 - (Port_Complete) - Invalid event "Consistency Check done on VD:255" coming when CC is running on a VD and VD is deleted
	SCGCQ00840019 - (Port_Complete) - Observing I/O stalls for longer duration in firmware version with throttling changes introduced
	SCGCQ00844704 - (Port_Complete) - Deleting a Cachecade VD (CC VD) results in a firmware hang situation.
	SCGCQ00814989 - (Port_Complete) - MegaRAID CPLD update improvements
	SCGCQ00821694 - (Port_Not_Required) - Host abort Command Implementation
	SCGCQ00822140 - (Port_Complete) - Hitting Assert in flush logic while doing write back cache recovery in code
	SCGCQ00861251 - (Port_Complete) - Observing I/O stalls for longer duration in firmware version with throttling changes introduced
	SCGCQ00824799 - (Port_Complete) - Patrol Read Properties window does not pop up on MSM
	SCGCQ00835242 - (Port_Complete) - Failed to import iMR RAID configuration to 12G MR
	SCGCQ00844085 - (Port_Complete) - Report controller flash device health status
	SCGCQ00818816 - (Port_Complete) - Removing OV workound for superCaps
	SCGCQ00822166 - (Port_Complete) - Improper handling of Redirtied bit pattern during write back cache recovery
	SCGCQ00829961 - (Port_Complete) - Firmware will POST bios message when there is a romId mismatch and no features present on the controller
	SCGCQ00845690 - (Port_Complete) - MSM displays error message if 'Schedule Consistency Check' is selected.
 UEFI_Driver 0x060E0300 (SIGNED)
	SCGCQ00844774 - (Closed) - Handle coverity defects
	SCGCQ00825741 - (Closed) - Compilation error when debug Flags are enabled
	SCGCQ00813457 - (Closed) - Rebranding effort for OEM
 Hii v03.14.09.00 (SIGNED)
	SCGCQ00820006 - (Closed) - Address review comments
	SCGCQ00825573 - (Closed) - Create Cache Cade VD option still available even after MaxConfgiureSSCSize is crossed.
	SCGCQ00852480 - (Closed) - "Question value mismatch type!Press Enter" message is displayed while entering create virtual drive page
	SCGCQ00816666 - (Closed) - Handle CCVD Changes Based on new MR.h bit supportExtendedSSCSize
	SCGCQ00830577 - (Closed) - on doing manage SSD caching, the landing page takes to VD management page
	SCGCQ00832946 - (Closed) - In the Reconfigure VD, suppress the Add Drives operation based on the UG drives available.
	SCGCQ00844160 - (Closed) - Allow CCVD Creation only if we have more than 1 GB space.
	SCGCQ00828425 - (Closed) - The help string for maintain PD fail history is not appropriate
	SCGCQ00828433 - (Closed) - No description or help for vd status field in HII
	SCGCQ00829216 - (Closed) - HII doesn't allow to reconfigure a RAID 6 partically degraded virtual drive to RAID 0
	SCGCQ00811352 - (Closed) - Handle Code Collaborator Defect and comments.
	SCGCQ00830579 - (Closed) - Raid level gets changed on trying to add a drive to the VD while performing Reconfigure virtual drive.
	SCGCQ00844784 - (Closed) - Handle coverity defects
	SCGCQ00845541 - (Closed) - Max SSC configurable size not shown
	SCGCQ00827376 - (Closed) - the default write policy doesn't change from WB to WT while creating a vd when there is a battery failure.
	SCGCQ00828427 - (Closed) - The help string for cache flush interval is not appropriate
	SCGCQ00828751 - (Closed) - Manage ssd caching comes under vd property instead of controller property
	SCGCQ00838756 - (Closed) - Manage SSD Caching: Empty string seen in warning message
	SCGCQ00811295 - (Reworked) - Generic RAID1 Profile based VD creation option is not grayed out after creating 64VD's.
	SCGCQ00829208 - (Closed) - In the Reconfigure VD page the help string for the 'New RAID level' is not appropriate
	SCGCQ00834097 - (Closed) - Option to migrate from r6 to r0 comes in HII when the VD is in degraded state.
	SCGCQ00827315 - (Closed) - Increase maximum cache size for Cachecade to 2048GB. This will be named CC 2.5
	SCGCQ00818001 - (Implemented) - Rebranding effort for OEM - Changes outside PNP ID addition
	SCGCQ00816310 - (Implemented) - HII & MSM Mismatch on write-back options - UI Inconsistancy issue
	SCGCQ00738144 - (Closed) - Code Redundancy in firing MR_DCMD_CTRL_GET_INFO
	SCGCQ00789492 - (Closed) - Support decimal fraction for PD/VD size in HII
	SCGCQ00804071 - (Closed) - Code refactor: Check return code of HiiGetString()
	SCGCQ00816305 - (Implemented) - Add "Remove Drives" option during Raid Level Migration
	SCGCQ00813457 - (Closed) - UEFI Driver: Rebranding effort for OEM
	SCGCQ00818583 - (Implemented) - Provide richer enclosure related information in the MegaRAID HII Enclosure Management pages.
	SCGCQ00805041 - (Port_Complete) - how error message when user clicks on Apply Change wihout choosing drive group
	SCGCQ00817320 - (Port_Complete) - PD Remove option is not available for offline drive
	SCGCQ00819329 - (Port_Complete) - Show error message when user clicks on Apply Change wihout choosing drive group
	SCGCQ00816978 - (Port_Complete) - Prepare For Removal" on PD does not work w/pending PD operations (HII)
	SCGCQ00816998 - (Port_Complete) - HII drive menu does not show 0MB drives
	SCGCQ00817317 - (Port_Complete) - HII does not provide assigned group array info for dedicated HSP
	SCGCQ00817323 - (Port_Complete) - Question value mismatch while Replacing Drive and while view assocaiated Drive Gorup
	SCGCQ00817869 - (Active) - Handle CCVD Changes Based on new MR.h bit supportExtendedSSCSize
	SCGCQ00817947 - (Port_Complete) - Enclosure properties are not accurate in HII
	SCGCQ00817018 - (Port_Complete) - Enclosure properties are not accurate in HII
	SCGCQ00817316 - (Port_Complete) - HII drive menu does not show 0MB drives
	SCGCQ00826109 - (Port_Complete) - Create Cache Cade VD option still available even after MaxConfgiureSSCSize is crossed.
 BIOS - 6.25.03.0
	SCGCQ00826174 - (Closed) - 64VDs found on Host adapter eventhough more than 64 VDs are present
	SCGCQ00845247 - (Closed) - Overlap of controller boot messages with the footage message.
	SCGCQ00826176 - (Port_Complete) - 64VDs found on Host adapter eventhough more than 64 VDs are present
 NVDATA - 3.1507.00-0006
	SCGCQ00832538 - Customer requests NVDATA addition
	SCGCQ00838062 - NVDATA changes to RX_LOSVREF values
	SCGCQ00840530 - Review and check-in latest NVData
	SCGCQ00793911 - Customer requests NVDATA addition
	SCGCQ00828494 - NVDATA change request for OEM - enable biosEnumerateLds
	SCGCQ00816668 - ignore64ldRestriction to be set to 0 for specific controllers for a customer
	SCGCQ00841002 - ignore64ldRestriction to be set to 1 for specific controllers for a customer
	SCGCQ00828761 - Customer request to add 3108 ROMB PNP IDs
 Ctrl-R - 5.10-0700
	SCGCQ00786895 - (Closed) - The warning message is not shown when user tries to create CCVD greater than max configurable SSC size.
	SCGCQ00844775 - (Closed) - Handled the coverity defects.
	SCGCQ00843395 - (Closed) - Not able to enter ctrl-R when two controllers are connected with one having subOEM=1
	SCGCQ00828788 - (Closed) - CTRL_R PD Page display is not proper, when set up is configured in Multipath mode
	SCGCQ00817003 - (Closed) - Handle CCVD Changes Based on new API change
	SCGCQ00827049 - (Closed) - Storcli cannot create R10 in iMR with 6 or 8 drives per span.
	SCGCQ00827299 - (Closed) - Storcli crashes instead of showing error message on enabling caching on Source VDs and C
	SCGCQ00839186 - (Closed) - While toggling previous tab at random midst sequence of forward tab, MonTask is hit
	SCGCQ00837197 - (Closed) - Cachevault flash size shows differently for different commands in storcli under RHEL6.6 PPC64
	SCGCQ00837342 - (Closed) - New PD_Degraded media events are not logging correctly in PPC
	SCGCQ00837219 - (Closed) - Change EnclIndex with EnclosureDevice ID.
	SCGCQ00840372 - (Closed) - Read policy should be 'NORA' for IMR controller instead of 'none'
	SCGCQ00846882 - (Closed) - Handled the memory corruption.
	SCGCQ00820392 - (Closed) - Segmentation fault while querying for GHSP/DHSP while drive is going in shield-HSP state.
	SCGCQ00830435 - (Closed) - LDViewMirror is giving segmentation fault
	SCGCQ00839321 - (Closed) - Storcli gives wrong error code with respect to FW state while converting JBOD to UG
	SCGCQ00845545 - (Closed) - CTRL_R pops up wrong message, when trying to import CCVD configuration after downgrading the FW from 6.8 to 6.7
	SCGCQ00844167 - (Closed) - Allow CCVD Creation only if we have more than 1 GB space.
	SCGCQ00830269 - (Closed) - storcli /call show all fails with "command invalid"
	SCGCQ00835758 - (Closed) - Storcli shows caching is enabled on Source VD when CCVD is in offline state
	SCGCQ00839919 - (Closed) - Passphrase fails during post with 2 cards in system if we try to launch CTRL+R in between the cards initilization
	SCGCQ00828415 - (Closed) - Make semicolumn is sync with other Rates.
	SCGCQ00825003 - (Closed) - CTR_R providing the option to create CCVD, when full size CCVD[512GB] is already configured
	SCGCQ00819046 - (Closed) - Wrong PD/VD Size value in CtrlR
	SCGCQ00836472 - (Closed) - DATA TLB Error observed when trying to create 2nd sliced VD in Degraded R1 DG using CTRL_R
	SCGCQ00818101 - (Implemented) - Add set "Fail PD on SMARTer" property feature to StorCLI
	SCGCQ00829204 - (Implemented) - Increase maximum cache size for Cachecade to 2048GB. This will be named CC 2.5
	SCGCQ00816303 - (Implemented) - Improve the View of Controller Selection Menu
	SCGCQ00818987 - (Closed) - LimMod changes related to CtrlH & MSM Mismatch on write-back options - UI Inconsistancy issue
	SCGCQ00828476 - (Closed) - Storcli Should display SAS Address N/A if its invalid and change Host interface type names from PCIX, PCIE to PCI-X, PCI-E
	SCGCQ00789493 - (Closed) - Support decimal fraction for PD/VD size in HII
	SCGCQ00827665 - (Closed) - Implemented the VD-VF mapping related commands in factory tool
	SCGCQ00816311 - (Implemented) - CtrlH & MSM Mismatch on write-back options - UI Inconsistancy issue
	SCGCQ00817977 - (Closed) - Monitoring Drive performance and predictive failure
	SCGCQ00827316 - (Closed) - Increase maximum cache size for Cachecade to 2048GB. This will be named CC 2.5
	SCGCQ00833194 - (Port_Complete) - Command /cx/ex show phyerrorcounters gives bus error in Orcale Enterprise Linux
	SCGCQ00824446 - (Port_Complete) - StorCLI when ran on HBA that does not support battery, displays “Missing Battery”. (SCGCQ00820005)
	SCGCQ00822503 - (Port_Complete) - Segmentation fault while querying for GHSP/DHSP while drive is going in shield-HSP state.
	SCGCQ00832852 - (Port_Complete) - Consistent Sorting of Controllers for End Users in Customer Facing Tools (EFI storcli)
	SCGCQ00834687 - (Port_Complete) - Personality mode not present in storclif show all command
	SCGCQ00819317 - (Port_Complete) - Wrong PD/VD Size value in CtrlR
	SCGCQ00817885 - (Port_Complete) - Handle CCVD Changes Based on new API change
	SCGCQ00832372 - (Port_Complete) - Libmods changes for defect SCGCQ00823772: StorCLI version 1.14.14 does not allow access to both expanders
	SCGCQ00839833 - (Port_Complete) - StorCli show drive FW command not working correctly
 FCODE - 4.17.08.00
 BootBlock - 3.07.00.00-0002
 PCLI - 1.07.05
 ROMENV - 1.09


Firmware Package:24.8.0-0022 (MR 6.7 P1)
 Firmware 4.280.00-4310
	SCGCQ00781736 - (Closed) - Customer ROMB design GPIO/SGPIO drive LED question
	SCGCQ00808221 - (Closed) - Correctable ECC errors are not getting detected.
	SCGCQ00819314 - (Closed) - SSDs getting data with bad PI CRC.
	SCGCQ00819811 - (Closed) - When consistency check is aborted/suspended, HBA resets
	SCGCQ00825126 - (Closed) - Unexpected controller reset during test run
	SCGCQ00829214 - (Closed) - MR firmware exposes more than 240 VD's to the host, even when the host driver doesn't support more than 64VD's.
	SCGCQ00830847 - (Closed) - Block CCVD creation if the number of CCVd?s > 1 and CCVDs are associated with SVD
	SCGCQ00839323 - (Resolved) - Authentication Raid key Failed! err:1 error while issuing OCR with IOs on multiple VDs
	SCGCQ00844698 - (Closed) - Deleting a Cachecade VD (CC VD) results in a firmware hang situation.
	SCGCQ00831398 - (Closed) - Deleting a Cachecade VD (CC VD) results in a firmware hang situation.
	SCGCQ00838953 - (Closed) - Deleting a Cachecade VD (CC VD) results in a firmware hang situation.
	SCGCQ00763934 - (Closed) - Storcli show device link speed is confused for SATA/SAS drive when connected expander have buffer feature enable
	SCGCQ00812842 - (Closed) - Firmware will POST bios message when there is a romId mismatch and no features present on the controller
	SCGCQ00833765 - (Closed) - Failed to import iMR RAID configuration to 12G MR
	SCGCQ00798701 - (Closed) - 4K virtual drive missing across power cyle on iMR controller
	SCGCQ00830918 - (Closed) - EFI driver health fails when more than 64VDs configured
	SCGCQ00825725 - (Closed) - FW upgrade from non 240VD FW to 240VD FW when OS is behind the controller results in BSOD
	SCGCQ00770194 - (Closed) - Include learn cycle failure debug command in FW.
	SCGCQ00812722 - (Closed) - Single write COL with FBU03 for OEM
	SCGCQ00820593 - (Closed) - Program CVFM(Cache Vault Flash Module) VPD without Supercap connected.
	SCGCQ00758178 - (Closed) - MegaRAID CPLD update improvements
	SCGCQ00758184 - (Closed) - GG update to include concatenated GG/VPD data for Invader product generation.
	SCGCQ00812724 - (Closed) - FW change for single write to be fully supported for 2:4.
	SCGCQ00820067 - (Closed) - Request to remove the repeated ROC temperature warnings in ttylog when above 104 deg C.
	SCGCQ00784955 - (Port_Complete) - Virtual Disk GUID field changes when a VD is moved. The LUID is supposed to be unique and invariant.
	SCGCQ00790037 - (Port_Complete) - Firmware logs are not dumped to flash during device discovery phase
	SCGCQ00791671 - (Port_Complete) - Command timeout happens though the response returns in 130ms.
	SCGCQ00791672 - (Port_Complete) - Command timeout happens though the response returns in 130ms.
	SCGCQ00804284 - (Port_Complete) - Calculation for minimum blocks required to offload is wrong for single image configuration.
	SCGCQ00813167 - (Port_Complete) - Offload timed out for single image configuration
	SCGCQ00813744 - (Port_Complete) - Offload timed out for single image configuration
	SCGCQ00814987 - (Port_Complete) - GG update to include concatenated GG/VPD data for Invader product generation.
	SCGCQ00814997 - (Port_Complete) - Correctable ECC errors are not getting detected.
	SCGCQ00825773 - (Port_Complete) - OS (CentOS 7.0) crash observed while doing online FW update on IMR Fury controller
	SCGCQ00825774 - (Port_Complete) - Background IO's on 235 R0 VD's and abrupt enclosure power cable pull resulting into Fatal FW error
	SCGCQ00839018 - (Port_Complete) - After successful reconstruction of VDs, they are not getting reflected in MSM unless the user reboots the system
	SCGCQ00840631 - (Port_Complete) - MegaRAID CPLD update improvements
	SCGCQ00787362 - (Port_Complete) - Firmware logs are not dumped to flash during device discovery phase
	SCGCQ00789739 - (Port_Complete) - Virtual Disk GUID field changes when a VD is moved. The LUID is supposed to be unique and invariant.
	SCGCQ00791673 - (Port_Complete) - Command timeout happens though the response returns in 130ms.
	SCGCQ00813062 - (Port_Complete) - Offload timed out for single image configuration
	SCGCQ00821693 - (Port_Complete) - Controller commands are getting failed resulting in application hang when Logical Drive (LD) is deleted during reconstruction
	SCGCQ00825765 - (Port_Complete) - Command timeouts with cdb=ff ff ff ff
	SCGCQ00844697 - (Port_Complete) - Deleting a Cachecade VD (CC VD) results in a firmware hang situation.
	SCGCQ00844801 - (Port_Complete) - Behavior change when FW hit fault code 0x81 (uncorrectable ECC error)
	SCGCQ00797554 - (Port_Complete) - Flash of incorrect GG on controller, does not restore VDs back to WB
	SCGCQ00814991 - (Port_Complete) - Include learn cycle failure debug command in FW.
	SCGCQ00825775 - (Port_Complete) - FW breaks into montask while making VDs offline when rebuild is going on with IOs
	SCGCQ00826980 - (Port_Complete) - Card reporting SDRAM Unrecoverable Error
	SCGCQ00844704 - (Port_Complete) - Deleting a Cachecade VD (CC VD) results in a firmware hang situation.
	SCGCQ00814989 - (Port_Complete) - MegaRAID CPLD update improvements
 ROMENV 1.09
 BootBlock 3.07.00.00-0002
 NVDATA  3.1503.00-0007
 UEFI_Driver 0x060D0200 (SIGNED)
 Hii v03.13.09.00(SIGNED)
 FCODE 4.17.08.00
 BIOS 6.24.05.0
 Ctrl-R 5.09-0700
 PCLI 1.07.05

Firmware Package:24.8.0-0020 (MR 6.7)
 Firmware 4.280.00-4226
	SCGCQ00774946 - (Closed) - MCTP over PCI-E: Assertion failure while flashing a FW through PCI-E path.
	SCGCQ00783365 - (Closed) - Dev defect to support for Dynamic Discovery
	SCGCQ00783813 - (Closed) - Dev defect with Dynamic discovery after OCR all commands from SL are timing out
	SCGCQ00785425 - (Closed) - MCTP over PCI-E: GetOobStatus command fails when OOB in resume state.
	SCGCQ00785435 - (Closed) - MCTP over PCI-E : Set OOB poll parameters are not reflecting in Get OOB poll
	SCGCQ00785564 - (Closed) - MCTP over PCI-E: FW hang is observed, when we fire any MCTP command during OCR
	SCGCQ00787768 - (Closed) - Dev defect: datalength calculation for eventing is not same as in i2c
	SCGCQ00793028 - (Closed) - Flash of incorrect GG on controller, does not restore VDs back to WB
	SCGCQ00793616 - (Closed) - MR 6.7::FW breaks to montask on line /ssd/ssd_cache_fw.c
	SCGCQ00794102 - (Closed) - In controller safe mode, still can access existing data and run IO on JBODs (Normal JBOD, Secure JBOD and PI JBOD)
	SCGCQ00795015 - (Closed) - In certain conditions foreign import of CacheCade VDs may result in catastrophic failure in FW, incorrect CacheCade VD size display
	SCGCQ00798606 - (Closed) - FOREIGN secure JBOD should not be exposed to OS.
	SCGCQ00798960 - (Closed) - Change the string "pass phrase" to "password" in all applicable Firmware Boot Messages
	SCGCQ00801724 - (Closed) - Automatically Controller Security is getting enabled after OCR
	SCGCQ00805295 - (Closed) - During CCVD creation applications may send unaligned size to the FW.
	SCGCQ00805661 - (Closed) - MR_6.7: Fw hits MonTask: line 245 in file ../../raid/1078int.c while upgrading the FW
	SCGCQ00807500 - (Closed) - Firmware fails to import PRL 11 VD in certain scenarios.
	SCGCQ00807514 - (Waiting_Info) - R10 8x HDDs have a large variance in performance with 32K SW 64QD workload
	SCGCQ00809660 - (Closed) - 240VD mode SLT displays the Write Cache Capable as YES
	SCGCQ00810211 - (Closed) - After successful reconstruction of VDs, they are not getting reflected in MSM unless the user reboots the system
	SCGCQ00812608 - (Closed) - Background IO's on 235 R0 VD's and abrupt enclosure power cable pull resulting into Fatal FW error
	SCGCQ00812661 - (Closed) - Remove the code changes added as part of CSET SCGCQ00791478
	SCGCQ00813616 - (Closed) - 240VD - LD Sync fails while installing Linux OS with inbox driver
	SCGCQ00814777 - (Closed) - Command block not getting granted on completing a diverted fast path I/O due to divert lock
	SCGCQ00814937 - (Closed) - Users can't change default access policy of SVD when it blocked by SSC removal
	SCGCQ00815077 - (Closed) - Secure JBODs are not exposed to the OS if the drive were pushed out and inserted back.
	SCGCQ00815569 - (Closed) - MCTPoverPCIE :Firmware part for the defect SCGCQ00797846 :SL throws error 0x7009
	SCGCQ00816137 - (Closed) - HII: Generic RAID1 Profile based VD creation option is not grayed out after creating 64VD's.
	SCGCQ00817045 - (Closed) - ssdModifyMagicBlock() Copying the VDGUID into wrong buffer.
	SCGCQ00820121 - (Closed) - OS (CentOS 7.0) crash observed while doing online FW update on IMR Fury controller
	SCGCQ00822477 - (Closed) - MR6.7-Beta:FW hits to MonTask: line 1272 in file ../../raid/1078dma.c after Injecting media error in loop on CCVD metadata
	SCGCQ00829214 - (Closed) - MR firmware exposes more than 240 VD's to the host, even when the host driver doesn't support more than 64VD's.
	SCGCQ00770120 - (Closed) - MCTP_Firmware: Exception core 0 and MonTask: line 243 in file ../../raid/1078int.c on formating a non existing physical disk
	SCGCQ00774000 - (Closed) - PRL11 CCVD import fails with event in FW logs"C0:createMegaraidCfg-Offline VD pinned-this VD may not be fully inserted"
	SCGCQ00780472 - (Closed) - Dev defect : To include Code Review comments
	SCGCQ00780477 - (Closed) - Dev defect : Support for STP passthrough
	SCGCQ00788270 - (Closed) - Dev defect : Move all the mctp pcie related changes to pciemctp.c
	SCGCQ00791316 - (Closed) - MSM does not show VD info under logical tab when reconstruction operation running in 240VD mode
	SCGCQ00793264 - (Closed) - After recon IO request to LBA in LDBBM list is not getting diverted to FW.
	SCGCQ00794609 - (Closed) - SSD caching set to OFF throws success even when VDs are in Blocked state, through storcli.
	SCGCQ00795263 - (Closed) - 3008 iMR - VPD failure with PCI SIG validation tools
	SCGCQ00802118 - (Closed) - MR6.7:FW hits to MonTask: line 1272 in file ../../raid/1078dma.c after Injecting media error in loop on cachecade VD metadata
	SCGCQ00802640 - (Closed) - Kill adapter during I/Os on VD associated with CCVD and with policy change script
	SCGCQ00807136 - (Closed) - MR6.7:Wrong Queue Depth showing for(MR Controller)
	SCGCQ00809773 - (Closed) - iMR compilation with PLDEBUG enabled fails in 6.7 codebase
	SCGCQ00811274 - (Closed) - 6.7 Alpha : VDs are going to foreign config after issuing OCR
	SCGCQ00811296 - (Closed) - MR6.7: SVD's are getting 'Access Blocked' after OCR followed by System Reboot
	SCGCQ00822385 - (Closed) - iMR compilation with PLDEBUG enabled fails in 6.7 codebase
	SCGCQ00827605 - (Closed) - 6.7: Windows BSOD observed when upgrading from 6.6 to 6.7 through OFU when the OS is behind the controller
	SCGCQ00769474 - (Closed) - MCTP_PCIE: Can not create more than 3 vds at the same 
	SCGCQ00778601 - (Closed) - MCTP over PCI-E : On performing set/get operation through BMC while installing os , system rebooted automatically.
	SCGCQ00783761 - (Closed) - Dev defect: Eventing is not working
	SCGCQ00785004 - (Closed) - MCTP over PCI-E : BMC chip reset happens, when fw prints the message Got MRAPI more than 1 time for same application msgTag
	SCGCQ00785950 - (Closed) - MR6.7: FW breaks into montask while making VDs offline when rebuild is going on with IOs
	SCGCQ00792454 - (Closed) - System hang observed when writing to controller eeprom
	SCGCQ00794698 - (Closed) - MR6.7:Montask at line 1272 in file../raid/1078dma.c after degrading the Spanned DG SVD's
	SCGCQ00795483 - (Closed) - "Adapter at Baseport not responding" message seen in POST, after performing Cache Offload Scenario
	SCGCQ00798645 - (Closed) - 6.7 : Order of Freeing Limd and Chain frames is not proper.
	SCGCQ00798758 - (Closed) - Applications such as Ctrl R, HII, MSM etc shows "Maximum Allowed Unconfigured Good Drives" as 256
	SCGCQ00804029 - (Closed) - Continuous "TASK_ABORT_INTERNAL" prints observed in FW, after running heavy IO's on JBOD configured using 12Gig SAS SSD
	SCGCQ00804775 - (Closed) - CacheCade needs to check 32 MB non-aligned sizes for CCVD
	SCGCQ00812842 - (Closed) - Firmware will POST bios message when there is a romId mismatch and no features present on the controller
	SCGCQ00816234 - (Closed) - iMR hits Kill Adapter on running IO's on secure JBOD's
	SCGCQ00831050 - (Closed) - FW faults with 4 RAID6 VDs with 12Gb/s SSDs
	SCGCQ00716928 - (Closed) - CC2.5:Cahecade VD gets deleted on powercycling enclosure
	SCGCQ00769756 - (Closed) - MCTP Over PCIE:Assertion failure MonTask: line 656 in file ../../i2c/i2COobMgmt.c
	SCGCQ00795477 - (Closed) - FW should not allow "makeSystem" when "DriveErase" is going on
	SCGCQ00799517 - (Closed) - MR6.7:CC2.5- Found DATA TLB ERROR(SRR0/1,ESR) after drives pull out
	SCGCQ00805129 - (Duplicate) - MR & iMR FW Work-around is required for 3x08 chip Errata ID - 2012-RC714 for PCIE 3.0 compliance
	SCGCQ00812136 - (Closed) - DEV defect to check in the SCGCQ00795477 code changes
	SCGCQ00828709 - (Closed) - Write perf drop in 24R0 WB 256KB large QD
	SCGCQ00830918 - (Closed) - EFI driver health fails when more than 64VDs configured
	SCGCQ00638918 - (Closed) - Invader based controllers may be in config retry mode for more than 1 second
	SCGCQ00825725 - (Closed) - FW upgrade from non 240VD FW to 240VD FW when OS is behind the controller results in BSOD
	SCGCQ00812658 - (Closed) - Offload timed out for single image configuration
	SCGCQ00227735 - (Closed) - MPI 2.6 Add Atomic Request Descriptor capability
	SCGCQ00700829 - (Closed) - MPI 2.5: BIOS Page 1 additions
	SCGCQ00685820 - (Closed) - MPI 2.5: distribute Target Command Buffers Received across multiple reply queues
	SCGCQ00680527 - (Closed) - MPI v2.6: Added Intruder / Cutlass device IDs for manufacturing pages
	SCGCQ00623271 - (Closed) - MPI 2.6: Added an additional signature value for the firmware image header
	SCGCQ00619371 - (Closed) - MPI 2.6: Add new FLASH region types
	SCGCQ00259613 - (Closed) - MPI v2.6: Additional request and reply descriptor formats
	SCGCQ00264755 - (Closed) - MPI 2.6: SOP Encapsulated request
	SCGCQ00264759 - (Closed) - MPI 2.6: NVMe Encapsulated request
	SCGCQ00294055 - (Closed) - MPI 2.6: add Escape Passthrough bit to IO Flags of SCSI IO Request & Target Assist Request
	SCGCQ00294131 - (Closed) - MPI 2.6: update SGL chapter to include PCIe
	SCGCQ00336383 - (Closed) - MPI 2.6: PCIe IO Unit Page 0 & 1 definitions
	SCGCQ00345258 - (Closed) - MPI 2.6: add IO Unit Control Request
	SCGCQ00345260 - (Closed) - MPI 2.6: add PCIe Event Data (Generic), PCIe Device Status Change Event, and PCIe Enumeration Event
	SCGCQ00345266 - (Closed) - MPI 2.6: PCIe Topology Change List Event
	SCGCQ00345270 - (Closed) - MPI 2.6: PCIe Switch Config Pages
	SCGCQ00345271 - (Closed) - MPI 2.6: add PCIe Device Config Pages
	SCGCQ00353339 - (Closed) - Device Info field for PCIe devices
	SCGCQ00357551 - (Closed) - MPI 2.6: add host page size to IOCInit Request and IOCFacts Reply
	SCGCQ00360843 - (Closed) - MPI 2.6: add Port Request bit to IoFlags field of SCSI IO Request
	SCGCQ00363600 - (Closed) - MPI 2.6: move all SAS IO Unit Page 4 functionality to IO Unit Page 11
	SCGCQ00397136 - (Closed) - Modified address space bits
	SCGCQ00397563 - (Closed) - MPI 2.6: Add PCIe IO Unit Page 4
	SCGCQ00397568 - (Closed) - MPI 2.6: PCIe Device Page 2 reporting MDTS for NVMe devs
	SCGCQ00397572 - (Closed) - MPI 2.6: Add board power fields to IO Unit Page 7
	SCGCQ00397577 - (Closed) - MPI 2.6: Add support for SAS Persistent Connections
	SCGCQ00398256 - (Closed) - MPI 2.6: Add NVMe SGL support
	SCGCQ00432541 - (Closed) - MPI 2.6: Add NVMe SGL support to IEEE SGL
	SCGCQ00480292 - (Closed) - Remove _SATA_TRANSMIT_PORT_SELECT_SIGNAL in IO Unit Control Request
	SCGCQ00523879 - (Closed) - Identify physical location of a target device
	SCGCQ00566306 - (Closed) - Add type BIOS for HashImageType.
	SCGCQ00569175 - (Closed) - MPI 2.0: Add product-specific Flag bit to Clean Tool
	SCGCQ00574070 - (Closed) - MPI 2.6: Add additional NVMe AccessStatus codes
	SCGCQ00574358 - (Closed) - MPI2: Allow UEFI and BIOS to be Enabled/Disabled individually
	SCGCQ00601869 - (Closed) - MPI 2.6: Add BootFlags field to Firmware Image Header
	SCGCQ00732904 - (Closed) - Changes to enable controller receive\send PCIe generic message
	SCGCQ00787920 - (Closed) - vSAN iMR Queue Depth change to 256 (Short term)
	SCGCQ00789467 - (Closed) - Enable L3 auto flush with ON
	SCGCQ00792731 - (Closed) - Increase maximum cache size for Cachecade to 2048GB.
	SCGCQ00797237 - (Closed) - Change command block framework to avoid sentinel lk
	SCGCQ00799438 - (Closed) - Block OFU for Firmware Updates Which Do not support Extended Commands
	SCGCQ00812722 - (Closed) - Single write COL with FBU03
	SCGCQ00820593 - (Closed) - Program CVFM(Cache Vault Flash Module) VPD without Supercap connected.
	SCGCQ00613375 - (Closed) - Reconstruction from R0 to R1 in the presence of Media error deos not show ldbbm entries
	SCGCQ00785739 - (Closed) - Antares needs LED activity for JBOD Fastpath.
	SCGCQ00791114 - (Closed) - Avoid L3 flush in I/O path
	SCGCQ00802656 - (Closed) - Change to allow configuration of I2C control registers for 100KHz vs 400 KHz bus
	SCGCQ00820067 - (Closed) - Request to remove the repeated ROC temperature warnings in ttylog when above 104 deg C.
	SCGCQ00735061 - (Closed) - MCTP over PCIE : Handling of packet
	SCGCQ00787939 - (Closed) - MR FW- Update Attribution Language - Copyright, Trademark, Confidentiality to Avago
	SCGCQ00789373 - (Closed) - Don’t wait for flush when unnecessary during a command block
	SCGCQ00791450 - (Closed) - MR, iMR + MegaSR Support for 16 Byte CDB for ATA Microcode Download Pass-Thr
	SCGCQ00764376 - (Port_Complete) - To fix S3 wakeup issue when boot mode is set to ignore errors(HCOE/HSM).
	SCGCQ00766242 - (Port_Complete) - Delay OOB init until fw is operational
	SCGCQ00775673 - (Port_Complete) - TFM FAULT assertion does not change the VDs to Write-Through(WT) mode if no flag in Safety Status is set.
	SCGCQ00789444 - (Port_Complete) - GG update to include concatenated GG/VPD data for Invader product generation.
	SCGCQ00791476 - (Port_Not_Required) - Add prints in the FW that would be helpful while debugging
	SCGCQ00791478 - (Ready) - Snapshot and CacheCade section offsets in DDF workspace
	SCGCQ00791479 - (Port_Not_Required) - Supercap FAULT does not get asserted until temperature reaches 75 degrees celsius
	SCGCQ00793009 - (Port_Complete) - Include learn cycle failure debug command in FW.
	SCGCQ00794411 - (Port_Complete) - MCTPoverPCIE: MonTask: line 243 in file ../../raid/10 DATA TLB error on importing foreign config in Hermosa canyon(IMR) card.
	SCGCQ00799380 - (Port_Complete) - Supercap FAULT does not get asserted until temperature reaches 75 degrees celsius
	SCGCQ00799744 - (Port_Complete) - MCTPoverPCIE:Hermosa Canyon(IMR) Fatal firmware error: Line 152 in ../../raid/2108vDma.c on firing show configuration comma
	SCGCQ00801979 - (Port_Complete) - Firmware breaks into megamon with DATA TLB
	SCGCQ00804586 - (Port_Complete) - MCTP_PCIE: Dev defect to check-in the changes for the defect SCGCQ00793277
	SCGCQ00808206 - (Port_Complete) - Raid failure alerts are coming for the Card 9341 - 8i which doesn't support BBU
	SCGCQ00814987 - (Port_Complete) - GG update to include concatenated GG/VPD data for Invader product generation.
	SCGCQ00814997 - (Port_Complete) - Correctable ECC errors are not getting detected.
	SCGCQ00815610 - (Port_Complete) - Condado Beach- FW pkg 23.22.0-0017 and later initialize drives ~50% slower
	SCGCQ00825773 - (Port_Complete) - OS (CentOS 7.0) crash observed while doing online FW update on IMR Fury controller
	SCGCQ00825774 - (Port_Complete) - Background IO's on 235 R0 VD's and abrupt enclosure power cable pull resulting into Fatal FW error
	SCGCQ00829759 - (Port_Complete) - MR firmware exposes more than 240 VD's to the host, even when the host driver doesn't support more than 64VD's.
	SCGCQ00831408 - (Port_Complete) - EFI driver health fails when more than 64VDs configured
	SCGCQ00789426 - (Port_Complete) - MegaRAID CPLD update improvements
	SCGCQ00794414 - (Port_Complete) - MCTPoverPCIE:FW prints messageGot MRAPI more than 1 time for same application msgTag on performing get/set through BMC.
	SCGCQ00798518 - (Port_Complete) - Break mirrored VD starts rebuilding with original PD after doing clear config
	SCGCQ00799379 - (Port_Complete) - Add prints in the FW that would be helpful while debugging
	SCGCQ00800782 - (Port_Complete) - Calculation for minimum blocks required to offload is wrong for single image configuration.
	SCGCQ00810855 - (Port_Complete) - Remove Lock/Unlock of NOR flash by iMR and MR firmware function
	SCGCQ00810860 - (Port_Complete) - Flash Improvement
	SCGCQ00813062 - (Port_Complete) - Offload timed out for single image configuration
	SCGCQ00821693 - (Port_Complete) - Controller commands are getting failed resulting in application hang when Logical Drive (LD) is deleted during reconstruction
	SCGCQ00794413 - (Port_Complete) - Dev defect: commands fail with timeout even after firmware moves to ready state
	SCGCQ00795822 - (Port_Complete) - Increase size of FCT table to 64 for MR and 32 for iMR
	SCGCQ00799745 - (Port_Complete) - MCTPoverPCIE: SL fails to detect controller on uninitializing and initializing library while installing OS.
	SCGCQ00810153 - (Port_Complete) - Patrol Read Properties window does not pop up on MSM
	SCGCQ00810844 - (Port_Complete) - Read flash timeout from CFI instead of hardcoding
	SCGCQ00810848 - (Port_Complete) - Error Handling for Flash parts using Intel SCS command set
	SCGCQ00814991 - (Port_Complete) - Include learn cycle failure debug command in FW.
	SCGCQ00814998 - (Port_Complete) - Correctable ECC errors are not getting detected.
	SCGCQ00825775 - (Port_Complete) - MR6.7: FW breaks into montask while making VDs offline when rebuild is going on with IOs
	SCGCQ00769827 - (Port_Complete) - Monitor the Safety Status Register flags when fault is asserted and take appropriate actions whenever necessary.
	SCGCQ00799746 - (Port_Complete) - MCTPoverPCIE: DATA TLB Error MonTask: line 243 in file ../../raid/1078int.c on trying to clear foreignconfig in large config.
	SCGCQ00772350 - (Port_Complete) - Drive activity can toggled by the user
	SCGCQ00814989 - (Port_Complete) - MegaRAID CPLD update improvements
	SCGCQ00827738 - (Port_Complete) - FW upgrade from non 240VD FW to 240VD FW when OS is behind the controller results in BSOD
 BIOS 6.24.05.0
	SCGCQ00808086 - (Closed) - LegacyBIOS - Exposes "SecureJBOD" to system BIOS when 'Ask password at boot' entered wrongly
	SCGCQ00809682 - (Closed) - BIOS - Shows expander as JBOD in POST
	SCGCQ00808137 - (Closed) - BIOS - Line between "VDs handling" prints to be removed to match with "JBODs handling" prints
	SCGCQ00798656 - (Closed) - Legacy BIOS: Handle new changes of BBU doc related to Battery Status
	SCGCQ00799339 - (Closed) - Legacy OpROM : Legacy OpROM doesn't show proper PCI slot number on Intel WCP system.
	SCGCQ00826174 - (Closed) - Legacy OpROM: 64VDs found on Host adapter eventhough more than 64 VDs are pre
	SCGCQ00787941 - (Closed) - Update Attribution Language - Copyright, Trademark, Confidentiality to Avago
	SCGCQ00795550 - (Closed) - Legacy BIOS: Address BBU/Supercap inconsistent Behavior across HSW a
	SCGCQ00819752 - (Port_Complete) - Legacy OpROM : Legacy OpROM doesn't show proper PCI slot number on Intel WCP system.
	SCGCQ00819755 - (Port_Complete) - LegacyBIOS - Exposes "SecureJBOD" to system BIOS when 'Ask password at boot' entered wrongly
	SCGCQ00804825 - (Port_Complete) - Legacy OpROM : SSHA boot support
	SCGCQ00819756 - (Port_Complete) - BIOS - Shows expander as JBOD in POST
	SCGCQ00803146 - (Port_Complete) - Boot Device Selection in multi boot configuration
 NVDATA  3.1503.00-0005
	Numerous changes for specific customers
 UEFI_Driver 0x060D0200 (SIGNED)
	SCGCQ00819632 - (Closed) - Rebranding effort for OEM
	SCGCQ00813456 - (Closed) - UEFI Driver: Rebranding effort for OEM
	SCGCQ00787943 - (Closed) - Update Attribution Language - Copyright, Trademark, Confidentiality to Av
	SCGCQ00804835 - (Port_Complete) - UEFI Driver : SSHA boot support
	SCGCQ00804837 - (Por_Complete) - Syncro 2.1 SSHA: Direction bit is not set for READ CAPACITY comm
 Hii v03.13.09.00(SIGNED)
	SCGCQ00783374 - (Closed) - HII reports CCVD deleted even though its still under deletion process by FW
	SCGCQ00795338 - (Closed) - HII: SSD caching enabled on a Recon VD .
	SCGCQ00797318 - (Closed) - Change UCM form set title from AVAGO to LSI
	SCGCQ00810827 - (Closed) - HII : 3 times wrong password at boot time – Handle the 'Manage Foreign Configuration' page options properly with Secure JBOD present
	SCGCQ00798739 - (Closed) - HII Server profile shows "SILENCE ALARM" instead of "SERVER" subtitle as per design
	SCGCQ00799642 - (Closed) - In copyback window the Associated Virtual Drive shows free space only for replacing drive
	SCGCQ00804281 - (Closed) - MR6.7:FW hangs during SVD and CCVD migration based on DDR Size
	SCGCQ00806514 - (Closed) - After entering security key it goes back to Manage Foreign config page
	SCGCQ00816666 - (Closed) - HII: Handle CCVD Changes Based on new MR.h bit supportExtendedSSCSize
	SCGCQ00803946 - (Closed) - HII does not show HDD /SSD information for the PDs in HII Drive management and Advanced drive properties page
	SCGCQ00798824 - (Closed) - HII - NVRAM size shown as 32MB instead of 32KB
	SCGCQ00783558 - (Closed) - HII Dashboard very sluggish when you have a 240 VD foreign config
	SCGCQ00798579 - (Closed) - Schedule consistency check gives invalid time when change from diable to hour, daily, weekly and monthly.
	SCGCQ00798820 - (Closed) - Does not show RAID level for CCVD in 'VD management' and 'View DG properties' pages
	SCGCQ00811359 - (Closed) - Change the Media type before the protocol.
	SCGCQ00798684 - (Closed) - HII -> Drive management does not show "Secure" when JBOD created from a SED drive
	SCGCQ00798806 - (Closed) - HII - Schedule CC right side info pane to be corrected (Add Monthly and Change Disabled to Disable as per drop down box)
	SCGCQ00798962 - (Closed) - When Bootable JBOD is present under controller management ''Question value mismatch with option value'' window is displayed.
	SCGCQ00808162 - (Closed) - HII allows to set 4Kn VD or 4Kn JBOD as bootable device even though legacyBIOS does not handle it
	SCGCQ00810866 - (Closed) - Advanced Properties of VD are not displayed when it is Selected under Virtual Drive Management.
	SCGCQ00811295 - (Reworked) - MR6.7Alpha HII: Generic RAID1 Profile based VD creation option is not grayed out after creating 64VD's.
	SCGCQ00791138 - (Closed) - HII: Handle the maximum cache size value based on the max supported by FW, in the warning message shown during CCVD creation.
	SCGCQ00798657 - (Closed) - HII: Handle new changes of BBU doc related to Battery Stat
	SCGCQ00765822 - (Implemented) - Display the expander firmware version under Controller properties in HII when there is an expander on the controller
	SCGCQ00819734 - (Closed) - HII : Rebranding effort for OEM
	SCGCQ00789495 - (Closed) - RRB 87 - Suppress UEFI HII Clear Configuration setting
	SCGCQ00787943 - (Closed) - Update Attribution Language - Copyright, Trademark, Confidentiality to Avago
	SCGCQ00789505 - (Closed) - HII: Replace the word enclosure with expander for 720ix
	SCGCQ00797917 - (Implemented) - HII: MegaRAID CPLD update improvements
	SCGCQ00804082 - (Closed) - HII reports 'Security key entered is incorrect' even though it sent this request to FW and FW report as success.
	SCGCQ00787942 - (Implemented) - Update Attribution Language - Copyright, Trademark, Confidentiality to Avago
	SCGCQ00789504 - (Closed) - Consistency check date entry fix issue and Start Immediately option required in SCC form
	SCGCQ00787964 - (Closed) - HII: Address BBU/Supercap inconsistent Behavior across HSW a
	SCGCQ00804190 - (Port_Complete) - CS2.0: HII : Domain ID should be displayed under High Availability properties
	SCGCQ00804835 - (Port_Complete) - UEFI Driver : SSHA boot support
	SCGCQ00805041 - (Port_Complete) - HII Create VD: Show error message when user clicks on Apply Change without choosing drive group
	SCGCQ00820020 - (Port_Complete) - HII -> Drive management does not show "Secure" when JBOD created from a SED drive
	SCGCQ00795791 - (Port_Complete) - HII Dashboard very sluggish when you have a 240 VD foreign config
	SCGCQ00804183 - (Port_Complete) - HEFU HII : SSHA boot support
	SCGCQ00816998 - (Port_Complete) - HII drive menu does not show 0MB drives
	SCGCQ00819694 - (Port_Complete) - HII : 3 times wrong password at boot time – Handle the 'Manage Foreign Configuration' page options properly with Secure JBOD present
	SCGCQ00791312 - (Port_Complete) - In HII, Not able to create Spaned Virtual Disk R50,R60 Back to 
	SCGCQ00804193 - (Port_Complete) - Syncro 2.1 SSHA :Remove Provide Shared Access option of virtual drive property in HII since this option is not apply for SSHA
	SCGCQ00804837 - (Port_Complete) - Syncro 2.1 SSHA: Direction bit is not set for READ CAPACITY commands
	SCGCQ00820021 - (Port_Complete) - HII Create VD: Show error message when user clicks on Apply Change without choosing drive group
	SCGCQ00820023 - (Port_Complete) - HII: SSD caching enabled on a Recon VD .
	SCGCQ00820025 - (Port_Complete) - HII Server profile shows "SILENCE ALARM" instead of "SERVER" subtitle as per design
	SCGCQ00769769 - (Port_Complete) - Implement password EFI_IFR_FLAG_CALLBACK bit requirement from UEFI spec 2.4 Errata B
	SCGCQ00804182 - (Port_Complete) - Handling code review defects
	SCGCQ00804188 - (Port_Complete) - Syncro 2.0: Support for SED.
	SCGCQ00819701 - (Port_Complete) - After entering security key it goes back to Manage Foreign config page
	SCGCQ00769225 - (Port_Complete) - Syncro 2.1 SSHA: Direction bit is not set for READ CAPACITY commands
	SCGCQ00791320 - (Port_Complete) - HII reports CCVD deleted even though its still under deletion process by FW
	SCGCQ00804176 - (Port_Complete) - Incompatibility details are not displayed under HII properties
	SCGCQ00820018 - (Port_Complete) - HII allows to set 4Kn VD or 4Kn JBOD as bootable device even though legacyBIOS does not handle it
	SCGCQ00820024 - (Port_Complete) - HII - NVRAM size shown as 32MB instead of 32KB
	SCGCQ00803516 - (Port_Complete) - HA-DAS: Add HA support to HII
	SCGCQ00804175 - (Port_Complete) - HAMR: HII Create VD- advance sees default as no share
	SCGCQ00804181 - (Port_Complete) - HII - Provide support for toggling the controller to and from MAINTENANCE mode.
	SCGCQ00804184 - (Port_Complete) - Syncro 2.0 HII: Support for SSC & SSHA configuration.
	SCGCQ00820019 - (Port_Complete) - When Bootable JBOD is present under controller management ''Question value mismatch with option value'' window is displayed.
	SCGCQ00804191 - (Port_Complete) - Display operation mode only if supportMaintenanceMode is set
	SCGCQ00817018 - (Port_Complete) - Enclosure properties are not accurate in HII
	SCGCQ00804185 - (Port_Complete) - Syncro 2.0 HII: Remove the option to create non-shared VD in the SSHA configuration
	SCGCQ00804189 - (Port_Complete) - Syncro: VD Properties-Advanced-GUID Value left blank and add customization for the string STR_FORM_HF115_PHNA_HELP
	SCGCQ00810873 - (Port_Complete) - Deallocate the memory that was allocated for pPdList in SH_HF034_To_HF044()
	SCGCQ00826109 - (Port_Complete) - Create Cache Cade VD option still available even after MaxConfgiureSSCSize is cro
 ROMENV 1.09
 BootBlock 3.07.00.00-0002
 FCODE 4.17.08.00
 BIOS 6.24.05.0
 Ctrl-R 5.08-0006
 PCLI 1.07.05

Firmware Package:24.7.0-0026 (MR 6.6)
 Firmware 4.270.01-3972
	SCGCQ00573118 - (Closed) - Change the comments to reflect updated offsets of struct fields due to increase in VD bitmap size, wherever applicable
	SCGCQ00596373 - (Closed) - MR: foreign import does not happen on doing pull push of enclosure.
	SCGCQ00596403 - (Closed) - MR: fw is allowing to set cachecade for more than 64th VD.
	SCGCQ00596410 - (Closed) - MR: fw is allowing to set bootdrive for VD's after first 64
	SCGCQ00598804 - (Closed) - MR: fw is allowing to create more than 64 raid 5 VD's
	SCGCQ00598823 - (Closed) - MR: Firmware breaks into montask on creating virtual drive on spundown drive.
	SCGCQ00624906 - (Closed) - MR6.3_240VD: When trying to import Virtual Drives to a JBOD enabled firmware that does not support 240 Virtual Drives, physical drives with configuration come as JBOD
	SCGCQ00634632 - (Closed) - MR_240VD_ctrl-R: Cannot delete 64th VD from ctrl-R
	SCGCQ00637521 - (Closed) - VD policy is not proper when auto Configuration direct command is fired.
	SCGCQ00650083 - (Closed) - Fixed merge issues
	SCGCQ00669493 - (Closed) - Code Cleanup and porting code review defects from auto Configuration ER of Tbolt.
	SCGCQ00673189 - (Closed) - Fixing code compilation in 240 ld stream
	SCGCQ00695591 - (Closed) - Firmware times out when removing cable from enclosure #2 causing a adapter kill.
	SCGCQ00711787 - (Closed) - Enable DIS feature for 240VD Support
	SCGCQ00716430 - (Closed) - MR6.5_FW: Firmware breaks while FW Upgrade and Downgrade followed by Dirty Shutdown of System
	SCGCQ00735503 - (Closed) - To remove ignore64ldRestriction check
	SCGCQ00738986 - (Closed) - Thermal Throttle – add controller shutdown logic if the ROC temperature is greater than Junction temperature(>115).
	SCGCQ00755031 - (Closed) - MR6.6_FW: FW Breaks while doing target drive offline-online through apps when reconstruction is in progress.
	SCGCQ00758821 - (Closed) - Firmware displaying device ID for only one of the expanders connected in multipath
	SCGCQ00758866 - (Closed) - Invader 6.6 : OFU with Ios results in exception core 0
	SCGCQ00758942 - (Closed) - Correctable Errors seen in Link disable/enable C-script test
	SCGCQ00759837 - (Closed) - identify secured JBOD state appropriately on Drive hotplug
	SCGCQ00759926 - (Closed) - MR 6.6 : Firmware breaks into montask at line line 1992 in file ../../raid/cache.c
	SCGCQ00761018 - (Closed) - Resolving compilation warning
	SCGCQ00762277 - (Closed) - Seginus 240 drive test failed
	SCGCQ00762588 - (Closed) - Firmware breaks while creating virtual drives in iMR controller
	SCGCQ00764584 - (Closed) - MR FW 6.6 : Montask at line 1272 in file ../../raid/1078dma.c when trying to do recon on vd 0 when 64 vd is present.
	SCGCQ00765750 - (Closed) - Disallow disabling security key on controller if there are any secure JBODs.
	SCGCQ00767050 - (Closed) - MR 6.6 : Montask at line 1272 in file ../../raid/1078dma.c
	SCGCQ00773743 - (Closed) - Handle secure erase operation on SATA SSD
	SCGCQ00774042 - (Closed) - MR6.6_FW: Access policy remain as HD even after unhidding the VDs after restoring the configuration
	SCGCQ00775075 - (Closed) - Disable OOB debug message during I2C initialization
	SCGCQ00775121 - (Closed) - MR6.6_FW: Excluded Virtual Drives from CC get automatically included after checking CC properties through MSM
	SCGCQ00775267 - (Closed) - 3008 iMR - DPA extended capabilities bits structure is invalid
	SCGCQ00779343 - (Closed) - All apps showing "Battery Learn in Progress" after 5th timeout with a supercapacitor flashed with Bad gas gauge.
	SCGCQ00783613 - (Closed) - Firmware logs are not dumped to flash during device discovery phase
	SCGCQ00784722 - (Closed) - Changing FW between 240 VD and non 240 VD versions will cause drives to go Unconfigured good if CCVDs are created.
	SCGCQ00790104 - (Closed) - Devdefect: Reverting changes of MCTP from 6.6
	SCGCQ00791909 - (Closed) - BSOD observed when tried to install OS with inbox driver using 240VD firmware
	SCGCQ00793021 - (Closed) - PL fault iopiFault:FaultCode = 0000d10e observed, when removed drives were inserted back to the configuration
	SCGCQ00793037 - (Closed) - MR_6.6: OCR is not triggered in OEL 5.11 UEK kernal with MRdiag running in background.
	SCGCQ00800534 - (Resolved) - Performance with large block IOs (typically 64K and greater) have a large drop in performance while scaling QD with HDDs with R10 raid level
	SCGCQ00575707 - (Closed) - DCMD cleanup
	SCGCQ00625672 - (Closed) - fixed merge issues
	SCGCQ00627932 - (Closed) - MR_6.4_FW: On creating a 2 drive R0 WT CC VD and a 2 drive R1 WB CC VD, FW hits 6916 in file ../../ssd/ssd_cache_fw.c
	SCGCQ00637078 - (Closed) - Changed the logic of acquiring and releasing command block for hot plug case during auto Configuration (as part of 240 VD implementation) of physical drives.
	SCGCQ00702586 - (Closed) - Added check to use old FW_RAID_MAP for iMR controllers as 240VD feature is not supported for iMR.
	SCGCQ00705660 - (Closed) - Source VD's are getting lost after continuous back to back OCR with background IO's
	SCGCQ00718552 - (Closed) - Hit Montask while creating R0 CC VD using 4 1TB SSD drives
	SCGCQ00753530 - (Closed) - Post an event when Dirty data is discarded for LD under deletion
	SCGCQ00759158 - (Closed) - MR 6.6 Coverity Defects
	SCGCQ00759189 - (Closed) - Do not enable fast path on security enabled JBODs.
	SCGCQ00760713 - (Closed) - Not able to set autobgi=on/off through storcli for a hidden VD
	SCGCQ00760785 - (Closed) - Fix Coverity Defects
	SCGCQ00762388 - (Closed) - Drives are coming as Full size 1 Drive R0 upon same drive Hot Plug
	SCGCQ00765254 - (Closed) - Unable to change policies of auto configured VDs
	SCGCQ00767393 - (Closed) - DDF_WORKSPACE data structure is made backward compatible
	SCGCQ00774702 - (Closed) - Firmware breaks after foreign configuration import
	SCGCQ00777721 - (Closed) - MR_6.6: Disable of MCTP for integration release
	SCGCQ00781764 - (Closed) - Gas Gauge parameters are not updated for config change
	SCGCQ00595201 - (Closed) - Firmware crash is seen when reconstruction operation is started on a VD
	SCGCQ00601801 - (Closed) - MR : On trying to create RAID0 volumes on all drives, FW breaks into montask.
	SCGCQ00701768 - (Closed) - Bandwidth falls as queue depth increases on R5/R6 24/40Dr SATA HDD configurations at 256KSW block size
	SCGCQ00706915 - (Closed) - MR_240VD: On discarding Preserved cache, Consistency Check gets initiated on VD
	SCGCQ00758012 - (Closed) - coverity defect 15429
	SCGCQ00759131 - (Closed) - A particular bad TFM(CV) can cause FW OCR at boot time due to Montask
	SCGCQ00759973 - (Closed) - MR FW 6.6: AWB option support should be removed with CCVD.
	SCGCQ00763930 - (Closed) - JBOD feature got disabled upon foreign import
	SCGCQ00765466 - (Closed) - Drives are detected as UG after migrating 240VD config from MR to IMR controller
	SCGCQ00767157 - (Closed) - MR6.6:Montask at line 203 in file ../../raid/timer.c after PR is triggered from HII
	SCGCQ00767346 - (Closed) - CacheCade: Delete/ modify the unnecessary debug prints
	SCGCQ00768394 - (Closed) - fwDownload memory was freed in check_for_flush_over() before the fw upgrade process is initiated
	SCGCQ00772348 - (Closed) - CCVD policy fails to change the policy from WB to WT from MSM/Storcli
	SCGCQ00783354 - (Closed) - MR_6.6_ALPHA: Kill adapter found while deleting ld with discardcache
	SCGCQ00792440 - (Closed) - Montask observed at line 1026 in file ../../dm/src/dm.c with Enclosure Cable Pull/Push Scenario
	SCGCQ00573110 - (Closed) - Optimize host command dispatch code in set_state()
	SCGCQ00715154 - (Closed) - Event logging for incoming controller property value is done incorrectly.
	SCGCQ00755042 - (Closed) - Consistency check starts even on excluded virtual drives
	SCGCQ00763683 - (Closed) - Delay OOB init until fw is operational
	SCGCQ00765165 - (Closed) - 6.6 Coverity : For 15356, 15353, 15351, 15349 and 15345 defects
	SCGCQ00767348 - (Closed) - Firmware indicating that PD can be spun down even in online state
	SCGCQ00772255 - (Closed) - CRC calculated wrongly after NVRAM layout migration from legacy to new format
	SCGCQ00777096 - (Closed) - Instruction TLB error seen during reboot after all 240 VD's policy being changed
	SCGCQ00800530 - (Resolved) - 6.6 Beta code has a regression from 6.5 GCA in 64K RW workloads with 40x SAS HDDs
	SCGCQ00739663 - (Closed) - MegaRAID CacheCade Pro 2.0 Feature will deactivate on restart
	SCGCQ00755332 - (Closed) - Fail to import foreign drives in iMR controller
	SCGCQ00759941 - (Closed) - nomChgVoltage displaying wrong value.
	SCGCQ00760182 - (Closed) - 6.6 Coverity : CID 13587 and 10827
	SCGCQ00764459 - (Closed) - FW Breaks into MonTask: line 1968 in file ../../bbu/onfi.c on doing OCR with Pinned cache and setting termolog ON
	SCGCQ00780134 - (Closed) - Disable sgpioSmpPresenceDetect for specific customer
	SCGCQ00787285 - (Closed) - StorCLI crashed when tried to enquire LD information
	SCGCQ00761748 - (Closed) - drives were identified as JBOD by default; add condition to verify enableJBOD is set to 1
	SCGCQ00762592 - (Closed) - Workaround for Hardware Issue - SCGCQ00632364
	SCGCQ00757456 - (Closed) - Handle the deadlock scenario which could occur during ld deletion with Discarding the dirty data.
	SCGCQ00765315 - (Closed) - MR6.6_FW_240: Virtual Drive deleted after OCR during reconstruction
	SCGCQ00765738 - (Closed) - Controller crashes on running dual core capable writes on dual core capable volumes whose VD # is greater then 64
	SCGCQ00779326 - (Closed) - Displaying wrong CCVD size in all applications
	SCGCQ00227735 - (Closed) - MPI 2.6 Add Atomic Request Descriptor capability
	SCGCQ00680527 - (Closed) - MPI v2.6: Added Intruder / Cutlass device IDs for manufacturing pages
	SCGCQ00623271 - (Closed) - MPI 2.6: Added an additional signature value for the firmware image header
	SCGCQ00619371 - (Closed) - MPI 2.6: Add new FLASH region types
	SCGCQ00601869 - (Closed) - MPI 2.6: Add BootFlags field to Firmware Image Header
	SCGCQ00574070 - (Closed) - MPI 2.6: Add additional NVMe AccessStatus codes
	SCGCQ00259613 - (Closed) - MPI v2.6: Additional request and reply descriptor formats
	SCGCQ00264755 - (Closed) - MPI 2.6: SOP Encapsulated request
	SCGCQ00264759 - (Closed) - MPI 2.6: NVMe Encapsulated request
	SCGCQ00294055 - (Closed) - MPI 2.6: add Escape Passthrough bit to IO Flags of SCSI IO Request & Target Assist Request
	SCGCQ00294131 - (Closed) - MPI 2.6: update SGL chapter to include PCIe
	SCGCQ00336383 - (Closed) - MPI 2.6: PCIe IO Unit Page 0 & 1 definitions
	SCGCQ00345258 - (Closed) - MPI 2.6: add IO Unit Control Request
	SCGCQ00345260 - (Closed) - MPI 2.6: add PCIe Event Data (Generic), PCIe Device Status Change Event, and PCIe Enumeration Event
	SCGCQ00345266 - (Closed) - MPI 2.6: PCIe Topology Change List Event
	SCGCQ00345270 - (Closed) - MPI 2.6: PCIe Switch Config Pages
	SCGCQ00345271 - (Closed) - MPI 2.6: add PCIe Device Config Pages
	SCGCQ00353339 - (Closed) - Device Info field for PCIe devices
	SCGCQ00357551 - (Closed) - MPI 2.6: add host page size to IOCInit Request and IOCFacts Reply
	SCGCQ00360843 - (Closed) - MPI 2.6: add Port Request bit to IoFlags field of SCSI IO Request
	SCGCQ00363600 - (Closed) - MPI 2.6: move all SAS IO Unit Page 4 functionality to IO Unit Page 11
	SCGCQ00397136 - (Closed) - Modified address space bits
	SCGCQ00397563 - (Closed) - MPI 2.6: Add PCIe IO Unit Page 4
	SCGCQ00397568 - (Closed) - MPI 2.6: PCIe Device Page 2 reporting MDTS for NVMe devs
	SCGCQ00397572 - (Closed) - MPI 2.6: Add board power fields to IO Unit Page 7
	SCGCQ00397577 - (Closed) - MPI 2.6: Add support for SAS Persistent Connections
	SCGCQ00398256 - (Closed) - MPI 2.6: Add NVMe SGL support
	SCGCQ00432541 - (Closed) - MPI 2.6: Add NVMe SGL support to IEEE SGL
	SCGCQ00480292 - (Closed) - Remove _SATA_TRANSMIT_PORT_SELECT_SIGNAL in IO Unit Control Request
	SCGCQ00552730 - (Closed) - Auto Configuration of Raid 0 volumes for 240 VD requirement.
	SCGCQ00563479 - (Closed) - Convert all 64-bit LD bitmaps to a generic bitmap mechanism, and RAID_MAP API changes
	SCGCQ00574463 - (Closed) - Integrating MR APIs for 240LD support into firmware
	SCGCQ00600962 - (Closed) - NVRAM migration from LEGACY to EXT format and NVRAM EXT struct reformatting (cleanup)
	SCGCQ00601214 - (Closed) - Write new extended DDF format on the physical drives.
	SCGCQ00710437 - (Closed) - Long term API solution, ability to change disableImmediate from MFI API
	SCGCQ00712485 - (Closed) - Expanders with diffrent SAS address but same ELI shown as single device
	SCGCQ00774902 - (Closed) - Match the FW configuration with our latest Gas Gauge settings for an OEM
	SCGCQ00732904 - (Implemented) - Changes to enable controller receive\send PCIe generic message
	SCGCQ00751803 - (Closed) - Enable 16k SS for custom business
	SCGCQ00573772 - (Closed) - DDF module changes to support 240 Virtual Drives.
	SCGCQ00625447 - (Closed) - Enabled R5/R6 240 VD support
	SCGCQ00741705 - (Closed) - Support 128K bypass threshold
	SCGCQ00571124 - (Closed) - implement IO path and NVRAM changes
	SCGCQ00712501 - (Closed) - LD Deletion stalling all IOs on Niwot HBA 12.12.0-0178
	SCGCQ00735061 - (Closed) - MCTP over PCIE : Handling of packet
	SCGCQ00711560 - (Closed) - Enable security on JBOD
	SCGCQ00751088 - (Closed) - Command block optimizations to avoid IO stalls
 BIOS 6.22.03.0
	SCGCQ00769239 - (Closed) - Don't issue REAID I/O on the 4K JBOD
	SCGCQ00783579 - (Closed) - Auto Select Boot device (alias multiboot): INT13 drive type is not set correctly for physical disk
	SCGCQ00769269 - (Closed) - Before calling Translate_LdTargetIdList_To_LdList set int13 drive type
	SCGCQ00550426 - (Closed) - Increase OpROM code size from 40k to 48k
 NVDATA  3.1411.01-0007
	Numerous changes for specific customers
 UEFI_Driver 0x060B0200 (SIGNED)	
	SCGCQ00638308 - (Closed) - FMP GetImageInfo could result in stack corruption - Code Review Defect ID D26304
	SCGCQ00335617 - (Closed) - Drives are reporting timeout on Write Buffer cmd on H310 and Nautilus.efi
	SCGCQ00378953 - (Closed) - HII not showing up + other enhancement for driver health formset
	SCGCQ00413986 - (Closed) - HII app doesnt appear when there is critical message and when platform uses SetOptions
	SCGCQ00479003 - (Closed) - Disable Debug print in UEFI Driver
	SCGCQ00618669 - (Closed) - UEFI Driver: StartHiiBackEnd() has Print statement with %g
	SCGCQ00320619 - (Closed) - UEFI: Build Device Path and Get Next Target function of SCSI Pass Thru is not returning correct EFI status for certain cases
	SCGCQ00339371 - (Closed) - UEFI Driver fails SCT Test
	SCGCQ00408333 - (Closed) - UEFI: Critical boot message formatting issue
	SCGCQ00691044 - (Closed) - Code refactor effort: Hii Image buffer clean-up
	SCGCQ00347171 - (Closed) - MR: on having pinned cache on oem -2GB controller, the option to invoke storage doesn't come.
	SCGCQ00384884 - (Closed) - Customize health formset + few other issues
	SCGCQ00395190 - (Closed) - HII - 03.02.03.00/When trying to create an R6/R5, I am unable to create though there are 3 SAS unconfigured good avail
	SCGCQ00396051 - (Closed) - UEFI Driver (MR 5.7) should not display finite boot messages
	SCGCQ00435384 - (Closed) - UEFI System hang if controller FW is in fault state
	SCGCQ00732773 - (Closed) - UEFI Driver: If the platform contains UEFI Spec Rev < than 2.3.0, then don't HII
	SCGCQ00688789 - (Closed) - DHP: Remove default value from numeric primitive that is present under suppressif
	SCGCQ00343869 - (Closed) - Enhance critical boot message handling
	SCGCQ00369636 - (Closed) - UEFI: Settime only when FW time is not set; DHP: Return appropriate health status when there is no critical boot message
	SCGCQ00408094 - (Closed) - Supermicro system with a critical message does not enter EFI preboot config utility
	SCGCQ00498925 - (Closed) - Not able to boot into BIOS boot menu in oem server
	SCGCQ00756810 - (Closed) - PKG 9 HII form/When you have a a critical message such as missing VDs, after select "C" <ENTER>, it will show an assert
	SCGCQ00312683 - (Closed) - UEFI Driver not timing out in 3 mins when FW is in undefined state
	SCGCQ00726723 - (Closed) - Ext/SCSI PassThru: UEFI Driver not filling direction flag correctly for Read
	SCGCQ00518791 - (Closed) - DriverDiagnostics2.c: In IsValidHandle() - Free the buffer if status is not EFI success for LocateHandle
	SCGCQ00493654 - (Closed) - Memory Leak issue in UEFI driver when reconnect happens
	SCGCQ00715450 - (Closed) - .
	SCGCQ00308870 - (Closed) - EFI Driver 518\When disconnecting the driver in EFI, I am still able to exectue the EFI utility menu.
	SCGCQ00696656 - (Closed) - Update Mbox value for 240VD Support
	SCGCQ00601851 - (Closed) - System hang when we press F1 on second time when we are in HII form
	SCGCQ00578194 - (Closed) - UEFI Driver should calculate checksum before setting bios data (MR_BIOS_DATA)
	SCGCQ00262858 - (Closed) - Debug message is shown from EFI app choice prompt on a Yilan system
	SCGCQ00589148 - (Closed) - Diskpart EFI utility can't create partition on a JBOD
	SCGCQ00483847 - (Closed) - EKMS: Remove private GUID and use EFI_KMS_PROTOCOL_GUID defined in UEFI 2.3.1 spec
	SCGCQ00628310 - (Closed) - Install FMP on Controller Handle at Start() and the exception
	SCGCQ00340581 - (Implemented) - UEFI Driver should check pMRCtrlInfo ->maxHANodes with > 1 to determine HAMR
	SCGCQ00365374 - (Implemented) - Add 3108 device ID for oem
	SCGCQ00385365 - (Closed) - UEFI Driver (FoD): 
	SCGCQ00285974 - (Implemented) - Add 4k sector boot support in UEFI Driver
	SCGCQ00404216 - (Closed) - Add 3008 device ID for iMR product.
	SCGCQ00318101 - (Closed) - Timed critical boot message under UEFI mode
	SCGCQ00347492 - (Closed) - UEFI: Retry read capacity if scsi status is not success
	SCGCQ00395996 - (Closed) - UEFI Driver: Parse Boot message and remove \r\n at the beginning and replace \n with \r in other parts
	SCGCQ00526851 - (Closed) - Support EFI_FIRMWARE_MANAGEMENT_PROTOCOL for controller firmware upgrade.
	SCGCQ00292963 - (Implemented) - UEFI Driver: LSIP200198414/LSIP200229508/LSIP200231613: Disables all requirement for human input at boot time
	SCGCQ00331573 - (Closed) - MR_UEFI_Driver: Remove dependency on deprecated Driver Configuration2 protocol from UEFI Driver
	SCGCQ00392836 - (Closed) - LSI to Support Remote Key Management
	SCGCQ00278257 - (Implemented) - Add FoD support for 3108 for oem
	SCGCQ00436609 - (Closed) - oem add PnPID's for 3004 and 3108
	SCGCQ00338782 - (Implemented) - If SetOptions is called for Invader don't show EFI WebBIOS and EFI CLI option
	SCGCQ00338066 - (Implemented) - UEFI - HAMR: Fire LD list query based on maxHANodes
	SCGCQ00550389 - (Closed) - WebCloud Group - Write Caching HBA, JBOD/R0 supported TB controller with 240 SystemPD/LD support
	SCGCQ00626601 - (Implemented) - VT-d/IOMMU support for iMR - Implement mechanism to allow system BIOS to put entries for iMR mem allocation into proper table
	SCGCQ00310476 - (Implemented) - Load HII when user responds to critical boot message by pressing C
	SCGCQ00650086 - (Implemented) - UEFI Driver UDK2010 compliance
	SCGCQ00635878 - (Port_Complete) - UEFI Driver- has debug print statements during POST
	SCGCQ00688987 - (Port_Complete) - Don't let user boot to OS until user discards dirty cache
	SCGCQ00484086 - (Port_Complete) - Sandstorm platfrom has UEFI hang when SATA is connected (the issue discovered in pre-dev 13G platform)
	SCGCQ00677776 - (Port_Complete) - Initialize the buffer that we allocate to load HII and return EFI_OUT_OF_RESOURCES if allocation fails
	SCGCQ00678154 - (Port_Not_Required) - For oemdont free the host memory during disconnect/unload process
	SCGCQ00736761 - (Port_Complete) - Return health status failed if we have returned device error from Start()
	SCGCQ00756861 - (Port_Complete) - ControllerInfo[CtrlIndex].ControllerHandle got initialized incorrectly or too early
	SCGCQ00468948 - (Port_Complete) - Uninstall HII CAP and Driver Health formset if platform calls Start again without calling GetHealthStatus
	SCGCQ00477828 - (Port_Complete) - 9240/9260/9270 UEFI driver issue with RD640/RD440 platforms when user having 2TB or 4TB VD
	SCGCQ00679073 - (Port_Complete) - Do not go to WebBIOS due to a bad health status when WebBIOS is disabled in NVDATA.
	SCGCQ00695249 - (Port_Complete) - Safe guard: Return health status failed if platform calls GetHealthStatus w/ NULL handle after we return intermediate status
	SCGCQ00716623 - (Port_Complete) - For oem change memory type from EfiRuntimeServicesData to EfiMemoryMappedIO
	SCGCQ00606367 - (Port_Complete) - UEFI Driver returns EFI_NOT_FOUND when platform passes valid Target for ExtSPT.BuildDevicePath()
	SCGCQ00644508 - (Port_Complete) - CPU EXCEPTION ERROR During CSIOR Stage- After Updating idrac X38 to X39 (Don't double free the memory)
	SCGCQ00478692 - (Port_Complete) - Block IO tests from SCT IHV test suite failed
	SCGCQ00484114 - (Port_Complete) - ATA PT: Follow UEFI Spec on interpreting In and Out Transfer Length that upper layer sends
	SCGCQ00580313 - (Port_Complete) - User can't access RAID HII in UEFI mode after removing a HDD
	SCGCQ00658168 - (Port_Complete) - ATA Pass thru: Timeout is not passed correctly to FW
	SCGCQ00716622 - (Port_Complete) - For oem don't free the host memory during disconnect/unload process
 Hii v03.11.08.00(SIGNED)
	SCGCQ00740787 - (Closed) - Cloning (alias Save/Restore) : HII issues Add Config when there is no config
	SCGCQ00764936 - (Closed) - Schd CC page/Consistency Check mode does not explain the difference between sequential & concurrent
	SCGCQ00768459 - (Closed) - HII 5.13 PKG 01/Enclosure Management screen and Drive managment screen do not match
	SCGCQ00771730 - (Closed) - HII: Locked PD is shown in Preview Foreign Configuration form.
	SCGCQ00758589 - (Closed) - Dashboard View Help Content: Reuse the string where possible and incorporate following changes suggested by tech pub
	SCGCQ00762860 - (Closed) - HII Dashboard/3.11.02.00/View server profile is showing two periods after the word "them" under Hardware Components
	SCGCQ00767605 - (Closed) - When you have a locked PD/FDE in a foreign state, it is not showing up on the dashboard only under configure
	SCGCQ00783556 - (Closed) - Question value mismatch when Fan3 and 4 is selected
	SCGCQ00756533 - (Closed) - Remove FRU from Enclosure Management
	SCGCQ00762856 - (Closed) - HII Dashboard/3.11.02.00/When preview foreign config from Dashboard, it is coming up as HF034 at the top
	SCGCQ00783558 - (Closed) - HII Dashboard very sluggish when you have a 240 VD foreign config
	SCGCQ00784597 - (Closed) - HII Configuration Management Enable Security On JBOD OK button is grayed out
	SCGCQ00783374 - (Closed) - HII reports CCVD deleted even though its still under deletion process by FW
	SCGCQ00714530 - (Closed) - HII: Firmware Update - On selecting empty folder, hang is seen.
	SCGCQ00755277 - (Closed) - Change "Consistency Check" to "Make Data Consistent" for CC Rate and Stop CC on error is not changed
	SCGCQ00770227 - (Closed) - HII displays supercap module version as "Firmware Version"
	SCGCQ00771193 - (Closed) - HII: Entering security key in HII to unlock PD fails to import afterwards
	SCGCQ00765519 - (Closed) - HII: R5/R6 creation fails in HII from Profilebased creation
	SCGCQ00755021 - (Closed) - HII 6.6: Operation's are not refreshed in Dashboard
	SCGCQ00760501 - (Closed) - DashBoard HII showing 1 enclosure connected even though there are 0 connected.
	SCGCQ00766787 - (Closed) - HII- DHS assigning fails in presence of 240 Vds
	SCGCQ00765523 - (Closed) - Invader 6.6: HII : BGops fails to start when VD erase is already running on the other VD
	SCGCQ00760435 - (Closed) - Date getting corrupted when selecting different Check Consistency Frequencies
	SCGCQ00768437 - (Closed) - Entering the wrong security key in HII & go back to enter the correct one the security key form should be cleared
	SCGCQ00684992 - (Closed) - Question about "Connected Port" in PD advance menu
	SCGCQ00779364 - (Closed) - Wrong drivegroup count shown with foreign config in safe mode
	SCGCQ00767138 - (Closed) - HII: Controller in Safe Mode - ASSERTs seen on console during the Preview of Foreign Configuration
	SCGCQ00765244 - (Closed) - Dashboard: comment out the refresh interval for all other fields except controller status.
	SCGCQ00756640 - (Closed) - MR_6.6_HII: In configuration Management creation of JBOD not possible as option to set JBOD is grey out.
	SCGCQ00761105 - (Closed) - Dashboard/HII 03.11.02.00/Using generic oem Controller or oem controller yields spaces in HII Dash
	SCGCQ00764215 - (Closed) - HII 5.13 PKG 01/3.11.02.00/Preview foreign configuration screen missing words
	SCGCQ00776052 - (Closed) - 5.13 HII PKG 02/When creating a VD that is more than 1TB in size in HII, you will loose the extra space after saving the VD
	SCGCQ00778462 - (Closed) - HII Boot time Asserts
	SCGCQ00760450 - (Closed) - HII: Need to remove Force Write Back option with CCVD creation
	SCGCQ00742103 - (Closed) - Remove Head Of Queue rebuild feature
	SCGCQ00750118 - (Closed) - Remove Head Of Queue rebuild feature
	SCGCQ00756784 - (Closed) - Chk the err status for HL_Get_PD_List() and HL_Get_PD_Info in UF002_PrepareData() + check Driver handle if index is valid
	SCGCQ00760432 - (Closed) - Getting question value mismatch when changing the Consistency check Frequency settings
	SCGCQ00768009 - (Closed) - HII : Locked PD on controller with security disabled does not show properly when viewing under Foreign config
	SCGCQ00730596 - (Closed) - UEFI: Refreshing individual field (in this case progress field)
	SCGCQ00711563 - (Closed) - RRB 71 - enable SED support for iMR JBOD
	SCGCQ00721161 - (Closed) - SAS3: HII Create Virtual Drive advanced option defaults Protect Virtual Drive to enabled
	SCGCQ00712484 - (Closed) - HII. Create dashboard view as a landing form in HII
	SCGCQ00756855 - (Port_Complete) - Chk the err status for HL_Get_PD_List() and HL_Get_PD_Info in UF002_PrepareData() + check Driver handle if index is valid
	SCGCQ00765468 - (Port_Complete) - Hardware Component Details are not being displayed under Hardware Components
	SCGCQ00780729 - (Port_Complete) - Enclosure properties are not accurate in HII
	SCGCQ00757730 - (Port_Complete) - Help string corrections + Suppress subtitle CACHECADE + Change Safe mode to Safe mode on errors
	SCGCQ00768167 - (Port_Complete) - H730p battery's manufacture date can be set to any date in the controllers HII environment
	SCGCQ00790204 - (Port_Complete) - 2TB and 4TB HDD show 1TB and 3TB in HII
 Ctrl-R 5.08-0006
	SCGCQ00759987 - (Closed) - CTRL+R: AWB option support with CCVD should not be there.
	SCGCQ00725192 - (Closed) - H330: Firmware Crash is hit while creating the Raid1 vd without drives selected
	SCGCQ00756647 - (Closed) - 6.6_StorCli: StorCli lists all cascaded enclosures at position 0.
	SCGCQ00757358 - (Closed) - Add adapterOperation support details in /c0 show all for cachebypassMode.
	SCGCQ00758770 - (Closed) - FW breaks in iMR when excluding VD's from CC
	SCGCQ00759187 - (Closed) - Boot Volume details is shown in Megacli but not with storcli.
	SCGCQ00759290 - (Closed) - SSM-FLASh drives property is displayed for regular drives.
	SCGCQ00759862 - (Closed) - OEMID is coming as "Unknown" for /c0 show all
	SCGCQ00761937 - (Closed) - MR 6.6 Prealpha2 Storcli:Similar PCI address(BDF number) is displayed for multiple controllers connected to FreeBSD 9.3.
	SCGCQ00771626 - (Closed) - Storcli errors are printing in a different line.
	SCGCQ00772243 - (Closed) - StorCLI shows CacheBypass Size and CacheBypass Mode feature enabled against a VD which is associated with a CacheCade VD
	SCGCQ00772302 - (Closed) - Storcli has option to set PR maxconcurrentpd but show is not present
	SCGCQ00772332 - (Closed) - vpdpage should be read from 4 bytes to get serial number of drive
	SCGCQ00779789 - (Closed) - Active operation(s) is coming as none when virtual drive erase is in progress.
	SCGCQ00779800 - (Closed) - MR6.6_CLI_FreeBSD: Displaying incorrect Driver name
	SCGCQ00783357 - (Closed) - CTRL-R:2 iMR Card in same System hitting Montask
	SCGCQ00790050 - (Closed) - "./storcli64 /c0 show all page" shows "cachevault flash size = 8.0 ZB
	SCGCQ00764750 - (Closed) - MR6.6_Ctrl+R: Not able to see Advanced Software Option (ASO) in Virtual Drive Management
	SCGCQ00759181 - (Closed) - Add adapterOperation support details in /c0 show all for Emulationtype.
	SCGCQ00759969 - (Closed) - Adapters are not listed in sorted order.
	SCGCQ00765759 - (Closed) - StorCLI shows wrong "Number of blocks" for a 65.5TB VD size
	SCGCQ00765762 - (Closed) - StorCLI VMware Binary not displaying detailed description for phyerrorcounters of enclosures
	SCGCQ00767347 - (Closed) - Patrol read delay is showing wrong value when set to continuous
	SCGCQ00778577 - (Closed) - GB scale to be added while showing CacheCade size in CLI
	SCGCQ00779806 - (Closed) - ASO count mismatch in show ASO w.r.t ASO in storcli show all cmd
	SCGCQ00782882 - (Closed) - MR6.6:StorCLI shows incorrect information about "Cache Vault Flash Size"
	SCGCQ00785679 - (Closed) - MR 6.6 Apha: Controllers are not sorted according to BDF(bus device function) in CTRL-R.
	SCGCQ00777828 - (Closed) - CTRL-R reports CCVD deleted even though its still under deletion process by FW
	SCGCQ00760989 - (Closed) - CTRL-R: FW hits MonTask, When CTRL-R is launched immediately after the MR Controller initialization is complete and before the iMR card initialization starts in the BIOS POST.
	SCGCQ00752000 - (Closed) - In Windows and Linux only controller grouping is working but not sorting
	SCGCQ00758101 - (Closed) - MR_6.6_Storcli: Storcli reports supercap state 'unknown' while learn is happening on the controller.
	SCGCQ00759183 - (Closed) - SED adapterOperation detailed is not shown in detailed show controller properties
	SCGCQ00759959 - (Closed) - Support details are not shown in /c0 show all for discard cache (stalling LD deletion)
	SCGCQ00760385 - (Closed) - MR_6.6: StorCLI showing incorrect value for next Schedule time for consistency check after disabling the CC
	SCGCQ00762663 - (Closed) - Storclio : Different error code is coming for 'set pcilinkspeed' in VMware 4.1U3
	SCGCQ00764658 - (Closed) - StorCLI /c0 show all command does not reflect the discard vd delete filed
	SCGCQ00765714 - (Closed) - StorCLI shows CacheBypass Size and CacheBypass Mode feature enabled against a CacheCade VD
	SCGCQ00767363 - (Closed) - Showing wrong creation date for Autoconfigured virtual drives
	SCGCQ00785400 - (Closed) - VD level hide/unhide is not possible through storcli in PPC
	SCGCQ00790062 - (Closed) - "./storcli64 /c0 show cc" fails in RHEL 6.6 PPC64 with more than 64 VDs present
	SCGCQ00756487 - (Closed) - Incorrectness in the popupmenu generated for the controller info when controller is in Safe Mode
	SCGCQ00765643 - (Closed) - Ctrl+R not handling VD policy change error case for Autoconfigured Virtual Drives
	SCGCQ00730505 - (Closed) - After Rebuilding, DHS and Expand VD operations failed to update as per VD properties
	SCGCQ00758924 - (Closed) - Exception with command /co show badblocks or "storcli /cx flasherase"
	SCGCQ00759178 - (Closed) - SupportMaxRate SATA is not listed in PD allowed operations.
	SCGCQ00760398 - (Closed) - MR6.6: Segmentation fault (Core Dumped) in CLI when setting any invalid value for PR start time
	SCGCQ00760752 - (Closed) - /c0 show all does not list hwCfg information as compared to MegaCLI.
	SCGCQ00790022 - (Closed) - ./storcli64 /c0 show pr gives segmentation fault on PPC with more than 64 VDs
	SCGCQ00755063 - (Closed) - Add support bits for uneven-span and SSHA support
	SCGCQ00765712 - (Closed) - StorCLI is not updated with the error Message for all new MFI_STAT added in mfistat.h
	SCGCQ00786895 - (Closed) - MR 6.6 CTRL-R: The warning message is not shown when user tries to create CCVD greater than max configurable SSC size.
	SCGCQ00786830 - (Closed) - In 2 iMR controller environment switching between iMR cards hits MonTask
	SCGCQ00758768 - (Closed) - Incorrectness in the confirmation popupmenu while creation of VD from available size.
	SCGCQ00760689 - (Closed) - CTRL+R: not able to set cacheflushint value to 255 for MR card.
	SCGCQ00760972 - (Closed) - Error code coming as "Unknown" while importing Foreign Configuration, when controller is in Safe Mode
	SCGCQ00696872 - (Closed) - Consistent Sorting of Controllers for End Users in Customer Facing Tools
	SCGCQ00735171 - (Closed) - Implemented the storcli command to print SATA drive's phy error counters and reset them.
	SCGCQ00755527 - (Closed) - Enable SED on JBOD
	SCGCQ00711564 - (Implemented) - RRB 71 - enable SED support for iMR JBOD
	SCGCQ00750164 - (Closed) - RRB 71 - enable SED support for iMR JBOD
	SCGCQ00757473 - (Closed) - LD Deletion stalling all IOs on oem HBA 12.12.0-0178
	SCGCQ00696872 - (Closed) - Consistent Sorting of Controllers for End Users in Customer Facing Tools
	SCGCQ00735171 - (Closed) - Implemented the storcli command to print SATA drive's phy error counters and reset them.
	SCGCQ00755527 - (Closed) - Enable SED on JBOD
	SCGCQ00711564 - (Implemented) - RRB 71 - enable SED support for iMR JBOD
	SCGCQ00750164 - (Closed) - RRB 71 - enable SED support for iMR JBOD
	SCGCQ00757473 - (Closed) - LD Deletion stalling all IOs on oem HBA 12.12.0-0178
 ROMENV 1.09
 BootBlock 3.06.00.00-0001
 FCODE 4.16.08.00
 PCLI 1.07.05

 Firmware Package:24.6.0-0036 (MR 6.5 point release 2)
	MR Firmware 4.260.00-4046
		SCGCQ00798701 - (Closed) - 4K virtual drive missing across power cyle on iMR controller 
		SCGCQ00808221 - (Closed) - Correctable ECC errors are not getting detected.
		SCGCQ00770194 - (Closed) - Include learn cycle failure debug command in FW. 
		SCGCQ00758178 - (Closed) - MegaRAID CPLD update improvements
		SCGCQ00758184 - (Closed) - GG update to include concatenated GG/VPD data for Invader product generation.
		SCGCQ00804284 - (Port_Complete) - Calculation for minimum blocks required to offload is wrong for single image configuration. 
		SCGCQ00813744 - (Port_Complete) - Offload timed out for single image configuration
		SCGCQ00791673 - (Port_Complete) - Command timeout happens though the response returns in 130ms. 
		SCGCQ00797554 - (Port_Complete) - Flash of incorrect GG on controller, does not restore VDs back to WB
	UEFI Driver 0x06090702 (SIGNED)
		SCGCQ00802129 - (Port_Complete) - Remove 8MB check for flashing
	MR NVDATA  3.1408.00-0009
		SCGCQ00741321 - (Closed) - Enable cache-bypass performance improvement feature
		SCGCQ00779416 - (Port_Complete) - Diagnostics test failed and SSD moved to failed state
	Ctrl-R 5.07-0008
		SCGCQ00734577 - (Closed) - VD property" Exposure to OS" equals to yes even after hidding the Virtual Drive. 
		SCGCQ00740008 - (Closed) - Incorrectness in the Patrol Read re-occurence time while setting delay value for continous PR
		SCGCQ00727361 - (Closed) - StorCLI crashing in *** glibc detected *** on trying to clear configuration on RHEL 5.10
		SCGCQ00766156 - (Closed) - Displaying entire 8-byte HDD drive firmware version. 
		SCGCQ00771136 - (Closed) - Add the capability to CTRL-R to set the Device Exposure NVDATA field
		SCGCQ00784138 - (Closed) - Creating diff size (GB/TB) VDs is not intutive using Cntrl+R
		SCGCQ00761091 - (Closed) - Drive List does not match the slot numbering
		SCGCQ00759695 - (Closed) - Prepare For Removal" on PD does not work w/pending PD operations
		SCGCQ00771864 - (Closed) - No option in CTRL-R to start manual bbu relearn
		SCGCQ00780015 - (Closed) - Type info is missing under PD in Cntrl-R
		SCGCQ00814612 - (Port_Complete) - CTRL-H "Prepare for removal appears even when Drives is in progress
		SCGCQ00769773 - (Port_Complete) - Implemented the storcli command to print the smart data of SATA drives. 
		SCGCQ00767783 - (Port_Complete) - StorCLI VMware Binary not displaying detailed description for phyerrorcounters of enclosures
		SCGCQ00769780 - (Port_Complete) - Implemented the storcli command to print SATA drive's phy error counters and reset them.
	ROMENV 1.09
	BootBlock 3.02.00.00-0001
	Hii v03.10.09.01(SIGNED)
	FCODE 4.16.08.00
	BIOS 6.20.04.1
	PCLI 1.07.05

Firmware Package:24.6.0-0030 (MR 6.5 Point Release)
 Firmware 4.260.00-3882
	SCGCQ00775267 - (Closed) - 3008 iMR - DPA extended capabilities bits structure is invalid
	SCGCQ00783613 - (Closed) - Firmware logs are not dumped to flash during device discovery phase
	SCGCQ00655162 - (Port_Not_Required) - Failed LED on 10HD BP does not light correctly for a bad drive
	SCGCQ00772911 - (Port_Complete) - Firmware indicating that PD can be spun down even in online state
	SCGCQ00783159 - (Port_Complete) - GPIO 24-31 is should be low when activity is going on drive
	SCGCQ00783186 - (Port_Complete) - Behavior change when FW hit fault code 0x81 (uncorrectable ECC error)
	SCGCQ00788250 - (Port_Complete) - Identify FDE drive compliant to Opal spec and mark them as non-FDE drive
	SCGCQ00775196 - (Port_Complete) - Workaround for Hardware Issue - SCGCQ00632364
	SCGCQ00779356 - (Port_Complete) - Virtual Disk GUID field changes when a VD is moved. The LUID is supposed to be unique and invariant.
	SCGCQ00783180 - (Port_Complete) - The field "expanderFwVersion=" is not populated under "ctrl info" in megamon
	SCGCQ00788252 - (Port_Complete) - Need MR 6.3 iMR Firmware Capable of Updating the SBR on a Customer Board in the Field
	SCGCQ00788283 - (Port_Complete) - Expander reports wrong active firmware version
	SCGCQ00783171 - (Port_Complete) - If diagnostic test fails on the copyback drive the FW does not allow a Recon, Copyback and CC on the same VD.
	SCGCQ00789243 - (Port_Complete) - OEM Expander (Truchas Valley) reporting temperature sensor error
 ROMENV 1.09
 BootBlock 3.02.00.00-0001
 NVDATA 3.1408.00-0007
	SCGCQ00762970 - (Port_Complete) - Customer needs NVDATA changes for PHY-to-SLOT mapping
	Various other changes for specific OEMs.
 UEFI_Driver 0x06090701 (SIGNED)
	SCGCQ00759757 - (Closed) - Direction bit is not set for READ CAPACITY commands
 Hii v03.10.09.01(SIGNED)
	SCGCQ00769319 - (Closed) - The last digit for Expander FW version is truncated
 FCODE 4.16.08.00
 BIOS 6.20.04.1
	SCGCQ00769239 - (Closed) - Don't issue REAID I/O on the 4K JBOD
 Ctrl-R 5.07-0006
 PCLI 1.07.05

Firmware Package:24.6.0-0023 (MR 6.5)
 Firmware 4.260.00-3735
	SCGCQ00584299 - (Closed) - R5/R6 SSD 4K Random Write IOps lower than expected (at a QD fo 256)
	SCGCQ00609808 - (Closed) - R0, R5, R6 read bandwidth drops abruptly at 256K block size with 24Dr SATA SSD configuration
	SCGCQ00630717 - (Closed) - SED: Montask fdeSM.c seen when using previously locked FDE drives.
	SCGCQ00649088 - (Closed) - Continuous Message in log "logGet: Found invalid event at fc570abc"
	SCGCQ00692488 - (Closed) - Assertion failure while running sequential reads on read ahead volume
	SCGCQ00693153 - (Closed) - The VDs when migrated from 6.4 to 6.5 will no longer be hidden from OS
	SCGCQ00699179 - (Closed) - Head of Queue Functionality is not getting executed
	SCGCQ00701317 - (Closed) - Change deviceExposure value from MegaMon for better debugging
	SCGCQ00704603 - (Closed) - Aspen firmware will crash or hang on unsupport cmd
	SCGCQ00705240 - (Closed) - Not able to set OEM value apart from 6
	SCGCQ00705302 - (Closed) - MR 6.5 FW:returning status failure while associating raid arrays to cachcade array.
	SCGCQ00710588 - (Closed) - MR6.5:Caching not happening after rebuild completed on R1 CCVD with BGIO's running on SVD
	SCGCQ00715282 - (Closed) - initialize the tempsensor to default full mode on restart
	SCGCQ00715395 - (Closed) - Virtual drive missing after online controller reset
	SCGCQ00715413 - (Closed) - Controller resets to its earlier time after OCR
	SCGCQ00719591 - (Closed) - Cannot change drive state while removing & inserting drive during recon and cannot start manual rebuild after recon.
	SCGCQ00724968 - (Closed) - Rebuild not starting on SSD, when Enclosure PD’s[used for SVD] and SSD's[used for CCVD] are foreign imported together
	SCGCQ00725070 - (Closed) - I/Os continue to run after hiding the VD for second time
	SCGCQ00726288 - (Closed) - New CMD_BLOCK added to initialize temperature sensor
	SCGCQ00732059 - (Closed) - Battery Learn Cycle is not getting initiated after CLBAD set for more than 3 mins.
	SCGCQ00734705 - (Closed) - Data TLB error seen on switching from FPM to HPM with OCR
	SCGCQ00643509 - (Closed) - Incorrect Max number of disks shown by LSA for Spanned Raid levels in IMR controller during Volume creation.
	SCGCQ00685640 - (Closed) - 3108 MR solution reports supercap is 254 C when actual ambient temp is -2 C
	SCGCQ00695428 - (Closed) - FW crashes during OS installation
	SCGCQ00696619 - (Closed) - MR 6.5 : Firmware breaks to Montask on line ../../raid/cache.c
	SCGCQ00696625 - (Closed) - PSOD observed while changing controller property 'enableJBOD' to 1.
	SCGCQ00701744 - (Closed) - FW got hung up during error handling of sence 0B/47/xx
	SCGCQ00704600 - (Closed) - Aspen firmware will crash when get to the end of "next devhandle"
	SCGCQ00705255 - (Closed) - Average Read response time for RAID 1 configuration is never calculated
	SCGCQ00712125 - (Closed) - iMR:6.5-Exception in core 0 is seen when drives are spun down and an ocr is triggered
	SCGCQ00716517 - (Closed) - MR6.5_FW: Pinned cache is not Flushing after second Foriegn Import while PD is removed in First Foriegn Import
	SCGCQ00725087 - (Closed) - Head Of Queue leads to negative delays between rebuild cycles
	SCGCQ00731286 - (Closed) - Core 0 exception in line 243 in file ../raid.c encountered when GG update fails with Stress IOs on all WB VDs
	SCGCQ00736509 - (Closed) - "Restore done successfully" prints available in firmware logs even after cache data is lost.
	SCGCQ00736863 - (Closed) - Inconsistent values reported for Write response times for RAID 1 VD's with HOQ and no IO
	SCGCQ00742024 - (Closed) - Disabling Control of HOQ Rebuild through applications
	SCGCQ00649094 - (Closed) - SSD VD association to CC VD through storcli shows success but actually it is not associated
	SCGCQ00692393 - (Closed) - LmidFifo Isr observed during drive pull with IO's on R5 VD
	SCGCQ00696256 - (Closed) - FW hit the Montask while running the TASIO
	SCGCQ00724961 - (Closed) - improper setting of targetSpeed in PCI link control 2 register to change pci link rate resulted in adapter reset.
	SCGCQ00713615 - (Closed) - MR6.4 random write throughput on 24SATA SSD R5/R6 configuration regressed compared to MR6.3
	SCGCQ00664261 - (Closed) - Port CQ Defect 421011 IOP: Asynchronous reset may cause system reset and PCIe Link Down
	SCGCQ00688064 - (Closed) - Foreign configuration import is successful but drive state still remains unconbad foreign during copyback
	SCGCQ00704310 - (Closed) - Disable DCR ERR LOG interrupt to fix DIS issue
	SCGCQ00712480 - (Closed) - Bypass cache for sequential writes which are greater than or equal to 128 KB
	SCGCQ00703189 - (Closed) - "Prepare For Removal" does not work on a PD when drive erase is in progress
	SCGCQ00700829 - (Closed) - MPI 2.5: BIOS Page 1 additions
	SCGCQ00685820 - (Closed) - MPI 2.5: distribute Target Command Buffers Received across multiple reply queues
	SCGCQ00683317 - (Closed) - Dirty Lba sorting is removed for fully SSD RAID Arrays.
	SCGCQ00682656 - (Closed) - Use region lock engine's capability to release local message identifier along with releasing region locks
	SCGCQ00634798 - (Closed) - Enable FastPath for all LSI Controllers
	SCGCQ00642226 - (Implemented) - Implement HEAD OF QUEUE to improve Rebuild performance over MR controllers
	SCGCQ00696862 - (Closed) - Ability to Support VPD Information in MR 6.3
	SCGCQ00652300 - (Closed) - MegaRAID power throttling implementation
	SCGCQ00650087 - (Closed) - Implemention to report HDD Temperature for Drives which does not support exceptional log page
	SCGCQ00656611 - (Implemented) - Add ability to take a VD offline, bring back VD online
	SCGCQ00667140 - (Port_Complete) - OEM Additional update required ontop of CritCom 66:PCIe SERDES parameter setting updates
	SCGCQ00675820 - (Port_Complete) - Updated long term WA for PPC errata #46
	SCGCQ00680739 - (Port_Complete) - Custom KeyGen Solution
	SCGCQ00682665 - (Port_Complete) - Cache offload failure with pinned cache on R5 VD
	SCGCQ00685986 - (Port_Complete) - Add better debugging functionality for Alarm related field issues
	SCGCQ00687878 - (Port_Complete) - Ctrl+R is not enabled after downgrade and upgrade FW
	SCGCQ00692232 - (Port_Complete) - OEM Data Corruption is taking place on Windows OS installed on top of ESX 5.5 U1 OS.
	SCGCQ00695333 - (Port_Complete) - Serial prints getting jumbled up due to print message inside spourious interrupt handler.
	SCGCQ00695385 - (Port_Complete) - 4K VDs missing after server reboot
	SCGCQ00695393 - (Port_Complete) - Postpone CC on boot for 5 minutes
	SCGCQ00702593 - (Port_Complete) - Issue a complete Gas Gauge reset on every boot
	SCGCQ00703177 - (Port_Complete) - Update Gas Guage Safety Status register bit positions
	SCGCQ00704303 - (Port_Complete) - Implemented Gas gauge FW update functionality .
	SCGCQ00710111 - (Port_Complete) - Reduce the monitoring time of CL (Capacitor Learning) flag in BQ33100 Operation Status register to 5Sec when a learn command is issued.
	SCGCQ00711812 - (Port_Complete) - Change SuperCap auto learn cycle period to 27 days and 22 hours.
	SCGCQ00712593 - (Port_Complete) - Prowl x24 not spinning up all disks (1.8 SSDs)
	SCGCQ00713099 - (Port_Complete) - OEM Data Corruption is taking place on Windows OS installed on top of ESX 5.5 U1 OS.
	SCGCQ00714527 - (Port_Complete) - Internal development defect to correct Module version validation logic for Gas Gauge firmware update
	SCGCQ00719724 - (Port_Complete) - FW doesn't do an Online Firmware Update (OFU) after a successful Gas Gauge firmware update .
	SCGCQ00722959 - (Ready) - Higher Jetstress average database writes latency
	SCGCQ00734987 - (Port_Complete) - The cache policy of Virtual Drives(VDs) do not change to Write-Through(WT) if FAULT is asserted and there is no indication in BQ33100 Safety Status register.
	SCGCQ00671448 - (Port_Complete) - ONFI: To properly handle the OCR case with RESET Status Register.
	SCGCQ00673627 - (Port_Complete) - Supercap properties reports wrong in storcli
	SCGCQ00687692 - (Port_Complete) - Foreign configuration import failure for spanned array with pinned cache
	SCGCQ00688780 - (Port_Complete) - Enable FastPath for all LSI Controllers
	SCGCQ00692233 - (Port_Complete) - Make sure numbers show up in Ctrl_R for drive Ids when drives connected through passive backplane
	SCGCQ00693961 - (Port_Complete) - [R630] Failed LED on 10HD BP does not light correctly
	SCGCQ00706922 - (Port_Complete) - Cache offload not triggered on few servers rarely
	SCGCQ00714523 - (Port_Complete) - Performing reboot immediately after updating the Gas Gauge (before learn completes) results in the FW reporting an update error on every subsequent boot.
	SCGCQ00723647 - (Port_Complete) - Flashing wrong Gas Gauge image (or any bad image) will force VDs to WT(Write Through) and fail and there is no path back to WB other than rebooting
	SCGCQ00757273 - (Port_Complete) - Performance degrade up to 35% in Write Back enabled 100% Random Writes as compared to MR 6.3 FW
	SCGCQ00679766 - (Port_Complete) - MR 6.4 : MonTask: line 4699 in file ../../raid/ld.c seen on iMR FW during boot to OS with R0 and PRL11 VD
	SCGCQ00695622 - (Port_Complete) - PPC exception seen during reboot test case on a VD
	SCGCQ00696014 - (Port_Complete) - PERC Data Corruption is taking place on Windows OS installed on top of ESX 5.5 U1 OS.
	SCGCQ00711847 - (Port_Complete) - Cache offload not triggered on few servers rarely
	SCGCQ00719701 - (Port_Complete) - When supercap learn is pending (overdue) at boot, exposure time in WB mode is seen for up to 1 minute 5 seconds.
	SCGCQ00730750 - (Port_Complete) - Flashing wrong Gas Gauge FW will succeed if flashed after good Gas Gauge FW is flashed and before the learn starts
	SCGCQ00695390 - (Port_Complete) - Serial prints getting jumbled up due to print message inside spourious interrupt handler.
	SCGCQ00703187 - (Port_Complete) - When we attempt to retrieve iMR Thunderbolt controller firmware logs using an application, we see some lines that are wrapped without starting on a new line.
	SCGCQ00704221 - (Port_Complete) - CSET: Continuous Message in log "logGet: Found invalid event at fc570abc" - (SCGCQ00649088)
	SCGCQ00716842 - (Port_Complete) - Preventing a specific supercap error message being printed in term log
	SCGCQ00734876 - (Port_Complete) - Few un-acceptable prints in serial log.
	SCGCQ00678585 - (Port_Complete) - Controller in JBOD mode is allowing a PD designated as a Hot Spare to be a configured via OOB as the boot drive
	SCGCQ00693962 - (Port_Complete) - RAID 5 Random Writes on SSDs
	SCGCQ00695613 - (Port_Complete) - 4K VDs missing after server reboot
	SCGCQ00700868 - (Port_Complete) - When we attempt to retrieve iMR Thunderbolt controller firmware logs using an application, we see some lines that are wrappedwithout starting on a new line.
 ROMENV 1.09
 BootBlock 3.02.00.00-0001
 NVDATA 3.1408.00-0007
	Numerous changes for specific customers
 UEFI_Driver 0x06090700 (SIGNED)
	SCGCQ00691044 - (Closed) - Code refactor effort: Hii Image buffer clean-up
	SCGCQ00688789 - (Closed) - DHP: Remove default value from numeric primitive that is present under suppressif
	SCGCQ00732773 - (Closed) - UEFI Driver: If the platform contains UEFI Spec Rev < than 2.3.0, then don't HII
	SCGCQ00756810 - (Closed) - PKG 9 HII form/When you have a a critical message such as missing VDs, after select "C" <ENTER>, it will show an assert
	SCGCQ00726723 - (Closed) - Ext/SCSI PassThru: UEFI Driver not filling direction flag correctly for Read
	SCGCQ00696656 - (Closed) - Update Mbox value for 240VD Support
	SCGCQ00650086 - (Implemented) - UEFI Driver UDK2010 complaince
	SCGCQ00688987 - (Port_Complete) - Don't let user boot to OS until user discards dirty cache
	SCGCQ00736761 - (Port_Complete) - Return health status failed if we have returned device error from Start()
	SCGCQ00756861 - (Port_Complete) - ControllerInfo[CtrlIndex].ControllerHandle got initialized incorrectly or too early
	SCGCQ00695249 - (Port_Complete) - Safe guard: Return health status failed if platform calls GetHealthStatus w/ NULL handle after we return intermediate status
	SCGCQ00716623 - (Port_Complete) - For OEM change memory type from EfiRuntimeServicesData to EfiMemoryMappedIO
	SCGCQ00716622 - (Port_Complete) - For OEM dont free the host memory during disconnect/unload process
 Hii v03.10.09.00(SIGNED)
	SCGCQ00689437 - (Closed) - Schedule consistency check gives an error message on Apply changes
	SCGCQ00692849 - (Closed) - When Controller is in Safe Mode don't remove UCM formset
	SCGCQ00696506 - (Closed) - Grammaical errors in HII warning message during FW Flash.
	SCGCQ00691938 - (Closed) - HII: Return device error when MR_DCMD_CTRL_PROPERTIES_SET fails.
	SCGCQ00700304 - (Closed) - MR_240VD:System fails to boot into SETUP[F2] and displays blank screen with 160 and 240 VDs
	SCGCQ00716628 - (Closed) - To Handle Code collab review Defect for SCGCQ00700199
	SCGCQ00700199 - (Closed) - After selcting Discard pinned Cache from Controller Management, Form will be taken to Cache and Memory after success.
	SCGCQ00702200 - (Closed) - Firmware Update feature fails to update firmware in HII
	SCGCQ00709543 - (Closed) - gHiiDriver.ExtLDSupport should be Filled with appropriate value before it's used
	SCGCQ00702196 - (Closed) - Asserts seen before loading HII
	SCGCQ00704309 - (Closed) - HII: Question value mismatch message seen in Enclosure Management screen.
	SCGCQ00714530 - (Closed) - HII: Firmware Update - On selecting empty folder, hang is seen.
	SCGCQ00731567 - (Closed) - use hwPresent.memory to determine iMR
	SCGCQ00706817 - (Closed) - MR_240VD: Virtual Drive properties[Read/Write/IO Policy] gets changed after VD creation from HII
	SCGCQ00710064 - (Closed) - Handline code collaborator Defect for SCGCQ00709543
	SCGCQ00716636 - (Closed) - Incomplete SAS Address
	SCGCQ00705577 - (Closed) - Unable to select the second enlcosure when multiple enclosures are connected to a controller .
	SCGCQ00715566 - (Closed) - .
	SCGCQ00723184 - (Closed) - Capacity Allocation in drive group properties is inappropriate
	SCGCQ00730496 - (Closed) - MR: HII gives the option to set -head of queue for raid 0
	SCGCQ00742103 - (Closed) - Remove Head Of Queue rebuild feature
	SCGCQ00704216 - (Closed) - HII hangs on selecting "View Drive Group Properties"
	SCGCQ00734447 - (Closed) - Patrol read prop page gives an error message on Apply changes
	SCGCQ00642228 - (Implemented) - Implement Head of Queue drive rebuild for MegaRAID controllers
	SCGCQ00650085 - (Implemented) - HEFU HII UDK2010 complaince
	SCGCQ00689070 - (Closed) - MR 6.2- Negative test HII browser- Mixing unsupported drives message needs update
	SCGCQ00664753 - (Closed) - Ability to enable/disable JBOD mode in HII & CTRL-R
	SCGCQ00656614 - (Closed) - Add ability to take a VD offline, bring back VD online
	SCGCQ00688454 - (Implemented) - HEFU HII UDK2010 complaince
	SCGCQ00695063 - (Port_Complete) - Call UninstallStoreLib when we call StopControllerHiiImpl function
	SCGCQ00695068 - (Port_Complete) - In HII Create VD option is enabled when resconstruction is in progress (on partial VD)
	SCGCQ00695072 - (Port_Complete) - H730P- Not showing PD to assign as DHS to R50/ R60 VD if PD is of lesser size than largest PD in V
	SCGCQ00695223 - (Port_Complete) - OEM 9.1.2 - HII: Contents of few help messages are improper
	SCGCQ00728678 - (Port_Complete) - Aspen UEFI creating a new VD in a "hole" in the drive group free space, hangs when viewing drive group properties
	SCGCQ00756855 - (Port_Complete) - Chk the err status for HL_Get_PD_List() and HL_Get_PD_Info in UF002_PrepareData() + check Driver handle if index is valid
 FCODE 4.16.08.00
 BIOS 6.20.04
	SCGCQ00720411 - (Closed) - OpROM 240VD: Not able to boot to OS from the VD whose target ID is greater than 128
	SCGCQ00455591 - (Closed) - Memory access issue for Mercury when loading Ctrl R
	SCGCQ00693494 - (Closed) - setting deviceExposure greater than or eaual to 128 will show wrong VD handled by bios
	SCGCQ00455597 - (Closed) - Memory allocation: Allocate only two 64k
	SCGCQ00736737 - (Port_Complete) - xprintf display issue when FW reports percentage for device scan
	SCGCQ00709995 - (Port_Complete) - OEM wants the battery status text in BIOS to change from "missing" to "N/A" for iMR solutions.
 Ctrl-R 5.07-0006
	SCGCQ00720815 - (Closed) - Ctrl+R: <prev> and <next> links in Properties Page both redirects to next page and vice versa.
	SCGCQ00716584 - (Closed) - /c0 show all page are having some incorrectness in controller information
	SCGCQ00704259 - (Closed) - Firmware Hangs/breaks while creation of RAID1 with GHS
	SCGCQ00738006 - (Closed) - Incorrectness in the popup for Virtual drive Expansion
	SCGCQ00712982 - (Closed) - Verify StorCLI warns on destructive operations - R0 with 2 x SED drives Deleted with no warning.
	SCGCQ00729691 - (Closed) - fault(coredump) observed on executing ./storcli /c1/v63 show all for 64th cachecade VD in ubuntu14.04
	SCGCQ00707450 - (Closed) - While creating cachecade vd with one SAS-SSD;Raid 1 option is also enabled
	SCGCQ00710520 - (Closed) - Ctrl+R_6.5: Incorrectness in Help file generated by pressing F1
	SCGCQ00712171 - (Closed) - While creating cachecade vd with one SAS-SSD;Raid 1 option is also enabled
	SCGCQ00730497 - (Closed) - MR: ctrl-r gives the option to set -head of queue for raid 0
	SCGCQ00727409 - (Closed) - CTRL-R:Incorrectness in CTRL Management while launching Manage Link Speed
	SCGCQ00706013 - (Closed) - VD I/O policy changes from cached to direct when VDs are created from Ctrl-R
	SCGCQ00725545 - (Closed) - In foreign Config Preview VD Size is coming as NA instead of actual size,when VD state is foreign.
	SCGCQ00735369 - (Closed) - not able to navigate through "join mirror -choose option" window
	SCGCQ00730412 - (Closed) - Incorrectness in the popup generated during deletion of Cachecade associated Virtual Drive
	SCGCQ00742106 - (Closed) - Remove Head Of Queue rebuild feature
	SCGCQ00731292 - (Closed) - Unable to see PD(s) Count in Cachecade RAID1 w.r.t to Cachecade RAID0
	SCGCQ00709969 - (Closed) - Ctrl+R_6.5: Showing incorrectness in Memory Size in Properties Page2
	SCGCQ00719102 - (Port_Complete) - Date Created field in storCLI display is incorrect after creating a VD in MSM using SWR versio 1.34 on ALM2-16
	SCGCQ00732019 - (Active) - CLI command to access/modify Immediate IO
	SCGCQ00694663 - (Port_Complete) - Simulator files check-in with changes in new API.
	SCGCQ00732058 - (Port_Complete) - CLI command to access/modify Drive Activity LED
	SCGCQ00699269 - (Port_Complete) - storcli is displaying only information of one enclosure when all option is given for phyerrorcounters, on multiple enclosures
 PCLI 1.07.05

Firmware Package: 24.5.0-0015 (MR 6.4)
 Firmware 4.250.00-3569
	SCGCQ00651356 - (Closed) - Cache offload not triggered on few servers rarely
	SCGCQ00663028 - (Closed) - Patrol read is in progress even after issuing stop patrol read command through App
	SCGCQ00669540 - (Closed) - PPC exception seen during reboot test case on a VD
	SCGCQ00672868 - (Closed) - Firmware crash @line 1266 in file ../../raid/1078dma.c while Clearing the configuration when reconstruction going on.
	SCGCQ00677415 - (Closed) - Patrol read suspended message continues to appear even after it is stopped
	SCGCQ00678651 - (Closed) - Firmware breaks into montask at line : 931 in file ../../raid/bladeDMA.c
	SCGCQ00685276 - (Closed) - Configuration lost on Controller while importing the configuration just as the drives start to show in discovery.
	SCGCQ00687265 - (Closed) - Exception in Core 0 on rebooting the System while reconstruction is in progress
	SCGCQ00695573 - (Closed) - Performance degrade up to 35% in Write Back enabled 100% Random Writes as compared to MR 6.3 FW
	SCGCQ00637612 - (Closed) - eccBucketSize set to threshold value 15 upon changing its value to 0 or 1
	SCGCQ00638190 - (Closed) - PD is reported as a 'HSP by storcl64 which is neither DHSP nor GHSP.
	SCGCQ00644645 - (Closed) - FW Breaks while importing Foreign Config(BS Assertion Failure while flushing the pinned cache)
	SCGCQ00652759 - (Closed) - set the BBUEnable flag as per the cacheoffload requirement
	SCGCQ00685001 - (Closed) - patrolread suspended message appears even after resuming it and while progress in PR
	SCGCQ00604480 - (Closed) - locate behavior will incorrect light some drive LED not located after some loop locate test on 3108 MR+PMC Expander
	SCGCQ00613357 - (Closed) - Able to perform PD format and PD secure erase operations simultaniously
	SCGCQ00620701 - (Closed) - All the menu items in MSM such as create VD are highlighted when the controller is in safe mode.
	SCGCQ00624038 - (Closed) - Changed the order of evaluation to compiler independent
	SCGCQ00633906 - (Closed) - Disable the HW assisted L3 cache flush prior to offload in case of powerloss.
	SCGCQ00634405 - (Closed) - Data Misscompare found on Raid 60 when pinned cache is created on Raid 50.
	SCGCQ00636277 - (Closed) - Battery Retention Test not reporting test result.
	SCGCQ00642679 - (Closed) - Assertion failure in ../../raid/cache.c at line 2772
	SCGCQ00653832 - (Closed) - Delay in OCR with IO timeouts is seen when Security is enabled
	SCGCQ00658494 - (Closed) - FW issuing false event saying VD policy change from WT to WB even the memory module is bad
	SCGCQ00664511 - (Closed) - Enable DIS feature in FW
	SCGCQ00672040 - (Closed) - MonTask: line 7204 in file ../../bbu/onfi.c with power cycle script
	SCGCQ00673991 - (Closed) - ocr does not trigger after deleting nvram
	SCGCQ00677803 - (Closed) - Cache offload failure with pinned cache on R5 VD
	SCGCQ00679787 - (Reworked) - Foreign configuration import is successful but drive state still remains unconbad foreign during copyback - SingleNode
	SCGCQ00681033 - (Closed) - Assertion in ../../raid/raidscsi.c at line 904 with controller reset while CacheCade toggling for mix of VDs.
	SCGCQ00630344 - (Closed) - Coverity Integrity Manager tool defect
	SCGCQ00645801 - (Closed) - Getting Question Value mismatch when entering Controller management screen in HII
	SCGCQ00655979 - (Closed) - Drive failures observed while issuing a pass through link reset to all phys in a loop
	SCGCQ00669055 - (Closed) - Hit a MonTask while running overnight learn cycles with OCR every 10mins
	SCGCQ00669713 - (Closed) - Solid amber LED does not reset on a failed SGPIO slot upon device recovery if locate is on before the drive fails
	SCGCQ00679180 - (Closed) - Foreign Config fails to import max config
	SCGCQ00642473 - (Closed) - Jetstress test fails after completion of rebuild
	SCGCQ00661244 - (Closed) - Mismatch in emulation properties observed on importing VD from foreign configuration
	SCGCQ00665670 - (Closed) - Join Mirror command with option 2 imports foreign configurations which are not part of broken mirror.
	SCGCQ00674868 - (Closed) - observed when OS was formatting the VD in which cluster double medium error injected
	SCGCQ00680326 - (Closed) - Failed import VDs with pinned cache after ONFI tranport
	SCGCQ00661190 - (Closed) - cache is not getting bypassed for 64 VD;s
	SCGCQ00671194 - (Closed) - Failed import a R5 VD with pinned cache after ONFI tranport
	SCGCQ00677411 - (Closed) - MonTask: line 6556 in file ../../bbu/onfiBBM.c is seen when you delete NVRAM
	SCGCQ00678566 - (Closed) - Automatically VD gets created for mirror arm of 1st VD on joining the mirror arm of 2nd VD as new virtual drive.
	SCGCQ00665475 - (Closed) - To properly handle the OCR case with RESET Status Register.
	SCGCQ00574358 - (Closed) - Allow UEFI and BIOS to be Enabled/Disabled individually
	SCGCQ00523879 - (Closed) - Identify physical location of a target device
	SCGCQ00566306 - (Closed) - Add type BIOS for HashImageType.
	SCGCQ00569175 - (Closed) - Add product-specific Flag bit to Clean Tool
	SCGCQ00621554 - (Closed) - Refactor Buffer Manager to avoid overheads with various lists
	SCGCQ00648403 - (Closed) - Roll back latency improvements from MR6.4
	SCGCQ00660441 - (Closed) - Short term fix for PPC476 Errata
	SCGCQ00674506 - (Closed) - Long term work around for PPC 476 Errata #46
	SCGCQ00692938 - (Closed) - Remove unwanted prints in sysDMA path
	SCGCQ00602088 - (Closed) - Command timeouts with cdb=ff ff ff ff
	SCGCQ00669013 - (Closed) - Disable cache bypass in least latency mode
	SCGCQ00674233 - (Closed) - F/w changes to set deviceExposure default from NVDATA
	SCGCQ00524743 - (Opened) - Enable support L3 auto-flush on power fail when BBU is connected
	SCGCQ00586309 - (Closed) - Enable cache bypass for better performance with large writes on WB volumes
	SCGCQ00599993 - (Closed) - Remove EBBU code as it is no longer needed
	SCGCQ00634750 - (Closed) - Requirement for 512e implementation changes
	SCGCQ00654566 - (Closed) - Work Around for PPC 476 Errata #46 in MR Firmware
	SCGCQ00626667 - (Closed) - Add Mirror Join functionality
	SCGCQ00654568 - (Closed) - Work Around for PPC476 Errata #46 in iMR Firmware
	SCGCQ00599829 - (Closed) - Refactor DM for modularity
	SCGCQ00634792 - (Closed) - Need to support both SAS and SATA disks in the same dual path/expander jbod/backplane
	SCGCQ00642323 - (Closed) - Driver support for read IO load balance on more a >2 drive R1 volume
	SCGCQ00589296 - (Closed) - Misc code cleanup for performance improvement
	SCGCQ00556387 - (Port_Complete) - VPD (Vital Product Data) needs to identify PCB hardware level
	SCGCQ00564594 - (Port_Complete) - Output async event message to upper layer when it detected "Write Timeout" in between on-board flash
	SCGCQ00574402 - (Port_Complete) - Display the NCQ enabled/disabled status of every SATA disk drive in the output of StorCLI and MegaCLI
	SCGCQ00605439 - (Port_Complete) - FW debugger scrolls continuous message and eventually resets after deleting Source VD during a Cachecade disassocation
	SCGCQ00609779 - (Port_Complete) - Add Fastpath Support by Default for a particular OEM.
	SCGCQ00619496 - (Port_Complete) - Storecli reporting incorrect values for tfm and supercap date of manufacture
	SCGCQ00630129 - (Port_Complete) - Bad battery warning message that comes up during POST isn't aligned properly.
	SCGCQ00630133 - (Port_Complete) - Static analysis tool defects
	SCGCQ00642804 - (Port_Complete) - Wrong behavior of Break Mirror operation on starts rebuild
	SCGCQ00643486 - (Port_Not_Required) - Getting Question Value mismatch when entering Controller management screen
	SCGCQ00651193 - (Port_Not_Required) - Battery learn cycle continues to more than one cycle even FW has marked it as bad in previous reboot
	SCGCQ00651381 - (Port_Not_Required) - DC observed upon performing OCR on a degraded R1 (AWB).
	SCGCQ00656141 - (Port_Complete) - CacheCade data loss after reboot
	SCGCQ00662365 - (Port_Complete) - Write buffer flash programming support
	SCGCQ00663056 - (Port_Complete) - CC doesn't correct medium error in P drive
	SCGCQ00666941 - (Port_Complete) - Start a learn even if the SuperCap is not completely charged.
	SCGCQ00666982 - (Port_Complete) - Change the cache policy of Virtual Drives(VDs) to Write Through(WT) if SuperCap temperature goes above 60 degree Celsius.
	SCGCQ00667965 - (Port_Complete) - CS2.0: Coverity defects (11619, 14267, 14334)
	SCGCQ00675271 - (Port_Complete) - Updated long term WA for PPC errata #46
	SCGCQ00675820 - (Port_Complete) - Updated long term WA for PPC errata #46
	SCGCQ00678184 - (Port_Complete) - MonTask: line 4699 in file ../../raid/ld.c seen on iMR FW during boot to OS with R0 and PRL11 VD
	SCGCQ00681040 - (Port_Complete) - PD is reported as a 'HSP by storcl64 which is neither DHSP nor GHSP.
	SCGCQ00682665 - (Port_Complete) - Cache offload failure with pinned cache on R5 VD
	SCGCQ00690088 - (Port_Complete) - DIS mismatch while running system reboot script with dirty data in DDR
	SCGCQ00692999 - (Port_Complete) - Data Corruption is taking place on Windows OS installed on top of ESX 5.5 U1 OS.
	SCGCQ00695994 - (Port_Complete) - Serial prints getting jumbled up due to print message inside spourious interrupt handler.
	SCGCQ00706936 - (Port_Complete) - Cache offload not triggered on few servers rarely
	SCGCQ00714274 - (Port_Complete) - Serial prints getting jumbled up due to print message inside spourious interrupt handler.
	SCGCQ00614988 - (Port_Not_Required) - not enough bs found during double Dip power cycle Test
	SCGCQ00630137 - (Port_Complete) - Unable to suspend the Patrol Read operation in iMR mode from the HII application
	SCGCQ00639588 - (Port_Complete) - Hitting montask line 1930 in file ../../bbu/onfi.c while running FP IO's on degraded VD's
	SCGCQ00642810 - (Port_Complete) - Copyback is not start immediately after reconstruction is completed in OS.
	SCGCQ00642816 - (Port_Complete) - Send Inquiry after expander responds with Unit Attention Microcode Change
	SCGCQ00650280 - (Port_Complete) - FW Breaks while importing Foreign Config(BS Assertion Failure while flushing the pinned cache)
	SCGCQ00654731 - (Port_Not_Required) - Fw hit montask with machinecheck exception on PD pushpull with IO on R5
	SCGCQ00662326 - (Port_Complete) - Prevent data correction in pagefil.sys to happen during Check Consistency after heavy I/O test.
	SCGCQ00662532 - (Port_Complete) - locate behavior will incorrect light some drive LED not located after some loop locate test on 3108 MR+PMC Expander
	SCGCQ00663057 - (Port_Complete) - Check and resume rebuild after a stipulated time 
	SCGCQ00671448 - (Port_Complete) - To properly handle the OCR case with RESET Status Register.
	SCGCQ00676945 - (Port_Complete) - For OEM do cache offload for when cache is is dirty (WB and ForceWB modes) and when there is a battery present (WT mode).
	SCGCQ00676950 - (Port_Complete) - DHS that becomes GHS does not start rebuilding automatically with an already degraded VD
	SCGCQ00679174 - (Port_Complete) - MonTask: line 4699 in file ../../raid/ld.c seen on iMR FW during boot to OS with R0 and PRL11 VD
	SCGCQ00682959 - (Port_Complete) - Enter Montask during rebuild after reboot
	SCGCQ00714465 - (Port_Complete) - When we attempt to retrieve iMR Thunderbolt controller firmware logs using an application, we see some lines that are wrapped without starting on a new line.
	SCGCQ00601065 - (Port_Not_Required) - Getting Question Value mismatch when entering Controller management screen
	SCGCQ00619497 - (Port_Complete) - Pinned cache gets flushed to incorrect VD for mirrored RAID levels
	SCGCQ00625016 - (Port_Complete) - montask seen with "Assertion failure in line 4168" on running IO on 4K VD.
	SCGCQ00628213 - (Port_Complete) - correct when copyback (replace) for R11 can be done.
	SCGCQ00630147 - (Port_Complete) - Unable to discard pinned cache in Headless Safe Mode.
	SCGCQ00650926 - (Port_Complete) - JetStress average database write latency is above previous generation controller
	SCGCQ00651383 - (Port_Not_Required) - Hitting montask line 1930 in file ../../bbu/onfi.c while running FP IO's on degraded VD's
	SCGCQ00662330 - (Port_Complete) - (SATA) Failed temperature Capture on when link up/down experienced
	SCGCQ00665693 - (Port_Complete) - TFM/BBU error seen with latest TFM FW/VPD
	SCGCQ00669083 - (Port_Complete) - Cannot import foreign configuration.
	SCGCQ00674858 - (Port_Complete) - Updated long term WA for PPC errata #46
	SCGCQ00677304 - (Port_Complete) - Estimated Time Left" shows confusing values
	SCGCQ00679755 - (Port_Complete) - Cell Disk With Status not Present Was Found to be Showing a Green Status Light
	SCGCQ00679766 - (Port_Complete) -  MonTask: line 4699 in file ../../raid/ld.c seen on iMR FW during boot to OS with R0 and PRL11 VD
	SCGCQ00696015 - (Port_Complete) - Data Corruption is taking place on Windows OS installed on top of ESX 5.5 U1 OS.
	SCGCQ00623210 - (Port_Complete) - expander not spinning up all disks (1.8 SSDs)
	SCGCQ00625642 - (Port_Complete) - Fault LED is not set when drive is bad
	SCGCQ00668344 - (Port_Complete) - Coverity defects (11619, 14267, 14334)
	SCGCQ00669082 - (Port_Complete) - Limit the number of retries when learn fails to start after firmware issues the learn command.
	SCGCQ00601559 - (Port_Complete) - Write buffer flash programming support
	SCGCQ00620171 - (Port_Complete) - RAID configured on PD been erased with Normal or Thorough will lost after system reboot/reset
	SCGCQ00664887 - (Port_Complete) - converting MR to IMR fails
	SCGCQ00670778 - (Port_Complete) - SecureVD erase is not resumed on reboot in ronaldo server.
	SCGCQ00673077 - (Port_Complete) - Data corruption after media error correction
	SCGCQ00570181 - (Port_Complete) - Deep learn will not start immediately when Relative State of Charge (RSOC) of battery is equal to 95%.
	SCGCQ00666938 - (Port_Complete) - If cache offload happens during a relearn, then the Firmware will halt at next boot for the learn completion.
	SCGCQ00676948 - (Port_Complete) - I2C Issue - Unintended failures following response timeout
	SCGCQ00646713 - (Port_Complete) - Cannot recover data from a recoverable media error after Patrol Read encounters recovery failure for RAID-1
	SCGCQ00651316 - (Port_Complete) - Change when checking if copyback can be done on a PD in a PRL11
 ROMENV 1.09
 BootBlock 3.02.00.00-0001
 NVDATA 3.1406.00-0075
	Numerous changes for specific customers
 UEFI_Driver 0x06080500 (SIGNED)
	SCGCQ00638308 - (Closed) - FMP GetImageInfo could result in stack corruption - Code Review Defect ID D26304
	SCGCQ00628627 - (Closed) - UEFI Driver- has debug print statements during POST
	SCGCQ00628310 - (Closed) - Install FMP on Controller Handle at Start() and the exception
	SCGCQ00550389 - (Closed) - Write Caching HBA, JBOD/R0 supported TB controller with 240 SystemPD/LD support
	SCGCQ00626601 - (Implemented) - VT-d/IOMMU support for iMR - Implement mechanism to allow system BIOS to put entries for iMR mem allocation into proper table
	SCGCQ00635878 - (Port_Complete) - UEFI Driver- has debug print statements during POST
	SCGCQ00677776 - (Port_Complete) - Initilize the buffer that we allocate to load HII and return EFI_OUT_OF_RESOURCES if allocation fails
	SCGCQ00678154 - (Port_Not_Required) - For OEM dont free the host memory during disconnect/unload process
	SCGCQ00679073 - (Port_Complete) - Do not go to WebBIOS due to a bad health status when WebBIOS is disabled in NVDATA.
	SCGCQ00644508 - (Port_Complete) - CPU EXCEPTION ERROR (Dont double free the memory)
	SCGCQ00644509 - (Port_Complete) - CPU EXCEPTION ERROR (Dont double free the memory)
	SCGCQ00644856 - (Port_Complete) - Install FMP on Controller Handle at Start() and the exception
	SCGCQ00661595 - (Port_Complete) - Timeout is not passed correctly to FW
	SCGCQ00644859 - (Port_Complete) - FMP GetImageInfo could result in stack corruption - Code Review Defect ID D26304
	SCGCQ00658168 - (Port_Complete) - ATA Pass thru: Timeout is not passed correctly to FW
 Hii v03.09.06.00 (SIGNED)
	SCGCQ00625438 - (Closed) - Minor Typos and consistency issues in HEFU HII help text
	SCGCQ00633320 - (Closed) - Handling code collaborator Defects: SCGCQ00573222 and SCGCQ00568814
	SCGCQ00602492 - (Closed) - HII fails to list the foreign configuration
	SCGCQ00658674 - (Closed) - Hii - Restrict the user from creating the 65th VD.
	SCGCQ00630532 - (Closed) - Consistency Check Start - remove mm/dd/yyyy from the string as the format is out of control of LSI
	SCGCQ00624890 - (Closed) - Handling Code Collaborator Defect: SCGCQ00573222
	SCGCQ00678695 - (Closed) - Change the Step Value to 0 for all numeric to make sure for free edit instead of Incrementing and decrementing using +/-
	SCGCQ00640534 - (Closed) - HII is showing RAID6 and RAID5 levels while creating VD when we have 2 512n drives and 1 4k Drives
	SCGCQ00645532 - (Closed) - Update the string for "
	SCGCQ00679861 - (Closed) - Not able to create VD with 4k drives 
	SCGCQ00637539 - (Closed) - Remove FMP installed on the controller handle in HII
	SCGCQ00678603 - (Closed) - HII does not display power state of a PD
	SCGCQ00627778 - (Closed) - Address review comments
	SCGCQ00672925 - (Closed) - Unable to set spinup drive count in HII
	SCGCQ00550390 - (Closed) - Write Caching HBA, JBOD/R0 supported TB controller with 240 SystemPD/LD support
	SCGCQ00626605 - (Closed) - Clone SCGCQ00556243 HII-based PCI Inventory - MR) into the mainline
	SCGCQ00620259 - (Closed) - Port 240VD change to Tbolt SCGCQ00441334
	SCGCQ00634019 - (Closed) - Change the default Setting of Disk Cahce Policy from Unchanged to Disable.
	SCGCQ00626591 - (Closed) - Add Mirror Join functionality - PR SCGCQ00521537
	SCGCQ00626585 - (Closed) - Requirement for 512e implementation changes - PR SCGCQ00425778
	SCGCQ00642232 - (Closed) - Ability to enable/disable JBOD mode in HII
	SCGCQ00621285 - (Closed) - Change the wording in HII from Check Consistency to Make data consistent
	SCGCQ00652171 - (Port_Complete) - HII is gave a option to start reconstruction from any degraded RAID level to RAID 0.
	SCGCQ00677103 - (Port_Complete) - Detail Drives info shows incorrectly in BIOS - unknown characters appearing
	SCGCQ00679042 - (Port_Complete) - Enhance strings for Locked foreign config import feature
	SCGCQ00644857 - (Port_Complete) - Remove FMP installed on the controller handle in HII
	SCGCQ00644858 - (Port_Complete) - RSOD during POST after enabling SecureBoot - HEFU.ROM should report exact size of .EFI image
	SCGCQ00661685 - (Port_Complete) - HII reports wrong data under 'Eligible JBOD Drives for conversion' while converting JBOD to UG
	SCGCQ00652168 - (Port_Complete) - In HII ,Full initialization is not grayed out for R6 DIF arrays.
	SCGCQ00603251 - (Port_Complete) - Creation+ FW updation+ Scan foreign Configuration is disabled/grayed out in HII page
	SCGCQ00652424 - (Port_Complete) - change the numeric primitive's maximum from MAX_PHYSICAL_DRIVES to 0xff
	SCGCQ00644788 - (Port_Complete) - Enhance help message for PD/VD Operation field
	SCGCQ00679036 - (Port_Complete) - After Rebuilding, DHS and Expand VD operations failed to update as per VD properties
	SCGCQ00634684 - (Port_Complete) - RSOD during POST after enabling SecureBoot - HEFU.ROM should report exact size of .EFI image
	SCGCQ00644575 - (Port_Complete) - Consistency Check Start - remove mm/dd/yyyy from the string as the format is out of control of LSI
	SCGCQ00652169 - (Port_Complete) - HII reports wrong data under 'Eligible JBOD Drives for conversion' while converting JBOD to UG
	SCGCQ00652170 - (Port_Complete) - HII is showing RAID levels, irrespective of drives to configure a new RAID level.
	SCGCQ00679049 - (Port_Complete) - "Make Unconfigured good" option missing in HII even if JBOD's are present in the config
	SCGCQ00682962 - (Port_Complete) - creation in HII is showing GB
	SCGCQ00644786 - (Port_Complete) - Enhance help message for PD/VD Operation field
	SCGCQ00682960 - (Port_Complete) - HII is not displaying the cachecade 512GB warning message
 FCODE 4.16.08.00
 BIOS 6.19.05.0
	SCGCQ00626821 - (Closed) - 240VD Support: In Post Restrict to 64 VD only
	SCGCQ00629987 - (Closed) - With more than 64 VD's in the configuration, number of Virtual Drives handled by BIOS message is not shown in the POST.
	SCGCQ00659974 - (Closed) - OpROM - If there is boot message, BIOS won't detect > 64 VDs
	SCGCQ00653048 - (Closed) - AutoSelectBootLd is not working if user has OS in VD > 64
	SCGCQ00632011 - (Closed) - Firmware enters faults state after a reboot on flashing firmware with IO in progress.
	SCGCQ00682646 - (Closed) - Display the first 64 VDs in the POST (in the same sequence we get it from FW)
	SCGCQ00626602 - (Implemented) - VT-d/IOMMU support for iMR - Implement mechanism to allow system BIOS to put entries for iMR mem allocation into proper table
	SCGCQ00621895 - (Closed) - WebBIOS of MR card hangs due to bios control mis-direct 
	SCGCQ00550388 - (Closed) - Write Caching HBA, JBOD/R0 supported TB controller with 240 SystemPD/LD support
	SCGCQ00679070 - (Port_Complete) - Display Warning Message when Preboot Configuration Utility are Disabled and User tries to lunch it
 Ctrl-R 5.06-0003
	SCGCQ00647392 (DFCT) - join mirror-mirror drive is not seen in join mirror-choose option in CTRL-R
	SCGCQ00648182 (DFCT) - Port informations are not displayed in Connector field for the drives attached to antares card.
	SCGCQ00663996 (DFCT) - Not able to change emulation properties in CTRL-R for iMR
	SCGCQ00666806 (DFCT) - Set factory defaults option is blocking the "prev" button in controller properties page
	SCGCQ00666807 (DFCT) - "enable jbod" help file is not opening with f1 option on it.
	SCGCQ00667550 (DFCT) - Not able to Manually stop or suspend the copyback operation once started
	SCGCQ00677458 (DFCT) - Under Join mirror-choose option page existing drives for second R1 VD are not listed.
	SCGCQ00677460 (DFCT) - Montask on joining the mirror arm as new virtual drive when doing with the second array.
	SCGCQ00678600 (DFCT) - Gramatical Error in Ctrl-R while modifying SuperCap properties
	SCGCQ00625148 (DFCT) - in-appropriate drive state is seen on connecting back the drives in ctrl-r .
	SCGCQ00625164 (DFCT) - not able to navigate in the warning message window for having more than 64VD.
	SCGCQ00625175 (DFCT) - on having more than 64 VD's and initiating a copyback from ctrl-r will result in montask
	SCGCQ00628684 (DFCT) - OEM enclosure connected in multi-path is not showing all ports
	SCGCQ00642546 (DFCT) - Help is missing for break and join mirror feature in Control-H
	SCGCQ00644056 (DFCT) - Join mirror is not enabled in CTRL-R 
	SCGCQ00646220 (DFCT) - Getting an option in join mirror to select both "add new vd" and "existing VD" in ctrl-r
	SCGCQ00647015 (DFCT) - LD emulation properties not getting set on updating VD properties
	SCGCQ00606059 (DFCT) - Ctrl-R - In iMR controller we are able to set VD properties to write back and cached .
	SCGCQ00614734 (DFCT) - unable to cretae VD with property "Write back with BBU"
	SCGCQ00615350 (DFCT) - In multicontroller environment unable to enter in to ctrl-R after 1st controller initililization.
	SCGCQ00635638 (DFCT) - spelling issue in help file of VD Size.
	SCGCQ00630099 (ENHREQ) - Requirement for 512e implementation changes
	SCGCQ00632051 (ENHREQ) - Added the OEM check for getting default disk-cache policy in Libmods as Disable.
	SCGCQ00634020 (ENHREQ) - Added the OEM check for getting default disk-cache policy in Libmods as Disable.
 PCLI 1.07.05

 Package: 24.3.0-0063 (MR6.3 point release)
 Firmware - 4.230.30-3728
  SCGCQ00755473 - Truchas Valley reporting temperature differential error

Package: 24.3.0-0054 (MR6.3 patch)
 Firmware - 4.230.30-3586
  SCGCQ00625524 - When we attempt to retrieve iMR Thunderbolt controller firmware logs using an application, we see some lines that are wrapped without starting on a new line.
  SCGCQ00695317 - Serial prints getting jumbled up due to print message inside spourious interrupt handler.
  SCGCQ00675262 - Data Corruption is taking place on Windows OS installed on top of ESX 5.5 U1 OS.
  SCGCQ00665475 - ONFI: To properly handle the OCR case with RESET Status Register.
  SCGCQ00677803 - Cache offload failure with pinned cache on R5 VD
  SCGCQ00674392 - Updated long term WA for PPC errata #46
  SCGCQ00568080 - Defect Fix for VPD and inquiry callback issues in DISM
  SCGCQ00568134 - Patrol read will not start on any VD after a PR is started, suspended and VD is deleted
  SCGCQ00569895 - Defect Fix for Command gets retried infinitely times when drive responds with 0B/47/03 always
  SCGCQ00572662 - FW failure during read on 3PD R5 with 1000 CME with skip count 2
  SCGCQ00574276 - FW breaks if wrong security key is entered
  SCGCQ00580162 - Only 1mb crash dump is getting generated of fw fault
  SCGCQ00580847 - not enough bs found during double Dip power cycle Test
  SCGCQ00586163 - cache restore failure message displayed though cache restore was successfull
  SCGCQ00588173 - Routines to inject bit error in NF and ecc error in DDR for ONFI
  SCGCQ00588185 - Mismatch in LD id and target ID during set/reset boot device
  SCGCQ00589365 - on breaking the multipath in loop while drives are spinnning up will result in montask
  SCGCQ00589728 - FW hangs while creating 64 VDs on the controller with SLES11 SP2
  SCGCQ00592996 - While running reconstruction from R1 to 4 drive PRL11 with IO,FW hits to MonTask: line 1270 in file ../../raid/1078dm
  SCGCQ00593776 - SMART poll needs to issue log sense with page control set to current/ cummulative value
  SCGCQ00602556 - Static analysis tool defects
  SCGCQ00602665 - Static analysis tool defect
  SCGCQ00602726 - Static Analysis Tool defects
  SCGCQ00602855 - Static analysis tool defect
  SCGCQ00603306 - static analysis tool defects resolution
  SCGCQ00603564 - added support for debugqueue
  SCGCQ00603779 - Not getting "Clear ldbbm badblocks" options on VD
  SCGCQ00611275 - FW goes to kill adaptor to handle partial copy of crash_dump
  SCGCQ00612927 - Montask in divert.c seen when injecting 64K consecutive errors on R0 VD, Patrol Read running in background.
  SCGCQ00614455 - Static analysis tool defects
  SCGCQ00625843 - PR Progress event is not generated for 1TB/3TB SATA drive
  SCGCQ00634578 - Defect fix for kenel panic with iMR Fury with Free BSD driver
  SCGCQ00636748 - Running Storcli /C0/CV show or (show all) starts a relearn on supercap issue
  SCGCQ00451219 - Defect Fix for Online DIF drives are getting punctured after PI enabled R5 VDs are offlined with pinned cache
  SCGCQ00574071 - md5sum mismatch seen on a copied file from R5 VD with CME
  SCGCQ00574277 - Power removal of enclosure FW hits to MonTask: line 4056 in file ../../bbu/onfiBBM.c
  SCGCQ00586190 - Fix GNU make file compilation
  SCGCQ00586341 - Crash Dump Error Handling
  SCGCQ00605227 - When OS on VD ,after collecting crash dump file system becomes readable
  SCGCQ00606571 - Physical drives go to power save mode just after restarting the server
  SCGCQ00610881 - storcli and CtrlR still show new PD information as 4K sector after replacing a 4K sector drive with a 512 sector drive
  SCGCQ00630075 - Unexpected power state change
  SCGCQ00631492 - Media error on Last sector of stripe isn't added to LDBBM list
  SCGCQ00524842 - CME logic using overlaid fields in c->rec
  SCGCQ00568655 - defect fix for Compilation issue
  SCGCQ00575006 - Too many unexpected sense AEN raised by CC during CME recovery on R5
  SCGCQ00593295 - Not able import foreign configuration immediately after breaking the mirror.
  SCGCQ00602561 - Static Analysis Tool defects
  SCGCQ00563498 - FW should not try to boot iMR mode without informing host if ECC error happens when OS is running.
  SCGCQ00577680 - spin up tracker dequeue is not handled for case in which TUR error happens even after MAX retries
  SCGCQ00603086 - Kill adapter is seen while performing CME recovery during Write operation.
  SCGCQ00466289 - PDs more than 32 which has configuration, is reporting as JBODs after importing from MR to IMR
  SCGCQ00546691 - hostCmdSortingWrites is not updated when VD policy changes(WT/WB)
  SCGCQ00576138 - The restore successful and unsuccessful prints to be handled properly
  SCGCQ00560474 - code review change implemented
  SCGCQ00531118 - Changes to support PD IO history
  SCGCQ00564339 - Enable break mirror support
  SCGCQ00574801 - Implemented Fix to Problem [PDs more than 32 which has configuration, is reporting as JBODs after importing from MR to IMR]
  SCGCQ00577793 - Moved divert code from iopath region to save memory
  SCGCQ00621767 - Update Ptolemy VPD and GasGauge with COL settings for a OEM
  SCGCQ00624326 - Disable sgpioSmpPresenceDetect for OEM
  SCGCQ00625006 - Show valid ROC temperatuer
  SCGCQ00625044 - Change SES Green/Amber LED behavior
  SCGCQ00567706 - Extened LDBBM table to hold more bad block entires (  SCGCQ00295621); with relevent increase in divert nodes.
  SCGCQ00588208 - Adding test routine for the bad block loop test for PR   SCGCQ00423195
  SCGCQ00563795 - Modify MR fw to eliminate four second window where drive swap is not recognized.
  SCGCQ00564166 - Single image support for ONFI
  SCGCQ00455360 - Implement CME solution for "Do not allow 3 minute timer to expire forceing driver to kill fw on CME/disk timeout/etc.
  SCGCQ00563486 - Make MR to iMR migration generic on TMM fault
  SCGCQ00562733 - Support for DIS feature in dual image
  SCGCQ00530866 - command storclif /c1 start diag duration=0 causes controller card to montask.
  SCGCQ00564367 - BGI operation still running on RAID0 VD even after PI protection disabled
  SCGCQ00566951 - LED Blink operation doesn't stop after VD deletion
  SCGCQ00579929 - SGPIO functionality is not working when only cable A is connected 
  SCGCQ00579931 - Potential null pointer derefence
  SCGCQ00614997 - Physical drives go to power save mode just after restarting the server
  SCGCQ00614998 - Physical drives go to power save mode just after restarting the server
  SCGCQ00615001 - Montask in divert.c seen when injecting 64K consecutive errors on R0 VD, Patrol Read running in background.
  SCGCQ00617621 - cache restore failure message displayed though cache restore was successfull
  SCGCQ00620166 - RAID configured on PD been erased with Normal or Thorough will lost after system reboot/reset
  SCGCQ00620168 - RAID configured on PD been erased with Normal or Thorough will lost after system reboot/reset
  SCGCQ00620169 - RAID configured on PD been erased with Normal or Thorough will lost after system reboot/reset
  SCGCQ00621785 - CME handling of Invader
  SCGCQ00622709 - storcli and CtrlR still show new PD information as 4K sector after replacing a 4K sector drive with a 512 sector drive
  SCGCQ00624531 - Cache policy of Virtual Drives(VD) does not change to Write Through(WT) mode even after detecting a bad supercap.
  SCGCQ00631230 - SSD causes system to hang at POST
  SCGCQ00631232 - Behavior change when FW hit fault code 0x81 (uncorrectable ECC error)
  SCGCQ00631474 - Power removal of enclosure FW hits to MonTask: line 4056 in file ../../bbu/onfiBBM.c
  SCGCQ00631478 - Adding 2GB DDR and 4GB Flash combination support for Single Image Write.
  SCGCQ00637535 - FW hits MonTask: line 1143 in file ../../raid/pd.c on starting VD erase in standard mode.
  SCGCQ00638312 - FW crash while launching Ctrl+R
  SCGCQ00640126 - 9240-4i is not getting required memory resources on boot, on Linux it waits 5 minutes, resets the
  SCGCQ00640469 - Running Storcli /C0/CV show or (show all) starts a relearn on supercap issue
  SCGCQ00640470 - L2/L3 cache error on H330 MM & H330 MB on reboot
  SCGCQ00643455 - Defect fix for kenel panic with iMR Fury with Free BSD driver
  SCGCQ00643524 - Defect fix for kenel panic with iMR Fury with Free BSD driver
  SCGCQ00643526 - 9240-4i is not getting required memory resources on boot, on Linux it waits 5 minutes, resets the
  SCGCQ00658583 - Work Around for PPC 476 Errata #46 in MR Firmware
  SCGCQ00658585 - Work Around for PPC476 Errata #46 in iMR Firmware
  SCGCQ00495877 - disableBatteryWarning should not be reset if changed by user
  SCGCQ00552416 - firmware 25.2.0-0013 causes the SEP to not be seen on x4 Equinox
  SCGCQ00555332 - Transparent Learn Cycle does not kick off and RSOC (Relative State Of Charge) eventually goes down to 0%.
  SCGCQ00559322 - EEprom CRC error is detected when WebBIOS is running
  SCGCQ00579928 - AdpDiags does not fail when the SAS link is down
  SCGCQ00588880 - HDD resume failed during dimmer switch test method.
  SCGCQ00630382 - Add MaintainPdFailHistory clear function
  SCGCQ00631340 - Single image support for ONFI
  SCGCQ00637536 - FW hits MonTask: line 1143 in file ../../raid/pd.c on starting VD erase in standard mode.
  SCGCQ00675820 - Updated long term WA for PPC errata #46
  SCGCQ00504394 - For a particular OEM, size of some 4TB drives is reported as zero
  SCGCQ00523966 - Rebuild failed event is not seen when rebuild fails due to LDBBM and SBBM tables getting full (puncturing disabled)
  SCGCQ00552446 - Implement I2C Slave Address for Sideband Management
  SCGCQ00563282 - OEM hi-temp warning not being displayed
  SCGCQ00570249 - OEM SGPIO support not working
  SCGCQ00574969 - Retention test failure during stress test
  SCGCQ00596686 - cntr-R fails to show correct PD sector size once PD's swapped to same slot 512B PD with 512e PD type
  SCGCQ00621783 - Assertion failure (not enough BS found) in double DIP power cycle test case
  SCGCQ00646386 - DIS mismatch while running system reboot script with dirty data in DDR
  SCGCQ00366011 - FW goes to montask at cache offload.
  SCGCQ00498741 - Megamon during Injecting errors to VD with 512e PDs on iMR controller
  SCGCQ00526627 - Faulty protocol used for changing the Disk Write Cache Policy
  SCGCQ00530868 - "OOB:Got DCMD, but FW is not ready " meesages are flooding in tty log during OCR .
  SCGCQ00553197 - Prevent overtemp warnings while charging between 45C and 50C
  SCGCQ00560388 - adapterOperations.alarmControl is being set to 1 even if controller doesnot have alarm on board
  SCGCQ00567378 - CLI Reporting of TMM VPD
  SCGCQ00556598 - megacli reports battery pack is missing on hot insertion
  SCGCQ00679766 - MonTask: line 4699 in file ../../raid/ld.c seen on iMR FW during boot to OS with R0 and PRL11 VD
  SCGCQ00550612 - Do not print VPD86 errors for BP/expander
  SCGCQ00552415 - Modify WCE bit for improved Linux performance
  SCGCQ00560393 - When attempting to secure LD during RLM, receive option to secure LD, LD not secured (message incorrect/misleading.)
  SCGCQ00558037 - Megamon issue when disabling the drive security on a MR controller with spun down FDE drives.
  SCGCQ00560476 - Unable to open "Set Patrol Read Properties" in MSM with 2008-iMR
 BIOS - 6.17.04.0
  SCGCQ00579962 - Initialize deviceExposure with MAX_INT13DISKS instead of 0xFF
  SCGCQ00572939 - Make sure all the make file adheres to the latest binary names.
  SCGCQ00559095 - Provide an option to limit the max number of INT 13h devices presented to system BIOS
 UEFI_Driver - 0x06060A01 (Signed)
  SCGCQ00618669 - StartHiiBackEnd() has Print statement with %g
  SCGCQ00578194 - UEFI Driver should calculate checksum before setting bios data (MR_BIOS_DATA)
  SCGCQ00601851 - System hang when we press F1 on second time when we are in HII form
  SCGCQ00628627 - UEFI Driver- has debug print statements during POST
  SCGCQ00589148 - Diskpart EFI utility can't create partition on a JBOD
  SCGCQ00526851 - Support EFI_FIRMWARE_MANAGEMENT_PROTOCOL for controller firmware upgrade.
  SCGCQ00579837 - UEFI Driver should calculate checksum before setting bios data (MR_BIOS_DATA)
  SCGCQ00606367 - UEFI Driver returns EFI_NOT_FOUND when platform passes valid Target for ExtSPT.BuildDevicePath()
  SCGCQ00644856 - Install FMP on Controller Handle at Start() and the exception
  SCGCQ00644859 - FMP GetImageInfo could result in stack corruption - Code Review Defect ID D26304
  SCGCQ00580313 - User can't access RAID HII in UEFI mode after removing a HDD
 Hii - 03.07.12.01 (Signed)
  SCGCQ00579816 - HII\EKM-LKM without reboot should show proper message
  SCGCQ00594011 - With out selecting any drives I am seeing the previous config VD size.
  SCGCQ00609737 - Confiuration Restore is not working
  SCGCQ00618674 - StartHiiImpl() WriteToLogger uses %g and EFIHiiDriverEntryPoint() Print statement uses %g for displaying EFI status
  SCGCQ00521488 - Getting error message when we suspend Patrol read operation through HII browser
  SCGCQ00565876 - Remove duplicated strings from the UNI FIle
  SCGCQ00571353 - Allow user to select RAID level when controller has other VD + error handling
  SCGCQ00573871 - fixing code review defects (AIM version + UCM GUID + deallocation)
  SCGCQ00614027 - Firmware updation fails in OEM machine
  SCGCQ00615221 - Form UF003 prints error messages (use WriteToLogger to log these debug messages)
  SCGCQ00617617 - FWMgmt Prtocol:<config ID="LSIMegaRAIDConfigurationTool"> has no "versionid" info.
  SCGCQ00565088 - Help content for Firmware Update in Controller Management is inappropriate
  SCGCQ00569098 - Enter security key for locked drives screen, press down to get to OK, OK will show up again on right
  SCGCQ00598822 - VD details display is improper in Expand Virtual Drive
  SCGCQ00613822 - Advanced Controller Properties- Power Saving Settings has broken form
  SCGCQ00556839 - Able to select EKM even when the EKM FOD key is removed from the system.
  SCGCQ00589301 - System/HII hang when clicks on Hardware Components menu option in HII.
  SCGCQ00595864 - On Success of creating Drive Security Form loads into Advacned controller properties
  SCGCQ00598431 - IMR Liberator Drop Down option in VD properties for Cached is present
  SCGCQ00610889 - Customize help string for Select Interface Type
  SCGCQ00615190 - Fill Controller Index in RouteConfig + for UF003 calculate checksume only for the actual config size
  SCGCQ00593558 - Auto Learn Mode is showing wrong data
  SCGCQ00612574 - Addressed review comments
  SCGCQ00613820 - Typo in HII form Controller Status
  SCGCQ00622464 - Toggling bewtween Legacy to Uefi mode vice versa junk values seen .
  SCGCQ00524969 - HII PKG 0006/Going from LKM to EKM asks for a Current Security key Identifier and Security key.
  SCGCQ00590465 - On selecting a wrong parameter for size while creating VDs, Options greyed, Create VD page exits to parent page.
  SCGCQ00595463 - Security feature is enabled but HII sees "Drive Security" as disabled
  SCGCQ00571359 - UCM Phase 1: Typo "Clear Configuaration" -> "Clear Configuration"
  SCGCQ00573222 - Handling Code Collaborator Review Defects for   SCGCQ00568814 and   SCGCQ00569197
  SCGCQ00575062 - added a while loop and take care of the multiple PD Groups scenario.
  SCGCQ00578190 - HII should calculate checksum before setting bios data (MR_BIOS_DATA)
  SCGCQ00597641 - MR6.3 HII aesthetic change
  SCGCQ00503036 - Changing Percentage of Space to Expand Does not Update Final VD Size
  SCGCQ00574041 - AIM (Agentless Inventory Manager) Issues
  SCGCQ00574989 - Creation+ FW updation+ Scan foreign Configuration is disabled/grayed out in HII page
  SCGCQ00614466 - HII 03.07.05.00/Under advanced controller properties and selecting Cache and Memory, it says's "scontroller cache"
  SCGCQ00614675 - To address FW Update help Strings
  SCGCQ00619028 - Not able to schedule CC in concurrent mode from HII(03.07.09.00).
  SCGCQ00526978 - HII. Provide controller FW update function
  SCGCQ00568814 - HEFU. Simplify controller propety page
  SCGCQ00568706 - Remove limitation for creating R6 in HII for OEM
  SCGCQ00612466 - Provide pop-up to display current version and update fw version as part of HEFU HII Firmware Update functionality
  SCGCQ00571579 - (Implemented) - Create a formset with classGUID that customer has provided. 
  SCGCQ00569197 - Move Disable Protection option from Controller Management to VD management
  SCGCQ00557522 - System hang observed when the "PdInfo.userDataBlockSize" is set to 0
  SCGCQ00601110 - Able to select EKM even when the EKM FOD key is removed from the system.
  SCGCQ00601103 - Enter security key for locked drives screen, press down to get to OK, OK will show up again on right
  SCGCQ00601107 - HII PKG 0006/Going from LKM to EKM asks for a Current Security key Identifier and Security key.
  SCGCQ00601119 - HII help for Boot error handling does not display "Stop On Error" option
  SCGCQ00644857 - Remove FMP installed on the controller handle in HII
  SCGCQ00644858 - RSOD during POST after enabling SecureBoot - HEFU.ROM should report exact size of .EFI image
  SCGCQ00629813 - RSOD during POST after enabling SecureBoot - HEFU.ROM should report exact size of .EFI image
  SCGCQ00601113 - HII\EKM-LKM without reboot should show proper message
  SCGCQ00601117 - UCM Phase 1: Allow user to select RAID level when controller has other VD + error handling
  SCGCQ00572986 - System hang observed when the "PdInfo.userDataBlockSize" is set to 0
  SCGCQ00644575 - Consistency Check Start - remove mm/dd/yyyy from the string as the format is out of control of LSI
  SCGCQ00596920 - Missing BBU caused disappearance of Enclosure Mgmt opt in BIOS setup
  SCGCQ00603235 - HII help window shows unsupported stripe sizes
  SCGCQ00601116 - added a while loop and take care of the multiple PD Groups scenario.
  SCGCQ00601118 - UCM Phase 1: Typo "Clear Configuaration" -> "Clear Configuration"
  SCGCQ00601120 - In HII on a ready drive we are able to see Used space as 40Gb.
  SCGCQ00644786 - Enhance help message for PD/VD Operation field
 FCODE - 4.16.08.00
  SCGCQ00553069 - PCLI(1.07.05) Sparc: Command "cli set securitykey=Lsi@12345" fails with errcd "1001" and errmsg "invalid key".
 NVDATA - 3.1403.00-0085
  SCGCQ00709554 - Revise Drive Spin-Up Timing on OEM 12G iMR and MR Boards
  SCGCQ00685089 - Addition of ManPage1 values to the xml file.
  SCGCQ00696438 - Customer NVDATA Change request for iMR
  SCGCQ00692947 - Dual write NVDATA changes for customer
  SCGCQ00673357 - Flatwoods Showing Same Slot Number for All Drives
  SCGCQ00658482 - breakMirrorRAIDSupport for single span Raid 1
 BootBlock - 3.02.00.00-0001
  SCGCQ00685115 - Memory/battery problems in Focused Regression
  SCGCQ00505902 - Coherency bit is disabled in SRAM TLBs
 Ctrl-R - 5.04-0002
  SCGCQ00644489 - Added a new Control to enable/disable JBOD on the controller in Ctrl Mgmt page.
  SCGCQ00648965 - Display the Battery status as N/A for iMR cards.
  SCGCQ00584991 - current write policy is not getting updated untill we press f5
  SCGCQ00584993 - unable to diplay the reason for difference in write policy
  SCGCQ00593822 - Both the Connector information(0-3 & 4-7) is not shown in PD properties while connected in Multipath
  SCGCQ00579583 - Write policy is not added with writeback with BBu when MFC is set
  SCGCQ00573077 - VD Erase will be disabled in Ctrl+R when Initlization on particular VD is aborted
  SCGCQ00585013 - Added the code to unset the boot-device to NONE
  SCGCQ00584991 - current write policy is not getting updated untill we press f5 .
  SCGCQ00584993 - unable to diplay the reason for difference in write policy
  SCGCQ00593822 - Both the Connector information(0-3 & 4-7) is not shown in PD properties while connected in Multipath
  SCGCQ00579600 - Write policy is not added with writeback with BBu when MFC is set
  SCGCQ00579607 - VD Erase will be disabled in Ctrl+R when Initlization on particular VD is aborted
  SCGCQ00585013 - Added the code to unset the boot-device to NONE
 PCLI - 1.07.05
  SCGCQ00501437 - StorCLI - MR 6.2 StorCLI help syntax is wrong for R1EC
  SCGCQ00518543 - PCLI Sparc(1.07.02):" Cli show all" command fails with error msg "Error! App exec failed in FW PCLIError! Internal".
 ROMENV - 1.09

Package: 24.2.1-0021 (MR 6.2)
 Firmware 4.220.40-3267
  SCGCQ00651072 - Battery learn cycle continues to more than one cycle even FW has marked it as bad in previous reboot
  SCGCQ00645802 - DIS mismatch while running system reboot script with dirty data in DDR
  SCGCQ00644122 - Optiomize onfi descriptor setting for offload
  SCGCQ00637239 - FW crash while launching Ctrl+R
  SCGCQ00612786 - Assertion failure in double DIP power cycle test case
  SCGCQ00604253 - Elapsed time of Patrol Read in tty log is incorrect
  SCGCQ00602839 - Elapsed time of Reconstruction is incorrect
  SCGCQ00598917 - Firmware not taking "SMARTerEnabled" from NVDATA
  SCGCQ00598825 - Rebuild triggered on an incompatible blocksize PD
  SCGCQ00573764 - Upgrade 3108 MR FW failing
  SCGCQ00569093 - PD erase does not work with SATA SSDs
  SCGCQ00558985 - Diagnostics failed after Drives goes to shield state
  SCGCQ00549095 - The DQlog.bin is getting corrupted after restarting the service of MRDiag
  SCGCQ00546653 - protect the removal of the device when the device is still under initialization
  SCGCQ00527932 - BIOS is not getting updated with the DISM progress
  SCGCQ00527416 - Running out of free entries in task list due to recursive addition of tasks
  SCGCQ00527397 - Wrong information of PD erase progress is shown by the firmware.
  SCGCQ00527241 - DM_DISM_LOG_SENSE state is not present in DISM
  SCGCQ00524801 - PI enabled VD is importing successfully even though "prevent PI Import" option is enabled
  SCGCQ00524040 - Change the CRC filed size
  SCGCQ00518855 - Fix the learn issue at powerup
  SCGCQ00505401 - LSI_MR Controllers fails to set "FACTORY SETTINGS"
  SCGCQ00503341 - VD's switch from Write Back with BBU to Write Through when an OCR is issued and BBU gets disabled.
  SCGCQ00503309 - Fix scheduling of hostspare correctly
  SCGCQ00503257 - seen DC error while running io's on 6.2 in Dev pull-push setup
  SCGCQ00499700 - chaos fails on R6 VD after importing failed R5 VD and one of R1 CacheCade drive
  SCGCQ00499455 - Defect fix for MSM doesnot show Create cachecade option
  SCGCQ00495896 - To fix task list overflow issue on max config setup
  SCGCQ00452322 - FW throws "MPT_LogDiscoveryErrors: SAS_TOPOLOGY_MAX_TOPO_PHYS_EXCEED" when connect 2 in multi-path
  SCGCQ00457909 - Assertion failure in ../../raid/raidpci.c at line 10522
  SCGCQ00461907 - Read VPD error message on 3108
  SCGCQ00464372 - Configurable drives count in iMR reflected wrongly to applications
  SCGCQ00466545 - wrong error code displayed and wrong error message for copyback command
  SCGCQ00466936 - FW hits to MonTask: while running enclosure power cycle with 4K drives
  SCGCQ00469174 - Issue with supercap energy calculations
  SCGCQ00470287 - modify scap energy calculation
  SCGCQ00471823 - directly attached SATA drive is not detected by controller
  SCGCQ00472614 - Dual Context to Single Context switching does not toggle when Cobra expanders are cascaded with EDFB enabled PHY's.
  SCGCQ00473420 - Defect fix for Montask observed while installing OS on JBOD
  SCGCQ00476945 - Controller Hangs during execution of Storcli command ''/c0 delete termlog''
  SCGCQ00477266 - Battery retention test failure during contnuous loop test when there was power failure during erase
  SCGCQ00477667 - Battery Enable (BBE) is asserted even when BBU/Supercap not present or even when all LDs are in WT mode
  SCGCQ00485545 - TM timeout during enclosure pull while running heavy IO
  SCGCQ00486810 - Learn is not completing at powerup
  SCGCQ00487215 - 3TB Seagate PD size being reported as 2TB in Apps/Firmware
  SCGCQ00493312 - Controller Reset due to Fatal Error with RAID6/60 configuration
  SCGCQ00494704 - Elapsed Seconds displayed in firmware logs for background operations progress is improper
  SCGCQ00384656 - Kill adapter observed while running IOs on JBODs and VDs
  SCGCQ00614723 - CME handling of Invader
  SCGCQ00599798 - Issue with Global Hot Spare assignment
  SCGCQ00596434 - Drives connected through enclosure showing wrong slot numbers.
  SCGCQ00580415 - issue with MR 24.1.1-003 with JBOD Mode enabled
  SCGCQ00557580 - (null) noticed while PD pull-push testing.
  SCGCQ00554546 - SMPpassthru is not happening through storlib.
  SCGCQ00551614 - System Reboots after issuing the OCR and kernel panic is observed
  SCGCQ00524812 - on breaking multipath while drives are spinnning up results in montask
  SCGCQ00523544 - Initialize invalid interrupt as part of intInitialize function
  SCGCQ00518692 - OEM server hangs after enabling EKM and rebooting.
  SCGCQ00505537 - Associating cachecade VD to a secured VD from Storcli does not fail.
  SCGCQ00496454 - Offload fails after corrupting BMT1 and BBT 2 address location
  SCGCQ00496422 - Adding the log event corresponding to ER   SCGCQ00493492
  SCGCQ00435204 - BGI kicks in on 5R5 but shows no progress at any point of time.
  SCGCQ00446327 - Defect fix for Unable create R0 in HII with 4K drives
  SCGCQ00451805 - FW-FW hit 'MonTask: line 243 in file ../../raid/1078in' while issuing OS reboot command on 9340 controller
  SCGCQ00470310 - CPLD input GPIO 21 driving when supercap is present and not present
  SCGCQ00472407 - Pinned cache gets flushed even after memory battery problem occurs.
  SCGCQ00474617 - VD erase restars instead of resuming after reboot.
  SCGCQ00477301 - Fix the cset issue
  SCGCQ00478707 - Cache Memory Size of controller Information is ZERO
  SCGCQ00484448 - Data Corruption observed while running FPIO on VDs; making-breaking multipath in overnight loop.
  SCGCQ00486766 - Config loss after OCR during creation of config - when the drives are still spinning up
  SCGCQ00486982 - Added an event to notify the user when command times out on PD
  SCGCQ00487803 - FDE/SED drives does not reflect as FDE/SED drives.
  SCGCQ00605077 - "Corrected medium error" event is logged for uncorrectable mendium errors during PR
  SCGCQ00530495 - To declare block bad at the earliest for the safer side the number of error correction bits shall be reduced
  SCGCQ00504346 - Re-enable EKMS for OEM
  SCGCQ00421822 - System reboots continuously after flashing Firmware in Solaris _11
  SCGCQ00460033 - MonTask: line 7193 in file ../../bbu/onfi.c
  SCGCQ00461733 - Kill adapter observed on large setup on enquiring Controller properties while drives spinning up from powersave.
  SCGCQ00463368 - coverity tool reported issue 13545(Wrong sizeof argument)
  SCGCQ00465561 - restore and flushing cache to PD are not reliable when 1st image of NF mem is corrupted
  SCGCQ00470502 - Firmware is allow to create slices in cachecade drivegroup using SMIS utility.
  SCGCQ00474005 - EKMS feature for OEM is disabled
  SCGCQ00474734 - max temperature bytes read from VPD is should be swapped before using
  SCGCQ00477996 - MR_6.2_DISM: FW hung due to DISM discovery failure on pulling the enclosure cable on reboot after running adpbattest.
  SCGCQ00488780 - Controller alarm continues to beep after transitioning VD from degraded to optimal state.
  SCGCQ00494084 - Handle OEM falut LED behavoir
  SCGCQ00556570 - MR6.2_iMR_fury_DM_Issue_TUR
  SCGCQ00524903 - In enclosure management page for DELL ,it shows some junk data in HII
  SCGCQ00501356 - Controller Reset due to Fatal Error with RAID6/60 configuration
  SCGCQ00402933 - CME logic using overlaid fields in c->rec
  SCGCQ00460254 - Montask appears on running IO's on 64VD's while changing LD policies
  SCGCQ00465672 - Enable OCR by default on GCA builds
  SCGCQ00480503 - MR: on FW init, controller post adapter base port missing
  SCGCQ00495361 - Invalid "Elapsed Seconds" value for FGI
  SCGCQ00531106 - Rebuild and Consistency Check aren't progressed when it is executed by CTL+R
  SCGCQ00518734 - Latest API changes in mr.h breaks FW compilation in mrdebug.c
  SCGCQ00464536 - Build Issue using GNUmakefile for MR and iMR
  SCGCQ00524913 - Storcli command to reset the boot ld on controller fails
  SCGCQ00506335 - boot block compile fails because of an erroneous macro definition
  SCGCQ00468366 - DATA TLB error faced while powercycle the enclosure during controller initialization 
  SCGCQ00490696 - foreign import fails if degraded VD is present in import
  SCGCQ00415512 - Toolbox Console Text Display Tool
  SCGCQ00451314 - Porting of the PR "spin up changes to accommodate multiple power domains simultaneously" to Invader.
  SCGCQ00460871 - Validate the requested blocks for SCSI VERIFY commands on RAID volumes
  SCGCQ00466819 - IOCInit multiple Reply Descriptor Post Queue addresses
  SCGCQ00471500 - Firmware Change for Pre-boot management tool & boot capability for SPARC
  SCGCQ00477817 - add reserved fields to IO Unit Page 7 for future use
  SCGCQ00481549 - Disable thermal throttle changes
  SCGCQ00493492 - Identifying the DDR, ONFI flash and SCap combination
  SCGCQ00518786 - SGPIO back plane requires ramdon slot number support.
  SCGCQ00595486 - Increase PCIe Receiver Margin
  SCGCQ00595487 - Increase margin in PCIe Rx Serdes
  SCGCQ00438437 - obsolete SAS IO Unit Control _TRANSMIT_PORT_SELECT_SIGNAL
  SCGCQ00471293 - obsolete "Limit SATA max rate to 1.5 Gbps"
  SCGCQ00490725 - Debug Queue Implementation and Support as part of enhanced MR Diagnostic support
  SCGCQ00573397 - Increase the support for 32 slots
  SCGCQ00585068 - Add Critical event in FW to indicate that an INIT operation was halted due to reboot or other failure
  SCGCQ00593824 - Update code to modify GG and VPD at powerup
  SCGCQ00468085 - Implement throttle mechanism to prevent thermal run away
  SCGCQ00472399 - Change hash algorithm for cache row hash from a bit mask to a modulo
  SCGCQ00556564 - DIS feature
  SCGCQ00469990 - Signed images for FWDownload
  SCGCQ00342679 - Don't interpret the cachecade BVD flags if the volume is created with old FW which does not support cachecade.
  SCGCQ00359329 - Code-review action item for removing and updating names for AEN dism.
  SCGCQ00454419 - Patrol Read - no progress
  SCGCQ00462259 - WB Logical disks are moving to WT after corrupting BMT1,BBT1 and reboot.
  SCGCQ00462309 - Deep Learn is not invoked in new battery, when the system is reboot before the first learn completes
  SCGCQ00462327 - Transparent Learn Cycle is rescheduled even though it is not completed
  SCGCQ00469037 - TFM error handling : Cache policy change for WB to WT if supercap is faulty
  SCGCQ00469755 - Intermittent SEP errors on iMR and MR controllers
  SCGCQ00471540 - When Cachecade LD is deleted invalid LD details is shown in the Cachecade size changed event.
  SCGCQ00473330 - Hotspare Recovery Doesn't Start after Inserting Failed Drives
  SCGCQ00478032 - FW sending wrong configuration data during boot msg pending state
  SCGCQ00479443 - Upgrading from Software RAID to 9260-8i causes Alarm to sound
  SCGCQ00482660 - ONFI_BBM Dev test build: FwTermLog does not preserve information before powerup. 
  SCGCQ00483590 - iMR TB Data loss when reconstructing from 1 drive R0 to 2 drive R1 with reboot
  SCGCQ00484771 - incorrectly uses a slot offset value to enumerate HDD.
  SCGCQ00485259 - In case of a certain OEM iMR shows R5 enabled.
  SCGCQ00492432 - MSM log warning: Controller booted in headless mode with errors
  SCGCQ00495888 - Set the Recovery mode page (WriteRetryCount and recoveryTimeLimit)
  SCGCQ00498734 - If VD is secured while reconstruction is going on does not stay secured once reconstruction is done.
  SCGCQ00498742 - SEAGATE hotspare drives remain spun up on LSI FW 12.12.0-0079
  SCGCQ00498946 - Firmware is not updating recovery timer as intended
  SCGCQ00502953 - Call DDF_discardInvalidPds only if DS3 is enabled
  SCGCQ00518879 - LSI_MR Controllers fails to set "FACTORY SETTINGS"
  SCGCQ00521513 - Controller Reset due to Fatal Error with RAID6/60 configuration
  SCGCQ00521758 - VPD output of lspci –vvxxx showing [RV] Reserved: checksum bad, 86 byte(s) reserved
  SCGCQ00523958 - Multi-stripe size in each raid level of R1,r5,r6 with SAS, DIF, 4K pinned cache offline vd import cause Montask
  SCGCQ00523962 - Remove memory module on MR controller to downgrade to iMR does not work
  SCGCQ00523970 - HII critical message form/Extra character "r" with configuration not supported critical message.
  SCGCQ00523976 - Fw defect in PdStateSet()
  SCGCQ00524442 - Controller Reset due to Fatal Error with RAID6/60 configuration
  SCGCQ00524493 - Correct how the SCL high and low period values are calculated for the I2C to run at 400Khz
  SCGCQ00524494 - For new spin up code get persistent devId for drives that are connected via internal back plane.
  SCGCQ00526284 - Controller Reset due to Fatal Error with RAID6/60 configuration
  SCGCQ00526632 - Drive security mode switching in MSM
  SCGCQ00526633 - Unable to create another Virtual Drive when pulling first drive (degrading) in partial Virtual Drive where all drives are configured
  SCGCQ00549320 - Baseboard Management Controller (BMC): STP passthru command failure
  SCGCQ00552443 - External Key management security for iMR
  SCGCQ00552444 - Re-keying a controller with External Key Management(EKM) security enabled, results in a corrupted key ID.
  SCGCQ00554050 - Performing an online firmware update or Online Controller Reset(OCR) on a controller with External Key Management(EKM) enabled, results in all secured drives marked as foreign.
  SCGCQ00558051 - MR 4K Validation : 4K VD assigned to 512K CacheCade
  SCGCQ00559254 - Re-keying in External Key Management mode followed by disabling security and enabling LKM results in a bail out while creating a Virtual Drive
  SCGCQ00562800 - VD goes offline when we start reconstruction on 32 Drive R0 VD
  SCGCQ00566690 - Raise priority of pci config trap interrupt to critical
  SCGCQ00567036 - Not seeing the correct Boot Message when the connection to the External Key Management server is down
  SCGCQ00575842 - Switching to Local Key Management Mode(LKM) after a rekey in External Key Management(EKM) rekey without rebooting results in HII saying key incorrect but Firmware says key was created.
  SCGCQ00575843 - On a controller with Local Key Management(LKM) enabled, user is asked to enter the security key to unlock and import a foreign, locked and External Key Management(EKM) enabled drive.
  SCGCQ00579499 - FwTermLog does not preserve information before powerup. 
  SCGCQ00579847 - Implement I2C Slave Address for Sideband Management
  SCGCQ00580752 - Defect Fix for VPD and inquiry callback issues in DISM
  SCGCQ00580771 - spin up tracker dequeue is not handled for case in which TUR error happens even after MAX retries
  SCGCQ00588963 - Too many unexpected sense AEN raised by CC during CME recovery on R5
  SCGCQ00588964 - Too many unexpected sense AEN raised by CC during CME recovery on R5
  SCGCQ00588973 - Fix GNU make file compilation
  SCGCQ00588977 - Routines to inject bit error in NF and ecc error in DDR for ONFI
  SCGCQ00588978 - Mismatch in LD id and target ID during set/reset boot device
  SCGCQ00588979 - Mismatch in LD id and target ID during set/reset boot device
  SCGCQ00593826 - Adding test routine for the bad block loop test for PR   SCGCQ00423195
  SCGCQ00595783 - SMART poll needs to issue log sense with page control set to current/ cummulative value
  SCGCQ00597425 - FW breaks if wrong security key is entered
  SCGCQ00604028 - on breaking the multipath in loop while drives are spinnning up will result in montask
  SCGCQ00604030 - FW hangs while creating 64 VDs on the controller with SLES11 SP2 PPC64
  SCGCQ00604033 - While running reconstruction from R1 to 4 drive PRL11 with IO,FW hits to MonTask: line 1270 in file ../../raid/1078dm
  SCGCQ00604041 - Static analysis tool defect
  SCGCQ00604042 - Static Analysis Tool defects
  SCGCQ00609872 - CLI Reporting of TMM VPD
  SCGCQ00610801 - Rebuild triggered on an incompatible blocksize PD
  SCGCQ00610813 - Issue with Global Hot Spare assignment
  SCGCQ00610824 - Elapsed time of Reconstruction is incorrect
  SCGCQ00610834 - Elapsed time of Patrol Read in tty log is incorrect
  SCGCQ00610846 - "Corrected medium error" event is logged for uncorrectable mendium errors during PR
  SCGCQ00612226 - Increase margin in PCIe Rx Serdes
  SCGCQ00612228 - Increase PCIe Receiver Margin
  SCGCQ00620118 - Liberator Card loses its boot VD after many reboots
  SCGCQ00635628 - Cache policy of Virtual Drives(VD) does not change to Write Through(WT) mode even after detecting a bad supercap.
  SCGCQ00638288 - RAID configured on PD been erased with Normal or Thorough will lost after system reboot/reset
  SCGCQ00646479 - Defect fix for kenel panic with iMR Fury with Free BSD driver
  SCGCQ00651117 - Hitting montask line 1930 in file ../../bbu/onfi.c while running FP IO's on degraded VD's
  SCGCQ00335860 - Cachecade configurations could not be created.
  SCGCQ00462330 - Deep learn doesn't start when it is requested during relaxing.
  SCGCQ00469041 - Write policy changed from WT to WB when the battery/Supercap is declared as bad
  SCGCQ00471509 - Firmware crash seen while doing continuous sas cable pull
  SCGCQ00471542 - Invalid "mode select(Page=0a)" issued during disk initialization phase.
  SCGCQ00477967 - Defect fix for Montask observed while installing OS on JBOD
  SCGCQ00478050 - Firmware returns asc value as 0 when failing IOs with medium errors
  SCGCQ00482662 - display BMU fw version in battery design info
  SCGCQ00482663 - Break Mirror for R10 should not be allowed
  SCGCQ00486553 - Medium error correction event is not logged during CC
  SCGCQ00498748 - 9240-4i on BCM RX67Q-6S motherboard is not getting required memory resources on boot
  SCGCQ00503258 - foreign import fails if degraded VD is present in import
  SCGCQ00504804 - L2/L3 cache error on reboot
  SCGCQ00514666 - search for one wire devices prints are masked after the boot
  SCGCQ00518020 - VPD info can't be retrieved for OEM enclosure
  SCGCQ00523959 - If a BOOT Passphrase is enabled with SafeStor "MegaCli adpbios dsply a0" will display "BIOS will Stop on error" even if any other mode is set.
  SCGCQ00523972 - Profile based VD creation - [Partial RAID options blocked until system reboot]
  SCGCQ00523975 - Hard coded values should be removed in TFM module
  SCGCQ00524802 - Fix repeated prints issue
  SCGCQ00559253 - A data TLB error occurs when the External Key Management Server(EKMS) is down and drive security is changed from External Key Management(EKM) mode to Local Key Management(LKM) mode.
  SCGCQ00563824 - HII & Ctrl-R: BGI operation still running on RAID0 VD even after PI protection disabled
  SCGCQ00575844 - Getting a non informative message when trying to import a Virtual Drive after a re-key without reboot
  SCGCQ00577296 - Deep learn will not start immediately when Relative State of Charge (RSOC) of battery is equal to 95%.
  SCGCQ00593485 - Raid configuration loss after reboot - PDs in POWERSAVE
  SCGCQ00600939 - Fix the learn issue at powerup
  SCGCQ00603399 - Faulty protocol used for changing the Disk Write Cache Policy
  SCGCQ00604029 - on breaking the multipath in loop while drives are spinnning up will result in montask
  SCGCQ00604031 - FW- FW hangs while creating 64 VDs on the controller with SLES11 SP2 PPC64
  SCGCQ00604038 - Static Analysis Tool defects
  SCGCQ00604039 - Static Analysis Tool defects
  SCGCQ00604074 - Enabling DQ support bit in FW
  SCGCQ00610444 - The restore successful and unsuccessful prints to be handled properly
  SCGCQ00614828 - not enough bs found during double Dip power cycle Test
  SCGCQ00615002 - Montask in divert.c seen when injecting 64K consecutive errors on R0 VD, Patrol Read running in background.
  SCGCQ00615537 - Single image support for ONFI
  SCGCQ00635323 - Assertion failure (not enough BS found) in double DIP power cycle test case
  SCGCQ00651115 - DC observed upon performing OCR on a degraded R1 (AWB).
  SCGCQ00450647 - 9260-8i(SAS2108) hitting OOB SRAT timeout for a long time causing OOB commands to fail
  SCGCQ00470568 - modify scap energy calculation
  SCGCQ00483575 - wrong error code displayed and wrong error message for copyback command
  SCGCQ00485096 - Bad or Missing TMM boot message is changed to Critical error
  SCGCQ00498752 - 9260-16i's drive locate/fault LED header doesn't work
  SCGCQ00518011 - MR Controller does OCR due to Temp Buffer overflow
  SCGCQ00523459 - The Firmware does not change the Virtual Drives's from Write Through to Write Back after a battery manual learn cycle is complete
  SCGCQ00554074 - SLES 11.3 x64 Halts when Loading Kernel During Warm Reboot Stress
  SCGCQ00555052 - Initialize invalid interrupt as part of intInitialize function
  SCGCQ00567037 - Switching the security mode from External Key Management(EKM) to Local Key Management(LKM) on iMR controller will result in a corrupted controller key.
  SCGCQ00595833 - SMART poll needs to issue log sense with page control set to current/ cummulative value
  SCGCQ00604043 - Static Analysis Tool defects
  SCGCQ00617625 - Power removal of enclosure FW hits to MonTask: line 4056 in file ../../bbu/onfiBBM.c
  SCGCQ00359282 - Multiple interposer drives will not be detected by MegaRAID firmware.
  SCGCQ00454415 - Infinite retry happens on Test Unit command when HDD didn't respond to TU command during the initialization.
  SCGCQ00462149 - Secondary RAID key data page read failure 6 seen on some controllers and key vault combination
  SCGCQ00478428 - StorCLI_F showed firmware download failed but really took
  SCGCQ00481856 - Assertion failure in ../../raid/raidpci.c at line 10522
  SCGCQ00484769 - FW Crash when using SCSI Passthrough SCSI_READ_10(0x28) to read 512 bytes on a RAID5 Native 4K drive.
  SCGCQ00492431 - When pinned cache present VD property not changing from WB to WT.
  SCGCQ00492433 - PDs go online without VD created & App doesn't allow any VD creation on passing a wrong parameter in Spanned VD.
  SCGCQ00497659 - Customer is hitting an ECC error
  SCGCQ00521514 - Invader: Cache Memory Size of controller Information is ZERO
  SCGCQ00554312 - Incorrect variable type in MR Read/Modify/Write path
  SCGCQ00598504 - StorCLI_F showed firmware download failed but really took
  SCGCQ00617620 - cache restore failure message displayed though cache restore was successfull
  SCGCQ00372236 - System hanged after pulling out drives from a 8Raid-6 array during OCR in Debian OS
  SCGCQ00454381 - Change SES Green/Amber LED behavior for OEM ACHILLES JBOD enclosure.
  SCGCQ00597426 - FW breaks if wrong security key is entered
  SCGCQ00366030 - While executing path-failover test with an SATA-SSD drive behind an interposer, the device is marked failed.
  SCGCQ00454368 - Card Running iMR Machine Checks when Requesting Host Memory
  SCGCQ00456776 - iMR FW update caused card to FW fault state and card cannot boot to OS.
  SCGCQ00479292 - system black screen during S1 Sleep test
  SCGCQ00490892 - Firmware Crash during Controller StartUp when large number of drives are connected
 UEFI_Driver 0x06030501
  SCGCQ00478652 - Block IO tests from SCT IHV test suite failed
  SCGCQ00479003 - Disable Debug print in UEFI Driver
  SCGCQ00498925 - Not able to boot into BIOS boot menu
  SCGCQ00518791 - In IsValidHandle() - Free the buffer if status is not EFI success for LocateHandle
  SCGCQ00493654 - Memory Leak issue in UEFI driver when reconnect happens
  SCGCQ00483847 - Remove private GUID and use EFI_KMS_PROTOCOL_GUID defined in UEFI 2.3.1 spec
  SCGCQ00479016 - Disable Debug print in UEFI Driver
  SCGCQ00484085 - UEFI hang when SATA is connected
  SCGCQ00484086 - UEFI hang when SATA is connected
  SCGCQ00579837 - UEFI Driver should calculate checksum before setting bios data (MR_BIOS_DATA)
  SCGCQ00468948 - Uninstall HII CAP and Driver Health formset if platform calls Start again without calling GetHealthStatus
  SCGCQ00477828 - 9240/9260/9270 UEFI driver issue with RD640/RD440 platforms when user having 2TB or 4TB VD
  SCGCQ00477705 - 9240/9260/9270 UEFI driver issue with RD640/RD440 platforms when user having 2TB or 4TB VD
  SCGCQ00484113 - Follow UEFI Spec on interpreting In and Out Transfer Length that upper layer sends
  SCGCQ00478692 - Block IO tests from SCT IHV test suite failed
  SCGCQ00484114 - Follow UEFI Spec on interpreting In and Out Transfer Length that upper layer sends
 Hii 03.05.11.03
  SCGCQ00470101 - Allow user to edit VD size (that is free form input) as it is cumbersome to modify the size using +/-
  SCGCQ00471830 - Save and Restore Configuration – MR
  SCGCQ00556209 - Transition a Thunderbolt MR controller to run in iMR mode = Controller fail in HII After Memory removed
  SCGCQ00556811 - When controller is in safe mode the PD menu displays inaccurate text and hangs when clicking a PD
  SCGCQ00579816 - HII\EKM-LKM without reboot should show proper message
  SCGCQ00452128 - HII cannot assign partial space less than 1 GB
  SCGCQ00573871 - fixing code review defects (AIM version + UCM GUID + deallocation)
  SCGCQ00529287 - Profile Based Raid1 Creation fails as invalid arguments
  SCGCQ00502940 - Naming inconsistency in option present in Create VD and Create VD - Advanced
  SCGCQ00482092 - condition checking is not right
  SCGCQ00474402 - Allows user to select EKM mode when supportEKM is set to 0
  SCGCQ00485401 - Using 84 PD encl when clicking on HW, Advanced then Enclosure Management, it completly freezes the system
  SCGCQ00571353 - Allow user to select RAID level when controller has other VD + error handling
  SCGCQ00569098 - Enter security key for locked drives screen, press down to get to OK, OK will show up again on right
  SCGCQ00473204 - unable to show UF003 as well the first two forms + XML special character handling
  SCGCQ00486457 - fixing memory leak of 128 drive enclosure implementation
  SCGCQ00556839 - Able to select EKM even when the EKM FOD key is removed from the system.
  SCGCQ00505566 - Drop down option to set phy linkspeed tp 12 Gbps in HII browser is not available.
  SCGCQ00473186 - Save and Restore Configuration - MR w/ Premium Features (SED and Cachecade)
  SCGCQ00501111 - Issues when trying to change EKM security key from change security key option.
  SCGCQ00523869 - EKMS is down but it is still possible to select drive security in MSM and HII during creation.
  SCGCQ00524969 - Going from LKM to EKM asks for a Current Security key Identifier and Security key.
  SCGCQ00527700 - Update the latest API change in HEFU
  SCGCQ00571359 - UCM Phase 1: Typo "Clear Configuaration" -> "Clear Configuration"
  SCGCQ00500945 - EXPAND operation fails in HII for prl11
  SCGCQ00494431 - Streamline the usage of max PD in limited configuration path (alias UCM)
  SCGCQ00494214 - Help content for Free space in Select Drive group is inappropriate
  SCGCQ00485932 - UCM Simple Configuration: Allow Clear Config always + Suppress Checkbox (Uf002.PDs) when VD count is >0
  SCGCQ00575062 - added a while loop and take care of the multiple PD Groups scenario.
  SCGCQ00574041 - AIM (Agentless Inventory Manager) Issues
  SCGCQ00481284 - Typos in help content for profile VD for Write Policy
  SCGCQ00472196 - Profile based VD creation path incorrectly showing protect VD/secure VD checkbox when user clicks on drive selection criteria
  SCGCQ00471209 - config using 8PDs/16 partial VDs and all stripe sizes and HSPs does not restore
  SCGCQ00487936 - After creating a VD with UCM tool the manual configuration PD section still shows configured PDs as UG, and duplicates
  SCGCQ00495236 - Controller not seen in HII Browsercan after switiching from EFI WebBIOS
  SCGCQ00505591 - Checking the Enclosure Management settings in HII causes the system to reboot.
  SCGCQ00475217 - Request to support 128 drives wihin single enclosure
  SCGCQ00468930 - UCM Phase 2 support
  SCGCQ00571579 - (Implemented) - Create a formset with classGUID that customer has provided. 
  SCGCQ00481277 - Request to change the help content for write policy in create VD form
  SCGCQ00415456 - Obtain the Physical Slot number from the PCI Bridge to which the Controller is connected.
  SCGCQ00557522 - System hang observed when the "PdInfo.userDataBlockSize" is set to 0
  SCGCQ00476607 - HII cannot assign partial space less than 1 GB
  SCGCQ00629813 - RSOD during POST after enabling SecureBoot - HEFU.ROM should report exact size of .EFI image
  SCGCQ00482099 - Typos in help content for profile VD for Write Policy
  SCGCQ00498521 - HII cannot create a VD using unconfigured good drives as long as PD locate is set on the drives
  SCGCQ00477863 - Obtain the Physical Slot number from the PCI Bridge to which the Controller is connected.
 BIOS 6.14.05.0
  SCGCQ00479507 - Getting memory conflict during boot 
  SCGCQ00455591 - Memory access issue when loading Ctrl R
  SCGCQ00495471 - OOB function corrupts EBDA area used by other server function
  SCGCQ00552308 - not allocating memory correctly when MR and iMR are in the same system
  SCGCQ00493680 - Optimize reading IO port in INT15h path
  SCGCQ00482283 - System reboots during IO because FW didnt receive permanent host memory from OpROM
  SCGCQ00503046 - OpROM is displaying incorrect value for the number of INT13h device it supports
  SCGCQ00559094 - Provide an option to limit the max number of INT 13h devices presented to system BIOS
  SCGCQ00466276 - Check the controller status bit in the function which hooks INT15
  SCGCQ00455597 - Allocate only two 64k
  SCGCQ00454086 - Add boundary checking when allocating EBDA and PMM memory for BIOS post.
  SCGCQ00504752 - OpROM is displaying incorrect value for the number of INT13h device it supports
  SCGCQ00460724 - Memory access issue for Mercury when loading Ctrl R
  SCGCQ00460725 - Memory allocation: Allocate only two 64k
  SCGCQ00501253 - OOB function corrupts EBDA area used by other server function
 Ctrl-R 5.03-0005
  SCGCQ00485184 - Change Emergency Spare to NONE with enable enmergency on Smarter checked will fail with error=03
  SCGCQ00487220 - ctrl-r dosent list all the drives to do replace drive.
  SCGCQ00487602 - Power savings button not enabled on Ctrl-R
  SCGCQ00490688 - ctrl-H doesn't list the drives to do replace drive while doing copyback in PD MGmt Screen
  SCGCQ00490789 - Selecting "Manage Link Speed" in CTL+R causes Fatal Error with SAS 9343-4i
  SCGCQ00493479 - Implemented the safe mode in Ctrl-R
  SCGCQ00518579 - Unable to make R10 through Ctrl R using 4k drives
  SCGCQ00593396 - Default (Initial) setting of VD doesn't reflect MFC's setting
  SCGCQ00606717 - /c0/pall show and Linkspeed information is not in same in Ctrl-R.
  SCGCQ00601637 - Changes in BIOS mode (pause on error) to be in sync
  SCGCQ00601691 - Need to display controller memory in Control-R
  SCGCQ00568108 - showing "BIOS Mode" in both the pages of ctrl mgmt
  SCGCQ00568688 - Help content is not updated with the Key stroke added
  SCGCQ00573077 - VD Erase will be disabled in Ctrl+R when Initlization on particular VD
  SCGCQ00579583 - Write policy is not added with writeback with BBu when MFC is set
 BootBlock 3.02.00.00-0000
  SCGCQ00288393 - iMR boot Block code intial changes
  SCGCQ00322313 - Errbios load fails on Fury adapters
  SCGCQ00337925 - Merged 6.0 boot block changes to 6.1
  SCGCQ00313425 - Bootblock is using NVRAM data even if NVRAM is uninitialized
  SCGCQ00371801 - Configure chip reset to link down
  SCGCQ00375108 - Added the code to enable OCM RMW errors
  SCGCQ00505902 - Coherency bit is disabled in SRAM TLBs
 NVDATA 3.1310.00-0070
  Numerous changes for specific customers
 FCODE 4.16.08.00
  SCGCQ00553069 - PCLI(1.07.05) Sparc: Command "cli set securitykey=L
  SCGCQ00471703 - Fcode CLI support for Invader (MR only)
  SCGCQ00486355 - Define and use capability bit to identify the StorCLI
 PCLI 1.07.05
 ROMENV 1.09

----------------------------------------------------------
Package: 24.1.1-0006 (MR 6.1)
 Firmware 4.210.50-3015
  SCGCQ00383439 - fix for the defect - 4k drives display wrong value of Coerced size.
  SCGCQ00573649 - JBOD mode drive cannot be set as Bootdrive when Only JBOD Mode drive exist in MR6.1
  SCGCQ00563950 - Fix for Infinite retries of command for sense code 0B/47/03
  SCGCQ00523831 - controller does not boot after Cache Offload
  SCGCQ00521575 - LSI BIOS POST displays F/W initialized percentage greater than 100% i.e 106%
  SCGCQ00452322 - FW throws "MPT_LogDiscoveryErrors: SAS_TOPOLOGY_MAX_TOPO_PHYS_EXCEED" when connect 2 enclosures in multi-path
  SCGCQ00448575 - Fix coverity defect 13424
  SCGCQ00448009 - Defect Fix for Exception in Core 0
  SCGCQ00440474 - MISCOMPARES FOUND DURING COPYBACK
  SCGCQ00433521 - boards have issue in bootup after the wait time was increased in finding the ONFI flash configuration
  SCGCQ00426148 - Fix the unhandled interrupt by minimizing the critical interrupt
  SCGCQ00422673 - FW hit Montask with line 782, L2/L3 cache error when one drive is pulled out from enclosure
  SCGCQ00421805 - Changes to SMARTerEnabled and SSDSMARTerEnabled are not reflected in controller properties
  SCGCQ00420102 - fw breaks into montask on transporting ONFI module from 4i contoller
  SCGCQ00419935 - Change IO time out value to 20 seconds for FW initiated IOs
  SCGCQ00415989 - Modify the code to support tty dump in interrupt context
  SCGCQ00413690 - MSM freezes until full initialization completes when configuration created
  SCGCQ00349837 - Sequential Read performance is less on CacheCade associated LD's.
  SCGCQ00567996 - ECC Errors in tty logs
  SCGCQ00550456 - removing the cset   SCGCQ00550153: Identifying the DDR, ONFI flash and SCap combination
  SCGCQ00456094 - Data Corruption seen upon OCR after injecting Medium Error on Metadata of one Drive of R0 WB CCVD
  SCGCQ00455015 - Unblock 4G DDR support for OEM controllers
  SCGCQ00454330 - Capacitance value as 0% for Supercap FBU03 even though capacitor is fully charged
  SCGCQ00451378 - Data corruption on Raid 6 volume while running smash raw io on 63 volume
  SCGCQ00448581 - Coverity Defect Fix
  SCGCQ00442609 - NVCache fails on sCapMaxESRThreshold exceeds after a battery relearn
  SCGCQ00435532 - CC SRAM optimization using overlapped sections in SRAM
  SCGCQ00433463 - Insertion of the boot messages and the evets for montoring the ONFI backup capacity.
  SCGCQ00427452 - Indifference between MR.H and FW implementation for lockKeyLength
  SCGCQ00427326 - Boot block Version is not displayed in CTRL+R
  SCGCQ00421908 - Remove NO_RETENTION flag as it is not used
  SCGCQ00418459 - Assertion failure observed after reconstruction over from R0 to R5
  SCGCQ00408827 - Raise priority of pci config trap interrupt to critical
  SCGCQ00396609 - Remove 4K toggle code to enable 4K support PR in 6.1.
  SCGCQ00558428 - Rebuild and Consistency Check aren't processed when it is executed by CTL+R
  SCGCQ00455583 - Memory battery problem seen while corrupting both the banks at alternative address in 8G Ptolemy.
  SCGCQ00452094 - Small Sequential Reads and Writes are lower than TB
  SCGCQ00450489 - replacePack bit is set to 1, still FW gives the battery(FBU03) status as optimal when apps queries the status
  SCGCQ00446931 - Firmware Version incorrectly displayed
  SCGCQ00446104 - MR: on doing cache offload and restore, the data loss is seen
  SCGCQ00427451 - bootMsgPending.needsEKM bit is not set when FW needs a key
  SCGCQ00423468 - ONFI: Reducing the onfi initialize time from 7sec to 2sec
  SCGCQ00422566 - Foreign config import fails with pinned cache when VD is migrated from one controller to another controller
  SCGCQ00415034 - Watchdog timer excetpion in core 1
  SCGCQ00413263 - Online R6 VD became offline after another R5 VD was removed during IO with a CC2.0 VD
  SCGCQ00412599 - Configuring SBR for operating DDR at 800MHz does not work
  SCGCQ00412591 - Removal of CacheCade VD causes Hang during foreign import reports Command block Data structure issue
  SCGCQ00408922 - Enable watchdog timer
  SCGCQ00396711 - FirmWare hitting Montask with PL fault(0000d115) while trying to create R5 vd on 3drives powersavemode
  SCGCQ00396324 - Defect fix for Montask ../../raid/mem.c at line 280
  SCGCQ00442641 - Defect fix for VD rebuild doesnot kickin and goes to foreign state after reboot
  SCGCQ00435715 - Loss or corruption of meta data information declares nvcache as bad and move from WB to WT
  SCGCQ00417354 - Firmware broke @ 639 in file ../../raid/routines for reading the puctured LBAs due to Reference Tag in PI enabled LDs.
  SCGCQ00415844 - Defect Fix for Montask Observed during cable pull/push
  SCGCQ00414361 - Inverted check for flush completion in L3CacheFlushAll
  SCGCQ00451974 - Unit attention for a FP IO is not handled
  SCGCQ00447956 - Recon progress shows improper estimated time left .
  SCGCQ00436260 - To resolve Failure of skinny compilation
  SCGCQ00415677 - Two different VDs getting same target IDs on MR controller and FW hangs
  SCGCQ00391804 - Firmware crash (MonTask: line 416 in file ../../dm/mpt2/mptrec.c) on reboot after installing ESX4.1U3 on VD
  SCGCQ00390068 - ONFI error hit when 4K sector PDs were used in CacheCade testing.
  SCGCQ00411644 - PD state changes from JBOD to Unconfigured Good across reboots for certain PDs
  SCGCQ00392627 - verification of error cases handling issues
  SCGCQ00434812 - Rebuild starts automatically on drive with foreign config after reboot
  SCGCQ00436221 - For certain OS versions, returning ASCQ=0 for TUR for an offline VD casues the storage stack to keep issuing SSU and TUR commands
  SCGCQ00441021 - Term log capture to include the RAID-Key phase of the boot
  SCGCQ00567340 - Add event in FW to indicate that an INIT operation was halted due to reboot or other failure 
  SCGCQ00394433 - Invader Boot Volumes
  SCGCQ00447612 - Cobra EDFB write performance not scaling to 6400MB/s for IOs > 32k
  SCGCQ00434810 - Enable OCR by default in all pre-GCA builds for OEM 
  SCGCQ00395865 - Transition of defect id   SCGCQ00393644 from MR_FW_SAS3_6.0 to MR_FW_SAS3_6.1
  SCGCQ00413395 - Sequential Read performance is less on CacheCade associated LD's.
  SCGCQ00420689 - BBU Charging gets disabled when Transparent Relearn fails to start due to low capacity
  SCGCQ00420710 - Implementing code review comments
  SCGCQ00420713 - Ability to power off and on individual HDD
  SCGCQ00420732 - Implementing code review comments for code collaborator review #14994
  SCGCQ00420739 - Firmware is sending totalElapsedSecs value as 0 for LD and PD progresses
  SCGCQ00420745 - 5.7 ‘Static Code Analysis Tool’ changes
  SCGCQ00420749 - MonTask: line 281 in file ../../raid/mem.c if running megacli AdpDiag
  SCGCQ00420767 - ‘Static Code Analysis Tool’ warnings 10071, 10100, 10162, 10174, 10288, 10332, 10361, 10363, 10503
  SCGCQ00433405 - Auto Foreign import fails when controller is booted with pinned cache.
  SCGCQ00434144 - Alarm continues to sound after copy-back is done, across reboot, from an unconfigured good drive that is used as an emergency spare.
  SCGCQ00434149 - Change RAID controller FW bad battery warning message that comes up during POST.
  SCGCQ00434151 - Setting the ASO key with storcli 1.02.08 (MegaCli 8.07.06) fails with an error code 3 on Windows or Linux if the MB BIOS PCI
  SCGCQ00434185 - Application could not make a JBOD bootable without a VD present
  SCGCQ00435943 - user is able to associate a DIF enabled VD to Cachecade
  SCGCQ00449870 - static variable used in PD Progress and LD Progress function which may affect multiple progresses running at the same time.
  SCGCQ00549466 - Cache Memory Size of controller Information is ZERO
  SCGCQ00549468 - Controller Reset due to Fatal Error with RAID6/60 configuration
  SCGCQ00550153 - Identifying the DDR, ONFI flash and SCap combination
  SCGCQ00550337 - Baseboard Management Controller (BMC): STP passthru command failure
  SCGCQ00556151 - SLES 11.3 x64 Halts when Loading Kernel During Warm Reboot Stress
  SCGCQ00558049 - MR 4K Validation : 4K VD assigned to 512K CacheCade
  SCGCQ00562722 - MR_6.2 Storlib : SMPpassthru is not happening through storlib.
  SCGCQ00562793 - Unable to create another Virtual Drive when pulling first drive (degrading) in partial Virtual Drive where all drives are configured
  SCGCQ00571048 - Elapsed Seconds displayed in firmware logs for background operations progress is improper
  SCGCQ00384606 - Assertion failure in ../../raid/raidpci.c at line 10011 , while running IO with medium errors on arrays.
  SCGCQ00420692 - The reliability and error recovery of the SuperCap firmware was improved.
  SCGCQ00420747 - ‘Static Code Analysis Tool’ code changes
  SCGCQ00420750 - ‘Static Code Analysis Tool’ Fixes: 10463, 10513, 10591, 10592
  SCGCQ00420760 - Delete VD while PR still in progress cause debugger to loop. Reboot the system, debugger still loops
  SCGCQ00423453 - Adding check to prevent WT->WB property update for SSC VD when enableSSCWB is 0
  SCGCQ00434184 - Skinny firmware does not progress background operations with certain systems when using WebBIOS in legacy mode
  SCGCQ00454467 - Stressing test on degrade raid with UNC drives or rebuilding on UNC drives will cause firmware hang
  SCGCQ00498743 - Don't interpret the cachecade BVD flags if the volume is created with old FW which does not support cachecade.
  SCGCQ00518877 - LSI_MR Controllers fails to set "FACTORY SETTINGS"
  SCGCQ00562792 - Incorrect variable type in MR Read/Modify/Write path
  SCGCQ00394788 - Firmware blocked firmware download to interposer
  SCGCQ00420686 - Firmware returns invalid data in OOB packet
  SCGCQ00420716 - T-bolt firmware : ECC memory error boot message and event log enhancement.
  SCGCQ00420757 - "Question value mismatch with Option Value" message in HII's Controller Management when in Safe Mode with pin cache
  SCGCQ00420764 - Grammatical spacing error in bios message at POST
  SCGCQ00420771 - HII /When user has a critical message and the conrtoller is in Safe Mode, going into CTRL mang will result an error msg
  SCGCQ00433450 - FW halts when you have pinned cahce and remove VD form the configuration.
  SCGCQ00452019 - Virtual drive configurations go missing during firmware upgrade from 5.3 to 5.7
  SCGCQ00454364 - OEM facing with incorrect SAS HDD's indication, MSM shows 2X drives connected
  SCGCQ00458466 - ONFI Coverity defects : 13414,13415,13416,13417,13418,13419,13420,13421,13422
  SCGCQ00558941 - Running out of free entries in task list due to recursive addition of tasks
  SCGCQ00420725 - 4K sector support - iMR, analyze all remaining hard-coded instances of "512"
  SCGCQ00434153 - Disable Band Gap feature for select customers
  SCGCQ00441739 - Allow Type2 DIF drive as JBOD drives
  SCGCQ00450979 - Incase of HW failure move to WT mode and also error case handling of flash tables
  SCGCQ00420724 - Port latency outlier fixes to FW (from legacy PR137246)
  SCGCQ00420753 - Fix code collaborator coding standard related comments for Review #18196.
  SCGCQ00432857 - Saved Release Note DataSLIB returning bad data as good data after host reboots
  SCGCQ00417871 - montask hit at the line "Fatal firmware error: Line 1057 in ../../dm/src/dm.c while running copyback
  SCGCQ00420744 - Provide Fastpath as a standard offering for TB based controllers
  SCGCQ00434156 - OEM- StorCli should not allow turning on JBOD in MR mode
  SCGCQ00436903 - Minimum Capacity needed for relearn is incorrect in 2208 MR FW
 UEFI_Driver 0x06010600
  SCGCQ00478652 - Block IO tests from SCT IHV test suite failed
  SCGCQ00435384 - UEFI System hang if controller FW is in fault state
  SCGCQ00404216 - Add 3008 device ID for iMR product.
  SCGCQ00392836 - LSI to Support Remote Key Management
  SCGCQ00436609 - add PnPID's for 3004 and 3108
  SCGCQ00479016 - Disable Debug print in UEFI Driver
  SCGCQ00484085 - platfrom has UEFI hang when SATA is connected
  SCGCQ00477705 - 9240/9260/9270 UEFI driver issue with platforms when user having 2TB or 4TB VD
  SCGCQ00484113 - Follow UEFI Spec on interpreting In and Out Transfer Length that upper layer sends
 Hii 03.03.10.00
  SCGCQ00415826 - UCM Driver - unable to create an 8PD R5
  SCGCQ00420950 - empty warning prompt is given when creating a CacheCade VD with forced writeback option
  SCGCQ00421615 - BBU information and propererties are not displayed in HII browser 
  SCGCQ00421618 - HII Manage Foreign Configuration menu is not available when a foreign lockeddrive is present in the configuration.
  SCGCQ00423622 - Tool to generate VFR
  SCGCQ00423659 - UCM - Virtual Drive Configuration summary does not report the "Interface Type"
  SCGCQ00431622 - Navigation issue from Enable Drive Security form
  SCGCQ00422725 - HII doesn not allow user to use the remain free capacity to configure additional VD for R50/R10.
  SCGCQ00427518 - HII failed to allow user to use the remains free capacity for R1 VD with 2 plus TB capacity.
  SCGCQ00431231 - Hii enter black screen/timeout when user switching between fields/form sub_form to create R10 VD
  SCGCQ00432915 - Hii failed to report warning that inappropriate drives are picked to config R10 VD.
  SCGCQ00419159 - New Field "package version" in Controller Management
  SCGCQ00441850 - Profile based configuration help issues
  SCGCQ00443864 - When creating an invalid argument in HII during VD creation and after correction, save is grayed out
  SCGCQ00437500 - Hii failed to report error warning when config 2pds R10 with different drive capacity.
  SCGCQ00452128 - HII cannot assign partial space less than 1 GB
  SCGCQ00472196 - Profile based VD creation path incorrectly showing protect VD/secure VD checkbox when user clicks on drive selection criteria
  SCGCQ00452128 - HII cannot assign partial space less than 1 GB
  SCGCQ00477863 - Obtain the Physical Slot number from the PCI Bridge to which the Controller is connected.
  SCGCQ00482099 - Typos in help content for profile VD for Write Policy
 BIOS 6.13.00.1
  SCGCQ00455591 - Memory access issue for OEM when loading Ctrl R
  SCGCQ00559094 - Provide an option to limit the max number of INT 13h devices presented to system BIOS
  SCGCQ00455597 - Memory allocation: Allocate only two 64k
  SCGCQ00504752 - OpROM is displaying incorrect value for the number of INT13h device it supports
  SCGCQ00501253 - OOB function corrupts EBDA area used by other server function
 Ctrl-R 5.01-0005
  SCGCQ00413334 - Ctrl+R- Shows 'Power Save Mode for Configured drives' as 'Enabled' for iMR Fury controller
  SCGCQ00419980 - CtrlR shows option to create VDs even after configuring 16VDs in one DG.
  SCGCQ00436692 - Implemented the old PR LSIP200082262 with this ER in Ctrl-H
  SCGCQ00442610 - Firmware crashed @Line 244 in ../../raid/1078int.c for entering into CTRL-R with Pinned cache in R60 and R6.
  SCGCQ00461680 - ctrlR display "cache offload" as a premium feature at the place of "safe secure" feature.
  SCGCQ00461965 - Unable to silence the alarm
  SCGCQ00468676 - Aligning with FW for strip calculation for 4K drives
  SCGCQ00461544 - Unable to Activate the Premium feature with PFK in Ctrl+R
  SCGCQ00472563 - not able to create r0 WB cachecade VD in ctrl-R
  SCGCQ00497771 - Selecting "Manage Link Speed" in CTL+R causes Fatal Error with SAS 9343-4i
  SCGCQ00497772 - Power savings button not enabled on Ctrl-R
  SCGCQ00558344 - Boot error handling settings are not consistent for HII and CTL-R
  SCGCQ00558359 - Added a shortcut Ctrl+S which saves the changes and refreshes the page.  
  SCGCQ00565105 - Implemented to list all 4 BIOS modes
 FCODE 4.14.05.00
 NVDATA 3.1310.00-0062
  Numerous changes for specific customers
 BootBlock 3.00.00.00-0009
 ROMENV 1.09

----------------------------------------------------------
Initial Release:
Package: 24.0.2-0013 (MR 6.0.1) 
 Firmware 4.200.20-2839
 UEFI_Driver 0x06000500
 Hii 03.02.11.01
 BIOS 6.12.00
 Ctrl-R 5.00-0007
 BootBlock 3.00.00.00-0009
 NVDATA 3.1304.00-0039
 FCODE 4.12.05.00
 ROMENV 1.09

*Third-party trademarks are the property of their respective owners.


