Intel® Quark™ Microcontroller Software Interface 1.4.0 Intel® Quark™ Microcontroller BSP

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
qm_irq_context_t Struct Reference
SoC Registers (Sensor Subsystem) | SoC Registers (SE)

SS IRQ context type. More...

`#include <qm_sensor_regs.h>`

## Data Fields
uint32_t | status32_irq_threshold
| STATUS32 Interrupt Threshold. More...
uint32_t | status32_irq_enable
| STATUS32 Interrupt Enable. More...
uint32_t | irq_ctrl
| Interrupt Context Saving Control Register. More...
uint8_t | irq_config [QM_SS_INT_VECTOR_NUM-QM_SS_EXCEPTION_NUM]
| IRQ configuration: More...
uint32_t | redtbl_entries [QM_IOAPIC_NUM_RTES]
| Redirection Table Entries. More...

## Detailed Description

SS IRQ context type.

IRQ context type.

Applications should not modify the content. This structure is only intended to be used by qm_irq_save_context and qm_irq_restore_context functions.

Definition at line 96 of file qm_sensor_regs.h.

## Field Documentation

uint8_t qm_irq_context_t::irq_config[QM_SS_INT_VECTOR_NUM-QM_SS_EXCEPTION_NUM]

IRQ configuration:

- IRQ Priority:BIT(6):BIT(2)
- IRQ Trigger:BIT(1)
- IRQ Enable:BIT(0)

Definition at line 107 of file qm_sensor_regs.h.

uint32_t qm_irq_context_t::irq_ctrl

Interrupt Context Saving Control Register.

Definition at line 99 of file qm_sensor_regs.h.

uint32_t qm_irq_context_t::redtbl_entries[QM_IOAPIC_NUM_RTES]

Redirection Table Entries.

Definition at line 272 of file qm_soc_regs.h.

uint32_t qm_irq_context_t::status32_irq_enable

STATUS32 Interrupt Enable.

Definition at line 98 of file qm_sensor_regs.h.

uint32_t qm_irq_context_t::status32_irq_threshold

STATUS32 Interrupt Threshold.

Definition at line 97 of file qm_sensor_regs.h.