Intel® Quark™ Microcontroller Software Interface 1.4.0 Intel® Quark™ Microcontroller BSP

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
qm_adc_config_t Struct Reference
Quark D2000 ADC

ADC configuration type. More...

`#include <qm_adc.h>`

## Data Fields
uint8_t | window
| Sample interval in ADC clock cycles, defines the period to wait between the start of each sample and can be in the range [(resolution+2) - 255].
qm_adc_resolution_t | resolution
| 12, 10, 8, 6-bit resolution. More...

## Detailed Description

ADC configuration type.

Definition at line 94 of file qm_adc.h.

## Field Documentation

qm_adc_resolution_t qm_adc_config_t::resolution

12, 10, 8, 6-bit resolution.

Definition at line 101 of file qm_adc.h.

Referenced by qm_adc_set_config().