Intel® Quark™ Microcontroller Software Interface 1.4.0 Intel® Quark™ Microcontroller BSP

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
qm_ss_adc_config_t Struct Reference
SS ADC

SS ADC configuration type. More...

`#include <qm_ss_adc.h>`

## Data Fields
uint8_t | window
| Sample interval in ADC clock cycles, defines the period to wait between the start of each sample and can be in the range [(resolution+2) - 255].
qm_ss_adc_resolution_t | resolution
| 12, 10, 8, 6-bit resolution. More...

## Detailed Description

SS ADC configuration type.

Definition at line 98 of file qm_ss_adc.h.

## Field Documentation

qm_ss_adc_resolution_t qm_ss_adc_config_t::resolution

12, 10, 8, 6-bit resolution.

Definition at line 105 of file qm_ss_adc.h.

Referenced by qm_ss_adc_set_config().