Intel® Quark™ Microcontroller Software Interface 1.4.0 Intel® Quark™ Microcontroller BSP

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
qm_mbox_msg_t Struct Reference
Mailbox

Definition of the mailbox message. More...

`#include <qm_mailbox.h>`

## Data Fields
uint32_t | ctrl
| Control word - bits 30 to 0 used as data/message id, bit 31 triggers channel interrupt when set by the driver.
uint32_t | data [QM_MBOX_PAYLOAD_NUM]
| Mailbox data buffer. More...

## Detailed Description

Definition of the mailbox message.

Definition at line 64 of file qm_mailbox.h.

## Field Documentation

uint32_t qm_mbox_msg_t::data[QM_MBOX_PAYLOAD_NUM]

Mailbox data buffer.

Definition at line 70 of file qm_mailbox.h.

Referenced by qm_mbox_ch_read(), and qm_mbox_ch_write().