Intel® Quark™ Microcontroller Software Interface 1.4.0 Intel® Quark™ Microcontroller BSP

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

- All
- Variables

- a
- b
- c
- d
- e
- f
- g
- h
- i
- k
- l
- m
- n
- o
- p
- r
- s
- t
- u
- v
- w

Here is a list of all documented struct and union fields with links to the struct/union documentation for each field:

### - a -

- adc_0_cal_int_mask : qm_interrupt_router_reg_t
- adc_0_pwr_int_mask : qm_interrupt_router_reg_t
- adc_calibration : qm_adc_reg_t
- adc_cmd : qm_adc_reg_t
- adc_ctrl : qm_ss_adc_context_t
- adc_divseqstat : qm_ss_adc_context_t
- adc_fifo_count : qm_adc_reg_t
- adc_intr_enable : qm_adc_reg_t
- adc_intr_status : qm_adc_reg_t
- adc_op_mode : qm_adc_reg_t
- adc_sample : qm_adc_reg_t
- adc_seq : qm_ss_adc_context_t
- adc_seq0 : qm_adc_reg_t
- adc_seq1 : qm_adc_reg_t
- adc_seq2 : qm_adc_reg_t
- adc_seq3 : qm_adc_reg_t
- adc_seq4 : qm_adc_reg_t
- adc_seq5 : qm_adc_reg_t
- adc_seq6 : qm_adc_reg_t
- adc_seq7 : qm_adc_reg_t
- adc_set : qm_ss_adc_context_t
- address_mode : qm_i2c_config_t , qm_ss_i2c_config_t
- aempty_thresh : qm_i2s_channel_cfg_data_t
- afull_thresh : qm_i2s_channel_cfg_data_t
- agent_read_en_mask : qm_mpr_config_t
- agent_write_en_mask : qm_mpr_config_t
- alarm_en : qm_rtc_config_t
- alarm_val : qm_rtc_config_t
- allow_agents : qm_fpr_config_t
- aon_gpio_0_int_mask : qm_interrupt_router_reg_t
- aon_vr : qm_scss_pmu_reg_t
- aonc_cfg : qm_aonc_reg_t
- aonc_cnt : qm_aonc_reg_t
- aonpt_0_int_mask : qm_interrupt_router_reg_t
- aonpt_cfg : qm_aonc_reg_t
- aonpt_cnt : qm_aonc_reg_t
- aonpt_ctrl : qm_aonc_reg_t
- aonpt_stat : qm_aonc_reg_t
- apr : qm_lapic_reg_t
- audio_buff_cfg : qm_i2s_channel_cfg_data_t
- audio_format : qm_i2s_channel_cfg_data_t
- audio_rate : qm_i2s_channel_cfg_data_t
- audio_stream : qm_i2s_channel_cfg_data_t