Intel® Quark™ Microcontroller Software Interface 1.4.0 Intel® Quark™ Microcontroller BSP

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
qm_flash_config_t Struct Reference
Flash

Flash configuration structure. More...

`#include <qm_flash.h>`

## Data Fields
uint8_t | wait_states
| Read wait state. More...
uint8_t | us_count
| Number of clocks in a microsecond. More...
qm_flash_disable_t | write_disable
| Write Disable. More...

## Detailed Description

Flash configuration structure.

Definition at line 41 of file qm_flash.h.

## Field Documentation

uint8_t qm_flash_config_t::us_count

Number of clocks in a microsecond.

Needed for program/erase operations.

Definition at line 48 of file qm_flash.h.

Referenced by qm_flash_set_config().

uint8_t qm_flash_config_t::wait_states

Read wait state.

Definition at line 42 of file qm_flash.h.

Referenced by qm_flash_set_config().

qm_flash_disable_t qm_flash_config_t::write_disable

Write Disable.

When this is set, only a reset will enable writes to Flash again.

Definition at line 55 of file qm_flash.h.

Referenced by qm_flash_set_config().