Intel® Quark™ Microcontroller Software Interface 1.4.0 Intel® Quark™ Microcontroller BSP

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
qm_pwm_reg_t Struct Reference
SoC Registers (D2000) | SoC Registers (SE)

PWM / Timer register map. More...

`#include <qm_soc_regs.h>`

## Data Fields
qm_pwm_channel_t | timer [QM_PWM_ID_NUM]
| 2 Timers. More...
QM_RW uint32_t | timersintstatus
| Timers Interrupt Status.
QM_RW uint32_t | timerseoi
| Timers End Of Interrupt.
QM_RW uint32_t | timersrawintstatus
| Timers Raw Interrupt Status.
QM_RW uint32_t | timerscompversion
| Timers Component Version.
QM_RW uint32_t | timer_loadcount2 [QM_PWM_ID_NUM]
| Timer Load Count 2.

## Detailed Description

PWM / Timer register map.

Definition at line 398 of file qm_soc_regs.h.

## Field Documentation

qm_pwm_channel_t qm_pwm_reg_t::timer

2 Timers.

4 Timers

Definition at line 399 of file qm_soc_regs.h.

Referenced by QM_ISR_DECLARE(), qm_pwm_get(), qm_pwm_restore_context(), qm_pwm_save_context(), qm_pwm_set(), qm_pwm_set_config(), qm_pwm_start(), and qm_pwm_stop().