Intel® Quark™ Microcontroller Software Interface 1.4.0 Intel® Quark™ Microcontroller BSP

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
qm_spi_context_t Struct Reference
SoC Registers (SE)

SPI context type. More...

`#include <qm_soc_regs.h>`

## Data Fields
uint32_t | ctrlr0
| Control Register 0. More...
uint32_t | ser
| Slave Enable Register. More...
uint32_t | baudr
| Baud Rate Select. More...

## Detailed Description

SPI context type.

Applications should not modify the content. This structure is only intended to be used by the qm_spi_save_context and qm_spi_restore_context functions.

Definition at line 1071 of file qm_soc_regs.h.

## Field Documentation

uint32_t qm_spi_context_t::baudr

Baud Rate Select.

Definition at line 1074 of file qm_soc_regs.h.

Referenced by qm_spi_restore_context(), and qm_spi_save_context().

uint32_t qm_spi_context_t::ctrlr0

Control Register 0.

Definition at line 1072 of file qm_soc_regs.h.

Referenced by qm_spi_restore_context(), and qm_spi_save_context().

uint32_t qm_spi_context_t::ser

Slave Enable Register.

Definition at line 1073 of file qm_soc_regs.h.

Referenced by qm_spi_restore_context(), and qm_spi_save_context().