================================================================================
Intel(R) Server Board S2600CW Family
Firmware Update Package for Intel(R) One Boot Flash Update Utility and
Windows* Preboot Execution Environment 
================================================================================
Intel(R) Server Boards and Systems
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA
================================================================================
DATE    :	Jan 28 2016
TO      :	Intel(R) Server Board S2600CW Family
SUBJECT : 	Release Notes for System Firmware Update Package 
================================================================================
                              ABOUT THIS RELEASE
================================================================================
BIOS   : 01.01.0015
ME     : 03.01.03.021
BMC    : 01.41.9579
FRUSDR : 1.13
================================================================================
                           Support Platforms and Dependency
================================================================================
Processors supported:
    Intel(R) Xeon(R) processor E5-2600 v3 series Processor
    Intel(R) Xeon(R) processor E5-2600 v4 series Processor
	
Microcode update versions:
CPUID     Version      Status
0x306f2   0x00000036   Production (E5-2600 v3 C0/C1)
0x406f1   0x0b000010   External   (E5-2600 v4 B0)  

The following update process must be followed to ensure a trouble free update.
1.	Manageability Engine (ME) firmware
2.	BIOS
3.	BMC firmware
4.	FRUSDR 

=============================================================================
                		 WARNING!!!                  
================================================================================
At the end of the update process when running the iflashupdt tool you may see the error "Cannot determine Chassis Type from HSBP FRU Info" and/or "SDR auto-update failed"
 
Workaround: This issue is resolved by running again the SDR update.

================================================================================
                  System Firmware Update Package Usage instructions                   
================================================================================
This package can be updated using one of the following methods:
 - Windows* or Linux* operating system using Intel(R) One-boot Flash Update (OFU)
   V11.0 Build 14 or later)
 - Windows* Preboot Execution Environment (WinPE)

To update from Windows* and Linux* or operating systems using the Intel(R) One Boot
Flash Update Utility (OFU)

Intel(R) One boot Flash Update utility can be downloaded from http://downloadcenter.intel.com/
and it is part of the "BIOS, Firmware Update & Configuration Utilities" for 
Windows* and Linux*. Please refer to Intel OFU user guide about the details of 
installation and usage of OFU.

Use OFU to update system firmware by the following steps:
- Install OFU on Windows* or Linux* system
- Download the latest firmware update package from http://downloadcenter.intel.com/
- Unzip package to a folder
- Run the following command in Windows* command line/Linux* terminal window:
  <OFU install folder name>:\flashupdt -u  <package folder name>\flashupdt.cfg
                       
To update from Windows* Preboot Execution Environment (WinPE)

The System Firmware Update Package can be inserted to Windows* PE customized image 
for creating a bootable Windows* PE CD. User is able to update system firmware from 
customized WinPE CD by the following steps:
- Boot server with customized WinPE CD
- Run script "WinPE21_x64_Update.bat" or "WinPE20_x86_Update.bat" 
  (name may be varied depends on your own customization)
  
Note:
1. The Intel(R) OFU utility is case sensitive. Therefore, when you transfer the 
Firmware Update Package using USB flash drive from a Microsoft Windows* system to a Linux
environment, you must first extract under the Linux* environment. Otherwise, you 
will need to mount the USB flash drive manually with 'vfat' option under Linux to avoid 
conversion from upper case to lower case and vice versa.

2. To make Intel(R) OFU utility run properly under x86 or x64 OS, you have to read
OFU release notes on known issues for OFU installation.

3. In this SFUP package, Intel only provide batch file "WinPE_x86_Update.bat"
for WinPE2.0 32 bit solution "WinPE_x64_Update.bat" for WinPE2.1/3.0 64 bit 
solution as an example. Please refer to white paper "White Paper-Intel Server 
Utilities Procedure for WinPE.pdf" for details on building your own customized 
WinPE CD.

4. Windows PE 2.0 - built from Windows Vista SP1 32bit or EM64T
5. Windows PE 2.1 - built from Windows Vista SP1 or Windows Server 2008, EM64T
6. Windows PE 3.1 - built from Windows Server 2008R2, EM64T
7. Microsoft IPMI driver is loaded by default from WinPE CD, if you want to use 
Intel IPMI driver instead of MS IPMI driver for firmware update, you can un-install
Microsoft IPMI driver by:
                Devicesetup.exe ¨Cv remove *IPI0001
                Note: IPI0001 is the device ID for Microsoft IPMI driver.

================================================================================
				BIOS R01.01.0015
================================================================================
Broadwell CPU full feature support

================================================================================
			KNOWN ISSUES in ME 03.01.03.021 release
================================================================================
Unexpected SmaRT&CLST events may be observed after removing 1 of 2 PSUs.

		 
================================================================================
                       KNOWN ISSUES in BMC 01.41.9579
===============================================================================
- This BMC FW update package is to be used only on PCSD server baseboards and
  does NOT support customer reference boards (CRB) or silicon reference
  platforms (SRP).
  Contact your Intel Representatives to determine where to download the BMC FW
  for these products.

- The BMC FW image file in this package is to be used only with the provided
  FWPIAUPD update utility.
  Using the FW image file with a SPI flash device programmer will result in a
  non-functional system.  

- Some open source ipmi utilities may automatically retry multiple times during  
  access BMC using bad password and supporting IPMI specification 1.5 in Linux OS.
  CCB310 will log more bad password login SEL.

================================================================================
                      FRUSDR Changes in release 1.13
================================================================================    
Issue Fixed:
- None.
Features added:
- None


=============================================================================
                            LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products. 
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation may 
have patents or pending patent applications, trademarks, copyrights, or other 
intellectual property rights that relate to the presented subject matter.  
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any 
such patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product 
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 
*Other names and brands are the property of their respective owners.
Copyright (c) 2016 Intel Corporation.

A portion of this firmware is open source code, which falls under the
GPL 2.0 license.  

[END OF RELEASE NOTES]
