Release Note for Nuvoton SIO CIR Device Driver
2015.05.28

Supported Windows: WinXP (32/x64), Vista (32/x64), Win7 (32/x64), Win8/8.1 (32/x64), Win10(32/x64)

CIR driver versions
--------------------
Win10   (2.4.2013.711)  - CIR port driver / WHLK-certified
Win8    (2.4.2013.711)  - CIR port driver / WHQL-certified
Win7    (2.4.2013.711)  - CIR port driver / WHQL-certified
Vista   (1.8.2009.514)  - CIR port driver / WHQL-certified
WinXP   (1.0.2010.505)  - HID minidriver  / WHQL-certified
 
Revision History
-------------------------------------------------------------------------------
2.11.1009 / 2015.05.28	
        1. Added Windows 10 driver.

2.10.1008 / 2015.03.10
        1. Fixed that Win7 driver cannot be upgraded to Win10 system(Preview 9926).

2.9.1007 / 2013.07.16
        1. Fixed that Win8 driver cannot be installed on Win8.1 system.

2.7.1005 / 2012.08.01
        1. Remove all the driver packages for the Nuvoton SIO CIR device from 
           the system when the setup program is executed to uninstall the CIR 
           driver.
        
2.6.1004 / 2012.07.30
        1. Fix the installation package that fails to update the CIR device 
           driver if there's a driver already installed by the previous version
           of the installation package.
        
2.5.1003 / 2012.07.19
        1. Added Win8 driver.
        
2.4.1002 / 2012.07.06
        1. Fix the Win7 driver to abnormally prevent the system from going to 
           sleeping state again once the system resumes from sleeping state due 
           to the wake event from Intel ISCT mechanism.
           
2.3.1001 / 2012.05.11
        1. Removed the request to restart the computer in "InstallShield Wizard 
           Complete" dialog window at the end of installation.
        
2.3.1000 / 2012.04.27 
        1. Fixed to install Win7 driver in Win8 system instead of Vista driver.
        2. Fixed for failed uninstallation of the device driver under Win8.                       