; BHTPCR.INF, O2Micro/BHT Integrated MMC/SD Controller INF file
; Copyright (c) 1997-2016 O2Micro/BHT Corp.

[Version]
Signature   = "$Windows NT$"
Class       = SCSIAdapter
ClassGuid   = {4D36E97B-E325-11CE-BFC1-08002BE10318}
Provider    = %BayHubTech%
DriverVer = 03/07/2016,1.1.1.1008
Catalogfile = bhtpcrdr.cat

[SourceDisksNames]
1 = %BHTPCRDR.DriverDisk%

[SourceDisksFiles]
bhtpcrdr.sys = 1
bhtv5Icon.dll = 1
SDPA8220.dll = 1

[DestinationDirs]
DefaultDestDir = 12
Copybhtv5Icon = 11
Copybhtv5Icon_WoW64 = 10, sysWoW64
CopySDPA8220 = 11, SDA
CopySDPA8220_WoW64 = 10, sysWoW64\SDA

[ControlFlags]
ExcludeFromSelect = *

[Manufacturer]
%BayHubTech% = BHTPCRDR,NTamd64,NTx86


[BHTPCRDR.NTx86]
%BHTPCRDR.DeviceDesc% = DriverInstallx86, PCI\VEN_1217&DEV_8520		;Default for Fujin2
%BHTPCRDR.DeviceDesc% = DriverInstallx86, PCI\VEN_1217&DEV_8420		;Default for SDS0
%BHTPCRDR.DeviceDesc% = DriverInstallx86, PCI\VEN_1217&DEV_8421		;Default for SDS1
%BHTPCRDR.DeviceDesc% = DriverInstallx86, PCI\VEN_1217&DEV_8620		;Default for Seabird
%BHTPCRDR.DeviceDesc% = DriverInstallx86, PCI\VEN_1217&DEV_8621		;Default for Seabird
%BHTPCRDR.DeviceDesc% = DriverInstallx86, PCI\VEN_1217&DEV_8720		;Default for SeaEagle2
%BHTPCRDR.DeviceDesc% = DriverInstallx86, PCI\VEN_1217&DEV_8721		;Default for SeaEagle2
%BHTPCRDR.DeviceDesc% = DriverInstallx86, PCI\VEN_1217&DEV_8722		;Default for SeaEagle2
%BHTPCRDR.DeviceDesc% = DriverInstallx86, PCI\VEN_1217&DEV_8723		;Default for SeaEagle2


%BHTPCRDR.DeviceDesc% = DriverInstallx86_221117aa, PCI\VEN_1217&DEV_8520&SUBSYS_221117aa ;idx 1
%BHTPCRDR.DeviceDesc% = DriverInstallx86_504117aa, PCI\VEN_1217&DEV_8620&SUBSYS_504117aa ;idx 2,3
%BHTPCRDR.DeviceDesc% = DriverInstallx86_504c17aa, PCI\VEN_1217&DEV_8520&SUBSYS_504c17aa ;idx 4
%BHTPCRDR.DeviceDesc% = DriverInstallx86_222c17aa, PCI\VEN_1217&DEV_8621&SUBSYS_222c17aa ;idx 5
%BHTPCRDR.DeviceDesc% = DriverInstallx86_380017aa, PCI\VEN_1217&DEV_8620&SUBSYS_380017aa ;idx 6
%BHTPCRDR.DeviceDesc% = DriverInstallx86_380117aa, PCI\VEN_1217&DEV_8620&SUBSYS_380117aa ;idx 7
%BHTPCRDR.DeviceDesc% = DriverInstallx86_380017aa_8621, PCI\VEN_1217&DEV_8621&SUBSYS_380017aa ;idx 8
%BHTPCRDR.DeviceDesc% = DriverInstallx86_390317aa, PCI\VEN_1217&DEV_8621&SUBSYS_390317aa ;idx 9
%BHTPCRDR.DeviceDesc% = DriverInstallx86_390217aa, PCI\VEN_1217&DEV_8621&SUBSYS_390217aa   ;idx 10
%BHTPCRDR.DeviceDesc% = DriverInstallx86_06EF1028, PCI\VEN_1217&DEV_8520&SUBSYS_06EF1028 ;idx 13
%BHTPCRDR.DeviceDesc% = DriverInstallx86_380017aa_8520, PCI\VEN_1217&DEV_8520&SUBSYS_380017aa ;idx 14
%BHTPCRDR.DeviceDesc% = DriverInstallx86_b28219da, PCI\VEN_1217&DEV_8520&SUBSYS_b28219da ;idx 15
%BHTPCRDR.DeviceDesc% = DriverInstallx86_10521025, PCI\VEN_1217&DEV_8621&SUBSYS_10521025 ;idx 16
%BHTPCRDR.DeviceDesc% = DriverInstallx86_10631025, PCI\VEN_1217&DEV_8621&SUBSYS_10631025 ;idx 17
%BHTPCRDR.DeviceDesc% = DriverInstallx86_000417aa, PCI\VEN_1217&DEV_8620&SUBSYS_000417aa ;idx 18
%BHTPCRDR.DeviceDesc% = DriverInstallx86_505b17aa, PCI\VEN_1217&DEV_8621&SUBSYS_505b17aa ;idx 19
%BHTPCRDR.DeviceDesc% = DriverInstallx86_511817aa, PCI\VEN_1217&DEV_8621&SUBSYS_511817aa ;idx 20
%BHTPCRDR.DeviceDesc% = DriverInstallx86_505c17aa, PCI\VEN_1217&DEV_8621&SUBSYS_505c17aa ;idx 21
%BHTPCRDR.DeviceDesc% = DriverInstallx86_609517aa, PCI\VEN_1217&DEV_8520&SUBSYS_609517aa ;idx 22
%BHTPCRDR.DeviceDesc% = DriverInstallx86_607E17aa, PCI\VEN_1217&DEV_8520&SUBSYS_607E17aa ;idx 23
%BHTPCRDR.DeviceDesc% = DriverInstallx86_369417aa, PCI\VEN_1217&DEV_8520&SUBSYS_369417aa ;idx 24
%BHTPCRDR.DeviceDesc% = DriverInstallx86_505417aa, PCI\VEN_1217&DEV_8520&SUBSYS_505417aa ;idx 25
%BHTPCRDR.DeviceDesc% = DriverInstallx86_380317aa, PCI\VEN_1217&DEV_8620&SUBSYS_380317aa ;idx 26
%BHTPCRDR.DeviceDesc% = DriverInstallx86_20648086, PCI\VEN_1217&DEV_8621&SUBSYS_20648086 ;idx 27

[BHTPCRDR.NTamd64]
%BHTPCRDR.DeviceDesc% = DriverInstallx64, PCI\VEN_1217&DEV_8520		;Default for Fujin2
%BHTPCRDR.DeviceDesc% = DriverInstallx86, PCI\VEN_1217&DEV_8420		;Default for SDS0
%BHTPCRDR.DeviceDesc% = DriverInstallx86, PCI\VEN_1217&DEV_8421		;Default for SDS1
%BHTPCRDR.DeviceDesc% = DriverInstallx64, PCI\VEN_1217&DEV_8620		;Default for Seabird
%BHTPCRDR.DeviceDesc% = DriverInstallx64, PCI\VEN_1217&DEV_8621		;Default for Seabird
%BHTPCRDR.DeviceDesc% = DriverInstallx64, PCI\VEN_1217&DEV_8720		;Default for SeaEagle2
%BHTPCRDR.DeviceDesc% = DriverInstallx64, PCI\VEN_1217&DEV_8721		;Default for SeaEagle2
%BHTPCRDR.DeviceDesc% = DriverInstallx64, PCI\VEN_1217&DEV_8722		;Default for SeaEagle2
%BHTPCRDR.DeviceDesc% = DriverInstallx64, PCI\VEN_1217&DEV_8723		;Default for SeaEagle2


%BHTPCRDR.DeviceDesc% = DriverInstallx64_221117aa, PCI\VEN_1217&DEV_8520&SUBSYS_221117aa ;idx 1
%BHTPCRDR.DeviceDesc% = DriverInstallx64_504117aa, PCI\VEN_1217&DEV_8620&SUBSYS_504117aa ;idx 2,3
%BHTPCRDR.DeviceDesc% = DriverInstallx64_504c17aa, PCI\VEN_1217&DEV_8520&SUBSYS_504c17aa ;idx 4
%BHTPCRDR.DeviceDesc% = DriverInstallx64_222c17aa, PCI\VEN_1217&DEV_8621&SUBSYS_222c17aa ;idx 5
%BHTPCRDR.DeviceDesc% = DriverInstallx64_380017aa, PCI\VEN_1217&DEV_8620&SUBSYS_380017aa ;idx 6
%BHTPCRDR.DeviceDesc% = DriverInstallx64_380117aa, PCI\VEN_1217&DEV_8620&SUBSYS_380117aa ;idx 7
%BHTPCRDR.DeviceDesc% = DriverInstallx64_380017aa_8621, PCI\VEN_1217&DEV_8621&SUBSYS_380017aa ;idx 8
%BHTPCRDR.DeviceDesc% = DriverInstallx64_390317aa, PCI\VEN_1217&DEV_8621&SUBSYS_390317aa ;idx 9
%BHTPCRDR.DeviceDesc% = DriverInstallx64_390217aa, PCI\VEN_1217&DEV_8621&SUBSYS_390217aa   ;idx 10
%BHTPCRDR.DeviceDesc% = DriverInstallx64_06EF1028, PCI\VEN_1217&DEV_8520&SUBSYS_06EF1028 ;idx 13
%BHTPCRDR.DeviceDesc% = DriverInstallx64_380017aa_8520, PCI\VEN_1217&DEV_8520&SUBSYS_380017aa ;idx 14
%BHTPCRDR.DeviceDesc% = DriverInstallx64_b28219da, PCI\VEN_1217&DEV_8520&SUBSYS_b28219da ;idx 15
%BHTPCRDR.DeviceDesc% = DriverInstallx64_10521025, PCI\VEN_1217&DEV_8621&SUBSYS_10521025 ;idx 16
%BHTPCRDR.DeviceDesc% = DriverInstallx64_10631025, PCI\VEN_1217&DEV_8621&SUBSYS_10631025 ;idx 17
%BHTPCRDR.DeviceDesc% = DriverInstallx64_000417aa, PCI\VEN_1217&DEV_8620&SUBSYS_000417aa ;idx 18
%BHTPCRDR.DeviceDesc% = DriverInstallx64_505b17aa, PCI\VEN_1217&DEV_8621&SUBSYS_505b17aa ;idx 19
%BHTPCRDR.DeviceDesc% = DriverInstallx64_511817aa, PCI\VEN_1217&DEV_8621&SUBSYS_511817aa ;idx 20
%BHTPCRDR.DeviceDesc% = DriverInstallx64_505c17aa, PCI\VEN_1217&DEV_8621&SUBSYS_505c17aa ;idx 21
%BHTPCRDR.DeviceDesc% = DriverInstallx64_609517aa, PCI\VEN_1217&DEV_8520&SUBSYS_609517aa ;idx 22
%BHTPCRDR.DeviceDesc% = DriverInstallx64_607E17aa, PCI\VEN_1217&DEV_8520&SUBSYS_607E17aa ;idx 23
%BHTPCRDR.DeviceDesc% = DriverInstallx64_369417aa, PCI\VEN_1217&DEV_8520&SUBSYS_369417aa ;idx 24
%BHTPCRDR.DeviceDesc% = DriverInstallx64_505417aa, PCI\VEN_1217&DEV_8520&SUBSYS_505417aa ;idx 25
%BHTPCRDR.DeviceDesc% = DriverInstallx64_380317aa, PCI\VEN_1217&DEV_8620&SUBSYS_380317aa ;idx 26
%BHTPCRDR.DeviceDesc% = DriverInstallx64_20648086, PCI\VEN_1217&DEV_8621&SUBSYS_20648086 ;idx 27

[DriverInstallx86.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86;, EventLogService

[DriverInstallx64.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64;, EventLogService

[DriverServicex64]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = default_cfg_se
AddReg         = default_cfg_sb
AddReg         = default_cfg_fj2
AddReg         = autorun_addreg

[DriverServicex86]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = default_cfg_se
AddReg         = default_cfg_sb
AddReg         = default_cfg_fj2
AddReg         = autorun_addreg

;cfg idx 1 
[DriverInstallx86_221117aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_221117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_221117aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_221117aa;, EventLogService

[DriverServicex86_221117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 221117aa_cfg
AddReg         = autorun_addreg

[DriverInstallx64_221117aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_221117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_221117aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_221117aa;, EventLogService

[DriverServicex64_221117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 221117aa_cfg
AddReg         = autorun_addreg

[221117aa_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seaeagle\pcr", "000_p0x300", 0x00010001, 0x00ff0044
HKR,"seaeagle\pcr", "001_p0x3e0", 0x00010001, 0x00400000
HKR,"seaeagle", "output_tuning", 0x00010001, 0x8001000a



;cfg idx 2,3
[DriverInstallx86_504117aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_504117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_504117aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_504117aa;, EventLogService

[DriverServicex86_504117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 504117aa_cfg
AddReg         = autorun_addreg

[DriverInstallx64_504117aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_504117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_504117aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_504117aa;, EventLogService

[DriverServicex64_504117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 504117aa_cfg
AddReg         = autorun_addreg

[504117aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird\pcr", "000_p0xe2", 0x00010001, 0xf0003000
HKR,"seabird\pcr", "001_p0xfe", 0x00010001, 0x000f0008
HKR,"seabird\pcr", "000_p0x300", 0x00010001, 0x00ff0055
HKR,"seabird\pcr", "001_p0x304", 0x00010001, 0x007e0048

;cfg idx 4 
[DriverInstallx86_504c17aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_504c17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_504c17aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_504c17aa;, EventLogService

[DriverServicex86_504c17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 504c17aa_cfg
AddReg         = autorun_addreg

[DriverInstallx64_504c17aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_504c17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_504c17aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_504c17aa;, EventLogService

[DriverServicex64_504c17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 504c17aa_cfg
AddReg         = autorun_addreg

[504c17aa_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seaeagle\pcr", "000_p0xe2", 0x00010001, 0xf0003000
HKR,"seaeagle\pcr", "001_p0xfe", 0x00010001, 0x000f0008
HKR,"seaeagle\pcr", "000_p0x300", 0x00010001, 0x00ff0055
HKR,"seaeagle\pcr", "001_p0x304", 0x00010001, 0x007e0048

;cfg idx 5 
[DriverInstallx86_222c17aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_222c17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_222c17aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_222c17aa;, EventLogService

[DriverServicex86_222c17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 222c17aa_cfg
AddReg         = autorun_addreg

[DriverInstallx64_222c17aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_222c17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_222c17aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_222c17aa;, EventLogService

[DriverServicex64_222c17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 222c17aa_cfg
AddReg         = autorun_addreg

[222c17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird\pcr", "000_p0xe2", 0x00010001, 0xf0003000
HKR,"seabird\pcr", "001_p0xfe", 0x00010001, 0x000f0008
HKR,"seabird\pcr", "000_p0x300", 0x00010001, 0x00ff0055
HKR,"seabird\pcr", "001_p0x304", 0x00010001, 0x007e0048
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

;cfg idx 6 
[DriverInstallx86_380017aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_380017aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_380017aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_380017aa;, EventLogService

[DriverServicex86_380017aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 380017aa_cfg
AddReg         = autorun_addreg

[DriverInstallx64_380017aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_380017aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_380017aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_380017aa;, EventLogService

[DriverServicex64_380017aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 380017aa_cfg
AddReg         = autorun_addreg

[380017aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird\pcr", "000_p0xe2", 0x00010001, 0xf0003000
HKR,"seabird\pcr", "001_p0xfe", 0x00010001, 0x000f0008
HKR,"seabird\pcr", "000_p0x300", 0x00010001, 0x00ff0055
HKR,"seabird\pcr", "001_p0x304", 0x00010001, 0x007e0048

;cfg idx 7 
[DriverInstallx86_380117aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_380117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_380117aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_380117aa;, EventLogService

[DriverServicex86_380117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 380117aa_cfg
AddReg         = autorun_addreg

[DriverInstallx64_380117aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_380117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_380117aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_380117aa;, EventLogService

[DriverServicex64_380117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 380117aa_cfg
AddReg         = autorun_addreg

[380117aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird\pcr", "000_p0xe2", 0x00010001, 0xf0003000
HKR,"seabird\pcr", "001_p0xfe", 0x00010001, 0x000f0008
HKR,"seabird\pcr", "000_p0x300", 0x00010001, 0x00ff0055
HKR,"seabird\pcr", "001_p0x304", 0x00010001, 0x007e0048

;cfg idx 8
[DriverInstallx86_380017aa_8621.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_380017aa_8621.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_380017aa_8621.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_380017aa_8621;, EventLogService

[DriverServicex86_380017aa_8621]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 380017aa_8621_cfg
AddReg         = autorun_addreg

[DriverInstallx64_380017aa_8621.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_380017aa_8621.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_380017aa_8621.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_380017aa_8621;, EventLogService

[DriverServicex64_380017aa_8621]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 380017aa_8621_cfg
AddReg         = autorun_addreg

[380017aa_8621_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird\pcr", "000_p0xe2", 0x00010001, 0xf0003000
HKR,"seabird\pcr", "001_p0xfe", 0x00010001, 0x000f0008
HKR,"seabird\pcr", "000_p0x300", 0x00010001, 0x00ff0055
HKR,"seabird\pcr", "001_p0x304", 0x00010001, 0x007e0048
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

;cfg idx 9
[DriverInstallx86_390317aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_390317aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_390317aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_390317aa;, EventLogService

[DriverServicex86_390317aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 390317aa_cfg
AddReg         = autorun_addreg

[DriverInstallx64_390317aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_390317aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_390317aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_390317aa;, EventLogService

[DriverServicex64_390317aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 390317aa_cfg
AddReg         = autorun_addreg

[390317aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird\pcr", "000_p0xe2", 0x00010001, 0xf0003000
HKR,"seabird\pcr", "001_p0xfe", 0x00010001, 0x000f0008
HKR,"seabird\pcr", "000_p0x300", 0x00010001, 0x00ff0055
HKR,"seabird\pcr", "001_p0x304", 0x00010001, 0x007e0048
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

;cfg idx 10
[DriverInstallx86_390217aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_390217aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_390217aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_390217aa;, EventLogService

[DriverServicex86_390217aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 390217aa_cfg
AddReg         = autorun_addreg

[DriverInstallx64_390217aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_390217aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_390217aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_390217aa;, EventLogService

[DriverServicex64_390217aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 390217aa_cfg
AddReg         = autorun_addreg

[390217aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird\pcr", "000_p0xe2", 0x00010001, 0xf0003000
HKR,"seabird\pcr", "001_p0xfe", 0x00010001, 0x000f0008
HKR,"seabird\pcr", "000_p0x300", 0x00010001, 0x00ff0055
HKR,"seabird\pcr", "001_p0x304", 0x00010001, 0x007e0048

;cfg idx 13
[DriverInstallx86_06EF1028.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_06EF1028.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_06EF1028.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_06EF1028;, EventLogService

[DriverServicex86_06EF1028]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 06EF1028_cfg
AddReg         = autorun_addreg

[DriverInstallx64_06EF1028.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_06EF1028.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_06EF1028.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_06EF1028;, EventLogService

[DriverServicex64_06EF1028]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 06EF1028_cfg
AddReg         = autorun_addreg

[06EF1028_cfg]
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "output_tuning", 0x00010001, 0x80010000

;cfg idx 14
[DriverInstallx86_380017aa_8520.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_380017aa_8520.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_380017aa_8520.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_380017aa_8520;, EventLogService

[DriverServicex86_380017aa_8520]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 380017aa_8520_cfg
AddReg         = autorun_addreg

[DriverInstallx64_380017aa_8520.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_380017aa_8520.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_380017aa_8520.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_380017aa_8520;, EventLogService

[DriverServicex64_380017aa_8520]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 380017aa_8520_cfg
AddReg         = autorun_addreg

[380017aa_8520_cfg]
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "MS_SDIO_CTRL", 0x00010001, 0x0

;cfg idx 15
[DriverInstallx86_b28219da.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_b28219da.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_b28219da.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_b28219da;, EventLogService

[DriverServicex86_b28219da]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = b28219da_cfg
AddReg         = autorun_addreg

[DriverInstallx64_b28219da.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_b28219da.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_b28219da.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_b28219da;, EventLogService

[DriverServicex64_b28219da]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = b28219da_cfg
AddReg         = autorun_addreg

[b28219da_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seaeagle\pcr", "000_p0x300", 0x00010001, 0x00ff0044
HKR,"seaeagle\pcr", "001_p0x3e0", 0x00010001, 0x00400000

;cfg idx 16
[DriverInstallx86_10521025.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_10521025.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_10521025.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_10521025;, EventLogService

[DriverServicex86_10521025]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 10521025_cfg
AddReg         = autorun_addreg

[DriverInstallx64_10521025.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_10521025.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_10521025.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_10521025;, EventLogService

[DriverServicex64_10521025]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 10521025_cfg
AddReg         = autorun_addreg

[10521025_cfg]
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

;cfg idx 17
[DriverInstallx86_10631025.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_10631025.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_10631025.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_10631025;, EventLogService

[DriverServicex86_10631025]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 10631025_cfg
AddReg         = autorun_addreg

[DriverInstallx64_10631025.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_10631025.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_10631025.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_10631025;, EventLogService

[DriverServicex64_10631025]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 10631025_cfg
AddReg         = autorun_addreg

[10631025_cfg]
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

;cfg idx 18
[DriverInstallx86_000417aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_000417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_000417aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_000417aa;, EventLogService

[DriverServicex86_000417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 000417aa_cfg
AddReg         = autorun_addreg

[DriverInstallx64_000417aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_000417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_000417aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_000417aa;, EventLogService

[DriverServicex64_000417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 000417aa_cfg
AddReg         = autorun_addreg

[000417aa_cfg]
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

;cfg idx 19
[DriverInstallx86_505b17aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_505b17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_505b17aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_505b17aa;, EventLogService

[DriverServicex86_505b17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 505b17aa_cfg
AddReg         = autorun_addreg

[DriverInstallx64_505b17aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_505b17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_505b17aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_505b17aa;, EventLogService

[DriverServicex64_505b17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 505b17aa_cfg
AddReg         = autorun_addreg

[505b17aa_cfg]
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

;cfg idx 20
[DriverInstallx86_511817aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_511817aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_511817aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_511817aa;, EventLogService

[DriverServicex86_511817aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 511817aa_cfg
AddReg         = autorun_addreg

[DriverInstallx64_511817aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_511817aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_511817aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_511817aa;, EventLogService

[DriverServicex64_511817aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 511817aa_cfg
AddReg         = autorun_addreg

[511817aa_cfg]
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x80010009

;cfg idx 21
[DriverInstallx86_505c17aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_505c17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_505c17aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_505c17aa;, EventLogService

[DriverServicex86_505c17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 505c17aa_cfg
AddReg         = autorun_addreg

[DriverInstallx64_505c17aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_505c17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_505c17aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_505c17aa;, EventLogService

[DriverServicex64_505c17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 505c17aa_cfg
AddReg         = autorun_addreg

[505c17aa_cfg]
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

;cfg idx 22 
[DriverInstallx86_609517aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_609517aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_609517aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_609517aa;, EventLogService

[DriverServicex86_609517aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 609517aa_cfg
AddReg         = autorun_addreg

[DriverInstallx64_609517aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_609517aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_609517aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_609517aa;, EventLogService

[DriverServicex64_609517aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 609517aa_cfg
AddReg         = autorun_addreg

[609517aa_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seaeagle", "MMC_MODE_DIS", 0x00010001, 0x80000000
HKR,"seaeagle", "output_tuning", 0x00010001, 0x80110000
HKR,"seaeagle\pcr", "000_p0x300", 0x00010001, 0x00ff0044
HKR,"seaeagle\pcr", "001_p0x3e0", 0x00010001, 0x00400000

;cfg idx 23
[DriverInstallx86_607E17aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_607E17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_607E17aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_607E17aa;, EventLogService

[DriverServicex86_607E17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 607E17aa_cfg
AddReg         = autorun_addreg

[DriverInstallx64_607E17aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_607E17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_607E17aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_607E17aa;, EventLogService

[DriverServicex64_607E17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 607E17aa_cfg
AddReg         = autorun_addreg

[607E17aa_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seaeagle", "MMC_MODE_DIS", 0x00010001, 0x80000000
HKR,"seaeagle", "output_tuning", 0x00010001, 0x80110000
HKR,"seaeagle\pcr", "000_p0x300", 0x00010001, 0x00ff0044
HKR,"seaeagle\pcr", "001_p0x3e0", 0x00010001, 0x00400000

;cfg idx 24
[DriverInstallx86_369417aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_369417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_369417aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_369417aa;, EventLogService

[DriverServicex86_369417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 369417aa_cfg
AddReg         = autorun_addreg

[DriverInstallx64_369417aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_369417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_369417aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_369417aa;, EventLogService

[DriverServicex64_369417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 369417aa_cfg
AddReg         = autorun_addreg

[369417aa_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seaeagle\pcr", "000_p0x300", 0x00010001, 0x00ff0044
HKR,"seaeagle\pcr", "001_p0x3e0", 0x00010001, 0x00400000

;cfg idx 25
[DriverInstallx86_505417aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_505417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_505417aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_505417aa;, EventLogService

[DriverServicex86_505417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 505417aa_cfg
AddReg         = autorun_addreg

[DriverInstallx64_505417aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_505417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_505417aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_505417aa;, EventLogService

[DriverServicex64_505417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 505417aa_cfg
AddReg         = autorun_addreg

[505417aa_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seaeagle\pcr", "000_p0x300", 0x00010001, 0x00ff0044
HKR,"seaeagle\pcr", "001_p0x3e0", 0x00010001, 0x00400000

;cfg idx 26 
[DriverInstallx86_380317aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_380317aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_380317aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_380317aa;, EventLogService

[DriverServicex86_380317aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 380317aa_cfg
AddReg         = autorun_addreg

[DriverInstallx64_380317aa.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_380317aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_380317aa.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_380317aa;, EventLogService

[DriverServicex64_380317aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 380317aa_cfg
AddReg         = autorun_addreg

[380317aa_cfg]
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001

;cfg idx 27
[DriverInstallx86_20648086.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,CopySDPA8220

[DriverInstallx86_20648086.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_20648086.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex86_20648086;, EventLogService

[DriverServicex86_20648086]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 20648086_cfg
AddReg         = autorun_addreg

[DriverInstallx64_20648086.NT]
CopyFiles = @bhtpcrdr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64,CopySDPA8220,CopySDPA8220_WoW64

[DriverInstallx64_20648086.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_20648086.NT.Services]
AddService = BHTPCRDR, 0x00000002 , DriverServicex64_20648086;, EventLogService

[DriverServicex64_20648086]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtpcrdr.sys
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = 20648086_cfg
AddReg         = autorun_addreg

[20648086_cfg]
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x80000000


[Copybhtv5Icon]
bhtv5Icon.dll

[Copybhtv5Icon_WoW64]
bhtv5Icon.dll


[CopySDPA8220]
SDPA8220.dll

[CopySDPA8220_WoW64]
SDPA8220.dll

[InterruptMgmtValues]
HKR, "Interrupt Management",0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties",0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties",MSISupported,0x00010001,1

[EventLogService]
AddReg = EventLogService_AddReg

[EventLogService_AddReg]
HKR,,EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,,TypesSupported,   0x00010001, 7

[pnpsafe_pci_addreg]
HKR, "Parameters\PnpInterface", "5", 0x00010001, 0x00000001

[bus_type]
HKR,"Parameters", "BusType", 0x00010001, 0x0000000C

[default_cfg_se]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seaeagle", "MMC_MODE_DIS", 0x00010001, 0x80000000
HKR,"seaeagle\pcr", "000_p0x300", 0x00010001, 0x00ff0044
HKR,"seaeagle\pcr", "001_p0x3e0", 0x00010001, 0x00400000

[default_cfg_sb]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "MMC_MODE_DIS", 0x00010001, 0x80000000
HKR,"seabird\pcr", "000_p0xe2", 0x00010001, 0xf0001000
HKR,"seabird\pcr", "001_p0xfe", 0x00010001, 0x000f000c
HKR,"seabird\pcr", "002_p0x3e6", 0x00010001, 0x00080008
HKR,"seabird\pcr", "003_p0x300", 0x00010001, 0x00ff0055

[default_cfg_fj2]
HKR,"fj2", "driver_item", 0x00010001, 0x8000001a
HKR,"fj2", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"fj2", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"fj2", "MMC_MODE_DIS", 0x00010001, 0x80000000
HKR,"fj2\pcr", "000_p0x66", 0x00010001, 0x80000
HKR,"fj2\pcr", "001_p0xec", 0x00010001, 0x10001
HKR,"fj2\pcr", "002_p0x64", 0x00010001, 0xc000400
HKR,"fj2\pcr", "003_p0xd4", 0x00010001, 0x80008
HKR,"fj2\pcr", "004_p0x306", 0x00010001, 0xffff1827
HKR,"fj2\pcr", "005_p0x328", 0x00010001, 0xff00c800
HKR,"fj2\pcr", "006_p0x300", 0x00010001, 0xff0066
HKR,"fj2\pcr", "007_p0x68", 0x00010001, 0x30000000
HKR,"fj2\pcr", "008_p0x350", 0x00010001, 0x7fff2492
HKR,"fj2\pcr", "009_p0x35c", 0x00010001, 0xf0002000
HKR,"fj2\pcr", "010_p0x35c", 0x00010001, 0xf10080
HKR,"fj2\pcr", "011_p0x35c", 0x00010001, 0x40004
HKR,"fj2\pcr", "012_p0x3e2", 0x00010001, 0x200000
HKR,"fj2\pcr", "013_p0x334", 0x00010001, 0x1e000c0
HKR,"fj2\pcr", "014_p0x334", 0x00010001, 0x1e000c
HKR,"fj2\pcr", "015_p0x88", 0x00010001, 0x70000000
HKR,"fj2\pcr", "016_p0x33c", 0x00010001, 0x1e000c
HKR,"fj2\pcr", "017_p0xe2", 0x00010001, 0xf0003000
HKR,"fj2\pcr", "018_p0xfe", 0x00010001, 0xf0008

[autorun_addreg] 
HKLM,"System\CurrentControlSet\Services\disk","AutoRunAlwaysDisable", 0x00010008,"SDHC"
HKLM,"System\CurrentControlSet\Services\disk","AutoRunAlwaysDisable", 0x00010008,"SDXC"
HKLM,"System\CurrentControlSet\Services\disk","AutoRunAlwaysDisable", 0x00010008,"SD"
HKLM,"System\CurrentControlSet\Services\disk","AutoRunAlwaysDisable", 0x00010008,"MMC"

[Strings]
REG_SZ        = 0x00000000
REG_MULTI_SZ  = 0x00010000
REG_EXPAND_SZ = 0x00020000
REG_BINARY    = 0x00000001
REG_DWORD     = 0x00010001
SERVICEROOT   = "System\CurrentControlSet\Services"

BayHubTech          = "BayHubTech"
BHTPCRDR.DeviceDesc = "BayHubTech Integrated MMC/SD controller"
BHTPCRDR.DriverDisk = "BayHubTech Integrated MMC/SD controller Driver Disk"
