//****************************************************************************
//                   INTEL CORPORATION PROPRIETARY INFORMATION
//       This software is supplied under the terms of a license agreement or
//       nondisclosure agreement with Intel Corporation and may not be copied
//       or disclosed except in accordance with the terms of that agreement.
//         Copyright (c) 2013 - 2014 Intel Corporation. All Rights Reserved.
//****************************************************************************
//
// SDR Tag Usage
//
//====================================================================//
// (1) Chassis related TAG
//====================================================================//
// _SDR_TAG    'BCP_2U4N'               // SDRs for 2U4N chassis
// _SDR_TAG    '2U4N_BP_X35'            // SDRs for 3.5" HDD-BP
// _SDR_TAG    '2U4N_BP_X25'            // SDRs for 2.5" HDD-BP
// _SDR_TAG    'OTHER'                  // SDRs for OTHER chassis
// _SDR_TAG    'OTHER_SR'               // SDRs for OTHER chassis Slow Ramp
// _SDR_TAG    'OTHER_MR'               // SDRs for OTHER chassis Medium Ramp
// _SDR_TAG    'OTHER_FR'               // SDRs for OTHER chassis Fast Ramp

//====================================================================//
// (2) Processor related sensors
//====================================================================//
// _SDR_TAG    'PROCESSOR_2'            // SDRs for Processor 2

//====================================================================//
// (3) Temperature sensors
//====================================================================//
// _SDR_TAG    'HSBP_TEMP'              // SDR for HSBP Temp
// _SDR_TAG    'IO_MODULE'              // SDR for IOM Temp
// _SDR_TAG    'SAS_MODULE'             // SDR for 'SAS Mod Temp 1' and 'SAS Mod Temp 2'
// _SDR_TAG    'PSOC_TEMP'              // SDR for HSBP PSOC Temp

//====================================================================//
// (4) Fan sensors
//====================================================================//
// _SDR_TAG    'SYS_FAN_2U4N'           //System Fan 2U4N SKU
// _SDR_TAG    'SYSTEM_FAN_1A'          //System Fan SYSTEM_FAN_1A
// _SDR_TAG    'SYSTEM_FAN_1B'          //System Fan SYSTEM_FAN_1B
// _SDR_TAG    'SYSTEM_FAN_2A'          //System Fan SYSTEM_FAN_2A
// _SDR_TAG    'SYSTEM_FAN_2B'          //System Fan SYSTEM_FAN_2B
// _SDR_TAG    'SYSTEM_FAN_3A'          //System Fan SYSTEM_FAN_3A
// _SDR_TAG    'SYSTEM_FAN_3B'          //System Fan SYSTEM_FAN_3B
// _SDR_TAG    'SYSTEM_FAN_4A'          //System Fan SYSTEM_FAN_4A
// _SDR_TAG    'SYSTEM_FAN_4B'          //System Fan SYSTEM_FAN_4B
// _SDR_TAG    'SYSTEM_FAN_5A'          //System Fan SYSTEM_FAN_5A
// _SDR_TAG    'SYSTEM_FAN_5B'          //System Fan SYSTEM_FAN_5B
// _SDR_TAG    'SYSTEM_FAN_6A'          //System Fan SYSTEM_FAN_6A
// _SDR_TAG    'SYSTEM_FAN_6B'          //System Fan SYSTEM_FAN_6B
// _SDR_TAG    'OTHER_FAN_1A'           //System Fan OTHER_FAN_1A
// _SDR_TAG    'OTHER_FAN_1B'           //System Fan OTHER_FAN_1B
// _SDR_TAG    'OTHER_FAN_2A'           //System Fan OTHER_FAN_2A
// _SDR_TAG    'OTHER_FAN_2B'           //System Fan OTHER_FAN_2B
// _SDR_TAG    'OTHER_FAN_3A'           //System Fan OTHER_FAN_3A
// _SDR_TAG    'OTHER_FAN_3B'           //System Fan OTHER_FAN_3B
// _SDR_TAG    'OTHER_FAN_4A'           //System Fan OTHER_FAN_4A
// _SDR_TAG    'OTHER_FAN_4B'           //System Fan OTHER_FAN_4B
// _SDR_TAG    'OTHER_FAN_5A'           //System Fan OTHER_FAN_5A
// _SDR_TAG    'OTHER_FAN_5B'           //System Fan OTHER_FAN_5B
// _SDR_TAG    'OTHER_FAN_6A'           //System Fan OTHER_FAN_6A
// _SDR_TAG    'OTHER_FAN_6B'           //System Fan OTHER_FAN_6B

//====================================================================//
// (5) Chassis Intrusion
//====================================================================//
// _SDR_TAG    'CHASSIS_INTRU'          // Physical Security sensor
// _SDR_TAG    'LAN_LEASH'              // Physical Security sensor

//====================================================================//
// (6) Power Supply related sensors
//====================================================================//
// _SDR_TAG    'PS1_750W'               // 750W Power Supply 1
// _SDR_TAG    'PS2_750W'               // 750W Power Supply 2
// _SDR_TAG    'PS1_1200W'              // 1200W Power Supply 1
// _SDR_TAG    'PS2_1200W'              // 1200W Power Supply 2
// _SDR_TAG    'PS1_1600WAC'            // 1600W AC Power Supply 1
// _SDR_TAG    'PS2_1600WAC'            // 1600W AC Power Supply 2
// _SDR_TAG    'PS1_1600WDC'            // 1600W DC Power Supply 1
// _SDR_TAG    'PS2_1600WDC'            // 1600W DC Power Supply 2
// _SDR_TAG    'REDUNDANT_PS'           // Power Supply Redundancy

//====================================================================//
// (7) Factory sensors
//====================================================================//
// _SDR_TAG    'SHIP'                   // SDRs for Shippings
// _SDR_TAG    'FCT'                    // SDRs for FCT
// _SDR_TAG    'FOQM'                   // SDRs for FOQM


//
// File Header Information
//
_LF_NAME       'S2600JF SDR File'
_LF_VERSION    '1.13'
_LF_FMT_VER    '1.50'
_IPMI_VERSION  '2.00'


//
// SDR Header Information
//
_SDR (
_START_ADDR     0000
_DATA_LEN       0000
_NVS_TYPE       'IMBDEVICE'
_DEV_BUS        FF
_DEV_ADDRESS    20


//====================================================================//
_SDR_TYPE   02
_REC_LEN    002F

   // Sensor Record Header
   0001               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   01                 // Sensor Number

   // Record Body Bytes
   15                 // Entity ID - power management / power distribution board
   01                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   40                 // Sensor Capabilities
   09                 // Sensor Type - power unit
   6F                 // Event / Reading Base Type
   7100               // Assertion Event Mask   --Power down/A/C lost/Soft power control failure/Power unit failure =7100
   7100               // Deassertion Event Mask --Power down/A/C lost/Soft power control failure/Power unit failure =7100
   7100               // Reading Mask & Settable / Readable Threshold Masks --Power down/A/C lost/Soft power control failure/Power unit failure =7100
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Pwr Unit Status'  // String Bytes


//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'REDUNDANT_PS'
_SDR_TAG    'FCT'
_REC_LEN    002F

   // Sensor Record Header
   0002               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   02                 // Sensor Number

   // Record Body Bytes
   15                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   09                 // Sensor Type
   0B                 // Event / Reading Base Type
   FF00               // Assertion Event Mask   --Redundancy regained/Non-red: suff res from redund/Redundancy lost/Redundancy degraded/Non-red: suff from insuff/Non-red: insufficient/Redun degrade from full/Redun degrade from non-redundant=FF00
   FF00               // Deassertion Event Mask --Redundancy regained/Non-red: suff res from redund/Redundancy lost/Redundancy degraded/Non-red: suff from insuff/Non-red: insufficient/Redun degrade from full/Redun degrade from non-redundant=FF00
   FF00               // Reading Mask & Settable / Readable Threshold Masks
                      //--Redundancy regained/Non-red: suff res from redund/Redundancy lost/Redundancy degraded/Non-red: suff from insuff/Non-red: insufficient/Redun degrade from full/Redun degrade from non-redundant=FF00
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Pwr Unit Redund'  // String Bytes


//====================================================================//
_SDR_TYPE   02
_REC_LEN    002D

   // Sensor Record Header
   0003               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   03                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   23                 // Sensor Type
   6F                 // Event / Reading Base Type
   0F01               // Assertion Event Mask   --Timer expired, status only/Hard reset/Power down/Power cycle/Timer interrupt =0F01
   0000               // Deassertion Event Mask --No Deassertion =0000
   0F01               // Reading Mask & Settable / Readable Threshold Masks --Timer expired, status only/Hard reset/Power down/Power cycle/Timer interrupt =0F01
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'IPMI Watchdog'    // String Bytes


//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'LAN_LEASH'
_REC_LEN    002E

   // Sensor Record Header
   0004               // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   04                 // Sensor Number

   // Record Body Bytes
   17                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   05                 // Sensor Type
   6F                 // Event / Reading Base Type
   1000               // Assertion Event Mask   --Chassis intrusion/LAN leash lost 1 =1100
   1000               // Deassertion Event Mask --Chassis intrusion/LAN leash lost 1 =1100
   1000               // Reading Mask & Settable / Readable Threshold Masks --Chassis intrusion/LAN leash lost 1 =1100
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Physical Scrty'   // String Bytes


//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'CHASSIS_INTRU'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    002E

   // Sensor Record Header
   0005               // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   04                 // Sensor Number

   // Record Body Bytes
   17                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   05                 // Sensor Type
   6F                 // Event / Reading Base Type
   1100               // Assertion Event Mask   --Chassis intrusion/LAN leash lost 1 =1100
   1100               // Deassertion Event Mask --Chassis intrusion/LAN leash lost 1 =1100
   1100               // Reading Mask & Settable / Readable Threshold Masks --Chassis intrusion/LAN leash lost 1 =1100
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Physical Scrty'   // String Bytes


//====================================================================//
_SDR_TYPE   02
_REC_LEN    002B

   // Sensor Record Header
   0006               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   06                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   41                 // Sensor Capabilities
   F3                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --State asserted =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'SMI TimeOut'      // String Bytes


//====================================================================//
_SDR_TYPE   02
_REC_LEN    0030

   // Sensor Record Header
   0007               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   07                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   10                 // Sensor Type
   6F                 // Event / Reading Base Type
   0400               // Assertion Event Mask  --Log area reset / cleared =0400
   0000               // Deassertion Event Mask --N/A
   0400               // Reading Mask & Settable / Readable Threshold Masks --Log area reset / cleared =0400
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'System Event Log' // String Bytes


//====================================================================//
_SDR_TYPE   02
_REC_LEN    002C

   // Sensor Record Header
   0008               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   08                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   12                 // Sensor Type
   6F                 // Event / Reading Base Type
   1000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   1000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'System Event'     // String Bytes


//====================================================================//
_SDR_TYPE   02
_REC_LEN    0026

   // Sensor Record Header
   0009               // Record ID
   51                 // SDR Version
   02                 // Record Type
   21                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   09                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   14                 // Sensor Type
   6F                 // Event / Reading Base Type
   0500               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0500               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C6                 // Type/Length Code
   'Button'           // String Bytes


//====================================================================//
_SDR_TYPE      03
_REC_LEN       001D

   // Sensor Record Header
   000A               // Record ID
   51                 // SDR Version
   03                 // Record Type
   18                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0A                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   28                 // Sensor type
   03                 // Event/Reading Type Code
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'BMC Watchdog'     // String Bytes


//====================================================================//
_SDR_TYPE   02
_REC_LEN    002B

   // Sensor Record Header
   000B               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0B                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   02                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --State asserted =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'VR Watchdog'      // String Bytes


//====================================================================//
_SDR_TYPE   02
_REC_LEN    002E

   // Sensor Record Header
   000C               // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0D                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   01                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --State asserted =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'SSB Therm Trip'   // String Bytes


//====================================================================//
_SDR_TYPE   02
_REC_LEN    002F

   // Sensor Record Header
   000D               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0E                 // Sensor Number

   // Record Body Bytes
   2C                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   15                 // Sensor Type
   08                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'IO Mod Presence'  // String Bytes


//====================================================================//
_SDR_TYPE   02
_REC_LEN    0030

   // Sensor Record Header
   000E               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0F                 // Sensor Number

   // Record Body Bytes
   2C                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   15                 // Sensor Type
   08                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'SAS Mod Presence' // String Bytes


//====================================================================//
_SDR_TYPE   02
_REC_LEN    002A

   // Sensor Record Header
   000F               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   10                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   28                 // Sensor Type
   6F                 // Event / Reading Base Type
   1000               // Assertion Event Mask   --State asserted =1000
   1000               // Deassertion Event Mask --State asserted =1000
   1000               // Reading Mask & Settable / Readable Threshold Masks --State asserted =1000
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'BMC Health'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    003E

   // Sensor Record Header
   0010               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   11                 // Sensor Number

   // Record Body Bytes
   17                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   63                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   11                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   02                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   00                 // Analog characteristic flags
   //------------------------------------------------------------------//
   64                 // Nominal Reading
   FA                 // Normal Maximum
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   //------------------------------------------------------------------//
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'System Airflow'   // String Bytes


//====================================================================//
_SDR_TYPE   03
_REC_LEN    0021

  // Sensor Record Header
  0011               // Record ID
  51                 // SDR Version
  03                 // Record Type
  1C                 // Record Length

  // Record Key Bytes
  20                 // Sensor Owner ID
  00                 // Sensor Owner LUN
  12                 // Sensor Number

  // Record Body Bytes
  07                 // Entity ID
  01                 // Entity Instance
  2B                 // Sensor type
  70                 // Event/Reading Type Code
  0000               // Sensor Record Sharing
  00                 // Reserved
  00                 // OEM
  D0                 // Type/Length Code
  'FW Update Status' // String Bytes


//====================================================================//
// Baseboard and chassis related temperature related sensors
//====================================================================//
_SDR_TYPE   01
_REC_LEN    003D

   // Sensor Record Header
   0012               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   20                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type -- (Temperature)
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- (Degrees C)
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   2D                 // Normal Reading (2Dh = 45 degrees C)
   69                 // Normal Maximum (69h = 105 degrees C)
   05                 // Normal Minimum (05h = 5 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   41                 // Upper critical (41h = 65 degrees C)
   3C                 // Upper non-critical (3Ch = 60 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   05                 // Lower critical (05h = 5 degrees C)
   0A                 // Lower non-critical (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'BB Inlet Temp'    // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'HSBP_TEMP'
_REC_LEN    0039

   // Sensor Record Header
   0013               // Record ID
   51                 // SDR Version
   01                 // Record Type
   34                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   21                 // Sensor Number

   // Record Body Bytes
   40                 // Entity ID
   01                 // Entity Instance
   7D                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   FB                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   1E                 // Normal Reading (1Eh = 25 degrees C)
   32                 // Normal Maximum (32h = 45 degrees C)
   0A                 // Normal Minimum (0Ah = 5 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degrees C)
   3C                 // Upper critical (3Ch = 55 degrees C)
   37                 // Upper non-critical (37h = 50 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   05                 // Lower critical (05h = 00 degrees C)
   0A                 // Lower non-critical (0Ah = 5 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type Length Code
   'HSBP Temp'        // String Bytes


//====================================================================//
_SDR_TYPE   01
_REC_LEN    0038

   // Sensor Record Header
   0014               // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   22                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type -- (Temperature)
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- (Degrees C)
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   50                 // Normal Reading (50h = 80 degrees C)
   5D                 // Normal Maximum (5Dh = 93 degrees C)
   05                 // Normal Minimum (0Ah = 5 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   67                 // Upper critical (67h = 103 degrees C)
   62                 // Upper non-critical (62h = 98 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   02                 // Lower critical (05h = 2 degrees C)
   05                 // Lower non-critical (0Ah = 5 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C8                 // Type/Length Code
   'SSB Temp'         // String Bytes


//====================================================================//
_SDR_TYPE   01
_REC_LEN    003B

   // Sensor Record Header
   0015               // Record ID
   51                 // SDR Version
   01                 // Record Type
   36                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   23                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type -- (Temperature)
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- (Degrees C)
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   50                 // Normal Reading (50h = 80 degrees C)
   69                 // Normal Maximum (69h = 105 degrees C)
   05                 // Normal Minimum (05h = 5 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   5A                 // Upper critical (5Ah = 90 degrees C)
   55                 // Upper non-critical (55h = 85 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   05                 // Lower critical (05h = 5 degrees C)
   0A                 // Lower non-critical (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'BB BMC Temp'      // String Bytes


//====================================================================//
_SDR_TYPE   01
_REC_LEN    003A

   // Sensor Record Header
   0016               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   24                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type -- (Temperature)
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- (Degrees C)
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   50                 // Normal Reading (50h = 80 degrees C)
   69                 // Normal Maximum (69h = 105 degrees C)
   05                 // Normal Minimum (05h = 5 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   73                 // Upper critical (73h = 115 degrees C)
   6E                 // Upper non-critical (6Eh = 110 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   05                 // Lower critical (05h = 5 degrees C)
   0A                 // Lower non-critical (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'P1 VR Temp'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_REC_LEN    0037

   // Sensor Record Header
   0017               // Record ID
   51                 // SDR Version
   01                 // Record Type
   32                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   25                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type -- (Temperature)
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- (Degrees C)
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   50                 // Normal Reading (50h = 80 degrees C)
   69                 // Normal Maximum (69h = 105 degrees C)
   05                 // Normal Minimum (05h = 5 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   73                 // Upper critical (73h = 115 degrees C)
   6E                 // Upper non-critical (6Eh = 110 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   05                 // Lower critical (05h = 5 degrees C)
   0A                 // Lower non-critical (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C7                 // Type/Length Code
   'IB Temp'          // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    003D

   // Sensor Record Header
   0018               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   2E                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type -- (Temperature)
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask   --[u,l][c,nc]=0000
   0000               // Deassertion Event Mask --[u,l][c,nc]=0000
   0000               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=0000
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- (Degrees C)
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   37                 // Normal Reading (37h = 55 degrees C)
   4B                 // Normal Maximum (4Bh = 75 degrees C)
   05                 // Normal Minimum (05h = 5 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   55                 // Upper critical (55h = 85 degrees C)
   50                 // Upper non-critical (50h = 80 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   05                 // Lower critical (05h = 5 degrees C)
   0A                 // Lower non-critical (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   04                 // Positive hysteresis value
   04                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Exit Air Temp'    // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'IO_MODULE'
_SDR_TAG    'FCT'
_REC_LEN    0038

   // Sensor Record Header
   0019               // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   26                 // Sensor Number

   // Record Body Bytes
   0C                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   28                 // Normal Reading (28h = 40 degrees C)
   46                 // Normal Maximum (46h = 70 degrees C)
   05                 // Normal Minimum (05h = 5 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   50                 // Upper critical (50h = 80 degrees C)
   4B                 // Upper non-critical (4Bh = 75 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   02                 // Lower critical (05h = 2 degrees C)
   05                 // Lower non-critical (0Ah = 5 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   C8                 // Type/Length Code
   'IOM Temp'         // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SAS_MODULE'
_REC_LEN    003E

   // Sensor Record Header
   001A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   2D                 // Sensor Number

   // Record Body Bytes
   0C                 // Entity ID
   03                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   28                 // Normal Reading (28h = 40 degrees C)
   46                 // Normal Maximum (46h = 70 degrees C)
   05                 // Normal Minimum (05h = 5 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   50                 // Upper critical (50h = 80 degrees C)
   4B                 // Upper non-critical (4Bh = 75 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   05                 // Lower critical (05h = 5 degrees C)
   0A                 // Lower non-critical (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CE                 // Type/Length Code
   'SAS Mod Temp 1'   // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SAS_MODULE'
_REC_LEN    003E

   // Sensor Record Header
   001B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   28                 // Sensor Number

   // Record Body Bytes
   0C                 // Entity ID
   04                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   32                 // Normal Reading (32h = 50 degrees C)
   55                 // Normal Maximum (55h = 85 degrees C)
   05                 // Normal Minimum (05h = 5 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   5F                 // Upper critical (5Fh = 95 degrees C)
   5A                 // Upper non-critical (5Ah = 90 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   05                 // Lower critical (05h = 5 degrees C)
   0A                 // Lower non-critical (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CE                 // Type/Length Code
   'SAS Mod Temp 2'   // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PSOC_TEMP'
_SDR_TAG    'TEST_PLATE'
_REC_LEN    0039

   // Sensor Record Header
   001C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   34                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   29                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   7D                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   19                 // Normal Reading (19h = 25 degrees C)
   2D                 // Normal Maximum (2Dh = 45 degrees C)
   05                 // Normal Minimum (05h = 5 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degrees C)
   73                 // Upper critical (73h = 115 degrees C)
   6E                 // Upper non-critical (6Eh = 110 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (00h = 0 degrees C)
   05                 // Lower non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type Length Code
   'HSBP PSOC'        // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'OTHER'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'SHIP'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003C

   // Sensor Record Header
   001D               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   2F                 // Sensor Number

   // Record Body Bytes
   0C                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   50                 // Normal Reading (50h = 80 degrees C)
   6E                 // Normal Maximum (6Eh = 110 degrees C)
   05                 // Normal Minimum (05h = 5 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   78                 // Upper critical (78h = 120 degrees C)
   73                 // Upper non-critical (73h = 115 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   05                 // Lower critical (05h = 5 degrees C)
   0A                 // Lower non-critical (0Ah = 10 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CC                 // Type/Length Code
   'LAN NIC Temp'     // String Bytes


//====================================================================//
// Fan tachometer sensors
//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SYS_FAN_2U4N'
_REC_LEN    003A

   // Sensor Record Header
   001E               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   30                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   53                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   85                 // Normal Reading (84h == 11200 RPM)
   FF                 // Normal Maximum (FFh == 21400 RPM)
   0B                 // Normal Minimum (0Ah == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 21400 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   08                 // Lower critical (08h == 664 RPM)
   09                 // Lower non-critical (09h == 747 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 1A'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SYS_FAN_2U4N'
_REC_LEN    003A

   // Sensor Record Header
   001F               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   31                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   56                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   85                 // Normal Reading (84h == 11550 RPM)
   FF                 // Normal Maximum (FFh == 22100 RPM)
   0B                 // Normal Minimum (0Ah == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 22100 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   08                 // Lower critical (08h == 688 RPM)
   09                 // Lower non-critical (09h == 774 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 1B'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SYS_FAN_2U4N'
_REC_LEN    003A

   // Sensor Record Header
   0020               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   32                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   03                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   53                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   85                 // Normal Reading (84h == 11200 RPM)
   FF                 // Normal Maximum (FFh == 21400 RPM)
   0B                 // Normal Minimum (0Ah == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 21400 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   08                 // Lower critical (08h == 664 RPM)
   09                 // Lower non-critical (09h == 747 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 2A'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SYS_FAN_2U4N'
_REC_LEN    003A

   // Sensor Record Header
   0021               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   33                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   04                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   56                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   85                 // Normal Reading (84h == 11550 RPM)
   FF                 // Normal Maximum (FFh == 22100 RPM)
   0B                 // Normal Minimum (0Ah == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 22100 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   08                 // Lower critical (08h == 688 RPM)
   09                 // Lower non-critical (09h == 774 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 2B'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SYS_FAN_2U4N'
_REC_LEN    003A

   // Sensor Record Header
   0022               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   34                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   05                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   53                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   85                 // Normal Reading (84h == 11200 RPM)
   FF                 // Normal Maximum (FFh == 21400 RPM)
   0B                 // Normal Minimum (0Ah == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 21400 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   08                 // Lower critical (08h == 664 RPM)
   09                 // Lower non-critical (09h == 747 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 3A'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SYS_FAN_2U4N'
_REC_LEN    003A

   // Sensor Record Header
   0023               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   35                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   06                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   56                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   85                 // Normal Reading (84h == 11550 RPM)
   FF                 // Normal Maximum (FFh == 22100 RPM)
   0B                 // Normal Minimum (0Ah == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 22100 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   08                 // Lower critical (08h == 688 RPM)
   09                 // Lower non-critical (09h == 774 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 3B'       // String Bytes


//====================================================================//
// PO Kit/Shipping/FCT/FOQM Fan tachometer sensors
//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_1A'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003A

   // Sensor Record Header
   0024               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   30                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   3E                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   87                 // Normal Reading (87h == 8500 RPM)
   FF                 // Normal Maximum (FFh == 16000 RPM)
   0F                 // Normal Minimum (0Fh == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 16000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   0B                 // Lower critical (0Bh == 682 RPM)
   0C                 // Lower non-critical (0Ch == 744 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 1A'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_1B'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003A

   // Sensor Record Header
   0025               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   31                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   3C                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   87                 // Normal Reading (87h == 8200 RPM)
   FF                 // Normal Maximum (FFh == 15400 RPM)
   10                 // Normal Minimum (10h == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 15400 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   0B                 // Lower critical (0Bh == 660 RPM)
   0D                 // Lower non-critical (0Dh == 780 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 1B'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_2A'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003A

   // Sensor Record Header
   0026               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   32                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   03                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   3E                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   87                 // Normal Reading (87h == 8500 RPM)
   FF                 // Normal Maximum (FFh == 16000 RPM)
   0F                 // Normal Minimum (0Fh == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 16000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   0B                 // Lower critical (0Bh == 682 RPM)
   0C                 // Lower non-critical (0Ch == 744 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 2A'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_2B'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003A

   // Sensor Record Header
   0027               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   33                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   04                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   3C                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   87                 // Normal Reading (87h == 8200 RPM)
   FF                 // Normal Maximum (FFh == 15400 RPM)
   10                 // Normal Minimum (10h == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 15400 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   0B                 // Lower critical (0Bh == 660 RPM)
   0D                 // Lower non-critical (0Dh == 780 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 2B'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_3A'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003A

   // Sensor Record Header
   0028               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   34                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   05                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   3E                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   87                 // Normal Reading (87h == 8500 RPM)
   FF                 // Normal Maximum (FFh == 16000 RPM)
   0F                 // Normal Minimum (0Fh == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 16000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   0B                 // Lower critical (0Bh == 682 RPM)
   0C                 // Lower non-critical (0Ch == 744 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 3A'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_3B'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003A

   // Sensor Record Header
   0029               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   35                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   06                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   3C                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   87                 // Normal Reading (87h == 8200 RPM)
   FF                 // Normal Maximum (FFh == 15400 RPM)
   10                 // Normal Minimum (10h == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 15400 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   0B                 // Lower critical (0Bh == 660 RPM)
   0D                 // Lower non-critical (0Dh == 780 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 3B'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_4A'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003A

   // Sensor Record Header
   002A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   36                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   07                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   3E                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   87                 // Normal Reading (87h == 8500 RPM)
   FF                 // Normal Maximum (FFh == 16000 RPM)
   0F                 // Normal Minimum (0Fh == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 16000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   0B                 // Lower critical (0Bh == 682 RPM)
   0C                 // Lower non-critical (0Ch == 744 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 4A'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_4B'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003A

   // Sensor Record Header
   002B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   37                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   08                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   3C                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   87                 // Normal Reading (87h == 8200 RPM)
   FF                 // Normal Maximum (FFh == 15400 RPM)
   10                 // Normal Minimum (10h == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 15400 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   0B                 // Lower critical (0Bh == 660 RPM)
   0D                 // Lower non-critical (0Dh == 780 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 4B'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_5A'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003A

   // Sensor Record Header
   002C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   38                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   09                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   3E                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   87                 // Normal Reading (87h == 8500 RPM)
   FF                 // Normal Maximum (FFh == 16000 RPM)
   0F                 // Normal Minimum (0Fh == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 16000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   0B                 // Lower critical (0Bh == 682 RPM)
   0C                 // Lower non-critical (0Ch == 744 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 5A'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_5B'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003A

   // Sensor Record Header
   002D               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   39                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0A                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   3C                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   87                 // Normal Reading (87h == 8200 RPM)
   FF                 // Normal Maximum (FFh == 15400 RPM)
   10                 // Normal Minimum (10h == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 15400 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   0B                 // Lower critical (0Bh == 660 RPM)
   0D                 // Lower non-critical (0Dh == 780 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 5B'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_6A'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003A

   // Sensor Record Header
   002E               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   3A                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0B                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   3E                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   87                 // Normal Reading (87h == 8500 RPM)
   FF                 // Normal Maximum (FFh == 16000 RPM)
   0F                 // Normal Minimum (0Fh == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 16000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   0B                 // Lower critical (0Bh == 682 RPM)
   0C                 // Lower non-critical (0Ch == 744 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 6A'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_6B'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003A

   // Sensor Record Header
   002F               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   3B                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0C                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   3C                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   87                 // Normal Reading (87h == 8200 RPM)
   FF                 // Normal Maximum (FFh == 15400 RPM)
   10                 // Normal Minimum (10h == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 15400 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   0B                 // Lower critical (0Bh == 660 RPM)
   0D                 // Lower non-critical (0Dh == 780 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 6B'       // String Bytes


//====================================================================//
// Other Fan tachometer sensors
//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_1A'
_REC_LEN    003A

   // Sensor Record Header
   0030               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   30                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   84                 // Normal Reading (87h == 13000 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   0A                 // Normal Minimum (0Ah == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 25000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   07                 // Lower critical (0Ch == 700 RPM)
   08                 // Lower non-critical (0Bh == 800 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 1A'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_1B'
_REC_LEN    003A

   // Sensor Record Header
   0031               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   31                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   84                 // Normal Reading (87h == 13000 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   0A                 // Normal Minimum (10h == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 25000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   07                 // Lower critical (0Ch == 700 RPM)
   08                 // Lower non-critical (0Bh == 800 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 1B'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_2A'
_REC_LEN    003A

   // Sensor Record Header
   0032               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   32                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   03                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   84                 // Normal Reading (84h == 13000 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   0A                 // Normal Minimum (0Fh == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 25000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   07                 // Lower critical (0Ch == 700 RPM)
   08                 // Lower non-critical (0Bh == 800 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 2A'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_2B'
_REC_LEN    003A

   // Sensor Record Header
   0033               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   33                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   04                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   84                 // Normal Reading (84h == 13000 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   0A                 // Normal Minimum (10h == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 25000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   07                 // Lower critical (0Ch == 700 RPM)
   08                 // Lower non-critical (0Bh == 800 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 2B'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_3A'
_REC_LEN    003A

   // Sensor Record Header
   0034               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   34                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   05                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   84                 // Normal Reading (84h == 13000 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   0A                 // Normal Minimum (0Ah == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 25000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   07                 // Lower critical (0Ch == 700 RPM)
   08                 // Lower non-critical (0Bh == 800 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 3A'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_3B'
_REC_LEN    003A

   // Sensor Record Header
   0035               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   35                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   06                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   84                 // Normal Reading (84h == 13000 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   0A                 // Normal Minimum (0ah == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 15400 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   07                 // Lower critical (07h == 700 RPM)
   08                 // Lower non-critical (08h == 800 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 3B'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_4A'
_REC_LEN    003A

   // Sensor Record Header
   0036               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   36                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   07                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   84                 // Normal Reading (87h == 13000 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   0A                 // Normal Minimum (0Fh == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 25000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   07                 // Lower critical (0Ch == 700 RPM)
   08                 // Lower non-critical (0Bh == 800 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 4A'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_4B'
_REC_LEN    003A

   // Sensor Record Header
   0037               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   37                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   08                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   84                 // Normal Reading (87h == 13000 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   0A                 // Normal Minimum (10h == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 15400 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   07                 // Lower critical (07h == 700 RPM)
   08                 // Lower non-critical (08h == 800 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 4B'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_5A'
_REC_LEN    003A

   // Sensor Record Header
   0038               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   38                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   09                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   84                 // Normal Reading (84h == 13000 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   0A                 // Normal Minimum (0ah == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 16000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   07                 // Lower critical (07h == 700 RPM)
   08                 // Lower non-critical (08h == 800 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 5A'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_5B'
_REC_LEN    003A

   // Sensor Record Header
   0039               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   39                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0A                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   84                 // Normal Reading (84h == 13000 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   0A                 // Normal Minimum (0ah == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 15400 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   07                 // Lower critical (07h == 700 RPM)
   08                 // Lower non-critical (08h == 800 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 5B'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_6A'
_REC_LEN    003A

   // Sensor Record Header
   003A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   3A                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0B                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   84                 // Normal Reading (84h == 13000 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   0A                 // Normal Minimum (0Ah == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 16000 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   07                 // Lower critical (07h == 700 RPM)
   08                 // Lower non-critical (08h == 800 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 6A'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_6B'
_REC_LEN    003A

   // Sensor Record Header
   003B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   35                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   3B                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0C                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask   --[l][c,nc]=0530
   0500               // Deassertion Event Mask --[l][c,nc]=0500
   0303               // Reading Mask & Settable / Readable Threshold Masks --[l][c,nc]=0303
   00                 // Sensor Units 1
   12                 // Sensor Units 2 (12h=RPM)
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   84                 // Normal Reading (84h == 13000 RPM)
   FF                 // Normal Maximum (FFh == 25000 RPM)
   0A                 // Normal Minimum (0Ah == 1000  RPM)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh == 15400 RPM)
   00                 // Sensor Minimum Reading (00h == 0 RPM)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical (not specified)
   00                 // Upper non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   07                 // Lower critical (0Ch == 700 RPM)
   08                 // Lower non-critical (0Bh == 800 RPM)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CA                 // Type/Length Code
   'Sys Fan 6B'       // String Bytes


//====================================================================//
// Power supply sensors (Only supported with PMBus enabled power supplies)
//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PS1_750W'
_SDR_TAG    'PS1_1200W'
_SDR_TAG    'PS1_1600WAC'
_SDR_TAG    'PS1_1600WDC'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    002A

   // Sensor Record Header
   003C               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   50                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   08                 // Sensor Type
   6F                 // Event / Reading Base Type
   4F00               // Assertion Event Mask   --Presence/Failure/Predictive Failure/A/C lost/Configuration error =4F00
   4F00               // Deassertion Event Mask --Presence/Failure/Predictive Failure/A/C lost/Configuration error =4F00
   4F00               // Reading Mask & Settable / Readable Threshold Masks --Presence/Failure/Predictive Failure/A/C lost/Configuration error =4F00
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'PS1 Status'       // String Bytes


//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PS2_750W'
_SDR_TAG    'PS2_1200W'
_SDR_TAG    'PS2_1600WAC'
_SDR_TAG    'PS2_1600WDC'
_SDR_TAG    'FCT'
_REC_LEN    002A

   // Sensor Record Header
   003D               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   51                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   08                 // Sensor Type
   6F                 // Event / Reading Base Type
   4F00               // Assertion Event Mask   --Presence/Failure/Predictive Failure/A/C lost/Configuration error =4F00
   4F00               // Deassertion Event Mask --Presence/Failure/Predictive Failure/A/C lost/Configuration error =4F00
   4F00               // Reading Mask & Settable / Readable Threshold Masks --Presence/Failure/Predictive Failure/A/C lost/Configuration error =4F00
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'PS2 Status'       // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PS1_750W'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003F

   // Sensor Record Header
   003E               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   54                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   04                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   66                 // Nomnal Reading (66h=4090Watt)
   CC                 // Normal Maximum (CCh=817.6Watt)
   00                 // Normal Minimum (00h=0Watt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh=1020.0Watt)
   00                 // Sensor Minimum Reading (00h=0.0Watt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   E6                 // Upper critical (E6h=923.1Watt)
   D9                 // Upper non-critical (D9h=870.3Watt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS1 Input Power'  // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PS1_1200W'
_REC_LEN    003F

   // Sensor Record Header
   003F               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   54                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   07                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   5E                 // Nomnal Reading (6Dh=659.0Watt)
   BC                 // Normal Maximum (DAh=1318.7Watt)
   00                 // Normal Minimum (00h=0Watt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh=1020.0Watt)
   00                 // Sensor Minimum Reading (00h=0.0Watt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   FA                 // Upper critical (FAh=1753.8Watt)
   DB                 // Upper non-critical (DBh=1536.3Watt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS1 Input Power'  // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PS1_1600WAC'
_REC_LEN    003F

   // Sensor Record Header
   0040               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   54                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   0A                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   57                 // Nomnal Reading (57h=877Watt)
   AF                 // Normal Maximum (AFh=1753.8Watt)
   00                 // Normal Minimum (00h=0Watt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh=1020.0Watt)
   00                 // Sensor Minimum Reading (00h=0.0Watt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   E6                 // Upper critical (E6h=2030.8Watt)
   CB                 // Upper non-critical (CBh=2307.7Watt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS1 Input Power'  // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PS1_1600WDC'
_REC_LEN    003F

   // Sensor Record Header
   0041               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   54                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   0A                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   5A                 // Nomnal Reading (5Ah=907Watt)
   B5                 // Normal Maximum (B5h=1813.6Watt)
   00                 // Normal Minimum (00h=0Watt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh=1020.0Watt)
   00                 // Sensor Minimum Reading (00h=0.0Watt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   EE                 // Upper critical (EEh=2386.4Watt)
   D2                 // Upper non-critical (D2h=2100.0Watt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS1 Input Power'  // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PS2_750W'
_SDR_TAG    'FCT'
_REC_LEN    003F

   // Sensor Record Header
   0042               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   55                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   04                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   66                 // Nomnal Reading (66h=4090Watt)
   CC                 // Normal Maximum (CCh=817.6Watt)
   00                 // Normal Minimum (00h=0Watt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh=1020.0Watt)
   00                 // Sensor Minimum Reading (00h=0.0Watt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   E6                 // Upper critical (E6h=923.1Watt)
   D9                 // Upper non-critical (D9h=870.3Watt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS2 Input Power'  // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PS2_1200W'
_REC_LEN    003F

   // Sensor Record Header
   0043               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   55                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   07                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   5E                 // Nomnal Reading (6Dh=659.0Watt)
   BC                 // Normal Maximum (DAh=1318.7Watt)
   00                 // Normal Minimum (00h=0Watt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh=1020.0Watt)
   00                 // Sensor Minimum Reading (00h=0.0Watt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   FA                 // Upper critical (FAh=1753.8Watt)
   DB                 // Upper non-critical (DBh=1536.3Watt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS2 Input Power'  // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PS2_1600WAC'
_REC_LEN    003F

   // Sensor Record Header
   0044               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   55                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   0A                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   57                 // Nomnal Reading (57h=877Watt)
   AF                 // Normal Maximum (AFh=1753.8Watt)
   00                 // Normal Minimum (00h=0Watt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh=1020.0Watt)
   00                 // Sensor Minimum Reading (00h=0.0Watt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   E6                 // Upper critical (E6h=2030.8Watt)
   CB                 // Upper non-critical (CBh=2307.7Watt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS2 Input Power'  // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PS2_1600WDC'
_REC_LEN    003F

   // Sensor Record Header
   0045               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   55                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   0A                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   5A                 // Nomnal Reading (5Ah=907Watt)
   B5                 // Normal Maximum (B5h=1813.6Watt)
   00                 // Normal Minimum (00h=0Watt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh=1020.0Watt)
   00                 // Sensor Minimum Reading (00h=0.0Watt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   EE                 // Upper critical (EEh=2386.4Watt)
   D2                 // Upper non-critical (D2h=2100.0Watt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysterisis value
   02                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS2 Input Power'  // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PS1_750W'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003E

   // Sensor Record Header
   0046               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   58                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   32                 // Normal Reading (32h = 50 %)
   64                 // Normal Maximum (64h = 100 %)
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   70                 // Upper critical (70h = 112.0 %)
   64                 // Upper non-critical (64h = 100.0 %)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical  (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysterisis value
   00                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS1 Curr Out %'   // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PS1_1200W'
_REC_LEN    003E

   // Sensor Record Header
   0047               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   58                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   32                 // Normal Reading (32h = 50 %)
   64                 // Normal Maximum (64h = 100 %)
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   85                 // Upper critical (85h = 133.0 %)
   64                 // Upper non-critical (64h = 100.0 %)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical  (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysterisis value
   00                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS1 Curr Out %'   // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PS1_1600WAC'
_SDR_TAG    'PS1_1600WDC'
_REC_LEN    003E

   // Sensor Record Header
   0048               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   58                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   32                 // Normal Reading (32h = 50 %)
   64                 // Normal Maximum (64h = 100 %)
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   83                 // Upper critical (83h = 131.0 %)
   64                 // Upper non-critical (64h = 100.0 %)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical  (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysterisis value
   00                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS1 Curr Out %'   // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PS2_750W'
_SDR_TAG    'FCT'
_REC_LEN    003E

   // Sensor Record Header
   0049               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   59                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   32                 // Normal Reading (32h = 50 %)
   64                 // Normal Maximum (64h = 100 %)
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   70                 // Upper critical (70h = 112.0 %)
   64                 // Upper non-critical (64h = 100.0 %)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical  (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysterisis value
   00                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS2 Curr Out %'   // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PS2_1200W'
_REC_LEN    003E

   // Sensor Record Header
   004A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   59                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   32                 // Normal Reading (32h = 50 %)
   64                 // Normal Maximum (64h = 100 %)
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   85                 // Upper critical (85h = 133.0 %)
   64                 // Upper non-critical (64h = 100.0 %)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical  (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysterisis value
   00                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS2 Curr Out %'   // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PS2_1600WAC'
_SDR_TAG    'PS2_1600WDC'
_REC_LEN    003E

   // Sensor Record Header
   004B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   59                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   32                 // Normal Reading (32h = 50 %)
   64                 // Normal Maximum (64h = 100 %)
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   83                 // Upper critical (83h = 131.0 %)
   64                 // Upper non-critical (64h = 100.0 %)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical  (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysterisis value
   00                 // Negative hysterisis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS2 Curr Out %'   // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PS1_750W'
_SDR_TAG    'PS1_1200W'
_SDR_TAG    'PS1_1600WAC'
_SDR_TAG    'PS1_1600WDC'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003F

   // Sensor Record Header
   004C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   5C                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   01                 // Sensor Type -- Temp
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- Degrees C
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   19                 // Normal Reading (19h = 25 degrees C)
   32                 // Normal Maximum (32h = 50 degrees C)
   05                 // Normal Minimum (05h = 5 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   3C                 // Upper critical (3Ch = 60 degrees C)
   37                 // Upper non-critical (37h = 55 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CF                 // Type/Length Code
   'PS1 Temperature'  // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PS2_750W'
_SDR_TAG    'PS2_1200W'
_SDR_TAG    'PS2_1600WAC'
_SDR_TAG    'PS2_1600WDC'
_SDR_TAG    'FCT'
_REC_LEN    003F

   // Sensor Record Header
   004D               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   5D                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7B                 // Sensor Initialization
   E8                 // Sensor Capabilities
   01                 // Sensor Type -- Temp
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2 -- Degrees C
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   19                 // Normal Reading (19h = 25 degrees C)
   32                 // Normal Maximum (32h = 50 degrees C)
   05                 // Normal Minimum (05h = 5 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   3C                 // Upper critical (3Ch = 60 degrees C)
   37                 // Upper non-critical (37h = 55 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CF                 // Type/Length Code
   'PS2 Temperature'  // String Bytes


//====================================================================//
// Processor (CPU) & DIMM sensors
//====================================================================//
_SDR_TYPE   02
_REC_LEN    0029

   // Sensor Record Header
   004E               // Record ID
   51                 // SDR Version
   02                 // Record Type
   24                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   70                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   6F                 // Event / Reading Base Type
   8200               // Assertion Event Mask   --Thermal trip/Presence/Processor disabled =8201
   8200               // Deassertion Event Mask --Thermal trip/Presence/Processor disabled =8201
   8200               // Reading Mask & Settable / Readable Threshold Masks --Thermal trip/Presence/Processor disabled=8201
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'P1 Status'        // String Bytes


//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0029

   // Sensor Record Header
   004F               // Record ID
   51                 // SDR Version
   02                 // Record Type
   24                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   71                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   6F                 // Event / Reading Base Type
   8200               // Assertion Event Mask   --Thermal trip/Presence/Processor disabled =8201
   8200               // Deassertion Event Mask --Thermal trip/Presence/Processor disabled =8201
   8200               // Reading Mask & Settable / Readable Threshold Masks --Thermal trip/Presence/Processor disabled =8201
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'P2 Status'        // String Bytes


//====================================================================//
_SDR_TYPE   01
_REC_LEN    003F

   // Sensor Record Header
   0050               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   74                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   F1                 // Normal Reading (F1h = -15 degree C)
   00                 // Normal Maximum (00h = 0 degree C)
   BA                 // Normal Minimum (BAh = -70 degree C)
   //------------------------------------------------------------------//
   00                 // Sensor Maximum Reading (00h = 0 degree C)
   80                 // Sensor Minimum Reading (80h = -128 degree C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degree C)
   00                 // Upper critical (00h = 0 degree C)
   00                 // Upper non-critical (00h = 0 degree C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degree C)
   00                 // Lower critical (00h = 0 degree C)
   00                 // Lower non-critical (00h = 0 degree C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CF                 // Type/Length Code
   'P1 Therm Margin'  // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    003F

   // Sensor Record Header
   0051               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   75                 // Sensor Number

   // Record Body Byte
   03                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   F1                 // Normal Reading (F1h = -15 degree C)
   00                 // Normal Maximum (00h = 0 degree C)
   BA                 // Normal Minimum (BAh = -70 degree C)
   //------------------------------------------------------------------//
   00                 // Sensor Maximum Reading (00h = 0 degree C)
   80                 // Sensor Minimum Reading (80h = -128 degree C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degree C)
   00                 // Upper critical (00h = 0 degree C)
   00                 // Upper non-critical (00h = 0 degree C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degree C)
   00                 // Lower critical (00h = 0 degree C)
   00                 // Lower non-critical (00h = 0 degree C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CF                 // Type/Length Code
   'P2 Therm Margin'  // String Bytes


//====================================================================//
_SDR_TYPE   01
_REC_LEN    003F

   // Sensor Record Header
   0052               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   78                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   00                 // Normal Reading (00h = 0 %)
   14                 // Normal Maximum (14h = 20 %)
   00                 // Normal Minimum (00h = 0 %)
   //------------------------------------------------------------------//
   64                 // Sensor Maximum Reading (64h = 100 %)
   00                 // Sensor Minimum Reading (00h = 0 %)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 %)
   32                 // Upper critical (32h = 50 %)
   1E                 // Upper non-critical (1Eh = 30 %)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 %)
   00                 // Lower critical (00h = 0 %)
   00                 // Lower non-critical (00h = 0 %)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'P1 Therm Ctrl %'  // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    003F

   // Sensor Record Header
   0053               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   79                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   00                 // Normal Reading (00h = 0 %)
   14                 // Normal Maximum (14h = 20 %)
   00                 // Normal Minimum (00h = 0 %)
   //------------------------------------------------------------------//
   64                 // Sensor Maximum Reading (64h = 100 %)
   00                 // Sensor Minimum Reading (00h = 0 %)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 %)
   32                 // Upper critical (32h = 50 %)
   1E                 // Upper non-critical (1Eh = 30 %)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 %)
   00                 // Lower critical (00h = 0 %)
   00                 // Lower non-critical (00h = 0 %)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'P2 Therm Ctrl %'  // String Bytes


//====================================================================//
_SDR_TYPE   02
_REC_LEN    0027

   // Sensor Record Header
   0054               // Record ID
   51                 // SDR Version
   02                 // Record Type
   22                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   7C                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   41                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C7                 // Type/Length Code
   'P1 ERR2'          // String Bytes


//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0027

   // Sensor Record Header
   0055               // Record ID
   51                 // SDR Version
   02                 // Record Type
   22                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   7D                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   41                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C7                 // Type/Length Code
   'P2 ERR2'          // String Bytes


//====================================================================//
_SDR_TYPE   02
_REC_LEN    0026

   // Sensor Record Header
   0056               // Record ID
   51                 // SDR Version
   02                 // Record Type
   21                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   80                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C6                 // Type/Length Code
   'CATERR'           // String Bytes


//====================================================================//
_SDR_TYPE   02
_REC_LEN    0030

   // Sensor Record Header
   0057               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   81                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'P1 MSID Mismatch' // String Bytes


//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0030

   // Sensor Record Header
   0058               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   87                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'P2 MSID Mismatch' // String Bytes


//====================================================================//
_SDR_TYPE   02
_REC_LEN    002B

   // Sensor Record Header
   0059               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   82                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'CPU Missing'      // String Bytes


//====================================================================//
_SDR_TYPE   01
_REC_LEN    0040

   // Sensor Record Header
   005A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   83                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   F1                 // Normal Reading (F1h = -15 degree C)
   00                 // Normal Maximum (00h = 0 degree C)
   BA                 // Normal Minimum (BAh = -70 degree C)
   //------------------------------------------------------------------//
   00                 // Sensor Maximum Reading (00h = 0 degree C)
   80                 // Sensor Minimum Reading (80h = -128 degree C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degree C)
   0F                 // Upper critical (0Fh = 15 degree C)
   0A                 // Upper non-critical (0Ah = 10 degree C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degree C)
   00                 // Lower critical (00h = 0 degree C)
   00                 // Lower non-critical (00h = 0 degree C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   D0                 // Type/Length Code
   'P1 DTS Therm Mgn' // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0040

   // Sensor Record Header
   005B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   84                 // Sensor Number

   // Record Body Byte
   03                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   F1                 // Normal Reading (F1h = -15 degree C)
   00                 // Normal Maximum (00h = 0 degree C)
   BA                 // Normal Minimum (BAh = -70 degree C)
   //------------------------------------------------------------------//
   00                 // Sensor Maximum Reading (00h = 0 degree C)
   80                 // Sensor Minimum Reading (80h = -128 degree C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degree C)
   0F                 // Upper critical (0Fh = 15 degree C)
   0A                 // Upper non-critical (0Ah = 10 degree C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degree C)
   00                 // Lower critical (00h = 0 degree C)
   00                 // Lower non-critical (00h = 0 degree C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   D0                 // Type/Length Code
   'P2 DTS Therm Mgn' // String Bytes


//====================================================================//
_SDR_TYPE   02
_REC_LEN    002A

   // Sensor Record Header
   005C               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   90                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   01                 // Sensor Type
   05                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --Limit exceeded =0200
   0200               // Deassertion Event Mask --Limit exceeded =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --Limit exceeded =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'P1 VRD Hot'       // String Bytes


//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    002A

   // Sensor Record Header
   005D               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   91                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   01                 // Sensor Type
   05                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --Limit exceeded =0200
   0200               // Deassertion Event Mask --Limit exceeded =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --Limit exceeded =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'P2 VRD Hot'       // String Bytes


//====================================================================//
// Power supply fan tachometer sensors
//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PS1_750W'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    002C

   // Sensor Record Header
   005E               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   A0                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0D                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   00                 // Sensor Capabilities -- Manual Rearm
   04                 // Sensor Type - Fan
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Mask
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'PS1 Fan Fail'     // String Bytes


//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PS2_750W'
_SDR_TAG    'FCT'
_REC_LEN    002C

   // Sensor Record Header
   005F               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   A4                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0E                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   00                 // Sensor Capabilities -- Manual Rearm
   04                 // Sensor Type - Fan
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Mask
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'PS2 Fan Fail'     // String Bytes


//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PS1_1200W'
_SDR_TAG    'PS1_1600WAC'
_SDR_TAG    'PS1_1600WDC'
_REC_LEN    002F

   // Sensor Record Header
   0060               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   A0                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0D                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   00                 // Sensor Capabilities -- Manual Rearm
   04                 // Sensor Type - Fan
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Mask
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS1 1a Fan Fail'  // String Bytes


//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PS1_1200W'
_SDR_TAG    'PS1_1600WAC'
_SDR_TAG    'PS1_1600WDC'
_REC_LEN    002F

   // Sensor Record Header
   0061               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   A1                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0E                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   00                 // Sensor Capabilities -- Manual Rearm
   04                 // Sensor Type - Fan
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Mask
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS1 1b Fan Fail'  // String Bytes


//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PS2_1200W'
_SDR_TAG    'PS2_1600WAC'
_SDR_TAG    'PS2_1600WDC'
_REC_LEN    002F

   // Sensor Record Header
   0062               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   A4                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0F                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   00                 // Sensor Capabilities -- Manual Rearm
   04                 // Sensor Type - Fan
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Mask
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS2 1a Fan Fail'  // String Bytes


//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PS2_1200W'
_SDR_TAG    'PS2_1600WAC'
_SDR_TAG    'PS2_1600WDC'
_REC_LEN    002F

   // Sensor Record Header
   0063               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   A5                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   10                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   00                 // Sensor Capabilities -- Manual Rearm
   04                 // Sensor Type - Fan
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Mask
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS2 1b Fan Fail'  // String Bytes


//====================================================================//
// Memory thermal margin sensors
//====================================================================//
_SDR_TYPE   01
_REC_LEN    0040

   // Sensor Record Header
   0064               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   B0                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   EC                 // Normal Reading(ECh = -20 degrees C)
   00                 // Normal Maximum (00h = 0 degrees C)
   BA                 // Normal Minimum (BAh = -70 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degrees C)
   0A                 // Upper critical (0Ah = 10 degrees C)
   05                 // Upper non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degrees C)
   00                 // Lower critical (00h = 0 degrees C)
   00                 // Lower non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   D0                 // Type/Length Code
   'DIMM Thrm Mrgn 1' // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'OTHER'
_SDR_TAG    'FCT'
_REC_LEN    0040

   // Sensor Record Header
   0065               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   B1                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   EC                 // Normal Reading(ECh = -20 degrees C)
   00                 // Normal Maximum (00h = 0 degrees C)
   BA                 // Normal Minimum (BAh = -70 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degrees C)
   0A                 // Upper critical (0Ah = 10 degrees C)
   05                 // Upper non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degrees C)
   00                 // Lower critical (00h = 0 degrees C)
   00                 // Lower non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   D0                 // Type/Length Code
   'DIMM Thrm Mrgn 2' // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0040

   // Sensor Record Header
   0066               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   B2                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   EC                 // Normal Reading(ECh = -20 degrees C)
   00                 // Normal Maximum (00h = 0 degrees C)
   BA                 // Normal Minimum (BAh = -70 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degrees C)
   0A                 // Upper critical (0Ah = 10 degrees C)
   05                 // Upper non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degrees C)
   00                 // Lower critical (00h = 0 degrees C)
   00                 // Lower non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   D0                 // Type/Length Code
   'DIMM Thrm Mrgn 3' // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0040

   // Sensor Record Header
   0067               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   B3                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask   --[u][c,nc]=8002
   8032               // Deassertion Event Mask --[u][c,nc]=8032
   1818               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=1818
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   EC                 // Normal Reading(ECh = -20 degrees C)
   00                 // Normal Maximum (00h = 0 degrees C)
   BA                 // Normal Minimum (BAh = -70 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degrees C)
   0A                 // Upper critical (0Ah = 10 degrees C)
   05                 // Upper non-critical (05h = 5 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degrees C)
   00                 // Lower critical (00h = 0 degrees C)
   00                 // Lower non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   D0                 // Type/Length Code
   'DIMM Thrm Mrgn 4' // String Bytes


//====================================================================//
_SDR_TYPE   02
_REC_LEN    002D

   // Sensor Record Header
   0068               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   B8                 // Sensor Number

   // Record Body Bytes
   15                 // Entity ID
   03                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   09                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask --State asserted =0200
   0200               // Reading Mask & Settable / Readable Threshold Masks --State asserted =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Auto Shutdown'    // String Bytes


//====================================================================//
// Memory thermal trip sensors
//====================================================================//
_SDR_TYPE   02
_REC_LEN    0030

   // Sensor Record Header
   0069               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   C0                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   0C                 // Sensor Type
   6F                 // Event / Reading Base Type
   0004               // Assertion Event Mask   --State asserted=0004
   0004               // Deassertion Event Mask --State asserted=0004
   0004               // Reading Mask & Settable / Readable Threshold Masks --State asserted=0004
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'Mem P1 Thrm Trip' // String Bytes


//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0030

   // Sensor Record Header
   006A               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   C1                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   0C                 // Sensor Type
   6F                 // Event / Reading Base Type
   0004               // Assertion Event Mask   --State asserted=0004
   0004               // Deassertion Event Mask --State asserted=0004
   0004               // Reading Mask & Settable / Readable Threshold Masks --State asserted=0004
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'Mem P2 Thrm Trip' // String Bytes


//====================================================================//
// Global aggregate thermal margin sensors
//====================================================================//
_SDR_TYPE   01
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    003E

   // Sensor Record Header
   006B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   C8                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask   --[u][c,nc]=0000
   0000               // Deassertion Event Mask --[u][c,nc]=0000
   0000               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=0000
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   EC                 // Normal Reading(ECh = -20 degrees C)
   00                 // Normal Maximum (00h = 0 degrees C)
   BA                 // Normal Minimum (BAh = -70 degrees C)
   //------------------------------------------------------------------//
   7F                 // Sensor Maximum Reading (7Fh = 127 degrees C)
   80                 // Sensor Minimum Reading (80h = -128 degrees C)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 degrees C)
   00                 // Upper critical (00h = 0 degrees C)
   00                 // Upper non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 degrees C)
   00                 // Lower critical (00h = 0 degrees C)
   00                 // Lower non-critical (00h = 0 degrees C)
   //------------------------------------------------------------------//
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   27                 // OEM used for filtering [7:5]= 1 Median [4:0]=7 Sample Count
   CE                 // Type/Length Code
   'Agg Thrm Mgn 1'   // String Bytes


//====================================================================//
// Voltage regulator sensors
//====================================================================//
_SDR_TYPE   01
_REC_LEN    0037

   // Sensor Record Header
   006C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   32                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D0                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask     --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   34                 // M
   00                 // M, Tolerance
   1F                 // B
   40                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   D0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E0                 // Normal Reading (E0h = 11.93 Volt)
   EC                 // Normal Maximum (ECh = 12.56 Volt)
   D5                 // Normal Minimum (D5h = 11.36 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 13.39 Volt)
   00                 // Sensor Minimum Reading (00h = 0.13 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0.13 Volt)
   FC                 // Upper critical (FCh = 13.23 Volt)
   F5                 // Upper non-critical (F5h = 12.87 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0.13 Volt)
   C7                 // Lower critical (C7h = 10.74 Volt)
   CD                 // Lower non-critical (CDh = 11.05 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C7                 // Type/Length Code
   'BB P12V'          // String Bytes


//====================================================================//
_SDR_TYPE   01
_REC_LEN    0038

   // Sensor Record Header
   006D               // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D2                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask     --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   8F                 // M
   00                 // M, Tolerance
   F6                 // B
   40                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E2                 // Normal Reading (E2h = 4.98 Volt)
   EE                 // Normal Maximum (EEh = 5.24 Volt)
   D7                 // Normal Minimum (D7h = 4.74 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 5.57 Volt)
   00                 // Sensor Minimum Reading (00h = 0.03 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0.03 Volt)
   FC                 // Upper critical (FCh = 5.50 Volt)
   F5                 // Upper non-critical (F5h = 5.35 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0.03 Volt)
   CB                 // Lower critical (CBh = 4.50 Volt)
   D1                 // Lower non-critical (D7h = 4.63 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C8                 // Type/Length Code
   'BB P3_3V'         // String Bytes


//====================================================================//
_SDR_TYPE   01
_REC_LEN    003B

   // Sensor Record Header
   006E               // Record ID
   51                 // SDR Version
   01                 // Record Type
   36                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D3                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask     --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   D9                 // M
   00                 // M, Tolerance
   62                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E1                 // Normal Reading (E1h = 3.28 Volt)
   ED                 // Normal Maximum (EDh = 3.45 Volt)
   D6                 // Normal Minimum (D6h = 3.12 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 3.65 Volt)
   00                 // Sensor Minimum Reading (00h = 0.01 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0.01 Volt)
   FC                 // Upper critical (FCh = 3.61 Volt)
   F5                 // Upper non-critical (F5h = 3.51 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0.01 Volt)
   C9                 // Lower critical (C9h = 2.98 Volt)
   CF                 // Lower non-critical (CFh = 3.07 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'BB P5V STBY'      // String Bytes


//====================================================================//
_SDR_TYPE   01
_REC_LEN    0039

   // Sensor Record Header
   006F               // Record ID
   51                 // SDR Version
   01                 // Record Type
   34                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D6                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3C                 // M
   00                 // M, Tolerance
   C1                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   B1                 // Normal Reading (B1h = 1.05 Volt)
   EF                 // Normal Maximum (EFh = 1.42 Volt)
   62                 // Normal Minimum (73h = 0.68 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.50 Volt)
   00                 // Sensor Minimum Reading (00h = -0.01 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = -0.01 Volt)
   FC                 // Upper critical (FCh = 1.48 Volt)
   F5                 // Upper non-critical (F5h = 1.44 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = -0.01 Volt)
   5C                 // Lower critical (6Dh = 0.66 Volt)
   5F                 // Lower non-critical (70h = 0.67 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'BB P1 Vcc'        // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0039

   // Sensor Record Header
   0070               // Record ID
   51                 // SDR Version
   01                 // Record Type
   34                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D7                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7B                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3C                 // M
   00                 // M, Tolerance
   C1                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   B1                 // Normal Reading (B1h = 1.05 Volt)
   EF                 // Normal Maximum (EFh = 1.42 Volt)
   62                 // Normal Minimum (73h = 0.68 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.50 Volt)
   00                 // Sensor Minimum Reading (00h = -0.01 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = -0.01 Volt)
   FC                 // Upper critical (FCh = 1.48 Volt)
   F5                 // Upper non-critical (F5h = 1.44 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = -0.01 Volt)
   5C                 // Lower critical (6Dh = 0.66 Volt)
   5F                 // Lower non-critical (70h = 0.67 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'BB P2 Vcc'        // String Bytes


//====================================================================//
_SDR_TYPE      01
_REC_LEN       0040

   // Sensor Record Header
   0071               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D8                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   44                 // M
   00                 // M, Tolerance
   C9                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E4                 // Normal Reading (E4h = 1.50 Volt)
   EF                 // Normal Maximum (EFh = 1.57 Volt)
   D9                 // Normal Minimum (D9h = 1.42 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.65 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.63 Volt)
   F5                 // Upper non-critical (F5h = 1.59 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CD                 // Lower critical (CDh = 1.37 Volt)
   D4                 // Lower non-critical (D4h = 1.41 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.5 P1DDR AB' // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'OTHER'
_SDR_TAG    'FCT'
_REC_LEN    0040

   // Sensor Record Header
   0072               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D9                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask     --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   44                 // M
   00                 // M, Tolerance
   C9                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E4                 // Normal Reading (E4h = 1.50 Volt)
   EF                 // Normal Maximum (EFh = 1.57 Volt)
   D9                 // Normal Minimum (D9h = 1.42 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.65 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.63 Volt)
   F5                 // Upper non-critical (F5h = 1.59 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CD                 // Lower critical (CDh = 1.37 Volt)
   D4                 // Lower non-critical (D4h = 1.41 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.5 P1DDR CD' // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0040

   // Sensor Record Header
   0073               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   DA                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask     --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   44                 // M
   00                 // M, Tolerance
   C9                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E4                 // Normal Reading (E4h = 1.50 Volt)
   EF                 // Normal Maximum (EFh = 1.57 Volt)
   D9                 // Normal Minimum (D9h = 1.42 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.65 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.63 Volt)
   F5                 // Upper non-critical (F5h = 1.59 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CD                 // Lower critical (CDh = 1.37 Volt)
   D4                 // Lower non-critical (D4h = 1.41 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.5 P2DDR AB' // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0040

   // Sensor Record Header
   0074               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   DB                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask     --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   44                 // M
   00                 // M, Tolerance
   C9                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E4                 // Normal Reading (E4h = 1.50 Volt)
   EF                 // Normal Maximum (EFh = 1.57 Volt)
   D9                 // Normal Minimum (D9h = 1.42 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.65 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.63 Volt)
   F5                 // Upper non-critical (F5h = 1.59 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CD                 // Lower critical (CDh = 1.37 Volt)
   D4                 // Lower non-critical (D4h = 1.41 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.5 P2DDR CD' // String Bytes


//====================================================================//
_SDR_TYPE   01
_REC_LEN    003C

   // Sensor Record Header
   0075               // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   DC                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask     --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   53                 // M
   00                 // M, Tolerance
   7C                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E9                 // Normal Reading (E9h = 1.50 Volt)
   EF                 // Normal Maximum (EFh = 1.57 Volt)
   E2                 // Normal Minimum (E2h = 1.42 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.65 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.63 Volt)
   F5                 // Upper non-critical (F5h = 1.59 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   D6                 // Lower critical (D6h = 1.37 Volt)
   DD                 // Lower non-critical (DDh = 1.41 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'BB P1_8V AUX'     // String Bytes


//====================================================================//
_SDR_TYPE   01
_REC_LEN    003B

   // Sensor Record Header
   0076               // Record ID
   51                 // SDR Version
   01                 // Record Type
   36                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   DD                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask     --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   D7                 // M
   40                 // M, Tolerance
   3F                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   B1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E8                 // Normal Reading (E8h = 1.80 Volt)
   EF                 // Normal Maximum (EFh = 1.85 Volt)
   E1                 // Normal Minimum (E1h = 1.74 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.95 Volt)
   00                 // Sensor Minimum Reading (00h = -0.01 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = -0.01 Volt)
   FC                 // Upper critical (FCh = 1.93 Volt)
   F5                 // Upper non-critical (F5h = 1.87 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = -0.01 Volt)
   D6                 // Lower critical (D6h = 1.67 Volt)
   DC                 // Lower non-critical (DCh = 1.73 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'BB +1.1V SB'      // String Bytes


//====================================================================//
_SDR_TYPE   01
_REC_LEN    003D

   // Sensor Record Header
   0077               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   DF                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask     --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   8F                 // M
   00                 // M, Tolerance
   F6                 // B
   40                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E2                 // Normal Reading (E2h = 1.10 Volt)
   EE                 // Normal Maximum (EEh = 1.13 Volt)
   D7                 // Normal Minimum (D7h = 1.07 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.19 Volt)
   00                 // Sensor Minimum Reading (00h = -0.01 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = -0.01 Volt)
   FC                 // Upper critical (FCh = 1.18 Volt)
   F5                 // Upper non-critical (F5h = 1.15 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = -0.01 Volt)
   CB                 // Lower critical (CBh = 1.02 Volt)
   D1                 // Lower non-critical (D1h = 1.06 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'BB P3_3V STBY'    // String Bytes


//====================================================================//
_SDR_TYPE   01
_REC_LEN    0040

   // Sensor Record Header
   0078               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   E4                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask     --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3D                 // M
   00                 // M, Tolerance
   15                 // B
   80                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E4                 // Normal Reading (E4h = 1.36 Volt)
   EF                 // Normal Maximum (EFh = 1.42 Volt)
   D9                 // Normal Minimum (D9h = 1.29 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.50 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.48 Volt)
   F5                 // Upper non-critical (F5h = 1.44 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CD                 // Lower critical (CDh = 1.24 Volt)
   D4                 // Lower non-critical (D4h = 1.28 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM used for filtering [7:5]= 1 Median [4:0]=5 Sample Count
   D0                 // Type/Length Code
   'BB +1.35 P1LV AB' // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'OTHER'
_SDR_TAG    'FCT'
_REC_LEN    0040

   // Sensor Record Header
   0079               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   E5                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask     --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3D                 // M
   00                 // M, Tolerance
   15                 // B
   80                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E4                 // Normal Reading (E4h = 1.36 Volt)
   EF                 // Normal Maximum (EFh = 1.42 Volt)
   D9                 // Normal Minimum (D9h = 1.29 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.50 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.48 Volt)
   F5                 // Upper non-critical (F5h = 1.44 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CD                 // Lower critical (CDh = 1.24 Volt)
   D4                 // Lower non-critical (D4h = 1.28 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.35 P1LV CD' // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0040

   // Sensor Record Header
   007A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   E6                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask     --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3D                 // M
   00                 // M, Tolerance
   15                 // B
   80                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E4                 // Normal Reading (E4h = 1.36 Volt)
   EF                 // Normal Maximum (EFh = 1.42 Volt)
   D9                 // Normal Minimum (D9h = 1.29 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.50 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.48 Volt)
   F5                 // Upper non-critical (F5h = 1.44 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CD                 // Lower critical (CDh = 1.24 Volt)
   D4                 // Lower non-critical (D4h = 1.28 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.35 P2LV AB' // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0040

   // Sensor Record Header
   007B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   E7                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   3E                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask     --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   3D                 // M
   00                 // M, Tolerance
   15                 // B
   80                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E4                 // Normal Reading (E4h = 1.36 Volt)
   EF                 // Normal Maximum (EFh = 1.42 Volt)
   D9                 // Normal Minimum (D9h = 1.29 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.50 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.48 Volt)
   F5                 // Upper non-critical (F5h = 1.44 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CD                 // Lower critical (CDh = 1.24 Volt)
   D4                 // Lower non-critical (D4h = 1.28 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB +1.35 P2LV CD' // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'IB_FDR'
_SDR_TAG    'IB_QDR'
_SDR_TAG    'IB_10G'
_SDR_TAG    'SHIP'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003F

   // Sensor Record Header
   007C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   EC                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask     --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   B7                 // M
   40                 // M, Tolerance
   71                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   B1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   D0                 // Normal Reading (E6h = 1.36 Volt)
   EF                 // Normal Maximum (FFh = 1.42 Volt)
   C6                 // Normal Minimum (DDh = 1.29 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.50 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.48 Volt)
   F5                 // Upper non-critical (F5h = 1.44 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   BB                 // Lower critical (D2h = 1.24 Volt)
   C1                 // Lower non-critical (D8h = 1.28 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'BB 0_9V_IB CORE'  // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'IB_FDR'
_SDR_TAG    'IB_QDR'
_SDR_TAG    'IB_10G'
_SDR_TAG    'SHIP'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003E

   // Sensor Record Header
   007D               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   ED                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask     --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   52                 // M
   00                 // M, Tolerance
   BF                 // B
   C0                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E4                 // Normal Reading (E6h = 1.36 Volt)
   EF                 // Normal Maximum (FFh = 1.42 Volt)
   D9                 // Normal Minimum (DDh = 1.29 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.50 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.48 Volt)
   F5                 // Upper non-critical (F5h = 1.44 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CE                 // Lower critical (D2h = 1.24 Volt)
   D4                 // Lower non-critical (D8h = 1.28 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'BB 1_8V IB I/O'   // String Bytes


//====================================================================//
_SDR_TYPE   01
_REC_LEN    003B

   // Sensor Record Header
   007E               // Record ID
   51                 // SDR Version
   01                 // Record Type
   36                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   EE                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask     --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   D7                 // M
   40                 // M, Tolerance
   3F                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   B1                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E8                 // Normal Reading (E8h = 1.36 Volt)
   EF                 // Normal Maximum (EFh = 1.42 Volt)
   E1                 // Normal Minimum (E1h = 1.29 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.50 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.48 Volt)
   F5                 // Upper non-critical (F5h = 1.44 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   D6                 // Lower critical (D6h = 1.24 Volt)
   DC                 // Lower non-critical (DCh = 1.28 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'BB 1_1V PCH'      // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'IB_FDR'
_SDR_TAG    'IB_QDR'
_SDR_TAG    'IB_10G'
_SDR_TAG    'SHIP'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    0040

   // Sensor Record Header
   007F               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   EF                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask     --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask   --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   34                 // M
   00                 // M, Tolerance
   B7                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   //------------------------------------------------------------------//
   E3                 // Normal Reading (E6h = 1.36 Volt)
   EE                 // Normal Maximum (EFh = 1.42 Volt)
   D7                 // Normal Minimum (DDh = 1.29 Volt)
   //------------------------------------------------------------------//
   FF                 // Sensor Maximum Reading (FFh = 1.50 Volt)
   00                 // Sensor Minimum Reading (00h = 0 Volt)
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (00h = 0 Volt)
   FC                 // Upper critical (FCh = 1.48 Volt)
   F5                 // Upper non-critical (F5h = 1.44 Volt)
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (00h = 0 Volt)
   CB                 // Lower critical (D1h = 1.24 Volt)
   D1                 // Lower non-critical (D8h = 1.28 Volt)
   //------------------------------------------------------------------//
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'BB 1_2V IB OTHER' // String Bytes


//====================================================================//
// Hot-swap backplane (HSBP) sensors
//====================================================================//
_SDR_TYPE   02
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    002C

   // Sensor Record Header
   0080               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F0                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   02                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 0 Status'     // String Bytes


//====================================================================//
_SDR_TYPE   02
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    002C

   // Sensor Record Header
   0081               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F1                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   03                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 1 Status'     // String Bytes


//====================================================================//
_SDR_TYPE   02
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    002C

   // Sensor Record Header
   0082               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F2                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   04                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 2 Status'     // String Bytes


//====================================================================//
_SDR_TYPE   02
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    002C

   // Sensor Record Header
   0083               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F3                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   05                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   AF01               // Assertion Event Mask
   AF01               // Deassertion Event Mask
   FF1F               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 3 Status'     // String Bytes


//====================================================================//
// Management Engine (ME controller) records
//====================================================================//
_SDR_TYPE   03
_REC_LEN    001E

   // Sensor Record Header
   0084               // Record ID
   51                 // SDR Version
   03                 // Record Type
   19                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   17                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   01                 // Entity Instance
   DC                 // Sensor type
   75                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'SPS FW Health'    // String Bytes


//====================================================================//
_SDR_TYPE   03
_REC_LEN    001D

   // Sensor Record Header
   0085               // Record ID
   51                 // SDR Version
   03                 // Record Type
   18                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   18                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   01                 // Entity Instance
   DC                 // Sensor type
   72                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'NM Exception'     // String Bytes


//====================================================================//
_SDR_TYPE   03
_REC_LEN    001A

   // Sensor Record Header
   0086               // Record ID
   51                 // SDR Version
   03                 // Record Type
   15                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   19                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   01                 // Entity Instance
   DC                 // Sensor type
   73                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'NM Health'        // String Bytes


//====================================================================//
_SDR_TYPE   02
_REC_LEN    002F

   // Sensor Record Header
   0087               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   1A                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   01                 // Entity Instance
   41                 // Sensor Initialization
   C3                 // Sensor Capabilities
   DC                 // Sensor Type
   74                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0700               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0000               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'NM Capabilities'  // String Bytes


//====================================================================//
_SDR_TYPE   03
_REC_LEN    001D

   // Sensor Record Header
   0088               // Record ID
   51                 // SDR Version
   03                 // Record Type
   18                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Channel Number / Sensor Owner LUN
   1B                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   01                 // Entity Instance
   DC                 // Sensor Type
   72                 // Event / Reading Base Type
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'NM Threshold'     // String Bytes


//====================================================================//
_SDR_TYPE      C0
_REC_LEN       0010

   // Sensor Record Header
   0089               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0B                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0D                 // Record subtype - NM Discovery
   01                 // Version number of record subtype
   2C                 // NM Device Slave Address ([7:1] - 7-bit address; [0] - reserved)
   60                 // [7:4] - channel number (6 for secondary IPMB) [3:2] - reserved [1:0] - sensor owner LUN)
   19                 // Node Manager Health Event sensor
   18                 // Node Manager Exception Event sensor
   1A                 // Node Manager Operational Capabilities sensor
   1B                 // Node Manager Threshold Exceeded sensor


//====================================================================//
_SDR_TYPE   01
_REC_LEN    0036

   // Sensor Record Header
   008A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   31                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   34                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   63                 // Sensor Initialization
   B8                 // Sensor Capabilities
   0C                 // Sensor Type -- Memory
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask   --[u][c,nc]=0000
   0000               // Deassertion Event Mask --[u][c,nc]=0000
   3F3F               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=0000
   01                 // Sensor Units 1
   00                 // Sensor Units 2 -- Degrees C
   00                 // Sensor Units 3
   00                 // Linearization
   05                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   F0                 // R exp, B exp
   00                 // Analog characteristic flags
   //------------------------------------------------------------------//
   00                 // Normal Reading
   00                 // Normal Maximum
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   00                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical
   00                 // Upper non-critical
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C6                 // Type/Length Code
   'P1 MTT'           // String Bytes


//====================================================================//
_SDR_TYPE   01
_SDR_TAG    'PROCESSOR_2'
_SDR_TAG    'FCT'
_REC_LEN    0036

   // Sensor Record Header
   008B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   31                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   35                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   02                 // Entity Instance
   63                 // Sensor Initialization
   B8                 // Sensor Capabilities
   0C                 // Sensor Type -- Memory
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask   --[u][c,nc]=0000
   0000               // Deassertion Event Mask --[u][c,nc]=0000
   3F3F               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=0000
   01                 // Sensor Units 1
   00                 // Sensor Units 2 -- Degrees C
   00                 // Sensor Units 3
   00                 // Linearization
   05                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   F0                 // R exp, B exp
   00                 // Analog characteristic flags
   //------------------------------------------------------------------//
   00                 // Normal Reading
   00                 // Normal Maximum
   00                 // Normal Minimum
   //------------------------------------------------------------------//
   00                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   //------------------------------------------------------------------//
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical
   00                 // Upper non-critical
   //------------------------------------------------------------------//
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   //------------------------------------------------------------------//
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C6                 // Type/Length Code
   'P2 MTT'           // String Bytes


//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PS1_750W'
_SDR_TAG    'PS1_1200W'
_SDR_TAG    'PS1_1600WAC'
_SDR_TAG    'PS1_1600WDC'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    002B

   // Sensor Record Header
   008C               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   66                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   27                 // Sensor Initialization
   40                 // Sensor Capabilities
   08                 // Sensor Type
   6F                 // Event / Reading Base Type
   2000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   2000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0000               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'PSU1 Status'      // String Bytes


//====================================================================//
_SDR_TYPE   02
_SDR_TAG    'PS2_750W'
_SDR_TAG    'PS2_1200W'
_SDR_TAG    'PS2_1600WAC'
_SDR_TAG    'PS2_1600WDC'
_SDR_TAG    'FCT'
_REC_LEN    002B

   // Sensor Record Header
   008D               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   67                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   27                 // Sensor Initialization
   40                 // Sensor Capabilities
   08                 // Sensor Type
   6F                 // Event / Reading Base Type
   2000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   2000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0000               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'PSU2 Status'      // String Bytes


//====================================================================//
// SDR Type 03 - Event Only Record for BIOS Boot Events
//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   008E               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   01                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   01                 // Entity Instance
   0C                 // Sensor Type
   0B                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mem Rdnc Sensor'  // Mirroring Redundancy State


//=========================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   008F               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   02                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID = Memory
   01                 // Entity Instance
   0C                 // Sensor Type
   09                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mem Conf Sensor'  // Memory RAS Configuration Status


//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   0090               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   02                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID = Memory Device
   02                 // Entity Instance
   0C                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mmry ECC Sensor'  // Memory ECC Error


//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   0091               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   03                 // Sensor Number

   // Record Body Bytes
   30                 // Entity ID = PCI
   01                 // Entity Instance
   13                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCI Lgcy Sensor'  // Legacy PCI Error


//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   0092               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   04                 // Sensor Number

   // Record Body Bytes
   31                 // Entity ID = PCI Express
   01                 // Entity Instance
   13                 // Sensor Type
   70                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCIe Fat Sensor'  // PCIe Fatal Error (see Sensor 14h for continuation)


//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   0093               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   05                 // Sensor Number

   // Record Body Bytes
   31                 // Entity ID = PCI Express
   02                 // Entity Instance
   13                 // Sensor Type
   71                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCIe Cor Sensor'  // PCIe Correctable Error


//=========================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   0094               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   06                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID-BIOS POST
   02                 // Entity Instance
   0F                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'POST Err Sensor'  // BIOS POST Error


//=========================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   0095               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   06                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID
   03                 // Entity Instance
   13                 // Sensor Type
   72                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'QPI Corr Sensor'  // QPI Correctable Errors


//=========================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   0096               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   07                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID
   04                 // Entity Instance
   13                 // Sensor Type
   73                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'QPI Fatl Sensor'  // QPI Fatal Error (see Sensor 17h for continuation)


//====================================================================//
_SDR_TYPE   03
_REC_LEN    001F

   // Sensor Record Header
   0097               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1A                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   08                 // Sensor Number

   // Record Body Bytes
   31                 // Entity ID = PCI Express
   03                 // Entity Instance
   19                 // Sensor Type
   75                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Chipset Sensor'   // Chipset Proprietary


//=========================================================================//
_SDR_TYPE   03
_REC_LEN    001F

   // Sensor Record Header
   0098               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1A                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   09                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID
   05                 // Entity Instance
   13                 // Sensor Type
   77                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'QPI Link Width'   // QPI Link Width Reduced


//====================================================================//
_SDR_TYPE   03
_REC_LEN    001F

   // Sensor Record Header
   0099               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1A                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   10                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID = Memory Device
   03                 // Entity Instance
   0C                 // Sensor Type
   7F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Mem err Sensor'   // Memory Error Extension


//====================================================================//
_SDR_TYPE   03
_REC_LEN    001D

   // Sensor Record Header
   009A               // Record ID
   51                 // SDR Version
   03                 // Record Type
   18                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   11                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   06                 // Entity Instance
   0C                 // Sensor Type
   0B                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'Sparing Rdnc'     // Sparing Redundancy State


//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   009B               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   12                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   07                 // Entity Instance
   0C                 // Sensor Type
   09                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Rdnc Mod Sensor'  // Memory RAS Mode Select


//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   009C               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   13                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID = Memory Device
   04                 // Entity Instance
   0C                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mmry Parity Err'  // Memory Parity Error


//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   009D               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   14                 // Sensor Number

   // Record Body Bytes
   31                 // Entity ID = PCI Express
   04                 // Entity Instance
   13                 // Sensor Type
   76                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCIe Fat Sensor'  // PCIe Fatal Error#2 (continuation of Sensor 04h)


//=========================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   009E               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   17                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID
   08                 // Entity Instance
   13                 // Sensor Type
   74                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'QPI Fatl Sensor'  // OPI Fatal Error (continuation of Sensor 07h)


//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   009F               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   83                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   09                 // Entity Instance
   12                 // Sensor Type
   6F                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'BIOS Evt Sensor'  // System Event


//====================================================================//
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   00A0               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   83                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   0A                 // Entity Instance
   12                 // Sensor Type
   6F                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'BIOS Evt Sensor'  // System Event


//====================================================================//
// SDR Type 11 Records
//====================================================================//
_SDR_TYPE   11
_REC_LEN    0019

   // Sensor Record Header
   00A1               // Record ID
   51                 // SDR Version
   11                 // Record Type
   14                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   00                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   07                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // OEM
   C9                 // Type/Length Code
   'Baseboard'        // String Bytes


//====================================================================//
_SDR_TYPE   11
_SDR_TAG    'PS1_750W'
_SDR_TAG    'PS1_1200W'
_SDR_TAG    'PS1_1600WAC'
_SDR_TAG    'PS1_1600WDC'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    0020
 
   // Sensor Record Header
   00A2               // Record ID
   51                 // SDR Version
   11                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   02                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   0A                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // Reserved for OEM use
   D0                 // Type/Length Code
   'Pwr Supply 1 FRU' // String Bytes


//====================================================================//
_SDR_TYPE   11
_SDR_TAG    'PS2_750W'
_SDR_TAG    'PS2_1200W'
_SDR_TAG    'PS2_1600WAC'
_SDR_TAG    'PS2_1600WDC'
_SDR_TAG    'FCT'
_REC_LEN    0020

   // Sensor Record Header
   00A3               // Record ID
   51                 // SDR Version
   11                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   03                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   0A                 // FRU Entity ID
   02                 // FRU Entity Instance
   00                 // Reserved for OEM use
   D0                 // Type/Length Code
   'Pwr Supply 2 FRU' // String Bytes


//====================================================================//
_SDR_TYPE   11
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_SDR_TAG    'FCT'
_REC_LEN    001C

   // Sensor Record Header
   00A4               // Record ID
   51                 // SDR Version
   11                 // Record Type
   17                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   08                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   0F                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // OEM
   CC                 // Type/Length Code
   'HS Backplane'     // String Bytes


//====================================================================//
// SDR Type 12 Records
//====================================================================//
_SDR_TYPE   12
_REC_LEN    0020

   // Sensor Record Header
   00A5               // Record ID
   51                 // SDR Version
   12                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   20                 // Device Slave Address
   00                 // Channel Number

   // Record Body Bytes
   08                 // Power state notification
   BF                 // Device capabilities
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   07                 // Entity ID
   01                 // Entity instance
   00                 // OEM
   D0                 // Type/Length Code
   'Basbrd Mgmt Ctlr' // String Bytes


//====================================================================//
_SDR_TYPE   12
_REC_LEN    0012

   // Sensor Record Header
   00A6               // Record ID
   51                 // SDR Version
   12                 // Record Type
   0D                 // Record Length

   // Record Key Bytes
   2C                 // Device Slave Address
   06                 // Channel number

   // Record Body Bytes
   24                 // Power State Notification
   21                 // Device Capabilities
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   2E                 // Entity ID
   01                 // Entity Instance
   00                 // OEM
   C2                 // Type/Length Code
   'ME'               // String Bytes


//====================================================================//
// Thermal Profile Data, Close Loop
//====================================================================//


//====================================================================//
// SDR Type C0/02 Record For Power Unit Map
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'REDUNDANT_PS'
_SDR_TAG    'FCT'
_REC_LEN    000E

   // Sensor Record Header
   00A7               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   09                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   02                 // Record Subtype Value
   02                 // Power Unit Redundancy sensor number
   00                 // Bits[7:1]: Reserved; Bit[0]: 1=No monitorable supplies present
   01                 // The number of present and operational
   50                 // Power Supply Status 1 Sensor Number
   51                 // Power Supply Status 2 Sensor Number


//====================================================================//
// SDR Type C0/09 Records For Voltage Sensor Scaling
//====================================================================//
_SDR_TYPE   C0
_REC_LEN    002E

   // Sensor Record Header
   00A8               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   29                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   09                 // Record Subtype Value - Voltage Sensor Scaling

   // Voltage Sensor Scaling Record
   0C                 // Number of entries following
   D0                 // Voltage Sensor Number
   B80A               // Scale Factor (LSB MSB)
   D2                 // Voltage Sensor Number
   980A               // Scale Factor (LSB MSB)
   D3                 // Voltage Sensor Number
   9D0A               // Scale Factor (LSB MSB)
   D6                 // Voltage Sensor Number
   1A10               // Scale Factor (LSB MSB)
   D7                 // Voltage Sensor Number
   1A10               // Scale Factor (LSB MSB)
   D8                 // Voltage Sensor Number
   7F0E               // Scale Factor (LSB MSB)
   D9                 // Voltage Sensor Number
   7F0E               // Scale Factor (LSB MSB)
   DA                 // Voltage Sensor Number
   7F0E               // Scale Factor (LSB MSB)
   DB                 // Voltage Sensor Number
   7F0E               // Scale Factor (LSB MSB)
   DC                 // Voltage Sensor Number
   510C               // Scale Factor (LSB MSB)
   DD                 // Voltage Sensor Number
   2214               // Scale Factor (LSB MSB)
   DF                 // Voltage Sensor Number
   980A               // Scale Factor (LSB MSB)


//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0022

   // Sensor Record Header
   00A9               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1D                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   09                 // Record Subtype Value - Voltage Sensor Scaling

   // Voltage Sensor Scaling Record
   08                 // Number of entries following
   E4                 // Voltage Sensor Number
   1A10               // Scale Factor (LSB MSB)
   E5                 // Voltage Sensor Number
   1A10               // Scale Factor (LSB MSB)
   E6                 // Voltage Sensor Number
   1A10               // Scale Factor (LSB MSB)
   E7                 // Voltage Sensor Number
   1A10               // Scale Factor (LSB MSB)
   EC                 // Voltage Sensor Number
   0916               // Scale Factor (LSB MSB)
   ED                 // Voltage Sensor Number
   150C               // Scale Factor (LSB MSB)
   EE                 // Voltage Sensor Number
   2214               // Scale Factor (LSB MSB)
   EF                 // Voltage Sensor Number
   4518               // Scale Factor (LSB MSB)


//====================================================================//
// SDR Type C0/0A Records For Fan Sensor Scaling SDR Record
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_REC_LEN    0023

   // Sensor Record Header
   00AA               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record Subtype Value - Fan Sensor Scaling SDR Record

   // Fan Sensor Scaling Record
   00                 // Return Format; Bit 0=Fan 0, Bit 1=Fan 1; etc. 0=RPM, 1=Period(***TBD***)
   00                 // Number of tach Pulses Per Revolution: Bit 0=Fan 0, Bit 1=Fan 1, etc.; 0=2 Pulses/Rev, 1=1 Pulse/Rev(***TBD***)
   9853               // Placeholder for System Fan 1a(SN:0x30), Max RPM: 21400RPM == 9853 (the order is LSB, MSB)
   5456               // Placeholder for System Fan 1b(SN:0x31), Max RPM: 22100RPM == 5456 (the order is LSB, MSB)
   9853               // Placeholder for System Fan 2a(SN:0x32), Max RPM: 21400RPM == 9853 (the order is LSB, MSB)
   5456               // Placeholder for System Fan 2b(SN:0x33), Max RPM: 22100RPM == 5456 (the order is LSB, MSB)
   9853               // Placeholder for System Fan 3a(SN:0x34), Max RPM: 21400RPM == 9853 (the order is LSB, MSB)
   5456               // Placeholder for System Fan 3b(SN:0x35), Max RPM: 22100RPM == 5456 (the order is LSB, MSB)
   0001               // Placeholder for System Fan 4a(SN:0x36), Max RPM: 256RPM == 0001 (the order is LSB, MSB)
   0001               // Placeholder for System Fan 4b(SN:0x37), Max RPM: 256RPM == 0001 (the order is LSB, MSB)
   0001               // Placeholder for System Fan 5a(SN:0x38), Max RPM: 256RPM == 0001 (the order is LSB, MSB)
   0001               // Placeholder for System Fan 5b(SN:0x39), Max RPM: 256RPM == 0001 (the order is LSB, MSB)
   0001               // Placeholder for System Fan 6a(SN:0x3A), Max RPM: 256RPM == 0001 (the order is LSB, MSB)
   0001               // Placeholder for System Fan 6b(SN:0x3B), Max RPM: 256RPM == 0001 (the order is LSB, MSB)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0023

   // Sensor Record Header
   00AB               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record Subtype Value - Fan Sensor Scaling SDR Record

   // Fan Sensor Scaling Record
   00                 // Return Format; Bit 0=Fan 0, Bit 1=Fan 1; etc. 0=RPM, 1=Period(***TBD***)
   00                 // Number of tach Pulses Per Revolution: Bit 0=Fan 0, Bit 1=Fan 1, etc.; 0=2 Pulses/Rev, 1=1 Pulse/Rev(***TBD***)
   A861               // Placeholder for System Fan 1a(SN:0x30), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 1b(SN:0x31), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 2a(SN:0x32), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 2b(SN:0x33), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 3a(SN:0x34), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 3b(SN:0x35), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 4a(SN:0x36), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 4b(SN:0x37), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 5a(SN:0x38), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 5b(SN:0x39), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 6a(SN:0x3A), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 6b(SN:0x3B), Max RPM: 25000RPM == A861 (the order is LSB, MSB)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    0023

   // Sensor Record Header
   00AC               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   1E                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record Subtype Value - Fan Sensor Scaling SDR Record

   // Fan Sensor Scaling Record
   00                 // Return Format; Bit 0=Fan 0, Bit 1=Fan 1; etc. 0=RPM, 1=Period(***TBD***)
   00                 // Number of tach Pulses Per Revolution: Bit 0=Fan 0, Bit 1=Fan 1, etc.; 0=2 Pulses/Rev, 1=1 Pulse/Rev(***TBD***)
   803E               // Placeholder for System Fan 1a(SN:0x30), Max RPM: 16000RPM == 803E (the order is LSB, MSB)
   283C               // Placeholder for System Fan 1b(SN:0x31), Max RPM: 15400RPM == 283C (the order is LSB, MSB)
   803E               // Placeholder for System Fan 2a(SN:0x32), Max RPM: 16000RPM == 803E (the order is LSB, MSB)
   283C               // Placeholder for System Fan 2b(SN:0x33), Max RPM: 15400RPM == 283C (the order is LSB, MSB)
   803E               // Placeholder for System Fan 3a(SN:0x34), Max RPM: 16000RPM == 803E (the order is LSB, MSB)
   283C               // Placeholder for System Fan 3b(SN:0x35), Max RPM: 15400RPM == 283C (the order is LSB, MSB)
   803E               // Placeholder for System Fan 4a(SN:0x36), Max RPM: 16000RPM == 803E (the order is LSB, MSB)
   283C               // Placeholder for System Fan 4b(SN:0x37), Max RPM: 15400RPM == 283C (the order is LSB, MSB)
   803E               // Placeholder for System Fan 5a(SN:0x38), Max RPM: 16000RPM == 803E (the order is LSB, MSB)
   283C               // Placeholder for System Fan 5b(SN:0x39), Max RPM: 15400RPM == 283C (the order is LSB, MSB)
   803E               // Placeholder for System Fan 6a(SN:0x3A), Max RPM: 16000RPM == 803E (the order is LSB, MSB)
   283C               // Placeholder for System Fan 6b(SN:0x3B), Max RPM: 15400RPM == 283C (the order is LSB, MSB)


//====================================================================//
// FSC Record Type = 00h (Global Clamp Header Record)
// All Chassis
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00AD           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   74             // Clamp Header ID
   74             // Temperature Sensor Number -- (P1 Therm Margin)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   1A             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   64             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   FA             // Temperature (FAh = -6 degree C)
   01             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 1 (use TControl)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00AE           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   75             // Clamp Header ID
   75             // Temperature Sensor Number -- (P2 Therm Margin)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   FC             // Temperature (FCh = -4 degree C)
   11             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 1 (use TControl)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00AF           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   B0             // Clamp Header ID
   B0             // Temperature Sensor Number -- (DIMM Thrm Mrgn 1)
   00             // Entity Presence Sensor Number -- (NA)
   00             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   FC             // Temperature (FCh = -4 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00B0           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   B1             // Clamp Header ID
   B1             // Temperature Sensor Number -- (DIMM Thrm Mrgn 2)
   00             // Entity Presence Sensor Number -- (NA)
   00             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   FC             // Temperature (FCh = -4 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00B1          // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   B2             // Clamp Header ID
   B2             // Temperature Sensor Number -- (DIMM Thrm Mrgn 3)
   00             // Entity Presence Sensor Number -- (NA)
   00             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   FC             // Temperature (FCh = -4 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00B2           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   B3             // Clamp Header ID
   B3             // Temperature Sensor Number -- (DIMM Thrm Mrgn 4)
   00             // Entity Presence Sensor Number -- (NA)
   00             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   FC             // Temperature (FCh = -4 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00B3          // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   24             // Clamp Header ID
   24             // Temperature Sensor Number -- (P1 VR Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   43             // Temperature (43h = 67 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00B4           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   23             // Clamp Header ID
   23             // Temperature Sensor Number -- (BB BMC Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   4A             // Temperature (4Ah = 74 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00B5           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   25             // Clamp Header ID
   25             // Temperature Sensor Number -- (IB Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   46             // Temperature (46h = 70 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00B6           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   22             // Clamp Header ID
   22             // Temperature Sensor Number -- (SSB Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   53             // Temperature (53h = 83 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00B7           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   26             // Clamp Header ID
   26             // Temperature Sensor Number -- (IOM Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   3C             // Temperature (3Ch = 60 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00B8           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   2D             // Clamp Header ID
   2D             // Temperature Sensor Number -- (SAS Module Temp 1)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   3C             // Temperature (3Ch = 60 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00B9           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   28             // Clamp Header ID
   28             // Temperature Sensor Number -- (SAS Module Temp 2)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   4B             // Temperature (4Bh = 75 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00BA           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   2F             // Clamp Header ID
   2F             // Temperature Sensor Number -- (Powerville Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   00             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   5A             // Temperature (5Ah = 90 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00BB           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   5C             // Clamp Header ID
   5C             // Temperature Sensor Number -- (PS1 Temperature)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   37             // Temperature (37h = 55 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00BC           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   5D             // Clamp Header ID
   5D             // Temperature Sensor Number -- (PS2 Temperature)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   37             // Temperature (37h = 55 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00BD           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   29             // Clamp Header ID
   29             // Temperature Sensor Number -- (HSBP PSOC)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   50             // Temperature (50h = 80 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use Fixed Temp)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00BE           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   83             // Clamp Header ID
   83             // Temperature Sensor Number -- (P1 DTS Therm Mgn)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   FC             // Temperature (FCh = -4 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 1 (use TControl)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00BF           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   84             // Clamp Header ID
   84             // Temperature Sensor Number -- (P2 DTS Therm Mgn)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   01             // Clamp Control Coefficient MSB
   FC             // Temperature (FCh = -4 degree C)
   10             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use TControl)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00C0           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   2E             // Clamp Header ID
   2E             // Temperature Sensor Number -- (Exit Air Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   10             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   64             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   42             // Temperature (42h = 66 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 1 (use Fixed Temp)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00C1           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   94             // Clamp Header ID
   74             // Temperature Sensor Number -- (P1 Therm Margin)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   28             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient MSB
   FA             // Temperature (FAh = -6 degree C)
   01             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 1 (use TControl)


//====================================================================//
// FSC Record Type = 01h (Global Stepwise Header Record)
// All Chassis
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0013

   // Sensor Record Header
   00C2           // Record ID
   51             // SDR Version
   C0             // Record Type
   0E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   01             // FSC Record Type (01h = Global Stepwise Header Records)

   // Global Stepwise Header Record
   00             // Stepwise Header ID
   21             // Temperature Sensor Number -- (HSBP Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   50             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 2; [2:0]-Positive Hysteresis = 0

   // Global Stepwise Header Record
   // Add More Stepwise Header Records Here (up to 64 bytes total record length)


//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0013

   // Sensor Record Header
   00C3           // Record ID
   51             // SDR Version
   C0             // Record Type
   0E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   01             // FSC Record Type (01h = Global Stepwise Header Records)

   // Global Stepwise Header Record
   01             // Stepwise Header ID
   20             // Temperature Sensor Number -- (BB Inlet Temp)
   00             // Entity Presence Sensor Number -- (NA)
   64             // Sensor Disabled Control Value
   64             // Sensor Fail Control Value
   64             // Sensor Unavailable Control Value
   00             // Sleep Control Value
   50             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 2; [2:0]-Positive Hysteresis = 0

   // Global Stepwise Header Record
   // Add More Stepwise Header Records Here (up to 64 bytes total record length)


//====================================================================//
// FSC Record Type = 02h (Global Stepwise Curve Record)
// All Chassis - Minimum Stepwise Linear Tables
// BP_35: 300 900 1500 3000 (LCC)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0033

   // Sensor Record Header
   00C4           // Record ID
   51             // SDR Version
   C0             // Record Type
   2E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   00             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   14             // Temperature 1 (14h = 20C)
   19             // Control Value 1 PWM (19h = 25%)
   1E             // Temperature 2 (1Eh = 30C)
   1E             // Control Value 2 PWM (1Eh = 30%)
   28             // Temperature 3 (28h = 40C)
   24             // Control Value 3 PWM (24h = 36%)
   32             // Temperature 4 (32h = 50C)
   64             // Control Value 4 PWM (64h = 100%)

   // Global Stepwise Curve Record
   01             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   14             // Temperature 1 (14h = 20C)
   1B             // Control Value 1 PWM (1Bh = 27%)
   1E             // Temperature 2 (1Eh = 30C)
   22             // Control Value 2 PWM (22h = 34%)
   28             // Temperature 3 (28h = 40C)
   2A             // Control Value 3 PWM (2Ah = 42%)
   32             // Temperature 4 (32h = 50C)
   64             // Control Value 4 PWM (64h = 100%)

   // Global Stepwise Curve Record
   03             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   14             // Temperature 1 (14h = 20C)
   20             // Control Value 1 PWM (20h = 32%)
   1E             // Temperature 2 (1Eh = 30C)
   27             // Control Value 2 PWM (27h = 39%)
   26             // Temperature 3 (26h = 38C)
   2E             // Control Value 3 PWM (2Eh = 46%)
   32             // Temperature 4 (32h = 50C)
   64             // Control Value 4 PWM (64h = 100%)

   // Global Stepwise Curve Record
   05             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   14             // Temperature 1 (14h = 20C)
   29             // Control Value 1 PWM (29h = 41%)
   1E             // Temperature 2 (1Eh = 30C)
   32             // Control Value 2 PWM (32h = 50%)
   21             // Temperature 3 (21h = 33C)
   38             // Control Value 3 PWM (38h = 56%)
   32             // Temperature 4 (32h = 50C)
   64             // Control Value 4 PWM (64h = 100%)


// BP_25: 300 900 1500 3000 (LCC)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0033

   // Sensor Record Header
   00C5           // Record ID
   51             // SDR Version
   C0             // Record Type
   2E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   07             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   14             // Temperature 1 (14h = 20C)
   14             // Control Value 1 PWM (14h = 20%)
   1E             // Temperature 2 (1Eh = 30C)
   19             // Control Value 2 PWM (19h = 25%)
   28             // Temperature 3 (28h = 40C)
   23             // Control Value 3 PWM (23h = 35%)
   32             // Temperature 4 (32h = 50C)
   64             // Control Value 4 PWM (64h = 100%)

   // Global Stepwise Curve Record
   08             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   14             // Temperature 1 (14h = 20C)
   19             // Control Value 1 PWM (19h = 25%)
   1E             // Temperature 2 (1Eh = 30C)
   1E             // Control Value 2 PWM (1Eh = 30%)
   28             // Temperature 3 (28h = 40C)
   28             // Control Value 3 PWM (28h = 40%)
   32             // Temperature 4 (32h = 50C)
   64             // Control Value 4 PWM (64h = 100%)

   // Global Stepwise Curve Record
   0A             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   14             // Temperature 1 (14h = 20C)
   1E             // Control Value 1 PWM (1Eh = 30%)
   1E             // Temperature 2 (1Eh = 30C)
   23             // Control Value 2 PWM (23h = 35%)
   26             // Temperature 3 (26h = 38C)
   2B             // Control Value 3 PWM (2Bh = 43%)
   32             // Temperature 4 (32h = 50C)
   64             // Control Value 4 PWM (64h = 100%)

   // Global Stepwise Curve Record
   0C             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   14             // Temperature 1 (14h = 20C)
   26             // Control Value 1 PWM (26h = 38%)
   1E             // Temperature 2 (1Eh = 30C)
   2D             // Control Value 2 PWM (2Dh = 45%)
   21             // Temperature 3 (21h = 33C)
   32             // Control Value 3 PWM (32h = 50%)
   32             // Temperature 4 (32h = 50C)
   64             // Control Value 4 PWM (64h = 100%)


// PSU / Test Plate / Slow Ramp: 900 (LCC)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0031

   // Sensor Record Header
   00C6           // Record ID
   51             // SDR Version
   C0             // Record Type
   2C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   0E             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   14             // Temperature 1 (14h = 20C)
   2D             // Control Value 1 PWM (2Dh = 45%)
   1E             // Temperature 2 (1Eh = 30C)
   2D             // Control Value 2 PWM (2Dh = 45%)
   28             // Temperature 3 (28h = 40C)
   2D             // Control Value 3 PWM (2Dh = 45%)
   34             // Temperature 4 (34h = 52C)
   64             // Control Value 4 PWM (64h = 100%)

   // Global Stepwise Curve Record
   0F             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   14             // Temperature 1 (14h = 20C)
   23             // Control Value 1 PWM (23h = 35%)
   1E             // Temperature 2 (1Eh = 30C)
   23             // Control Value 2 PWM (23h = 35%)
   28             // Temperature 3 (28h = 40C)
   23             // Control Value 3 PWM (23h = 35%)
   34             // Temperature 4 (34h = 52C)
   64             // Control Value 4 PWM (64h = 100%)

   // Global Stepwise Curve Record
   10             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   14             // Temperature 1 (14h = 20C)
   4B             // Control Value 1 PWM (4Bh = 75%)
   1E             // Temperature 2 (1Eh = 30C)
   4B             // Control Value 2 PWM (4Bh = 75%)
   21             // Temperature 3 (21h = 33C)
   4B             // Control Value 3 PWM (4Bh = 75%)
   26             // Temperature 4 (26h = 38C)
   4B             // Control Value 4 PWM (4Bh = 75%)
   28             // Temperature 5 (28h = 40C)
   4B             // Control Value 5 PWM (4Bh = 75%)

   // Global Stepwise Curve Record
   5B             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   1E             // Temperature 1 (1Eh = 30C)
   19             // Control Value 1 PWM (19h = 25%)
   78             // Temperature 2 (78h = 120C)
   64             // Control Value 2 PWM (64h = 100%)


// Slow Ramp: 1500 3000 / Medium: 900 1500 (LCC)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0023

   // Sensor Record Header
   00C7           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   5C             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   1E             // Temperature 1 (1Eh = 30C)
   20             // Control Value 1 PWM (20h = 32%)
   70             // Temperature 2 (70h = 112C)
   64             // Control Value 2 PWM (64h = 100%)

   // Global Stepwise Curve Record
   5D             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   1E             // Temperature 1 (1Eh = 30C)
   33             // Control Value 1 PWM (33h = 51%)
   59             // Temperature 2 (59h = 89C)
   64             // Control Value 2 PWM (64h = 100%)

   // Global Stepwise Curve Record
   5F             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   1E             // Temperature 1 (1Eh = 30C)
   19             // Control Value 1 PWM (19h = 25%)
   4B             // Temperature 2 (4Bh = 75C)
   64             // Control Value 2 PWM (64h = 100%)

   // Global Stepwise Curve Record
   60             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   1E             // Temperature 1 (1Eh = 30C)
   20             // Control Value 1 PWM (20h = 32%)
   47             // Temperature 2 (47h = 71C)
   64             // Control Value 2 PWM (64h = 100%)


// Medium: 3000 / Fast: 900 1500 3000 (LCC)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0023

   // Sensor Record Header
   00C8           // Record ID
   51             // SDR Version
   C0             // Record Type
   1E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   61             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   1E             // Temperature 1 (1Eh = 30C)
   33             // Control Value 1 PWM (33h = 51%)
   3C             // Temperature 2 (3Ch = 60C)
   64             // Control Value 2 PWM (64h = 100%)

   // Global Stepwise Curve Record
   62             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   1E             // Temperature 1 (1Eh = 30C)
   19             // Control Value 1 PWM (19h = 25%)
   3C             // Temperature 2 (3Ch = 60C)
   64             // Control Value 2 PWM (64h = 100%)

   // Global Stepwise Curve Record
   63             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   1E             // Temperature 1 (1Eh = 30C)
   20             // Control Value 1 PWM (20h = 32%)
   3A             // Temperature 2 (3Ah = 58C)
   64             // Control Value 2 PWM (64h = 100%)

   // Global Stepwise Curve Record
   64             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   1E             // Temperature 1 (1Eh = 30C)
   33             // Control Value 1 PWM (33h = 51%)
   32             // Temperature 2 (32h = 50C)
   64             // Control Value 2 PWM (64h = 100%)


//====================================================================//
// FSC Record Type = 02h (Global Stepwise Curve Record)
// All Chassis - Maximum Stepwise Linear Tables
// BP_35 / BP_25 (UCC)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    002D

   // Sensor Record Header
   00C9           // Record ID
   51             // SDR Version
   C0             // Record Type
   28             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   02             // Stepwise Curve ID
   83             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   14             // Temperature 1 (14h = 20C)
   42             // Control Value 1 PWM (42h = 66%)
   1E             // Temperature 2 (1Eh = 30C)
   50             // Control Value 2 PWM (50h = 80%)
   28             // Temperature 3 (28h = 40C)
   64             // Control Value 3 PWM (64h = 100%)

   // Global Stepwise Curve Record
   04             // Stepwise Curve ID
   83             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   14             // Temperature 1 (14h = 20C)
   47             // Control Value 1 PWM (47h = 71%)
   1E             // Temperature 2 (1Eh = 30C)
   55             // Control Value 2 PWM (55h = 85%)
   21             // Temperature 3 (26h = 38C)
   64             // Control Value 3 PWM (64h = 100%)

   // Global Stepwise Curve Record
   06             // Stepwise Curve ID
   83             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   14             // Temperature 1 (14h = 20C)
   50             // Control Value 1 PWM (50h = 80%)
   1E             // Temperature 2 (1Eh = 30C)
   5F             // Control Value 2 PWM (5Fh = 95%)
   21             // Temperature 3 (21h = 33C)
   64             // Control Value 3 PWM (64h = 100%)

   // Global Stepwise Curve Record
   09             // Stepwise Curve ID
   84             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   14             // Temperature 1 (14h = 20C)
   31             // Control Value 1 PWM (31h = 49%)
   1E             // Temperature 2 (1Eh = 30C)
   3A             // Control Value 2 PWM (3Ah = 58%)
   28             // Temperature 3 (28h = 40C)
   50             // Control Value 3 PWM (50h = 80%)
   32             // Temperature 4 (32h = 50C)
   64             // Control Value 4 PWM (64h = 100%)


// BP_25 / Slow Ramp (UCC)
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0025

   // Sensor Record Header
   00CA           // Record ID
   51             // SDR Version
   C0             // Record Type
   20             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   0B             // Stepwise Curve ID
   84             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   14             // Temperature 1 (14h = 20C)
   34             // Control Value 1 PWM (34h = 52%)
   1E             // Temperature 2 (1Eh = 30C)
   41             // Control Value 2 PWM (41h = 65%)
   26             // Temperature 3 (26h = 38C)
   52             // Control Value 3 PWM (52h = 82%)
   32             // Temperature 4 (32h = 50C)
   64             // Control Value 4 PWM (64h = 100%)

   // Global Stepwise Curve Record
   0D             // Stepwise Curve ID
   84             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   14             // Temperature 1 (14h = 20C)
   3C             // Control Value 1 PWM (3Ch = 60%)
   1E             // Temperature 2 (1Eh = 30C)
   50             // Control Value 2 PWM (50h = 80%)
   21             // Temperature 3 (21h = 33C)
   5A             // Control Value 3 PWM (5Ah = 90%)
   32             // Temperature 4 (32h = 50C)
   64             // Control Value 4 PWM (64h = 100%)

   // Global Stepwise Curve Record
   5E             // Stepwise Curve ID
   82             // Domain max and Count [7]-Domain Max (0=no) [6:0]-Count
   1E             // Temperature 1 (1Eh = 30C)
   64             // Control Value 1 PWM (64h = 100%)
   32             // Temperature 2 (32h = 50C)
   64             // Control Value 2 PWM (64h = 100%)


//====================================================================//
// FSC Record Type = 03h (Fan Sensor Domain Map Record)
// H2300JF / H2200JF Chassis
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    0017

   // Sensor Record Header
   00CB           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   03             // FSC Record Type (03h = Fan Sensor Domain Map)

   // Domain Fan Configuration
   06             // [7:4]-Domain Number = 0; [3:0]-Count of sensor numbers = 6
   30             // Fan Sensor Number 1 (30h = Sys Fan 1A)
   31             // Fan Sensor Number 2 (31h = Sys Fan 1B)
   32             // Fan Sensor Number 3 (32h = Sys Fan 2A)
   33             // Fan Sensor Number 4 (33h = Sys Fan 2B)
   34             // Fan Sensor Number 5 (34h = Sys Fan 3A)
   35             // Fan Sensor Number 6 (35h = Sys Fan 3B)
   24             // [7:4]-Domain Number = 2; [3:0]-Count of sensor numbers = 4
   A0             // Fan Sensor Number 7 (A0h = PS1 Fan Fail / PS1 1a Fan Fail)
   A1             // Fan Sensor Number 8 (A1h = PS1 1b Fan Fail)
   A4             // Fan Sensor Number 9 (A4h = PS2 Fan Fail / PS2 1a Fan Fail)
   A5             // Fan Sensor Number 10 (A5h = PS2 1b Fan Fail)


//====================================================================//
// FSC Record Type = 03h (Fan Sensor Domain Map Record)
// Other Chassis
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0019

   // Sensor Record Header
   00CC           // Record ID
   51             // SDR Version
   C0             // Record Type
   14             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   03             // FSC Record Type (03h = Fan Sensor Domain Map)

   // Domain Fan Configuration
   06             // [7:4]-Domain Number = 0; [3:0]-Count of sensor numbers = 6
   30             // Fan Sensor Number 1 (30h = Sys Fan 1A)
   31             // Fan Sensor Number 2 (31h = Sys Fan 1B)
   32             // Fan Sensor Number 3 (32h = Sys Fan 2A)
   33             // Fan Sensor Number 4 (33h = Sys Fan 2B)
   34             // Fan Sensor Number 5 (34h = Sys Fan 3A)
   35             // Fan Sensor Number 6 (35h = Sys Fan 3B)
   16             // [7:4]-Domain Number = 1; [3:0]-Count of sensor numbers = 6
   36             // Fan Sensor Number 7 (36h = Sys Fan 4A)
   37             // Fan Sensor Number 8 (37h = Sys Fan 4B)
   38             // Fan Sensor Number 9 (38h = Sys Fan 5A)
   39             // Fan Sensor Number 10 (39h = Sys Fan 5B)
   3A             // Fan Sensor Number 11 (3Ah = Sys Fan 6A)
   3B             // Fan Sensor Number 12 (3Bh = Sys Fan 6B)


//====================================================================//
// Domain 0 - H2300JF / H2200JF
//====================================================================//
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// H2300JF Chassis, Domain 0, Profiles 0 & 1
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    001C

   // Sensor Record Header
   00CD           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   03             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value (19h = 25%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (0h = No sensors to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   00             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   02             // Stepwise Curve ID


// H2300JF Chassis, Domain 0, Profiles 2 & 3
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    001C

   // Sensor Record Header
   00CE           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   0C             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   1E             // Normal Control Value (1Eh = 30%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (0h = No sensors to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   01             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   02             // Stepwise Curve ID


// H2300JF Chassis, Domain 0, Profiles 4 & 5
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    001C

   // Sensor Record Header
   00CF           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   30             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   23             // Normal Control Value (23h = 35%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (0h = No sensors to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   03             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   04             // Stepwise Curve ID


// H2300JF Chassis, Domain 0, Profiles 6 & 7
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    001C

   // Sensor Record Header
   00D0           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   C0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   28             // Normal Control Value (28h = 40%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (0h = No sensors to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   05             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   06             // Stepwise Curve ID


//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// H2200JF Chassis, Domain 0, Profiles 0 & 1
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    001C

   // Sensor Record Header
   00D1           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   03             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (0h = No sensors to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   07             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   09             // Stepwise Curve ID


// H2200JF Chassis, Domain 0, Profiles 2 & 3
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    001C

   // Sensor Record Header
   00D2           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   0C             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value (19h = 25%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (0h = No sensors to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   09             // Stepwise Curve ID


// H2200JF Chassis, Domain 0, Profiles 4 & 5
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    001C

   // Sensor Record Header
   00D3           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   30             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   1E             // Normal Control Value (1Eh = 30%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (0h = No sensors to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0A             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0B             // Stepwise Curve ID


// H2300JF Chassis, Domain 0, Profiles 6 & 7
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    001C

   // Sensor Record Header
   00D4           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   C0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   26             // Normal Control Value (26h = 38%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (0h = No sensors to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0C             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0D             // Stepwise Curve ID


//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// H2300JF / H2200JF Chassis, Domain 0, All Profiles
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    002B

   // Sensor Record Header
   00D5           // Record ID
   51             // SDR Version
   C0             // Record Type
   26             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID (74h = 74h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID (75h = 75h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID (80h = B0h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID (B1h = B1h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID (B2h = B2h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID (24h = 24h)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID (25h = 25h)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID (22h = 22h)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID (26h = 26h)
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID (2Fh = 2Fh)
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID (2Eh = 2Eh)
   // Clamp Sub-Record 14
   03             // FSC Sub-Record Type (03h = Clamp)
   2D             // Clamp ID (2Dh = 2Dh)
   // Clamp Sub-Record 15
   03             // FSC Sub-Record Type (03h = Clamp)
   28             // Clamp ID (28h = 28h)


//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// FSC Sub-record Type = 05h (Fans Off)
// H2300JF Chassis, Domain 0, All Profiles
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    001B

   // Sensor Record Header
   00D6           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   64             // Domain 0 Fan Failure Value (64h = 100% PWM)
   FF             // Domain 1 Fan Failure Value (FFh = No Change)
   FF             // Domain 2 Fan Failure Value (FFh = No Change)
   FF             // Domain 3 Fan Failure Value (FFh = No Change)
   FF             // Domain 4 Fan Failure Value (FFh = No Change)
   FF             // Domain 5 Fan Failure Value (FFh = No Change)
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)

   // Fans Off Sub-Record
   05             // FSC Sub-Record Type (05h = Fans Off)
   C8             // Sensor Number Controlling Operation (C8h = Agg Thrm Mgn 1)
   E2             // Fans Off Control Value (E2h = -30 Degrees)
   0A             // Hysteresis (0Ah = 10)
   19             // Fans Off PWM (19h = 25%)


// H2200JF Chassis, Domain 0, All Profiles
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    001B

   // Sensor Record Header
   00D7           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   64             // Domain 0 Fan Failure Value (64h = 100% PWM)
   FF             // Domain 1 Fan Failure Value (FFh = No Change)
   FF             // Domain 2 Fan Failure Value (FFh = No Change)
   FF             // Domain 3 Fan Failure Value (FFh = No Change)
   FF             // Domain 4 Fan Failure Value (FFh = No Change)
   FF             // Domain 5 Fan Failure Value (FFh = No Change)
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)

   // Fans Off Sub-Record
   05             // FSC Sub-Record Type (05h = Fans Off)
   C8             // Sensor Number Controlling Operation (C8h = Agg Thrm Mgn 1)
   E2             // Fans Off Control Value (E2h = -30 Degrees)
   0A             // Hysteresis (0Ah = 10)
   14             // Fans Off PWM (14h = 20%)


//====================================================================//
// Domain 2 - H2300JF / H2200JF
//====================================================================//
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// H2300JF Chassis, Domain 2(Power Supply), All Profiles
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    0022

   // Sensor Record Header
   00D8           // Record ID
   51             // SDR Version
   C0             // Record Type
   1D             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   18             // FSC Record Type (18h = Power Supply Main Domain)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   2D             // Normal Control Value (2Dh = 45%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (0h = No sensors to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0E             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   06             // Stepwise Curve ID

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID (5Ch = 5Ch)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID (5Dh = 5Dh)


// H2200JF Chassis, Domain 2(Power Supply), All Profiles
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    0022

   // Sensor Record Header
   00D9           // Record ID
   51             // SDR Version
   C0             // Record Type
   1D             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   18             // FSC Record Type (18h = Power Supply Main Domain)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   23             // Normal Control Value (23h = 35%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (0h = No sensors to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0F             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   06             // Stepwise Curve ID

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID (5Ch = 5Ch)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID (5Dh = 5Dh)


//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// H2300JF / H2200JF Chassis, Domain 2(Power Supply), All Profiles
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    0016

   // Sensor Record Header
   00DA           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   18             // FSC Record Type (18h = Power Supply Main Domain)
   04             // Domain Mask
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   FF             // Domain 0 Fan Failure Value (FFh = No Change)
   FF             // Domain 1 Fan Failure Value (FFh = No Change)
   64             // Domain 2 Fan Failure Value (64h = 100% PWM)
   FF             // Domain 3 Fan Failure Value (FFh = No Change)
   FF             // Domain 4 Fan Failure Value (FFh = No Change)
   FF             // Domain 5 Fan Failure Value (FFh = No Change)
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)


//====================================================================//
// All Domains - for FCT & FOQM FSC
//====================================================================//
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// Domain 0 & 1, Profiles 0 & 1 & 2 & 3 & 4 & 5 & 6 & 7
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    0015

   // Sensor Record Header
   00DB           // Record ID
   51             // SDR Version
   C0             // Record Type
   10             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   03             // Domain Mask
   FF             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost


//====================================================================//
// All Domains - OTHER Master
//====================================================================//
//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Other Master Chassis, Domain 0, Profiles 0 & 1 & 2 & 3
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0018

   // Sensor Record Header
   00DC           // Record ID
   51             // SDR Version
   C0             // Record Type
   13             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   03             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5E             // Stepwise Curve ID


// Other Master Chassis, Domain 0, Profiles 4 & 5
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0018

   // Sensor Record Header
   00DD           // Record ID
   51             // SDR Version
   C0             // Record Type
   13             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   03             // Domain Mask
   30             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5E             // Stepwise Curve ID


// Other Master Chassis, Domain 0, Profiles 6 & 7
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0018

   // Sensor Record Header
   00DE           // Record ID
   51             // SDR Version
   C0             // Record Type
   13             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   03             // Domain Mask
   C0             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5E             // Stepwise Curve ID


//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Other Master Chassis, Domain 0, All Profiles
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0025

   // Sensor Record Header
   00DF           // Record ID
   51             // SDR Version
   C0             // Record Type
   20             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID (74h = 74h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID (75h = 75h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID (B0h = B0h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID (B1h = B1h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID (B2h = B2h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID (24h = 24h)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID (25h = 25h)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID (22h = 22h)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID (26h = 26h)
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID (2Fh = 2Fh)


//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Other Master Chassis, Domain 1, All Profiles
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0025

   // Sensor Record Header
   00E0           // Record ID
   51             // SDR Version
   C0             // Record Type
   20             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   02             // Domain Mask
   FF             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID (74h = 74h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID (75h = 75h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID (B0h = B0h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID (B1h = B1h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID (B2h = B2h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID (24h = 24h)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID (25h = 25h)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID (22h = 22h)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID (26h = 26h)
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID (2Fh = 2Fh)


//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Other Chassis Slow Ramp, All Domains, Profiles 0 & 1 & 2 & 3
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_REC_LEN    0010

   // Sensor Record Header
   00E1           // Record ID
   51             // SDR Version
   C0             // Record Type
   0B             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   03             // Domain Mask
   0F             // Fan Profile Support

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5B             // Stepwise Curve ID


// Other Chassis Slow Ramp, All Domains, Profiles 4 & 5
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_REC_LEN    0010

   // Sensor Record Header
   00E2           // Record ID
   51             // SDR Version
   C0             // Record Type
   0B             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   03             // Domain Mask
   30             // Fan Profile Support

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5C             // Stepwise Curve ID


// Other Chassis Slow Ramp, All Domains, Profiles 6 & 7
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_SR'
_REC_LEN    0010

   // Sensor Record Header
   00E3           // Record ID
   51             // SDR Version
   C0             // Record Type
   0B             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   03             // Domain Mask
   C0             // Fan Profile Support

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5D             // Stepwise Curve ID


//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Other Chassis Medium Ramp, All Domains, Profiles 0 & 1 & 2 & 3
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_MR'
_REC_LEN    0010

   // Sensor Record Header
   00E4           // Record ID
   51             // SDR Version
   C0             // Record Type
   0B             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   03             // Domain Mask
   0F             // Fan Profile Support

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5F             // Stepwise Curve ID


// Other Chassis Medium Ramp, All Domains, Profiles 4 & 5
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_MR'
_REC_LEN    0010

   // Sensor Record Header
   00E5           // Record ID
   51             // SDR Version
   C0             // Record Type
   0B             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   03             // Domain Mask
   30             // Fan Profile Support

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   60             // Stepwise Curve ID


// Other Chassis Medium Ramp, All Domains, Profiles 6 & 7
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_MR'
_REC_LEN    0010

   // Sensor Record Header
   00E6           // Record ID
   51             // SDR Version
   C0             // Record Type
   0B             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   03             // Domain Mask
   C0             // Fan Profile Support

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   61             // Stepwise Curve ID


//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// Other Chassis Fast Ramp, All Domains, Profiles 0 & 1 & 2 & 3
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_FR'
_REC_LEN    0010

   // Sensor Record Header
   00E7           // Record ID
   51             // SDR Version
   C0             // Record Type
   0B             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   03             // Domain Mask
   0F             // Fan Profile Support

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   62             // Stepwise Curve ID


// Other Chassis Fast Ramp, All Domains, Profiles 4 & 5
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_FR'
_REC_LEN    0010

   // Sensor Record Header
   00E8           // Record ID
   51             // SDR Version
   C0             // Record Type
   0B             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   03             // Domain Mask
   30             // Fan Profile Support

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   63             // Stepwise Curve ID


// Other Chassis Fast Ramp, All Domains, Profiles 6 & 7
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER_FR'
_REC_LEN    0010

   // Sensor Record Header
   00E9           // Record ID
   51             // SDR Version
   C0             // Record Type
   0B             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   03             // Domain Mask
   C0             // Fan Profile Support

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID


//====================================================================//
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Test_Plate FSC, Domain 0, Profiles 0 & 1 & 2 & 3 & 4 & 5 & 6 & 7
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'TEST_PLATE'
_REC_LEN    0033

   // Sensor Record Header
   00EA           // Record ID
   51             // SDR Version
   C0             // Record Type
   2E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   03             // Domain Mask
   0F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   64             // Fan Fault Boost Value (64h = 100%)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   00             // Sensor Exclusion Count

   // Stepwise min Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   10             // Stepwise Curve ID

   // Stepwise max Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   06             // Stepwise Curve ID

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID (74h = 74h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   75             // Clamp ID (75h = 75h)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID (B0h = B0h)
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID (B1h = B1h)
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   B2             // Clamp ID (B2h = B2h)
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   B3             // Clamp ID (B3h = B3h)
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID (24h = 24h)
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID (23h = 23h)
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID (25h = 25h)
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID (22h = 22h)
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   26             // Clamp ID (26h = 26h)
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   2F             // Clamp ID (2Fh = 2Fh)


//====================================================================//
// FSC Record Type = 11h (System Airflow Formula)
// 2U4N 3.5" SKU H2300JF.
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    0012

   //Sensor Record Header
   00EB               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0D                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   11                 // Record sub-type (11h = System Airflow)
   01                 // Domain mask (Domains 0)
   1E00               // Correction Factor 1 (1Eh = 30 units of .01)
   2700               // Correction Factor 2 (27h = 39 units of .01)
   19                 // PWM for Correction Factor 1 (19h = 25%)
   64                 // PWM for Correction Factor 2 (64h = 100%)
   23                 // Max CFM of Fan (23h = 35)
   03                 // Quantity of fans in this equation


// 2U4N 2.5" SKU H2200JF.
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    0012

   //Sensor Record Header
   00EC               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0D                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   11                 // Record sub-type (11h = System Airflow)
   01                 // Domain mask (Domains 0)
   1E00               // Correction Factor 1 (1Eh = 30 units of .01)
   3A00               // Correction Factor 2 (3Ah = 58 units of .01)
   14                 // PWM for Correction Factor 1 (14h = 20%)
   64                 // PWM for Correction Factor 2 (64h = 100%)
   23                 // Max CFM of Fan (23h = 35)
   03                 // Quantity of fans in this equation


//====================================================================//
// FSC Record Type = 12h (Aggregate Sensor Configuration Record)
// 2U4N 3.5" SKU H2300JF / 2U4N 2.5" SKU H2200JF..
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    0019

   //Sensor Record Header
   00ED               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   14                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   12                 // Record sub-type (12h = Aggregate Sensor Configuration)
   C8                 // Aggregate sensor number (C8h = Agg Thrm Mgn 1)
   08                 // Number of input pairs to follow
   83                 // Input 1 sensor number (83h = P1 DTS Therm Mgn)
   00                 // Input 1 margin reference value (00h = 0)
   B1                 // Input 2 sensor number (B1h = DIMM Thrm Mrgn 2)
   00                 // Input 2 margin reference value (00h = 0)
   B0                 // Input 3 sensor number (B0h = DIMM Thrm Mrgn 1)
   00                 // Input 3 margin reference value (00h = 0)
   25                 // Input 4 sensor number (25h = IB Temp)
   46                 // Input 4 margin reference value (46h = 70)
   22                 // Input 5 sensor number (22h = SSB Temp)
   53                 // Input 5 margin reference value (53h = 83)
   23                 // Input 6 sensor number (23h = BB BMC Temp)
   4A                 // Input 6 margin reference value (4Ah = 74)
   2F                 // Input 7 sensor number (2Fh = Powerville Temp)
   62                 // Input 7 margin reference value (62h = 98)


//====================================================================//
// FSC Record Type = 13h (DIMM Air Velocity Record)
// 2U4N 3.5" SKU H2300JF.
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    002D

   // Sensor Record Header
   00EE               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   28                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   13                 // Record Subtype (13h = DIMM Air Velocity)

   B0                 // DIMM aggregate sensor number (B0h = DIMM Thrm Mrgn 1)
   01                 // Domain bit mask (01h = Domain 0)
   32                 // Reference PWM % 1 (32h = 50%)
   46                 // Reference PWM % 2 (46h = 70%)
   64                 // Reference PWM % 3 (64h = 100%)
   16                 // PWM 1 Velocity (16h = 22)
   20                 // PWM 2 Velocity (20h = 32)
   25                 // PWM 3 Velocity (25h = 37)
   07                 // Smoothing coefficient (07h = 7)

   B1                 // DIMM aggregate sensor number (B1h = DIMM Thrm Mrgn 2)
   01                 // Domain bit mask (01h = Domain 0)
   32                 // Reference PWM % 1 (32h = 50%)
   46                 // Reference PWM % 2 (46h = 70%)
   64                 // Reference PWM % 3 (64h = 100%)
   10                 // PWM 1 Velocity (10h = 16)
   16                 // PWM 2 Velocity (16h = 22)
   1F                 // PWM 3 Velocity (1Fh = 31)
   07                 // Smoothing coefficient (07h = 7)

   B2                 // DIMM aggregate sensor number (B2h = DIMM Thrm Mrgn 3)
   01                 // Domain bit mask (01h = Domain 0)
   32                 // Reference PWM % 1 (32h = 50%)
   46                 // Reference PWM % 2 (46h = 70%)
   64                 // Reference PWM % 3 (64h = 100%)
   16                 // PWM 1 Velocity (16h = 22)
   1F                 // PWM 2 Velocity (1Fh = 31)
   2B                 // PWM 3 Velocity (2Bh = 43)
   07                 // Smoothing coefficient (07h = 7)

   B3                 // DIMM aggregate sensor number (B3h = DIMM Thrm Mrgn 4)
   01                 // Domain bit mask (01h = Domain 0)
   32                 // Reference PWM % 1 (32h = 50%)
   46                 // Reference PWM % 2 (46h = 70%)
   64                 // Reference PWM % 3 (64h = 100%)
   12                 // PWM 1 Velocity (12h = 18)
   1B                 // PWM 2 Velocity (1Bh = 27)
   26                 // PWM 3 Velocity (26h = 38)
   07                 // Smoothing coefficient (07h = 7)


//====================================================================//
// FSC Record Type = 13h (DIMM Air Velocity Record)
// 2U4N 2.5" SKU H2200JF.
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    002D

   // Sensor Record Header
   00EF               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   28                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   13                 // Record Subtype (13h = DIMM Air Velocity)

   B0                 // DIMM aggregate sensor number (B0h = DIMM Thrm Mrgn 1)
   01                 // Domain bit mask (01h = Domain 0)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   23                 // PWM 1 Velocity (23h = 35)
   30                 // PWM 2 Velocity (30h = 48)
   3E                 // PWM 3 Velocity (3Eh = 62)
   07                 // Smoothing coefficient (07h = 7)

   B1                 // DIMM aggregate sensor number (B1h = DIMM Thrm Mrgn 2)
   01                 // Domain bit mask (01h = Domain 0)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   17                 // PWM 1 Velocity (17h = 23)
   28                 // PWM 2 Velocity (28h = 40)
   37                 // PWM 3 Velocity (37h = 55)
   07                 // Smoothing coefficient (07h = 7)

   B2                 // DIMM aggregate sensor number (B2h = DIMM Thrm Mrgn 3)
   01                 // Domain bit mask (01h = Domain 0)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   13                 // PWM 1 Velocity (13h = 19)
   1C                 // PWM 2 Velocity (1Ch = 28)
   2D                 // PWM 3 Velocity (2Dh = 45)
   07                 // Smoothing coefficient (07h = 7)

   B3                 // DIMM aggregate sensor number (B3h = DIMM Thrm Mrgn 4)
   01                 // Domain bit mask (01h = Domain 0)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   14                 // PWM 1 Velocity (14h = 20)
   1E                 // PWM 2 Velocity (1Eh = 30)
   35                 // PWM 3 Velocity (35h = 53)
   07                 // Smoothing coefficient (07h = 7)


//====================================================================//
// FSC Record Type = 13h (DIMM Air Velocity Record)
// OTHER SKU.
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    002D

   // Sensor Record Header
   00F0               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   28                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   13                 // Record Subtype (13h = DIMM Air Velocity)

   B0                 // DIMM aggregate sensor number (B0h = DIMM Thrm Mrgn 1)
   03                 // Domain bit mask
   3C                 // Reference PWM % 1 (3Ch = 60%)
   50                 // Reference PWM % 2 (50h = 80%)
   64                 // Reference PWM % 3 (64h = 100%)
   0A                 // PWM 1 Velocity (0Ah = 10)
   0A                 // PWM 2 Velocity (0Ah = 10)
   0A                 // PWM 3 Velocity (0Ah = 10)
   07                 // Smoothing coefficient (07h = 7)

   B1                 // DIMM aggregate sensor number (B1h = DIMM Thrm Mrgn 2)
   03                 // Domain bit mask
   3C                 // Reference PWM % 1 (3Ch = 60%)
   50                 // Reference PWM % 2 (50h = 80%)
   64                 // Reference PWM % 3 (64h = 100%)
   0A                 // PWM 1 Velocity (0Ah = 10)
   0A                 // PWM 2 Velocity (0Ah = 10)
   0A                 // PWM 3 Velocity (0Ah = 10)
   07                 // Smoothing coefficient (07h = 7)

   B2                 // DIMM aggregate sensor number (B2h = DIMM Thrm Mrgn 3)
   03                 // Domain bit mask
   3C                 // Reference PWM % 1 (3Ch = 60%)
   50                 // Reference PWM % 2 (50h = 80%)
   64                 // Reference PWM % 3 (64h = 100%)
   0A                 // PWM 1 Velocity (0Ah = 10)
   0A                 // PWM 2 Velocity (0Ah = 10)
   0A                 // PWM 3 Velocity (0Ah = 10)
   07                 // Smoothing coefficient (07h = 7)

   B3                 // DIMM aggregate sensor number (B3h = DIMM Thrm Mrgn 4)
   03                 // Domain bit mask
   3C                 // Reference PWM % 1 (3Ch = 60%)
   50                 // Reference PWM % 2 (50h = 80%)
   64                 // Reference PWM % 3 (64h = 100%)
   0A                 // PWM 1 Velocity (0Ah = 10)
   0A                 // PWM 2 Velocity (0Ah = 10)
   0A                 // PWM 3 Velocity (0Ah = 10)
   07                 // Smoothing coefficient (07h = 7)


//====================================================================//
// FSC Record Type = 16h (Half-Width Virtual Exit Air Temperature Sub Record)
// 2U4N 3.5" SKU H2300JF / 2U4N 2.5" SKU H2200JF.
//====================================================================//
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    000B

   // Sensor Record Header
   00F1               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   06                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   16                 // Record Subtype (16h = Half width exit air temp)
   5D                 // Efficiency coefficient of power conversion (5Dh = 93%)
   2D                 // Watts of DC power to account for HDD (2Dh = 45 Watts)


//====================================================================//
// SDR Version Records
//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0015

   // Sensor Record Header
   00F2               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   10                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   'SDR File 1.13'    // String Bytes


//====================================================================//
_SDR_TYPE   C0
_REC_LEN    0018

   // Sensor Record Header
   00F3               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   13                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   'SDR Package 1.13' // String Bytes
)
