================================================================================
Intel(R) Server Platform BIOS Release Notes
================================================================================

INTEL(R) Server Boards and Systems
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA


================================================================================

DATE    : Jan 20, 2017
TO      : Multi-Core Intel(R) Xeon(R) Processor-Based Server Platform customers
SUBJECT : BIOS Release notes for version 01.01.0044

================================================================================
                           LEGAL INFORMATION
================================================================================

INFORMATION IN THIS DOCUMENT IS PROVIDED IN CONNECTION WITH INTEL PRODUCTS. NO 
LICENSE, EXPRESS OR IMPLIED, BY ESTOPPEL OR OTHERWISE, TO ANY INTELLECTUAL 
PROPERTY RIGHTS IS GRANTED BY THIS DOCUMENT. EXCEPT AS PROVIDED IN INTEL'S TERMS 
AND CONDITIONS OF SALE FOR SUCH PRODUCTS, INTEL ASSUMES NO LIABILITY WHATSOEVER 
AND INTEL DISCLAIMS ANY EXPRESS OR IMPLIED WARRANTY, RELATING TO SALE AND/OR USE 
OF INTEL PRODUCTS INCLUDING LIABILITY OR WARRANTIES RELATING TO FITNESS FOR A 
PARTICULAR PURPOSE, MERCHANTABILITY, OR INFRINGEMENT OF ANY PATENT, COPYRIGHT OR 
OTHER INTELLECTUAL PROPERTY RIGHT. 

A "Mission Critical Application" is any application in which failure of the Intel 
Product could result, directly or indirectly, in personal injury or death. SHOULD 
YOU PURCHASE OR USE INTEL'S PRODUCTS FOR ANY SUCH MISSION CRITICAL APPLICATION, 
YOU SHALL INDEMNIFY AND HOLD INTEL AND ITS SUBSIDIARIES, SUBCONTRACTORS AND 
AFFILIATES, AND THE DIRECTORS, OFFICERS, AND EMPLOYEES OF EACH, HARMLESS AGAINST 
ALL CLAIMS COSTS, DAMAGES, AND EXPENSES AND REASONABLE ATTORNEYS' FEES ARISING OUT 
OF, DIRECTLY OR INDIRECTLY, ANY CLAIM OF PRODUCT LIABILITY, PERSONAL INJURY, OR 
DEATH ARISING IN ANY WAY OUT OF SUCH MISSION CRITICAL APPLICATION, WHETHER OR NOT 
INTEL OR ITS SUBCONTRACTOR WAS NEGLIGENT IN THE DESIGN, MANUFACTURE, OR WARNING OF 
THE INTEL PRODUCT OR ANY OF ITS PARTS. 

Intel may make changes to specifications and product descriptions at any time, 
without notice. Designers must not rely on the absence or characteristics of any 
features or instructions marked "reserved" or "undefined". Intel reserves these for 
future definition and shall have no responsibility whatsoever for conflicts or 
incompatibilities arising from future changes to them. The information here is 
subject to change without notice. Do not finalize a design with this information. 

The products described in this document may contain design defects or errors known 
as errata which may cause the product to deviate from published specifications. 
Current characterized errata are available on request. 

Contact your local Intel sales office or your distributor to obtain the latest 
specifications and before placing your product order. 

Copies of documents which have an order number and are referenced in this document, 
or other Intel literature, may be obtained by calling 1-800-548-4725, 
or go to: http://www.intel.com/design/literature.htm

Intel is a registered trademark of Intel Corporation. 

*Other names and brands are the property of their respective owners.

Copyright (C) 2017 Intel Corporation.

================================================================================
                              ABOUT THIS RELEASE
================================================================================
Build Stamp : S1200SP.86B.01.01.0044
Build Date  : Dec 22, 2016

================================================================================
                           KNOWN ISSUE
================================================================================


================================================================================
                           CRC32 VALUE
================================================================================
D01.01.0044_SilverPassRO.bin CRC32:   0x7e73f931
        
================================================================================
                           BIOS COMPONENTS/CONTENTS
================================================================================
Processors supported: 
    Intel(R) Xeon(R) processor E3-1200 v5 series

Microcode update versions
CPUID     Version      Status
0x506E3   0000009E     Debug(E3-1200 v5 UP R0/S0)



On-Board Component Option ROM Versions:
all_gigabit_pxe_vxx.LOM   - 1G PXE OpROM v1.5.53 (for all EPSD gigabit controllers, including LOMs and I/O modules)
all_iscsi_vxx.LOM         - iSCSI Boot OpROM v3.0.34(for all EPSD gigabit and 10G EPSD controllers, including LOMs and I/O modules)
AHCIOR.BIN                - sata AHCI Oprom
Vbt.bin                   - iGFX graphic UEFI driver VBT file, VBT version 193
MATROXVIDEOOPROM.BIN      - Onbaord VGA legacy Oprom v3.8SQ

ACM				    : v1.3
Security Revision                   : 2.0
Memory Reference Code Version       : v1.9.0.0
Management Engine Firmware Version  : v4.0.3.124

================================================================================
                       SYSTEM FIRMWARE REQUIREMENTS
================================================================================
BIOS Update Utility: 
  UEFI iFlash32 V14.0 build10
  
Beta/Silver/Gold boards:
  Product   Fab Version   BMC      FRUSDR    EEPROM     HSC 


IMPORTANT NOTICE:

================================================================================
              INTRODUCTION
================================================================================ 

================================================================================
             INSTALLATION NOTES
================================================================================
================================================================================
                           INSTALLATION NOTES
================================================================================

WARNING:  It is very important to follow these instructions as they are written.
Failure to update using the proper procedure may cause damage to your system.

User can update BIOS flash image via either of the follow methods...
A. UEFI iFlash32 
   1.  Boot the system to EFI Shell
   2.  Copy IFlash32.efi and BIOS .CAP file to a HD or USB Flash Drive
       ( Do not use the *Rec.CAP file as it will clear NVRAM and should
         only be used for Recovery - See Recovery Instructions below )
   3.  Map the respective storage device in system with the command
       Shell> map -r
   4.  Change the Shell to mapped device file system
       Example: Shell> fs0: (or fs1:)
   5.  Run the IFlash32 utility on the prompt
       fs0:\> IFlash32 [File Name] /u /ni
   6.  Reboot system after the update is completed.

B. Use flash programmer to burn the new BIOS ROM image (16MB) into the flash chip.

c. Backup BIOS update instructions
   1.  Boot the system to EFI Shell
   2.  Copy IFlash32.efi and BIOS .CAP file to a HD or USB Flash Drive
       ( Do not use the *Rec.CAP file as it will clear NVRAM and should
         only be used for Recovery - See Recovery Instructions below )
   3.  Map the respective storage device in system with the command
       Shell> map -r
   4.  Change the Shell to mapped device file system
       Example: Shell> fs0: (or fs1:)
   5.  Run the IFlash32 utility on the prompt
       fs0:\> IFlash32 [File Name] /u /ni UpdateBackupBios
   6.  It will update primary BIOS with processed capsule and the backup BIOS update will be completed in next normal boot.
   7.  Restart unit, Backup flash update done.


================================================================================
                        BIOS RECOVERY INSTRUCTIONS
================================================================================
The Recovery process can be initiated by setting the recovery jumper (called BIOS Recovery Boot Jumper)
 
A BIOS recovery can be accomplished from backup BIOS region. 
 
The recovery media must contain the following files under the root directory:
   1.  UEFI iFlash32 (including IFlash32.efi and ipmi.efi )
   2.  *Rec.CAP
   3.  Startup.nsh (update accordingly to use proper *Rec.CAP file)
 
BIOS starts the recovery process by first loading and booting to the recovery image from backup BIOS region.
This process takes place before any video or console is available. Once the system boots 
to recovery image, it will boot automatically into EFI Shell to 
invoke the Startup.nsh script and start the flash update application (IFlash32.efi). 
IFlash32.efi requires the supporting BIOS Capsule image file (*Rec.CAP). 
After the update is complete, there will be a message displayed stating that the
"BIOS has been updated successfully" indicating the recovery process is finished.
The User should then switch the recovery jumper back to normal operation and restart
the system by performing a power cycle.
 
The following steps demonstrate this recovery process:
   1.  Power OFF the system.
   2.  Switch the recovery jumper. Details regarding the jumper ID and location
       can be obtained from the Board EPS for that Platform.
   3.  Power ON the system.
   4.  The BIOS POST screen will appear displaying the progress and system automatically 
       boots to the EFI SHELL.
   5.  Startup.nsh file executes, and initiates the flash update (IFlash32.efi)
       with new capsule file (*Rec.CAP). The regular IFlash message will be displayed at
       the end of the process, once the flash update succeeds.
   6.  Power OFF the system, and revert the recovery jumper position to "normal operation".
   7.  Power ON the system. 
   8.  Do *NOT* interrupt the BIOS POST during the first boot.


================================================================================
                ME FW Capsule INSTALLATION NOTES
================================================================================
A. UEFI iFlash32 
   1.  Boot the system to EFI Shell
   2.  Copy IFlash32.efi and ME.CAP and FD.CAP file to a HD or USB Flash Drive
   3.  Map the respective storage device in system with the command
       Shell> map -r
   4.  Change the Shell to mapped device file system
       Example: Shell> fs0: (or fs1:)
   5.  Run the IFlash32 utility on the prompt
           fs0:\> IFlash32 ME.CAP /u /ni 
           fs0:\> IFlash32 FD.CAP /u /ni 
   6.  AC cycle the system after the update is completed.

================================================================================
				IMPORTANT NOTICE
================================================================================
D01.01.0021 - This BIOS has set SGX to enabled by default, please press F9 to load default if online update method is used. No this requirement if offline update method is used.
D01.01.0023 - This BIOS has SMM communication buffer fix: causing older version of utilities are not functional, only version equal or newer than below ones can be used together with this new BIOS.(Sysinfo V14.0 Build 18, Selviewer V14.0 Build 17, Syscfg V14.0 Build 15, iFlash32 v14.0 Build10, FWPIAUPD v14.0 Build 8, FRUSDR v14.0 Build 8, OFU v14.0 Build 13)
D01.01.0043 - This BIOS has updated Security Revision to 2.0 following SPRD requirement, causing BIOS can't be downgraded to previous version with Security Revision 01.00 under normal mode. No impact under Recovery Mode. The same limitation when downgrade BIOS to non-SGX BIOS.
================================================================================
				KNOWN ISSUES/WORKAROUND
================================================================================

================================================================================
				FEATURES ADDED/REMOVED
================================================================================
				01.01.R0044
================================================================================
1. Change sign key to production key based on D01.01.0044.
================================================================================
				01.01.D0044
================================================================================
1. EPSD100036080:"In UEFI ESTE2 RAID Mode, BIOS Setup UI halt at "Drive Management" interface when enter "View Drive Properties"".
================================================================================
				01.01.D0043
================================================================================
1. Klocwork Issues fix
2. Security Revision upgrade to 2.0
3. fix usbrt runtime security hole 
4. EPSD100256270_[X] Boot menu page does not disappear when boot to IPv4 device.
================================================================================
				01.01.D0023
================================================================================
1. [S1200SP] EPSD100034709:Memory Error Injection behavior incorrect
2. [S1200SP] EPSD100254486:System Auto Rebooted during FSUP Bios 01.03.0010 ME 04.00.03.096 BMC 01.03.9805 frusdr 1.19 update under Linux
3. [S1200SP]EPSD100254632:[SGX]Chipsec UEFI NVRAM variables protect test failed - Part4: Remove RT attribute of "HDDP" to align with Greenlow R.
4. Update BP patch for security SMM commucation buffer based on BP 1.2.2.2 release candidate.
5. EPSD100249787:Chipsec security Test failed in SMI 0x26, 0x28 and 0xef.(SMM communcation buffer enhancement)
================================================================================
				01.01.D0021
================================================================================
1. [S1200SP]Clean up Security issue on Greenlow by removing all  usages/references to EFI_SMM_RUNTIME_PROTOCOL.
2. [S1200SP]Sync to BP 1221.331 to address core security issue defined in PSIRT-TA-201607.
3. [S1200SP]Hide correctable error threshold option in BIOS setup because this function doesn't support on Greenlow platform.
4. Fix regression issue because of CL406852.
5. EPSD100034161 :[SGX]Connect 4 port add-in NIC card, the add-in card show on top and onboard NIC show on bottom on setup network device.
6. EPSD100034413:[SGX]Enable Payload,boot manager has UEFI Network option under UEFI mode
7. EPSD100254667 Syscfg cannot enable "static boot order". Add a check which only do boot order check when "static boot order" is enabled by F2 setup.
8. EPSD100033233 System Status LED and the value of ED2 in SEL are incorrect when inject Correctable/Uncorrectable Error.
9. EPSD100034578£º[SGX]The CPU max speed in SMBIOS type 4 is not 4200MHz
10. EPSD100254632 [SGX]Chipsec UEFI NVRAM variables protect test failed
11. EPSD100034642: BMC version is incorrect on Diagnostic screen
12. Changed EnableSgx BIOS setup default value from disabled to enabled. 
13. EPSD100254632 [SGX]Chipsec UEFI NVRAM variables protect test failed. Remove RT attribute of "NvBootDevOptions" during loading BIOS default. Otherwise it cannot be deleted.

================================================================================
				01.01.D0013
================================================================================
1. EPSD100033112:[SGX]Enable SGX,PRMRR Size Option show INVALID PRMRR as one selected item.(merged CRB CL398110)
2. [S1200SP]EPSD100253661_[x]Customer report the DMI type 41 record bug on Silver Pass RO system-part2
3. [S1200SP][SGX][No Slighting] Microcode update to 0x9E
4. [S1200SP] EPSD100031108: Get Yellow-Mark devices in Device Manager when installed Windows 10 OS.
5. [S1200SP]EPSD100253790 Clone of: Issue found when checking ACPI dumped log.
6. EPSD100034123:[SGX]PCIe link speed cannot down to Gen2/Gen1 on slot 6 with Gen3 device, cannot down to Gen1 with Gen2 IO Module
7. Updating BIOS ID to D0013.
================================================================================
				01.01.D0009
================================================================================
1. EPSD100252071 SMI timeout failure appeared with Intel RAID module RMS25JB080 during soft reset cycling test
2. EPSD100032992 Connect TPM1.2,use PCR reading tool to dump PCR0-7 value ,after reboot or shutdown some times, PCR1 value dumped always different.
3. EPSD100032790 Use ITK to hide AER Support/Log Correct Errors/WHEA support options and flashed the capsule file, at Sever Management page, bottom info show on left-top screen when login to BIOS setup as an User privilege.
4. EPSD100033014 “Remote Management Module” option detects whether SUT have Dedicated Management Lan module or not.
5. EPSD100033331 [SGX]Log as user,"UEFI Option ROM Control" option can be changed in UEFI mode
6. [S1200SP RO][SGX][No Sighting] SGX reference code in siliver pass codebase - Part 1. 
7. [S1200SP RO][SGX][No Sighting] SGX reference code in siliver pass codebase - Part 2(CL225867). 
8. EPSD100033163:[SGX]change SGX from 'enabled' to 'Software Controlled',boot to Windows directly ,test tool show still SGX enabled.
9. [S1200SP][SGX][No Slighting] Microcode update to 0x96
10. [S1200SP][SGX][No Slighting] sync up CRB CL385217.
11. [S1200SP][SGX][No Slighting]Update SPS to SPS_E3_04.00.03.124.0 PLR4 version
12. [S1200SP] EPSD100253789:Clone of Total Width field value is 0x40 in SMBIOS Type 17 log
13. [S1200SP] EPSD100253788 Clone of: At BIOS setup, current Memory speed show 1867Mhz when set memory speed to 1866MHz.
14. [S1200SP] EPSD100253661_[x]Customer report the DMI type 41 record bug on Silver Pass RO system
15. [SGX][No sighting]40G NIC card at legacy mode, only one boot item at Legacy Network Device Order

================================================================================
				01.01.D0004
================================================================================
1. [Silver Pass][No Sighting] Initial version for SGX enablement with RC code update


================================================================================
                01.03.R0006
================================================================================
    1. Re-sign BIOS package with production key.
================================================================================
                01.03.D0006
================================================================================
    1. SPS ME FW update to 4.0.3.94.
    2. Disable CLK_RUN# logic following HW design for EPSD100031770.
================================================================================
                01.03.D0005
================================================================================
    1. Update SPS ME to 4.0.3.096.
================================================================================
                01.03.D0004
================================================================================
    1. Roll back SPS ME to 4.0.3.075.

================================================================================
                01.03.D0002
================================================================================
    1. [EPSD100251676] SE Sku show incorrect SATA information.

================================================================================
                01.03.D0001
================================================================================
    1. Roll back to old ESRTII OPROM due to new one can't support 4K HDD.
    2. Roll back to remove VS2013 support to adviod side effect that system hang 0x96 with D89 com port connected.

================================================================================
                01.02.R0021
================================================================================
    1. Microcode update to 0074.

================================================================================
                01.02.R0020
================================================================================
    1. [EPSD100251465] UEFI Production ESRTII Driver 04080000 intergate.
    2. SPS ME FW update to 4.0.3.94.
    3. WA for system reset will hang at POST code 0x36 due to TCO_STS issue.

================================================================================
                01.02.R0018
================================================================================
    1. Microcode update to 0x6A.

================================================================================
                01.02.R0017
================================================================================
    1. [EPSD100251369] Some errors reported in selftest7_7.0.22.3774.
    2. [EPSD100031058] During WIN2012R2 Cert with SE SKU and SUT show "USB Exposed Port System Test" test item fail.
    3. [EPSD100031074] BIOS message display User Name already Exits when type the same user name in User Configuration.

================================================================================
                01.02.R0015
================================================================================
    1. Fixed the issue that the time value in RTC register is not valid when CMOS battery is bad because removed for long time.
================================================================================
                01.02.R0014
================================================================================
    1. Microcode update to 0x5c.
    2. SPS FW update to 4.0.3.89.
================================================================================
                01.02.R0012
================================================================================
    1. Bios update progress will always stay on 0% ,if set recovery jumper and a previous version BIOS has been programmed at first.
================================================================================
                01.02.R0011
================================================================================
    1. [EPSD100030687] Static Boot Order would not change to Disabled when change boot order via ITK.
================================================================================
                01.02.R0010
================================================================================
    1. Enable TPM2.0 Support.
    2. Sync CRB BIOS V104_03, RC version is 1.8.0.1.
    3. [EPSD100250712] Abnormal SEL of "POST Err Sensor reports Processor 01 disabled" observed after global reset from MFG mode.
================================================================================
                01.02.R0008
================================================================================
    1. [EPSD100029833] System couldn't install Windows 2008 R2 under UEFI mode.
================================================================================
                01.02.R0007
================================================================================
    1. [EPSD100029962] In the process of installing win 2008 R2 with RS3WC080, screen will stay at "Starting Windows".
================================================================================
                01.02.R0005
================================================================================
    1. [EPSD100250675] Auto-Reboot time is too long with TPM module and MFG jumper attached.
    2. Implement clear screen after PXE oprom and before main screen.
================================================================================
                01.02.R0004
================================================================================
    1. [EPSD100250586] Abnormal SSB Therm Trip SEL observed on Silver2 build LC boards in EFI shell, MFG mode.
================================================================================
                01.02.R0003
================================================================================
    1. Microcode update to 0056.
================================================================================
                01.02.R0001
================================================================================
    1. Update BIOS version to 01.02.0001 for gold build.

================================================================================
                01.01.D150
================================================================================
    1. Sync Iflash32 code with the latest CP code.

================================================================================
                01.01.D149
================================================================================
    1. Update TXT BIOS ACM with version HF 1.3.
    2. [EPSD100030209] SUT will reboot when press ESC under PMC ASR 71605 UEFI oprom.
    3. [EPSD100250524] Inappropriate prompt message when only DIMM A1/B1 slot is populated.

================================================================================
                01.01.D148
================================================================================
    1. Microcode update to 0x49_4A.
    2. ME status report error if some region is corrupted during ME update.
    3. TXT function implement.
    4. Fixed RTC debug assert issue.
    5. [EPSD100030229] System time is abnormal after Linux OS installation completed.
    6. Fixed recovery hang issue and flash issue.

================================================================================
                01.01.D146
================================================================================
    1. SPS ME FW 4.0.3.75 updated.

================================================================================
                01.01.D145
================================================================================
    1. [EPSD100028819] "Submit fail for form:!." box will pop up after some specific steps with RMS3CC080.
    2. [EPSD100029971] UUT recorded CATERR in AC/DC/Reset cycling test with varies hang point 0xCC/0xD5/0x55.

================================================================================
                01.01.D144
================================================================================
    1. [EPSD100250133] BIOS Setup Options shows incorrectly with Client S0 CPU.
    2. [EPSD100030065] System cannot install Legacy W2012R2 OS in RSTe Mode if the RAID volume has included SATA Port 1, Port 6 and Port 7.

================================================================================
                01.01.D143
================================================================================
    1. [EPSD100029901] System stay long time at RMS25PB080 Legacy  UEFI option rom.
    2. [EPSD100250171] SSB Therm Trip error will be trigger during system warm reset.

================================================================================
                01.01.D142
================================================================================
    1. [EPSD100029430] System show error message "Unknown opcode 0x18 at table offset 0x04B7" when installed SUSE 12 x64.

================================================================================
                01.01.D141
================================================================================
    1. SPS ME FW 4.0.3.68 updated.
    2. S1200SP Klockwork Issue.

================================================================================
                01.01.D140
================================================================================
    1. [EPSD100029964] NO 8300 and 84F4 error info in error manager.
    2. [EPSD100250135] There is no screen output when set to DP + Processor graphics with Client CPU QJZW which is 2 + 1 processor.

================================================================================
                01.01.D138
================================================================================
    1. Upgrade ME to be version ME E3_04.00.03.061.0.
    2. Set PCH Hot Level to be 98 degree C.

================================================================================
                01.01.D136
================================================================================
    1. 450w PSU PMBus hang issue.
    2. check all USB policy and over current pin align with HW.

================================================================================
                01.01.D135
================================================================================
    1. [EPSD100029793] There are three logs recorded ME version change in SEL after online update ME.
    2. [EPSD100249379] Chipsec security Test failed.
    3. [EPSD100247152] Error message didn't display correctly in Error Manager after clear remove CMOS battery or clear CMOS jumper.

================================================================================
                01.01.D133
================================================================================
    1. Upgrade ME to be version ME E3_04.00.03.056.0.

================================================================================
                01.01.D132
================================================================================
    1. Roll back Chipsec lock register.
    2. Latest VBIOS(9.0.1027) /GOP(9.0.1033) to support S stepping pgfx.
    3. [EPSD100249773] Update backup BIOS failed with correct command after flash backup BIOS with incorrect command.
    4. [EPSD100028816] Processor Graphics Driver "15.40.4146.win64" cannot installed completely in W2012R2 OS with VGA Add-on card connected. It would stop at driver installation
    5. [EPSD100029875] [SE sku] Some removed devices list in SMBIOS Type8.
    6. update V97_13 PV RC 1.6.0.0 to RC 1.6.0.0.1  

================================================================================
                01.01.D130
================================================================================
    1. Sync CRB bios V97_09 with RC 1.6

================================================================================
                01.01.D129
================================================================================
    1. [EPSD100029869] There are "USB Exposed Port System test" fail items when running Win2012R2 Cert Test
    2. [EPSD100029657] System stay long time at RMS25CB080 Legacy/UEFI option rom.
    3. [EPSD100249590] SE board show incorrect PCIe information in BIOS setup.
    4. [EPSD100249646] CMOS Date/Time still be cleared on first reboot after clear CMOS or remove CMOS battery.
    6. [EPSD100028474] BIOS can't detect IO module 82599 10G UEFI iSCSI. But onboard ROM UEFI ISCS can detect.
    7. [EPSD100249731] Production ESRT2 OpROM(A.15.08211538I) and EFI(A.15.08131643I) for inclusion into S1200SP BIOS.
    8. Microcode update to 0x3A.

================================================================================
                01.01.D127
================================================================================
    1. [EPSD100248742] No DIMM info.
    2. [EPSD100249280] System will hangs up on 0X0C on next boot when interrupt update BIOS in EFI shell.
    3. Implement IPMI Command " Set PCIe card presence command".
    4. [EPSD100249567] System information show incorrect in BIOS setup.
    5. [EPSD100249547] After F9 load default and Press F10 save,system will pop-up warning message and hangs up on BIOS Setup
    6. [EPSD100249379] Chipsec security Test failed

================================================================================
                01.01.D126
================================================================================
    1. [EPSD100248742] No DIMM Power info.
    2. [EPSD100249552] Extra messages display in remote system Hyperterminal when CR is enabled on Legacy mode.
    3. Fixed BMC user help string error.
    4. Update ME module to be aligned with FTool_SPS_E3_04.00.03.046.0.
    5. New AHCI OPROM replace debug verison AHCI oprom.

================================================================================
                01.01.D124
================================================================================
    1. [EPSD100249525] Error information status is gray and error description can't shown in Error manager.
    2. Re-structure code to align other server platform
    3. Open one setup item "PciePllSsc" only for ITK tool.
    4. Integrate ESRT2 latest release OPROM and EFI driver.

================================================================================
                01.01.D122
================================================================================
    1. [EPSD100028351] There is no black space between "number" and "MB" for value of filed "Effective Memory" in BIOS Setup.
    2. [EPSD100249355] System will display error message "An unknown error occurred while running this application" when execute RSTe Utilitie tool under UEFI Win2012R2.
    3. [EPSD100249328] Set Admin/User PWD function incorrect and Admin/User PWD status show abnormal at BIOS R021.
    4. [EPSD100029073] Memory ECC error injection information is incorrect in both SEL Viewer and system log.
    5. Update XML file for SE SKU settings.
    6. Update microcode to 0034.
    7. Change setup help string according new setup spec
    8. Align setup spec 1.0 new secure boot setup help string.
    9. Secure Boot Symptoms.    

================================================================================
                01.01.D120
================================================================================
    1. [EPSD100248742]FAIL: There is no DIMM power information.
    2. Update BIOS flash map.

================================================================================
                01.01.D119
================================================================================
    1. [EPSD100248742] There is no DIMM power information.
    2. Support MMIO above 4GB when memory size >= 64GB

================================================================================
                01.01.D118
================================================================================
    1. [EPSD100029653] BIOS flash can't run in Quad mode.
    2. Update ME to be version E3_04.00.03.044.0 with enabled SPI Qual mode.
    3. [EPSD100247099] There are some errors in SMBIOS log. 

================================================================================
                01.01.D115
================================================================================
    1. [EPSD100029655] One more option "Early System Boot Timeout" lists in Advanced Boot Options page.
    2. [EPSD100029336] When there is BIOS Recovery log in SEL, it cannot see any log and USB Key will be crashed after executed SELViewer under EFI Shell.
    3. [EPSD100249269] Update D111_ME.cap will show "Warning: No SMBIOS entry for KCS address - using fixed value of 0xCA2"
    4. [EPSD100029436] Unable to boot to HDD (with UEFI OS) by LCD.
    5. [EPSD100242988] Internal:SCT test has below items fail: Runtime Services Test/Console Support Test/Bootable Image Support Test/EFI Byte Code Test/HII Test/ATA Bus Support Test/ISCSI BootTest/SCSI Bus Support Test.
    6. Enable Secure Boot on SLP.
    7. flash ME region change request.
    8. Modify the CommonSetupLib to display total L1 cache size in Setup menu.
    9. PCH PCIE CTLE setting is missed after PCH RC updating in D108.
    10.UpdateSmbios function of UBA is not executed.

================================================================================
                01.01.D113
================================================================================
    1. [EPSD100029680] NMI button function does not work.
    2. [EPSD100029628] Processor information in BIOS Processor Configuration page display "N/A". 
    3. [EPSD100029293] When install Windows7sp1 will show blue screen.
    4. [EPSD100029621] Window 2K8 SP2 32/64 can't install and it will show BSOD with legacy mode
    5. [EPSD100029308] Starting from BIOS 92, HECI error logged in dmesg after SUSE 12 setup in UEFI mode.
    6. Fixed iBMC vidio can't be disabled.
    7. Fixed NMI buttom code lost during RC sync.
    8. Sync ME related ASL code.

================================================================================
                01.01.D111
================================================================================
    1. Fixed Xd feature didn't be enable due to code sync issue.
    2. Fixed D110 BIOS can't update issue.
    3. [EPSD100248881] After install drivers,device manage still show yellow mark.
    4. [EPSD100028791] There are some fail items when running Win2012R2 Cert test.

================================================================================
                01.01.D110
================================================================================
    1. Porting Smbios Type 148 to SLP.
    2. Fix CpPcPlatPkg Klockwork scan issue.
    3. [EPSD100248820] System hang up on 0x34 randomly when MFG jumper is connected on RO board.

================================================================================
                01.01.D109
================================================================================
    1. [EPSD100028598] Get Node Manager Power Characterization Range value is 00 via ipmitool NM command
    2. Change "System Date" help string following product Setup Spec.
    3. [EPSD100029148] Boot Manager couldn't detect SATA DVDROM under legacy RSTe RAID Mode.

================================================================================
                01.01.D108
================================================================================
    1. [EPSD100028942] System time will become 01/01/2015 after set System Date before year 2015 and then Save & Reset.
    2. [EPSD100248985] 71605 Raid card OpRom control option cannot be seen under UEFI mode.
    3. [EPSD100248795] "Load User Default Values" option no function for some BIOS settings.
    4. Sync CRB BIOS V90_14 RC 1.2
    5. Microcode upate to 0002E

================================================================================
                01.01.D106
================================================================================
    1. BP/CP core sync to latest common tree.
    2. Roll back CP sync 4K HDD support code.
    3. Update ME update code according to the new ME layout.
    4. [EPSD100029105] New connected Network device will not list in bottom of DBOL.

================================================================================
                01.01.D105
================================================================================
    1. Sync latest CPPC code.
    2. Update ME FW to PC RC3 4.0.3.36

================================================================================
                01.01.D104
================================================================================
    1. [EPSD100246878] It is ineffective when you press NMI button.
    2. [EPSD100029092] New connected USB device will not list at buttom of DBOL when USB boot priority is disabled and SBOL snapshot has been taken.
    3. [EPSD100248942] No error report both in Error manage and SEL viewer when Microcode is updated missing.

================================================================================
                01.01.D103
================================================================================
    1. Update FVLEGACYCSMBIN to CL_255301.

================================================================================
                01.01.D102
================================================================================
    1. [EPSD100029339] Set core number to 1 under "Active Processor Cores" option, save and reboot to OS will occur BSOD:ACPI_BIOS_ERROR.
    2. [EPSD100029073] Memory ECC error injection information is incorrect in both SEL Viewer and system log.
    3. [EPSD100249024] ITK support for OA2.x.
    4. Based on EA team suggestion to set the PCH PCIE Rx CTLE in High Speed I/O (HSIO) Control Register.
    5. [EPSD100247152] Error message didn't display correctly in Error Manager after clear remove CMOS battery or clear CMOS jumper.
    6. Update RSTe option ROM and EFI driver to be version 4.3.0.1018.

================================================================================
                01.01.D101
================================================================================
    1. [EPSD100248853] DFT 1914 rule test was failed.
    2. [EPSD100248881] After install drivers, device manage still yellow mark.
    3. [EPSD100248945] UEFI RHEL7.0 and UEFI RHEL 7.1 will be hang in black screen with a cursor under UEFI mode.
    4. [EPSD100248131] Sysinfo_v14.0.4:  incorrect BIOS option was dumped in 'BIOS Settings' part in sysinfo_log.txt.
    5. [EPSD100248865] SUT can't boot up after 4 hynix 16G DIMMs attached on Beta1 board.
    6. [EPSD100248472] Total Memory can't indentified on Main and Memory Configuration screen with "hynix 16G" memory.

================================================================================
                01.01.D099
================================================================================
    1. [EPSD100248817] No nvram auto recovery error i BIOS error manage after corrupt whole nvram region.
    2. 'PCI out of resource error" can't triggered in error manage.
    3. [EPSD100248449] pci_error_sig_check() has warnings about pcie root port setting.

================================================================================
                01.01.D098
================================================================================
    1. [EPSD100248595] Syscfg_v14.0.6: Run cmd syscfg /bbosys "" 7 6 5 4 3 2 1 change bbo order will be fail.
    2. [EPSD100248558] 3% of the Beta1 build FAB2 boards can not keep the correct system date and time after reboot/cold boot.
    3. [EPSD100029353] Temp WA to SUT can't boot up after 4 hynix 4G/8G DIMMs attached on Beta2 board.
    4. [EPSD100029259] Failed to boot from Legacy PXE for X540-T2 Add-on card. (Error message: PXE-EC8: !PXE structures was not found in UNDI driver code segment.)

================================================================================
                01.01.D097
================================================================================
    1. [EPSD100028746] After disable the "Reset on CATERR" in BIOS,  SUT still reset after CATERR occurred for a while.
    2. [EPSD100029115] Console Redirection working with previous settings when SOL is Enabled.
    3. [EPSD100247152] Error message didn't display correctly in Error Manager after clear remove CMOS battery or clear CMOS jumper.
    4. [EPSD100028126] [2nd sourcen M/B] System stops at 234 loops during DC cycle test.
    5. Integrate new version option ROM and EFI driver for ESRT2.

================================================================================
                01.01.D096
================================================================================
    1. [EPSD100029073] Memory ECC error injection information is incorrect in both SEL Viewer and system log.
    2. [EPSD100248814] F10 key behavior is inconsistent after change different BIOS setting.

================================================================================
                01.01.D095
================================================================================
    1. [EPSD100029076] SBO is still enabled when use syscfg utility to change Boot Order.
    2. [EPSD100247075] Need develop a debug revision of runtime setvariable driver.
    3. Fixed hynix 4G DIMM can't enter OS issue.

================================================================================
                01.01.D093
================================================================================
    1. [EPSD100029115] Console Redirection working with previous settings when SOL is Enabled.
    2. [EPSD100028476] BIOS Nic configuration show IO module 82599 as X520.

================================================================================
                01.01.D092
================================================================================
    1. [EPSD100248538] System will pop-up warning message after change some settings via BIOS setup.
    2. [EPSD100245845] Console Redirection item will show disable and gray out when press F9 to load default BIOS setting.(setup browser issue)
    3. [EPSD100248007] CP_CR_1258:EPSD100242284: sysinfo V13.10: The value of "Microcode Revision" in sysinfo_log.txt is not consistent with Setup Page value with two CPUs.
    4. [EPSD100028808] No Payload Boot entry in Boot Manager page after update BIOS with  'Pay Load Boot' enabled.
    5. [EPSD100029102] "PCI out of resource error" can't triggered in error manage.
    6. [EPSD100028253] Flash ME fail via OFU tool that will show error message "error while parsing the cfg file
    7. [EPSD100248478] iFlash32_v14.0.2:ME update fail
    8. [EPSD100029234] Fail to install legacy Windows2012R2, UUT will BSOD and reset after loading files.
    9. Update micro code to 001E
    10.Sync V89_03 RC and ACPI table update.

================================================================================
                01.01.D089
================================================================================
    1. [EPSD100248757] UUID will chang back to primary value after remove MFG jumper.
    2. [EPSD100028283] The word string "Legacy Network Device Order" would be changed when remove USB key during storage OPROM/Network OPROM.
    3. [EPSD100248532] Change Execute Disable Bit option then press F10 or select "Save Changes and Exit", SUT not reboot will boot to the first boot device.
    4. [EPSD100246997] Intergrated IO Configuration /fast boot/OverClocking/SVID/FIVR/Override ICC Spread Spectrum Configuration/  list in BIOS cap file with ITK ,but these option does not display in BIOS Setup.
    5. [EPSD100028454] SATA SI setting data is different between BIOS RD006 and RD032.
    6. [EPSD100248758] SUT will hang up on first power after corrupt nvram blocks.
    7. [EPSD100248791] DP port and VGA Port Output options don't displayed in D087 BIOS.

================================================================================
                01.01.D087
================================================================================
    1. [EPSD100028454] SATA SI setting data is different between BIOS RD006 and RD032.
    2. [EPSD100028401] A few of symptom about onboard NICs can found within Type 41.
    3. [EPSD100028542] SUT could not dump the NVRAM area for onbaord NIC by running the dmpstore EFI shell command under MFG mode.
    4. [EPSD100028616] System cannot occurs memory multi-bit event after switch rework multi-bit memory jumper.
    5. Sync CRB bios V88_05, RC 1.0 and microcode update.

================================================================================
                01.01.D085
================================================================================
    1. Updated to Legacy ESRTII A.15.06081622I.
    2. Updated to Legacy/EFI RSTe 4.3.0.1013
    3. [EPSD100029151] SUT would hang at black screen after boot to SATA DVDROM under Legacy ESRT2 RAID Mode.

================================================================================
                01.01.D084
================================================================================
    01. [EPSD100248005] CP_CR_1277:Fix Klocwork Scan failures.
    02. [EPSD100028945] There should no "8541 Memory disabled DIMM_A2" error in Error Manager when an DIMM is installed in Slot 1(Black Slot) and no DIMM is installed in Slot 0(Blue Slot).
    03. [EPSD100248538] System will pop-up warning message after change some settings via BIOS setup.
    04. [EPSD100027755] "System Boot Timeout" default setting that modified by ITK would be changed after Clear CMOS.
    05. [EPSD100248673] R1+D0 board will hang up 0x96 during post after VGA Out put set to processor graphics.
    06. ME FW update to Pre-PC2 4.0.3.15

================================================================================
                01.01.D081
================================================================================
    01. [EPSD100248132] "Enter Password"  is dispatched,even password is not set in BIOS Setup.

================================================================================
                01.01.D080
================================================================================
    01. [EPSD100248372] Get SPS version by spsinfo utility failed.
    02. [EPSD100248453] System screen will hang up after ESRT2 oprom dispatched.
    03. [EPSD100028585] Help Text of field "PCIe Link Speed Control" is empty.
    04. [EPSD100248448] There is no BIOS "platformID" variable available in EFI shell.

================================================================================
                01.01.D079
================================================================================
    01. [EPSD100248154] The new added EFI boot option will be deleted when press F2 directly enter BIOS setup.
    02. [EPSD100247184] The BIOS admin password could be cleared after BIOS update NVRAM.
    03. [EPSD100028042] SUT cannot power on successfully when populated Xeon phi 7120 card to SUT.
    04. [EPSD100028485] Similar uefi network boot device name listed in boot manager page while populated powerville on RO sku.
    05. [EPSD100027982] The system GUID which retrieved by "Get System GUID" command does not match with the BIOS Setting

================================================================================
                01.01.D078
================================================================================
    01. Fixed ECC error cause smi storm.
    02. Roll back ME config to fix ME in recovery mode issue.

================================================================================
                01.01.D077
================================================================================
    01. [EPSD100248531] Board ID of IFWI Version is incorrect for S1200SP in both POST and Setup Menu.
    02. [EPSD100248326] After Press F12 during post,system will boot up from first boot sequence rather than boot from network with UEFI mode.
    03. [EPSD100028474] BIOS can't detect IO module 82599 10G UEFI iSCSI. But onboard ROM UEFI ISCS can detect.

================================================================================
                01.01.D076
================================================================================
    01. [EPSD100247859] SMBIOS type 38 show 2 times at BIOS R014.
    02. [EPSD100247244] Unecessary logs for system event appear after DC cycle.
    03. [EPSD100028746] After disable the "Reset on CATERR" in BIOS,  SUT still reset after CATERR occurred for a while.
    04. [EPSD100028818] J9K1 RAID key, J9K2 MFC, and J9B2 Chassis INTR are not defined in SMBIOS Type 12.
    05. [EPSD100027827] it's useless to change some settings under Processor Configuration and CPU P state Control.

================================================================================
                01.01.D074
================================================================================
    01. CSM&USB stack updated.

================================================================================
                01.01.D073
================================================================================
    01. [EPSD100027827] it's useless to change some settings under Processor Configuration and CPU P state Control.
    02. [EPSD100027619] Only one ME update log in SEL when update D008 ME successfully/
    03. [EPSD100027561] Failed to update ME with iflash tool. It would show error message.
    04. [EPSD100247015] There are some failures in SCT2.3.1C test log.
    05. [EPSD100248483] BIOS option cannot be saved correctly in syscfg.ini.

================================================================================
                01.01.D071
================================================================================
    01. [EPSD100028600] The field of Core Count with Type 4 would be changed when Active Processor Cores changed.
    02. [EPSD100247019] Some table can not be found when excute Acpitest utility.Table: ERST, BERT, HEST, EINJ, SPCR, WDDT.
    03. [EPSD100028809] NIC1 will be disabled while [VGA Port Output] = [Processor graphics], [Primary Display] = [Display port].
    04. [EPSD100247936] Many incorrect BIOS options were dumped in syscfg.ini.
    05. [EPSD100028674] BMC SOL will not load back to default setting and CR option is grayed out after press F9 to load BIOS default.
    06. [EPSD100248420] "AHCI Capable Controller" information in POST Diagnostic Screen is incorrect.
    07. [EPSD100027666] Windows 2012R2 boot fail after installed with HDD:ST6000NM0004.
    08. [EPSD100028674] BMC SOL will not load back to default setting and CR option is grayed out after press F9 to load BIOS default.
    09. [EPSD100028673] When BMC SOL is enabled, the Console Redirection related options would not be kept with their before value.
    10. [EPSD100027631] The prompt time of the OPROM is too short while RSTe RAID had been set.
    11. [EPSD100028841] SUT would emit 3 beep code and hang at 80port 0xE8 after set "Memory Operating Speed Selection" to 1866MHz.

================================================================================
                01.01.D069
================================================================================
    01. [EPSD100028804] Both of item name and Help Text are incorrect for "Primary Display" in BIOS Setup.
    02. [EPSD100027755] "Resume on AC Power loss" and "System Boot Timeout" default setting that modified by ITK would be changed after Clear CMOS.

================================================================================
                01.01.D068
================================================================================
    01. [EPSD100027524] No "Invalid DIMM Population" event on POST screen when DIMM populateion invalid.
    02. [EPSD100028674] BMC SOL will not load back to default setting and CR option is grayed out after press F9 to load BIOS default.
    03. [EPSD100027570] "Auto Recovery to backup BIOS image" function is not workable, SUT would hang at 80port 0xF2.
    04. [EPSD100247064] SUT can not boot from backup area after primary BIOS image corruption.
    05. Update ME module to 4.00.03.08.
    06. Update ESRT2 EFI driver to A.14.05071212I.

================================================================================
                01.01.D066
================================================================================
    01. [EPSD100027558] System Boot Timeout continued counted even pressing hot key to booting system.
    02. [EPSD100248299] Change boot order and press F10,system will boot driectly rather than save and reboot.
    03. [EPSD100027800] Payload boot failed with IPMI command to force payload boot.
    04. [EPSD100028108] The [Esc] key can't be used in Setup to initiate a "Discard Changes & Exit" action.

================================================================================
                01.01.D064
================================================================================
    01. [EPSD100027682] SUT would hang at 80port 0x96 after set both NIC1 Controller/NIC2 Controller to disabled and then save & reset.
    02. [EPSD100027800] Payload boot failed with IPMI command to force payload boot.
    03. [EPSD100247713] Sysinfo_v14.0.3:some value of BIOS option display "Unknow" in sysinfo_log.txt.
    04. [EPSD100028540] BIOS option PCIe slot5 OpROM control still can found within RO sku even SUT without the PCIe slot.
    05. [EPSD100247182] C state show incorrectly after disable processor C3/C6 support in BIOS setup menu.

================================================================================
                01.01.D063
================================================================================
    01. [EPSD100247936] many incorrect BIOS options were dumped in syscfg.ini & some BIOS options cannot be dumped in.
    02. [EPSD100247723] "AHCI Capable Controller" Information in POST Diagnostic Screen is disappeared when disable the AHCI Capable SATA Controller.
    03. [EPSD100028486] IOM port 1 and 2 PXE for Niantic module are gray out. BIOS setting of "Enable PXE 10GbE Option ROM" changed to Disabled after populated it on RO.
    04. [EPSD100028005] No 0012/5220 error messages in Error Manager and SEL when remove CMOS battery.
    05. [EPSD100028654] ESRT2_Silver_Pass: Hotplug is not working in EFI/HII.
    06. Update RC v83_05 and update microcode, AHCI legacy oprom.
    07. [EPSD100248090] Some PCH GPIO setting doesn't match requirement.
    08. [EPSD100028657] DHP failed to reconnect automatically after a critical message.

================================================================================
                01.01.D061
================================================================================
    01. [EPSD100028227] "OEMID" field is not "INTEL" and "OEM Table ID" field is not "S1200SPL" for some ACPI "SSDT" Table.
    02. [EPSD100247911] CP_CR_1533:CCB261-Enable/Disable MCE SMI by setup option.
    03. [EPSD100027827] it's useless to change the options Intel(R) Hyper-threading Tech, Active Processor Cores, Execute Disable Bit,
                            Intel(R) VT for Directed i/o under processor configuration,enhanced intel SpeedStep(R))Tech,Intel(R)Turbo Boost
                            Tech under CPU P state controle.
    04. [EPSD100027847] No "Invalid DIMM Population" event and 8501 error message on POST screen when DIMM population invalid.

================================================================================
                01.01.D059
================================================================================
    01. Update label to D059.

================================================================================
                01.01.D056
================================================================================
    01. [EPSD100247951] Wording mistake in  "User Configuration"and Setup Server Information Page.
    02. [EPSD100027633] ESRT2 OPROM loading time is too long and hotkey "CTRL+E" does not work.
    03. [EPSD100248178] BIOS update is fail with "iflash32.efi" tool.
    04. [EPSD100248067] Setup menu for other misc items.
    05. [EPSD100247863] The help text of "Early System Boot Timeout" show incorrect.
    06. [EPSD100248196] Update Varstore patch tool to support more variables.
    07. [EPSD100027630] LightUiApp feature update.
    08. [EPSD100027682] SUT would hang at 80port 0x96 after set both NIC1 Controller/NIC2 Controller to Disabled and then save & reset.
    09. ME FW update to 4.0.2.47

================================================================================
                01.01.D054
================================================================================
    01. [EPSD100028584] There is no Legacy FCoE OpROM in POST for IOM X540.
    02. [EPSD100028541] BIOS option "FCoE 10GbE Option ROM" can found within BIOS setup even no IOM connected to SUT.
    03. [EPSD100247513] Some ports connector information lost in SMBIOS.
    04. Update ACM Binary file.

================================================================================
                01.01.D053
================================================================================
    01. [EPSD100027462] The value of memory Device Locator string within SMBIOS not consistent with silkscreen.
    02. [EPSD100028068] BMC Web display DIMM_A1 and DIMM_B1 info when DIMMs insert slot A2 and B2 in M/B.
    03. [EPSD100247512] J4K1 jumper information should not exist SMBIOS type 12.
    04. [EPSD100028262] Memory speed downgrade from 2133MHz to 1867MHz during AC cycle test (7-1,14cycles,10-1,10cycles,25C).
    05. [EPSD100027533] Boot Manager displayed duplicated UEFI boot device after reboot from UEFI RHEL 7 OS with UEFI W2012R2 OS HDD connected.
    06. [EPSD100027590] When system into sleep S1 or S3, power LED always is ON under W2012R2 with November update.
    07. [EPSD100245821] At UEFI RAID ESRT2 mode, "Check All" option no function when config RAID.
    08. [EPSD100028004] The "Mass Storage Devices" option is hidden when press F9 to load default.
    09. [EPSD100027855] 4 PCIe slots table within Type 9 wtih BIOS D0017. It's not consistent with HW designed.
    10. [EPSD100027856] All Slot Type field within Type 9 under BIOS D0017 having similar value.
    11. [EPSD100027631] The prompt time of the OPROM is too short while RSTe RAID had been set.
    12. [EPSD100027682] SUT hang at 80port 0x96 after set both NIC1/NIC2 controller to disabled.
    13. Solve issue that OEM Logo shows at diagnostic even Quiet boot is disabled.

================================================================================
                01.01.D051
================================================================================
    01. ID change based on D050.

================================================================================
                01.01.D050 (#219679)
================================================================================
    01. [EPSD100027442] "BMC DHCP Host Name" is still grayed out and inactive even IP Source is set to "Dynamic".
    02. [EPSD100028365] Add blank line between each NIC Type in BIOS Setup/NIC Configuration.
    03. [EPSD100028435] Delete SGX Option in setup.
    04. [EPSD100247788] Linux(both Redhat7&SUSE12) OS installation failed in both legacy and UEFI mode.
    05. [EPSD100028420] SUT would not boot into EFI shell automatically in BIOS Recovery mode.
    06. [EPSD100247939] Backup BIOS cannot be updated successfully by command:iflash32.efi -u D036.cap UpdateBackupBios
    07. Update ME FW to 4.0.2.44

================================================================================
                01.01.D048
================================================================================
    01. [EPSD100247173] SUT can not use Oa2intel tool to insert OEM data.
    02. [EPSD100247531] With Grantley code, LegacyRegion->Unlock can not enable memory write under release mode
    03. [EPSD100028393] Unknown field "DPR Memory Size" appeared after set "Intel(R) TXT" to Enabled in BIOS Setup.
    04. [EPSD100247664] SUT would auto reboot when boot into RMS25JC080 OPROM about 20 sec.
    05. [EPSD100027352] Primary BIOS Version showed as "8" in diagnostics screen.
    06. [EPSD100028402] Incorrect value of Cache Configuration Field for L2 and L3 cache within Type 7.
    07. [EPSD100247513] Some ports connector information lost in SMBIOS.
    08. [EPSD100027740] USB device is still functional even when the USB Controller option is disabled.
    09. [EPSD100247538] syscfg cannot read "Current Memory Speed" under Windows.
    10. [EPSD100027695] Help Text for item "Correctable Error Threshold" is not correct.
    11. [EPSD100027847] There is no retries of the boot when change Boot Option Retry to enable.
    12. [EPSD100027594] The Console Redirection option is gray out and unchangeable after press F9 to load BIOS default values.
    13. [EPSD100028087] In BMC LAN Configuration/User Configuration, the default privilege of User3 is Administrator, but it should be User.
    14. [EPSD100247593] Failed to write the GUID to BIOS flash in MFG mode.

================================================================================
                01.01.D046
================================================================================
    01. For AutoBuild debug after code merge.

================================================================================
                01.01.D044
================================================================================
    01. [EPSD100027353] Fix Processor/Memory info not correct in OemPostScreen issue.
    02. [EPSD100027597] Enable 60/64 emulation for E3-1200 v5 PCH, fix USB keyboard/mouse not work under dos.
    03. [EPSD100027672] Type 7 Error Correction type is incorrect in SMBIOS log of BIOS D008. 
    04. [EPSD100027506] DIMM manufacturer field did not be filled with "Empty/NO DIMM" when no DIMM populated on slots. 
    05. [EPSD100027461] The value of number of memory devices within SMBIOS not consistent HW spec defined. 
    06. [EPSD100027462] The value of memory Device Locator string within SMBIOS not consistent with silkscreen printed. 
    07. [EPSD100027460] The value of maximum memory capacity within SMBIOS not consistent HW spec defined.
    08. [EPSD100027517] When press NMI button in W2K12R2-64_November, system cannot display BSOD.
    09. [EPSD100028308] Remove boot device will cause SBOchange to disabled.
    10. [EPSD100027381] There is no Help Text for items "Uncore Power Management", "CPU P State Control" and "CPU C State Control" in BIOS Setup.
    11. [EPSD100245848] Enable Console Redirection, Remote system show garbage when set Baud Rate to 9.6/19.2/38.4/57.6K.
    12. [EPSD100028006] POST Code LEDs show 0xFF not 0xE8 when no DIMM installed.
    13. [EPSD100027336] Few of processor infomration within Processor Configuration page under BIOS display N/A.
    14. [EPSD100027603] Console Redirection setting is disabled and unchangeable after Enable any of the three BMC LAN SOL.
    15. [EPSD100247097] The power policy don't support S1, but support S4.
    16. [EPSD100028089] NIC1 will be disabled while [VGA Port Output] = [Processor graphicd], [Primary Video] = [VGA port].
    17. [EPSD100027936] "Intel(R) Storage Module" showed as "None" even connected RMS25JB080.
    18. [EPSD100027573] There is only one log "BIOS Recovery Complete" in SEL indicating recovery boot.

================================================================================
                01.01.D036
================================================================================
    01. [EPSD100247290] SUT can't power on and hang with POST error code 0x96 when no any boot device connect and disable NIC PXE boot at BIOS R011.
    02. [EPSD100027644] "OEM Table ID" is not correct in ACPI DMAR Table.
    03. [EPSD100027739] One onboard LAN boot device disappear and "Not enough memory available" event logged in BIOS Error Manager & SEL when populate x540-T2 LAN card in MB.
    04. [EPSD100027406] No RMM4 Lite port connector information table within SMBIOS.
    05. [EPSD100027852] Value of Processor Upgrade Field within Type 4 in BIOS D0017 not consistent with HW spec defined.
    06. [EPSD100247230] DIMM Thrm Mrgn 1 sensor is always in unknown state

================================================================================
                01.01.D032
================================================================================
    01. [EPSD100247059] BIOS need to filter ITK security items.
    02. [EPSD100027936] "Intel(R) Storage Module" showed as "None" even connected RMS25JB080.
    03. [EPSD100027775] No OPROM for IOMs during POST and new network boot devices listed in Boot Maintenance Manager page after boot into BIOS Setup.
    04. [EPSD100027731] Fix POST dignostic screen doesn't display USB keyboard/mouse detected info.
    05. [EPSD100247241] Boot Order can't be changed when SBO is enabled at BIOS R011.
    06. Update CPU Microcode to 0000001D revision.
    07. [EPSD100246833] No beep code during POST.
    08. [EPSD100246630] No "Early System Boot Timeout" option at Advanced Boot Options, but PCSD BIOS Setup Design Document has.
    09. [EPSD100027474] It cannot identify which one is NIC1 or NIC2 for Onboard LAN UEFI boot device.
    10. [EPSD100028038] No COM Port device in device manager in W2k12R2-64.
    11. [EPSD100247177] Enter BIOS setup through User password then Press F9 to load default, all BIOS settings becomes available and can be modified.
    12. [EPSD100027342] MSR IA32_MISC_ENABLE bit 34 is not 1 when execute disable bit set to disable.
    13. [EPSD100027672] Type 7 Error Correction type is incorrect in SMBIOS log of BIOS D008.
    14. [EPSD100027373] Socket Designation string within type 4 not consistent with requested displayed "CPU x".
    15. [EPSD100027511] Incorrect value of Device Type field within SMBIOS Type 41 for integrated SATA Controller.
    16. [EPSD100027503] USB flash drive would not detect as a floppy drive when set the Storage Emulation to "Forced FDD".

================================================================================
                01.01.D026
================================================================================
    01. [EPSD100027505] IPMI Device Information table is Required but was not found by PETS tool.
    02. [EPSD100247152] The 5220 error message didn't display in Error Manager after clear remove CMOS battery or clear CMOS jumper.
    03. [EPSD100027596] Information of System Configuration Options within SMBIOS not consistent with HW silkscreen.
    04. [EPSD100247149] The help text of AHCI Capable SATA Controller displays incorrectly.
    05. [EPSD100027682] SUT would hang at 80port 0x96 after set both NIC1 Controller/NIC2 Controller to Disabled.
    06. Sync RC to V78_01 and ME to 4.0.2.12 and microcode to 0019.
    07. [EPSD100246635] Connect a PCI-E RAID module or SAS RAID module, no RAID info at BIOS setup.
    08. [EPSD100027517] When press NMI button in W2K12R2-64_November, system cannot display BSOD.
    09. [EPSD100027362] Serial port not detected message displayed after clean CMOS.
    10. [EPSD100027377] Storage Infomaion is not correct in post screen.
    11. [EPSD100246757] Windows2012 R2 OS can not be installed or booted-into with all 4 DIMMs applied.
    12. [EPSD100247149] The help text of AHCI Capable SATA Controller displays incorrectly.
    13. [EPSD100027517] When press NMI button in W2K12R2-64_November, system cannot display BSOD.
    14. [EPSD100027796] Help Text for "Change Boot Order" is not clear enough to let user know how to change Boot Order.
    15. [EPSD100247165] Yellow mark display in device manager.
    16. [EPSD100027643] "Preferred_PM_Profile" field is not correct in ACPI FADT Table.
    17. [EPSD100027943] "Creator ID" is empty in ACPI TCPA Table.

================================================================================
                01.01.D023
================================================================================
    01. EPSD100027326 It display “Press F7 to show boot menu option” during POST, but S1200SP not support this function.
    02. [EPSD100027343] When system power on without memory, speaker cannot beep. 
    03. [EPSD100027443]  Speaker does not beep during speaker 1KHz to 10KHz test
    04. Update ServerAmiRestrictedPkg binary to CP CL203208
    05. [No slighting]MSR Value is wrong after change CPU Power and Performance setting
    06. [No slighting] There is no item iSCSI Option ROM in BIOS Setup
    07. [EPSD100027700]Item name is not correct for "NIC2 Controller" in BIOS Setup.
    08. NO_SIGHTING: Sync BootOrder code from PCSD_COMMON tree
    09. [No Slighting]Some RAID mode under UEFI mode issue. 
    10. [EPSD100247056]Fixed The option of Primary Video and VGA Port Output is not gray out and accessible issue. 
    11. [EPSD100027637] Fixed No screen output when set "VGA Port Output" to "Processor graphics" issue.
    12. [EPSD100027741]Sometimes the "Submit fail for form:!." box will pop up when press F10 to save changed BIOS setting
    13. [No Sighting]Some RAID mode and UEFI issue For RO SKU, SE SKU and EV.
    14. [EPSD100027341] There is no popup message to notice user to confirm when pressing F10 Hot Key in BIOS Setup. 
    15. [EPSD100027381]There is no Help Text for items "Uncore Power Management", "CPU P State Control" and "CPU C State Control" in BIOS Setup.
    16. [EPSD100027409]The Data rows arrangement not align with title under error manager.
    17. [EPSD100027508]System Date did not roll back to 01/01/2013 after CMOS battery or clean CMOS with jumper
    18. [EPSD100027409]The Data rows arrangement not align with title under error manage
    19. [EPSD100244684]Enter 3 times incorrect Admin PWD, no error log at Error manager and SEL log
    20. [No slighting] Update setup page according 0.9 setup spec
    21. [EPSD100027511] - Incorrect value of Device Type field within SMBIOS Type 41 for integrated SATA Controller. 
    22. [EPSD100027515] - All of onboard devices have similar value within SMBIOS for Bus Number, Device Number and Function Number field except Integrated SATA Controller. 
    23. [EPSD100027514] - Incorrect value of Device Type field within SMBIOS Type 41 for device enabled or not. 
    24. [EPSD100027507] - Reference Designation String within Type 41 for onbaord network not consistent HW designed. 
    25. [EPSD100027509] - Onboard IO Module information could found in type 41 even connector removed from current baseboard. 
    26. [EPSD100027373] Socket Designation string within type 4 not consistent with requested displayed "CPU x". 
    27. [EPSD100247027] Type 4 Socket Designation string is "U3E1" , not "CPU x" 
    28. [EPSD10002766]  The HDD's(ST6000NM0004) capacity detects wrong in BIOS 
    29. [No slighting] Pvmode test error on the Greenlow platform.
    30. [EPSD100027506] DIMM manufacturer field did not be filled with "Empty/NO DIMM" when no DIMM populated on slots. 
    31. [EPSD100027462]  The value of memory Device Locator string within SMBIOS not consistent with silkscreen printed. 
    32. [EPSD100027471] All of DIMMs populated on SUT having similar Asset Tag string within SMBIOS. 
    33. [EPSD100247155][Platform/Common] [Enable FRB2 and make sure it workable then change FRB2 to disable, at the first time FRB2 still has function.]

================================================================================
                01.01.D017
================================================================================
    01. Memory and PCIe error logging feature add
       
================================================================================
                01.01.D014
================================================================================
    01.[EPSD100246882][Password clear jumper function is  ineffective]
    02.[EPSD100246757]Windows2012 R2 OS can not be installed or booted-into with all 4 DIMMs applied
    03. VT-D enable function 
    04.[EPSD100027384]["AHCI Controller Configuration" is still showed as "8 ports of 6Gb/s SATA" even "AHCI Capable SATA Controller" is set to Disabled..]
    05.[EPSD100247017][No Gigabit NIC driver can be found in EFI shell under UEFI mode.]
    06.[EPSD100027382][There is a lot of unsupported selection for item "Memory Operating Speed Selection" in BIOS Setup..]
    07.[EPSD100027387][There is no item "iSCSI Option ROM" in BIOS Setup.]
    08.[EPSD100246581][MSR value is wrong after change CPU Power and Performance setting]
    09.[EPSD100027345&EPSD100246426&EPSD100027330][Getting the value "Not Supported" even enabled or disable BIOS option "Direct Cache Access".]
    10.[EPSD100246961,EPSD100246874] Fixed issue "S1200SP Mezz device lost when slot4/6 has PCIE add-in card installed" and "SUT will hang when install PCIE RAID card in slot 4"
    11.Add SMBIOS type10 for SE/RO and Type13 issue fix
    12.[EPSD100246877] System can't shutdown


================================================================================
                01.01.D008
================================================================================
    1. Update RC 071_08
    2. Add iGFX legacy option rom.
    3. Update CPU microcode.
    4. Update ME firmware to revision to:4.0.2.5
    5. Add RSTe Legacy oprom and UEFI driver. add ESRT2 oprom.
    
================================================================================
                01.01.D006
================================================================================
    1. Added the UBA Multi Platform support for Greenlow platform.
    2. Add UBA Oprom control and PCIe Link Speed function
    3. Add password & NMI button & Frontpanel lock support
    4. Add PMI acpi table support.
    5. Add system uuid support

===============================================================================
                    Issues Fixed
================================================================================
================================================================================
                01.01.D008
================================================================================
    1. [EPSD100246852] Fixed Power LED of Front Panel is always off in Chassis issue.
    2. Fixed SilverPssLC Sku no Pcie Slot6 item in setup
    3. Fixed BIOS setup can't get ME firmware revision number
    4. Update GPIO table for PCIe slot5 clock output.
    5. Fixed SUT can not update FD regions or ME regions with iflash32 utility issue.
    6. Update SATA Port number string from "0-5" to "0-7".
    7. SMBIOS type 8/9/10 LC sku porting


================================================================================
                01.01.D006
================================================================================
    1. Update SPS ME FW to support C0 PCH and fixed SATA port can't detect HDD issue.
    2. Fix system will have blue screen when install windows 2008 R2 under legacy mode (Linux legacy install only)
    3. Temp WA for SMBIOS type 1/2/3, need to be roll back after final solution completed
    4. Modify TCO base address
    5. update BP core to 1.2.1.1
    6. Fixed debug serial port output abnormal issue
    7. update legacy stack binary, enable usb stack
    8. Fixed Reovery mode support code and memory info dpx add in RC code


















