//****************************************************************************
//                   INTEL CORPORATION PROPRIETARY INFORMATION
//       This software is supplied under the terms of a license agreement or
//       nondisclosure agreement with Intel Corporation and may not be copied
//       or disclosed except in accordance with the terms of that agreement.
//         Copyright (c) 2016 Intel Corporation. All Rights Reserved.
//***************************************************************************
//
// Data in this file is based on the S7200AP rev 0.85 FSC SDR spreadsheet, minus LAAC settings.
//
//
// SDR Tag Usage
//
//====================================================================//
// (1) Chassis related TAG
//====================================================================//
// _SDR_TAG    'BCP_2U4N'               // SDRs for 2U4N chassis
// _SDR_TAG    '2U4N_BP_X35'            // SDRs for 3.5" HDD-BP
// _SDR_TAG    '2U4N_BP_X25'            // SDRs for 2.5" HDD-BP
// _SDR_TAG    'TEST_PLATE'             // SDRs for Test Plate for NPI: PO Kit
// _SDR_TAG    'OTHER'                  // SDRs for OTHER chassis

//====================================================================//
// (2) Temperature sensors
//====================================================================//
// _SDR_TAG    'HSBP_TEMP'              // SDR for HSBP Temp
// _SDR_TAG    'PSOC_TEMP'              // SDR for HSBP PSOC Temp
// _SDR_TAG    'DIMM_THRM_2'            // SDR for DIMM Thermal Margin 2

//====================================================================//
// (3) Fan sensors
//====================================================================//
// _SDR_TAG    'SYS_FAN_2U4N'           //System Fan 2U4N SKU
// _SDR_TAG    'SYSTEM_FAN_1A'          //System Fan SYSTEM_FAN_1A
// _SDR_TAG    'SYSTEM_FAN_1B'          //System Fan SYSTEM_FAN_1B
// _SDR_TAG    'SYSTEM_FAN_2A'          //System Fan SYSTEM_FAN_2A
// _SDR_TAG    'SYSTEM_FAN_2B'          //System Fan SYSTEM_FAN_2B
// _SDR_TAG    'SYSTEM_FAN_3A'          //System Fan SYSTEM_FAN_3A
// _SDR_TAG    'SYSTEM_FAN_3B'          //System Fan SYSTEM_FAN_3B
// _SDR_TAG    'SYSTEM_FAN_4A'          //System Fan SYSTEM_FAN_4A
// _SDR_TAG    'SYSTEM_FAN_4B'          //System Fan SYSTEM_FAN_4B
// _SDR_TAG    'SYSTEM_FAN_5A'          //System Fan SYSTEM_FAN_5A
// _SDR_TAG    'SYSTEM_FAN_5B'          //System Fan SYSTEM_FAN_5B
// _SDR_TAG    'SYSTEM_FAN_6A'          //System Fan SYSTEM_FAN_6A
// _SDR_TAG    'SYSTEM_FAN_6B'          //System Fan SYSTEM_FAN_6B
// _SDR_TAG    'OTHER_FAN_1A'           //System Fan OTHER_FAN_1A
// _SDR_TAG    'OTHER_FAN_1B'           //System Fan OTHER_FAN_1B
// _SDR_TAG    'OTHER_FAN_2A'           //System Fan OTHER_FAN_2A
// _SDR_TAG    'OTHER_FAN_2B'           //System Fan OTHER_FAN_2B
// _SDR_TAG    'OTHER_FAN_3A'           //System Fan OTHER_FAN_3A
// _SDR_TAG    'OTHER_FAN_3B'           //System Fan OTHER_FAN_3B
// _SDR_TAG    'OTHER_FAN_4A'           //System Fan OTHER_FAN_4A
// _SDR_TAG    'OTHER_FAN_4B'           //System Fan OTHER_FAN_4B
// _SDR_TAG    'OTHER_FAN_5A'           //System Fan OTHER_FAN_5A
// _SDR_TAG    'OTHER_FAN_5B'           //System Fan OTHER_FAN_5B
// _SDR_TAG    'OTHER_FAN_6A'           //System Fan OTHER_FAN_6A
// _SDR_TAG    'OTHER_FAN_6B'           //System Fan OTHER_FAN_6B

//====================================================================//
// (4) Chassis Intrusion
//====================================================================//
// _SDR_TAG    'CHASSIS_INTRU'          // Physical Security sensor
// _SDR_TAG    'LAN_LEASH'              // Physical Security sensor

//====================================================================//
// (5) Power Supply related sensors
//====================================================================//
// _SDR_TAG    'STICKY_PS1_VALID'       // PS1 has valid FRU
// _SDR_TAG    'STICKY_PS2_VALID'       // PS2 has valid FRU
// _SDR_TAG    'STICKY_PS1_1600W'       // 1600W Power Supply 1
// _SDR_TAG    'STICKY_PS2_1600W'       // 1600W Power Supply 2
// _SDR_TAG    'STICKY_PS1_2130W'       // 2130W Power Supply 1
// _SDR_TAG    'STICKY_PS2_2130W'       // 2130W Power Supply 2
// _SDR_TAG    'STICKY_REDUND_PS'       // Power Supply Redundancy

//====================================================================//
// (6) Factory sensors
//====================================================================//
// _SDR_TAG    'SHIPPING'               // SDRs for Shippings
// _SDR_TAG    'FCT'                    // SDRs for FCT
// _SDR_TAG    'FOQM'                   // SDRs for FOQM

//====================================================================//
// (7) Others
//====================================================================//
// Miscellaneous support tags:
// _SDR_TAG    'RISER_1_FRU'                   // SDRs for PCI Riser 1 
// _SDR_TAG    'RISER_2_FRU'                   // SDRs for PCI Riser 2 

//
// File Header Information
//

_LF_NAME       'S7200AP SDR File'
_LF_VERSION    '1.24'
_LF_FMT_VER    '1.50'
_IPMI_VERSION  '2.00'

//
// SDR Header Information
//

_SDR (
_START_ADDR    0000
_DATA_LEN      0000
_NVS_TYPE      'IMBDEVICE'
_DEV_BUS       FF
_DEV_ADDRESS   20

//*****************************************************************************
//
// Miscellaneous core sensor data records
//
//*****************************************************************************


_SDR_TYPE   02
_REC_LEN    002F

   // Sensor Record Header
   0001               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   01                 // Sensor Number

   // Record Body Bytes
   15                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   09                 // Sensor Type
   6F                 // Event / Reading Base Type
   7500               // Assertion Event Mask   --Power down/240VA power down/ A/C lost/Soft power control failure/Power unit failure =7500
   7500               // Deassertion Event Mask --Power down/240VA power down/ A/C lost/Soft power control failure/Power unit failure =7500
   7500               // Reading Mask & Settable / Readable Threshold Masks --Power down//240VA power down/ A/C lost/Soft power control failure/Power unit failure =7500
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Pwr Unit Status'  // String Bytes


_SDR_TYPE   02
_SDR_TAG    'STICKY_REDUND_PS'
_REC_LEN    002F

   // Sensor Record Header
   0002               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   02                 // Sensor Number

   // Record Body Bytes
   15                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   09                 // Sensor Type
   0B                 // Event / Reading Base Type
   FF00               // Assertion Event Mask
   FF00               // Deassertion Event Mask
   FF00               // Reading Mask & Settable / Readable Threshold Masks
                      //--Redundancy regained/Non-red: suff res from redund/Redundancy lost/Redundancy degraded/Non-red: suff from insuff/Non-red: insufficient/Redun degrade from full/Redun degrade from non-redundant=FF00
   00                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Pwr Unit Redund'  // String Bytes


_SDR_TYPE   02
_REC_LEN    002D

   // Sensor Record Header
   0003               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   03                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   23                 // Sensor Type
   6F                 // Event / Reading Base Type
   0F01               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0F01               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'IPMI Watchdog'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'BCP_2U4N'
_REC_LEN    002E

   // Sensor Record Header
   0004               // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   04                 // Sensor Number

   // Record Body Bytes
   17                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   05                 // Sensor Type
   6F                 // Event / Reading Base Type
   1000               // Assertion Event Mask
   1000               // Deassertion Event Mask
   1000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Physical Scrty'   // String Bytes


_SDR_TYPE   02
_SDR_TAG    'OTHER'
_REC_LEN    002F

   // Sensor Record Header
   0005               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   05                 // Sensor Number

   // Record Body Bytes
   0C                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   13                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0100               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'FP NMI Diag Int'  // String Bytes


_SDR_TYPE   02
_REC_LEN    002B

   // Sensor Record Header
   0006               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   06                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   F3                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'SMI Timeout'      // String Bytes


_SDR_TYPE   02
_REC_LEN    0030

   // Sensor Record Header
   0007               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   07                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   10                 // Sensor Type
   6F                 // Event / Reading Base Type
   1400               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0400               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'System Event Log' // String Bytes


_SDR_TYPE   02
_REC_LEN    002C

   // Sensor Record Header
   0008               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   08                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   12                 // Sensor Type
   6F                 // Event / Reading Base Type
   1000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   1000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'System Event'     // String Bytes


_SDR_TYPE   02
_REC_LEN    0026

   // Sensor Record Header
   0009               // Record ID
   51                 // SDR Version
   02                 // Record Type
   21                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   09                 // Sensor Number

   // Record Body Bytes
   0C                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   14                 // Sensor Type
   6F                 // Event / Reading Base Type
   0500               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0500               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C6                 // Type/Length Code
   'Button'           // String Bytes


_SDR_TYPE   02
_REC_LEN    002C

   // Sensor Record Header
   000A               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0A                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   28                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'BMC Watchdog'     // String Bytes


_SDR_TYPE   02
_REC_LEN    002B

   // Sensor Record Header
   000B               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0B                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   02                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'VR Watchdog'      // String Bytes


_SDR_TYPE   02
_REC_LEN    002E

   // Sensor Record Header
   000C               // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   0D                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   01                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'SSB Therm Trip'   // String Bytes


_SDR_TYPE   02
_REC_LEN    002D

   // Sensor Record Header
   000F               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   10                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   28                 // Sensor Type
   6F                 // Event / Reading Base Type
   1000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   1000               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'BMC FW Health'   // String Bytes


_SDR_TYPE   01
_SDR_TAG    'BCP_2U4N'
_REC_LEN    003E

   // Sensor Record Header
   0010               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   11                 // Sensor Number

   // Record Body Bytes
   17                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   63                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   11                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   02                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   14                 // Nominal Reading
   32                 // Normal Maximum
   00                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'System Airflow'   // String Bytes


_SDR_TYPE   03
_REC_LEN    0021

   // Sensor Record Header
   0011               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1C                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   12                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   01                 // Entity Instance
   2B                 // Sensor type
   70                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'FW Update Status' // String Bytes

_SDR_TYPE      03
_REC_LEN       001F

   // Sensor Record Header
   0012               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   87                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   01                 // Entity Instance
   28                 // Sensor type
   03                 // Event/Reading Type Code
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'AutoCfg Status'   // String Bytes

_SDR_TYPE   03
_REC_LEN    001F

   // Sensor Record Header
   0013               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   81                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   01                 // Entity Instance
   28                 // Sensor type
   03                 // Event/Reading Type Code
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'MTM Lvl Change'   // String Bytes
   
_SDR_TYPE   03
_REC_LEN    001D

   // Sensor Record Header
   0152           // Record ID
   51                 // SDR Version
   03                 // Record Type
   18                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D7                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   2A                 // Sensor type
   6F                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'Bad User PWD'   // String Bytes


//*****************************************************************************
//
// Baseboard and chassis related temperature related sensors
//
//*****************************************************************************

_SDR_TYPE   01
_REC_LEN    003D

   // Sensor Record Header
   0014               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   20                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   28                 // Nominal Reading
   32                 // Normal Maximum
   05                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   3C                 // Upper critical
   37                 // Upper non-critical
   00                 // Lower non-recoverable
   02                 // Lower critical
   04                 // Lower non-critical
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CD                 // Type/Length Code
   'BB Inlet Temp'	  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'HSBP_TEMP'
_REC_LEN    0039

   // Sensor Record Header
   0015               // Record ID
   51                 // SDR Version
   01                 // Record Type
   34                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   21                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   853A               // Assertion Event Mask   --[u,l][c,nc]=853A
   857A               // Deassertion Event Mask --[u,l][c,nc]=857A
   3B3B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=3B3B
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   19                 // Nominal Reading
   2D                 // Normal Maximum
   05                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   3C                 // Upper non-recoverable
   37                 // Upper critical
   32                 // Upper non-critical
   00                 // Lower non-recoverable
   02                 // Lower critical
   04                 // Lower non-critical
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   C9                 // Type/Length Code
   'HSBP Temp'        // String Bytes


_SDR_TYPE   01
_REC_LEN    0038

   // Sensor Record Header
   0016               // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   22                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   50                 // Nominal Reading
   5F                 // Normal Maximum
   05                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   67                 // Upper critical
   62                 // Upper non-critical
   00                 // Lower non-recoverable
   02                 // Lower critical
   04                 // Lower non-critical
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   C8                 // Type/Length Code
   'SSB Temp'		  // String Bytes


_SDR_TYPE   01
_REC_LEN    0038

   // Sensor Record Header
   0017               // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   23                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   3C                 // Nominal Reading
   5A                 // Normal Maximum
   05                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   64                 // Upper critical
   5F                 // Upper non-critical
   00                 // Lower non-recoverable
   02                 // Lower critical
   04                 // Lower non-critical
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   C8                 // Type/Length Code
   'BMC Temp'     // String Bytes


_SDR_TYPE   01
_REC_LEN    003D

   // Sensor Record Header
   001A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   25                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   50                 // Nominal Reading
   69                 // Normal Maximum
   05                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   73                 // Upper critical
   6E                 // Upper non-critical
   00                 // Lower non-recoverable
   02                 // Lower critical
   04                 // Lower non-critical
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CD                 // Type/Length Code
   'BB P1 VR Temp'  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_REC_LEN    003E

   // Sensor Record Header
   001B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   29                 // Sensor Number

   // Record Body Bytes
   0F                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask   --[u,l][c,nc]=8532
   8532               // Deassertion Event Mask --[u,l][c,nc]=8532
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=1B1B
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   19                 // Normal Reading 
   2D                 // Normal Maximum 
   05                 // Normal Minimum 
   7F                 // Sensor Maximum Reading 
   80                 // Sensor Minimum Reading 
   00                 // Upper non-recoverable 
   37                 // Upper critical 
   32                 // Upper non-critical 
   00                 // Lower non-recoverable 
   02                 // Lower critical 
   04                 // Lower non-critical 
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CE                 // Type Length Code
   'HSBP PSOC Temp'   // String Bytes


_SDR_TYPE   01
_SDR_TAG    'BCP_2U4N'
_REC_LEN    003D

   // Sensor Record Header
   001C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   2E                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks --[u,l][c,nc]=0000
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   37                 // Nominal Reading
   4B                 // Normal Maximum
   05                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   55                 // Upper critical
   50                 // Upper non-critical
   00                 // Lower non-recoverable
   02                 // Lower critical
   04                 // Lower non-critical
   04                 // Positive hysteresis value
   04                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Exit Air Temp'    // String Bytes


_SDR_TYPE   01
_REC_LEN    003E

   // Sensor Record Header
   001F               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   24                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   3C                 // Nominal Reading
   69                 // Normal Maximum
   05                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   73                 // Upper critical
   6E                 // Upper non-critical
   00                 // Lower non-recoverable
   02                 // Lower critical
   04                 // Lower non-critical
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CE                 // Type/Length Code
   'BB Mem VR Temp'	  // String Bytes

_SDR_TYPE   01
_SDR_TAG    'RISER_1_FRU'
_SDR_TAG    'FCT'
_REC_LEN    003C

   // Sensor Record Header
   1C00			// Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   27                 // Sensor Number

   // Record Body Bytes
   10                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   37                 // Nominal Reading
   69                 // Normal Maximum
   05                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   73                 // Upper critical
   6E                 // Upper non-critical
   00                 // Lower non-recoverable
   02                 // Lower critical
   04                 // Lower non-critical
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CC                 // Type/Length Code
   'Riser 1 Temp'	  // String Bytes
  
_SDR_TYPE   01
_SDR_TAG    'RISER_2_FRU'
_SDR_TAG    'FCT'
_REC_LEN    003C

   // Sensor Record Header
   1C00           // Record ID
   51                 // SDR Version
   01                 // Record Type
   37                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   2C                 // Sensor Number

   // Record Body Bytes
   10                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   37                 // Nominal Reading
   69                 // Normal Maximum
   05                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   73                 // Upper critical
   6E                 // Upper non-critical
   00                 // Lower non-recoverable
   02                 // Lower critical
   04                 // Lower non-critical
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   CC                 // Type/Length Code
   'Riser 2 Temp'	  // String Bytes

   
//*****************************************************************************
//
// Bobcat Peak Fan tachometer sensors
//
//*****************************************************************************


_SDR_TYPE   01
_SDR_TAG    'SYS_FAN_2U4N'
_REC_LEN    003D

   // Sensor Record Header
   0020               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   35                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 1a'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYS_FAN_2U4N'
_REC_LEN    003D

   // Sensor Record Header
   0021               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   36                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 1b'   // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYS_FAN_2U4N'
_REC_LEN    003D

   // Sensor Record Header
   0022               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   37                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   03                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 2a'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYS_FAN_2U4N'
_REC_LEN    003D

   // Sensor Record Header
   0023               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   38                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   04                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 2b'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYS_FAN_2U4N'
_REC_LEN    003D

   // Sensor Record Header
   0024               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   3B                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   05                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 3a'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYS_FAN_2U4N'
_REC_LEN    003D

   // Sensor Record Header
   0025               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   3C                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   06                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 3b'    // String Bytes


//*****************************************************************************
//
// FCT/FOQM Fan tachometer sensors
//
//*****************************************************************************


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_CPU_FAN'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    0037

   // Sensor Record Header
   0026               // Record ID
   51                 // SDR Version
   01                 // Record Type
   32                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   34                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0D                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   0F                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   9C                 // Nominal Reading
   FF                 // Normal Maximum
   39                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   28                 // Lower critical
   2D                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   C7                 // Type/Length Code
   'CPU Fan'          // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_1A'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   0027               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   35                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 1a'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_1B'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   0028               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   36                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 1b'   // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_2A'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   0029               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   37                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   03                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 2a'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_2B'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   002A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   38                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   04                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 2b'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_3A'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   002B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   3B                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   05                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 3a'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_3B'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   002C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   3C                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   06                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 3b'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_4A'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   002D               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   30                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   07                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 4a'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_4B'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   002E               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   31                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   08                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 4b'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_5A'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   002F               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   32                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   09                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 5a'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_5B'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   0030               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   33                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0A                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 5B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_6A'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   0031               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   39                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0B                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 6a'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'SYSTEM_FAN_6B'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003D

   // Sensor Record Header
   0032               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   3A                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0C                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 6b'    // String Bytes


//*****************************************************************************
//
// Other Fan tachometer sensors
//
//*****************************************************************************


_SDR_TYPE   01
_SDR_TAG    'OTHER_CPU_FAN'
_REC_LEN    0037

   // Sensor Record Header
   0033               // Record ID
   51                 // SDR Version
   01                 // Record Type
   32                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   34                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0D                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   27                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   8C                 // Nominal Reading
   FF                 // Normal Maximum
   19                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   11                 // Lower critical
   14                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   C7                 // Type/Length Code
   'CPU Fan'          // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_1A'
_REC_LEN    003D

   // Sensor Record Header
   0034               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   35                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 1a'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_1B'
_REC_LEN    003D

   // Sensor Record Header
   0035               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   36                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 1b'   // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_2A'
_REC_LEN    003D

   // Sensor Record Header
   0036               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   37                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   03                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 2a'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_2B'
_REC_LEN    003D

   // Sensor Record Header
   0037               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   38                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   04                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 2b'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_3A'
_REC_LEN    003D

   // Sensor Record Header
   0038               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   3B                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   05                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 3a'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_3B'
_REC_LEN    003D

   // Sensor Record Header
   0039               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   3C                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   06                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 3b'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_4A'
_REC_LEN    003D

   // Sensor Record Header
   003A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   30                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   07                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 4a'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_4B'
_REC_LEN    003D

   // Sensor Record Header
   003B               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   31                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   08                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 4b'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_5A'
_REC_LEN    003D

   // Sensor Record Header
   003C               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   32                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   09                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 5a'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_5B'
_REC_LEN    003D

   // Sensor Record Header
   003D               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   33                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0A                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 5B'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_6A'
_REC_LEN    003D

   // Sensor Record Header
   003E               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   39                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0B                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 6a'    // String Bytes


_SDR_TYPE   01
_SDR_TAG    'OTHER_FAN_6B'
_REC_LEN    003D

   // Sensor Record Header
   003F               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   3A                 // Sensor Number

   // Record Body Bytes
   1D                 // Entity ID
   0C                 // Entity Instance
   7F                 // Sensor Initialization
   28                 // Sensor Capabilities
   04                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   12                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   62                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   84                 // Nominal Reading
   FF                 // Normal Maximum
   0A                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   07                 // Lower critical
   08                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   45                 // OEM used for filtering [7:5]= 1 Mean (avg) [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'System Fan 6b'    // String Bytes


//*****************************************************************************
//
// Power supply sensors (Only supported with PMBus enabled power supplies)
//
//*****************************************************************************


_SDR_TYPE   02
_SDR_TAG    'STICKY_PS1_1600W'
_SDR_TAG    'STICKY_PS1_2130W'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    002A

   // Sensor Record Header
   0040               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   50                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   08                 // Sensor Type
   6F                 // Event / Reading Base Type
   4F00               // Assertion Event Mask
   4F00               // Deassertion Event Mask
   4F00               // Reading Mask &  Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'PS1 Status'       // String Bytes


_SDR_TYPE   02
_SDR_TAG    'STICKY_PS2_1600W'
_SDR_TAG    'STICKY_PS2_2130W'
_REC_LEN    002A

   // Sensor Record Header
   0041               // Record ID
   51                 // SDR Version
   02                 // Record Type
   25                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   51                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   08                 // Sensor Type
   6F                 // Event / Reading Base Type
   4F00               // Assertion Event Mask
   4F00               // Deassertion Event Mask
   4F00               // Reading Mask &  Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00          		  // Reserved
   00                 // Reserved
   00                 // OEM
   CA                 // Type/Length Code
   'PS2 Status'       // String Bytes


_SDR_TYPE   01
_SDR_TAG    'STICKY_PS1_1600W'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003F

   // Sensor Record Header
   0042               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   54                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   0A                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   57                 // Nominal Reading
   AF                 // Normal Maximum
   00                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   E6                 // Upper critical
   CB                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS1 Input Power'  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'STICKY_PS2_1600W'
_REC_LEN    003F

   // Sensor Record Header
   0043               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   55                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   0A                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   57                 // Nominal Reading
   AF                 // Normal Maximum
   00                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   E6                 // Upper critical
   CB                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS2 Input Power'  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'STICKY_PS1_2130W'
_REC_LEN    003F

   // Sensor Record Header
   0042               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   54                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   0B                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   6A                 // Nominal Reading
   D5                 // Normal Maximum
   00                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   FB                 // Upper critical
   E8                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS1 Input Power'  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'STICKY_PS2_2130W'
_REC_LEN    003F

   // Sensor Record Header
   0043               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   55                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   0B                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   06                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   0B                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   6A                 // Nominal Reading
   D5                 // Normal Maximum
   00                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   FB                 // Upper critical
   E8                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PS2 Input Power'  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'STICKY_PS1_1600W'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003E

   // Sensor Record Header
   0044               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   58                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   32                 // Nominal Reading
   64                 // Normal Maximum
   00                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   83                 // Upper critical
   64                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS1 Curr Out %'   // String Bytes


_SDR_TYPE   01
_SDR_TAG    'STICKY_PS2_1600W'
_REC_LEN    003E

   // Sensor Record Header
   0045               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   59                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   32                 // Nominal Reading
   64                 // Normal Maximum
   00                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   83                 // Upper critical
   64                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS2 Curr Out %'   // String Bytes


_SDR_TYPE   01
_SDR_TAG    'STICKY_PS1_2130W'
_REC_LEN    003E

   // Sensor Record Header
   0044               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   58                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   32                 // Nominal Reading
   64                 // Normal Maximum
   00                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   75                 // Upper critical
   64                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS1 Curr Out %'   // String Bytes


_SDR_TYPE   01
_SDR_TAG    'STICKY_PS2_2130W'
_REC_LEN    003E

   // Sensor Record Header
   0045               // Record ID
   51                 // SDR Version
   01                 // Record Type
   39                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   59                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   03                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   32                 // Nominal Reading
   64                 // Normal Maximum
   00                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   75                 // Upper critical
   64                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS2 Curr Out %'   // String Bytes


_SDR_TYPE   01
_SDR_TAG    'STICKY_PS1_1600W'
_SDR_TAG    'STICKY_PS1_2130W'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    003F

   // Sensor Record Header
   0046               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   5C                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   19                 // Nominal Reading
   32                 // Normal Maximum
   05                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   3C                 // Upper critical
   37                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM used for filtering [7:5]= 0 [4:0]=0 Sample Count
   CF                 // Type/Length Code
   'PS1 Temperature'  // String Bytes


_SDR_TYPE   01
_SDR_TAG    'STICKY_PS2_1600W'
_SDR_TAG    'STICKY_PS2_2130W'
_REC_LEN    003F

   // Sensor Record Header
   0047               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   5D                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   19                 // Nominal Reading
   32                 // Normal Maximum
   05                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   3C                 // Upper critical
   37                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM used for filtering [7:5]= 0 [4:0]=0 Sample Count
   CF                 // Type/Length Code
   'PS2 Temperature'  // String Bytes


//*****************************************************************************
//
// Processor (CPU) sensors
//
//*****************************************************************************


_SDR_TYPE   02
_REC_LEN    0029

   // Sensor Record Header
   0048               // Record ID
   51                 // SDR Version
   02                 // Record Type
   24                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   70                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   6F                 // Event / Reading Base Type
   8200               // Assertion Event Mask
   8200               // Deassertion Event Mask
   8200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'P1 Status'        // String Bytes


_SDR_TYPE   01
_REC_LEN    003F

   // Sensor Record Header
   0049               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   74                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   F1                 // Nominal Reading
   00                 // Normal Maximum
   BA                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'P1 Therm Margin'  // String Bytes


_SDR_TYPE   01
_REC_LEN    003F

   // Sensor Record Header
   004A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   78                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   01                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   00                 // Nominal Reading
   14                 // Normal Maximum
   00                 // Normal Minimum
   64                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   32                 // Upper critical
   1E                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'P1 Therm Ctrl %'  // String Bytes


_SDR_TYPE   02
_REC_LEN    0028

   // Sensor Record Header
   004B               // Record ID
   51                 // SDR Version
   02                 // Record Type
   23                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   7C                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   41                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C8                 // Type/Length Code
   'CPU ERR2'         // String Bytes


_SDR_TYPE   03
_REC_LEN    001E

   // Sensor Record Header
   004C               // Record ID
   51                 // SDR Version
   03                 // Record Type
   19                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   7D                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   D1                 // Sensor type
   70                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'IERR Rec Info'    // String Bytes


_SDR_TYPE   02
_REC_LEN    0024

   // Sensor Record Header
   004D               // Record ID
   51                 // SDR Version
   02                 // Record Type
   1F               // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   80                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C4                 // Type/Length Code
   'IERR'             // String Bytes


_SDR_TYPE   02
_REC_LEN    002B

   // Sensor Record Header
   004F               // Record ID
   51                 // SDR Version
   02                 // Record Type
   26                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   82                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   07                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CB                 // Type/Length Code
   'CPU Missing'      // String Bytes


_SDR_TYPE   01
_REC_LEN    0040

   // Sensor Record Header
   0050               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   83                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   F1                 // Normal Reading
   00                 // Normal Maximum
   BA                 // Normal Minimum
   00                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   0F                 // Upper critical
   0A                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM
   D0                 // Type/Length Code
   'P1 DTS Therm Mgn' // String Bytes


//*****************************************************************************
//
// Voltage regulator sensors
//
//*****************************************************************************


_SDR_TYPE   02
_REC_LEN    0027

   // Sensor Record Header
   0051               // Record ID
   51                 // SDR Version
   02                 // Record Type
   22                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   90                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   01                 // Sensor Type
   05                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C7                 // Type/Length Code
   'VRD Hot'          // String Bytes


//*****************************************************************************
//
// Power supply fan tachometer sensors
//
//*****************************************************************************


_SDR_TYPE   02
_SDR_TAG    'STICKY_PS1_1600W'
_SDR_TAG    'STICKY_PS1_2130W'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    002E

   // Sensor Record Header
   0055               // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   A0                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   00                 // Sensor Capabilities -- Manual Rearm
   04                 // Sensor Type - Fan
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Mask
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS1 Fan Fail 1'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'STICKY_PS1_1600W'
_SDR_TAG    'STICKY_PS1_2130W'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    002E

   // Sensor Record Header
   0056               // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   A1                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   00                 // Sensor Capabilities -- Manual Rearm
   04                 // Sensor Type - Fan
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Mask
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS1 Fan Fail 2'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'STICKY_PS2_1600W'
_SDR_TAG    'STICKY_PS2_2130W'
_REC_LEN    002E

   // Sensor Record Header
   0057               // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   A4                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   00                 // Sensor Capabilities -- Manual Rearm
   04                 // Sensor Type - Fan
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Mask
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS2 Fan Fail 1'    // String Bytes


_SDR_TYPE   02
_SDR_TAG    'STICKY_PS2_1600W'
_SDR_TAG    'STICKY_PS2_2130W'
_REC_LEN    002E

   // Sensor Record Header
   0058               // Record ID
   51                 // SDR Version
   02                 // Record Type
   29                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   A5                 // Sensor Number

   // Record Body Bytes
   0A                 // Entity ID
   02                 // Entity Instance
   67                 // Sensor Initialization - [6]-Init Scanning; [5]-Init Events; [2]-Init Sensor Type;
   00                 // Sensor Capabilities -- Manual Rearm
   04                 // Sensor Type - Fan
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Mask
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS2 Fan Fail 2'    // String Bytes


//*****************************************************************************
//
// Memory thermal margin sensors
//
//*****************************************************************************


_SDR_TYPE   01
_REC_LEN    0040

   // Sensor Record Header
   0059               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   B0                 // Sensor Number

   // Record Body Bytes
   08                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   EC                 // Nominal Reading
   00                 // Normal Maximum
   BA                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   0A                 // Upper critical
   05                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM used for filtering [7:5]= 1 Median [4:0]=5 Sample Count
   D0                 // Type/Length Code
   'DIMM Thrm Mrgn 1' // String Bytes


_SDR_TYPE   01
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'OTHER'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'FCT'
_REC_LEN    0040

   // Sensor Record Header
   005A               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   B1                 // Sensor Number

   // Record Body Bytes
   08                 // Entity ID
   02                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   8002               // Assertion Event Mask
   8032               // Deassertion Event Mask
   1818               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   EC                 // Nominal Reading
   00                 // Normal Maximum
   BA                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   0A                 // Upper critical
   05                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM used for filtering [7:5]= 1 Median [4:0]=5 Sample Count
   D0                 // Type/Length Code
   'DIMM Thrm Mrgn 2' // String Bytes


_SDR_TYPE   02
_REC_LEN    002D

   // Sensor Record Header
   005B               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   B8                 // Sensor Number

   // Record Body Bytes
   15                 // Entity ID
   03                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   09                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask   --State asserted =0200
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks --State asserted =0200
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Auto Shutdown'    // String Bytes


//*****************************************************************************
//
// Memory thermal trip sensors
//
//*****************************************************************************


_SDR_TYPE   02
_REC_LEN    0030

   // Sensor Record Header
   005C               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2B                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   C0                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   00                 // Sensor Capabilities
   0C                 // Sensor Type
   6F                 // Event / Reading Base Type
   0004               // Assertion Event Mask
   0004               // Deassertion Event Mask
   0004               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'P1 Mem Thrm Trip' // String Bytes


//*****************************************************************************
//
// Global aggregate thermal margin sensors
//
//*****************************************************************************


_SDR_TYPE   01
_SDR_TAG    'BCP_2U4N'
_REC_LEN    003F

   // Sensor Record Header
   005D               // Record ID
   51                 // SDR Version
   01                 // Record Type
   3A                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   C8                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   01                 // Sensor Type
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0000               // Reading Mask & Settable / Readable Threshold Masks
   80                 // Sensor Units 1
   01                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   01                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   00                 // R exp, B exp
   07                 // Analog characteristic flags
   EC                 // Nominal Reading
   00                 // Normal Maximum
   BA                 // Normal Minimum
   7F                 // Sensor Maximum Reading
   80                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable
   00                 // Lower critical
   00                 // Lower non-critical
   02                 // Positive hysteresis value
   02                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM used for filtering [7:5]= 1 Median [4:0]=5 Sample Count
   CF                 // Type/Length Code
   'Agg Therm Mgn 1'  // String Bytes


//*****************************************************************************
//
// Voltage sensors
//
//*****************************************************************************


_SDR_TYPE   01
_REC_LEN    0039

   // Sensor Record Header
   005E               // Record ID
   51                 // SDR Version
   01                 // Record Type
   34                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D0                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   8532               // Assertion Event Mask
   8532               // Deassertion Event Mask
   1B1B               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   36                 // M
   00                 // M, Tolerance
   F7                 // B
   40                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   DF                 // R exp, B exp
   07                 // Analog characteristic flags
   DC                 // Normal Reading
   EC                 // Normal Maximum
   CD                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   FC                 // Upper critical
   F5                 // Upper non-critical
   00                 // Lower non-recoverable
   BF                 // Lower critical
   C5                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'BB +12.0V'        // String Bytes


_SDR_TYPE   01
_REC_LEN    003D

   // Sensor Record Header
   005F               // Record ID
   51                 // SDR Version
   01                 // Record Type
   38                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   DE                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   7F                 // Sensor Initialization
   68                 // Sensor Capabilities
   02                 // Sensor Type
   01                 // Event / Reading Base Type
   0530               // Assertion Event Mask
   0500               // Deassertion Event Mask
   0303               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   04                 // Sensor Units 2
   00                 // Sensor Units 3
   00                 // Linearization
   85                 // M
   00                 // M, Tolerance
   91                 // B
   80                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   C0                 // R exp, B exp
   07                 // Analog characteristic flags
   E4                 // Normal Reading
   EF                 // Normal Maximum
   C2                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable
   FC                 // Upper critical
   F7                 // Upper non-critical
   00                 // Lower non-recoverable
   A3                 // Lower critical
   BC                 // Lower non-critical
   01                 // Positive hysteresis value
   01                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   25                 // OEM used for filtering [7:5]= 1 Median [4:0]=5 Sample Count
   CD                 // Type/Length Code
   'BB +3.0V VBAT'    // String Bytes


_SDR_TYPE   02
_REC_LEN    002D

   // Sensor Record Header
   0060               // Record ID
   51                 // SDR Version
   02                 // Record Type
   28                 // Record Length

   // Record Key Bytes
   20                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   D1                 // Sensor Number

   // Record Body Bytes
   07                 // Entity ID
   01                 // Entity Instance
   67                 // Sensor Initialization
   40                 // Sensor Capabilities
   02                 // Sensor Type
   03                 // Event / Reading Base Type
   0200               // Assertion Event Mask
   0200               // Deassertion Event Mask
   0200               // Reading Mask & Settable / Readable Threshold Masks
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'Voltage Fault'    // String Bytes


//*****************************************************************************
//
// Hot-swap backplane (HSBP) sensors
//
//*****************************************************************************


_SDR_TYPE   02
_SDR_TAG    'BCP_2U4N'
_REC_LEN    002C

   // Sensor Record Header
   0061               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F0                 // Sensor Number

   // Record Body Bytes
   04                 // Entity ID
   01                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 0 Status'     // String Bytes


_SDR_TYPE   02
_SDR_TAG    'BCP_2U4N'
_REC_LEN    002C

   // Sensor Record Header
   0062               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F1                 // Sensor Number

   // Record Body Bytes
   04                 // Entity ID
   02                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 1 Status'     // String Bytes


_SDR_TYPE   02
_SDR_TAG    'BCP_2U4N'
_REC_LEN    002C

   // Sensor Record Header
   0063               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F2                 // Sensor Number

   // Record Body Bytes
   04                 // Entity ID
   03                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 2 Status'     // String Bytes


_SDR_TYPE   02
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    002C

   // Sensor Record Header
   0064               // Record ID
   51                 // SDR Version
   02                 // Record Type
   27                 // Record Length

   // Record Key Bytes
   20                 // Sensor ID
   00                 // Sensor LUN
   F3                 // Sensor Number

   // Record Body Bytes
   04                 // Entity ID
   04                 // Entity Instance
   6D                 // Sensor Initialization
   40                 // Sensor Capabilities
   0D                 // Sensor Type
   6F                 // Event / Reading Base Type
   8300               // Assertion Event Mask
   8300               // Deassertion Event Mask
   8300               // Reading Mask &
   C0                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0100               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'HDD 3 Status'     // String Bytes


//*****************************************************************************
//
//  SDR Type 3 Manageability Engine (ME controller) Records
//
//*****************************************************************************

_SDR_TYPE   03
_REC_LEN    001E

   // Sensor Record Header
   006D               // Record ID
   51                 // SDR Version
   03                 // Record Type
   19                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   17                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   01                 // Entity Instance
   DC                 // Sensor type
   75                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CD                 // Type/Length Code
   'SPS FW Health'    // String Bytes


_SDR_TYPE   03
_REC_LEN    001D

   // Sensor Record Header
   006E               // Record ID
   51                 // SDR Version
   03                 // Record Type
   18                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   18                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   01                 // Entity Instance
   DC                 // Sensor type
   72                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'NM Exception'     // String Bytes


_SDR_TYPE   03
_REC_LEN    001A

   // Sensor Record Header
   006F               // Record ID
   51                 // SDR Version
   03                 // Record Type
   15                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   19                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   01                 // Entity Instance
   DC                 // Sensor type
   73                 // Event/Reading Type Code
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   C9                 // Type/Length Code
   'NM Health'        // String Bytes


_SDR_TYPE   02
_REC_LEN    002F

   // Sensor Record Header
   0070               // Record ID
   51                 // SDR Version
   02                 // Record Type
   2A                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   1A                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   01                 // Entity Instance
   41                 // Sensor Initialization
   C3                 // Sensor Capabilities
   DC                 // Sensor Type
   74                 // Event / Reading Base Type
   0000               // Assertion Event Mask
   0000               // Deassertion Event Mask
   0700               // Reading Mask & Settable / Readable Threshold Masks
   00                 // Sensor Units 1
   00                 // Sensor Units 2
   00                 // Sensor Units 3
   0000               // Sensor Record Sharing
   00                 // Positive-going Threshold Hysteresis
   00                 // Negative-going Threshold Hysteresis
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'NM Capabilities'  // String Bytes


_SDR_TYPE   03
_REC_LEN    001D

   // Sensor Record Header
   0071               // Record ID
   51                 // SDR Version
   03                 // Record Type
   18                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Channel Number / Sensor Owner LUN
   1B                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   05                 // Entity Instance
   DC                 // Sensor Type
   72                 // Event / Reading Base Type
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'NM Threshold'     // String Bytes


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   0072               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Channel Number / Sensor Owner LUN
   B2                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   02                 // Entity Instance
   DC                 // Sensor Type
   03                 // Event / Reading Base Type
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'SmaRT-CLST Stat'  // String Bytes

_SDR_TYPE   03
_REC_LEN    001F

   // Sensor Record Header
   0069               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1A                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Channel Number / Sensor Owner LUN
   66                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   06                 // Entity Instance
   DC                 // Sensor Type
   03                 // Event / Reading Base Type
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS1 SmaRT-CLST'   // String Bytes

_SDR_TYPE   03
_REC_LEN    001F

   // Sensor Record Header
   0069               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1A                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Channel Number / Sensor Owner LUN
   67                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   06                 // Entity Instance
   DC                 // Sensor Type
   03                 // Event / Reading Base Type
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'PS2 SmaRT-CLST'   // String Bytes
   
_SDR_TYPE   03
_REC_LEN    001F

   // Sensor Record Header
   0069               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1A                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Channel Number / Sensor Owner LUN
   16                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   06                 // Entity Instance
   16                 // Sensor Type
   03                 // Event / Reading Base Type
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'ME Power State'   // String Bytes   
   
_SDR_TYPE   03
_REC_LEN    0021

   // Sensor Record Header
   0069               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1C                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Channel Number / Sensor Owner LUN
   1C                 // Sensor Number

   // Record Body Bytes
   2E                 // Entity ID
   06                 // Entity Instance
   07                 // Sensor Type
   76                 // Event / Reading Base Type
   0000               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'CPU 0 Therm Stat' // String Bytes   
   

//*******************************************************
// SDR Type C0 Records For NodeManager discovery data
//*******************************************************

_SDR_TYPE   C0
_REC_LEN    0010

   // Sensor Record Header
   0073               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0B                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0D		          // Record subtype - NM Discovery
   01		          // Version number of record subtype
   2C                 // NM Device Slave Address ([7:1] - 7-bit address; [0] - reserved)
   60		          // [7:4] - channel number (0 for primary) [3:2] - reserved (b'00) [1:0] - sensor owner LUN
   19                 // Node Manager Health Event sensor
   18                 // Node Manager Exception Event sensor
   1A                 // Node Manager Operational Capabilities sensor
   1B                 // Node Manager Threshold Exceeded sensor


_SDR_TYPE   01
_REC_LEN    0038

   // Sensor Record Header
   0074               // Record ID
   51                 // SDR Version
   01                 // Record Type
   33                 // Record Length

   // Record Key Bytes
   2C                 // Sensor Owner ID
   60                 // Sensor Owner LUN
   34                 // Sensor Number

   // Record Body Bytes
   03                 // Entity ID
   01                 // Entity Instance
   63                 // Sensor Initialization
   B8                 // Sensor Capabilities
   0C                 // Sensor Type -- Memory
   01                 // Event / Reading Base Type
   0000               // Assertion Event Mask   --[u][c,nc]=0000
   0000               // Deassertion Event Mask --[u][c,nc]=0000
   3F3F               // Reading Mask & Settable / Readable Threshold Masks --[u][c,nc]=0000
   01                 // Sensor Units 1
   00                 // Sensor Units 2 -- Degrees C
   00                 // Sensor Units 3
   00                 // Linearization
   05                 // M
   00                 // M, Tolerance
   00                 // B
   00                 // B, Accuracy
   00                 // Accuracy, Accuracy Exp
   F0                 // R exp, B exp
   00                 // Analog characteristic flags
   00                 // Normal Reading
   00                 // Normal Maximum
   00                 // Normal Minimum
   FF                 // Sensor Maximum Reading
   00                 // Sensor Minimum Reading
   00                 // Upper non-recoverable (not specified)
   00                 // Upper critical
   00                 // Upper non-critical
   00                 // Lower non-recoverable (not specified)
   00                 // Lower critical (not specified)
   00                 // Lower non-critical (not specified)
   00                 // Positive hysteresis value
   00                 // Negative hysteresis value
   00                 // Reserved
   00                 // Reserved
   00                 // OEM
   C8                 // Type/Length Code
   'MTT CPU1'         // String Bytes


//*****************************************************************************
//
// SDR Type 3 BIOS Sensor Data Records
//
//*****************************************************************************

_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   0075               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   01                 // Sensor Number

   // Record Body Bytes
   22                 // Entity ID = Processor/Memory Module
   01                 // Entity Instance
   0C                 // Sensor Type
   0B                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mem Rdnc Sensor'  // Memory Redundancy State


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   0076               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   02                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID = Memory Device
   01                 // Entity Instance
   0C                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mmry ECC Sensor'   // Memory ECC Error Sensor


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   0077               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   03                 // Sensor Number

   // Record Body Bytes
   30                 // Entity ID = PCI
   01                 // Entity Instance
   13                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCI Lgcy Sensor'   // Legacy PCI Sensor


_SDR_TYPE   03
_REC_LEN    0021

   // Sensor Record Header
   0078               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1C                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   04                 // Sensor Number

   // Record Body Bytes
   31                 // Entity ID = PCI Express
   01                 // Entity Instance
   13                 // Sensor Type
   70                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   D0                 // Type/Length Code
   'PCIe Fatal Error' // PCI Express Fatal Error Sensor


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   0079               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   05                 // Sensor Number

   // Record Body Bytes
   31                 // Entity ID = PCI Express
   01                 // Entity Instance
   13                 // Sensor Type
   71                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCIe Cor Sensor'  // PCI Express Correctable Error Sensor


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   007A               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   06                 // Sensor Number

   // Record Body Bytes
   22                 // Entity ID-BIOS POST  (System Firmware-BIOS)
   01                 // Entity Instance
   0F                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'POST Err Sensor'  // POST Error Sensor


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   007B               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   06                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID
   04                 // Entity Instance
   13                 // Sensor Type
   72                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'QPI Corr Sensor'  // QPI Correctable Event Sensor


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   007C               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   07                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID
   01                 // Entity Instance
   13                 // Sensor Type
   73                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'QPI Fatl Sensor'   //  QPI Fatal/Uncorrectable Errors


_SDR_TYPE   03
_REC_LEN    001F

   // Sensor Record Header
   007D               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1A                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   08                 // Sensor Number

   // Record Body Bytes
   31                 // Entity ID = PCI Express
   01                 // Entity Instance
   19                 // Sensor Type
   75                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Chipset Sensor'   // Chipset Proprietary Errors


_SDR_TYPE   03
_REC_LEN    001F

   // Sensor Record Header
   007E               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1A                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   09                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID
   05                 // Entity Instance
   13                 // Sensor Type
   77                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'QPI Link Width'   // QPI Link Width Reduced

_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   007F               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   02                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID = Memory
   01                 // Entity Instance
   0C                 // Sensor Type
   09                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mem Conf Sensor'  // Memory configuration failed


_SDR_TYPE   03
_REC_LEN    001D

   // Sensor Record Header
   0080               // Record ID
   51                 // SDR Version
   03                 // Record Type
   18                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   11                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   01                 // Entity Instance
   0C                 // Sensor Type
   0B                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CC                 // Type/Length Code
   'Sparing Rdnc'     // Sparing Redundancy State


_SDR_TYPE   03
_REC_LEN    001F

   // Sensor Record Header
   0081               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1A                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   10                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID = Memory Device
   01                 // Entity Instance
   0C                 // Sensor Type
   7F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CE                 // Type/Length Code
   'Mem err Sensor'   //Memory Error Extension


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   0082               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   12                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   01                 // Entity Instance
   0C                 // Sensor Type
   09                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Rdnc Mod Sensor'  // Memory Redundancy Configuration


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   0083               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   13                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID = Memory Device
   01                 // Entity Instance
   0C                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'Mmry Parity Err'  // Memory Parity Error


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   0084               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   14                 // Sensor Number

   // Record Body Bytes
   31                 // Entity ID = PCI Express
   01                 // Entity Instance
   13                 // Sensor Type
   76                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'PCIe Fat Sensor'  // PCI Express Fatal Error Sensor


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   0085               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   17                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID
   01                 // Entity Instance
   13                 // Sensor Type
   74                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'QPI Fatl Sensor'  // QPI Fatal/Uncorrectable Errors

   
_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   0085               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   1C                 // Sensor Number

   // Record Body Bytes
   20                 // Entity ID
   01                 // Entity Instance
   0C                 // Sensor Type
   6F                 // Event / Reading Base Type
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'MCDRAM/EDC  ERR'  // MCDRAM/ECC ERROR   


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   0086               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   01                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   83                 // Sensor Number

   // Record Body Bytes
   22                 // Entity ID = System Firmware (BIOS)
   01                 // Entity Instance
   12                 // Sensor Type
   6F                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'BIOS Evt Sensor'  // BIOS Boot Event Sensor


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   0087               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   83                 // Sensor Number

   // Record Body Bytes
   22                 // Entity ID = System Firmware (BIOS)
   01                 // Entity Instance
   12                 // Sensor Type
   6F                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'BIOS Evt Sensor'  // BIOS Boot Event Sensor


_SDR_TYPE   03
_REC_LEN    0020

   // Sensor Record Header
   0088               // Record ID
   51                 // SDR Version
   03                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   33                 // Sensor Owner ID
   00                 // Sensor Owner LUN
   83                 // Sensor Number

   // Record Body Bytes
   2B                 // Entity ID = Processor/Memory Module
   01                 // Entity Instance
   12                 // Sensor Type
   6F                 // Event / Reading Base Type = Entity Enabled/Disabled
   0100               // Sensor Record Sharing
   00                 // Reserved
   00                 // OEM
   CF                 // Type/Length Code
   'BIOS Evt Sensor'  // BIOS Boot Event Sensor


//*******************************************************
//
// SDR Type 11 FRU Device Locator Records
//
//*******************************************************


_SDR_TYPE   11
_REC_LEN    0019

   // Sensor Record Header
   0089               // Record ID
   51                 // SDR Version
   11                 // Record Type
   14                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   00                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   07                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // OEM
   C9                 // Type/Length Code
   'Baseboard'        // String Bytes


_SDR_TYPE   11
_SDR_TAG    'STICKY_PS1_1600W'
_SDR_TAG    'STICKY_PS1_2130W'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    0020

   // Sensor Record Header
   008A               // Record ID
   51                 // SDR Version
   11                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   02                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   0A                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // Reserved for OEM use
   D0                 // Type/Length Code
   'Pwr Supply 1 FRU' // String Bytes


_SDR_TYPE   11
_SDR_TAG    'STICKY_PS2_1600W'
_SDR_TAG    'STICKY_PS2_2130W'
_REC_LEN    0020

   // Sensor Record Header
   008B               // Record ID
   51                 // SDR Version
   11                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   03                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   0A                 // FRU Entity ID
   02                 // FRU Entity Instance
   00                 // Reserved for OEM use
   D0                 // Type/Length Code
   'Pwr Supply 2 FRU' // String Bytes


_SDR_TYPE   11
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    001C

   // Sensor Record Header
   008D               // Record ID
   51                 // SDR Version
   11                 // Record Type
   17                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   08                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   0F                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // OEM
   CC                 // Type/Length Code
   'HS Backplane'     // String Bytes

_SDR_TYPE   11
_SDR_TAG    'RISER_1_FRU'
_REC_LEN    001B

   // Sensor Record Header
   C800          	 // Record ID
   51                 // SDR Version
   11                 // Record Type
   16                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   0B                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   10                 // FRU Entity ID
   01                 // FRU Entity Instance
   00                 // OEM
   CB                 // Type/Length Code
   'PCI Riser 1'     // String Bytes   
   
_SDR_TYPE   11
_SDR_TAG    'RISER_2_FRU'
_REC_LEN    001B

   // Sensor Record Header
   C800           // Record ID
   51                 // SDR Version
   11                 // Record Type
   16                 // Record Length

   // Record Key Bytes
   20                 // Device Access Address
   0C                 // FRU Device ID / Device Slave Address
   80                 // Access LUN / Bus ID
   00                 // Channel Number

   // Record Body Bytes
   00                 // Reserved
   10                 // Device Type
   00                 // Device Type Modifier
   10                 // FRU Entity ID
   02                 // FRU Entity Instance
   00                 // OEM
   CB                 // Type/Length Code
   'PCI Riser 2'     // String Bytes   
   
//*******************************************************
//
// SDR Type 12 Management Controller Records
//
//*******************************************************


_SDR_TYPE   12
_REC_LEN    0020

   // Sensor Record Header
   0090               // Record ID
   51                 // SDR Version
   12                 // Record Type
   1B                 // Record Length

   // Record Key Bytes
   20                 // Device Slave Address
   00                 // Channel Number

   // Record Body Bytes
   08                 // Power state notification
   BF                 // Device capabilities
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   2E                 // Entity ID
   01                 // Entity instance
   00                 // OEM
   D0                 // Type/Length Code
   'Basbrd Mgmt Ctlr' // String Bytes


_SDR_TYPE   12
_REC_LEN    001B

   // Sensor Record Header
   0091               // Record ID
   51                 // SDR Version
   12                 // Record Type
   16                 // Record Length

   // Record Key Bytes
   2C                 // Device Slave Address
   06                 // Channel number

   // Record Body Bytes
   24                 // Power State Notification
   21                 // Device Capabilities
   00                 // Reserved
   00                 // Reserved
   00                 // Reserved
   2E                 // Entity ID
   02                 // Entity Instance
   00                 // OEM
   CB                 // Type/Length Code
   'Mgmt Engine'      // String Bytes


//*******************************************************
//
// SDR Type C0/02 Record For Power Unit Map
//
//*******************************************************

_SDR_TYPE   C0
_SDR_TAG    'STICKY_REDUND_PS'
_REC_LEN    000E

   // Sensor Record Header
   0092               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   09                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   02                 // Record Subtype Value
   02                 // Power Unit Redundancy sensor number
   00                 // Bits [7:1]-Reserved; Bit[0]-1=No monitorable supplies present
   01                 // The number of present and operational
   50                 // Power Supply Status 1 Sensor Number
   51                 // Power Supply Status 2 Sensor Number


//*******************************************************
//
// SDR Type C0/09 Records For Voltage Sensor Scaling
//
//*******************************************************

_SDR_TYPE   C0
_REC_LEN    0010

   // Sensor Record Header
   0093               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0B                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   09                 // Record sub-type - Voltage Sensor Scaling
   02                 // Number of entries following
   D0                 // Voltage Sensor Number
   0A0B               // Scale Factor (LSB MSB)
   DE                 // Voltage Sensor Number
   AA09               // Scale Factor (LSB MSB)


//*****************************************************************************
//
// SDR Type C0/0A Records For Fan Sensor Scaling
//
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_REC_LEN    0025

  //Sensor Record Header
   0094               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   20                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record sub-type - Fan Sensor Scaling

   // Fan Sensor Scaling Record
   00                 // Format - Bit fields, 1 == Raw time, 0 = RPM
   00                 // Pulses Per Revolution - Bit Field - 1 == 1 PPR, 0 == 2 PPR
   1450               // Placeholder for System Fan 1a(SN:0x30), Max RPM: 22500RPM == E457 (the order is LSB, MSB)
   1450               // Placeholder for System Fan 1b(SN:0x31), Max RPM: 20500RPM == 1450 (the order is LSB, MSB)
   1450               // Placeholder for System Fan 2a(SN:0x32), Max RPM: 22500RPM == E457 (the order is LSB, MSB)
   1450               // Placeholder for System Fan 2b(SN:0x33), Max RPM: 20500RPM == 1450 (the order is LSB, MSB)
   1450               // Placeholder for System Fan 3a(SN:0x34), Max RPM: 22500RPM == E457 (the order is LSB, MSB)
   1450               // Placeholder for System Fan 3b(SN:0x35), Max RPM: 20500RPM == 1450 (the order is LSB, MSB)
   1450               // Placeholder for System Fan 4a(SN:0x36), Not Used
   1450               // Placeholder for System Fan 4b(SN:0x37), Not Used
   1450               // Placeholder for System Fan 5a(SN:0x38), Not Used
   1450               // Placeholder for System Fan 5b(SN:0x39), Not Used
   1450               // Placeholder for System Fan 6a(SN:0x3A), Not Used
   1450               // Placeholder for System Fan 6b(SN:0x3B), Not Used
   1450               // Placeholder for CPU Fan 01(SN:0x3C), Not Used


_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0025

  //Sensor Record Header
   0095               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   20                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record sub-type - Fan Sensor Scaling

   // Fan Sensor Scaling Record
   00                 // Format - Bit fields, 1 == Raw time, 0 = RPM
   00                 // Pulses Per Revolution - Bit Field - 1 == 1 PPR, 0 == 2 PPR
   A861               // Placeholder for System Fan 1a(SN:0x30), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 1b(SN:0x31), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 2a(SN:0x32), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 2b(SN:0x33), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 3a(SN:0x34), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 3b(SN:0x35), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 4a(SN:0x36), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 4b(SN:0x37), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 5a(SN:0x38), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 5b(SN:0x39), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 6a(SN:0x3A), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for System Fan 6b(SN:0x3B), Max RPM: 25000RPM == A861 (the order is LSB, MSB)
   A861               // Placeholder for CPU Fan 01(SN:0x3C), Not Used


_SDR_TYPE   C0
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'FCT'
_SDR_TAG    'FOQM'
_REC_LEN    0025

  //Sensor Record Header
   0096               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   20                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   0A                 // Record sub-type - Fan Sensor Scaling

   // Fan Sensor Scaling Record
   00                 // Format - Bit fields, 1 == Raw time, 0 = RPM
   00                 // Pulses Per Revolution - Bit Field - 1 == 1 PPR, 0 == 2 PPR
   803E               // Placeholder for System Fan 1a(SN:0x30), Max RPM: 16000RPM == 803E (the order is LSB, MSB)
   283C               // Placeholder for System Fan 1b(SN:0x31), Max RPM: 15400RPM == 283C (the order is LSB, MSB)
   803E               // Placeholder for System Fan 2a(SN:0x32), Max RPM: 16000RPM == 803E (the order is LSB, MSB)
   283C               // Placeholder for System Fan 2b(SN:0x33), Max RPM: 15400RPM == 283C (the order is LSB, MSB)
   803E               // Placeholder for System Fan 3a(SN:0x34), Max RPM: 16000RPM == 803E (the order is LSB, MSB)
   283C               // Placeholder for System Fan 3b(SN:0x35), Max RPM: 15400RPM == 283C (the order is LSB, MSB)
   803E               // Placeholder for System Fan 4a(SN:0x36), Max RPM: 16000RPM == 803E (the order is LSB, MSB)
   283C               // Placeholder for System Fan 4b(SN:0x37), Max RPM: 15400RPM == 283C (the order is LSB, MSB)
   803E               // Placeholder for System Fan 5a(SN:0x38), Max RPM: 16000RPM == 803E (the order is LSB, MSB)
   283C               // Placeholder for System Fan 5b(SN:0x39), Max RPM: 15400RPM == 283C (the order is LSB, MSB)
   803E               // Placeholder for System Fan 6a(SN:0x3A), Max RPM: 16000RPM == 803E (the order is LSB, MSB)
   283C               // Placeholder for System Fan 6b(SN:0x3B), Max RPM: 15400RPM == 283C (the order is LSB, MSB)
   803E               // Placeholder for CPU Fan 01(SN:0x3C), Not Used


//*****************************************************************************
//
// Fan Speed Control (FSC) configuration records
//
//*****************************************************************************

//*****************************************************************************
// FSC Record Type = 00h (Global Clamp Header Record)
// All Chassis
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    001B

   // Sensor Record Header
   0097           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   03             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   74             // Clamp Header ID
   74             // Temperature Sensor Number (74h = Processor Thermal Margin)
   00             // Entity Presence Sensor Number (0h = Not used)
   64             // Sensor Disabled Control Value (00h = Ignore this subrecord)
   64             // Sensor Fail Control Value (00h = Ignore this subrecord)
   64             // Sensor Unavailable Control Value (00h = Ignore this subrecord)
   00             // Sleep Control Value (0h = 0% PWM)
   18             // Sleep State and Hysteresis [7:6]-S1 support = 0 (ignore); [5:3]-Negative Hysteresis = 3; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient Is LSB
   01             // Clamp Control Coefficient Is MSB
   E8             // Clamp Control Coefficient If LSB
   03             // Clamp Control Coefficient If MSB
   C4             // Clamp Control Coefficient D LSB
   09             // Clamp Control Coefficient D MSB
   FE             // Temperature (00h = -2 degree C)
   01             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 1 (use TControl)

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    001B

   // Sensor Record Header
   0097           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   03             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   94             // Clamp Header ID
   74             // Temperature Sensor Number (74h = Processor Thermal Margin)
   00             // Entity Presence Sensor Number (0h = Not used)
   64             // Sensor Disabled Control Value (00h = Ignore this subrecord)
   64             // Sensor Fail Control Value (00h = Ignore this subrecord)
   64             // Sensor Unavailable Control Value (00h = Ignore this subrecord)
   00             // Sleep Control Value (0h = 0% PWM)
   28             // Sleep State and Hysteresis [7:6]-S1 support = 0 (ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient Is LSB
   01             // Clamp Control Coefficient Is MSB
   E8             // Clamp Control Coefficient If LSB
   03             // Clamp Control Coefficient If MSB
   C4             // Clamp Control Coefficient D LSB
   09             // Clamp Control Coefficient D MSB
   EE             // Temperature (00h = -18 degree C)
   01             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 1 (use TControl)
   
   

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    001B

   // Sensor Record Header
   0098           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   03             // FSC version 3
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   B0             // Clamp Header ID
   B0             // Temperature Sensor Number (B0h = DIMM Aggregate Thermal Margin ABC)
   00             // Entity Presence Sensor Number (0h = Not used)
   00             // Sensor Disabled Control Value (00h = Ignore this subrecord)
   64             // Sensor Fail Control Value (00h = Ignore this subrecord)
   00             // Sensor Unavailable Control Value (00h = Ignore this subrecord)
   00             // Sleep Control Value (0h = 0% PWM)
   28             // Sleep State and Hysteresis [7:6]-S1 support = 0 (ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient Is LSB
   00             // Clamp Control Coefficient Is MSB
   D0             // Clamp Control Coefficient If LSB
   01             // Clamp Control Coefficient If MSB
   88             // Clamp Control Coefficient D LSB
   13             // Clamp Control Coefficient D MSB
   FC             // Temperature (FCh = -4 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use fixed temp)


_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    001B

   // Sensor Record Header
   0099           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   03             // FSC version 3
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   B1             // Clamp Header ID
   B1             // Temperature Sensor Number (B1h = DIMM Aggregate Thermal Margin DEF)
   00             // Entity Presence Sensor Number (0h = Not used)
   00             // Sensor Disabled Control Value (00h = Ignore this subrecord)
   64             // Sensor Fail Control Value (00h = Ignore this subrecord)
   00             // Sensor Unavailable Control Value (00h = Ignore this subrecord)
   00             // Sleep Control Value (0h = 0% PWM)
   28             // Sleep State and Hysteresis [7:6]-S1 support = 0 (ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient Is LSB
   00             // Clamp Control Coefficient Is MSB
   D0             // Clamp Control Coefficient If LSB
   01             // Clamp Control Coefficient If MSB
   88             // Clamp Control Coefficient D LSB
   13             // Clamp Control Coefficient D MSB
   FC             // Temperature (FCh = -4 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use fixed temp)


_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    001B

   // Sensor Record Header
   009A           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   03             // FSC version 3
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   25             // Clamp Header ID
   25             // Temperature Sensor Number (25h = BB CPU VR Temp)
   00             // Entity Presence Sensor Number (0h = Not used)
   64             // Sensor Disabled Control Value (00h = Ignore this subrecord)
   64             // Sensor Fail Control Value (00h = Ignore this subrecord)
   64             // Sensor Unavailable Control Value (00h = Ignore this subrecord)
   00             // Sleep Control Value (0h = 0% PWM)
   28             // Sleep State and Hysteresis [7:6]-S1 support = 0 (ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   E8             // Clamp Control Coefficient Is LSB
   03             // Clamp Control Coefficient Is MSB
   70             // Clamp Control Coefficient If LSB
   17             // Clamp Control Coefficient If MSB
   D0             // Clamp Control Coefficient D LSB
   07             // Clamp Control Coefficient D MSB
   50             // Temperature (50h = 80 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use fixed temp)


_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    001B

   // Sensor Record Header
   009B           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   03             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   24             // Clamp Header ID
   24             // Temperature Sensor Number (24h = BB Memory VR Temp)
   00             // Entity Presence Sensor Number (0h = Not used)
   64             // Sensor Disabled Control Value (00h = Ignore this subrecord)
   64             // Sensor Fail Control Value (00h = Ignore this subrecord)
   64             // Sensor Unavailable Control Value (00h = Ignore this subrecord)
   00             // Sleep Control Value (0h = 0% PWM)
   28             // Sleep State and Hysteresis [7:6]-S1 support = 0 (ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   E8             // Clamp Control Coefficient Is LSB
   03             // Clamp Control Coefficient Is MSB
   70             // Clamp Control Coefficient If LSB
   17             // Clamp Control Coefficient If MSB
   D0             // Clamp Control Coefficient D LSB
   07             // Clamp Control Coefficient D MSB
   4A             // Temperature (4Ah = 74 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use fixed temp)


_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    001B

   // Sensor Record Header
   009C           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   03             // FSC version 3
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   23             // Clamp Header ID
   23             // Temperature Sensor Number (23h = BMC Temp)
   00             // Entity Presence Sensor Number (0h = Not used)
   64             // Sensor Disabled Control Value (00h = Ignore this subrecord)
   64             // Sensor Fail Control Value (00h = Ignore this subrecord)
   64             // Sensor Unavailable Control Value (00h = Ignore this subrecord)
   00             // Sleep Control Value (0h = 0% PWM)
   28             // Sleep State and Hysteresis [7:6]-S1 support = 0 (ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   E8             // Clamp Control Coefficient Is LSB
   03             // Clamp Control Coefficient Is MSB
   70             // Clamp Control Coefficient If LSB
   17             // Clamp Control Coefficient If MSB
   D0             // Clamp Control Coefficient D LSB
   07             // Clamp Control Coefficient D MSB
   4B             // Temperature (4Bh = 75 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use fixed temp)


_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    001B

   // Sensor Record Header
   009D           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   03             // FSC version 3
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   22             // Clamp Header ID
   22             // Temperature Sensor Number (22h = PCH Temp)
   00             // Entity Presence Sensor Number (0h = Not used)
   64             // Sensor Disabled Control Value (00h = Ignore this subrecord)
   64             // Sensor Fail Control Value (00h = Ignore this subrecord)
   64             // Sensor Unavailable Control Value (00h = Ignore this subrecord)
   00             // Sleep Control Value (0h = 0% PWM)
   28             // Sleep State and Hysteresis [7:6]-S1 support = 0 (ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   E8             // Clamp Control Coefficient Is LSB
   03             // Clamp Control Coefficient Is MSB
   70             // Clamp Control Coefficient If LSB
   17             // Clamp Control Coefficient If MSB
   D0             // Clamp Control Coefficient D LSB
   07             // Clamp Control Coefficient D MSB
   53             // Temperature (53h = 83 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use fixed temp)

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    001B

   // Sensor Record Header
   009D           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   03             // FSC version 3
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   27             // Clamp Header ID
   27             // Temperature Sensor Number (27h = PCI Riser 1 Temp)
   00             // Entity Presence Sensor Number (0h = Not used)
   64             // Sensor Disabled Control Value (00h = Ignore this subrecord)
   64             // Sensor Fail Control Value (00h = Ignore this subrecord)
   64             // Sensor Unavailable Control Value (00h = Ignore this subrecord)
   00             // Sleep Control Value (0h = 0% PWM)
   28             // Sleep State and Hysteresis [7:6]-S1 support = 0 (ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient Is LSB
   00             // Clamp Control Coefficient Is MSB
   D0             // Clamp Control Coefficient If LSB
   01             // Clamp Control Coefficient If MSB
   E8             // Clamp Control Coefficient D LSB
   03             // Clamp Control Coefficient D MSB
   36             // Temperature (36h = 54 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use fixed temp)
 
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    001B

   // Sensor Record Header
   009D           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   03             // FSC version 3
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   2C             // Clamp Header ID
   2C             // Temperature Sensor Number (2Ch = PCI Riser 2 Temp)
   00             // Entity Presence Sensor Number (0h = Not used)
   64             // Sensor Disabled Control Value (00h = Ignore this subrecord)
   64             // Sensor Fail Control Value (00h = Ignore this subrecord)
   64             // Sensor Unavailable Control Value (00h = Ignore this subrecord)
   00             // Sleep Control Value (0h = 0% PWM)
   28             // Sleep State and Hysteresis [7:6]-S1 support = 0 (ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient Is LSB
   00             // Clamp Control Coefficient Is MSB
   D0             // Clamp Control Coefficient If LSB
   01             // Clamp Control Coefficient If MSB
   E8             // Clamp Control Coefficient D LSB
   03             // Clamp Control Coefficient D MSB
   37             // Temperature (37h = 55 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use fixed temp)
   

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    001B

   // Sensor Record Header
   009F           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   03             // FSC version 3
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   5C             // Clamp Header ID
   5C             // Temperature Sensor Number (5Ch = PSU1 Temperature)
   00             // Entity Presence Sensor Number (0h = Not used)
   64             // Sensor Disabled Control Value (00h = Ignore this subrecord)
   64             // Sensor Fail Control Value (00h = Ignore this subrecord)
   64             // Sensor Unavailable Control Value (00h = Ignore this subrecord)
   00             // Sleep Control Value (0h = 0% PWM)
   28             // Sleep State and Hysteresis [7:6]-S1 support = 0 (ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   E8             // Clamp Control Coefficient Is LSB
   03             // Clamp Control Coefficient Is MSB
   70             // Clamp Control Coefficient If LSB
   17             // Clamp Control Coefficient If MSB
   D0             // Clamp Control Coefficient D LSB
   07             // Clamp Control Coefficient D MSB
   37             // Temperature (37h = 55 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use fixed temp)


_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    001B

   // Sensor Record Header
   00A0           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   03             // FSC version 3
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   5D             // Clamp Header ID
   5D             // Temperature Sensor Number (5Dh = PSU2 Temperature)
   00             // Entity Presence Sensor Number (0h = Not used)
   64             // Sensor Disabled Control Value (00h = Ignore this subrecord)
   64             // Sensor Fail Control Value (00h = Ignore this subrecord)
   64             // Sensor Unavailable Control Value (00h = Ignore this subrecord)
   00             // Sleep Control Value (0h = 0% PWM)
   28             // Sleep State and Hysteresis [7:6]-S1 support = 0 (ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   E8             // Clamp Control Coefficient Is LSB
   03             // Clamp Control Coefficient Is MSB
   70             // Clamp Control Coefficient If LSB
   17             // Clamp Control Coefficient If MSB
   D0             // Clamp Control Coefficient D LSB
   07             // Clamp Control Coefficient D MSB
   37             // Temperature (37h = 55 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use fixed temp)


_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    001B

   // Sensor Record Header
   00A1           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   03             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   29             // Clamp Header ID
   29             // Temperature Sensor Number (29h = HSBP PSOC 1 Temp)
   00             // Entity Presence Sensor Number (0h = Not used)
   64             // Sensor Disabled Control Value (00h = Ignore this subrecord)
   64             // Sensor Fail Control Value (00h = Ignore this subrecord)
   64             // Sensor Unavailable Control Value (00h = Ignore this subrecord)
   00             // Sleep Control Value (0h = 0% PWM)
   28             // Sleep State and Hysteresis [7:6]-S1 support = 0 (ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   E8             // Clamp Control Coefficient Is LSB
   03             // Clamp Control Coefficient Is MSB
   70             // Clamp Control Coefficient If LSB
   17             // Clamp Control Coefficient If MSB
   D0             // Clamp Control Coefficient D LSB
   07             // Clamp Control Coefficient D MSB
   37             // Temperature (37h = 55 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use fixed temp)


_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    001B

   // Sensor Record Header
   00A2           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   03             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   83             // Clamp Header ID
   83             // Temperature Sensor Number (83h = P1 DTS Therm Margin)
   00             // Entity Presence Sensor Number (0h = Not used)
   64             // Sensor Disabled Control Value (00h = Ignore this subrecord)
   64             // Sensor Fail Control Value (00h = Ignore this subrecord)
   64             // Sensor Unavailable Control Value (00h = Ignore this subrecord)
   00             // Sleep Control Value (0h = 0% PWM)
   18             // Sleep State and Hysteresis [7:6]-S1 support = 0 (ignore); [5:3]-Negative Hysteresis = 3; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient Is LSB
   01             // Clamp Control Coefficient Is MSB
   E8             // Clamp Control Coefficient If LSB
   03             // Clamp Control Coefficient If MSB
   C4             // Clamp Control Coefficient D LSB
   09             // Clamp Control Coefficient D MSB
   FE             // Temperature (FCh = -2 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use fixed temp)

   
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    001B

   // Sensor Record Header
   00A2           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   03             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   93             // Clamp Header ID
   83             // Temperature Sensor Number (83h = P1 DTS Therm Margin)
   00             // Entity Presence Sensor Number (0h = Not used)
   64             // Sensor Disabled Control Value (00h = Ignore this subrecord)
   64             // Sensor Fail Control Value (00h = Ignore this subrecord)
   64             // Sensor Unavailable Control Value (00h = Ignore this subrecord)
   00             // Sleep Control Value (0h = 0% PWM)
   28             // Sleep State and Hysteresis [7:6]-S1 support = 0 (ignore); [5:3]-Negative Hysteresis = 5; [2:0]-Positive Hysteresis = 0
   40             // Clamp Control Coefficient Is LSB
   01             // Clamp Control Coefficient Is MSB
   E8             // Clamp Control Coefficient If LSB
   03             // Clamp Control Coefficient If MSB
   C4             // Clamp Control Coefficient D LSB
   09             // Clamp Control Coefficient D MSB
   EE             // Temperature (EEh = -18 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use fixed temp)


_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    001B

   // Sensor Record Header
   00A3           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   03             // Record Version
   00             // FSC Record Type (00h = Global Clamp Header Records)

   // Global Clamp Header Record
   2E             // Clamp Header ID
   2E             // Temperature Sensor Number (2Eh = Texit Temp)
   00             // Entity Presence Sensor Number (0h = Not used)
   64             // Sensor Disabled Control Value (00h = Ignore this subrecord)
   64             // Sensor Fail Control Value (00h = Ignore this subrecord)
   64             // Sensor Unavailable Control Value (00h = Ignore this subrecord)
   00             // Sleep Control Value (0h = 0% PWM)
   10             // Sleep State and Hysteresis [7:6]-S1 support = 0 (ignore); [5:3]-Negative Hysteresis = 2; [2:0]-Positive Hysteresis = 0
   80             // Clamp Control Coefficient LSB
   00             // Clamp Control Coefficient Is MSB
   D0             // Clamp Control Coefficient If LSB
   01             // Clamp Control Coefficient If MSB
   E8             // Clamp Control Coefficient D LSB
   03             // Clamp Control Coefficient D MSB
   42             // Temperature (42h = 66 degree C)
   00             // Clamp Flags [7:4] - CPU Number = 0; [3:1] - Reserved=0; [0] - Temp Source = 0 (use fixed temp)


//*****************************************************************************
// FSC Record Type = 01h (Global Stepwise Header Record)
// All Chassis
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0013

   // Sensor Record Header
   00A4           // Record ID
   51             // SDR Version
   C0             // Record Type
   0E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   21             // FSC Record Type (01h = Global Stepwise Header Records)

   // Global Stepwise Header Record
   00             // Stepwise Header ID
   21             // Temperature Sensor Number (21h = HSBP Temp)
   00             // Entity Presence Sensor Number (0h = Not Used)
   64             // Sensor Disabled Control Value (00h = Ignore this subrecord)
   64             // Sensor Fail Control Value (00h = Ignore this subrecord)
   64             // Sensor Unavailable Control Value (00h = Ignore this subrecord)
   00             // Sleep Control Value (0h = 0% PWM)
   50             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 2; [2:0]-Positive Hysteresis = 0


_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0013

   // Sensor Record Header
   00A5           // Record ID
   51             // SDR Version
   C0             // Record Type
   0E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   21             // FSC Record Type (01h = Global Stepwise Header Records)

   // Global Stepwise Header Record
   01             // Stepwise Header ID
   20             // Temperature Sensor Number (20h = BB Inlet Temp)
   00             // Entity Presence Sensor Number (0h = Not Used)
   64             // Sensor Disabled Control Value (00h = Ignore this subrecord)
   64             // Sensor Fail Control Value (00h = Ignore this subrecord)
   64             // Sensor Unavailable Control Value (00h = Ignore this subrecord)
   00             // Sleep Control Value (0h = 0% PWM)
   50             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 2; [2:0]-Positive Hysteresis = 0


_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0013

   // Sensor Record Header
   00A5           // Record ID
   51             // SDR Version
   C0             // Record Type
   0E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   11             // FSC Record Type (01h = Global Stepwise Header Records)

   // Global Stepwise Header Record
   02             // Stepwise Header ID
   01             // Temperature Sensor Number (01h = PS)
   00             // Entity Presence Sensor Number (0h = Not Used)
   00             // Sensor Disabled Control Value (00h = Ignore this subrecord)
   00             // Sensor Fail Control Value (00h = Ignore this subrecord)
   00             // Sensor Unavailable Control Value (00h = Ignore this subrecord)
   00             // Sleep Control Value (0h = 0% PWM)
   00             // Sleep State and Hysteresis [7:6]-Supported in S1 (1=yes); [5:3]-Negative Hysteresis = 0; [2:0]-Positive Hysteresis = 0


//*****************************************************************************
// FSC Record Type = 02h (Global Stepwise Curve Record)
// All Chassis
//*****************************************************************************

//*****************************************************************************
// Adams Pass BCP 3.5" HDD

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    003D

   // Sensor Record Header
   00A6           // Record ID
   51             // SDR Version
   C0             // Record Type
   38             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   00             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=No); [6:0]- Count of control pairs = 4
   0F             // Temperature 1 (0Fh = 15C)
   1E             // Control Value 1 PWM (1Eh = 30%)
   19             // Temperature 2 (19h = 25C)
   28             // Control Value 2 PWM (28h = 40%)
   23             // Temperature 3 (23h = 35C)
   32             // Control Value 3 PWM (32h = 50%)
   2D             // Temperature 4 (2Dh = 45C)
   64             // Control Value 4 PWM (64h = 100%)

   // Global Stepwise Curve Record
   01             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=No); [6:0]- Count of control pairs = 4
   0F             // Temperature 1 (0Fh = 15C)
   20             // Control Value 1 PWM (20h = 32%)
   19             // Temperature 2 (19h = 25C)
   2A             // Control Value 2 PWM (2Ah = 42%)
   23             // Temperature 3 (23h = 35C)
   34             // Control Value 3 PWM (34h = 52%)
   2D             // Temperature 4 (2Dh = 45C)
   64             // Control Value 4 PWM (64h = 100%)

   // Global Stepwise Curve Record
   02             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=No); [6:0]- Count of control pairs = 4
   0F             // Temperature 1 (0Fh = 15C)
   23             // Control Value 1 PWM (23h = 35%)
   19             // Temperature 2 (19h = 25C)
   2D             // Control Value 2 PWM (2Dh = 45%)
   23             // Temperature 3 (23h = 35C)
   3C             // Control Value 3 PWM (3Ch = 60%)
   2D             // Temperature 4 (2Dh = 45C)
   64             // Control Value 4 PWM (64h = 100%)

   // Global Stepwise Curve Record
   03             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=No); [6:0]- Count of control pairs = 4
   0F             // Temperature 1 (0Fh = 15C)
   28             // Control Value 1 PWM (28h = 40%)
   19             // Temperature 2 (19h = 25C)
   3C             // Control Value 2 PWM (3Ch = 60%)
   35             // Temperature 3 (23h = 35C)
   4B             // Control Value 3 PWM (4Bh = 75%)
   2D             // Temperature 4 (2Dh = 45C)
   64             // Control Value 4 PWM (64h = 100%)

   // Global Stepwise Curve Record
   04             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=No); [6:0]- Count of control pairs = 4
   0F             // Temperature 1 (0Fh = 15C)
   2D             // Control Value 1 PWM (2Dh = 45%)
   19             // Temperature 2 (19h = 25C)
   41             // Control Value 2 PWM (41h = 65%)
   23             // Temperature 3 (23h = 35C)
   50             // Control Value 3 PWM (50h = 80%)
   2D             // Temperature 4 (2Dh = 45C)
   64             // Control Value 4 PWM (64h = 100%)


_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    0031

   // Sensor Record Header
   00A7           // Record ID
   51             // SDR Version
   C0             // Record Type
   2C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   05             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=No); [6:0]- Count of control pairs = 4
   0F             // Temperature 1 (0Fh = 15C)
   32             // Control Value 1 PWM (32h = 50%)
   19             // Temperature 2 (19h = 25C)
   46             // Control Value 2 PWM (46h = 70%)
   23             // Temperature 3 (23h = 35C)
   55             // Control Value 3 PWM (55h = 85%)
   2D             // Temperature 4 (2Dh = 45C)
   64             // Control Value 4 PWM (64h = 100%)

   // Global Stepwise Curve Record
   06             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=No); [6:0]- Count of control pairs = 4
   0F             // Temperature 1 (0Fh = 15C)
   37             // Control Value 1 PWM (37h = 55%)
   19             // Temperature 2 (19h = 25C)
   4B             // Control Value 2 PWM (4Bh = 75%)
   23             // Temperature 3 (23h = 35C)
   5A             // Control Value 3 PWM (5Ah = 90%)
   2D             // Temperature 4 (2Dh = 45C)
   64             // Control Value 4 PWM (64h = 100%)

      // Global Stepwise Curve Record
   07             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=No); [6:0]- Count of control pairs = 4
   0F             // Temperature 1 (0Fh = 15C)
   3C             // Control Value 1 PWM (3Ch = 60%)
   19             // Temperature 2 (19h = 25C)
   50             // Control Value 2 PWM (50h = 80%)
   23             // Temperature 3 (23h = 35C)
   5F             // Control Value 3 PWM (5Fh = 95%)
   2D             // Temperature 4 (2Dh = 45C)
   64             // Control Value 4 PWM (64h = 100%)

   // Global Stepwise Curve Record
   08             // Stepwise Curve ID
   83             // Domain max and Count [7]-Domain Max (0=No); [6:0]- Count of control pairs = 3
   0F             // Temperature 1 (0Fh = 15C)
   64             // Control Value 1 PWM (64h = 100%)
   19             // Temperature 2 (19h = 25C)
   64             // Control Value 2 PWM (64h = 100%)
   23             // Temperature 3 (23h = 35C)
   64             // Control Value 3 PWM (64h = 100%)
   

//*****************************************************************************
// Adams Pass BCP 2.5" HDD

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    0033

   // Sensor Record Header
   00A8           // Record ID
   51             // SDR Version
   C0             // Record Type
   2E             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   09             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (1=Yes); [6:0]- Count of control pairs = 4
   0F             // Temperature 1 (0Fh = 15C)
   19             // Control Value 1 PWM (19h = 25%)
   19             // Temperature 2 (19h = 25C)
   23             // Control Value 2 PWM (23h = 35%)
   23             // Temperature 3 (23h = 35C)
   2D             // Control Value 3 PWM (2Dh = 45%)
   2D             // Temperature 4 (2Dh = 45C)
   64             // Control Value 4 PWM (64h = 100%)

   // Global Stepwise Curve Record
   0A             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=No); [6:0]- Count of control pairs = 4
   0F             // Temperature 1 (0Fh = 15C)
   1B             // Control Value 1 PWM (1Bh = 27%)
   19             // Temperature 2 (19h = 25C)
   25             // Control Value 2 PWM (25h = 37%)
   23             // Temperature 3 (23h = 35C)
   2F             // Control Value 3 PWM (2Fh = 47%)
   2D             // Temperature 4 (2Dh = 45C)
   64             // Control Value 4 PWM (64h = 100%)


   // Global Stepwise Curve Record
   0B             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=No); [6:0]- Count of control pairs = 4
   0F             // Temperature 1 (0Fh = 15C)
   23             // Control Value 1 PWM (23h = 35%)
   19             // Temperature 2 (19h = 25C)
   2D             // Control Value 2 PWM (2Dh = 45%)
   23             // Temperature 3 (23h = 35C)
   37             // Control Value 3 PWM (37h = 55%)
   2D             // Temperature 4 (2Dh = 45C)
   64             // Control Value 4 PWM (64h = 100%)


   // Global Stepwise Curve Record
   0C             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=No); [6:0]- Count of control pairs = 4
   0F             // Temperature 1 (0Fh = 15C)
   28             // Control Value 1 PWM (28h = 40%)
   19             // Temperature 2 (19h = 25C)
   32             // Control Value 2 PWM (32h = 50%)
   23             // Temperature 3 (23h = 35C)
   3C             // Control Value 3 PWM (3Ch = 60%)
   2D             // Temperature 4 (2Dh = 45C)
   64             // Control Value 4 PWM (64h = 100%)


  
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    003D

   // Sensor Record Header
   00A9           // Record ID
   51             // SDR Version
   C0             // Record Type
   38             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   0D             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=No); [6:0]- Count of control pairs = 4
   0F             // Temperature 1 (0Fh = 15C)
   2D             // Control Value 1 PWM (2Dh = 45%)
   19             // Temperature 2 (19h = 25C)
   37             // Control Value 2 PWM (37h = 55%)
   23             // Temperature 3 (23h = 35C)
   41             // Control Value 3 PWM (41h = 65%)
   2D             // Temperature 4 (2Dh = 45C)
   64             // Control Value 4 PWM (64h = 100%)


   // Global Stepwise Curve Record
   0E             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (1=Yes); [6:0]- Count of control pairs = 4
   0F             // Temperature 1 (0Fh = 15C)
   32             // Control Value 1 PWM (32h = 50%)
   19             // Temperature 2 (19h = 25C)
   3C             // Control Value 2 PWM (3Ch = 60%)
   23             // Temperature 3 (23h = 35C)
   46             // Control Value 3 PWM (46h = 70%)
   2D             // Temperature 4 (2Dh = 45C)
   64             // Control Value 4 PWM (64h = 100%)


   // Global Stepwise Curve Record
   0F             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=No); [6:0]- Count of control pairs = 4
   0F             // Temperature 1 (0Fh = 15C)
   37             // Control Value 1 PWM (37h = 55%)
   19             // Temperature 2 (19h = 25C)
   41             // Control Value 2 PWM (41h = 65%)
   23             // Temperature 3 (23h = 35C)
   4B             // Control Value 3 PWM (4Bh = 75%)
   2D             // Temperature 4 (2Dh = 45C)
   64             // Control Value 4 PWM (64h = 100%)

   
   // Global Stepwise Curve Record
   10             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=No); [6:0]- Count of control pairs = 4
   0F             // Temperature 1 (0Fh = 15C)
   3C             // Control Value 1 PWM (3Ch = 60%)
   19             // Temperature 2 (19h = 25C)
   46             // Control Value 2 PWM (46h = 70%)
   23             // Temperature 3 (23h = 35C)
   50             // Control Value 3 PWM (50h = 80%)
   2D             // Temperature 4 (2Dh = 45C)
   64             // Control Value 4 PWM (64h = 100%)
   

   // Global Stepwise Curve Record
   11             // Stepwise Curve ID
   84             // Domain max and Count [7]-Domain Max (0=No); [6:0]- Count of control pairs = 4
   0F             // Temperature 1 (0Fh = 15C)
   64             // Control Value 1 PWM (64h = 100%)
   19             // Temperature 2 (19h = 25C)
   64             // Control Value 2 PWM (64h = 100%)
   23             // Temperature 3 (23h = 35C)
   64             // Control Value 3 PWM (64h = 100%)
   2D             // Temperature 4 (2Dh = 45C)
   64             // Control Value 4 PWM (64h = 100%)



//*****************************************************************************
// PSU LCC 3.5"

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    0015

   // Sensor Record Header
   00AA           // Record ID
   51             // SDR Version
   C0             // Record Type
   10             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   12             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=No); [6:0]- Count of control pairs = 3
   0F             // Temperature 1 (0Fh = 15C)
   1E             // Control Value 1 PWM (1Eh = 30%)
   19             // Temperature 2 (19h = 25C)
   23             // Control Value 2 PWM (23h = 35%)
   23             // Temperature 3 (23h = 35C)
   2D             // Control Value 3 PWM (2Dh = 45%)
   2D             // Temperature 4 (2Dh = 45C)
   64             // Control Value 4 PWM (64h = 100%)


//*****************************************************************************
// PSU LCC 2.5"

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    0015

   // Sensor Record Header
   00AB           // Record ID
   51             // SDR Version
   C0             // Record Type
   10             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   13             // Stepwise Curve ID
   04             // Domain max and Count [7]-Domain Max (0=No); [6:0]- Count of control pairs = 4
   0F             // Temperature 1 (0Fh = 15C)
   1E             // Control Value 1 PWM (1Eh = 30%)
   19             // Temperature 2 (19h = 25C)
   23             // Control Value 2 PWM (23h = 35%)
   23             // Temperature 3 (23h = 35C)
   2D             // Control Value 3 PWM (2Dh = 45%)
   2D             // Temperature 4 (2Dh = 45C)
   64             // Control Value 4 PWM (64h = 100%)

//*****************************************************************************
// Test Plate

_SDR_TYPE   C0
_SDR_TAG    'TEST_PLATE'
_REC_LEN    0017

   // Sensor Record Header
   00AC           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   14             // Stepwise Curve ID
   05             // Domain max and Count [7]-Domain Max (0=No); [6:0]- Count of control pairs = 4
   0F             // Temperature 1 (0Fh = 15C)
   4B             // Control Value 1 PWM (4Bh = 75%)
   19             // Temperature 2 (19h = 25C)
   4B             // Control Value 2 PWM (4Bh = 75%)
   1C             // Temperature 3 (1Ch = 28C)
   4B             // Control Value 3 PWM (4Bh = 75%)
   21             // Temperature 4 (21h = 33C)
   4B             // Control Value 4 PWM (4Bh = 75%)
   23             // Temperature 5 (23h = 35C)
   4B             // Control Value 5 PWM (4Bh = 75%)

//*****************************************************************************
// OTHER Acoustic

_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0017

   // Sensor Record Header
   00AD           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   5B             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=No); [6:0]- Count of control pairs = 2
   1E             // Temperature 1 (1Eh = 30C)
   19             // Control Value 1 PWM (19h = 25%)
   64             // Temperature 2 (64h = 100C)
   53             // Control Value 2 PWM (53h = 83%)

//*****************************************************************************
// OTHER Performance

   // Global Stepwise Curve Record
   5C             // Stepwise Curve ID
   02             // Domain max and Count [7]-Domain Max (0=No); [6:0]- Count of control pairs = 2
   1E             // Temperature 1 (1Eh = 30C)
   28             // Control Value 1 PWM (28h = 40%)
   41             // Temperature 2 (41h = 65C)
   64             // Control Value 2 PWM (64h = 100%)


//*****************************************************************************
// ucc all

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0011

   // Sensor Record Header
   00AE           // Record ID
   51             // SDR Version
   C0             // Record Type
   0C             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   02             // FSC Record Type (02h = Global Stepwise Curve Records)

   // Global Stepwise Curve Record
   64             // Stepwise Curve ID
   82             // Domain max and Count [7]-Domain Max (1=Yes); [6:0]- Count of control pairs = 2
   1E             // Temperature 1 (1Eh = 30C)
   64             // Control Value 1 PWM (64h = 100%)
   3C             // Temperature 2 (3Ch = 60C)
   64             // Control Value 2 PWM (64h = 100%)


//*****************************************************************************
// FSC Record Type = 03h (Fan Sensor Domain Map Record)
// H2300KNP / H2200KNP Chassis
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    0017

   // Sensor Record Header
   00AF           // Record ID
   51             // SDR Version
   C0             // Record Type
   12             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   03             // FSC Record Type (03h = Fan Sensor Domain Map)

   // Domain Fan Configuration
   06             // [7:4]-Domain Number = 0; [3:0]-Count of sensor numbers = 6
   35             // Fan Sensor Number 1 (35h = Sys Fan 1A)
   36             // Fan Sensor Number 2 (36h = Sys Fan 1B)
   37             // Fan Sensor Number 3 (37h = Sys Fan 2A)
   38             // Fan Sensor Number 4 (38h = Sys Fan 2B)
   3B             // Fan Sensor Number 5 (3Bh = Sys Fan 3A)
   3C             // Fan Sensor Number 6 (3Ch = Sys Fan 3B)
   24             // [7:4]-Domain Number = 2; [3:0]-Count of sensor numbers = 4
   A0             // Fan Sensor Number 7 (A0h = PS1 Fan Fail / PS1 1a Fan Fail)
   A1             // Fan Sensor Number 8 (A1h = PS1 1b Fan Fail)
   A4             // Fan Sensor Number 9 (A4h = PS2 Fan Fail / PS2 1a Fan Fail)
   A5             // Fan Sensor Number 10 (A5h = PS2 1b Fan Fail)


//*****************************************************************************
// FSC Record Type = 03h (Fan Sensor Domain Map Record)
// Other Chassis
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0019

   // Sensor Record Header
   00B0           // Record ID
   51             // SDR Version
   C0             // Record Type
   14             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   03             // FSC Record Type (03h = Fan Sensor Domain Map)

   // Domain Fan Configuration
   06             // [7:4]-Domain Number = 0; [3:0]-Count of sensor numbers = 6
   35             // Fan Sensor Number 1 (35h = Sys Fan 1A)
   36             // Fan Sensor Number 2 (36h = Sys Fan 1B)
   37             // Fan Sensor Number 3 (37h = Sys Fan 2A)
   38             // Fan Sensor Number 4 (38h = Sys Fan 2B)
   3B             // Fan Sensor Number 5 (3Bh = Sys Fan 3A)
   3C             // Fan Sensor Number 6 (3Ch = Sys Fan 3B)
   16             // [7:4]-Domain Number = 1; [3:0]-Count of sensor numbers = 6
   36             // Fan Sensor Number 7 (36h = Sys Fan 4A)
   37             // Fan Sensor Number 8 (37h = Sys Fan 4B)
   38             // Fan Sensor Number 9 (38h = Sys Fan 5A)
   39             // Fan Sensor Number 10 (39h = Sys Fan 5B)
   3A             // Fan Sensor Number 11 (3Ah = Sys Fan 6A)
   3B             // Fan Sensor Number 12 (3Bh = Sys Fan 6B)


//*****************************************************************************
// Domain 0 - H2300KNP / H2200KNP
//*****************************************************************************
//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//*****************************************************************************


//*****************************************************************************
// H2300KNP Chassis, Domain 0, Profiles 0 & 1

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    001C

   // Sensor Record Header
   00B1           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Support
   01             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value (19h = 25%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use Advanced Fan Failure sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E		      // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   00             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    001C

   // Sensor Record Header
   00B2           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Support
   02             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value (19h = 25%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   01             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID


//*****************************************************************************
// H2300KNP Chassis, Domain 0, Profiles 2 & 3

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    001C

   // Sensor Record Header
   00B3           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Support
   04             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value (19h = 25%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   02             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    001C

   // Sensor Record Header
   00B4           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Support
   08             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value (19h = 25%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   03             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID


//*****************************************************************************
// H2300KNP Chassis, Domain 0, Profiles 4 & 5

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    001C

   // Sensor Record Header
   00B5           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Support
   10             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value (19h = 25%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   04             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    001C

   // Sensor Record Header
   00B6           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Support
   20             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value (19h = 25%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   05             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID


//*****************************************************************************
// H2300KNP Chassis, Domain 0, Profile 6

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    001C

   // Sensor Record Header
   00B7           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Support
   40             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value (19h = 25%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   06             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

//*****************************************************************************
// H2300KNP Chassis, Domain 0, Profile 7

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    001C

   // Sensor Record Header
   00B7           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Support
   80             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value (19h = 25%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   07             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID



//*****************************************************************************
// H2200KNP Chassis, Domain 0, Profiles 0 & 1

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    001C

   // Sensor Record Header
   00B8           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Support
   01             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value (19h = 25%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   09             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    001C

   // Sensor Record Header
   00B9           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Support
   02             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value (19h = 25%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0A             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID


//*****************************************************************************
// H2200KNP Chassis, Domain 0, Profiles 2 & 3

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    001C

   // Sensor Record Header
   00BA           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Support
   04             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value (19h = 25%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0B             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    001C

   // Sensor Record Header
   00BB           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Support
   08             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value (19h = 25%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0C             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//*****************************************************************************
// H2200KNP Chassis, Domain 0, Profiles 4 & 5

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    001C

   // Sensor Record Header
   00BC           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Support
   10             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value (19h = 25%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0D             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    001C

   // Sensor Record Header
   00BD           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Support
   20             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value (19h = 25%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0E             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

//*****************************************************************************
// H2200KNP Chassis, Domain 0, Profile 6 & 7

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    001C

   // Sensor Record Header
   00BE           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Support
   40             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value (19h = 25%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   0F             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID
   
_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    001C

   // Sensor Record Header
   00BE           // Record ID
   51             // SDR Version
   C0             // Record Type
   17             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Support
   80             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   19             // Normal Control Value (19h = 25%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   10             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID



//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// H2300KNP / H2200KNP Chassis, Domain 0, Profiles 0,1,2
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    0027

   // Sensor Record Header
   00BF           // Record ID
   51             // SDR Version
   C0             // Record Type
   22             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Support
   07             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID 
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID 
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID 
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   83             // Clamp ID 
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID 
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID 
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID 
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID 
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID 
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   27             // Clamp ID 
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   2C             // Clamp ID 
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID 
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID 
    
   
   
//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// H2300KNP / H2200KNP Chassis, Domain 0, Profiles 3,4,5,6,7
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    0027

   // Sensor Record Header
   00BF           // Record ID
   51             // SDR Version
   C0             // Record Type
   22             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Support
   F8             // Fan Profile Support

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   94             // Clamp ID 
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID 
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID 
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   93             // Clamp ID 
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID 
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID 
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID 
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID 
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID 
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   27             // Clamp ID 
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   2C             // Clamp ID 
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID 
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID 
 


//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// FSC Sub-record Type = 05h (Fans Off)
// H2300KNP / H2200KNP Chassis, Domain 0, All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    001B

   // Sensor Record Header
   00C0           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   01             // Domain Support
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   64             // Domain 0 Fan Failure Value (64h = 100% PWM)
   FF             // Domain 1 Fan Failure Value (FFh = No Change)
   FF             // Domain 2 Fan Failure Value (FFh = No Change)
   FF             // Domain 3 Fan Failure Value (FFh = No Change)
   FF             // Domain 4 Fan Failure Value (FFh = No Change)
   FF             // Domain 5 Fan Failure Value (FFh = No Change)
   FF             // Domain 6 Fan Failure Value (FFh = No Change)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)

   // Fans-off and Low Speed sub-record
   05             // FSC Sub-Record Type (05h = Fans Off)
   C8             // Sensor Number Controlling Operation (C8h = Agg Thrm Mgn 1)
   C4             // Fans Off Control Value (C4h = -60 Degrees)
   0A             // Hysteresis (0Ah = 10)
   00             // Fans Off PWM (0%), and fan tachometer sensor scanning will be turned off


//*****************************************************************************
// Domain 2 - H2300KNP / H2200KNP
//*****************************************************************************
//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//*****************************************************************************


//*****************************************************************************
// H2300KNP Chassis, Domain 2(Power Supply), All Profiles

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    0022

   // Sensor Record Header
   00C1           // Record ID
   51             // SDR Version
   C0             // Record Type
   1D             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   18             // FSC Record Type (18h = Power Supply Main Domain)
   04             // Domain Support
   7F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   2D             // Normal Control Value (2Dh = 45%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   12             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   08             // Stepwise Curve ID

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID (5Ch = 5Ch)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID (5Dh = 5Dh)


//*****************************************************************************
// H2200KNP Chassis, Domain 2(Power Supply), All Profiles

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    0022

   // Sensor Record Header
   00C2           // Record ID
   51             // SDR Version
   C0             // Record Type
   1D             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   18             // FSC Record Type (18h = Power Supply Main Domain)
   04             // Domain Support
   7F             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   2D             // Normal Control Value (2Dh = 45%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   01             // Sensor Exclusion Count (1h = 1 sensor to exclude)
   2E             // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   13             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   00             // Stepwise Header ID
   11             // Stepwise Curve ID

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   29             // Clamp ID (29h = 29h)
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID (5Ch = 5Ch)
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID (5Dh = 5Dh)


//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 04h (Advanced Fan Failure)
// H2300KNP / H2200KNP Chassis, Domain 2(Power Supply), All Profiles
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    0016

   // Sensor Record Header
   00C3           // Record ID
   51             // SDR Version
   C0             // Record Type
   11             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype (0Ch = Fan Speed Control Configuration Record)
   02             // Record Version
   18             // FSC Record Type (18h = Power Supply Main Domain)
   40             // Domain Support
   FF             // Fan Profile Support

   // Advanced Fan Failure Sub-Record
   04             // FSC Sub-Record Type (04h = Advanced Fan Failure)
   FF             // Domain 0 Fan Failure Value (FFh = No Change)
   FF             // Domain 1 Fan Failure Value (FFh = No Change)
   FF             // Domain 2 Fan Failure Value (FFh = No Change)
   FF             // Domain 3 Fan Failure Value (FFh = No Change)
   FF             // Domain 4 Fan Failure Value (FFh = No Change)
   FF             // Domain 5 Fan Failure Value (FFh = No Change)
   64             // Domain 6 Fan Failure Value (64h = 100% PWM)
   FF             // Domain 7 Fan Failure Value (FFh = No Change)


//*****************************************************************************
// All Domains, Shipping & Test Plate Configuration
//*****************************************************************************
//*****************************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
// FSC Sub-record Type = 03h (Clamp sub-record)
// Domain 0 & 1, Profiles 0
//*****************************************************************************

_SDR_TYPE   C0
_SDR_TAG    'TEST_PLATE'
_REC_LEN    0035

   // Sensor Record Header
   00C4           // Record ID
   51             // SDR Version
   C0             // Record Type
   30             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   03             // Domain Mask (All Domains)
   01             // Fan Profile Support (All Profiles)

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (64h = 100%)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   00             // Sensor Exclusion Count (0h = 0 sensors to exclude)
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   06             // Stepwise Curve ID

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   08             // Stepwise Curve ID

   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID 
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID 
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID 
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   83             // Clamp ID 
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID 
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID 
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID 
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID 
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID 
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   27             // Clamp ID 
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   2C             // Clamp ID 
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID 
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID 

//****************************************************************
// All Domains - OTHER Master Acoustic, Performance
//****************************************************************
//****************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 01h (Domain Configuration)
// FSC Sub-record Type = 02h (Stepwise sub-record)
//****************************************************************

//****************************************************************
// Other Master Chassis, Domains 0, 1, 2 Profile 0

_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    001B

   // Sensor Record Header
   00C5           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   07             // Domain Support
   01             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   14             // Normal Control Value (14h = 20%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID (64h = 100)

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID (64h = 100)


//****************************************************************
// Other Master Chassis, Domains 0, 1, 2 Profile 1

_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    001B

   // Sensor Record Header
   00C6           // Record ID
   51             // SDR Version
   C0             // Record Type
   16             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   07             // Domain Support
   02             // Fan Profile Support

   // Domain Configuration
   01             // FSC Sub-Record Type (01h = Domain Configuration)
   28             // Normal Control Value (28h = 40%)
   64             // Ramp Step (64h = 100%)
   01             // Scan Rate
   FF             // Fan Fault Boost Value (FFh = Use sub-record type 04h)
   64             // Temperature Threshold Boost Value (64h = 100%)
   64             // Chassis Cover Boost Value (64h = 100%)
   00             // Sensor Exclusion Count
                  // Sensor Number To Exclude From Fan Boost

   // Stepwise Lower Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   5C             // Stepwise Curve ID (5Ch = 92)

   // Stepwise Upper Clipping Curve Sub-Record
   02             // FSC Sub-Record Type (02h = Stepwise)
   01             // Stepwise Header ID
   64             // Stepwise Curve ID (64h = 100)


//****************************************************************
// FSC Record Type = 08h (Main Domain Record)
// FSC Sub-record Type = 03h (Clamp sub-record)
//****************************************************************

//****************************************************************
// Other Master Chassis, Domain 0, All Profiles

_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    0027

   // Sensor Record Header
   00C7           // Record ID
   51             // SDR Version
   C0             // Record Type
   22             // Record Length

   // Record Body Bytes
   570100         // Manufacturer ID
   0C             // Record Subtype Value (Fan Speed Control SDR Record, rev 2)
   02             // Record Version
   08             // FSC Record Type (08h = Main Domain)
   07             // Domain Support
   03             // Fan Profile Support
   // Clamp Sub-Record 1
   03             // FSC Sub-Record Type (03h = Clamp)
   74             // Clamp ID 
   // Clamp Sub-Record 2
   03             // FSC Sub-Record Type (03h = Clamp)
   B0             // Clamp ID 
   // Clamp Sub-Record 3
   03             // FSC Sub-Record Type (03h = Clamp)
   B1             // Clamp ID 
   // Clamp Sub-Record 4
   03             // FSC Sub-Record Type (03h = Clamp)
   83             // Clamp ID 
   // Clamp Sub-Record 5
   03             // FSC Sub-Record Type (03h = Clamp)
   22             // Clamp ID 
   // Clamp Sub-Record 6
   03             // FSC Sub-Record Type (03h = Clamp)
   25             // Clamp ID 
   // Clamp Sub-Record 7
   03             // FSC Sub-Record Type (03h = Clamp)
   24             // Clamp ID 
   // Clamp Sub-Record 8
   03             // FSC Sub-Record Type (03h = Clamp)
   23             // Clamp ID 
   // Clamp Sub-Record 9
   03             // FSC Sub-Record Type (03h = Clamp)
   2E             // Clamp ID 
   // Clamp Sub-Record 10
   03             // FSC Sub-Record Type (03h = Clamp)
   27             // Clamp ID 
   // Clamp Sub-Record 11
   03             // FSC Sub-Record Type (03h = Clamp)
   2C             // Clamp ID 
   // Clamp Sub-Record 12
   03             // FSC Sub-Record Type (03h = Clamp)
   5C             // Clamp ID 
   // Clamp Sub-Record 13
   03             // FSC Sub-Record Type (03h = Clamp)
   5D             // Clamp ID 



//****************************************************************
// FSC Record Type = 13h (DIMM Air Velocity Record)
//****************************************************************

//****************************************************************
// 2U4N 3.5" SKU H2300KNP.

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    001B

   // Sensor Record Header
   00CB               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   16                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   13                 // Record Subtype (13h = DIMM Air Velocity)

   B0                 // DIMM aggregate sensor number (B0h = DIMM Thrm Mrgn 1)
   01                 // Domain bit mask (01h = Domain 0)
   32                 // Reference PWM % 1 (32h = 50%)
   46                 // Reference PWM % 2 (46h = 70%)
   64                 // Reference PWM % 3 (64h = 100%)
   16                 // PWM 1 Velocity (16h = 22)
   20                 // PWM 2 Velocity (20h = 32)
   25                 // PWM 3 Velocity (25h = 37)
   07                 // Smoothing coefficient (07h = 7)

   B1                 // DIMM aggregate sensor number (B1h = DIMM Thrm Mrgn 2)
   01                 // Domain bit mask (01h = Domain 0)
   32                 // Reference PWM % 1 (32h = 50%)
   46                 // Reference PWM % 2 (46h = 70%)
   64                 // Reference PWM % 3 (64h = 100%)
   16                 // PWM 1 Velocity (16h = 22)
   20                 // PWM 2 Velocity (20h = 32)
   25                 // PWM 3 Velocity (25h = 37)
   07                 // Smoothing coefficient (07h = 7)
   

//****************************************************************
// FSC Record Type = 13h (DIMM Air Velocity Record)
//****************************************************************

//****************************************************************
// 2U4N 2.5" SKU H2200KNP.

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    001B

   // Sensor Record Header
   00CC               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   16                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   13                 // Record Subtype (13h = DIMM Air Velocity)

   B0                 // DIMM aggregate sensor number (B0h = DIMM Thrm Mrgn 1)
   01                 // Domain bit mask (01h = Domain 0)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   23                 // PWM 1 Velocity (23h = 35)
   30                 // PWM 2 Velocity (30h = 48)
   3E                 // PWM 3 Velocity (3Eh = 62)
   07                 // Smoothing coefficient (07h = 7)

   B1                 // DIMM aggregate sensor number (B1h = DIMM Thrm Mrgn 2)
   01                 // Domain bit mask (01h = Domain 0)
   23                 // Reference PWM % 1 (23h = 35%)
   3C                 // Reference PWM % 2 (3Ch = 60%)
   64                 // Reference PWM % 3 (64h = 100%)
   23                 // PWM 1 Velocity (23h = 35)
   30                 // PWM 2 Velocity (30h = 48)
   3E                 // PWM 3 Velocity (3Eh = 62)
   07                 // Smoothing coefficient (07h = 7)
   
//****************************************************************
// FSC Record Type = 13h (DIMM Air Velocity Record)
//****************************************************************

//****************************************************************
// OTHER SKU.

_SDR_TYPE   C0
_SDR_TAG    'OTHER'
_REC_LEN    001B

   // Sensor Record Header
   00CD               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   16                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   13                 // Record Subtype (13h = DIMM Air Velocity)

   B0                 // DIMM aggregate sensor number (B0h = DIMM Thrm Mrgn 1)
   03                 // Domain bit mask
   00                 // Reference PWM % 1 (00h = 0%)
   32                 // Reference PWM % 2 (32h = 50%)
   64                 // Reference PWM % 3 (64h = 100%)
   0A                 // PWM 1 Velocity (0Ah = 10)
   0A                 // PWM 2 Velocity (0Ah = 10)
   0A                 // PWM 3 Velocity (0Ah = 10)
   07                 // Smoothing coefficient (07h = 7)

   B1                 // DIMM aggregate sensor number (B1h = DIMM Thrm Mrgn 2)
   03                 // Domain bit mask
   00                 // Reference PWM % 1 (00h = 0%)
   32                 // Reference PWM % 2 (32h = 50%)
   64                 // Reference PWM % 3 (64h = 100%)
   0A                 // PWM 1 Velocity (0Ah = 10)
   0A                 // PWM 2 Velocity (0Ah = 10)
   0A                 // PWM 3 Velocity (0Ah = 10)
   07                 // Smoothing coefficient (07h = 7)
   
//****************************************************************
// FSC Record Type = 12h (Aggregate Sensor Configuration Record)
//****************************************************************

//****************************************************************
// 2U4N 3.5" SKU H2300KNP / 2U4N 2.5" SKU H2200KNP

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    0019

   //Sensor Record Header
   00CA               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   14                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   12                 // Record sub-type (12h = Aggregate Sensor Configuration)
   C8                 // Aggregate sensor number (C8h = Agg Thrm Mgn 1)
   07                 // Number of input pairs to follow
   74                 // Input 1 sensor number (74h = P1 Therm Margin)
   FC                 // Input 1 margin reference value (FCh = -4)
   B1                 // Input 2 sensor number (B1h = DIMM Thrm Mrgn 2)
   00                 // Input 2 margin reference value (00h = 0)
   B0                 // Input 3 sensor number (B0h = DIMM Thrm Mrgn 1)
   00                 // Input 3 margin reference value (00h = 0)
   22                 // Input 4 sensor number (22h = SSB Temp)
   53                 // Input 4 margin reference value (53h = 83)
   25                 // Input 5 sensor number (25h = BB P1 VR Temp)
   62                 // Input 5 margin reference value (62h = 98)
   24                 // Input 6 sensor number (24h = BB Mem VR Temp)
   50                 // Input 6 margin reference value (50h = 80)
   21                 // Input 7 sensor number (21h = HSBP Temp)
   14                 // Input 7 margin reference value (14h = 20)

//****************************************************************
// FSC Record Type = 11h (System Airflow Formula)
//****************************************************************

//****************************************************************
// 2U4N 3.5" SKU H2300KNP.

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    0012

   //Sensor Record Header
   00C8               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0D                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   11                 // Record sub-type (11h = System Airflow)
   01                 // Domain Support (Domains 0)
   2200               // Correction Factor 1 (22h = 34 units of .01)
   2C00               // Correction Factor 2 (2Ch = 44 units of .01)
   1E                 // PWM for Correction Factor 1 (1Eh = 30%)
   64                 // PWM for Correction Factor 2 (64h = 100%)
   20                 // Max CFM of Fan (20h = 32)
   03                 // Quantity of fans in this equation


//****************************************************************
// 2U4N 2.5" SKU H2200KNP.

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    0012

   //Sensor Record Header
   00C9               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0D                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   11                 // Record sub-type (11h = System Airflow)
   01                 // Domain Support (Domains 0)
   2C00               // Correction Factor 1 (2Ch = 44 units of .01)
   3000               // Correction Factor 2 (30h = 48 units of .01)
   14                 // PWM for Correction Factor 1 (14h = 20%)
   64                 // PWM for Correction Factor 2 (64h = 100%)
   20                 // Max CFM of Fan (20h = 32)
   03                 // Quantity of fans in this equation


//*****************************************************************************
// FSC Record Type = 19h Exit Air Temp
//*****************************************************************************

//*****************************************************************************
// H2300KNP Chassis

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    0012

   //Sensor Record Header
   00CE               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0D                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   19                 // Record sub-type (19h = Exit Air Temp)
   0200   	          // Alpha S LSB first (0002h = 2 units of .001)
   1100               // Alpha F LSB first (0011h = 17 units of .001)
   07                 // Qmin (07h = 14 CFM)
   15                 // Qmax (15h = 42 CFM)
   00                 // P Offset (00h = 0)
   08                 // Correction Factor at Qmin (08h = 8)
   0B                 // Correction Factor at Qmax (0Bh = 11)


//*****************************************************************************
// H2200KNP Chassis

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    0012

   //Sensor Record Header
   00CF               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   0D                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   19                 // Record sub-type (19h = Exit Air Temp)
   0200   	          // Alpha S LSB first (0002h = 2 units of .001)
   1100               // Alpha F LSB first (0011h = 17 units of .001)
   07                 // Qmin (07h = 14 CFM)
   18                 // Qmax (18h = 44 CFM)
   00                 // P Offset (00h = 0)
   07                 // Correction Factor at Qmin (07h = 7)
   0A                 // Correction Factor at Qmax (0Ah = 10)


//*****************************************************************************
// FSC Record Type = 1Ah (Autoprofile record)
//*****************************************************************************

//*****************************************************************************
// H2300KNP Chassis

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    0019


   //Sensor Record Header
   00D0               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   14                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   1A                 // Record sub-type (1Ah = Auto-profile Record)
   01                 // 70W CPU Multiplier (01h = 1 units of 0.1)
   01     	          // >70W and <105W CPU Multiplier (01h = 1 units of .1)
   01                 // >105W and <145W CPU Multiplier(01h = 1 units of .1)
   02                 // Memory Multiplier (02h = 2 units of 0.1)
   0A                 // HDD Multiplier (28h = 40 units of 0.1)
   03                 // Minimum Performance Profile (03h = 3)
   14                 // Profile 0 Threshold (14h = 20 units of 10)
   1E                 // Profile 1 Threshold (1Eh = 30 units of 10)
   28                 // Profile 2 Threshold (28h = 40 units of 10)
   32                 // Profile 3 Threshold (32h = 50 units of 10)
   3C                 // Profile 4 Threshold (3Ch = 60 units of 10)
   64                 // Profile 5 Threshold (64h = 100 units of 10)
   96                 // Profile 6 Threshold (96h = 150 units of 10)
   23                 // MIC Max/Shift
   23                 // PCI Slot 0 Max/Shift
   13                 // PCI Slot 1 Max/Shift


//*****************************************************************************
// H2200KNP Chassis

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    0019


   //Sensor Record Header
   00D1               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   14                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   1A                 // Record sub-type (1Ah = Auto-profile Record)
   01                 // 70W CPU Multiplier (01h = 1 units of 0.1)
   01     	          // >70W and <105W CPU Multiplier (01h = 1 units of .1)
   01                 // >105W and <145W CPU Multiplier(01h = 1 units of .1)
   02                 // Memory Multiplier (02h = 2 units of 0.1)
   0A                 // HDD Multiplier (28h = 40 units of 0.1)
   03                 // Minimum Performance Profile (03h = 3)
   14                 // Profile 0 Threshold (14h = 20 units of 10)
   1E                 // Profile 1 Threshold (1Eh = 30 units of 10)
   28                 // Profile 2 Threshold (28h = 40 units of 10)
   32                 // Profile 3 Threshold (32h = 50 units of 10)
   3C                 // Profile 4 Threshold (3Ch = 60 units of 10)
   64                 // Profile 5 Threshold (64h = 100 units of 10)
   96                 // Profile 6 Threshold (96h = 150 units of 10)
   23                 // Zeon Phi Max/Shift
   23                 // PCI Slot 0 Max/Shift
   13                 // PCI Slot 1 Max/Shift


//*****************************************************************************
// FSC Record Type = 1Bh (Hard Disk Drive Power)
//*****************************************************************************

//*****************************************************************************
// H2300KNP Chassis - 12x3.5 HDD

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X35'
_REC_LEN    000A


   //Sensor Record Header
   00D2               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   05                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   1B                 // Record sub-type (1Bh = HDD Power)
   16                 // HDD Watts (16h = 45 Units of 2)


//*****************************************************************************
// H2200KNP Chassis - 16x2.5 HDD

_SDR_TYPE   C0
_SDR_TAG    '2U4N_BP_X25'
_REC_LEN    000A

   //Sensor Record Header
   00D3               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   05                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   1B                 // Record sub-type (1Bh = HDD Power)
   12                 // HDD Watts (12h = 36 Units of 2)


//*****************************************************************************
// SDR Version Records
//*****************************************************************************

//*****************************************************************************
//Normal Chassis Version Records

_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0015

   // Sensor Record Header
   00D4               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   10                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   'SDR File 1.24'    // String Bytes


_SDR_TYPE   C0
_SDR_TAG    'BCP_2U4N'
_SDR_TAG    'TEST_PLATE'
_SDR_TAG    'OTHER'
_REC_LEN    0018

   // Sensor Record Header
   00D5               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   13                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   'SDR Package 1.24' // String Bytes
)

//====================================================================//
//Shipping (Default) Version Records
//
_SDR_TYPE   C0
_SDR_TAG    'SHIPPING'
_REC_LEN    0016

   // Sensor Record Header
   00D6               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   11                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   'SDR File D1.22'   // String Bytes


_SDR_TYPE   C0
_SDR_TAG    'SHIPPING'
_REC_LEN    0019

   // Sensor Record Header
   00D7               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   14                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   'SDR Package D1.22'// String Bytes
)

//====================================================================//
//Functional Test Version Records
//
_SDR_TYPE   C0
_SDR_TAG   'FCT'
_REC_LEN    0016

   // Sensor Record Header
   00D8               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   11                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   'SDR File F1.22'   // String Bytes

_SDR_TYPE   C0
_SDR_TAG   'FCT'
_REC_LEN    0019

   // Sensor Record Header
   00D9               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   14                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   'SDR Package F1.22'// String Bytes

//====================================================================//
//Functional Test 2 (FOQM) Version Records
//
_SDR_TYPE   C0
_SDR_TAG   'FOQM'
_REC_LEN    0016

   // Sensor Record Header
   00DA               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   11                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   'SDR File f1.22'   // String Bytes

_SDR_TYPE   C0
_SDR_TAG   'FOQM'
_REC_LEN    0019

   // Sensor Record Header
   00DB               // Record ID
   51                 // SDR Version
   C0                 // Record Type
   14                 // Record Length

   // Record Body Bytes
   570100             // Manufacturer ID
   'SDR Package f1.22'// String Bytes
)
