EFI System Firmware Update Package Install Instructions

Intel (R) Server Boards S2400BB, Intel (R) Server Systems R1000BB/R2000BB family
Firmware Update Package Update Instructions 

Released - July 13, 2017

*************************************************************************************
This Update package includes the following system software updates:

  System BIOS  - 02.06.0006
  ME Firmware  - 02.01.07.328
  BMC Firmware - 01.28.10603
  FRUSDR       - 1.06

Important NOTES: 

- All the updates provided in this package are EFI based (unless otherwise noted).To 
  run these updates, you must boot the system to the embedded EFI shell and then 
  access the USB device or hard disk containing the system software updates.

 
*************************************************************************************
                       SYSTEM HARDWARE and SOFTWARE REQUIREMENTS
*************************************************************************************
The contents of this update package is used to update the System Firmware for 
the following Intel Server Products only:

  - Intel(R) Server Board S2400BB Fab 2 or later
  - Intel(R) Server System R1000BB family
  - Intel(R) Server System R2000BB family


This update package can only be used if the board has following BIOS/ME/BMC/FRUSDR versions or above:
  - BIOS 01.06.0002
  - ME 02.01.05.107
  - BMC 01.16.4010
  - FRUSDR 1.02

The utilities used to update the System Firmware are:
  - Iflash32 11.0 build 11
  - FWPIAUPD 11.0 build 9
  - FRUSDR 11.0 build 9

*************************************************************************************
                 Standard Update Procedure from the embedded EFI Shell
*************************************************************************************

- Unzip package and copy all files to a folder in USB disk on key
- Insert USB disk on key to server / workstation USB port
- Boot Server to EFI shell
- Run command "map -r" in EFI shell to mount USB disk on key
- Run command "fs0:" to change folder to USB disk on key, USB key may also mount to
  fs1:. The number of "fs#" is dependent on the result of command "map -r"
- Change folder to the folder storing the firmware package
- Run command "Startup.nsh" to start updating all the firmware and BIOS

Warning: 
!!Do NOT reboot or shut down power from your system during following software update!!

*************************************************************************************
If you want to update single components like BMC/BIOS/ME/FRUSDR separately, please go to the 
root folder and execute the specified scripts separately, and follow below 
update process:
  1) Update BMC Firmware
  2) Update System BIOS
  3) Update ME Firmware
  4) Update FRUSDR
*************************************************************************************

*************************************************************************************
                                Update BMC Firmware
*************************************************************************************
IMPORTANT BMC UPDATE NOTES:

!!!!**********************************************************************!!!!
- If BMC 1.10 is not pre-installed then please install that release first
   prior to installing this release. 
!!!!**********************************************************************!!!!

1) Boot the system to the EFI shell and go to root folder
2) At the shell prompt, run "UpdateBMC.nsh" to start BMC Firmware update
3) When complete, go to the BIOS update section described below, or power off the 
   system and cycle AC power before continuing.

*************************************************************************************
                                 Update System BIOS 
*************************************************************************************

Warning:
!!Ensure BIOS 01.03.0002 or later is installed in your system prior to running this BIOS update!!

1) Boot the system to the EFI shell and go to root folder
2) At the shell prompt, run "UpdateBIOS.nsh" to start BIOS update
3) When complete, reboot the system and enter BIOS Setup by pressing the F2 Key during
   POST 
4) Verify the BIOS string on main BIOS menu
5) Press F9 to load defaults and press F10 to save and reset the system
6) Go to the ME firmware update section described below
The BIOS update is complete. Either reboot the server or go to the ME firmware Update section described below.


*************************************************************************************
                                   Update ME Firmware
*************************************************************************************
1) Boot the system to the EFI shell and go to root folder
2) At the shell prompt, run "UpdateME.nsh" to start ME firwmare update
3) When complete, go to the FRUSDR update section described below, or power off the 
   system and cycle AC power before continuing.
   
*************************************************************************************
                                      Update FRUSDR
*************************************************************************************
1) Boot the system to the EFI shell and go to root folder
2) At the EFI command prompt, run "UpdateFRUSDR.nsh" to start FRUSDR update
3) Answer questions and enter desired information when prompted.
4) When complete, reboot the system by front control panel

*************************************************************************************
                                    Verifying updates
*************************************************************************************

1)  During POST, hit the F2 Key when prompted to access the BIOS Setup Utility
2)  Hit the F9 key to load BIOS Defaults
3)  At the MAIN menu verify the BIOS revision
4)  Move cursor to the SERVER MANAGEMENT Menu
5)  Move cursor down to the SYSTEM INFORMATION Option and hit Enter
6)  Verify the BMC Firmware revision
7)  Verify the SDR revision
8)  Verify the ME Firmware revision
9)  Hit the F10 Key to save changes and Exit


The System Software Update is Complete.



*******************************************************************************
BIOS Recovery Process
*******************************************************************************
In the unlikely event the BIOS is corrupted, leaving the system in an 
unbootable state, it may be necessary to perform the following BIOS Recovery 
procedure.  

1.  Copy the following BIOS update files to the root directory of a USB media 
device (Recovery Media):
Note: These specific files will be located in the "BIOS Recovery Files" folder 
included in the System Update Package.

- IPMI.EFI 
- IFlash32.EFI 
- RML.ROM 
- R##.##.####REC.CAP (where ##.##.#### = BIOS revision number) 
- STARTUP.NSH (modified to support BIOS recovery)


2.  Power OFF the system

3.  Locate the BIOS Recovery Jumper on the server board and move the jumper 
block from pins 1-2 (default) to pins 2-3 (recovery setting)

4.  Insert the recovery media into any available USB port on the back of 
the server
Note: The front panel USB ports may not work for this procedure on some server 
systems.

5.  Power ON the system

6.  The system will automatically boot into the embedded EFI Shell

7.  The STARTUP.NSH file automatically executes and initiates the flash update.
When complete, the IFlash utility will display a message

8.  Power OFF the system and return the BIOS Recovery jumper to its default 
position

9.  Remove recovery media from the USB port

10. Power ON the system 

11. Do *NOT* interrupt the BIOS POST during the first boot.

=============================================================================
                            LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products. 
No license, express or implied, by estoppel or otherwise, to any intellectual 
property rights is granted by this document. Except as provided in Intel's 
Terms and Conditions of Sale for such products, Intel assumes no liability 
whatsoever, and Intel disclaims any express or implied warranty, relating to 
sale and/or use of Intel products including liability or warranties relating 
to fitness for a particular purpose, merchantability, or infringement of any 
patent, copyright or other intellectual property right. Intel Corporation may 
have patents or pending patent applications, trademarks, copyrights, or other 
intellectual property rights that relate to the presented subject matter.  
The furnishing of documents and other materials and information does not 
provide any license, express or implied, by estoppel or otherwise, to any 
such patents, trademarks, copyrights, or other intellectual property rights.  
Intel products are not intended for use in medical, life saving, or life 
sustaining applications. Intel may make changes to specifications and product 
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation. 
*Other names and brands are the property of their respective owners.
Copyright (c) 2017 Intel Corporation.

A portion of this firmware is open source code, which falls under the
GPL 2.0 license.  

[END OF RELEASE NOTES]