This release note and the software that accompanies it are copyright (c) 2017, Intel Corporation or its suppliers, 
and may only be installed and used in accordance with the license that accompanies the software.

This Software is furnished under license and may only be used or copied in accordance with the terms of that license. 
No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. 
The Software is subject to change without notice, and should not be construed as a commitment by Intel Corporation or 
its suppliers to market, license, sell or support any product or technology. Unless otherwise provided for in the license under 
which this Software is provided, the Software is provided AS IS, with no warranties of any kind, express or implied. 
Except as expressly permitted by the Software license, neither Intel Corporation nor its suppliers assumes any responsibility or 
liability for any errors or inaccuracies that may appear herein. Except as expressly permitted by the Software license, no part 
of the Software may be reproduced, stored in a retrieval system, transmitted in any form, or distributed by any means  without 
the express written consent of Intel Corporation.

This download supports Intel(R) RAID Controllers RMSP3JD160J, RSP3GD016J, RSP3QD160J.


================
Package Information
================
Package version: 2.00.06.01 (Phase 2 patch 1)

================
Known Restrictions
================
Legacy OpROMs are not supported.  Use UEFI mode only.
Mixed mode (NVMe & SAS/SATA) is not supported in Phase 2 FW.
Amber LEDs are not supported with NVMe disks in Phase 2 FW.

================
Known Bugs
================
N/A

================
Update Instructions
================
1. Unzip all of the files from the zip package onto USB key, maintaining the directory structure. Please make sure that the USB key is fully compatible with the EFI version on your motherboard. Some incompatible versions may prevent USB key working normally.

2. Boot to the EFI shell
    - Press 'F2'  during POST to enter BIOS Setup
    - Select Boot Manager -> EFI Shell

3. Change drive and directory location to where you unzipped the package by typing the following commands:
     fs0: <press Enter>     
     cd <SAS FW directory name>

   Note:  You can always get a list of files and sub-directories in the current directory by typing 'dir' command.
          Instead of 'fs0: you may need to type 'fs1:' or 'fs2:', etc. depending on your drive configuration and removable media type.


4. Type in the name of the batch file that matches your board model and press <Enter>: 

   rmsp3jd160j.nsh          RMSP3JD160J	with SATA/SAS support only
   rsp3gd016j.nsh		  	RSP3GD016J with SATA/SAS support only
   rsp3qd160j.nsh		    RSP3QD160J with SATA/SAS support only
   rmsp3jd160j.nvme.nsh     RMSP3JD160J	with NVME support only
   rsp3qd160j.nvme.nsh		RSP3QD160J with NVME support only
   
   
5. Wait for the flash to complete. Do NOT reboot the system during the update.

================
Fixes/Updates
================
Package Version 02.00.06.01
1) Fix to Incorrect memory access in 3416/3516 startup
2) Fix to 3416/3516 IOP: Firmware becomes unresponsive if host performs I2C transactions

Package Version 02.00.05.05
1) This version is the initial release

*Third-party trademarks are the property of their respective owners.