You are here: Introduction > Intel AMT and Security Considerations > Password Format

# Password Format

Most passwords you define in Intel SCS must be between 8-32 characters, with a minimum of one of each of these:

- A number
- A non alphanumeric character
- A lowercase Latin letter
- An uppercase Latin letter

Note:
The underscore (_) character is counted as an alphanumeric character. The Remote Frame Buffer (RFB) password must be EXACTLY 8 characters long. This password is only used for KVM sessions using port 5900 (see VNC Clients). The colon (:), comma (,), and double quote (“) characters are NOT permitted in these passwords: Intel MEBX password Digest user passwords (including the Admin user) RFB password